-- *******************************************************************
-- CISCO-LWAPP-CDP-MIB.my
-- Mar 2007 ,   Ambika Prasad Mohanty
-- Copyright (c) 2007 by Cisco Systems Inc.
-- All rights reserved.
-- ******************************************************************

CISCO-LWAPP-CDP-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Unsigned32,
    Counter32
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP
        FROM SNMPv2-CONF
    DisplayString,
    TruthValue
        FROM SNMPv2-TC
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    InetAddress,
    InetAddressType
        FROM INET-ADDRESS-MIB
    InterfaceIndexOrZero
        FROM IF-MIB
    cLApSysMacAddress
        FROM CISCO-LWAPP-AP-MIB
    CLCdpAdvtVersionType
        FROM CISCO-LWAPP-TC-MIB
    ciscoMgmt
        FROM CISCO-SMI;

-- ********************************************************************
-- *  MODULE IDENTITY
-- ********************************************************************

ciscoLwappCdpMIB MODULE-IDENTITY
    LAST-UPDATED    "200703280000Z"
    ORGANIZATION    "Cisco Systems Inc."
    CONTACT-INFO
            "Cisco Systems,
            Customer Service

            Postal: 170 West Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            Email: cs-wnbu-snmcp@cisco.com"
    DESCRIPTION
        "This MIB is intended to be implemented on all those
        devices operating as Central Controllers (CC) that
        terminate the Light Weight Access Point Protocol
        tunnel from Light-weight LWAPP Access Points.

        This MIB provides configuration and status information
        about CDP neighbors of LWAPP APs. The MIB provides  
        configuration of CDP feature on the LWAPP Access Points.
        The MIB can also be used to retrive the status of the 
        CDP cache information on the various LWAPP LWAPP Access
        Points.

        The CDP MIB is also supported by Controller and provides
        configuration and status information about CDP neighbours
        of the controller.

        The relationship between CC and the LWAPP APs
        can be depicted as follows:

        +......+     +......+     +......+           +......+
        +      +     +      +     +      +           +      +
        +  CC  +     +  CC  +     +  CC  +           +  CC  +
        +      +     +      +     +      +           +      +
        +......+     +......+     +......+           +......+
        ..            .             .                 .
        ..            .             .                 .
        .  .            .             .                 .
        .    .            .             .                 .
        .      .            .             .                 .
        .        .            .             .                 .
        +......+ +......+     +......+      +......+          +......+
        +      + +      +     +      +      +      +          +      +
        +  AP  + +  AP  +     +  AP  +      +  AP  +          +  AP  +
        +      + +      +     +      +      +      +          +      +
        +......+ +......+     +......+      +......+          +......+
        .              .             .                 .
        .  .              .             .                 .
        .    .              .             .                 .
        .      .              .             .                 .
        .        .              .             .                 .
        +......+ +......+     +......+      +......+          +......+
        +      + +      +     +      +      +      +          +      +
        +  MN  + +  MN  +     +  MN  +      +  MN  +          +  MN  +
        +      + +      +     +      +      +      +          +      +
        +......+ +......+     +......+      +......+          +......+


        The LWAPP tunnel exists between the controller and
        the APs.  The MNs communicate with the APs through
        the protocol defined by the 802.11 standard.

        LWAPP APs, upon bootup, discover and join one of the
        controllers and the controller pushes the configuration,
        that includes the WLAN parameters, to the LWAPP APs.
        The APs then encapsulate all the 802.11 frames from
        wireless clients inside LWAPP frames and forward
        the LWAPP frames to the controller.

                           GLOSSARY

        Access Point ( AP )

        An entity that contains an 802.11 medium access
        control ( MAC ) and physical layer ( PHY ) interface
        and provides access to the distribution services via
        the wireless medium for associated clients.  

        LWAPP APs encapsulate all the 802.11 frames in
        LWAPP frames and sends it to the controller to which
        it is logically connected.

        Basic Service Set Identifier (BSSID)

        The identifier for the service set comprising of
        all the 802.11 stations under the control of
        one coordinating Access Point.  This identifier
        happens to be the MAC address of the dot11 radio
        interface of the Access Point.  The wireless
        clients that associate with the Access Point
        get the wired uplink through this particular 
        dot11 interface. 

        Central Controller ( CC )

        The central entity that terminates the LWAPP protocol
        tunnel from the LWAPP APs.  Throughout this MIB,
        this entity also referred to as 'controller'. 

        Light Weight Access Point Protocol ( LWAPP ) 

        This is a generic protocol that defines the 
        communication between the Access Points and the
        Central Controller. 

        Cisco Discovery Protocol ( CDP )

        Protocol for discovery of neighboring devices.


        REFERENCE

        [1] Part 11 Wireless LAN Medium Access Control ( MAC )
        and Physical Layer ( PHY ) Specifications.

        [2] Draft-obara-capwap-lwapp-00.txt, IETF Light 
        Weight Access Point Protocol."
    REVISION        "200703280000Z"
    DESCRIPTION
        "This is the initial version of this module."
    ::= { ciscoMgmt 623 }


ciscoLwappCdpMIBNotifs  OBJECT IDENTIFIER
    ::= { ciscoLwappCdpMIB 0 }

ciscoLwappCdpMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoLwappCdpMIB 1 }

ciscoLwappCdpMIBConform  OBJECT IDENTIFIER
    ::= { ciscoLwappCdpMIB 2 }

clcCdpTraffic  OBJECT IDENTIFIER
    ::= { ciscoLwappCdpMIBObjects 1 }

clcCdpGlobalConfig  OBJECT IDENTIFIER
    ::= { ciscoLwappCdpMIBObjects 2 }

clcCdpApCacheStatus  OBJECT IDENTIFIER
    ::= { ciscoLwappCdpMIBObjects 3 }

clcCdpApCacheConfig  OBJECT IDENTIFIER
    ::= { ciscoLwappCdpMIBObjects 4 }


-- *******************************************************************
-- The CDP Traffic Metrics
-- *******************************************************************
clcCdpInPackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of total CDP packets received by the Controller." 
    ::= { clcCdpTraffic 1 }

clcCdpOutPackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of total CDP packets sent by the Controller." 
    ::= { clcCdpTraffic 2 }

clcCdpChecksumErrorPackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Total number of CDP packets that experienced
        checksum error." 
    ::= { clcCdpTraffic 3 }

clcCdpNoMemoryPackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Total number of CDP packets that were dropped
        because of no memory availability." 
    ::= { clcCdpTraffic 4 }

clcCdpInvalidPackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Total number of CDP packets that were invalid." 
    ::= { clcCdpTraffic 5 }

-- ********************************************************************
-- *  Global CDP Configuration
-- ********************************************************************
clcCdpAdvtVersion OBJECT-TYPE
    SYNTAX          CLCdpAdvtVersionType
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Cisco Discovery Protocol advertisement version."
    DEFVAL          { cdpv1 } 
    ::= { clcCdpGlobalConfig 1 }

clcCdpMessageInterval OBJECT-TYPE
    SYNTAX          Unsigned32 (5..900 )
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The interval (in seconds) at which CDP messages
        are to be generated."
    DEFVAL          { 60 } 
    ::= { clcCdpGlobalConfig 2 }

clcCdpGlobalEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This is a template variable to enable / disable CDP
        on all APs.
        When 'true' is set, then internally CDP is enabled 
        on all APs associated with the Controller.
        When 'false' is set, then internally CDP is disabled 
        on all APs associated with the Controller.
        However, setting this attribute has no effect when CDP
        is disabled globally, that is when the cdpGlobalRun from 
        the CISCO-CDP-MIB is set to 'false'on the Controller."
    DEFVAL          { false } 
    ::= { clcCdpGlobalConfig 3 }
-- *******************************************************************
-- The CDP configurations at AP level
-- *******************************************************************

clcCdpApTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF ClcCdpApEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The (conceptual) table containing the status of Cisco
        Discovery Protocol on LWAPP Access Points. An entry is added
        to the table when an Aceess Point joins a controller. An entry
        is deleted when the Access Point disassociates from the 
        controller. This table is used to configure CDP feature per Access
        Point."
    ::= { clcCdpApCacheConfig 1 }

clcCdpApEntry OBJECT-TYPE
    SYNTAX          ClcCdpApEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry (conceptual row) in the clcCdpApTable,
        containing the status of CDP on an AP.

        Consider a setup where two APs, 'AP1' and 'AP2'
        have been connected to a CISCO-3750 switch.
        Both the APs register with WLAN CONTROLLER 440x
        which is on LAN/Internet/Intranet.

        +.........................+   
        +                         +   
        +  WLAN CONTROLLER 4400   +   
        +       10.14.2.11        +   
        +.........................+   
                  .. 
                  .. 
         INTERNET  ..  LAN
                  .. 
           +...............+   
           +               +   
           +  SWITCH-3750  +   
           +   10.16.1.1   +   
           +...............+   
                  .. 
                .    .
              .        .
            .            .
          .                .
        .                    .
        +......+                  +......+          
        +      +                  +      +          
        + AP1  +                  +  AP2 +          
        +      +                  +      +          
        +......+                  +......+ 

        00:12:CF:DA:29:11        23:43:CE:9A:66:76

        10.16.1.43                  10.16.1.45  

        Given the above example, the clcCdpApEntry on 
        WLAN CONTROLLER 4400 looks like :    

        ------------------------------------------------------------------
        |  MIB - ATTRIBUTES   |       ROW#1        |       ROW#2         |
        ------------------------------------------------------------------
        | cLApSysMacAddress   | 00:12:CF:DA:29:11  | 23:43:CE:9A:66:76   |
        ------------------------------------------------------------------
        | clcCdpApStatus       |       true         |       false         |
        ------------------------------------------------------------------"
    INDEX           { cLApSysMacAddress } 
    ::= { clcCdpApTable 1 }

ClcCdpApEntry ::= SEQUENCE {
        clcCdpApCdpEnable TruthValue
}

clcCdpApCdpEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "An indication of whether the Cisco Discovery Protocol
        is currently running on this AP. 
        When set to 'true', that means CDP is enabled on
        the AP denoted by MAC address cLApSysMacAddress.
        When set to 'false', that means CDP is disabled on
        the AP denoted by MAC address cLApSysMacAddress.

        This variable has no effect when CDP is globally
        disabled. That is when the cdpGlobalRun from the
        CISCO-CDP-MIB is set to 'false'."
    DEFVAL          { false } 
    ::= { clcCdpApEntry 1 }
 

-- *******************************************************************
-- The CDP-AP Address Cache Table
-- *******************************************************************

clcCdpApCacheTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF ClcCdpApCacheEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the cached neighbor
        information obtained via receiving CDP messages on APs.
        Entries are added to this table when a CDP advertisement
        is received from a neighboring device. Entries get deleted 
        when CDP is disabled on the interface or globally."
    ::= { clcCdpApCacheStatus 1 }

clcCdpApCacheEntry OBJECT-TYPE
    SYNTAX          ClcCdpApCacheEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in the clcCdpApCacheTable,
        containing the information received via CDP on one
        interface from one device.  Entries appear when
        a CDP advertisement is received from a neighbor
        device.  Entries disappear when CDP is disabled
        on the interface or globally.

        Consider a setup where two APs, 'AP1' and 'AP2'
        have been connected to a CISCO-3750 switch.
        Both the APs register with WLAN CONTROLLER 4400
        which is on LAN/Internet/Intranet.

        +.........................+   
        +                         +   
        +  WLAN CONTROLLER 4400   +   
        +       10.14.2.11        +   
        +.........................+   
                  .. 
                  .. 
         INTERNET  ..  LAN
                  .. 
           +...............+   
           +               +   
           +  SWITCH-3750  +   
           +   10.16.1.1   +   
           +...............+   
        FE 0/13      ..    FE 0/15
                .    .
              .        .
            .            .
          .                .
        .                    .
        +......+                  +......+          
        +      +                  +      +          
        + AP1  +                  +  AP2 +          
        +      +                  +      +          
        +......+                  +......+ 

        00:12:CF:DA:29:11        23:43:CE:9A:66:76

        10.16.1.43                  10.16.1.45  

        Given the above example, the clcCdpApEntry on 
        WLAN CONTROLLER 4400 looks like :    

        ----------------------------------------------------------------------
        |  MIB - ATTRIBUTES           |       ROW#1       |       ROW#2      |
        ----------------------------------------------------------------------
        | cLApSysMacAddress           | 00:12:CF:DA:29:11 | 23:43:CE:9A:66:76|
        ----------------------------------------------------------------------
        | clcCdpApCacheDeviceIndex     |   16              | 16               |
        ----------------------------------------------------------------------
        | clcCdpApCacheApName          | AP1               | AP2              |
        ----------------------------------------------------------------------
        | clcCdpApCacheApAddressType   |  ip(1)            | ip(1)            |
        ----------------------------------------------------------------------
        | clcCdpApCacheApAddress       | 10.16.1.43        | 10.16.1.45       |
        ----------------------------------------------------------------------
        | clcCdpApCacheLocalInterface  | Port - 1          | Port -2          |
        ----------------------------------------------------------------------
        | clcCdpApCacheNeighName       | SWITCH-3750       | SWITCH-3750      |
        ----------------------------------------------------------------------
        | clcCdpApCacheNeighAddressType| ip(1)             | ip(1)            |
        ----------------------------------------------------------------------
        | clcCdpApCacheNeighAddress    | 10.16.1.1         | 10.16.1.1        |
        ----------------------------------------------------------------------
        | clcCdpApCacheNeighInterface  | FE 0/13           | FE 0/45          |
        ----------------------------------------------------------------------
        | clcCdpApCacheNeighVersion    | IOS Ver2.2. ...   | IOS Ver 2.2. ... |
        ----------------------------------------------------------------------
        | clcCdpApCacheAdvtVersion     | cdpv1(1)          | cdpv2(2)         |
        ----------------------------------------------------------------------
        | clcCdpApCachePlatform        | WS-C3750-24P      | WS-C3750-24P     |
        ----------------------------------------------------------------------
        | clcCdpApCacheCapabilities    | RSI               | RSI              |
        ----------------------------------------------------------------------
        | clcCdpApCacheHoldtimeLeft    | 179               | 165              |
        ----------------------------------------------------------------------"
    INDEX           {
                        cLApSysMacAddress,
                        clcCdpApCacheDeviceIndex
                    } 
    ::= { clcCdpApCacheTable 1 }

ClcCdpApCacheEntry ::= SEQUENCE {
        clcCdpApCacheDeviceIndex      Unsigned32,
        clcCdpApCacheApName           SnmpAdminString,
        clcCdpApCacheApAddressType    InetAddressType,
        clcCdpApCacheApAddress        InetAddress,
        clcCdpApCacheLocalInterface   InterfaceIndexOrZero,
        clcCdpApCacheNeighName        DisplayString,
        clcCdpApCacheNeighAddressType InetAddressType,
        clcCdpApCacheNeighAddress     InetAddress,
        clcCdpApCacheNeighInterface   DisplayString,
        clcCdpApCacheNeighVersion     DisplayString,
        clcCdpApCacheAdvtVersion      CLCdpAdvtVersionType,
        clcCdpApCachePlatform         DisplayString,
        clcCdpApCacheCapabilities     OCTET STRING,
        clcCdpApCacheHoldtimeLeft     Unsigned32
}

clcCdpApCacheDeviceIndex OBJECT-TYPE
    SYNTAX          Unsigned32 (0..2147483647 )
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A unique value for each device from which CDP messages
        are being received." 
    ::= { clcCdpApCacheEntry 1 }

clcCdpApCacheApName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Name assigned to this AP. If an AP is not configured its
        factory default name will be ap:<last three byte of MAC
        Address>.
        eg. ap:af:12:be" 
    ::= { clcCdpApCacheEntry 2 }

clcCdpApCacheApAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "An indication of the type of address contained in the
        corresponding instance of clcCdpApCacheAddress for the AP." 
    ::= { clcCdpApCacheEntry 3 }

clcCdpApCacheApAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This is the address of the AP.
        For example, if the the corresponding instance of
        clcCdpApCacheApAddressType had the value 'ip(1)', then this object
        would be an IP-address." 
    ::= { clcCdpApCacheEntry 4 }

clcCdpApCacheLocalInterface OBJECT-TYPE
    SYNTAX          InterfaceIndexOrZero
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This is the local port on which LWAPP encapsulated CDP
        packets was received." 
    ::= { clcCdpApCacheEntry 5 }

clcCdpApCacheNeighName OBJECT-TYPE
    SYNTAX          DisplayString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The Device-ID string as reported in the most recent CDP
        message.  The zero-length string indicates no Device-ID
        field (TLV) was reported in the most recent CDP
        message." 
    ::= { clcCdpApCacheEntry 6 }

clcCdpApCacheNeighAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "An indication of the type of address contained in the
        corresponding instance of clcCdpApCacheAddress of Neighbor." 
    ::= { clcCdpApCacheEntry 7 }

clcCdpApCacheNeighAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The (first) network-layer address of the device's
        SNMP-agent as reported in the most recent CDP message.
        For example, if the the corresponding instance of
        clcCdpApCacheApAddressType had the value 'ip(1)', then this object
        would be an IP-address." 
    ::= { clcCdpApCacheEntry 8 }

clcCdpApCacheNeighInterface OBJECT-TYPE
    SYNTAX          DisplayString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The Port-ID string as reported in the most recent CDP
        message.  This will typically be the value of the ifName
        object (e.g., 'Ethernet0').  The zero-length string
        indicates no Port-ID field (TLV) was reported in the
        most recent CDP message." 
    ::= { clcCdpApCacheEntry 9 }

clcCdpApCacheNeighVersion OBJECT-TYPE
    SYNTAX          DisplayString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The Version string refers to the software running on
        neighboring device." 
    ::= { clcCdpApCacheEntry 10 }

clcCdpApCacheAdvtVersion OBJECT-TYPE
    SYNTAX          CLCdpAdvtVersionType
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Cisco Discovery Protocol advertisement version."
    DEFVAL          { cdpv1 } 
    ::= { clcCdpApCacheEntry 11 }

clcCdpApCachePlatform OBJECT-TYPE
    SYNTAX          DisplayString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The Device's Hardware Platform as reported in the most
        recent CDP message.  The zero-length string indicates
        that no Platform field (TLV) was reported in the most
        recent CDP message." 
    ::= { clcCdpApCacheEntry 12 }

clcCdpApCacheCapabilities OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (0..32))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The Device's Functional Capabilities as reported in the
        most recent CDP message.  For latest set of specific
        values, see the latest version of the CDP specification.
        The zero-length string indicates no Capabilities field
        (TLV) was reported in the most recent CDP message." 
    ::= { clcCdpApCacheEntry 13 }

clcCdpApCacheHoldtimeLeft OBJECT-TYPE
    SYNTAX          Unsigned32 (10..255 )
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The time left, in seconds, before the CDP
        neighbor entry gets aged-out."
    DEFVAL          { 180 } 
    ::= { clcCdpApCacheEntry 14 }
 

-- *******************************************************************
-- *    Compliance statements
-- *******************************************************************
ciscoLwappCdpMIBCompliances  OBJECT IDENTIFIER
    ::= { ciscoLwappCdpMIBConform 1 }

ciscoLwappCdpMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoLwappCdpMIBConform 2 }


ciscoLwappCdpMIBCompliance MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappCdpMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        clcCdpRev01ConfigGroup,
                        clcCdpRev01StatusGroup
                    }
    ::= { ciscoLwappCdpMIBCompliances 1 }

-- *******************************************************************
-- *    Units of conformance
-- *******************************************************************
clcCdpRev01ConfigGroup OBJECT-GROUP
    OBJECTS         {
                        clcCdpApCdpEnable,
                        clcCdpAdvtVersion,
                        clcCdpMessageInterval,
                        clcCdpGlobalEnable
                    }
    STATUS          current
    DESCRIPTION
        "This is a collection of objects which can
        configured to control functional parameters 
        of Cisco Discovery Protocol feature in 
        WLAN controllers and LWAPP APs."
    ::= { ciscoLwappCdpMIBGroups 1 }

clcCdpRev01StatusGroup OBJECT-GROUP
    OBJECTS         {
                        clcCdpApCacheApName,
                        clcCdpApCacheApAddressType,
                        clcCdpApCacheApAddress,
                        clcCdpApCacheLocalInterface,
                        clcCdpApCacheNeighName,
                        clcCdpApCacheNeighAddressType,
                        clcCdpApCacheNeighAddress,
                        clcCdpApCacheNeighInterface,
                        clcCdpApCacheNeighVersion,
                        clcCdpApCacheAdvtVersion,
                        clcCdpApCachePlatform,
                        clcCdpApCacheCapabilities,
                        clcCdpApCacheHoldtimeLeft,
                        clcCdpInPackets,
                        clcCdpOutPackets,
                        clcCdpChecksumErrorPackets,
                        clcCdpNoMemoryPackets,
                        clcCdpInvalidPackets
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represents the information
        about the general status attributes of Cisco Discovery
        Protocol in WLAN controllers and LWAPP APs."
    ::= { ciscoLwappCdpMIBGroups 2 }

END



















































