LIEBERT-GP-ENVIRONMENTAL-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, 
    OBJECT-IDENTITY, 
    OBJECT-TYPE,
    Unsigned32, 
    Integer32
        FROM SNMPv2-SMI
    lgpEnvironmental, 
    liebertEnvironmentalModuleReg
        FROM LIEBERT-GP-REGISTRATION-MIB
    ;

-- =============================================================================
-- Module Identification and Registration
-- =============================================================================

liebertGlobalProductsEnvironmentalModule MODULE-IDENTITY
  LAST-UPDATED "200811170000Z"
  ORGANIZATION "Liebert Corporation"
  CONTACT-INFO
      "Contact:   Technical Support

      Postal:
      Liebert Corporation
      1050 Dearborn Drive
      P.O. Box 29186
      Columbus OH, 43229
      US

      Tel: +1 (800) 222-5877

      E-mail: liebert.monitoring@emerson.com
      Web:    www.liebert.com

      Author:  Gregory M. Hoge"

   DESCRIPTION
      "The MIB module used to register Liebert SNMP OIDs.

      Copyright 2000-2008 Liebert Corporation. All rights reserved.
      Reproduction of this document is authorized on the condition
      that the forgoing copyright notice is included.

      This Specification is supplied 'AS IS' and Liebert Corporation
      makes no warranty, either express or implied, as to the use,
      operation, condition, or performance of the Specification."

   REVISION "200811170000Z"
   DESCRIPTION
    "Added support for NXL unit."

   REVISION "200807020000Z"
   DESCRIPTION
    "SMIv2 changes (INTEGER to Integer32.
     Corrected spelling errors."

   REVISION "200801100000Z"
   DESCRIPTION
    "Modified contact email address."

   REVISION "200705290000Z"
   DESCRIPTION
    "Added support for XDF Unit."

   REVISION "200608150000Z"
   DESCRIPTION
    "Added support for HP release."

   REVISION "200602220000Z"
   DESCRIPTION
    "Added support for Liebert DS Unit."

   ::= { liebertEnvironmentalModuleReg 1 }

-- =============================================================================
--  lgpEnvironmental - Liebert Environmental Registrations
-- =============================================================================

lgpEnvTemperature OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "This sub-tree is used to register Liebert temperature object
        identifiers."
    REFERENCE
        "The registrations for the objects in this sub-tree are
        defined below in the sub-section titled Liebert Environmental
        Temperature Group."
    ::= { lgpEnvironmental 1 }

lgpEnvHumidity OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "This sub-tree is used to register Liebert humidity object
        identifiers."
    REFERENCE
        "The registrations for the objects in this sub-tree are
        defined below in the sub-section titled Liebert Environmental
        Humidity Group."
    ::= { lgpEnvironmental 2 }

lgpEnvState OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "This sub-tree is used to register Liebert environmental state object
        identifiers."
    REFERENCE
        "The registrations for the objects in this sub-tree are
        defined below in the sub-section titled Liebert Environmental
        State Group."
    ::= { lgpEnvironmental 3 }

lgpEnvConfig OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "This sub-tree is used to register Liebert environmental configuration
        object identifiers."
    REFERENCE
        "The registrations for the objects in this sub-tree are
        defined below in the sub-section titled Liebert Environmental
        Configuration Group."
    ::= { lgpEnvironmental 4 }

lgpEnvControl OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "This sub-tree is used to register Liebert environmental control
         object identifiers."
    REFERENCE
        "The registrations for the objects in this sub-tree are
        defined below in the sub-section titled Liebert Environmental
        Control Group."
    ::= { lgpEnvironmental 5 }

lgpEnvStatistics OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "This sub-tree is used to register Liebert environmental statistic
        object identifiers."
    REFERENCE
        "The registrations for the objects in this sub-tree are
        defined below in the sub-section titled Liebert Environmental
        Statistics Group."
    ::= { lgpEnvironmental 6 }

lgpEnvPoints OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "This sub-tree is used to register Liebert environmental point
        object identifiers."
    REFERENCE
        "The registrations for the objects in this sub-tree are
        defined below in the sub-section titled Liebert Environmental
        point Group."
    ::= { lgpEnvironmental 7 }

lgpEnvUnits OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "This sub-tree is used to register Liebert environmental unit
        object identifiers."
    REFERENCE
        "The registrations for the objects in this sub-tree are
        defined below in the sub-section titled Liebert Environmental
        units Group."
    ::= { lgpEnvironmental 8 }

lgpEnvRemoteSensors OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "This sub-tree is used to register Liebert environmental remote
        sensor object identifiers."
    REFERENCE
        "The registrations for the objects in this sub-tree are
        defined below in the sub-section titled Liebert Environmental 
        Remote Sensor Group."
    ::= { lgpEnvironmental 9 }

-- =============================================================================
-- lgpEnvTemperature - Liebert Environmental Temperature Group
-- =============================================================================

lgpEnvTemperatureWellKnown OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Liebert well known temperature objects are identified by OIDs that
        reside in this sub-tree."
    ::= { lgpEnvTemperature 1 }

lgpEnvTemperatureFahrenheit OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "This sub-tree contains OIDs that are used to control and monitor
        temperature using the Fahrenheit temperature scale."
    REFERENCE
        "The registrations for the objects in this sub-tree are defined below
        in the sub-section titled Liebert Environmental Fahrenheit Temperature
        Group."
    ::= { lgpEnvTemperature 2 }

lgpEnvTemperatureCelsius OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "This sub-tree contains OIDs that are used to control and monitor
        temperature using the Celsius temperature scale."
    REFERENCE
        "The registrations for the objects in this sub-tree are defined below
        in the sub-section titled Liebert Environmental Celsius Temperature
        Group."
    ::= { lgpEnvTemperature 3 }

lgpEnvTemperatureControlMode OBJECT-TYPE
    SYNTAX      OBJECT IDENTIFIER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A reference to a temperature description object. The object
        referenced should not be accessible, but rather be used to provide
        a unique description of the temperature object that is used for
        control."
    ::= { lgpEnvTemperature 4 }

-- =============================================================================
-- lgpEnvHumidity - Liebert Environmental Humidity Group
-- =============================================================================

lgpEnvHumidityWellKnown OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Liebert well known humidity objects are defined by OIDs that reside
        in this sub-tree."
    ::= { lgpEnvHumidity 1 }

lgpEnvHumidityRelative OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "This sub-tree contains OIDs that are used to control and monitor
        relative humidity."
    REFERENCE
        "The registrations for the objects in this sub-tree are defined below
        in the sub-section titled Liebert Environmental Relative Humidity
        Group."
    ::= { lgpEnvHumidity 2 }

-- =============================================================================
-- lgpEnvState - Liebert Environmental State Group
-- =============================================================================

lgpEnvStateSystem OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        on(1), 
        off(2), 
        standby(3)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The present state of the system."
    ::= { lgpEnvState 1 }

lgpEnvStateCooling OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        on(1), 
        off(2) 
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The present state of the cooling subsystem."
    ::= { lgpEnvState 2 }

lgpEnvStateHeating OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        on(1), 
        off(2) 
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The present state of the heating subsystem."
    ::= { lgpEnvState 3 }

lgpEnvStateHumidifying OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        on(1), 
        off(2) 
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The present state of the humidifier subsystem."
    ::= { lgpEnvState 4 }

lgpEnvStateDehumidifying OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        on(1), 
        off(2) 
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The present state of the dehumidifier subsystem"
    ::= { lgpEnvState 5 }

lgpEnvStateEconoCycle OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        on(1), 
        off(2) 
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The present state of the Econ-o-cycle subsystem."
    ::= { lgpEnvState 6 }

lgpEnvStateFan OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        on(1), 
        off(2) 
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The present state of the system fan."
    ::= { lgpEnvState 7 }

lgpEnvStateGeneralAlarmOutput OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        on(1), 
        off(2) 
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The present state of the general alarm output.  This indicates if
        an alarm is active in the system."
    ::= { lgpEnvState 8 }

lgpEnvStateCoolingCapacity OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "percent"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The percentage of the cooling capacity presently in use."
    ::= { lgpEnvState 9 }

lgpEnvStateHeatingCapacity OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "percent"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The percentage of the heating capacity presently in use."
    ::= { lgpEnvState 10 }

lgpEnvStateAudibleAlarm OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        on(1), 
        off(2) 
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The present state of the audible alarm output."
    ::= { lgpEnvState 11 }

lgpEnvStateCoolingUnits OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "This sub-tree contains OIDs that are used to indicate the status
        of cooling units."
    ::= { lgpEnvState 12 }

    lgpEnvStateCoolingUnit1 OBJECT-TYPE
        SYNTAX      INTEGER 
        { 
            on(1), 
            off(2) 
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The present state of cooling unit 1."
       ::= { lgpEnvStateCoolingUnits 2 }

    lgpEnvStateCoolingUnit2 OBJECT-TYPE
        SYNTAX      INTEGER 
        { 
            on(1), 
            off(2) 
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The present state of cooling unit 2."
       ::= { lgpEnvStateCoolingUnits 3 }

    lgpEnvStateCoolingUnit3 OBJECT-TYPE
        SYNTAX      INTEGER 
        { 
            on(1), 
            off(2) 
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The present state of cooling unit 3."
       ::= { lgpEnvStateCoolingUnits 4 }

    lgpEnvStateCoolingUnit4 OBJECT-TYPE
        SYNTAX      INTEGER 
        { 
            on(1), 
            off(2) 
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The present state of cooling unit 4."
       ::= { lgpEnvStateCoolingUnits 5 }

lgpEnvStateHeatingUnits OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "This sub-tree contains OIDs that are used to indicate the status
        of heating units."
    ::= { lgpEnvState 13 }

    lgpEnvStateHeatingUnit1 OBJECT-TYPE
        SYNTAX      INTEGER 
        { 
            on(1), 
            off(2) 
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The present state of heating unit 1."
       ::= { lgpEnvStateHeatingUnits 2 }

    lgpEnvStateHeatingUnit2 OBJECT-TYPE
        SYNTAX      INTEGER 
        { 
            on(1), 
            off(2) 
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The present state of heating unit 2."
       ::= { lgpEnvStateHeatingUnits 3 }

    lgpEnvStateHeatingUnit3 OBJECT-TYPE
        SYNTAX      INTEGER 
        { 
            on(1), 
            off(2) 
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The present state of heating unit 3."
       ::= { lgpEnvStateHeatingUnits 4 }

    lgpEnvStateHeatingUnit4 OBJECT-TYPE
        SYNTAX      INTEGER 
        { 
            on(1), 
            off(2) 
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The present state of heating unit 4."
       ::= { lgpEnvStateHeatingUnits 5 }

lgpEnvStateOperatingReason OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        none(1), 
        localUser(2), 
        alarm(3), 
        schedule(4), 
        remoteUser(5), 
        externalDevice(6), 
        localDisplay(7)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The reason for the current operating state of the system."
    ::= { lgpEnvState 14 }

lgpEnvStateOperatingMode OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        auto(1), 
        manual(2)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The present operating mode of the system."
    ::= { lgpEnvState 15 }

lgpEnvStateFanCapacity OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "percent"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The percentage of the fan capacity presently in use."
    ::= { lgpEnvState 16 }

lgpEnvStateFreeCoolingCapacity OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "percent"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The percentage of the free cooling capacity presently in use."
    ::= { lgpEnvState 17 }

lgpEnvStateDehumidifyingCapacity OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "percent"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The percentage of the dehumidifying capacity presently in use."
    ::= { lgpEnvState 18 }

lgpEnvStateHumidifyingCapacity OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "percent"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The percentage of the humidifying capacity presently in use."
    ::= { lgpEnvState 19 }

lgpEnvStateFreeCooling OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        on(1), 
        off(2), 
        start(3), 
        unavailable(4) 
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The present state of the system free cooling process of heat
        exchange.  When 'off', free cooling is not in use. When 'on'
        free cooling is in use.  When 'start', free cooling is preparing
        to turn on.  When 'unavailable', the state information is
        unavailable."
    ::= { lgpEnvState 20 }

lgpEnvStateElectricHeater OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        on(1), 
        off(2) 
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The present state of the electric heaters."
    ::= { lgpEnvState 21 }

lgpEnvStateHotWater OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        on(1), 
        off(2) 
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The present state of hot water system."
    ::= { lgpEnvState 22 }

lgpEnvStateOperatingEfficiency OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "percent"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The ratio of cooling energy provided to the amount of total energy
         being used."
    ::= { lgpEnvState 23 }

lgpEnvComponentStateTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF LgpEnvComponentStateEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains a list of the units components that have
        a state associated with them.
        The table contains zero, one, or more rows, depending
        upon the number of components associated with the unit.
        The NMS cannot create or delete rows in the table. The rows are
        created by the agent based upon the capabilities of the units
        being monitored."
    ::= { lgpEnvState 50 }

    lgpEnvComponentStateEntry OBJECT-TYPE
        SYNTAX      LgpEnvComponentStateEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "This entry defines the attributes to be populated in the
            various columns of the 'lgpEnvComponentStateTable'."
        INDEX       
        { 
            lgpEnvComponentStateIndex
        }
        ::= { lgpEnvComponentStateTable 1 }

    LgpEnvComponentStateEntry ::= SEQUENCE 
    {
        lgpEnvComponentStateIndex                   Unsigned32,
        lgpEnvComponentStateDescr                   OBJECT IDENTIFIER,
        lgpEnvComponentState                        INTEGER
    }

    lgpEnvComponentStateIndex OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "This is the index indicating the nth element of the table."
        ::= { lgpEnvComponentStateEntry 1 }

    lgpEnvComponentStateDescr OBJECT-TYPE
        SYNTAX      OBJECT IDENTIFIER
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "A reference to a component description object. The object
            referenced should not be accessible, but rather be used
            to provide a unique description of the component being 
            described in the row of the table."
        ::= { lgpEnvComponentStateEntry 2 }

    lgpEnvComponentState OBJECT-TYPE
        SYNTAX      INTEGER
        {
            not-specified(0),
            on(1),
            off(2)
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "not-specified
                The state of the component is unknown.
             on
                The component is on.
             off
                The component is off."
        ::= { lgpEnvComponentStateEntry 3 }

lgpEnvValveTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF LgpEnvValveEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains a list of the unit valves that have
        information associated with them.
        The table contains zero, one, or more rows, depending
        upon the number of valves associated with the unit.
        The NMS cannot create or delete rows in the table. The rows are
        created by the agent based upon the capabilities of the units
        being monitored."
    ::= { lgpEnvState 70 }

    lgpEnvValveEntry OBJECT-TYPE
        SYNTAX      LgpEnvValveEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "This entry defines the attributes to be populated in the
            various columns of the 'lgpEnvValveTable'."
        INDEX       
        { 
            lgpEnvValveIndex
        }
        ::= { lgpEnvValveTable 1 }

    LgpEnvValveEntry ::= SEQUENCE 
    {
        lgpEnvValveIndex                   Unsigned32,
        lgpEnvValveDescr                   OBJECT IDENTIFIER,
        lgpEnvValveState                   INTEGER,
        lgpEnvValvePositionTenths          Unsigned32
    }

    lgpEnvValveIndex OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "This is the index indicating the nth element of the table."
        ::= { lgpEnvValveEntry 1 }

    lgpEnvValveDescr OBJECT-TYPE
        SYNTAX      OBJECT IDENTIFIER
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "A reference to a valve description object. The object
            referenced should not be accessible, but rather be used
            to provide a unique description of the valve being 
            described in the row of the table."
        ::= { lgpEnvValveEntry 2 }

    lgpEnvValveState OBJECT-TYPE
        SYNTAX      INTEGER
        {
            not-specified(0),
            open(1),
            closed(2)
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "not-specified
                The state of the component is unknown.
             open
                The valve is open.
             off
                The valve is closed."
        ::= { lgpEnvValveEntry 3 }

    lgpEnvValvePositionTenths OBJECT-TYPE
        SYNTAX      Unsigned32
        UNITS       ".1 percent"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "This gives a value describing the position of the valve."
        ::= { lgpEnvValveEntry 20 }

-- =============================================================================
-- lgpEnvConfig - Liebert Environmental Configuration Group
-- =============================================================================

lgpEnvConfigReheatLockout OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        lockedOut(1), 
        notLockedOut(2) 
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "If locked-out the reheats will not operate even if controller calls
        for its operation."
    ::= { lgpEnvConfig 1 }

lgpEnvConfigHumLockout OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        lockedOut(1), 
        notLockedOut(2) 
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "If locked-out the humidifier will not operate even if controller
        calls for its operation."
    ::= { lgpEnvConfig 2 }

lgpEnvConfigRestartDelay OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "When utility power is disrupted, this is the delay interval to wait
        before restarting the system after the utility power is restored.
        A Restart Delay of zero denotes a manual restart, the unit will NOT
        automatically restart."
    ::= { lgpEnvConfig 4 }

lgpEnvConfigRemoteShutdown OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        disabled(1), 
        enabled(2) 
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "When in the disabled state, the remote shutdown feature should
        be locked out.  The enabled state is self-describing."
    ::= { lgpEnvConfig 7 }

lgpEnvConfigCoolingServiceInterval OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "hours"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The amount of time, in hours, between scheduled maintenance
        of the cooling system.  When the cooling service timer reaches
        this value an lgpConditionServiceCooling will be activated.
        Once service has been completed the cooling service timer
        should be reset to 0."
    ::= { lgpEnvConfig 8 }

lgpEnvConfigHumidifierServiceInterval OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "hours"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The amount of time, in hours, between scheduled maintenance
        of the humidifier.  When the humidifier service timer reaches
        this value an lgpConditionServiceHumidifier will be activated.
        Once service has been completed humidifier service timer
        should be reset to 0."
    ::= { lgpEnvConfig 9 }

lgpEnvConfigFilterServiceInterval OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "hours"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The amount of time, in hours, between scheduled maintenance
        of the system filter.  When the filter service timer reaches this
        value an lgpConditionChangeFilter will be activated.  Once service
        has been completed the filter service timer should be reset to 0."
    ::= { lgpEnvConfig 10 }

lgpEnvConfigSleepModeDeadbandRangeDegC OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       ".1 degrees Celsius"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The allowable deviation above and below the temperature set point used
         to create a no control region, a dead-band, where  heating and
         cooling  control are disabled.  This dead-band is applied only
         when the system's sleep mode function is in operation."
    ::= { lgpEnvConfig 11 }

lgpEnvConfigSleepModeDeadbandRangeDegF OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       ".1 degrees Fahrenheit"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The allowable deviation above and below the temperature set point used
         to create a no control region, a dead-band, where  heating and
         cooling  control are disabled.  This dead-band is applied only
         when the system's sleep mode function is in operation."
    ::= { lgpEnvConfig 12 }

lgpEnvConfigSupplyTempLowLimitDegF OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "degrees Fahrenheit"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The minimum allowable supply temperature."
    ::= { lgpEnvConfig 13 }

lgpEnvConfigSupplyTempLowLimitDegC OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "degrees Celsius"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The minimum allowable supply temperature."
    ::= { lgpEnvConfig 14 }

lgpEnvConfigTemperatureIntegTime OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "minutes"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value used as the integration factor in the proportional
        integral derivative (PID) temperature calculation."
    ::= { lgpEnvConfig 15 }

lgpEnvConfigLocalTemperatureUnit OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        degC(1), 
        degF(2) 
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The local temperature unit of the system."
    ::= { lgpEnvConfig 16 }

lgpEnvConfigSleepMode OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        enabled(1), 
        disabled(2), 
        auto(3)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The configured mode of the device's sleep function.  If 'enabled',
        the device will sleep, or not operate, for each 'lgpEnvSleepDay' that
        is enabled and also during the periods defined in the
        'lgpEnvSleepTimeTable' each day.  If 'disabled', the device will
        operate continually and not sleep at all.  If 'auto', the device will
        sleep, or not operate, for each 'lgpEnvSleepDay' that is enabled and
        also during the periods defined in the 'lgpEnvSleepTimeTable' each
        day unless the environmental conditions fall outside the desired
        operation ranges."
    ::= { lgpEnvConfig 17 }

lgpEnvConfigHumidityIntegTime OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "minutes"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value used as the integration factor in the proportional
        integral derivative (PID) humidity calculation."
    ::= { lgpEnvConfig 18 }

lgpEnvConfigFreecoolingDeltaDegF OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "degrees Fahrenheit"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The minimum temperature differential between the control
        temperature measurement and the coolant required to utilize
        free-cooling."
    ::= { lgpEnvConfig 19 }

lgpEnvConfigFreecoolingDeltaDegC OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "degrees Celsius"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The minimum temperature differential between the control
        temperature measurement and the coolant required to utilize
        free-cooling."
    ::= { lgpEnvConfig 20 }

lgpEnvConfigSupplyTempLowLimit OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        disabled(1), 
        enabled(2) 
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The system configuration parameter to enable or disable the supply
        air low  temperature limit."
    ::= { lgpEnvConfig 21 }

lgpEnvConfigSensorEventsStandard OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        disabled(1), 
        enabled(2) 
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The system configuration parameter to enable or disable the standard
        sensor events."
    ::= { lgpEnvConfig 22 }

lgpEnvConfigSensorEvents1 OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        disabled(1), 
        enabled(2) 
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The system configuration parameter to enable or disable sensor 1 events."
    ::= { lgpEnvConfig 23 }

lgpEnvConfigSleepModeDeadbandRange OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        disabled(1), 
        enabled(2) 
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The system configuration parameter to enable or disable the use of
        the sleep interval dead-band range in the sleep mode temperature
        calculations and control algorithm."
    ::= { lgpEnvConfig 24 }

lgpEnvConfigAutoConfiguration OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        disabled(1), 
        enabled(2) 
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The system configuration parameter to enable or disable the auto
        configuration feature.  This feature configures temperature and
        humidity control parameters."
    ::= { lgpEnvConfig 25 }

lgpEnvConfigDeltaGlycolType OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        disabled(1), 
        contact(2), 
        value(3) 
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The system configuration parameter that specifies how the system
        will determine if there is enough capacity to initiate free
        cooling. If 'disabled', the system will use the valve temperature
        to initiate free cooling.  If 'contact', a input to the system
        will initiate free cooling.  If 'valve', the system compares the
        room and glycol temperature differential with the valve temperature
        to initiate free cooling.  If the temperature differential is
        greater than or equal to the valve temperature, free cooling will
        be initiated."

    ::= { lgpEnvConfig 26 }

lgpEnvConfigChillWaterControl OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        disabled(1), 
        enabled(2) 
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The system configuration parameter to enable or disable the minimum
        chill water temperature control."

    ::= { lgpEnvConfig 27 }

lgpEnvConfigInfaredFlushRate OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "percent"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The Infrared humidifier pan overfill rate.  This parameter configures
        the amount of water that flows into the humidifier pan when the
        'humidifier is in operation."

    ::= { lgpEnvConfig 28 }

lgpEnvConfigHumidityControl OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        relative(1), 
        compensated(2),     
        predictive(3) 
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The present configured state of the automatic humidity compensation
        algorithm."
    ::= { lgpEnvConfig 29 }

lgpEnvConfigCompressorLockout OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        lockedOut(1), 
        notLockedOut(2) 
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The system as locked out the compressor(s).  If locked-out, the
        compressor(s) will not operate even if the controller calls for their
        operation."

    ::= { lgpEnvConfig 30 }

lgpEnvConfigReheatAndHumidifierLockout OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        lockedOut(1), 
        notLockedOut(2) 
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The system as locked out the compressor(s).  If locked-out, the
        electrical reheats and humidifier will not operate even if the
        controller calls for their operation."

    ::= { lgpEnvConfig 31 }

-- -----------------------------------------------------------------------------
-- Operational Time Table
-- -----------------------------------------------------------------------------

lgpEnvOperationalTimeTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF LgpEnvOperationalTimeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A list of environmental operational time ranges for a given
        environmental unit.  The entries in this table may be duplicated from
        values in the 'lgpEnvStatistics' group.

        This table contains zero, one, or many rows, depending upon the number
        of 'lgpEnvOperationTimePoint' and 'lgpEnvOperationTimeSubID' available
        in the table.

        The NMS cannot create or delete rows from the table.
        The rows are created by the agent based upon the capabilities of
        the managed device."
    ::= { lgpEnvConfig 32 }

    lgpEnvOperationalTimeEntry OBJECT-TYPE
        SYNTAX      LgpEnvOperationalTimeEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "This entry defines the contents of the columns for the table
            'lgpEnvOperationalTimeTable'."
        REFERENCE
            "The 'lgpEnvOperationTimePoint' in this table corresponds to what
            the operation time applies to."
        INDEX       { lgpEnvOperationTimeIndex }
        ::= { lgpEnvOperationalTimeTable 1 }

    LgpEnvOperationalTimeEntry ::= SEQUENCE 
    {
        lgpEnvOperationTimeIndex            Unsigned32,
        lgpEnvOperationTimePoint            OBJECT IDENTIFIER,
        lgpEnvOperationTimeSubID            Integer32,
        lgpEnvOperationTimeUnit             OBJECT IDENTIFIER,
        lgpEnvOperationTimeValue            Integer32,
        lgpEnvOperationTimeHighWarning      Integer32
    }

    lgpEnvOperationTimeIndex OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "This is the index indicating the nth element of the table."
        ::= { lgpEnvOperationalTimeEntry 1 }

    lgpEnvOperationTimePoint OBJECT-TYPE
        SYNTAX      OBJECT IDENTIFIER
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "An OID representing a well known operation point.
            These object identifiers can indicate a point, location, or mode
            of an operation for which a measurement is recorded.  The OID's
            name usually implies a location of the measurement point such as
            'fan', 'compressor', etc."
        REFERENCE
            "The object identifiers  in this column can be found in the sub-tree
            'lgpEnvWellKnownPoints' and correspond to the entry in the table
            'lgpEnvOperationalTimeTable'."
        ::= { lgpEnvOperationalTimeEntry 2 }

    lgpEnvOperationTimeSubID OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "This is a sub identifier for the 'lgpEnvOperationPoint'.
            It indicates the instance number of the well known operation
            point.  For example, a system could have two fans installed.
            This variable would identify fan 1 with a lgpEnvOperationSubID
            equal to 1 and fan 2 with a lgpEnvOperationSubID equal to 2."
        ::= { lgpEnvOperationalTimeEntry 3 }

    lgpEnvOperationTimeUnit OBJECT-TYPE
        SYNTAX      OBJECT IDENTIFIER
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "An OID representing a well known operation time unit type.
            These object identifiers indicate the units of the operation time.
            The OID's name usually implies a measurement type such as
            'lgpEnvHours', etc."
        REFERENCE
            "The object identifiers  in this column can be found in the sub-tree
            'lgpEnvWellKnownUnits' and correspond to the
            entry in the table lgpEnvOperationalTimeTable."
        ::= { lgpEnvOperationalTimeEntry 4 }

    lgpEnvOperationTimeValue OBJECT-TYPE
        SYNTAX      Integer32
        UNITS       "hours"
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "The actual operation time value of the
            'lgpEnvOperationTimePoint'.
            If multiple operation times are available for a
            'lgpEnvOperationTimePoint' the 'lgpEnvOperationTimeSubID' will
            differentiate between them."
        ::= { lgpEnvOperationalTimeEntry 5 }

    lgpEnvOperationTimeHighWarning OBJECT-TYPE
        SYNTAX      Integer32
        UNITS       "hours"
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "The high warning time of the operation designated by the
            'lgpEnvOperationTimePoint'.  If operation times are available at
            a single 'lgpEnvOperationTimePoint' the 'lgpEnvOperationTimeSubID'
            will differentiate between them."
        ::= { lgpEnvOperationalTimeEntry 6 }

lgpEnvConfigTempControlAlgorithm OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        pi(1), 
        pid(2), 
        intelligent(3), 
        proportional(4) 
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Selects the algorithm for controlling temperature."
    ::= { lgpEnvConfig 33 }

lgpEnvConfigFanSpeedMode OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        manual(1), 
        auto(2) 
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Changes the function of the fan speed output.  If auto, then the fan
        speed is modulated.  If manual, the fan speed output follows
        lgpEnvConfigFanSpeedCapacity."
    ::= { lgpEnvConfig 34 }

lgpEnvConfigFanSpeedCapacity OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "percent"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Sets the fan speed output if lgpEnvConfigFanSpeedMode is set to
        'manual'.  Typical values range from 0 to 100% (actual valid ranges may
        differ from unit to unit)."
    ::= { lgpEnvConfig 35 }

lgpEnvConfigBmsResetTimer OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "minutes"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The current count-down time for a BMS to continue controlling the fan
        speed.  If this value reaches 0, then the condition
        lgpConditionBmsResetTimerExpired will be generated.  If a BMS wants to
        continue controlling the fan speed, it must reset this timer.  Typical
        values range from 0 to 120 minutes (actual valid ranges may differ from
        unit to unit)."
    ::= { lgpEnvConfig 36 }

lgpEnvConfigDisableSensorOffsetDegC OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "degrees Celsius"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "If any of the enclosure temperature sensors
        (lgpEnvEnclosureTemperatureSensors) are outside the average reading by
        this amount, that sensor's readings will not be used."
    ::= { lgpEnvConfig 37 }

lgpEnvConfigDisableSensorOffsetDegF OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "degrees Fahrenheit"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "If any of the enclosure temperature sensors
        (lgpEnvEnclosureTemperatureSensors) are outside the average reading by
        this amount, that sensor's readings will not be used."
    ::= { lgpEnvConfig 38 }

lgpEnvConfigCabinetSensorAlarms OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        disabled(0), 
        enabled(1) 
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Enable or Disable Cabinet Sensor Alarms."
    ::= { lgpEnvConfig 39 }

lgpEnvConfigAirTemperatureControlSensor OBJECT-TYPE
    SYNTAX      INTEGER
    {
        supply(1),
        remote(2),
        return(3)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Sensor from which air temperature measurements will be used for
        cooling and heating control."
    ::= { lgpEnvConfig 42 }

lgpEnvConfigFanSpeedControlSensor OBJECT-TYPE
    SYNTAX      INTEGER 
    { 
        supply(1),
        remote(2),
        return(3)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Sensor from which air temperature measurements will be used for fan
        speed control."
    ::= { lgpEnvConfig 43 }

lgpEnvConfigMinFanSpeed OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "percent"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Sets the minimum fan speed output if lgpEnvConfigFanSpeedMode is set
         to 'Auto'."
    ::= { lgpEnvConfig 44 }

lgpEnvConfigMaxFanSpeed OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "percent"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Sets the maximum fan speed output if lgpEnvConfigFanSpeedMode is set
         to 'Auto'."
    ::= { lgpEnvConfig 45 }

lgpEnvConfigFanSpeedPropBandDegC OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "degrees Celsius"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Temperature control band above the temperature set point calculated
         for proportional fan speed control.  If measured air temperature is
         within this band, fan speed operations are proportionally controlled."
    ::= { lgpEnvConfig 46 }

lgpEnvConfigFanSpeedPropBandDegF OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "degrees Fahrenheit"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Temperature control band above the temperature set point calculated
         for proportional fan speed control.  If measured air temperature is
         within this band, fan speed operations are proportionally controlled."
    ::= { lgpEnvConfig 47 }

-- =============================================================================
-- lgpEnvControl - Liebert Environmental Control Group
-- =============================================================================

lgpEnvControlShutdownAfterDelay OBJECT-TYPE
    SYNTAX      Integer32 (-1..2147483647)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Setting this object will shutdown (i.e., turn off)
        the system after the indicated number of seconds. Setting
        this object to 0 will cause the shutdown to occur
        immediately.  Setting this object to -1 will abort the
        countdown.  If the system is already in the desired
        state at the time the countdown reaches 0, then
        nothing will happen.  When read, lgpEnvControlShutdownAfterDelay
        will return the number of seconds remaining until shutdown,
        or -1 if no shutdown countdown is in effect.  On some systems,
        if the agent is restarted while a shutdown countdown is in effect,
        the countdown may be aborted.  Sets to this object
        override any lgpEnvControlShutdownAfterDelay already in effect."
    ::= { lgpEnvControl 1 }

lgpEnvControlStartupAfterDelay OBJECT-TYPE
    SYNTAX      Integer32 (-1..2147483647)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Setting this object will start the system after the
        indicated number of seconds.  Setting this object to 0 will
        cause the startup to occur immediately.  Setting this
        object to -1 will abort the countdown.  If the system
        is already on at the time the countdown reaches 0,
        then nothing will happen.  Sets to this object
        override the effect of any lgpEnvControlStartupAfterDelay
        countdown in progress.  When read, lgpEnvControlStartupAfterDelay
        will return the number of seconds until startup, or -1 if no
        startup countdown is in effect.  On some systems, if the agent
        is restarted while a startup countdown is in effect, the
        countdown is aborted."
    ::= { lgpEnvControl 2 }

lgpEnvSleepIntervalTimeTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF LgpEnvSleepIntervalTimeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A sleep time interval table containing a list of the start and stop
        times to be used to take a device online or offline.

        The NMS cannot create or delete rows from the table.
        The rows are created by the agent based upon the capabilities of
        the managed device."
    ::= { lgpEnvControl 3 }

    lgpEnvSleepIntervalTimeEntry OBJECT-TYPE
        SYNTAX      LgpEnvSleepIntervalTimeEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "This entry defines the contents of the columns for the table
            'lgpEnvSleepIntervalTimeTable'."
        INDEX       { lgpEnvSleepTimeIndex }
        ::= { lgpEnvSleepIntervalTimeTable 1 }

    LgpEnvSleepIntervalTimeEntry ::= SEQUENCE 
    {
            lgpEnvSleepTimeIndex            Unsigned32,
            lgpEnvSleepTimeSubID            Integer32,
            lgpEnvSleepTimeStartHour        Integer32,
            lgpEnvSleepTimeStartMinute      Integer32,
            lgpEnvSleepTimeStopHour         Integer32,
            lgpEnvSleepTimeStopMinute       Integer32
    }

    lgpEnvSleepTimeIndex OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "This is the index indicating the row of the table
             'lgpEnvSleepIntervalTimeTable'."
        ::= { lgpEnvSleepIntervalTimeEntry 1 }

    lgpEnvSleepTimeSubID OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "This is a sub identifier for each 'lgpEnvSleepIntervalTimeEntry'.
            It indicates the instance number of the
            'lgpEnvSleepIntervalTimeEntry'.
            For example, a system could have two sleep intervals and the first
            interval's sub ID would be 1 and the second interval's sub ID
            would be 2."
        ::= { lgpEnvSleepIntervalTimeEntry 2 }

    lgpEnvSleepTimeStartHour OBJECT-TYPE
        SYNTAX      Integer32(0..23)
        UNITS       "hour"
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "This is the hours digit of the time when the system will be put
            online."
        ::= { lgpEnvSleepIntervalTimeEntry 3 }

    lgpEnvSleepTimeStartMinute OBJECT-TYPE
        SYNTAX      Integer32(0..59)
        UNITS       "minute"
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "This is the minutes digit of the time when the system will be put
            online."
        ::= { lgpEnvSleepIntervalTimeEntry 4 }

    lgpEnvSleepTimeStopHour OBJECT-TYPE
        SYNTAX      Integer32(0..23)
        UNITS       "hour"
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "This is the hours digit containing the time when the system will
            be taken offline."
        ::= { lgpEnvSleepIntervalTimeEntry 5 }

    lgpEnvSleepTimeStopMinute OBJECT-TYPE
        SYNTAX      Integer32(0..59)
        UNITS       "minute"
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "This is the minutes digit containing the time when the system
            will be taken offline."
        ::= { lgpEnvSleepIntervalTimeEntry 6 }

lgpEnvSleepDayTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF LgpEnvSleepDayEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A sleep table containing a list of the days of the week the system
        will be offline.

        The NMS cannot create or delete rows from the table.
        The rows are created by the agent based upon the capabilities of
        the managed device."
    ::= { lgpEnvControl 4 }

    lgpEnvSleepDayEntry OBJECT-TYPE
        SYNTAX      LgpEnvSleepDayEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "This entry defines the contents of the columns for the table
            'lgpEnvSleepDayTable'."
        INDEX       { lgpEnvSleepDayIndex }
        ::= { lgpEnvSleepDayTable 1 }

    LgpEnvSleepDayEntry ::= SEQUENCE 
    {
            lgpEnvSleepDayIndex             Unsigned32,
            lgpEnvSleepDay                  INTEGER,
            lgpEnvSleepAllDayEnabled        INTEGER
    }

    lgpEnvSleepDayIndex OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "This is the index indicating the row of the table
             'lgpEnvSleepDayTable'."
        ::= { lgpEnvSleepDayEntry 1 }

    lgpEnvSleepDay OBJECT-TYPE
        SYNTAX      INTEGER 
        {
            sunday(1), 
            monday(2), 
            tuesday(3), 
            wednesday(4),
            thursday(5), 
            friday(6), 
            saturday(7)
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "This is a sub identifier for the day of the week within
            'lgpEnvSleepDayTable'."
        ::= { lgpEnvSleepDayEntry 2 }

    lgpEnvSleepAllDayEnabled OBJECT-TYPE
        SYNTAX      INTEGER 
        { 
            yes(1), 
            no(2)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "The all day sleep functionality has been enabled for the
            corresponding 'lgpEnvSleepDay' in the 'lgpEnvSleepDayTable'."
        ::= { lgpEnvSleepDayEntry 3 }

-- =============================================================================
-- lgpEnvStatistics - Liebert Environmental Statistics Group
-- =============================================================================

lgpEnvStatisticsComp1RunHr OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "hours"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Accumulated run hours of compressor 1.  This value may be duplicated
        in the 'lgpEnvOperationalTimeTable'."
    ::= { lgpEnvStatistics 1 }

lgpEnvStatisticsComp2RunHr OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "hours"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Accumulated run hours of compressor 2.  This value may be duplicated
        in the 'lgpEnvOperationalTimeTable'."
    ::= { lgpEnvStatistics 2 }

lgpEnvStatisticsFanRunHr OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        " Accumulated run hours of the main fan.  This value may be duplicated
        in the 'lgpEnvOperationalTimeTable'."
    ::= { lgpEnvStatistics 3 }

lgpEnvStatisticsHumRunHr OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        " Accumulated run hours of the humidifier.  This value may be
        duplicated in the 'lgpEnvOperationalTimeTable'."
    ::= { lgpEnvStatistics 4 }

lgpEnvStatisticsReheat1RunHr OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "hours"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Accumulated run hours of reheat element 1.  This value may be
        duplicated in the 'lgpEnvOperationalTimeTable'."
    ::= { lgpEnvStatistics 7 }

lgpEnvStatisticsReheat2RunHr OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "hours"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Accumulated run hours of reheat element 2.  This value may be
        duplicated in the 'lgpEnvOperationalTimeTable'."
    ::= { lgpEnvStatistics 8 }

lgpEnvStatisticsReheat3RunHr OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "hours"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Accumulated run hours of reheat element 3.  This value may be
        duplicated in the 'lgpEnvOperationalTimeTable'."
    ::= { lgpEnvStatistics 9 }

lgpEnvStatisticsCoolingModeHrs OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "hours"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Accumulated run hours while lgpEnvStateCooling is on(1).
        This value may be duplicated in the 'lgpEnvOperationalTimeTable'."
    ::= { lgpEnvStatistics 10 }

lgpEnvStatisticsHeatingModeHrs OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "hours"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Accumulated run hours while lgpEnvStateHeating is on(1).
        This value may be duplicated in the 'lgpEnvOperationalTimeTable'."
    ::= { lgpEnvStatistics 11 }

lgpEnvStatisticsHumidifyModeHrs OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "hours"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Accumulated run hours of the humidifying process of the system.
        This value may be duplicated in the 'lgpEnvOperationalTimeTable'."
    ::= { lgpEnvStatistics 12 }

lgpEnvStatisticsDehumidifyModeHrs OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "hours"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Accumulated run hours of the dehumidifying process of the system.
        This value may be duplicated in the 'lgpEnvOperationalTimeTable'."
    ::= { lgpEnvStatistics 13 }

lgpEnvStatisticsHotGasRunHr OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "hours"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Accumulated run hours of the hot gas system.  This value may be
        duplicated in the 'lgpEnvOperationalTimeTable'."
    ::= { lgpEnvStatistics 14 }

lgpEnvStatisticsHotWaterRunHr OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "hours"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Accumulated run hours of the hot water system.  This value may be
        duplicated in the 'lgpEnvOperationalTimeTable'."
    ::= { lgpEnvStatistics 15 }

lgpEnvStatisticsFreeCoolRunHr OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "hours"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Accumulated run hours of the free cooling process.  This value may
        be duplicated in the 'lgpEnvOperationalTimeTable'."
    ::= { lgpEnvStatistics 16 }

lgpEnvStatisticsComp3RunHr OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
     " Accumulated run hours of compressor 3."
    ::= { lgpEnvStatistics 17 }

lgpEnvStatisticsComp4RunHr OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
     " Accumulated run hours of compressor 4."
    ::= { lgpEnvStatistics 18 }

-- =============================================================================
-- lgpEnvWellKnownPoints - Liebert "well-known" points
-- =============================================================================

lgpEnvWellKnownPoints OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "This sub-tree registers well known Liebert Environmental Points.
         The object identifier names usually encompass a process, or location,
         where measurements are recorded or where values are applied."
        ::= { lgpEnvPoints 1  }

    lgpEnvFanPoint      OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "This identifier represents a well known fan measurement point."
        ::= { lgpEnvWellKnownPoints 1 }

    lgpEnvCompressorPoint      OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "This identifier represents a well known compressor measurement
            point."
        ::= { lgpEnvWellKnownPoints 2 }

    lgpEnvElectricHeaterPoint      OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "This identifier represents a well known electric heater measurement
            point."
        ::= { lgpEnvWellKnownPoints 3 }

    lgpEnvChilledWaterPoint      OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "This identifier represents a well known chilled water measurement
            point."
        ::= { lgpEnvWellKnownPoints 4 }

    lgpEnvHumidifierPoint      OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "This identifier represents a well known humidifier measurement
            point."
        ::= { lgpEnvWellKnownPoints 5 }

    lgpEnvDehumidifierPoint      OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "This identifier represents a well known dehumidifier measurement
            point."
        ::= { lgpEnvWellKnownPoints 6 }

    lgpEnvFreeCoolingPoint      OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "This identifier represents a well known free-cooling measurement
            process."
        ::= { lgpEnvWellKnownPoints 7 }

    lgpEnvHotWaterPoint      OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "This identifier represents a well known hot water measurement
            point."
        ::= { lgpEnvWellKnownPoints 8 }

    lgpEnvHotGasPoint      OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "This identifier represents a well known hot gas measurement
            point."
        ::= { lgpEnvWellKnownPoints 9 }

    lgpEnvBatteryCabinetPoint OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "This identifier represents a well known cabinet point.
            To determine the cabinet being described in a multi-cabinet system, 
            this point implements two additional indexes. The first index 
            describes the module being supplied with battery power. The second 
            index identifies the number of the battery cabinet, which is 
            typically a sequential number.

            Example: lgpPwrMeasBatteryCabinet.2.4

            'lgpEnvBatteryCabinetPoint' = Point is a battery cabinet.
                                   '.2' = Cabinet is in the second module.
                                   '.4' = Cabinet number 4"
        ::= { lgpEnvWellKnownPoints 10 }

    lgpEnvPumpPoints      OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "This sub-tree identifies well-known pumps in the system."
        ::= { lgpEnvWellKnownPoints 11 }

        lgpEnvPump1Point      OBJECT-IDENTITY
            STATUS      current
            DESCRIPTION
                "This identifier represents pump 1."
            ::= { lgpEnvPumpPoints 1 }

        lgpEnvPump2Point      OBJECT-IDENTITY
            STATUS      current
            DESCRIPTION
                "This identifier represents pump 2."
            ::= { lgpEnvPumpPoints 2 }

    lgpEnvCompressorPoints      OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "This sub-tree identifies well-known compressors in the system."
        ::= { lgpEnvWellKnownPoints 12 }

        lgpEnvCompressor1Point      OBJECT-IDENTITY
            STATUS      current
            DESCRIPTION
                "This identifier represents compressor 1."
            ::= { lgpEnvCompressorPoints 1 }

            lgpEnvCompressor1APoint      OBJECT-IDENTITY
                STATUS      current
                DESCRIPTION
                  "This identifier represents compressor 1A."
                ::= { lgpEnvCompressor1Point 1 }

            lgpEnvCompressor1BPoint      OBJECT-IDENTITY
                STATUS      current
                DESCRIPTION
                    "This identifier represents compressor 1B."
                ::= { lgpEnvCompressor1Point 2 }

        lgpEnvCompressor2Point      OBJECT-IDENTITY
            STATUS      current
            DESCRIPTION
                "This identifier represents compressor 2."
            ::= { lgpEnvCompressorPoints 2 }

            lgpEnvCompressor2APoint      OBJECT-IDENTITY
                STATUS      current
                DESCRIPTION
                    "This identifier represents compressor 2A."
                ::= { lgpEnvCompressor2Point 1 }

            lgpEnvCompressor2BPoint      OBJECT-IDENTITY
                STATUS      current
                DESCRIPTION
                    "This identifier represents compressor 2B."
                ::= { lgpEnvCompressor2Point 2 }

    lgpEnvValvePoints      OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "This sub-tree identifies well-known valves in the system."
        ::= { lgpEnvWellKnownPoints 13 }

        lgpEnvHotGasValve1Point      OBJECT-IDENTITY
            STATUS      current
            DESCRIPTION
                "This identifier represents hot gas valve 1."
            ::= { lgpEnvValvePoints 1 }

        lgpEnvHotGasValve2Point      OBJECT-IDENTITY
            STATUS      current
            DESCRIPTION
                "This identifier represents hot gas valve 2."
            ::= { lgpEnvValvePoints 2 }

    lgpEnvRemoteSensorStatisticPoints      OBJECT-IDENTITY
       STATUS      current
       DESCRIPTION
           "This sub-tree identifies well-known remote sensor statistics in the
            system."
       ::= { lgpEnvWellKnownPoints 14 }

        lgpEnvRemoteSensorMinimumPoint      OBJECT-IDENTITY
            STATUS      current
            DESCRIPTION
                "This identifier represents the minimum value for remote sensor
                 readings."
            ::= { lgpEnvRemoteSensorStatisticPoints 1 }

        lgpEnvRemoteSensorMaximumPoint      OBJECT-IDENTITY
            STATUS      current
            DESCRIPTION
                "This identifier represents the maximum value for remote sensor
                 readings."
            ::= { lgpEnvRemoteSensorStatisticPoints 2 }

        lgpEnvRemoteSensorAveragePoint      OBJECT-IDENTITY
            STATUS      current
            DESCRIPTION
                "This identifier represents the average value for remote sensor
                 readings."
            ::= { lgpEnvRemoteSensorStatisticPoints 3 }

    -- =============================================================================
    -- lgpEnvWellKnownUnits - Liebert "well-known" units
    -- =============================================================================

    lgpEnvWellKnownUnits OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "This sub-tree registers well known Liebert Environmental Units.
             The object identifier names usually encompass a process, or location,
             where measurements are recorded or where values are applied."
            ::= { lgpEnvUnits 1  }

        lgpEnvHours      OBJECT-IDENTITY
            STATUS      current
            DESCRIPTION
                "This identifier represents well known time unit of hours."
            ::= { lgpEnvWellKnownUnits 1 }

    -- =============================================================================
    -- lgpEnvTemperatureMeasurements - Liebert "well-known" temperature objects
    -- =============================================================================

    lgpEnvControlTemperature      OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "Temperature measurement used as control feedback."
        ::= { lgpEnvTemperatureWellKnown 1 }

    lgpEnvReturnAirTemperature    OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
        "Temperature measurement of return air."
    ::= { lgpEnvTemperatureWellKnown 2 }

lgpEnvSupplyAirTemperature    OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Temperature measurement of supply air."
    ::= { lgpEnvTemperatureWellKnown 3 }

lgpAmbientTemperature    OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Ambient temperature measurement."
    ::= { lgpEnvTemperatureWellKnown 4 }

lgpInverterTemperature    OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Temperature measurement of the inverter."
    ::= { lgpEnvTemperatureWellKnown 5 }

lgpBatteryTempterature    OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Temperature measurement of the battery."
    ::= { lgpEnvTemperatureWellKnown 6 }

lgpAcDcConverterTemperature    OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Temperature measurement of the AC-to-DC Converter."
    ::= { lgpEnvTemperatureWellKnown 7 }

lgpPfcTemperature    OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Temperature measurement of the power factor correction circuitry."
    ::= { lgpEnvTemperatureWellKnown 8 }

lgpTransformerTemperature    OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Temperature measurement of the transformer."
    ::= { lgpEnvTemperatureWellKnown 9 }

lgpLocalTemperature    OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Temperature measurement of local temperature sensor."
    ::= { lgpEnvTemperatureWellKnown 10 }

    lgpLocal1Temperature    OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "Temperature and humidity measurements of Local Sensor 1."
        ::= { lgpLocalTemperature 1 }

    lgpLocal2Temperature    OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "Temperature and humidity measurements of Local Sensor 2."
        ::= { lgpLocalTemperature 2 }

    lgpLocal3Temperature    OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "Temperature and humidity measurements of Local Sensor 3."
        ::= { lgpLocalTemperature 3 }

lgpDigitalScrollCompressorTemperature    OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Temperature and humidity measurements of a digital Scroll Compressor."
    ::= { lgpEnvTemperatureWellKnown 11 }

    lgpDigitalScrollCompressor1Temperature    OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "Temperature and humidity measurements of a digital Scroll
            Compressor 1."
        ::= { lgpDigitalScrollCompressorTemperature 1 }

    lgpDigitalScrollCompressor2Temperature    OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "Temperature and humidity measurements of a digital Scroll
            Compressor 2."
        ::= { lgpDigitalScrollCompressorTemperature 2 }

lgpChillWaterTemperature    OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Temperature measurements of a chill water system."
    ::= { lgpEnvTemperatureWellKnown 12 }

lgpCoolantTemperature    OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Temperature measurements of an environmental system's coolant."
    ::= { lgpEnvTemperatureWellKnown 13 }

lgpEnvEnclosureTemperatureSensors OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Enclosure temperature sensors"
    ::= { lgpEnvTemperatureWellKnown 14 }

    lgpEnvEnclosureTemperatureSensor1 OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
                "Enclosure temperature sensor 1"
        ::= { lgpEnvEnclosureTemperatureSensors 1 }

    lgpEnvEnclosureTemperatureSensor2 OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
                "Enclosure temperature sensor 2"
        ::= { lgpEnvEnclosureTemperatureSensors 2 }

    lgpEnvEnclosureTemperatureSensor3 OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
                "Enclosure temperature sensor 3"
        ::= { lgpEnvEnclosureTemperatureSensors 3 }

    lgpEnvEnclosureTemperatureSensor4 OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
                "Enclosure temperature sensor 4"
        ::= { lgpEnvEnclosureTemperatureSensors 4 }

lgpEnvValueAmbientRoomTemperature OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Temperature outside enclosure."
    ::= { lgpEnvTemperatureWellKnown 15 }

lgpEnvDewPointTemperature OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "The calculated temperature outside of the enclosure at which
        condensation is likely to occur."
    ::= { lgpEnvTemperatureWellKnown 16 }

lgpEnvEnclosureTemperature OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Temperature inside of enclosure."
    ::= { lgpEnvTemperatureWellKnown 17 }

lgpEnvAdjustedTemperature OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "The current temperature set-point which is computed by the system and
         may be temporarily different from the user set-point because of
         external factors."
    ::= { lgpEnvTemperatureWellKnown 18 }

lgpEnvExternalSensors OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "External sensors to monitor environmental variables such as 
        temperature and humidity"
    ::= { lgpEnvTemperatureWellKnown 19 }

    lgpEnvExternalAirSensorA OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
                "Temperature and humidity measurements from external air
                sensor A."
        ::= { lgpEnvExternalSensors 1 }

    lgpEnvExternalAirSensorADewPoint OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
                "Dewpoint temperature for External Air Sensor A."
        ::= { lgpEnvExternalSensors 2 }

    lgpEnvExternalAirSensorB OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
                "Temperature and humidity measurements from external air
                sensor B."
        ::= { lgpEnvExternalSensors 3 }

    lgpEnvExternalAirSensorBDewPoint OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
                "Dewpoint temperature for External Air Sensor B."
        ::= { lgpEnvExternalSensors 4 }

lgpEnvSupplyFluidTemperature OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "The current temperature of the fluid being supplied."
    ::= { lgpEnvTemperatureWellKnown 20 }

lgpEnvSupplyRefrigerantTemperature OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "The current temperature of the refrigerant being supplied."
    ::= { lgpEnvTemperatureWellKnown 21 }

lgpEnvMinDesiredRoomAirTemperature OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "The minimum desired room air temperature. If the room air temperature
         falls below this set point, the unit will reduce the cooling."
    ::= { lgpEnvTemperatureWellKnown 22 }

lgpEnvDewPointTemperatures OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "This sub-tree identifies well-known dew point temperatures in the
         system."
    ::= { lgpEnvTemperatureWellKnown 23 }

    lgpEnvInletDewPointTemperature OBJECT-IDENTITY
        STATUS      current
        DESCRIPTION
            "Dew point temperature measured at the inlet of the unit."
        ::= { lgpEnvDewPointTemperatures 1 }

-- =============================================================================
-- lgpEnvTemperatureFahrenheit - Liebert Environmental Fahrenheit
-- Temperature Group
-- =============================================================================

lgpEnvTemperatureSettingDegF OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "degrees Fahrenheit"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The temperature setting used to control the well known temperature
        object 'lgpEnvControlTemperature'.  This setting is cloned in
        'lgpEnvTemperatureSettingDegC' with the value converted to Celsius."
    ::= { lgpEnvTemperatureFahrenheit 1 }

lgpEnvTemperatureToleranceDegF OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "0.1 degrees Fahrenheit"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The acceptable variance from 'lgpEnvTemperatureSettingDegF', without
        initiating a control action.  This setting is cloned in
        'lgpEnvTemperatureToleranceDegC' with the value converted to Celsius."
    ::= { lgpEnvTemperatureFahrenheit 2 }

lgpEnvTemperatureTableDegF OBJECT-TYPE
    SYNTAX      SEQUENCE OF LgpEnvTemperatureEntryDegF
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A list of temperature table entries.  The table contains zero, one,
        or many rows, depending upon the number of temperature objects
        available.  The NMS cannot create or delete rows from the table. The
        rows are created by the agent based upon the capabilities of the
        managed device.  The entries in this table are cloned in
        'lgpEnvTemperatureTableDegC' where Fahrenheit values are converted to
        Celsius."
    ::= { lgpEnvTemperatureFahrenheit 3 }

lgpEnvTemperatureDeadbandRangeDegF  OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       ".1 degrees Fahrenheit"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The allowable deviation above and below the temperature set point
         used to create a no control region, a dead-band, where  heating
         and cooling  control are disabled."

    ::= { lgpEnvTemperatureFahrenheit 4 }

lgpEnvTemperatureEntryDegF OBJECT-TYPE
    SYNTAX      LgpEnvTemperatureEntryDegF
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This entry defines the contents of the rows for the table
        'lgpEnvTemperatureTableDegF'."
    INDEX       { lgpEnvTemperatureIdDegF }
    ::= { lgpEnvTemperatureTableDegF 1 }

LgpEnvTemperatureEntryDegF ::= SEQUENCE 
{
    lgpEnvTemperatureIdDegF                     Unsigned32,
    lgpEnvTemperatureDescrDegF                  OBJECT IDENTIFIER,
    lgpEnvTemperatureMeasurementDegF            Integer32,
    lgpEnvTemperatureHighThresholdDegF          Integer32,
    lgpEnvTemperatureLowThresholdDegF           Integer32,
    lgpEnvTemperatureSetPointDegF               Integer32,
    lgpEnvTemperatureDailyHighDegF              Integer32,
    lgpEnvTemperatureDailyLowDegF               Integer32,
    lgpEnvTempDailyHighTimeHourDegF             Integer32,
    lgpEnvTempDailyHighTimeMinuteDegF           Integer32,
    lgpEnvTempDailyHighTimeSecondDegF           Integer32,
    lgpEnvTempDailyLowTimeHourDegF              Integer32,
    lgpEnvTempDailyLowTimeMinuteDegF            Integer32,
    lgpEnvTempDailyLowTimeSecondDegF            Integer32,
    lgpEnvTemperatureMeasurementTenthsDegF      Integer32,
    lgpEnvTemperatureHighThresholdTenthsDegF    Integer32,
    lgpEnvTemperatureLowThresholdTenthsDegF     Integer32,
    lgpEnvTemperatureSetPointTenthsDegF         Integer32,
    lgpEnvTemperatureDeadBandTenthsDegF         Integer32,
    lgpEnvTempHeatingPropBandTenthsDegF         Integer32,
    lgpEnvTempCoolingPropBandTenthsDegF         Integer32

}

lgpEnvTemperatureIdDegF OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This OID is used as an index to identify a row in the table
        'lgpEnvTemperatureTableDegF'."
    ::= { lgpEnvTemperatureEntryDegF 1 }

lgpEnvTemperatureDescrDegF OBJECT-TYPE
    SYNTAX      OBJECT IDENTIFIER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A reference to a temperature description object. The object
        referenced should not be accessible, but rather be used to provide
        a unique description of the temperature."
    ::= { lgpEnvTemperatureEntryDegF 2 }

lgpEnvTemperatureMeasurementDegF OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "degrees Fahrenheit"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The measured temperature value."
    ::= { lgpEnvTemperatureEntryDegF 3 }

lgpEnvTemperatureHighThresholdDegF OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "degrees Fahrenheit"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The high temperature notification threshold.  This is the maximum
        value of 'lgpEnvTemperatureMeasurementDegF' before the agent sends a
        notification."
    ::= { lgpEnvTemperatureEntryDegF 4 }

lgpEnvTemperatureLowThresholdDegF OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "degrees Fahrenheit"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The low temperature notification threshold.  This is the minimum
        value of 'lgpEnvTemperatureMeasurementDegF' before the agent sends a
        notification."
    ::= { lgpEnvTemperatureEntryDegF 5 }

lgpEnvTemperatureSetPointDegF OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "degrees Fahrenheit"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The temperature setting for the well known
        'lgpEnvTemperatureDescrDegF' point.  This setting may or may not be
        the setting used from control.  Some systems have the capability to
        dynamically change the control setting based on environmental
        conditions and/or user configuration."
    ::= { lgpEnvTemperatureEntryDegF 6 }

lgpEnvTemperatureDailyHighDegF OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "degrees Fahrenheit"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The daily high temperature measurement."
    ::= { lgpEnvTemperatureEntryDegF 7 }

lgpEnvTemperatureDailyLowDegF OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "degrees Fahrenheit"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The daily low temperature measurement."
    ::= { lgpEnvTemperatureEntryDegF 8 }

lgpEnvTempDailyHighTimeHourDegF OBJECT-TYPE
    SYNTAX      Integer32(0..23)
    UNITS       "hours"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The hours digit of the time corresponding to the daily high
         temperature measurement."
    ::= { lgpEnvTemperatureEntryDegF 9 }

lgpEnvTempDailyHighTimeMinuteDegF OBJECT-TYPE
    SYNTAX      Integer32(0..59)
    UNITS       "minutes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The minutes digit of the time corresponding to the daily high
         temperature measurement."
    ::= { lgpEnvTemperatureEntryDegF 10 }

lgpEnvTempDailyHighTimeSecondDegF OBJECT-TYPE
    SYNTAX      Integer32(0..59)
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The seconds digit of the time corresponding to the daily high
         temperature measurement."
    ::= { lgpEnvTemperatureEntryDegF 11 }

lgpEnvTempDailyLowTimeHourDegF OBJECT-TYPE
    SYNTAX      Integer32(0..23)
    UNITS       "hours"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The hours digit of the time corresponding to the daily low
         temperature measurement."
    ::= { lgpEnvTemperatureEntryDegF 12 }

lgpEnvTempDailyLowTimeMinuteDegF OBJECT-TYPE
    SYNTAX      Integer32(0..59)
    UNITS       "minutes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The minutes digit of the time corresponding to the daily low
         temperature measurement."
    ::= { lgpEnvTemperatureEntryDegF 13 }

lgpEnvTempDailyLowTimeSecondDegF OBJECT-TYPE
    SYNTAX      Integer32(0..59)
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The seconds digit of the time corresponding to the daily low
         temperature measurement."
    ::= { lgpEnvTemperatureEntryDegF 14 }

lgpEnvTemperatureMeasurementTenthsDegF OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       ".1 degrees Fahrenheit"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The measured temperature value."
    ::= { lgpEnvTemperatureEntryDegF 50 }

lgpEnvTemperatureHighThresholdTenthsDegF OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       ".1 degrees Fahrenheit"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The high temperature notification threshold.  This is the maximum
        value of 'lgpEnvTemperatureMeasurementTenthsDegF' before the agent sends a
        notification."
    ::= { lgpEnvTemperatureEntryDegF 51 }

lgpEnvTemperatureLowThresholdTenthsDegF OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       ".1 degrees Fahrenheit"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The low temperature notification threshold.  This is the minimum
        value of 'lgpEnvTemperatureMeasurementTenthsDegF' before the agent sends a
        notification."
    ::= { lgpEnvTemperatureEntryDegF 52 }

lgpEnvTemperatureSetPointTenthsDegF OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       ".1 degrees Fahrenheit"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The temperature setting for the well known
        'lgpEnvTemperatureDescrDegF' point.  This setting may or may not be
        the setting used from control.  Some systems have the capability to
        dynamically change the control setting based on environmental
        conditions and/or user configuration."
    ::= { lgpEnvTemperatureEntryDegF 53 }

lgpEnvTemperatureDeadBandTenthsDegF OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       ".1 degrees Fahrenheit"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The deadband region around the setpoint value 
        (lgpEnvTemperatureSetPointTenthsDegF) where no heating or cooling will occur."
    ::= { lgpEnvTemperatureEntryDegF 60 }

lgpEnvTempHeatingPropBandTenthsDegF OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       ".1 degrees Fahrenheit"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The proportional region below the setpoint value
        (lgpEnvTemperatureSetPointTenthsDegF) where heating will be
        proportionally controlled."
    ::= { lgpEnvTemperatureEntryDegF 61 }

lgpEnvTempCoolingPropBandTenthsDegF OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       ".1 degrees Fahrenheit"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The proportional region above the setpoint value
        (lgpEnvTemperatureSetPointTenthsDegF) where cooling will be
        proportionally controlled."
    ::= { lgpEnvTemperatureEntryDegF 62 }

-- =============================================================================
-- lgpEnvTemperatureCelsius - Liebert Environmental Celsius
-- Temperature Group
-- =============================================================================

lgpEnvTemperatureSettingDegC OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "degrees Celsius"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The temperature setting used to control the well known temperature
        object 'lgpEnvControlTemperature'.  This setting is cloned in
        'lgpEnvTemperatureSettingDegF' with the value converted to Fahrenheit."
    ::= { lgpEnvTemperatureCelsius 1 }

lgpEnvTemperatureToleranceDegC OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "0.1 degrees Celsius"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The acceptable variance from 'lgpEnvTemperatureSettingDegC', without
        initiating a control action.  This setting is cloned in
        'lgpEnvTemperatureToleranceDegF' with the value converted to Fahrenheit."
    ::= { lgpEnvTemperatureCelsius 2 }

lgpEnvTemperatureTableDegC OBJECT-TYPE
    SYNTAX      SEQUENCE OF LgpEnvTemperatureEntryDegC
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A list of temperature table entries.  The table contains zero, one,
        or many rows, depending upon the number of temperature objects
        available.  The NMS cannot create or delete rows from the table. The
        rows are created by the agent based upon the capabilities of the
        managed device.  The entries in this table are cloned in
        'lgpEnvTemperatureTableDegF' where Celsius values are converted to
        Fahrenheit."
    ::= { lgpEnvTemperatureCelsius 3 }

lgpEnvTemperatureDeadbandRangeDegC OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       ".1 degrees Celsius"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The allowable deviation above and below the temperature set point
         used to create a no control region, a dead-band, where  heating
         and cooling  control are disabled."
    ::= { lgpEnvTemperatureCelsius 4 }

lgpEnvTemperatureEntryDegC OBJECT-TYPE
    SYNTAX      LgpEnvTemperatureEntryDegC
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This entry defines the contents of the rows for the table
        'lgpEnvTemperatureTableDegC'."
    INDEX       { lgpEnvTemperatureIdDegC }
    ::= { lgpEnvTemperatureTableDegC 1 }

LgpEnvTemperatureEntryDegC ::= SEQUENCE 
{
    lgpEnvTemperatureIdDegC                     Unsigned32,
    lgpEnvTemperatureDescrDegC                  OBJECT IDENTIFIER,
    lgpEnvTemperatureMeasurementDegC            Integer32,
    lgpEnvTemperatureHighThresholdDegC          Integer32,
    lgpEnvTemperatureLowThresholdDegC           Integer32,
    lgpEnvTemperatureSetPointDegC               Integer32,
    lgpEnvTemperatureDailyHighDegC              Integer32,
    lgpEnvTemperatureDailyLowDegC               Integer32,
    lgpEnvTempDailyHighTimeHourDegC             Integer32,
    lgpEnvTempDailyHighTimeMinuteDegC           Integer32,
    lgpEnvTempDailyHighTimeSecondDegC           Integer32,
    lgpEnvTempDailyLowTimeHourDegC              Integer32,
    lgpEnvTempDailyLowTimeMinuteDegC            Integer32,
    lgpEnvTempDailyLowTimeSecondDegC            Integer32,
    lgpEnvTemperatureMeasurementTenthsDegC      Integer32,
    lgpEnvTemperatureHighThresholdTenthsDegC    Integer32,
    lgpEnvTemperatureLowThresholdTenthsDegC     Integer32,
    lgpEnvTemperatureSetPointTenthsDegC         Integer32,
    lgpEnvTemperatureDeadBandTenthsDegC         Integer32,
    lgpEnvTempHeatingPropBandTenthsDegC         Integer32,
    lgpEnvTempCoolingPropBandTenthsDegC         Integer32

}

lgpEnvTemperatureIdDegC OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This OID is used as an index to identify a row in the table
        'lgpEnvTemperatureTableDegC'."
    ::= { lgpEnvTemperatureEntryDegC 1 }

lgpEnvTemperatureDescrDegC OBJECT-TYPE
    SYNTAX      OBJECT IDENTIFIER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A reference to a temperature description object. The object
        referenced should not be accessible, but rather be used to provide
        a unique description of the temperature."
    ::= { lgpEnvTemperatureEntryDegC 2 }

lgpEnvTemperatureMeasurementDegC OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "degrees Celsius"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The measured temperature value."
    ::= { lgpEnvTemperatureEntryDegC 3 }

lgpEnvTemperatureHighThresholdDegC OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "degrees Celsius"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The high temperature notification threshold.  This is the maximum
        value of 'lgpEnvTemperatureMeasurementDegC' before the agent sends a
        notification."
    ::= { lgpEnvTemperatureEntryDegC 4 }

lgpEnvTemperatureLowThresholdDegC OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "degrees Celsius"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The low temperature notification threshold.  This is the minimum
        value of 'lgpEnvTemperatureMeasurementDegC' before the agent sends a
        notification."
    ::= { lgpEnvTemperatureEntryDegC 5 }

lgpEnvTemperatureSetPointDegC OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "degrees Celsius"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The temperature setting for the well known
        'lgpEnvTemperatureDescrDegC' point.  This setting may or may not be
        the setting used from control.  Some systems have the capability to
        dynamically change the control setting based on environmental
        conditions and/or user configuration."
    ::= { lgpEnvTemperatureEntryDegC 6 }

lgpEnvTemperatureDailyHighDegC OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "degrees Celsius"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The daily high temperature measurement."
    ::= { lgpEnvTemperatureEntryDegC 7 }

lgpEnvTemperatureDailyLowDegC OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "degrees Celsius"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The daily low temperature measurement."
    ::= { lgpEnvTemperatureEntryDegC 8 }

lgpEnvTempDailyHighTimeHourDegC OBJECT-TYPE
    SYNTAX      Integer32(0..23)
    UNITS       "hours"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The hours digit of the time corresponding to the daily high
        temperature measurement."
    ::= { lgpEnvTemperatureEntryDegC 9 }

lgpEnvTempDailyHighTimeMinuteDegC OBJECT-TYPE
    SYNTAX      Integer32(0..59)
    UNITS       "minutes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The minutes digit of the time corresponding to the daily high
        temperature measurement."
    ::= { lgpEnvTemperatureEntryDegC 10 }

lgpEnvTempDailyHighTimeSecondDegC OBJECT-TYPE
    SYNTAX      Integer32(0..59)
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The seconds digit of the time corresponding to the daily high
        temperature measurement."
    ::= { lgpEnvTemperatureEntryDegC 11 }

lgpEnvTempDailyLowTimeHourDegC OBJECT-TYPE
    SYNTAX      Integer32(0..23)
    UNITS       "hours"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The hours digit of the time corresponding to the daily low
        temperature measurement."
    ::= { lgpEnvTemperatureEntryDegC 12 }

lgpEnvTempDailyLowTimeMinuteDegC OBJECT-TYPE
    SYNTAX      Integer32(0..59)
    UNITS       "minutes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The minutes digit of the time corresponding to the daily low
        temperature measurement."
    ::= { lgpEnvTemperatureEntryDegC 13 }

lgpEnvTempDailyLowTimeSecondDegC OBJECT-TYPE
    SYNTAX      Integer32(0..59)
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The seconds digit of the time corresponding to the daily low
        temperature measurement."
    ::= { lgpEnvTemperatureEntryDegC 14 }

lgpEnvTemperatureMeasurementTenthsDegC OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       ".1 degrees Celsius"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The measured temperature value."
    ::= { lgpEnvTemperatureEntryDegC 50 }

lgpEnvTemperatureHighThresholdTenthsDegC OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       ".1 degrees Celsius"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The high temperature notification threshold.  This is the maximum
        value of 'lgpEnvTemperatureMeasurementTenthsDegC' before the agent sends a
        notification."
    ::= { lgpEnvTemperatureEntryDegC 51 }

lgpEnvTemperatureLowThresholdTenthsDegC OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       ".1 degrees Celsius"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The low temperature notification threshold.  This is the minimum
        value of 'lgpEnvTemperatureMeasurementTenthsDegC' before the agent sends a
        notification."
    ::= { lgpEnvTemperatureEntryDegC 52 }

lgpEnvTemperatureSetPointTenthsDegC OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       ".1 degrees Celsius"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The temperature setting for the well known
        'lgpEnvTemperatureDescrDegC' point.  This setting may or may not be
        the setting used from control.  Some systems have the capability to
        dynamically change the control setting based on environmental
        conditions and/or user configuration."
    ::= { lgpEnvTemperatureEntryDegC 53 }

lgpEnvTemperatureDeadBandTenthsDegC OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       ".1 degrees Celsius"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The deadband region around the setpoint value 
        (lgpEnvTemperatureSetPointTenthsDegC) where no heating or cooling will occur."
    ::= { lgpEnvTemperatureEntryDegC 60 }

lgpEnvTempHeatingPropBandTenthsDegC OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       ".1 degrees Celsius"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The proportional region below the setpoint value
        (lgpEnvTemperatureSetPointTenthsDegC) where heating will be
        proportionally controlled."
    ::= { lgpEnvTemperatureEntryDegC 61 }

lgpEnvTempCoolingPropBandTenthsDegC OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       ".1 degrees Celsius"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The proportional region above the setpoint value
        (lgpEnvTemperatureSetPointTenthsDegC) where cooling will be
        proportionally controlled."
    ::= { lgpEnvTemperatureEntryDegC 62 }

-- =============================================================================
-- lgpEnvHumidityMeasurements - Liebert "well-known" Humidity objects
-- =============================================================================

lgpEnvControlHumidity      OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Humidity measurement used as control feedback."
    ::= { lgpEnvHumidityWellKnown 1 }

lgpEnvReturnAirHumidity    OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Humidity measurement of return air."
    ::= { lgpEnvHumidityWellKnown 2 }

lgpEnvSupplyAirHumidity    OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Humidity measurement of supply air."
    ::= { lgpEnvHumidityWellKnown 3 }

lgpEnvValueAmbientHumidity OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Humidity outside enclosure."
    ::= { lgpEnvHumidityWellKnown 4 }

-- =============================================================================
-- lgpEnvRelativeHumidity - Liebert Environmental Relative Humidity Group
-- =============================================================================

lgpEnvHumiditySettingRel OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "percent Relative Humidity"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The humidity setting used to control the well known humidity
        point."
    ::= { lgpEnvHumidityRelative 1 }

lgpEnvHumidityToleranceRel OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "percent Relative Humidity"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Acceptable variance from lgpEnvHumiditySettingRel, without
        initiating a control action."
    ::= { lgpEnvHumidityRelative 2 }

lgpEnvHumidityTableRel OBJECT-TYPE
    SYNTAX      SEQUENCE OF LgpEnvHumidityEntryRel
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A list of humidity table entries.  The table contains zero, one,
        or many rows, depending upon the number of humidity objects available.
        The NMS cannot create or delete rows from the table. The rows are
        created by the agent based upon the capabilities of the managed device."
    ::= { lgpEnvHumidityRelative 3 }

lgpEnvHumidityDeadbandRange OBJECT-TYPE
       SYNTAX      Integer32
       UNITS       ".1 percent RH"
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
       "The allowable deviation above and below the humidity set point used
        to create a no control region, a dead-band, where humidifying and
        dehumidifying control are disabled."
       ::= { lgpEnvHumidityRelative 4 }

lgpEnvHumidityEntryRel OBJECT-TYPE
    SYNTAX      LgpEnvHumidityEntryRel
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "This entry defines the contents of the rows for the table
       'lgpEnvHumidityTableRel'."
    INDEX       { lgpEnvHumidityIdRel }
    ::= { lgpEnvHumidityTableRel 1 }

LgpEnvHumidityEntryRel ::= SEQUENCE 
{
    lgpEnvHumidityIdRel                         Unsigned32,
    lgpEnvHumidityDescrRel                      OBJECT IDENTIFIER,
    lgpEnvHumidityMeasurementRel                Integer32,
    lgpEnvHumidityHighThresholdRel              Integer32,
    lgpEnvHumidityLowThresholdRel               Integer32,
    lgpEnvHumiditySetPoint                      Integer32,
    lgpEnvHumidityDailyHigh                     Integer32,
    lgpEnvHumidityDailyLow                      Integer32,
    lgpEnvHumidityDailyHighTimeHour             Integer32,
    lgpEnvHumidityDailyHighTimeMinute           Integer32,
    lgpEnvHumidityDailyHighTimeSecond           Integer32,
    lgpEnvHumidityDailyLowTimeHour              Integer32,
    lgpEnvHumidityDailyLowTimeMinute            Integer32,
    lgpEnvHumidityDailyLowTimeSecond            Integer32,
    lgpEnvHumidityDeadBand                      Integer32,
    lgpEnvHumidifyPropBand                      Integer32,
    lgpEnvDehumidifyPropBand                    Integer32,
    lgpEnvHumidityMeasurementRelTenths          Integer32,
    lgpEnvHumidityHighThresholdRelTenths        Integer32,
    lgpEnvHumidityLowThresholdRelTenths         Integer32
}

lgpEnvHumidityIdRel OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This OID is used as an index to identify a row in the table
        'lgpEnvHumidityTableRel'."
    ::= { lgpEnvHumidityEntryRel 1 }

lgpEnvHumidityDescrRel OBJECT-TYPE
    SYNTAX      OBJECT IDENTIFIER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A reference to a humidity description object. The object
        referenced should not be accessible, but rather be used
        to provide a unique description of the humidity."
    ::= { lgpEnvHumidityEntryRel 2 }

lgpEnvHumidityMeasurementRel OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "percent Relative Humidity"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The measured humidity value."
    ::= { lgpEnvHumidityEntryRel 3 }

lgpEnvHumidityHighThresholdRel OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "percent Relative Humidity"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The high humidity notification threshold.  This is the maximum
        value of 'lgpEnvHumidityMeasurementRel' before the agent sends a
        notification."
    ::= { lgpEnvHumidityEntryRel 4 }

lgpEnvHumidityLowThresholdRel OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "percent Relative Humidity"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The low humidity notification threshold.  This is the minimum
        value of 'lgpEnvHumidityMeasurementRel' before the agent sends a
        notification."
    ::= { lgpEnvHumidityEntryRel 5 }

lgpEnvHumiditySetPoint OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "percent Relative Humidity"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The humidity setting used to control the well known humidity
        object 'lgpEnvHumidityDescrRel'.  This setting may or may not be
        the setting used from control.  Some systems have the capability to
        dynamically change the control setting based on environmental
        conditions and/or user configuration."
    ::= { lgpEnvHumidityEntryRel 6 }

lgpEnvHumidityDailyHigh OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "percent Relative Humidity"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The daily high relative humidity measurement."
    ::= { lgpEnvHumidityEntryRel 7 }

 lgpEnvHumidityDailyLow OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "percent Relative Humidity"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The daily low relative humidity measurement."
    ::= { lgpEnvHumidityEntryRel 8 }

lgpEnvHumidityDailyHighTimeHour OBJECT-TYPE
    SYNTAX      Integer32(0..23)
    UNITS       "hours"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The hours digit of the time corresponding to the daily high
        humidity measurement."
    ::= { lgpEnvHumidityEntryRel 9 }

lgpEnvHumidityDailyHighTimeMinute OBJECT-TYPE
    SYNTAX      Integer32(0..59)
    UNITS       "minutes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The minutes digit of the time corresponding to the daily high
        humidity measurement."
    ::= { lgpEnvHumidityEntryRel 10 }

lgpEnvHumidityDailyHighTimeSecond OBJECT-TYPE
    SYNTAX      Integer32(0..59)
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The seconds digit of the time corresponding to the daily high
        humidity measurement."
    ::= { lgpEnvHumidityEntryRel 11 }

lgpEnvHumidityDailyLowTimeHour OBJECT-TYPE
    SYNTAX      Integer32(0..23)
    UNITS       "hours"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The hours digit of the time corresponding to the daily low humidity measurement."
    ::= { lgpEnvHumidityEntryRel 12 }

lgpEnvHumidityDailyLowTimeMinute OBJECT-TYPE
    SYNTAX      Integer32(0..59)
    UNITS       "minutes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The minutes digit of the time corresponding to the daily low
        humidity measurement."
    ::= { lgpEnvHumidityEntryRel 13 }

lgpEnvHumidityDailyLowTimeSecond OBJECT-TYPE
    SYNTAX      Integer32(0..59)
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The seconds digit of the time corresponding to the daily low humidity measurement."
    ::= { lgpEnvHumidityEntryRel 14 }

lgpEnvHumidityDeadBand OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "percent Relative Humidity"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The deadband region around the setpoint value 
        (lgpEnvHumiditySetPoint) where no humidifying or dehumidifying will occur."
    ::= { lgpEnvHumidityEntryRel 15 }

lgpEnvHumidifyPropBand OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "percent Relative Humidity"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The proportional region below the setpoint value
        (lgpEnvHumiditySetPoint) where humidifying will be
        proportionally controlled."
    ::= { lgpEnvHumidityEntryRel 16 }

lgpEnvDehumidifyPropBand OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "percent Relative Humidity"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The proportional region above the setpoint value
        (lgpEnvHumiditySetPoint) where dehumidifying will be
        proportionally controlled."
    ::= { lgpEnvHumidityEntryRel 17 }

lgpEnvHumidityMeasurementRelTenths OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       ".1 percent Relative Humidity"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The measured humidity value."
    ::= { lgpEnvHumidityEntryRel 50 }

lgpEnvHumidityHighThresholdRelTenths OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       ".1 percent Relative Humidity"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The high humidity notification threshold.  This is the maximum
        value of 'lgpEnvHumidityMeasurementRelTenths' before the agent sends a
        notification."
    ::= { lgpEnvHumidityEntryRel 51 }

lgpEnvHumidityLowThresholdRelTenths OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       ".1 percent Relative Humidity"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The low humidity notification threshold.  This is the minimum
        value of 'lgpEnvHumidityMeasurementRelTenths' before the agent sends a
        notification."
    ::= { lgpEnvHumidityEntryRel 52 }

-- =============================================================================
-- lgpEnvRemoteSensors - Liebert Environmental Remote Sensor Group
-- =============================================================================

lgpEnvRemoteSensorCalc OBJECT-TYPE
    SYNTAX      INTEGER
    {
        average(1),
        maximum(2)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Calculation method applied to temperature readings from the remote
        sensors to determine a single temperature measurement value for
        cooling and heating control."
    ::= { lgpEnvRemoteSensors 1 }

lgpEnvRemoteSensorTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF LgpEnvRemoteSensorEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains a list of remote sensors attached to the
        environmental unit. The table contains zero, one, or more rows,
        depending upon the number of sensors attached to the unit."
    ::= { lgpEnvRemoteSensors 10 }

    lgpEnvRemoteSensorEntry OBJECT-TYPE
        SYNTAX      LgpEnvRemoteSensorEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "This entry defines the attributes to be populated in the
            various columns of the 'lgpEnvRemoteSensorTable'."
        INDEX       
        { 
            lgpEnvRemoteSensorIndex
        }
        ::= { lgpEnvRemoteSensorTable 1 }

    LgpEnvRemoteSensorEntry ::= SEQUENCE 
    {
        lgpEnvRemoteSensorIndex                   Unsigned32,
        lgpEnvRemoteSensorId                      Unsigned32,
        lgpEnvRemoteSensorMode                    Integer32,
        lgpEnvRemoteSensorUsrLabel                DisplayString,
        lgpEnvRemoteSensorTempMeasurementDegF     Integer32,
        lgpEnvRemoteSensorTempMeasurementDegC     Integer32
    }

    lgpEnvRemoteSensorIndex OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "This is the index indicating the nth element of the table."
        ::= { lgpEnvRemoteSensorEntry 1 }

    lgpEnvRemoteSensorId OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "This is the sensor number identifying the sensor."
        ::= { lgpEnvRemoteSensorEntry 2 }

    lgpEnvRemoteSensorMode OBJECT-TYPE
        SYNTAX      INTEGER
        {
            disable(0),
            reference(1),
            control(2)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "Function assigned to remote sensor.  When set to control(2) the
            sensor will be used in calculation of remote sensor temperature which
            may be used for heating and cooling control.  When set to disable(0)
            the remote sensor reading is not available.  When set to reference(1)
            the remote sensor reading is available but not used for control."
        ::= { lgpEnvRemoteSensorEntry 3 }

    lgpEnvRemoteSensorUsrLabel OBJECT-TYPE 
        SYNTAX      DisplayString 
        MAX-ACCESS  read-write 
        STATUS      current 
        DESCRIPTION 
            "User assigned remote sensor label." 
        ::= { lgpEnvRemoteSensorEntry 4 } 

    lgpEnvRemoteSensorTempMeasurementDegF OBJECT-TYPE
        SYNTAX      Integer32
        UNITS       "degrees Fahrenheit"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Temperature measured at the temperature sensor reported in
             degrees Fahrenheit."
        ::= { lgpEnvRemoteSensorEntry 5 }

    lgpEnvRemoteSensorTempMeasurementDegC OBJECT-TYPE
        SYNTAX      Integer32
        UNITS       "degrees Celsius"
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Temperature measured at the temperature sensor reported in
             degrees Celsius."
        ::= { lgpEnvRemoteSensorEntry 6 }

END

