ADSL2-LINE-TC-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    transmission
        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION
        FROM SNMPv2-TC;


adsl2TCMIB MODULE-IDENTITY
    LAST-UPDATED    "200610040000Z"
    ORGANIZATION    "ADSLMIB Working Group"
    CONTACT-INFO
            "WG-email:  adslmib@ietf.org
            Info:      https://www1.ietf.org/mailman/listinfo/adslmib

                      Chair:     Mike Sneed
                                 Sand Channel Systems
                      Postal:    P.O. Box 37324
                                 Raleigh NC 27627-732
                      Email:     sneedmike@hotmail.com
                      Phone:     +1 206 600 7022

                      Co-Chair & Co-editor:
                                 Menachem Dodge
                                 ECI Telecom Ltd.
                      Postal:    30 Hasivim St.
                                 Petach Tikva 49517,
                                 Israel.
                      Email:     mbdodge@ieee.org
                      Phone:     +972 3 926 8421
                      Co-editor: Moti Morgenstern
                                 ECI Telecom Ltd.
                      Postal:    30 Hasivim St.
                                 Petach Tikva 49517,
                                 Israel.
                      Email:     moti.morgenstern@ecitele.com
                      Phone:     +972 3 926 6258

                      Co-editor: Scott Baillie
                                 NEC Australia
                      Postal:    649-655 Springvale Road,
                                 Mulgrave, Victoria 3170,
                                 Australia.
                      Email:     scott.baillie@nec.com.au
                      Phone:     +61 3 9264 3986

                      Co-editor: Umberto Bonollo
                                 NEC Australia
                      Postal:    649-655 Springvale Road,
                                 Mulgrave, Victoria 3170,
                                 Australia.
                      Email:     umberto.bonollo@nec.com.au
                      Phone:     +61 3 9264 3385"
    DESCRIPTION
        "This MIB Module provides Textual Conventions to be
        used by the ADSL2-LINE-MIB module for the purpose of
        managing ADSL, ADSL2, and ADSL2+ lines.

        Copyright (C) The Internet Society (2006).  This version of
        this MIB module is part of RFC 4706: see the RFC itself for
        full legal notices."
    REVISION        "200610040000Z"
    DESCRIPTION
        "Initial version, published as RFC 4706."
    ::= { transmission 238 2 }



-- adsl2MIB 2
--   
-- ----------------------------------------------
-- Textual Conventions               --
-- ----------------------------------------------

Adsl2Unit ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Identifies a transceiver as being either an ATU-C or
        an ATU-R.  An ADSL line consists of two transceivers, an ATU-C
        and an ATU-R.  Attributes with this syntax reference the two
        sides of a line.  Specified as an INTEGER, the two values
        are:

         atuc(1)  -- Central office ADSL terminal unit (ATU-C).
         atur(2)  -- Remote ADSL terminal unit (ATU-R)."
    SYNTAX          INTEGER  {
                        atuc(1),
                        atur(2)
                    }

Adsl2Direction ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Identifies the direction of a band as being
        either upstream or downstream.  Specified as an INTEGER,
        the two values are:
         upstream(1), and
         downstream(2)."
    SYNTAX          INTEGER  {
                        upstream(1),
                        downstream(2)
                    }

Adsl2TransmissionModeType ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "A set of ADSL2 line transmission modes, with one bit
        per mode.  The notes (F) and (L) denote Full-Rate
        and Lite/splitterless, respectively:
           Bit 00 : Regional Std. (ANSI T1.413) (F)
           Bit 01 : Regional Std. (ETSI DTS/TM06006) (F)
           Bit 02 : G.992.1 POTS non-overlapped (F)
           Bit 03 : G.992.1 POTS overlapped (F)
           Bit 04 : G.992.1 ISDN non-overlapped (F)
           Bit 05 : G.992.1 ISDN overlapped (F)
           Bit 06 : G.992.1 TCM-ISDN non-overlapped (F)
           Bit 07 : G.992.1 TCM-ISDN overlapped (F)
           Bit 08 : G.992.2 POTS non-overlapped (L)
           Bit 09 : G.992.2 POTS overlapped (L)
           Bit 10 : G.992.2 with TCM-ISDN non-overlapped (L)
           Bit 11 : G.992.2 with TCM-ISDN overlapped (L)
           Bit 12 : G.992.1 TCM-ISDN symmetric (F) -- not in G.997.1
           Bit 13-17: Reserved
           Bit 18 : G.992.3 POTS non-overlapped (F)
           Bit 19 : G.992.3 POTS overlapped (F)
           Bit 20 : G.992.3 ISDN non-overlapped (F)
           Bit 21 : G.992.3 ISDN overlapped (F)
           Bit 22-23: Reserved
           Bit 24 : G.992.4 POTS non-overlapped (L)
           Bit 25 : G.992.4 POTS overlapped (L)
           Bit 26-27: Reserved
           Bit 28 : G.992.3 Annex I All-Digital non-overlapped (F)
           Bit 29 : G.992.3 Annex I All-Digital overlapped (F)
           Bit 30 : G.992.3 Annex J All-Digital non-overlapped (F)
           Bit 31 : G.992.3 Annex J All-Digital overlapped (F)
           Bit 32 : G.992.4 Annex I All-Digital non-overlapped (L)
           Bit 33 : G.992.4 Annex I All-Digital overlapped (L)
           Bit 34 : G.992.3 Annex L POTS non-overlapped, mode 1,
                                    wide U/S (F)
           Bit 35 : G.992.3 Annex L POTS non-overlapped, mode 2,
                                    narrow U/S(F)
           Bit 36 : G.992.3 Annex L POTS overlapped, mode 3,
                                    wide U/S (F)
           Bit 37 : G.992.3 Annex L POTS overlapped, mode 4,
                                    narrow U/S (F)
           Bit 38 : G.992.3 Annex M POTS non-overlapped (F)
           Bit 39 : G.992.3 Annex M POTS overlapped (F)
           Bit 40 : G.992.5 POTS non-overlapped (F)
           Bit 41 : G.992.5 POTS overlapped (F)
           Bit 42 : G.992.5 ISDN non-overlapped (F)
           Bit 43 : G.992.5 ISDN overlapped (F)
           Bit 44-45: Reserved
           Bit 46 : G.992.5 Annex I All-Digital non-overlapped (F)
           Bit 47 : G.992.5 Annex I All-Digital overlapped (F)
           Bit 48 : G.992.5 Annex J All-Digital non-overlapped (F)
           Bit 49 : G.992.5 Annex J All-Digital overlapped (F)
           Bit 50 : G.992.5 Annex M POTS non-overlapped (F)
           Bit 51 : G.992.5 Annex M POTS overlapped (F)
           Bit 52-55: Reserved"
    SYNTAX          BITS {
                        ansit1413(0),
                        etsi(1),
                        g9921PotsNonOverlapped(2),
                        g9921PotsOverlapped(3),
                        g9921IsdnNonOverlapped(4),
                        g9921isdnOverlapped(5),
                        g9921tcmIsdnNonOverlapped(6),
                        g9921tcmIsdnOverlapped(7),
                        g9922potsNonOverlapped(8),
                        g9922potsOverlapped(9),
                        g9922tcmIsdnNonOverlapped(10),
                        g9922tcmIsdnOverlapped(11),
                        g9921tcmIsdnSymmetric(12),
                        reserved1(13),
                        reserved2(14),
                        reserved3(15),
                        reserved4(16),
                        reserved5(17),
                        g9923PotsNonOverlapped(18),
                        g9923PotsOverlapped(19),
                        g9923IsdnNonOverlapped(20),
                        g9923isdnOverlapped(21),
                        reserved6(22),
                        reserved7(23),
                        g9924potsNonOverlapped(24),
                        g9924potsOverlapped(25),
                        reserved8(26),
                        reserved9(27),
                        g9923AnnexIAllDigNonOverlapped(28),
                        g9923AnnexIAllDigOverlapped(29),
                        g9923AnnexJAllDigNonOverlapped(30),
                        g9923AnnexJAllDigOverlapped(31),
                        g9924AnnexIAllDigNonOverlapped(32),
                        g9924AnnexIAllDigOverlapped(33),
                        g9923AnnexLMode1NonOverlapped(34),
                        g9923AnnexLMode2NonOverlapped(35),
                        g9923AnnexLMode3Overlapped(36),
                        g9923AnnexLMode4Overlapped(37),
                        g9923AnnexMPotsNonOverlapped(38),
                        g9923AnnexMPotsOverlapped(39),
                        g9925PotsNonOverlapped(40),
                        g9925PotsOverlapped(41),
                        g9925IsdnNonOverlapped(42),
                        g9925isdnOverlapped(43),
                        reserved10(44),
                        reserved11(45),
                        g9925AnnexIAllDigNonOverlapped(46),
                        g9925AnnexIAllDigOverlapped(47),
                        g9925AnnexJAllDigNonOverlapped(48),
                        g9925AnnexJAllDigOverlapped(49),
                        g9925AnnexMPotsNonOverlapped(50),
                        g9925AnnexMPotsOverlapped(51),
                        reserved12(52),
                        reserved13(53),
                        reserved14(54),
                        reserved15(55)
                    }

Adsl2RaMode ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Specifies the rate adaptation behavior for the line.
        The three possible behaviors are:
         manual(1)    - No Rate-Adaptation.  The initialization
                        process attempts to synchronize to a
                        specified rate.
         raInit(2)    - Rate-Adaptation during initialization process
                        only, which attempts to synchronize to a rate
                        between minimum and maximum specified values.
         dynamicRa(3) - Dynamic Rate-Adaptation during initialization
                        process as well as during SHOWTIME."
    SYNTAX          INTEGER  {
                        manual(1),
                        raInit(2),
                        dynamicRa(3)
                    }

Adsl2InitResult ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Specifies the result of a full initialization attempt; the
        six possible result values are:
         noFail(0)            - Successful initialization.
         configError(1)       - Configuration failure.
         configNotFeasible(2) - Configuration details not supported.
         commFail(3)          - Communication failure.
         noPeerAtu(4)         - Peer ATU not detected.
         otherCause(5)        - Other initialization failure reason.

        The values used are as defined in ITU-T G.997.1,
        paragraph 7.5.1.3"
    SYNTAX          INTEGER  {
                        noFail(0),
                        configError(1),
                        configNotFeasible(2),
                        commFail(3),
                        noPeerAtu(4),
                        otherCause(5)
                    }

Adsl2OperationModes ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "The ADSL2 management model specified includes an ADSL Mode
        attribute that identifies an instance of ADSL Mode-Specific
        PSD Configuration object in the ADSL Line Profile.  The
        following classes of ADSL operating mode are defined.
        The notes (F) and (L) denote Full-Rate and Lite/splitterless
        respectively:

        +-------+--------------------------------------------------+
        | Value |         ADSL operation mode description          |
        +-------+--------------------------------------------------+

            1   - The default/generic PSD configuration.  Default
                  configuration will be used when no other matching
                  mode-specific configuration can be found.
            2   - ADSL family.  The attributes included in the Mode-
                  Specific PSD Configuration are irrelevant for
                  ITU-T G.992.1 and G.992.2 ADSL modes.  Hence, it
                  is possible to map those modes to this generic
                  class.
           3-7  - Unused. Reserved for future ITU-T specification.
            8   - G.992.3 POTS non-overlapped (F)
            9   - G.992.3 POTS overlapped (F)
           10   - G.992.3 ISDN non-overlapped (F)
           11   - G.992.3 ISDN overlapped (F)
         12-13  - Unused. Reserved for future ITU-T specification.
           14   - G.992.4 POTS non-overlapped (L)
           15   - G.992.4 POTS overlapped (L)
         16-17  - Unused. Reserved for future ITU-T specification.
           18   - G.992.3 Annex I All-Digital non-overlapped (F)
           19   - G.992.3 Annex I All-Digital overlapped (F)
           20   - G.992.3 Annex J All-Digital non-overlapped (F)
           21   - G.992.3 Annex J All-Digital overlapped (F)
           22   - G.992.4 Annex I All-Digital non-overlapped (L)
           23   - G.992.4 Annex I All-Digital overlapped (L)
           24   - G.992.3 Annex L POTS non-overlapped, mode 1,
                  wide U/S (F)
           25   - G.992.3 Annex L POTS non-overlapped, mode 2,
                  narrow U/S(F)
           26   - G.992.3 Annex L POTS overlapped, mode 3,
                  wide U/S (F)
           27   - G.992.3 Annex L POTS overlapped, mode 4,
                  narrow U/S (F)
           28   - G.992.3 Annex M POTS non-overlapped (F)
           29   - G.992.3 Annex M POTS overlapped (F)
           30   - G.992.5 POTS non-overlapped (F)
           31   - G.992.5 POTS overlapped (F)
           32   - G.992.5 ISDN non-overlapped (F)
           33   - G.992.5 ISDN overlapped (F)
         34-35  - Unused. Reserved for future ITU-T specification.
           36   - G.992.5 Annex I All-Digital non-overlapped (F)
           37   - G.992.5 Annex I All-Digital overlapped (F)
           38   - G.992.5 Annex J All-Digital non-overlapped (F)
           39   - G.992.5 Annex J All-Digital overlapped (F)
           40   - G.992.5 Annex M POTS non-overlapped (F)
           41   - G.992.5 Annex M POTS overlapped (F)"
    SYNTAX          INTEGER  {
                        defMode(1),
                        adsl(2),
                        g9923PotsNonOverlapped(8),
                        g9923PotsOverlapped(9),
                        g9923IsdnNonOverlapped(10),
                        g9923isdnOverlapped(11),
                        g9924potsNonOverlapped(14),
                        g9924potsOverlapped(15),
                        g9923AnnexIAllDigNonOverlapped(18),
                        g9923AnnexIAllDigOverlapped(19),
                        g9923AnnexJAllDigNonOverlapped(20),
                        g9923AnnexJAllDigOverlapped(21),
                        g9924AnnexIAllDigNonOverlapped(22),
                        g9924AnnexIAllDigOverlapped(23),
                        g9923AnnexLMode1NonOverlapped(24),
                        g9923AnnexLMode2NonOverlapped(25),
                        g9923AnnexLMode3Overlapped(26),
                        g9923AnnexLMode4Overlapped(27),
                        g9923AnnexMPotsNonOverlapped(28),
                        g9923AnnexMPotsOverlapped(29),
                        g9925PotsNonOverlapped(30),
                        g9925PotsOverlapped(31),
                        g9925IsdnNonOverlapped(32),
                        g9925isdnOverlapped(33),
                        g9925AnnexIAllDigNonOverlapped(36),
                        g9925AnnexIAllDigOverlapped(37),
                        g9925AnnexJAllDigNonOverlapped(38),
                        g9925AnnexJAllDigOverlapped(39),
                        g9925AnnexMPotsNonOverlapped(40),
                        g9925AnnexMPotsOverlapped(41)
                    }

Adsl2PowerMngState ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Attributes with this syntax uniquely identify each power
        management state defined for the ADSL/ADSL2 or ADSL2+ link.
        The possible values are:
          l0(1) - L0 - Full power management state.
          l1(2) - L1 - Low power management state (for G.992.2).
          l2(3) - L2 - Low power management state (for G.992.3,
                       G.992.4, and G.992.5).
          l3(4) - L3 - Idle power management state."
    SYNTAX          INTEGER  {
                        l0(1),
                        l1(2),
                        l2(3),
                        l3(4)
                    }

Adsl2ConfPmsForce ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Attributes with this syntax are configuration parameters
        that reference the desired power management state for the
        ADSL/ADSL2 or ADSL2+ link:
          l3toL0(0)          - Perform a transition from L3 to L0
                               (Full power management state).
          l0toL2(2)          - Perform a transition from L0 to L2
                               (Low power management state).
          l0orL2toL3(3)      - Perform a transition into L3 (Idle
                               power management state).

        The values used are as defined in ITU-T G.997.1,
        paragraph 7.3.1.1.3"
    SYNTAX          INTEGER  {
                        l3toL0(0),
                        l0toL2(2),
                        l0orL2toL3(3)
                    }

Adsl2LConfProfPmMode ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Attributes with this syntax are configuration parameters
        that reference the power modes/states into which the ATU-C or
        ATU-R may autonomously transit.

        It is a BITS structure that allows control of the following
        transit options:
         allowTransitionsToIdle(0)     - XTU may autonomously transit
                                         to idle (L3) state.
         allowTransitionsToLowPower(1) - XTU may autonomously transit
                                         to low-power (L2) state."
    SYNTAX          BITS {
                        allowTransitionsToIdle(0),
                        allowTransitionsToLowPower(1)
                    }

Adsl2LineLdsf ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Attributes with this syntax are configuration parameters
        that control the Loop Diagnostic mode for the ADSL/ADSL2 or
        ADSL2+ link.  The possible values are:
          inhibit(0)  - Inhibit Loop Diagnostic mode.
          force(1)    - Force/Initiate Loop Diagnostic mode.

        The values used are as defined in ITU-T G.997.1,
        paragraph 7.3.1.1.8"
    SYNTAX          INTEGER  {
                        inhibit(0),
                        force(1)
                    }

Adsl2LdsfResult ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Possible failure reasons associated with performing
        a Dual Ended Loop Test (DELT) on a DSL line.
        Possible values are:
         none(1)         - The default value in case LDSF was never
                           requested for the associated line.
         success(2)      - The recent command completed
                           successfully.
         inProgress(3)   - The Loop Diagnostics process is in
                           progress.
         unsupported(4)  - The NE or the line card doesn't support
                           LDSF.
         cannotRun(5)    - The NE cannot initiate the command, due
                           to a nonspecific reason.
         aborted(6)      - The Loop Diagnostics process aborted.
         failed(7)       - The Loop Diagnostics process failed.
         illegalMode(8)  - The NE cannot initiate the command, due
                           to the specific mode of the relevant
                           line.
         adminUp(9)      - The NE cannot initiate the command, as
                           the relevant line is administratively
                           'Up'.
         tableFull(10)   - The NE cannot initiate the command, due
                           to reaching the maximum number of rows
                           in the results table.
         noResources(11) - The NE cannot initiate the command, due
                           to lack of internal memory resources."
    SYNTAX          INTEGER  {
                        none(1),
                        success(2),
                        inProgress(3),
                        unsupported(4),
                        cannotRun(5),
                        aborted(6),
                        failed(7),
                        illegalMode(8),
                        adminUp(9),
                        tableFull(10),
                        noResources(11)
                    }

Adsl2SymbolProtection ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Attributes with this syntax are configuration parameters
        that reference the minimum-length impulse noise protection
        (INP) in terms of number of symbols.  The possible values are:
        noProtection (i.e., INP not required), halfSymbol (i.e., INP
        length is 1/2 symbol), and 1-16 symbols in steps of 1 symbol."
    SYNTAX          INTEGER  {
                        noProtection(1),
                        halfSymbol(2),
                        singleSymbol(3),
                        twoSymbols(4),
                        threeSymbols(5),
                        fourSymbols(6),
                        fiveSymbols(7),
                        sixSymbols(8),
                        sevenSymbols(9),
                        eightSymbols(10),
                        nineSymbols(11),
                        tenSymbols(12),
                        elevenSymbols(13),
                        twelveSymbols(14),
                        thirteeSymbols(15),
                        fourteenSymbols(16),
                        fifteenSymbols(17),
                        sixteenSymbols(18)
                    }

Adsl2MaxBer ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Attributes with this syntax are configuration parameters
        that reference the maximum Bit Error Rate (BER).
        The possible values are:

          eminus3(1)   - Maximum BER=E^-3
          eminus5(2)   - Maximum BER=E^-5
          eminus7(3)   - Maximum BER=E^-7"
    SYNTAX          INTEGER  {
                        eminus3(1),
                        eminus5(2),
                        eminus7(3)
                    }

Adsl2ScMaskDs ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Each one of the 512 bits in this OCTET
        STRING array represents the corresponding bin
        in the downstream direction.  A value of one
        indicates that the bin is not in use."
    SYNTAX          OCTET STRING (SIZE (0..64))

Adsl2ScMaskUs ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Each one of the 64 bits in this OCTET
        STRING array represents the corresponding bin
        in the upstream direction.  A value of one
        indicates that the bin is not in use."
    SYNTAX          OCTET STRING (SIZE (0..8))

Adsl2RfiDs ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Each one of the 512 bits in this OCTET
        STRING array represents the corresponding bin
        in the downstream direction.  A value of one
        indicates that the bin is part of a notch
        filter."
    SYNTAX          OCTET STRING (SIZE (0..64))

Adsl2PsdMaskDs ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This is a structure that represents up to
        32 PSD Mask breakpoints.
        Each breakpoint occupies 3 octets: The first
        two octets hold the index of the sub-carrier
        associated with the breakpoint.  The third octet
        holds the PSD reduction at the breakpoint from 0
        (0 dBm/Hz) to 255 (-127.5 dBm/Hz) using units of
        0.5 dBm/Hz."
    SYNTAX          OCTET STRING (SIZE (0..96))

Adsl2PsdMaskUs ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This is a structure that represents up to
        4 PSD Mask breakpoints.
        Each breakpoint occupies 3 octets: The first
        two octets hold the index of the sub-carrier
        associated with the breakpoint.  The third octet
        holds the PSD reduction at the breakpoint from 0
        (0 dBm/Hz) to 255 (-127.5 dBm/Hz) using units of
        0.5 dBm/Hz."
    SYNTAX          OCTET STRING (SIZE (0..12))

Adsl2Tssi ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This is a structure that represents up to
        32 transmit spectrum shaping (TSSi) breakpoints.
        Each breakpoint occupies 3 octets: The first
        two octets hold the index of the sub-carrier
        associated with the breakpoint.  The third octet
        holds the shaping parameter at the breakpoint.  It
        is a value from 0 to 127 (units of -0.5 dB).  The
        special value 127 indicates that the sub-carrier
        is not transmitted."
    SYNTAX          OCTET STRING (SIZE (0..96))

Adsl2LastTransmittedState ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This parameter represents the last successfully
        transmitted initialization state in the last full
        initialization performed on the line.  States are
        per the specific xDSL technology and are numbered
        from 0 (if G.994.1 is used) or 1 (if G.994.1 is
        not used) up to Showtime."
    SYNTAX          INTEGER  {
                        atucG9941(0),
                        atucQuiet1(1),
                        atucComb1(2),
                        atucQuiet2(3),
                        atucComb2(4),
                        atucIcomb1(5),
                        atucLineprob(6),
                        atucQuiet3(7),
                        atucComb3(8),
                        atucIComb2(9),
                        atucMsgfmt(10),
                        atucMsgpcb(11),
                        atucQuiet4(12),
                        atucReverb1(13),
                        atucTref1(14),
                        atucReverb2(15),
                        atucEct(16),
                        atucReverb3(17),
                        atucTref2(18),
                        atucReverb4(19),
                        atucSegue1(20),
                        atucMsg1(21),
                        atucReverb5(22),
                        atucSegue2(23),
                        atucMedley(24),
                        atucExchmarker(25),
                        atucMsg2(26),
                        atucReverb6(27),
                        atucSegue3(28),
                        atucParams(29),
                        atucReverb7(30),
                        atucSegue4(31),
                        atucShowtime(32),
                        aturG9941(100),
                        aturQuiet1(101),
                        aturComb1(102),
                        aturQuiet2(103),
                        aturComb2(104),
                        aturIcomb1(105),
                        aturLineprob(106),
                        aturQuiet3(107),
                        aturComb3(108),
                        aturIcomb2(109),
                        aturMsgfmt(110),
                        aturMsgpcb(111),
                        aturReverb1(112),
                        aturQuiet4(113),
                        aturReverb2(114),
                        aturQuiet5(115),
                        aturReverb3(116),
                        aturEct(117),
                        aturReverb4(118),
                        aturSegue1(119),
                        aturReverb5(120),
                        aturSegue2(121),
                        aturMsg1(122),
                        aturMedley(123),
                        aturExchmarker(124),
                        aturMsg2(125),
                        aturReverb6(126),
                        aturSegue3(127),
                        aturParams(128),
                        aturReverb7(129),
                        aturSegue4(130),
                        aturShowtime(131)
                    }

Adsl2LineStatus ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Attributes with this syntax are status parameters
        that reflect the failure status for a given endpoint of
        ADSL/ADSL2 or ADSL2+ link.

        This BITS structure can report the following failures:

         noDefect(0)       - This bit position positively reports
                             that no defect or failure exists.
         lossOfFrame(1)    - Loss of frame synchronization.
         lossOfSignal(2)   - Loss of signal.
         lossOfPower(3)    - Loss of power.  Usually this failure may
                             be reported for ATU-Rs only.
         initFailure(4)    - Recent initialization process failed.
                             Never active on ATU-R."
    SYNTAX          BITS {
                        noDefect(0),
                        lossOfFrame(1),
                        lossOfSignal(2),
                        lossOfPower(3),
                        initFailure(4)
                    }

Adsl2ChAtmStatus ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Attributes with this syntax are status parameters that
        reflect the failure status for Transmission Convergence (TC)
        layer of a given ATM interface (data path over an ADSL/ADSL2
        or ADSL2+ link).

        This BITS structure can report the following failures:
         noDefect(0)              - This bit position positively
                                    reports that no defect or failure
                                    exists.
         noCellDelineation(1)     - The link was successfully
                                    initialized, but cell delineation
                                    was never acquired on the
                                    associated ATM data path.
         lossOfCellDelineation(2) - Loss of cell delineation on the
                                    associated ATM data path."
    SYNTAX          BITS {
                        noDefect(0),
                        noCellDelineation(1),
                        lossOfCellDelineation(2)
                    }

Adsl2ChPtmStatus ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Attributes with this syntax are status parameters that
        reflect the failure status for a given PTM interface (packet
        data path over an ADSL/ADSL2 or ADSL2+ link).

        This BITS structure can report the following failures:
            noDefect(0)     - This bit position positively
                              reports that no defect or failure exists.
            outOfSync(1)    - Out of synchronization."
    SYNTAX          BITS {
                        noDefect(0),
                        outOfSync(1)
                    }

END



