EXTREME-DLCS-MIB DEFINITIONS ::= BEGIN

    IMPORTS
                MODULE-IDENTITY, OBJECT-TYPE, IpAddress, TimeTicks
                                FROM SNMPv2-SMI
                TruthValue      FROM SNMPv2-TC
        DisplayString   FROM RFC1213-MIB
                extremeAgent
                                FROM EXTREME-BASE-MIB;

        extremeDlcs MODULE-IDENTITY
                LAST-UPDATED "9903040000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION 
                        "Extreme Dynamic-Link Context System (DLCS) status objects"
        ::= { extremeAgent 8 }


--
-- Enable/disable DLCS
--
    extremeDlcsEnable OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
                      "Setting this to true will allow the agent to start 
                        collecting DLCS binding information."
    ::= { extremeDlcs 1 }

    extremeDlcsNetbiosEnable OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
                      "Setting this to true will allow the agent to start 
                        collecting DLCS binding information using the
                        NetBios protocol."
    ::= { extremeDlcs 2 }

    extremeDlcsKerberos5Enable OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
                      "Setting this to true will allow the agent to start 
                        collecting DLCS binding information using the
                        Kerberos V5 protocol."
    ::= { extremeDlcs 3 }

    extremeDlcsRsvpEnable OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
                      "Setting this to true will allow the agent to start 
                        collecting DLCS binding information using the RSVP
                        protocol."
    ::= { extremeDlcs 4 }

    extremeDlcsDnsEnable OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
                      "Setting this to true will allow the agent to start 
                        collecting DLCS binding information using the
                        DNS protocol."
    ::= { extremeDlcs 5 }

--
-- DLCS Binding Table
--
--
-- How is this table used?
-- 
-- (1) Manager creates extremeSmartTrapRulesEntry with
-- extremeSmartTrapRulesIndex = XXXX
-- extremeSmartTrapRulesDesiredOID = extremeDlcsBindingTable
-- extremeSmartTrapRulesOperation = any
-- 
-- (2) Events are reported by agent creating a extremeSmartTrapInstanceEntry with:
-- 
-- extremeSmartTrapInstanceRule = XXXX
-- extremeSmartTrapInstanceChangedOid = extremeDlcsBindingIndex
-- extremeSmartTrapInstanceActualOperation = add, delete or modify
-- 
-- and generating the actual trap.
-- 

        extremeDlcsBindingTable OBJECT-TYPE
         SYNTAX      SEQUENCE OF ExtremeDlcsBindingEntry
        MAX-ACCESS  not-accessible
        STATUS      current
                DESCRIPTION
                "Table of DLCS Binding information. Entries are added and deleted
                by the agent based on information gathered from the local network 
                environment. Multiple entries may exist for almost identical sets
                of bindings although the agent will ensure that exactly matching
                entries are coalesced."
    ::= { extremeDlcs 6 }

        extremeDlcsBindingEntry OBJECT-TYPE
        SYNTAX  ExtremeDlcsBindingEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
                "Entry in table of DLCS bindings."
               INDEX { extremeDlcsBindingIndex } 
    ::= { extremeDlcsBindingTable 1 }

        ExtremeDlcsBindingEntry ::= SEQUENCE
        {
                extremeDlcsBindingIndex         INTEGER,
                extremeDlcsBindingType          BITS,
                extremeDlcsBindingSource        INTEGER,
                extremeDlcsBindingUser          DisplayString,
                extremeDlcsBindingGroup         DisplayString,
                extremeDlcsBindingApplication   DisplayString,
                extremeDlcsBindingHost          DisplayString,
                extremeDlcsBindingIpAddress     IpAddress,
                extremeDlcsBindingPhysPort      INTEGER,
                extremeDlcsBindingUpdateTime    TimeTicks
        }

        extremeDlcsBindingIndex  OBJECT-TYPE
            SYNTAX INTEGER
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "An index into this table, chosen by the agent. This has
                no significance to the manager beyond its uniqueness
                within this agent."
    ::= { extremeDlcsBindingEntry 1 }

        extremeDlcsBindingType  OBJECT-TYPE
            SYNTAX  BITS { user2ip(0), user2port(1), ip2port(2), 
                           application2user(3), application2ip(4), 
                           host2ip(5), group2ip(6), group2port(7), 
                           user2group(8) }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The type of binding expressed here. A given bit is set if DLCS
                has detected that the two relevant items are bound together. 
                e.g. an entry with application2user(3) set to 1 implies that
                the username extremeDlcsBindingUser has been seen to be using 
                the application extremeDlcsBindingApplication. In addition, if
                this entry also has user2port(1) set to 1 then this user and
                application have been detected as running on the physical
                switch port extremeDlcsBindingPhysPort."
    ::= { extremeDlcsBindingEntry 2 }

        extremeDlcsBindingSource  OBJECT-TYPE
            SYNTAX  INTEGER { other (1), local(2), netbiosquery(3),
             netbiosbind (4), dns(5), kerberos5(6), rsvp(7) }
            MAX-ACCESS  read-only
            STATUS  current
            DESCRIPTION
                "The source of the information binding."
    ::= { extremeDlcsBindingEntry 3 }

        extremeDlcsBindingUser  OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The User name detected by DLCS. A string of length zero
         indicates no valid User name has been detected for this
         binding."
    ::= { extremeDlcsBindingEntry 4 }

        extremeDlcsBindingGroup  OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The Group name detected by DLCS. A string of length zero
                 indicates no valid Group name has been detected for this
         binding."
    ::= { extremeDlcsBindingEntry 5 }

        extremeDlcsBindingApplication  OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The Application name detected by DLCS. A string of length 
                zero indicates no valid Application name has been detected 
                for this binding."
    ::= { extremeDlcsBindingEntry 6 }

        extremeDlcsBindingHost  OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The Host name detected by DLCS. A string of length 
                zero indicates no valid Host name has been detected 
                for this binding."
    ::= { extremeDlcsBindingEntry 7 }

        extremeDlcsBindingIpAddress  OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The IP address detected by DLCS. A value of 0.0.0.0
                indicates no valid IP address has been detected 
                for this binding."
    ::= { extremeDlcsBindingEntry 8 }

        extremeDlcsBindingPhysPort  OBJECT-TYPE
            SYNTAX INTEGER
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The physical port number (ifIndex) detected by DLCS.
                This is valid in all bindings."
    ::= { extremeDlcsBindingEntry 9 }

        extremeDlcsBindingUpdateTime  OBJECT-TYPE
            SYNTAX TimeTicks
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of sysUpTime when this entry was last updated."
    ::= { extremeDlcsBindingEntry 10 }

END

-- ################################################################################

