    EXTREME-SNMPV3-MIB DEFINITIONS ::= BEGIN

    IMPORTS  
                MODULE-IDENTITY                 FROM SNMPv2-SMI
                OBJECT-TYPE                     FROM SNMPv2-SMI
                TruthValue                      FROM SNMPv2-TC
                extremeAgent                    FROM EXTREME-BASE-MIB
                snmpTargetAddrEntry             FROM SNMP-TARGET-MIB;

            
        extremeSnmpv3 MODULE-IDENTITY
                LAST-UPDATED "0007240000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme-specific SNMPv3 objects"
        ::= { extremeAgent 23 }

        extremeTarget   OBJECT IDENTIFIER ::= { extremeSnmpv3 1 }
        
        extremeTargetAddrExtTable OBJECT-TYPE
                SYNTAX  SEQUENCE OF ExtremeTargetAddrExtEntry
                MAX-ACCESS  not-accessible
                STATUS current
                DESCRIPTION
                "This table is an extension to the snmpTargetAddrTable found in the 
                SNMP-TARGET-MIB. It contains Extreme Networks specific objects needed for
                each management target."
                        ::= { extremeTarget 1 }

        extremeTargetAddrExtEntry OBJECT-TYPE
                SYNTAX  ExtremeTargetAddrExtEntry
                MAX-ACCESS  not-accessible
                STATUS current
                DESCRIPTION
                "An entry in the extremeTargetAddrExtTable."
                AUGMENTS { snmpTargetAddrEntry }
                        ::= { extremeTargetAddrExtTable 1 }

        ExtremeTargetAddrExtEntry ::= SEQUENCE {
                extremeTargetAddrExtIgnoreMPModel               TruthValue,
                extremeTargetAddrExtStandardMode                TruthValue,
                extremeTargetAddrExtTrapDestIndex               Integer32,
                extremeTargetAddrExtUseEventComm                TruthValue
        }
        
        
        extremeTargetAddrExtIgnoreMPModel OBJECT-TYPE
                SYNTAX TruthValue
                MAX-ACCESS read-write
                STATUS current
                DESCRIPTION
                "When this object is set to TRUE, the version of the trap/notification sent to 
                the corresponding management target (trap receiver) will be the same as in 
                releases of Extremeware prior to 7.1.0. Thus, the value of the 
                snmpTargetParamsMPModel object in the snmpTargetParamsTable will be ignored while
                determining the version of the trap/notification to be sent. When a trap-receiver
                is created via the RMON trapDestTable or from the CLI command 'configure snmp add
                trapreceiver ....', the value of this object will be set to TRUE for the 
                corresponding entry in this table."
                DEFVAL { false }
                ::= { extremeTargetAddrExtEntry 1 }

        extremeTargetAddrExtStandardMode OBJECT-TYPE
                SYNTAX TruthValue
                MAX-ACCESS read-write
                STATUS current
                DESCRIPTION
                "When this object is set to TRUE, the management target will be treated as 
                a 'standard mode' one, in that any Extreme Networks specific extra varbinds 
                present in a standards-based trap/notification will not be sent to this 
                management target. Only the varbinds defined in the standard will be sent."
                DEFVAL { false }
                ::= { extremeTargetAddrExtEntry 2 }

        extremeTargetAddrExtTrapDestIndex OBJECT-TYPE
                SYNTAX Integer32
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "This object contains the value of the trapDestIndex in the corresponding 
                entry of the RMON trapDestTable."
                ::= { extremeTargetAddrExtEntry 3 }

        extremeTargetAddrExtUseEventComm OBJECT-TYPE
                SYNTAX TruthValue
                MAX-ACCESS read-write
                STATUS current
                DESCRIPTION
                "This object is used only when sending RMON alarms as SNMPv3 traps.
                When it is set to TRUE and an RMON risingAlarm or fallingAlarm is being sent
                for an event, then the eventCommunity in the RMON event table is compared to 
                the snmpTargetAddrName in the snmpTargetAddrTable. The alarm is sent to the 
                target only when the two are the same. This behavior is exhibited only when the
                snmpTargetParamsMPModel corresponding to the target indicates an SNMPv3 trap. For 
                SNMPv1/v2c traps, the community in the RMON trapDestTable is used for the 
                comparision, which is the 'regular' method, as per the standards.
                When this object is set to FALSE, then the RMON alarm (if being sent as an SNMPv3
                trap) is sent without using the event community for any comparision."
                DEFVAL { true }        
                ::= { extremeTargetAddrExtEntry 4 }
    
END


-- ################################################################################

