# -----------------------------------------------------------------------------
# APC PowerNet & RFC 1628 UPS Trap Definition File
# -----------------------------------------------------------------------------
# Copyright (c) 2007 American Power Conversion, Inc.
#
# Name : apctraps387.fmt
#
# Generated by script: tofmt.awk
#
# Input File: powernetPS.mib
#
# Created: Wednesday, January, 03, 2007
#
# Revision History:
# -----------------------------------------------------------------------------
#
#
# Enterprise ID's
#
OID_ALIAS APC_PowerNet .1.3.6.1.4.1.318
#
# APC PowerNet Traps
#
#
#
EVENT communicationLost .1.3.6.1.4.1.318.0.1 "Status Events" Critical
FORMAT APC UPS: Communication lost, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communication lost between the agent and the UPS.
EDESC
#
#
#
EVENT upsOverload .1.3.6.1.4.1.318.0.2 "Status Events" Critical
FORMAT APC UPS: Overload, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS has sensed a load greater than 100 percent of its rated capacity.
EDESC
#
#
#
EVENT upsDiagnosticsFailed .1.3.6.1.4.1.318.0.3 "Status Events" Critical
FORMAT APC UPS: Failed self-test, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS has failed its internal self-test.
EDESC
#
#
#
EVENT upsDischarged .1.3.6.1.4.1.318.0.4 "Status Events" Critical
FORMAT APC UPS: batteries are discharged, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS batteries are discharged.
EDESC
#
#
#
EVENT upsOnBattery .1.3.6.1.4.1.318.0.5 "Status Events" Minor
FORMAT APC UPS: On battery, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS has switched to battery backup power.
EDESC
#
#
#
EVENT smartBoostOn .1.3.6.1.4.1.318.0.6 "Status Events" Minor
FORMAT APC UPS: SmartBoost(TM), Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS has enabled SmartBoost(TM); low incoming line voltage.
EDESC
#
#
#
EVENT lowBattery .1.3.6.1.4.1.318.0.7 "Status Events" Critical
FORMAT APC UPS: Low battery, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS system's batteries are low and will soon be exhausted.
EDESC
#
#
#
EVENT communicationEstablished .1.3.6.1.4.1.318.0.8 "Status Events" Normal
FORMAT APC UPS: Communication established, Trap Arguments:($#):$* [APC PowerNet]
SDESC
UPS communication has been established.
EDESC
#
#
#
EVENT powerRestored .1.3.6.1.4.1.318.0.9 "Status Events" Normal
FORMAT APC UPS: Utility power restored, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Returned from battery backup power; utility power restored.
EDESC
#
#
#
EVENT upsDiagnosticsPassed .1.3.6.1.4.1.318.0.10 "Status Events" Normal
FORMAT APC UPS: Passed self-test, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS passed internal self-test.
EDESC
#
#
#
EVENT returnFromLowBattery .1.3.6.1.4.1.318.0.11 "Status Events" Normal
FORMAT APC UPS: Returned from Low-Battery condition, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS has returned from a Low-Battery condition.
EDESC
#
#
#
EVENT upsTurnedOff .1.3.6.1.4.1.318.0.12 "Status Events" Minor
FORMAT APC UPS: Turned off, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS has been switched off by a management station.
EDESC
#
#
#
EVENT upsSleeping .1.3.6.1.4.1.318.0.13 "Status Events" Minor
FORMAT APC UPS: Entered sleep mode, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS entered sleep mode. Power to the load will be cut off.
EDESC
#
#
#
EVENT upsWokeUp .1.3.6.1.4.1.318.0.14 "Status Events" Normal
FORMAT APC UPS: Wake up, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS has returned from sleep mode. Power to the load has been restored.
EDESC
#
#
#
EVENT upsRebootStarted .1.3.6.1.4.1.318.0.15 "Status Events" Minor
FORMAT APC UPS: Starting reboot, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS has started its reboot sequence.
EDESC
#
#
#
EVENT upsDipSwitchChanged .1.3.6.1.4.1.318.0.16 "Status Events" Minor
FORMAT APC UPS: DIP switch altered, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The DIP switch settings on the UPS have been changed.
EDESC
#
#
#
EVENT upsBatteryNeedsReplacement .1.3.6.1.4.1.318.0.17 "Status Events" Critical
FORMAT APC UPS: UPS batteries need replacement, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS batteries require immediate replacement.
EDESC
#
#
#
EVENT contactFault .1.3.6.1.4.1.318.0.18 "Status Events" Critical
FORMAT APC Environment: Contact $1 fault, Trap Arguments:($#):$* [APC PowerNet]
SDESC
An Environment contact $1 closure has faulted.
EDESC
#
#
#
EVENT contactFaultResolved .1.3.6.1.4.1.318.0.19 "Status Events" Normal
FORMAT APC Environment: Contact $1 fault cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A Environment contact $1 closure has returned to it's default state.
EDESC
#
#
#
EVENT hardwareFailureBypass .1.3.6.1.4.1.318.0.20 "Status Events" Critical
FORMAT APC UPS: On bypass due to internal fault, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS is on bypass due to an internal fault.
EDESC
#
#
#
EVENT softwareBypass .1.3.6.1.4.1.318.0.21 "Status Events" Minor
FORMAT APC UPS: On bypass by user via software or panel, Trap Arguments:($#):$* [APC PowerNet]
SDESC
UPS put on bypass by user via software or front UPS panel.
EDESC
#
#
#
EVENT switchedBypass .1.3.6.1.4.1.318.0.22 "Status Events" Minor
FORMAT APC UPS: On bypass initiated by user, Trap Arguments:($#):$* [APC PowerNet]
SDESC
UPS put on bypass by user.
EDESC
#
#
#
EVENT returnFromBypass .1.3.6.1.4.1.318.0.23 "Status Events" Normal
FORMAT APC UPS: UPS has returned from bypass, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS has returned from bypass mode.
EDESC
#
#
#
EVENT bypassPowerSupplyFailure .1.3.6.1.4.1.318.0.24 "Status Events" Critical
FORMAT APC UPS: Base module bypass power supply needs repair, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The base module bypass power supply needs repair.
EDESC
#
#
#
EVENT baseFanFailure .1.3.6.1.4.1.318.0.25 "Status Events" Critical
FORMAT APC UPS: Base module fan needs repair, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The base module fan needs repair.
EDESC
#
#
#
EVENT batteryPackCommLost .1.3.6.1.4.1.318.0.26 "Status Events" Critical
FORMAT APC UPS: Communication lost with battery packs, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communication lost with external battery packs, check battery signal cable.
EDESC
#
#
#
EVENT batteryPackCommEstablished .1.3.6.1.4.1.318.0.27 "Status Events" Normal
FORMAT APC UPS: Communication established with battery packs, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communication established with external battery packs.
EDESC
#
#
#
EVENT calibrationStart .1.3.6.1.4.1.318.0.28 "Status Events" Normal
FORMAT APC UPS: Calibration initiated, Trap Arguments:($#):$* [APC PowerNet]
SDESC
A battery run time calibration test has been initiated.
EDESC
#
#
#
EVENT restartAgent .1.3.6.1.4.1.318.0.29 "Status Events" Normal
FORMAT APC SNMP Agent: Agent restarting, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Agent restarting as commanded by manager.
EDESC
#
#
#
EVENT upsTurnedOn .1.3.6.1.4.1.318.0.30 "Status Events" Normal
FORMAT APC UPS: A UPS is turned on., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A UPS is turned on.
EDESC
#
#
#
EVENT smartAvrReducing .1.3.6.1.4.1.318.0.31 "Status Events" Minor
FORMAT APC UPS: SmartTrim(TM) reducing, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS has enabled SmartTrim(TM) voltage reduction.
EDESC
#
#
#
EVENT codeAuthenticationDone .1.3.6.1.4.1.318.0.32 "Status Events" Normal
FORMAT APC CODE: Authentication on agent code image is done., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Authentication on agent code image is done.
EDESC
#
#
#
EVENT upsOverloadCleared .1.3.6.1.4.1.318.0.33 "Status Events" Normal
FORMAT APC UPS: Overload cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The overload condition has been cleared. .
EDESC
#
#
#
EVENT smartBoostOff .1.3.6.1.4.1.318.0.34 "Status Events" Normal
FORMAT APC UPS: SmartBoost(TM) off., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS has returned from SmartBoost(TM).
EDESC
#
#
#
EVENT smartAvrReducingOff .1.3.6.1.4.1.318.0.35 "Status Events" Normal
FORMAT APC UPS: SmartTrim(TM) reducing off, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS has returned from SmartTrim(TM) voltage reduction.
EDESC
#
#
#
EVENT upsBatteryReplaced .1.3.6.1.4.1.318.0.36 "Status Events" Normal
FORMAT APC UPS: Bad battery replaced, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS has returned from a bad battery fault.
EDESC
#
#
#
EVENT calibrationEnd .1.3.6.1.4.1.318.0.37 "Status Events" Normal
FORMAT APC UPS: Calibration end, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS has finished calibrating
EDESC
#
#
#
EVENT dischargeCleared .1.3.6.1.4.1.318.0.38 "Status Events" Normal
FORMAT APC UPS: Discharge cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS discharge condition has been cleared.
EDESC
#
#
#
EVENT gracefullShutdown .1.3.6.1.4.1.318.0.39 "Status Events" Normal
FORMAT APC UPS: A graceful shutdown has been initiated., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A graceful shutdown has been initiated.
EDESC
#
#
#
EVENT outletOn .1.3.6.1.4.1.318.0.41 "Status Events" Minor
FORMAT APC PDU: Outlet $1 has been turned on., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Outlet $1 has been turned on
EDESC
#
#
#
EVENT outletOff .1.3.6.1.4.1.318.0.42 "Status Events" Minor
FORMAT APC PDU: Outlet $1 has turned off., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Outlet $1 has turned off.
EDESC
#
#
#
EVENT outletReboot .1.3.6.1.4.1.318.0.43 "Status Events" Minor
FORMAT APC PDU: Outlet $1 has rebooted., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Outlet $1 has rebooted.
EDESC
#
#
#
EVENT configChangeSNMP .1.3.6.1.4.1.318.0.44 "Status Events" Minor
FORMAT APC: The SNMP configuration has been changed., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The SNMP configuration has been changed.
EDESC
#
#
#
EVENT configChangeOutlet .1.3.6.1.4.1.318.0.45 "Status Events" Minor
FORMAT APC PDU: Outlet $1 configuration has been changed., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Outlet $1 configuration has been changed.
EDESC
#
#
#
EVENT accessViolationConsole .1.3.6.1.4.1.318.0.46 "Status Events" Minor
FORMAT APC: Access violation via the console., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Three unsuccessful logins have been attempted via the console.
EDESC
#
#
#
EVENT accessViolationHTTP .1.3.6.1.4.1.318.0.47 "Status Events" Minor
FORMAT APC: Access violation via HTTP., Trap Arguments:($#):$* [APC PowerNet]
SDESC
An unsuccessful attempt to login via HTTP.
EDESC
#
#
#
EVENT passwordChange .1.3.6.1.4.1.318.0.48 "Status Events" Minor
FORMAT APC: Password change for the device., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Someone has changed the password on the device.
EDESC
#
#
#
EVENT badVoltage .1.3.6.1.4.1.318.0.49 "Status Events" Minor
FORMAT APC UPS: Bad output voltage., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The output voltage is not within acceptable range.
EDESC
#
#
#
EVENT badVoltageCleared .1.3.6.1.4.1.318.0.50 "Status Events" Normal
FORMAT APC UPS: The bad voltage output condition has been cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The output voltage has returned to an acceptable level.
EDESC
#
#
#
EVENT chargerFailure .1.3.6.1.4.1.318.0.51 "Status Events" Minor
FORMAT APC UPS: The battery charger has failed., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The battery charger has failed.
EDESC
#
#
#
EVENT chargerFailureCleared .1.3.6.1.4.1.318.0.52 "Status Events" Normal
FORMAT APC UPS: The battery charger failure condition cleared, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The battery charger failure condition has been cleared.
EDESC
#
#
#
EVENT batteryOverTemperature .1.3.6.1.4.1.318.0.53 "Status Events" Minor
FORMAT APC UPS: The battery temperature threshold has been violated., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The battery temperature threshold has been violated.
EDESC
#
#
#
EVENT batteryOverTemperatureCleared .1.3.6.1.4.1.318.0.54 "Status Events" Normal
FORMAT APC UPS: The battery over temperature has been cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The battery over temperature has been cleared.
EDESC
#
#
#
EVENT smartRelayFault .1.3.6.1.4.1.318.0.55 "Status Events" Minor
FORMAT APC UPS: SmartBoost(TM) or SmartTrim(TM) relay fault., Trap Arguments:($#):$* [APC PowerNet]
SDESC
SmartBoost(TM) or SmartTrim(TM) relay fault.
EDESC
#
#
#
EVENT smartRelayFaultCleared .1.3.6.1.4.1.318.0.56 "Status Events" Normal
FORMAT APC UPS: SmartBoost(TM) or SmartTrim(TM) relay fault cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
SmartBoost(TM) or SmartTrim(TM) relay fault has been cleared.
EDESC
#
#
#
EVENT humidityThresholdViolation1 .1.3.6.1.4.1.318.0.57 "Status Events" Critical
FORMAT APC Environmental Monitor: Probe 1 humidity threshold violation, Trap Arguments:($#):$* [APC PowerNet]
SDESC
A humidity threshold has been violated on probe 1. Humidity is $1 percent.
EDESC
#
#
#
EVENT humidityThresholdViolationCleared1 .1.3.6.1.4.1.318.0.58 "Status Events" Normal
FORMAT APC Environmental Monitor: Probe 1 humidity violation cleared, Trap Arguments:($#):$* [APC PowerNet]
SDESC
A humidity threshold violation has been cleared on probe 1.
EDESC
#
#
#
EVENT temperatureThresholdViolation1 .1.3.6.1.4.1.318.0.59 "Status Events" Critical
FORMAT APC Environmental Monitor: Probe 1 temperature violation, Trap Arguments:($#):$* [APC PowerNet]
SDESC
A temperature threshold has been violated on probe 1. Temperature is $1.
EDESC
#
#
#
EVENT temperatureThresholdViolationCleared1 .1.3.6.1.4.1.318.0.60 "Status Events" Normal
FORMAT APC Environmental Monitor: Probe 1 temperature violation cleared, Trap Arguments:($#):$* [APC PowerNet]
SDESC
A temperature threshold violation has been cleared on probe 1.
EDESC
#
#
#
EVENT humidityThresholdViolation2 .1.3.6.1.4.1.318.0.61 "Status Events" Critical
FORMAT APC Environmental Monitor: Probe 2 humidity violation, Trap Arguments:($#):$* [APC PowerNet]
SDESC
A humidity threshold has been violated on probe 2. Humidity is $1 percent.
EDESC
#
#
#
EVENT humidityThresholdViolationCleared2 .1.3.6.1.4.1.318.0.62 "Status Events" Normal
FORMAT APC Environmental Monitor: Probe 2 humidity violation cleared, Trap Arguments:($#):$* [APC PowerNet]
SDESC
A humidity threshold violation has been cleared on probe 2.
EDESC
#
#
#
EVENT temperatureThresholdViolation2 .1.3.6.1.4.1.318.0.63 "Status Events" Critical
FORMAT APC Environmental Monitor: Probe 2 temperature violation, Trap Arguments:($#):$* [APC PowerNet]
SDESC
A temperature threshold has been violated on probe 2. Temperature is $1.
EDESC
#
#
#
EVENT temperatureThresholdViolationCleared2 .1.3.6.1.4.1.318.0.64 "Status Events" Normal
FORMAT APC Environmental Monitor: Probe 2 temperature violation cleared, Trap Arguments:($#):$* [APC PowerNet]
SDESC
A temperature threshold violation has been cleared on probe 2.
EDESC
#
#
#
EVENT mupsCommunicationEstablished .1.3.6.1.4.1.318.0.65 "Status Events" Normal
FORMAT APC Environmental Monitor: Communication established, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communication established between the agent and the Environmental Monitor.
EDESC
#
#
#
EVENT mupsCommunicationLost .1.3.6.1.4.1.318.0.66 "Status Events" Critical
FORMAT APC Environmental Monitor: Communication failure, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communication lost between the agent and the Environmental Monitor.
EDESC
#
#
#
EVENT batteryIncrease .1.3.6.1.4.1.318.0.67 "Status Events" Normal
FORMAT APC UPS: The number of batteries has increased., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The number of batteries has increased.
EDESC
#
#
#
EVENT batteryDecrease .1.3.6.1.4.1.318.0.68 "Status Events" Normal
FORMAT APC UPS: The number of batteries has decreased., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The number of batteries has decreased.
EDESC
#
#
#
EVENT powerModuleIncrease .1.3.6.1.4.1.318.0.69 "Status Events" Normal
FORMAT APC UPS: The number of power modules has increased., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The number of power modules has increased.
EDESC
#
#
#
EVENT powerModuleDecrease .1.3.6.1.4.1.318.0.70 "Status Events" Normal
FORMAT APC UPS: The number of power modules has decreased., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The number of power modules has decreased.
EDESC
#
#
#
EVENT intelligenceModuleInserted .1.3.6.1.4.1.318.0.71 "Status Events" Normal
FORMAT APC UPS: An intelligence module has been inserted., Trap Arguments:($#):$* [APC PowerNet]
SDESC
An intelligence module has been inserted.
EDESC
#
#
#
EVENT intelligenceModuleRemoved .1.3.6.1.4.1.318.0.72 "Status Events" Normal
FORMAT APC UPS: An intelligence module has been removed., Trap Arguments:($#):$* [APC PowerNet]
SDESC
An intelligence module has been removed.
EDESC
#
#
#
EVENT rintelligenceModuleInserted .1.3.6.1.4.1.318.0.73 "Status Events" Normal
FORMAT APC UPS: A redundant intelligence module has been inserted., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A redundant intelligence module has been inserted.
EDESC
#
#
#
EVENT rintelligenceModuleRemoved .1.3.6.1.4.1.318.0.74 "Status Events" Normal
FORMAT APC UPS: A redundant intelligence module has been removed., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A redundant intelligence module has been removed.
EDESC
#
#
#
EVENT extBatteryFrameIncease .1.3.6.1.4.1.318.0.75 "Status Events" Normal
FORMAT APC UPS: An external battery frame has been added., Trap Arguments:($#):$* [APC PowerNet]
SDESC
An external battery frame has been added.
EDESC
#
#
#
EVENT extBatteryFrameDecrease .1.3.6.1.4.1.318.0.76 "Status Events" Normal
FORMAT APC UPS: An external battery frame has been removed., Trap Arguments:($#):$* [APC PowerNet]
SDESC
An external battery frame has been removed.
EDESC
#
#
#
EVENT abnormalCondition .1.3.6.1.4.1.318.0.77 "Status Events" Critical
FORMAT APC $2, Trap Arguments:($#):$* [APC PowerNet]
SDESC
APC $2
EDESC
#
#
#
EVENT abnormalConditionCleared .1.3.6.1.4.1.318.0.78 "Status Events" Normal
FORMAT APC $2, Trap Arguments:($#):$* [APC PowerNet]
SDESC
APC $2
EDESC
#
#
#
EVENT deviceStatusChange .1.3.6.1.4.1.318.0.79 "Status Events" Normal
FORMAT APC : The status of the device being monitored has changed., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The status of the device being monitored has changed.
EDESC
#
#
#
EVENT noBatteries .1.3.6.1.4.1.318.0.80 "Status Events" Minor
FORMAT APC UPS: No batteries attached., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS has no batteries attached.
EDESC
#
#
#
EVENT noBatteriesCleared .1.3.6.1.4.1.318.0.81 "Status Events" Normal
FORMAT APC UPS: The no batteries attached condition has been cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The UPS's batteries have been attached.
EDESC
#
#
#
EVENT userAdded .1.3.6.1.4.1.318.0.82 "Status Events" Normal
FORMAT APC: A new user has been added., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A new user has been added.
EDESC
#
#
#
EVENT userDeleted .1.3.6.1.4.1.318.0.83 "Status Events" Normal
FORMAT APC: A user has been deleted., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A user has been deleted.
EDESC
#
#
#
EVENT userModified .1.3.6.1.4.1.318.0.84 "Status Events" Normal
FORMAT APC: A user has been modified., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A user has been modified.
EDESC
#
#
#
EVENT msvmCommunicationEstablished .1.3.6.1.4.1.318.0.85 "Status Events" Normal
FORMAT APC: Communications established with the MasterSwitch VM., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communications with the MasterSwitch VM has been established.
EDESC
#
#
#
EVENT msvmCommunicationLost .1.3.6.1.4.1.318.0.86 "Status Events" Critical
FORMAT APC: Communications lost with the MasterSwitch VM., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communications with the MasterSwitch VM has been lost.
EDESC
#
#
#
EVENT msvmOverload .1.3.6.1.4.1.318.0.87 "Status Events" Critical
FORMAT APC: The MasterSwitch VM is near or at an overload condition., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The MasterSwitch VM is near or at an overload condition.
EDESC
#
#
#
EVENT msvmOverloadCleared .1.3.6.1.4.1.318.0.88 "Status Events" Normal
FORMAT APC: The overload condition cleared on the MasterSwitch VM., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The overload condition on the MasterSwitch VM has been cleared.
EDESC
#
#
#
EVENT msvmOutletOn .1.3.6.1.4.1.318.0.89 "Status Events" Normal
FORMAT APC: An outlet on the MasterSwitch VM has turned on., Trap Arguments:($#):$* [APC PowerNet]
SDESC
An outlet on the MasterSwitch VM has turned on.
EDESC
#
#
#
EVENT msvmOutletOff .1.3.6.1.4.1.318.0.90 "Status Events" Normal
FORMAT APC: An outlet on the MasterSwitch VM has turned off., Trap Arguments:($#):$* [APC PowerNet]
SDESC
An outlet on the MasterSwitch VM has turned off.
EDESC
#
#
#
EVENT msvmDeviceConfigChange .1.3.6.1.4.1.318.0.91 "Status Events" Normal
FORMAT APC: A device configuration change on a MasterSwitch VM., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A device configuration change has been made on a MasterSwitch VM.
EDESC
#
#
#
EVENT msvmOutletConfigChange .1.3.6.1.4.1.318.0.92 "Status Events" Normal
FORMAT APC: An outlet configuration change on a MasterSwitch VM., Trap Arguments:($#):$* [APC PowerNet]
SDESC
An outlet configuration change has been made on a MasterSwitch VM.
EDESC
#
#
#
EVENT msvmLowLoad .1.3.6.1.4.1.318.0.93 "Status Events" Normal
FORMAT APC: The MasterSwitch VM has violated the low load threshold., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The MasterSwitch VM has violated the low load threshold.
EDESC
#
#
#
EVENT msvmLowLoadCleared .1.3.6.1.4.1.318.0.94 "Status Events" Normal
FORMAT APC: The low load condition cleared on the MasterSwitch VM., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The low load condition on the MasterSwitch VM has been cleared.
EDESC
#
#
#
EVENT msvmNearOverload .1.3.6.1.4.1.318.0.95 "Status Events" Critical
FORMAT APC: The MasterSwitch VM is near or at an overload condition., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The MasterSwitch VM is near or at an overload condition.
EDESC
#
#
#
EVENT msvmNearOverloadCleared .1.3.6.1.4.1.318.0.96 "Status Events" Normal
FORMAT APC: The overload condition cleared on the MasterSwitch VM., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The overload condition on the MasterSwitch VM has been cleared.
EDESC
#
#
#
EVENT msvmPowerSupplyStatusChange .1.3.6.1.4.1.318.0.97 "Status Events" Minor
FORMAT APC: The power supply status changed on MasterSwitch VM, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The power supply status of the MasterSwitch VM has changed.
EDESC
#
#
#
EVENT mspCommunicationEstablished .1.3.6.1.4.1.318.0.98 "Status Events" Normal
FORMAT APC: Communications established with the MasterSwitch plus., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communications with the MasterSwitch plus has been established.
EDESC
#
#
#
EVENT mspCommunicationLost .1.3.6.1.4.1.318.0.99 "Status Events" Critical
FORMAT APC: Communications lost with the MasterSwitch plus., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communications with the MasterSwitch plus has been lost.
EDESC
#
#
#
EVENT mspOutletOn .1.3.6.1.4.1.318.0.100 "Status Events" Normal
FORMAT APC: An outlet on the MasterSwitch plus has turned on., Trap Arguments:($#):$* [APC PowerNet]
SDESC
An outlet on the MasterSwitch plus has turned on.
EDESC
#
#
#
EVENT mspOutletOff .1.3.6.1.4.1.318.0.101 "Status Events" Normal
FORMAT APC: An outlet on the MasterSwitch plus has turned off., Trap Arguments:($#):$* [APC PowerNet]
SDESC
An outlet on the MasterSwitch plus has turned off.
EDESC
#
#
#
EVENT mspDeviceConfigChange .1.3.6.1.4.1.318.0.102 "Status Events" Normal
FORMAT APC: A device configuration change on a MasterSwitch plus., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A device configuration change has been made on a MasterSwitch plus.
EDESC
#
#
#
EVENT mspOutletConfigChange .1.3.6.1.4.1.318.0.103 "Status Events" Normal
FORMAT APC: An outlet configuration change on a MasterSwitch plus., Trap Arguments:($#):$* [APC PowerNet]
SDESC
An outlet configuration change has been made on a MasterSwitch plus.
EDESC
#
#
#
EVENT rsSourceSwitched .1.3.6.1.4.1.318.0.104 "Status Events" Normal
FORMAT APC Redundant Switch: The Redundant Switch has switched source, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The Redundant Switch has switched source.
EDESC
#
#
#
EVENT rsLostRedundancy .1.3.6.1.4.1.318.0.105 "Status Events" Critical
FORMAT APC Redundant Switch: The Redundant Switch has lost redundancy, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The Redundant Switch has lost redundancy.
EDESC
#
#
#
EVENT rsRedundancyRestored .1.3.6.1.4.1.318.0.106 "Status Events" Normal
FORMAT APC Redundant Switch: Redundancy has been restored., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Redundancy has been restored to the Redundant Switch .
EDESC
#
#
#
EVENT rsConfigChange .1.3.6.1.4.1.318.0.107 "Status Events" Normal
FORMAT APC: A configuration change on a Redundant Switch., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A configuration change has been made on a Redundant Switch.
EDESC
#
#
#
EVENT rsCommunicationEstablished .1.3.6.1.4.1.318.0.108 "Status Events" Normal
FORMAT APC: Communications established with the Redundant Switch., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communications with the Redundant Switch has been established.
EDESC
#
#
#
EVENT rsCommunicationLost .1.3.6.1.4.1.318.0.109 "Status Events" Critical
FORMAT APC: Communications lost with the Redundant Switch., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communications with the Redundant Switch has been lost.
EDESC
#
#
#
EVENT dcCommunicationEstablished .1.3.6.1.4.1.318.0.110 "Status Events" Normal
FORMAT APC: Communications established with the DC power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communications with the DC power plant has been established.
EDESC
#
#
#
EVENT dcCommunicationLost .1.3.6.1.4.1.318.0.111 "Status Events" Critical
FORMAT APC: Communications lost with the DC power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communications with the DC power plant has been lost.
EDESC
#
#
#
EVENT dcPINChanged .1.3.6.1.4.1.318.0.112 "Status Events" Normal
FORMAT APC: The active PIN on the DC controller has been changed., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The active PIN on the DC controller has been changed.
EDESC
#
#
#
EVENT dcMajorAlarm .1.3.6.1.4.1.318.0.113 "Status Events" Critical
FORMAT APC: A Major alarm is active in the DC power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A Major alarm is active in the DC power plant.
EDESC
#
#
#
EVENT dcMajorAlarmCleared .1.3.6.1.4.1.318.0.114 "Status Events" Normal
FORMAT APC: A Major alarm is no longer active in the DC power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A Major alarm is no longer active in the DC power plant.
EDESC
#
#
#
EVENT dcMinorAlarm .1.3.6.1.4.1.318.0.115 "Status Events" Minor
FORMAT APC: A Minor alarm is active in the DC power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A Minor alarm is active in the DC power plant.
EDESC
#
#
#
EVENT dcMinorAlarmCleared .1.3.6.1.4.1.318.0.116 "Status Events" Normal
FORMAT APC: A Minor alarm is no longer active in the DC power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A Minor alarm is no longer active in the DC power plant.
EDESC
#
#
#
EVENT dcOutputRelayOn .1.3.6.1.4.1.318.0.117 "Status Events" Minor
FORMAT APC: An output relay has gone on., Trap Arguments:($#):$* [APC PowerNet]
SDESC
An output relay has gone on in the DC power plant.
EDESC
#
#
#
EVENT dcOutputRelayOff .1.3.6.1.4.1.318.0.118 "Status Events" Normal
FORMAT APC: An output relay has gone off., Trap Arguments:($#):$* [APC PowerNet]
SDESC
An output relay has gone off in the DC power plant.
EDESC
#
#
#
EVENT dcInputRelayOn .1.3.6.1.4.1.318.0.119 "Status Events" Minor
FORMAT APC: An input relay has gone on., Trap Arguments:($#):$* [APC PowerNet]
SDESC
An input relay has gone on in the DC power plant.
EDESC
#
#
#
EVENT dcInputRelayOff .1.3.6.1.4.1.318.0.120 "Status Events" Normal
FORMAT APC: An input relay has gone off., Trap Arguments:($#):$* [APC PowerNet]
SDESC
An input relay has gone off in the DC power plant.
EDESC
#
#
#
EVENT logicPowerSuppliesIncreased .1.3.6.1.4.1.318.0.121 "Status Events" Normal
FORMAT APC UPS: The number of system power supplies has increased., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The number of system power supplies has increased.
EDESC
#
#
#
EVENT logicPowerSuppliesDecreased .1.3.6.1.4.1.318.0.122 "Status Events" Normal
FORMAT APC UPS: The number of system power supplies has decreased., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The number of system power supplies has decreased.
EDESC
#
#
#
EVENT externalSwitchGearClosed .1.3.6.1.4.1.318.0.123 "Status Events" Normal
FORMAT APC UPS: External Switch Gear $1 closed., Trap Arguments:($#):$* [APC PowerNet]
SDESC
External Switch Gear $1 closed.
EDESC
#
#
#
EVENT externalSwitchGearOpened .1.3.6.1.4.1.318.0.124 "Status Events" Normal
FORMAT APC UPS: External Switch Gear $1 opened., Trap Arguments:($#):$* [APC PowerNet]
SDESC
External Switch Gear $1 opened.
EDESC
#
#
#
EVENT generalDeviceEvent .1.3.6.1.4.1.318.0.125 "Status Events" Normal
FORMAT APC Device: $1, Trap Arguments:($#):$* [APC PowerNet]
SDESC
$1 APC Device event.
EDESC
#
#
#
EVENT atsSourceSwitched .1.3.6.1.4.1.318.0.126 "Status Events" Normal
FORMAT APC Automatic Transfer Switch: The ATS has switched source, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The Automatic Transfer Switch has switched source.
EDESC
#
#
#
EVENT atsLostRedundancy .1.3.6.1.4.1.318.0.127 "Status Events" Critical
FORMAT APC Automatic Transfer Switch: The ATS has lost redundancy. , Trap Arguments:($#):$* [APC PowerNet]
SDESC
The Automatic Transfer Switch has lost redundancy.
EDESC
#
#
#
EVENT atsRedundancyRestored .1.3.6.1.4.1.318.0.128 "Status Events" Normal
FORMAT APC Automatic Transfer Switch: Redundancy has been restored., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Redundancy has been restored to the Automatic Transfer Switch .
EDESC
#
#
#
EVENT atsConfigChange .1.3.6.1.4.1.318.0.129 "Status Events" Normal
FORMAT APC Automatic Transfer Switch: ATS configuration changed., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A configuration change has been made on a Automatic Transfer Switch.
EDESC
#
#
#
EVENT atsCommunicationEstablished .1.3.6.1.4.1.318.0.130 "Status Events" Normal
FORMAT APC Automatic Transfer Switch: Communications established., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communications with the Automatic Transfer Switch has been established.
EDESC
#
#
#
EVENT atsCommunicationLost .1.3.6.1.4.1.318.0.131 "Status Events" Critical
FORMAT APC Automatic Transfer Switch: Communications lost., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communications with the Automatic Transfer Switch has been lost.
EDESC
#
#
#
EVENT atsOverCurrent .1.3.6.1.4.1.318.0.132 "Status Events" Critical
FORMAT APC Automatic Transfer Switch: Output Current exceeded threshold, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output Current has exceeded Threshold. 
EDESC
#
#
#
EVENT atsOverCurrentCleared .1.3.6.1.4.1.318.0.133 "Status Events" Normal
FORMAT APC Automatic Transfer Switch: Output Current below threshold., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output Current has returned below threshold.
EDESC
#
#
#
EVENT atsPowerSupplyFailure .1.3.6.1.4.1.318.0.134 "Status Events" Critical
FORMAT APC Automatic Transfer Switch: The ATS Power Supply has failed., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The Automatic Transfer Switch Power Supply has failed.
EDESC
#
#
#
EVENT atsPowerSupplyFailureCleared .1.3.6.1.4.1.318.0.135 "Status Events" Normal
FORMAT APC Automatic Transfer Switch: Power Supply Failure Cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The Automatic Transfer Switch Power Supply Failure Cleared.
EDESC
#
#
#
EVENT dcMainsFailAlarm .1.3.6.1.4.1.318.0.136 "Status Events" Minor
FORMAT APC: A Mains Fail alarm is active in the DC power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A Mains Fail alarm is active in the DC power plant.
EDESC
#
#
#
EVENT dcMainsFailAlarmCleared .1.3.6.1.4.1.318.0.137 "Status Events" Normal
FORMAT APC: Mains Fail alarm is no longer active in the DC power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Mains Fail alarm is no longer active in the DC power plant.
EDESC
#
#
#
EVENT dcFanFailAlarm .1.3.6.1.4.1.318.0.138 "Status Events" Minor
FORMAT APC: A Fan Fail alarm is active in the DC power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A Fan Fail alarm is active in the DC power plant.
EDESC
#
#
#
EVENT dcFanFailAlarmCleared .1.3.6.1.4.1.318.0.139 "Status Events" Normal
FORMAT APC: A Fan Fail alarm is no longer active in the DC power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A Fan Fail alarm is no longer active in the DC power plant.
EDESC
#
#
#
EVENT dcRectifierOvertempAlarm .1.3.6.1.4.1.318.0.140 "Status Events" Minor
FORMAT APC: Rect. Overtemp alarm is active in the power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Rect. Overtemp alarm is active in the power plant.
EDESC
#
#
#
EVENT dcRectifierOvertempAlarmCleared .1.3.6.1.4.1.318.0.141 "Status Events" Normal
FORMAT APC: Rect. Overtmp alarm is no longer active in the power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Rect. Overtemp alarm is no longer active in the power plant.
EDESC
#
#
#
EVENT dcCurrentLimitAlarm .1.3.6.1.4.1.318.0.142 "Status Events" Minor
FORMAT APC: A Current Limit alarm is active in the power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A Current Limit alarm is active in the power plant.
EDESC
#
#
#
EVENT dcCurrentLimitAlarmCleared .1.3.6.1.4.1.318.0.143 "Status Events" Normal
FORMAT APC: Current Limit alarm is no longer active in the power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Current Limit alarm is no longer active in the power plant.
EDESC
#
#
#
EVENT dcRectifierFailAlarm .1.3.6.1.4.1.318.0.144 "Status Events" Minor
FORMAT APC: A Rect. Fail alarm is active in the power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A Rect. Fail alarm is active in the power plant.
EDESC
#
#
#
EVENT dcRectifierFailAlarmCleared .1.3.6.1.4.1.318.0.145 "Status Events" Normal
FORMAT APC: Rect. Fail alarm is no longer active in the power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Rect. Fail alarm is no longer active in the power plant.
EDESC
#
#
#
EVENT dcMultRectFailAlarm .1.3.6.1.4.1.318.0.146 "Status Events" Minor
FORMAT APC: Multiple Rect. Fail alarm is active in the powerplant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Multiple Rect. Fail alarm is active in the powerplant.
EDESC
#
#
#
EVENT dcMultRectFailAlarmCleared .1.3.6.1.4.1.318.0.147 "Status Events" Normal
FORMAT APC: Multiple Rect Fail alarm is no longer active in powerplant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Multiple Rect Fail alarm is no longer active in the powerplant.
EDESC
#
#
#
EVENT dcBatteryBreakerAlarm .1.3.6.1.4.1.318.0.148 "Status Events" Minor
FORMAT APC: Batt. Breaker alarm is active in the power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Batt. Breaker alarm is active in the power plant.
EDESC
#
#
#
EVENT dcBatteryBreakerAlarmCleared .1.3.6.1.4.1.318.0.149 "Status Events" Normal
FORMAT APC: Batt. Breaker alarm is no longer active in the power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Batt. Breaker alarm is no longer active in the power plant.
EDESC
#
#
#
EVENT dcRectifierOVPAlarm .1.3.6.1.4.1.318.0.150 "Status Events" Minor
FORMAT APC: A Rect. OVP alarm is active in the power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A Rect. OVP alarm is active in the power plant.
EDESC
#
#
#
EVENT dcRectifierOVPAlarmCleared .1.3.6.1.4.1.318.0.151 "Status Events" Normal
FORMAT APC: A Rect. OVP alarm is no longer active in the power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A Rect. OVP alarm is no longer active in the power plant.
EDESC
#
#
#
EVENT dcLVDImminentAlarm .1.3.6.1.4.1.318.0.152 "Status Events" Minor
FORMAT APC: A LVD Imminent alarm is active in the powerplant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A LVD Imminent alarm is active in the powerplant.
EDESC
#
#
#
EVENT dcLVDImminentAlarmCleared .1.3.6.1.4.1.318.0.153 "Status Events" Normal
FORMAT APC: A LVD Imminent alarm is no longer active in the powerplant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A LVD Imminent alarm is no longer active in the powerplant.
EDESC
#
#
#
EVENT dcFuseCBAlarm .1.3.6.1.4.1.318.0.154 "Status Events" Minor
FORMAT APC: A Fuse/CB alarm is active in the DC power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A Fuse/CB alarm is active in the DC power plant.
EDESC
#
#
#
EVENT dcFuseCBAlarmCleared .1.3.6.1.4.1.318.0.155 "Status Events" Normal
FORMAT APC: A Fuse/CB alarm is no longer active in the DC power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A Fuse/CB alarm is no longer active in the DC power plant.
EDESC
#
#
#
EVENT dcBatteryTestFail .1.3.6.1.4.1.318.0.156 "Status Events" Minor
FORMAT APC: A Battery Test failed in the DC power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A Battery Test failed in the DC power plant.
EDESC
#
#
#
EVENT dcTemperatureAlarm .1.3.6.1.4.1.318.0.157 "Status Events" Minor
FORMAT APC: A Temperature alarm is active in the power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A Temperature alarm is active in the power plant.
EDESC
#
#
#
EVENT dcTemperatureAlarmCleared .1.3.6.1.4.1.318.0.158 "Status Events" Normal
FORMAT APC: A Temperature alarm is no longer active in the power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A Temperature alarm is no longer active in the power plant.
EDESC
#
#
#
EVENT dcHumidityAlarm .1.3.6.1.4.1.318.0.159 "Status Events" Minor
FORMAT APC: A Humidity alarm is active in the DC power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A Humidity alarm is active in the DC power plant.
EDESC
#
#
#
EVENT dcHumidityAlarmCleared .1.3.6.1.4.1.318.0.160 "Status Events" Normal
FORMAT APC: A Humidity alarm is no longer active in the DC power plant., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A Humidity alarm is no longer active in the DC power plant.
EDESC
#
#
#
EVENT dcBBCommunicationEstablished .1.3.6.1.4.1.318.0.161 "Status Events" Normal
FORMAT APC: Power plant bridging board communications established., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Power plant bridging board communications established.
EDESC
#
#
#
EVENT dcBBCommunicationLost .1.3.6.1.4.1.318.0.162 "Status Events" Critical
FORMAT APC: Power plant bridging board communications lost., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Power plant bridging board communications lost.
EDESC
#
#
#
EVENT iemHighTempThresholdViolation .1.3.6.1.4.1.318.0.163 "Status Events" Critical
FORMAT APC IEM: High temperature violation of $1 $2 on probe $3, $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
High temperature threshold of violation of $1 $2 on probe $3, $4.
EDESC
#
#
#
EVENT iemHighTempThresholdViolationCleared .1.3.6.1.4.1.318.0.164 "Status Events" Normal
FORMAT APC IEM: High temperature violation on probe $1, $2, cleared. , Trap Arguments:($#):$* [APC PowerNet]
SDESC
High temperature threshold violation has been cleared on probe $1, $2.
EDESC
#
#
#
EVENT iemLowTempThresholdViolation .1.3.6.1.4.1.318.0.165 "Status Events" Critical
FORMAT APC IEM: Low temperature of $1 $2 on probe $3, $4. , Trap Arguments:($#):$* [APC PowerNet]
SDESC
Low temperature threshold of violation of $1 $2 on probe $3, $4.
EDESC
#
#
#
EVENT iemLowTempThresholdViolationCleared .1.3.6.1.4.1.318.0.166 "Status Events" Normal
FORMAT APC IEM: Low temperature violation on probe $1, $2, cleared. , Trap Arguments:($#):$* [APC PowerNet]
SDESC
Low temperature threshold violation has been cleared on probe $1, $2.
EDESC
#
#
#
EVENT iemHighHumidThresholdViolation .1.3.6.1.4.1.318.0.167 "Status Events" Critical
FORMAT APC IEM: High humidity of $1 percent humidity on probe $2, $3. , Trap Arguments:($#):$* [APC PowerNet]
SDESC
High humidity threshold of violation of $1 percent relative humidity on probe $2, $3.
EDESC
#
#
#
EVENT iemHighHumidThresholdViolationCleared .1.3.6.1.4.1.318.0.168 "Status Events" Normal
FORMAT APC IEM: High humidity violation on probe $1, $2, cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
High humidity threshold violation on probe $1, $2, has been cleared.
EDESC
#
#
#
EVENT iemLowHumidThresholdViolation .1.3.6.1.4.1.318.0.169 "Status Events" Critical
FORMAT APC IEM: Low humidity of $1 percent humidity on probe $2, $3. , Trap Arguments:($#):$* [APC PowerNet]
SDESC
High humidity threshold of violation of $1 percent relative humidity on probe $2, $3.
EDESC
#
#
#
EVENT iemLowHumidThresholdViolationCleared .1.3.6.1.4.1.318.0.170 "Status Events" Normal
FORMAT APC IEM: Low humidity violation on probe $1, $2, cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Low humidity threshold violation on probe $1, $2, has been cleared.
EDESC
#
#
#
EVENT iemProbeDisconnected .1.3.6.1.4.1.318.0.171 "Status Events" Minor
FORMAT APC IEM: Probe disconnected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Probe has been disconnected.
EDESC
#
#
#
EVENT iemProbeConnected .1.3.6.1.4.1.318.0.172 "Status Events" Normal
FORMAT APC IEM: Probe Connected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Probe has been connected.
EDESC
#
#
#
EVENT iemContactFault .1.3.6.1.4.1.318.0.173 "Status Events" Critical
FORMAT APC IEM: Contact $1, $2, fault., Trap Arguments:($#):$* [APC PowerNet]
SDESC
There is a fault on contact $1, $2.
EDESC
#
#
#
EVENT iemContactFaultCleared .1.3.6.1.4.1.318.0.174 "Status Events" Normal
FORMAT APC IEM: Fault cleared on contact $1, $2., Trap Arguments:($#):$* [APC PowerNet]
SDESC
There is a fault on contact $1, $2.
EDESC
#
#
#
EVENT iemRelayFault .1.3.6.1.4.1.318.0.175 "Status Events" Critical
FORMAT APC IEM: Output relay $1, $2, has faulted because $3., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output relay $1, $2, has faulted because $3.
EDESC
#
#
#
EVENT iemRelayFaultCleared .1.3.6.1.4.1.318.0.176 "Status Events" Normal
FORMAT APC IEM: Output relay, $1, $2, fault cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output relay $1, $2 fault cleared.
EDESC
#
#
#
EVENT bmBatManCommEstab .1.3.6.1.4.1.318.0.177 "Status Events" Normal
FORMAT BatMan : Unit $1 Communications Established., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Unit $1 Communications Established.
EDESC
#
#
#
EVENT bmBatManCommLost .1.3.6.1.4.1.318.0.178 "Status Events" Critical
FORMAT BatMan : Unit $1 Communications Lost., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Unit $1 Communications Lost.
EDESC
#
#
#
EVENT bmBatManKneeAlarm .1.3.6.1.4.1.318.0.179 "Status Events" Critical
FORMAT BatMan : Unit $1 Knee Alarm Detected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Unit $1 Knee Alarm Detected.
EDESC
#
#
#
EVENT bmBatManKneeAlarmCleared .1.3.6.1.4.1.318.0.180 "Status Events" Normal
FORMAT BatMan : Unit $1 Knee Alarm Cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Unit $1 Knee Alarm Cleared.
EDESC
#
#
#
EVENT bmBatManChargerAlarm .1.3.6.1.4.1.318.0.181 "Status Events" Minor
FORMAT BatMan : Unit $1 Charger Alarm Detected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Unit $1 Charger Alarm Detected.
EDESC
#
#
#
EVENT bmBatManChargerAlarmCleared .1.3.6.1.4.1.318.0.182 "Status Events" Normal
FORMAT BatMan : Unit $1 Charger Alarm Cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Unit $1 Charger Alarm Cleared.
EDESC
#
#
#
EVENT bmBatManBatteryAlarm .1.3.6.1.4.1.318.0.183 "Status Events" Minor
FORMAT BatMan : Unit $1 Battery Alarm Detected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Unit $1 Battery Alarm Detected.
EDESC
#
#
#
EVENT bmBatManBatteryAlarmCleared .1.3.6.1.4.1.318.0.184 "Status Events" Normal
FORMAT BatMan : Unit $1 Battery Alarm Cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Unit $1 Battery Alarm Cleared.
EDESC
#
#
#
EVENT bmBatManEnvironmentAlarm .1.3.6.1.4.1.318.0.185 "Status Events" Minor
FORMAT BatMan : Unit $1 Environment Alarm Detected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Unit $1 Environment Alarm Detected.
EDESC
#
#
#
EVENT bmBatManEnvironmentAlarmCleared .1.3.6.1.4.1.318.0.186 "Status Events" Normal
FORMAT BatMan : Unit $1 Environment Alarm Cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Unit $1 Environment Alarm Cleared.
EDESC
#
#
#
EVENT bmBatManMaintenanceAlarm .1.3.6.1.4.1.318.0.187 "Status Events" Normal
FORMAT BatMan : Unit $1 Maintenance Due Alarm Detected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Unit $1 Maintenance Due Alarm Detected.
EDESC
#
#
#
EVENT bmBatManMaintenanceAlarmCleared .1.3.6.1.4.1.318.0.188 "Status Events" Normal
FORMAT BatMan : Unit $1 Maintenance Due Alarm Cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Unit $1 Maintenance Due Alarm Cleared.
EDESC
#
#
#
EVENT pduCommunicationEstablished .1.3.6.1.4.1.318.0.189 "Status Events" Normal
FORMAT APC PDU [$1, $2]: Communication Established., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communication Established.
EDESC
#
#
#
EVENT pduCommunicationLost .1.3.6.1.4.1.318.0.190 "Status Events" Critical
FORMAT APC PDU [$1, $2]: Communication Lost., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communication Lost.
EDESC
#
#
#
EVENT pduUtilityLineUndervoltage .1.3.6.1.4.1.318.0.191 "Status Events" Critical
FORMAT APC PDU [$1, $2]: Utility Line Undervoltage L$3., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Utility Line Undervoltage L$3.
EDESC
#
#
#
EVENT pduUtilityLineUndervoltageCleared .1.3.6.1.4.1.318.0.192 "Status Events" Normal
FORMAT APC PDU [$1, $2]: Utility Line Undervoltage Cleared L$3., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Utility Line Undervoltage Cleared L$3.
EDESC
#
#
#
EVENT pduUtilityLineOvervoltage .1.3.6.1.4.1.318.0.193 "Status Events" Critical
FORMAT APC PDU [$1, $2]: Utility Line Overvoltage L$3., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Utility Line Overvoltage L$3.
EDESC
#
#
#
EVENT pduUtilityLineOvervoltageCleared .1.3.6.1.4.1.318.0.194 "Status Events" Normal
FORMAT APC PDU [$1, $2]: Utility Line Overvoltage Cleared L$3., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Utility Line Overvoltage Cleared L$3.
EDESC
#
#
#
EVENT pduGroundOvercurrent .1.3.6.1.4.1.318.0.195 "Status Events" Critical
FORMAT APC PDU [$1, $2]: Ground Overcurrent., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Ground Overcurrent.
EDESC
#
#
#
EVENT pduGroundOvercurrentCleared .1.3.6.1.4.1.318.0.196 "Status Events" Normal
FORMAT APC PDU [$1, $2]: Ground Overcurrent Cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Ground Overcurrent Cleared.
EDESC
#
#
#
EVENT pduCircuitPanelInputUndervoltage .1.3.6.1.4.1.318.0.197 "Status Events" Critical
FORMAT APC PDU [$1, $2]: Circuit Panel Input Undervoltage L$3., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Circuit Panel Input Undervoltage L$3.
EDESC
#
#
#
EVENT pduCircuitPanelInputUndervoltageCleared .1.3.6.1.4.1.318.0.198 "Status Events" Normal
FORMAT APC PDU [$1, $2]: Circuit Panel Input Undervoltage Cleared L$3., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Circuit Panel Input Undervoltage Cleared L$3.
EDESC
#
#
#
EVENT pduCircuitPanelInputOvervoltage .1.3.6.1.4.1.318.0.199 "Status Events" Critical
FORMAT APC PDU [$1, $2]: Circuit Panel Input Overvoltage L$3., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Circuit Panel Input Overvoltage L$3.
EDESC
#
#
#
EVENT pduCircuitPanelInputOvervoltageCleared .1.3.6.1.4.1.318.0.200 "Status Events" Normal
FORMAT APC PDU [$1, $2]: Circuit Panel Input Overvoltage Cleared L$3., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Circuit Panel Input Overvoltage Cleared L$3.
EDESC
#
#
#
EVENT pduCircuitPanelInputUndercurrent .1.3.6.1.4.1.318.0.201 "Status Events" Critical
FORMAT APC PDU [$1, $2]: Circuit Panel Input Undercurrent L$3., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Circuit Panel Input Undercurrent L$3.
EDESC
#
#
#
EVENT pduCircuitPanelInputUndercurrentCleared .1.3.6.1.4.1.318.0.202 "Status Events" Normal
FORMAT APC PDU [$1, $2]: Circuit Panel Input Undercurrent Cleared L$3., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Circuit Panel Input Undercurrent Cleared L$3.
EDESC
#
#
#
EVENT pduCircuitPanelInputOvercurrent .1.3.6.1.4.1.318.0.203 "Status Events" Critical
FORMAT APC PDU [$1, $2]: Circuit Panel Input Overcurrent L$3., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Circuit Panel Input Overcurrent L$3.
EDESC
#
#
#
EVENT pduCircuitPanelInputOvercurrentCleared .1.3.6.1.4.1.318.0.204 "Status Events" Normal
FORMAT APC PDU [$1, $2]: Circuit Panel Input Overcurrent Cleared L$3., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Circuit Panel Input Overcurrent Cleared L$3.
EDESC
#
#
#
EVENT pduCircuitPanelFrequencyOutOfRange .1.3.6.1.4.1.318.0.205 "Status Events" Critical
FORMAT APC PDU [$1, $2]: Circuit Panel Input Frequency Out Of Range., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Circuit Panel Input Frequency Out Of Range.
EDESC
#
#
#
EVENT pduCircuitPanelFrequencyOutofRangeCleared .1.3.6.1.4.1.318.0.206 "Status Events" Normal
FORMAT APC PDU [$1, $2]: Circuit Panel Input Frequency No Longer Out Of Range., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Circuit Panel Input Frequency No Longer Out Of Range.
EDESC
#
#
#
EVENT pduCircuitPanelNeutralOvercurrent .1.3.6.1.4.1.318.0.207 "Status Events" Critical
FORMAT APC PDU [$1, $2]: Circuit Panel Input Neutral Overcurrent., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Circuit Panel Input Neutral Overcurrent.
EDESC
#
#
#
EVENT pduCircuitPanelNeutralOvercurrentCleared .1.3.6.1.4.1.318.0.208 "Status Events" Normal
FORMAT APC PDU [$1, $2]: Circuit Panel Input Neutral Overcurrent Cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Circuit Panel Input Neutral Overcurrent Cleared.
EDESC
#
#
#
EVENT pduSystemOff .1.3.6.1.4.1.318.0.209 "Status Events" Critical
FORMAT APC PDU [$1, $2]: System Off., Trap Arguments:($#):$* [APC PowerNet]
SDESC
PDU System Off.
EDESC
#
#
#
EVENT pduOnBatteryMode .1.3.6.1.4.1.318.0.210 "Status Events" Critical
FORMAT APC PDU [$1, $2]: On Battery Mode., Trap Arguments:($#):$* [APC PowerNet]
SDESC
PDU is in On Battery Mode.
EDESC
#
#
#
EVENT pduMaintenanceBypassMode .1.3.6.1.4.1.318.0.211 "Status Events" Normal
FORMAT APC PDU [$1, $2]: Maintenance Bypass Mode., Trap Arguments:($#):$* [APC PowerNet]
SDESC
PDU is in Maintenance Bypass Mode.
EDESC
#
#
#
EVENT pduAtypicalBypassMode .1.3.6.1.4.1.318.0.212 "Status Events" Minor
FORMAT APC PDU [$1, $2]: Atypical Bypass Mode., Trap Arguments:($#):$* [APC PowerNet]
SDESC
PDU is in Atypical Bypass Mode.
EDESC
#
#
#
EVENT pduNoPanelFeedMode .1.3.6.1.4.1.318.0.213 "Status Events" Critical
FORMAT APC PDU [$1, $2]: No Panel Feed Mode., Trap Arguments:($#):$* [APC PowerNet]
SDESC
PDU is in No Panel Feed Mode.
EDESC
#
#
#
EVENT pduUpsOperationMode .1.3.6.1.4.1.318.0.214 "Status Events" Normal
FORMAT APC PDU [$1, $2]: Ups Operation Mode., Trap Arguments:($#):$* [APC PowerNet]
SDESC
PDU is in Ups Operation Mode.
EDESC
#
#
#
EVENT pduForcedBypassMode .1.3.6.1.4.1.318.0.215 "Status Events" Minor
FORMAT APC PDU [$1, $2]: Forced Bypass Mode., Trap Arguments:($#):$* [APC PowerNet]
SDESC
PDU is in Forced Bypass Mode.
EDESC
#
#
#
EVENT pduInputTransformerOverTemperature .1.3.6.1.4.1.318.0.216 "Status Events" Critical
FORMAT APC PDU [$1, $2]: Input Transformer Over Temperature., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Input Transformer Over Temperature.
EDESC
#
#
#
EVENT pduInputTransformerOverTemperatureCleared .1.3.6.1.4.1.318.0.217 "Status Events" Normal
FORMAT APC PDU [$1, $2]: Input Transformer Over Temperature Cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Input Transformer Over Temperature Cleared.
EDESC
#
#
#
EVENT pduUPSInputVoltageLost .1.3.6.1.4.1.318.0.218 "Status Events" Critical
FORMAT APC PDU [$1, $2]: UPS Input Voltage L$3-N Lost., Trap Arguments:($#):$* [APC PowerNet]
SDESC
UPS Input Voltage L$3-N Lost.
EDESC
#
#
#
EVENT pduUPSInputVoltageRestored .1.3.6.1.4.1.318.0.219 "Status Events" Normal
FORMAT APC PDU [$1, $2]: UPS Input Voltage L$3-N Restored., Trap Arguments:($#):$* [APC PowerNet]
SDESC
UPS Input Voltage L$3-N Restored.
EDESC
#
#
#
EVENT pduContactFault .1.3.6.1.4.1.318.0.220 "Status Events" Critical
FORMAT APC PDU [$1, $2]: Contact $3 Abnormal., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Contact $3 Abnormal.
EDESC
#
#
#
EVENT pduContactFaultCleared .1.3.6.1.4.1.318.0.221 "Status Events" Normal
FORMAT APC PDU [$1, $2]: Contact $3 Normal., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Contact $3 Normal.
EDESC
#
#
#
EVENT rPDUBankPhaseLowLoad .1.3.6.1.4.1.318.0.222 "Status Events" Minor
FORMAT APC Rack PDU: Violation of bank or phase low load threshold., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A bank or phase on the Rack PDU has violated the low load threshold.
EDESC
#
#
#
EVENT rPDUBankPhaseLowLoadCleared .1.3.6.1.4.1.318.0.223 "Status Events" Normal
FORMAT APC Rack PDU: Bank or phase low load condition cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The bank or phase low load condition on a Rack PDU has been cleared.
EDESC
#
#
#
EVENT rPDUBankPhaseNearOverload .1.3.6.1.4.1.318.0.224 "Status Events" Minor
FORMAT APC Rack PDU: Bank or phase near an overload condition., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A bank or phase of the Rack PDU is near an overload condition.
EDESC
#
#
#
EVENT rPDUBankPhaseNearOverloadCleared .1.3.6.1.4.1.318.0.225 "Status Events" Normal
FORMAT APC Rack PDU: Bank or phase near overload condition has cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Rack PDU bank or phase near overload condition has cleared.
EDESC
#
#
#
EVENT rPDUBankPhaseOverload .1.3.6.1.4.1.318.0.226 "Status Events" Critical
FORMAT APC Rack PDU: Bank or phase overload condition., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A bank or phase of the Rack PDU is in an overload condition.
EDESC
#
#
#
EVENT rPDUBankPhaseOverloadCleared .1.3.6.1.4.1.318.0.227 "Status Events" Normal
FORMAT APC Rack PDU: Bank or phase overload condition has cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The bank or phase overload condition on a Rack PDU has cleared.
EDESC
#
#
#
EVENT aruDeviceConfigChange .1.3.6.1.4.1.318.0.228 "Status Events" Normal
FORMAT APC ARU [$4]: ARU Device configuration change., Trap Arguments:($#):$* [APC PowerNet]
SDESC
ARU device configuration change.
EDESC
#
#
#
EVENT rmPDUCommunicationLost .1.3.6.1.4.1.318.0.229 "Status Events" Critical
FORMAT APC RM PDU [$1, $2]: Communication Lost., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communication Lost.
EDESC
#
#
#
EVENT emsCommunicationEstablished .1.3.6.1.4.1.318.0.230 "Status Events" Normal
FORMAT APC EMS [$2]: Communications Established., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communication Established.
EDESC
#
#
#
EVENT emsCommunicationLost .1.3.6.1.4.1.318.0.231 "Status Events" Critical
FORMAT APC EMS [$2]: Communications Lost., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communication Lost.
EDESC
#
#
#
EVENT emsProbeConnected .1.3.6.1.4.1.318.0.232 "Status Events" Normal
FORMAT APC EMS [$2]: Probe $3 Connected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Probe $3 Connected.
EDESC
#
#
#
EVENT emsProbeDisconnected .1.3.6.1.4.1.318.0.233 "Status Events" Critical
FORMAT APC EMS [$2]: Probe $3 Disconnected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Probe $3 Disconnected.
EDESC
#
#
#
EVENT emsSensorConnected .1.3.6.1.4.1.318.0.234 "Status Events" Normal
FORMAT APC EMS [$2]: Sensor $3 Connected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Sensor $3 Connected.
EDESC
#
#
#
EVENT emsSensorDisconnected .1.3.6.1.4.1.318.0.235 "Status Events" Critical
FORMAT APC EMS [$2]: Sensor $3 Disconnected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Sensor $3 Disconnected.
EDESC
#
#
#
EVENT emsSensorFault .1.3.6.1.4.1.318.0.236 "Status Events" Critical
FORMAT APC EMS [$2]: Sensor $3 Fault., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Sensor $3 Fault.
EDESC
#
#
#
EVENT emsSensorFaultCleared .1.3.6.1.4.1.318.0.237 "Status Events" Normal
FORMAT APC EMS [$2]: Sensor $3 Fault Cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Sensor $3 Fault Cleared.
EDESC
#
#
#
EVENT emsBeaconConnected .1.3.6.1.4.1.318.0.238 "Status Events" Normal
FORMAT APC EMS [$2]: Beacon Connected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Beacon Connected.
EDESC
#
#
#
EVENT emsBeaconDisconnected .1.3.6.1.4.1.318.0.239 "Status Events" Critical
FORMAT APC EMS [$2]: Beacon Disconnected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Beacon Disconnected.
EDESC
#
#
#
EVENT emsBeaconOn .1.3.6.1.4.1.318.0.240 "Status Events" Normal
FORMAT APC EMS [$2]: Beacon On., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Beacon On.
EDESC
#
#
#
EVENT emsBeaconOff .1.3.6.1.4.1.318.0.241 "Status Events" Normal
FORMAT APC EMS [$2]: Beacon Off., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Beacon Off.
EDESC
#
#
#
EVENT emsMajorAlarm .1.3.6.1.4.1.318.0.242 "Status Events" Critical
FORMAT APC EMS [$2]: Major Alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Major Alarm.
EDESC
#
#
#
EVENT emsMajorAlarmCleared .1.3.6.1.4.1.318.0.243 "Status Events" Normal
FORMAT APC EMS [$2]: Major Alarm Cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Major Alarm Cleared.
EDESC
#
#
#
EVENT emsMinorAlarm .1.3.6.1.4.1.318.0.244 "Status Events" Critical
FORMAT APC EMS [$2]: Minor Alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Minor Alarm.
EDESC
#
#
#
EVENT emsMinorAlarmCleared .1.3.6.1.4.1.318.0.245 "Status Events" Normal
FORMAT APC EMS [$2]: Minor Alarm Cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Minor Alarm Cleared.
EDESC
#
#
#
EVENT emsOutletStateAbnormal .1.3.6.1.4.1.318.0.246 "Status Events" Minor
FORMAT APC EMS [$2]: Outlet $3 to abnormal state $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Outlet $3 to abnormal state $5.
EDESC
#
#
#
EVENT emsOutletStateNormal .1.3.6.1.4.1.318.0.247 "Status Events" Normal
FORMAT APC EMS [$2]: Outlet $3 to normal state $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Outlet $3 to normal state $5.
EDESC
#
#
#
EVENT emsInputContactStateAbnormal .1.3.6.1.4.1.318.0.248 "Status Events" Minor
FORMAT APC EMS [$2]: Contact $3 to abnormal state $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Contact $3 to abnormal state $5.
EDESC
#
#
#
EVENT emsInputContactStateNormal .1.3.6.1.4.1.318.0.249 "Status Events" Normal
FORMAT APC EMS [$2]: Contact $3 to normal state $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Contact $3 to normal state $5.
EDESC
#
#
#
EVENT emsOutputRelayStateAbnormal .1.3.6.1.4.1.318.0.250 "Status Events" Minor
FORMAT APC EMS [$2]: Relay $3 to abnormal state $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Relay $3 to abnormal state $5.
EDESC
#
#
#
EVENT emsOutputRelayStateNormal .1.3.6.1.4.1.318.0.251 "Status Events" Normal
FORMAT APC EMS [$2]: Relay $3 to normal state $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Relay $3 to normal state $5.
EDESC
#
#
#
EVENT emsDeviceConfigChange .1.3.6.1.4.1.318.0.252 "Status Events" Normal
FORMAT APC EMS [$2]: Device configuration change., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A device configuration change has been made on a EMS.
EDESC
#
#
#
EVENT envHighTempThresholdViolation .1.3.6.1.4.1.318.0.253 "Status Events" Critical
FORMAT APC ENV [$2]: Overtemp ($3,$4) on Probe $5)., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Overtemp ($3,$4) on Probe $5.
EDESC
#
#
#
EVENT envHighTempThresholdViolationCleared .1.3.6.1.4.1.318.0.254 "Status Events" Normal
FORMAT APC ENV [$2]: Overtemp ($3,$4) on Probe $5 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Overtemp ($3,$4) on Probe $5 cleared.
EDESC
#
#
#
EVENT envLowTempThresholdViolation .1.3.6.1.4.1.318.0.255 "Status Events" Critical
FORMAT APC ENV [$2]: Undertemp ($3,$4) on Probe $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Undertemp ($3,$4) on Probe $5.
EDESC
#
#
#
EVENT envLowTempThresholdViolationCleared .1.3.6.1.4.1.318.0.256 "Status Events" Normal
FORMAT APC ENV [$2]: Undertemp ($3,$4) on Probe $5 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Undertemp ($3,$4) on Probe $5 cleared.
EDESC
#
#
#
EVENT envHighHumidityThresholdViolation .1.3.6.1.4.1.318.0.257 "Status Events" Critical
FORMAT APC ENV [$2]: Over Humidity ($3) on Probe $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Over Humidity ($3) on Probe $4.
EDESC
#
#
#
EVENT envHighHumidityThresholdViolationCleared .1.3.6.1.4.1.318.0.258 "Status Events" Normal
FORMAT APC ENV [$2]: Over Humidity ($3) on Probe $4 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Over Humidity ($3) on Probe $4 cleared.
EDESC
#
#
#
EVENT envLowHumidityThresholdViolation .1.3.6.1.4.1.318.0.259 "Status Events" Critical
FORMAT APC ENV [$2]: Under Humidity ($3) on Probe $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Under Humidity ($3) on Probe $4.
EDESC
#
#
#
EVENT envLowHumidityThresholdViolationCleared .1.3.6.1.4.1.318.0.260 "Status Events" Normal
FORMAT APC ENV [$2]: Under Humidity ($3) on Probe $4 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Under Humidity ($3) on Probe $4 cleared.
EDESC
#
#
#
EVENT nlCommunicationEstablished .1.3.6.1.4.1.318.0.261 "Status Events" Normal
FORMAT APC NL [$2]: Communication Established., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communication Established.
EDESC
#
#
#
EVENT rPDUCommunicationEstablished .1.3.6.1.4.1.318.0.266 "Status Events" Normal
FORMAT APC Rack PDU: Communication established., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communication with Rack PDU [$2] established.
EDESC
#
#
#
EVENT rPDUCommunicationLost .1.3.6.1.4.1.318.0.267 "Status Events" Critical
FORMAT APC Rack PDU: Communication lost., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communication with Rack PDU [$2] has been lost.
EDESC
#
#
#
EVENT rPDUOutletOn .1.3.6.1.4.1.318.0.268 "Status Events" Normal
FORMAT APC Switched Rack PDU: An outlet has turned on., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Outlet $3 [$4] on Switched Rack PDU [$2] has turned on.
EDESC
#
#
#
EVENT rPDUOutletOff .1.3.6.1.4.1.318.0.269 "Status Events" Normal
FORMAT APC Switched Rack PDU: An outlet has turned off., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Outlet $3 [$4] on Switched Rack PDU [$2] has turned off.
EDESC
#
#
#
EVENT rPDUDeviceConfigChange .1.3.6.1.4.1.318.0.270 "Status Events" Normal
FORMAT APC Rack PDU: Device configuration change made., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Device configuration change made on Rack PDU [$2].
EDESC
#
#
#
EVENT rPDUOutletConfigChange .1.3.6.1.4.1.318.0.271 "Status Events" Normal
FORMAT APC Switched Rack PDU: Outlet configuration change made., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Outlet $3 [$4] configuration change made on Switched Rack PDU [$2].
EDESC
#
#
#
EVENT rPDULowLoad .1.3.6.1.4.1.318.0.272 "Status Events" Minor
FORMAT APC Rack PDU: Violation of low load threshold., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Rack PDU [$2], phase $3 has violated the low load threshold.
EDESC
#
#
#
EVENT rPDULowLoadCleared .1.3.6.1.4.1.318.0.273 "Status Events" Normal
FORMAT APC Rack PDU: Low load condition cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Rack PDU [$2], phase $3 low load condition cleared.
EDESC
#
#
#
EVENT rPDUNearOverload .1.3.6.1.4.1.318.0.274 "Status Events" Minor
FORMAT APC Rack PDU: Near an overload condition., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Rack PDU [$2], phase $3 is near an overload condition.
EDESC
#
#
#
EVENT rPDUNearOverloadCleared .1.3.6.1.4.1.318.0.275 "Status Events" Normal
FORMAT APC Rack PDU: Near overload condition has cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Rack PDU [$2], phase $3 near overload condition has cleared.
EDESC
#
#
#
EVENT rPDUOverload .1.3.6.1.4.1.318.0.276 "Status Events" Critical
FORMAT APC Rack PDU: Overload condition., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Rack PDU [$2], phase $3 is in an overload condition.
EDESC
#
#
#
EVENT rPDUOverloadCleared .1.3.6.1.4.1.318.0.277 "Status Events" Normal
FORMAT APC Rack PDU: Overload condition has cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Rack PDU [$2], phase $3 overload condition has cleared.
EDESC
#
#
#
EVENT rPDUPowerSupply1Fail .1.3.6.1.4.1.318.0.278 "Status Events" Critical
FORMAT APC Rack PDU: Power Supply 1 is in FAIL state., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Power Supply 1 on Rack PDU [$2] is in FAIL state.
EDESC
#
#
#
EVENT rPDUPowerSupply1Ok .1.3.6.1.4.1.318.0.279 "Status Events" Normal
FORMAT APC Rack PDU: Power Supply 1 is operating normally., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Power Supply 1 on Rack PDU [$2] is operating normally.
EDESC
#
#
#
EVENT rPDUPowerSupply2Fail .1.3.6.1.4.1.318.0.280 "Status Events" Critical
FORMAT APC Rack PDU: Power Supply 2 is in FAIL state., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Power Supply 2 on Rack PDU [$2] is in FAIL state.
EDESC
#
#
#
EVENT rPDUPowerSupply2Ok .1.3.6.1.4.1.318.0.281 "Status Events" Normal
FORMAT APC Rack PDU: Power Supply 2 is operating normally., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Power Supply 2 on Rack PDU [$2] is operating normally.
EDESC
#
#
#
EVENT rPDUPhaseConfigChange .1.3.6.1.4.1.318.0.282 "Status Events" Normal
FORMAT APC Rack PDU: Phase configuration change made., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Phase $3 configuration change made on Rack PDU [$2].
EDESC
#
#
#
EVENT rPDUCancelPendingCommand .1.3.6.1.4.1.318.0.283 "Status Events" Normal
FORMAT APC Switched Rack PDU: Cancel Pending Command made., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Cancel Pending Command made for outlet $3 [$4], on Switched Rack PDU $2.
EDESC
#
#
#
EVENT aruAlinkCommunicationEstablished .1.3.6.1.4.1.318.0.284 "Status Events" Normal
FORMAT APC ARU [$4]: Communication Established., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communication Established.
EDESC
#
#
#
EVENT aruAlinkCommunicationLost .1.3.6.1.4.1.318.0.285 "Status Events" Critical
FORMAT APC ARU [$4]: Communication Lost., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communication Lost.
EDESC
#
#
#
EVENT aruFanFail .1.3.6.1.4.1.318.0.286 "Status Events" Critical
FORMAT APC ARU [$4]: Fan Fail., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Fan Fail.
EDESC
#
#
#
EVENT aruFanFailCleared .1.3.6.1.4.1.318.0.287 "Status Events" Normal
FORMAT APC ARU [$4]: Fan Fail Cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Fan Fail Cleared.
EDESC
#
#
#
EVENT aruSmokeAlarm .1.3.6.1.4.1.318.0.288 "Status Events" Critical
FORMAT APC ARU [$4]: Smoke Alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Smoke Alarm.
EDESC
#
#
#
EVENT aruSmokeAlarmCleared .1.3.6.1.4.1.318.0.289 "Status Events" Normal
FORMAT APC ARU [$4]: Smoke Alarm Cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Smoke Alarm Cleared.
EDESC
#
#
#
EVENT aruHighTemperatureAlarm .1.3.6.1.4.1.318.0.290 "Status Events" Minor
FORMAT APC ARU [$4]: High Temperature Alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
High Temperature Alarm.
EDESC
#
#
#
EVENT aruHighTemperatureAlarmCleared .1.3.6.1.4.1.318.0.291 "Status Events" Normal
FORMAT APC ARU [$4]: High Temperature Alarm Cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
High Temperature Alarm Cleared.
EDESC
#
#
#
EVENT aruExhaustTemperatureAlarm .1.3.6.1.4.1.318.0.292 "Status Events" Critical
FORMAT APC ARU [$4]: Exhaust Temperature Alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Exhaust Temperature Alarm.
EDESC
#
#
#
EVENT aruExhaustTemperatureAlarmCleared .1.3.6.1.4.1.318.0.293 "Status Events" Normal
FORMAT APC ARU [$4]: Exhaust Temperature Alarm Cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Exhaust Temperature Alarm Cleared.
EDESC
#
#
#
EVENT envAlinkCommunicationEstablished .1.3.6.1.4.1.318.0.294 "Status Events" Normal
FORMAT APC ENV [$4]: Communication Established., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communication Established.
EDESC
#
#
#
EVENT envAlinkCommunicationLost .1.3.6.1.4.1.318.0.295 "Status Events" Critical
FORMAT APC ENV [$4]: Communication Lost., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communication Lost.
EDESC
#
#
#
EVENT emsAlinkPowerOverload .1.3.6.1.4.1.318.0.296 "Status Events" Critical
FORMAT APC EMS [$2]: Alink Power Overload., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Alink Power Overload.
EDESC
#
#
#
EVENT emsAlinkPowerOverloadCleared .1.3.6.1.4.1.318.0.297 "Status Events" Normal
FORMAT APC EMS [$2]: Alink Power Overload Cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Alink Power Overload Cleared.
EDESC
#
#
#
EVENT upsOutletGroupTurnedOn .1.3.6.1.4.1.318.0.298 "Status Events" Normal
FORMAT APC UPS: Outlet Group $1 turned on., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Outlet Group $1 turned on
EDESC
#
#
#
EVENT upsOutletGroupTurnedOff .1.3.6.1.4.1.318.0.299 "Status Events" Minor
FORMAT APC UPS: Outlet Group $1 turned off., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Outlet Group $1 turned off.
EDESC
#
#
#
EVENT smwCriticalCondition .1.3.6.1.4.1.318.0.300 "Status Events" Critical
FORMAT APC Symmetra MW UPS: A critical condition has been detected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A critical condition has been detected.
EDESC
#
#
#
EVENT smwCriticalConditionCleared .1.3.6.1.4.1.318.0.301 "Status Events" Normal
FORMAT APC Symmetra MW UPS: A critical condition has been cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A critical condition has been cleared.
EDESC
#
#
#
EVENT smwWarningCondition .1.3.6.1.4.1.318.0.302 "Status Events" Minor
FORMAT APC Symmetra MW UPS: A warning condition has been detected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A warning condition has been detected.
EDESC
#
#
#
EVENT smwWarningConditionCleared .1.3.6.1.4.1.318.0.303 "Status Events" Normal
FORMAT APC Symmetra MW UPS: A warning condition has been cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A warning condition has been cleared.
EDESC
#
#
#
EVENT smwInformationalCondition .1.3.6.1.4.1.318.0.304 "Status Events" Normal
FORMAT APC Symmetra MW UPS: Informational condition detected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
An informational condition has been detected.
EDESC
#
#
#
EVENT smwInformationalConditionCleared .1.3.6.1.4.1.318.0.305 "Status Events" Normal
FORMAT APC Symmetra MW UPS: Informational condition cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
An informational condition has been cleared.
EDESC
#
#
#
EVENT airCriticalCondition .1.3.6.1.4.1.318.0.306 "Status Events" Critical
FORMAT APC Air: $1, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Critical condition: $1
EDESC
#
#
#
EVENT airCriticalConditionCleared .1.3.6.1.4.1.318.0.307 "Status Events" Normal
FORMAT APC Air: $1, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Critical condition cleared: $1
EDESC
#
#
#
EVENT airWarningCondition .1.3.6.1.4.1.318.0.308 "Status Events" Minor
FORMAT APC Air: $1, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Warning condition set: $1
EDESC
#
#
#
EVENT airWarningConditionCleared .1.3.6.1.4.1.318.0.309 "Status Events" Normal
FORMAT APC Air: $1, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Warning condition cleared: $1
EDESC
#
#
#
EVENT airInformationalCondition .1.3.6.1.4.1.318.0.310 "Status Events" Normal
FORMAT APC Air: $1, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Informational condition set: $1
EDESC
#
#
#
EVENT airInformationalConditionCleared .1.3.6.1.4.1.318.0.311 "Status Events" Normal
FORMAT APC Air: $1, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Informational condition cleared: $1
EDESC
#
#
#
EVENT xPDUInputVoltageLowAlarm .1.3.6.1.4.1.318.0.312 "Status Events" Critical
FORMAT APC XPDU [$2]: Input voltage $4 below threshold $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Input voltage $4 is below threshold$5.
EDESC
#
#
#
EVENT xPDUInputVoltageLowAlarmCleared .1.3.6.1.4.1.318.0.313 "Status Events" Normal
FORMAT APC XPDU [$2]: Main input low voltage $4 alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Main input voltage $4 alarm cleared.
EDESC
#
#
#
EVENT xPDUInputVoltageHighAlarm .1.3.6.1.4.1.318.0.314 "Status Events" Critical
FORMAT APC XPDU [$2]: Main input voltage $4 above threshold $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Input voltage $4 is above threshold $5.
EDESC
#
#
#
EVENT xPDUInputVoltageHighAlarmCleared .1.3.6.1.4.1.318.0.315 "Status Events" Normal
FORMAT APC XPDU [$2]: Main input high voltage $4 alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Main input high voltage $4 alarm cleared.
EDESC
#
#
#
EVENT xPDUBypassVoltageLowAlarm .1.3.6.1.4.1.318.0.316 "Status Events" Critical
FORMAT APC XPDU [$2]: Bypass voltage $4 below threshold $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Bypass input voltage $4 is below threshold $5.
EDESC
#
#
#
EVENT xPDUBypassVoltageLowAlarmCleared .1.3.6.1.4.1.318.0.317 "Status Events" Normal
FORMAT APC XPDU [$2]: Bypass low voltage $4 alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Bypass input low voltage $4 alarm cleared.
EDESC
#
#
#
EVENT xPDUBypassVoltageHighAlarm .1.3.6.1.4.1.318.0.318 "Status Events" Critical
FORMAT APC XPDU [$2]: Bypass voltage $4 above threshold $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Bypass input voltage $4 is above threshold $5.
EDESC
#
#
#
EVENT xPDUBypassVoltageHighAlarmCleared .1.3.6.1.4.1.318.0.319 "Status Events" Normal
FORMAT APC XPDU [$2]: Bypass high voltage $4 alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Bypass input high voltage $4 alarm cleared.
EDESC
#
#
#
EVENT xPDUOutputVoltageLowAlarm .1.3.6.1.4.1.318.0.320 "Status Events" Critical
FORMAT APC XPDU [$2]: Output voltage $4 below threshold $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output voltage $4 is above threshold $5.
EDESC
#
#
#
EVENT xPDUOutputVoltageLowAlarmCleared .1.3.6.1.4.1.318.0.321 "Status Events" Normal
FORMAT APC XPDU [$2]: Output low voltage $4 alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output low voltage $4 alarm cleared.
EDESC
#
#
#
EVENT xPDUOutputVoltageHighAlarm .1.3.6.1.4.1.318.0.322 "Status Events" Critical
FORMAT APC XPDU [$2]: Output voltage $4 above threshold $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output voltage $4 is above threshold $5.
EDESC
#
#
#
EVENT xPDUOutputVoltageHighAlarmCleared .1.3.6.1.4.1.318.0.323 "Status Events" Normal
FORMAT APC XPDU [$2]: Output high voltage $4 alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output high voltage $4 alarm cleared.
EDESC
#
#
#
EVENT xPDUOutputCurrentLowAlarm .1.3.6.1.4.1.318.0.324 "Status Events" Critical
FORMAT APC XPDU [$2]: Output current $4 below threshold $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output current $4 is below threshold $5.
EDESC
#
#
#
EVENT xPDUOutputCurrentLowAlarmCleared .1.3.6.1.4.1.318.0.325 "Status Events" Normal
FORMAT APC XPDU [$2]: Output low current $4 alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output low current $4 alarm cleared.
EDESC
#
#
#
EVENT xPDUOutputCurrentHighAlarm .1.3.6.1.4.1.318.0.326 "Status Events" Critical
FORMAT APC XPDU [$2]: Output current $4 above threshold $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output current $4 is above threshold $5.
EDESC
#
#
#
EVENT xPDUOutputCurrentHighAlarmCleared .1.3.6.1.4.1.318.0.327 "Status Events" Normal
FORMAT APC XPDU [$2]: Output high current $4 alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output high current $4 alarm cleared.
EDESC
#
#
#
EVENT xPDUOutputFrequencyAlarm .1.3.6.1.4.1.318.0.328 "Status Events" Critical
FORMAT APC XPDU [$2]: Output frequency out-of-range., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output frequency alarm.
EDESC
#
#
#
EVENT xPDUOutputFrequencyAlarmCleared .1.3.6.1.4.1.318.0.329 "Status Events" Normal
FORMAT APC XPDU [$2]: Output frequency in range., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output frequency in range.
EDESC
#
#
#
EVENT xPDUSystemGroundCurrentAlarm .1.3.6.1.4.1.318.0.330 "Status Events" Critical
FORMAT APC XPDU [$2]: Earth ground current $3 above threshold $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Earth ground current $3 is above threshold $4.
EDESC
#
#
#
EVENT xPDUSystemGroundCurrentAlarmCleared .1.3.6.1.4.1.318.0.331 "Status Events" Normal
FORMAT APC XPDU [$2]: Earth ground high current $3 alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Earth ground high current $3 alarm cleared.
EDESC
#
#
#
EVENT xPDUInputContactStateAbnormal .1.3.6.1.4.1.318.0.332 "Status Events" Critical
FORMAT APC XPDU [$2]: Contact $3 to abnormal state $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Input contact $3 to abnormal state $5.
EDESC
#
#
#
EVENT xPDUInputContactStateNormal .1.3.6.1.4.1.318.0.333 "Status Events" Normal
FORMAT APC XPDU [$2]: Contact $3 to normal state $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Input contact $3 to normal state $5.
EDESC
#
#
#
EVENT xPDUOutputNeutralCurrentHighAlarm .1.3.6.1.4.1.318.0.334 "Status Events" Minor
FORMAT APC XPDU [$2]: Output neutral current $3 above threshold $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output neutral current $3 is above threshold $4.
EDESC
#
#
#
EVENT xPDUOutputNeutralCurrentHighAlarmCleared .1.3.6.1.4.1.318.0.335 "Status Events" Normal
FORMAT APC XPDU [$2]: Output neutral high current $3 alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output neutral high current $3 alarm cleared.
EDESC
#
#
#
EVENT xPDUCoolingFanAlarm .1.3.6.1.4.1.318.0.336 "Status Events" Critical
FORMAT APC XPDU [$2]: Cooling fan failure., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Cooling fan failure.
EDESC
#
#
#
EVENT xPDUCoolingFanAlarmCleared .1.3.6.1.4.1.318.0.337 "Status Events" Normal
FORMAT APC XPDU [$2]: Cooling fan alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Cooling fan alarm cleared.
EDESC
#
#
#
EVENT xPDUTransformerTempAlarm .1.3.6.1.4.1.318.0.338 "Status Events" Critical
FORMAT APC XPDU [$2]: Transformer over temp alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Transformer temp alarm.
EDESC
#
#
#
EVENT xPDUTransformerTempAlarmCleared .1.3.6.1.4.1.318.0.339 "Status Events" Normal
FORMAT APC XPDU [$2]: Isolation transformer temperature alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Transformer temp alarm cleared.
EDESC
#
#
#
EVENT xPDUBranchCurrentLowAlarm .1.3.6.1.4.1.318.0.340 "Status Events" Minor
FORMAT APC XPDU [$2]: Branch circuit current $4 below threshold $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Branch circuit current $4 is below threshold $5.
EDESC
#
#
#
EVENT xPDUBranchCurrentLowAlarmCleared .1.3.6.1.4.1.318.0.341 "Status Events" Normal
FORMAT APC XPDU [$2]: Branch circuit low current $3 alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Branch circuit low current $4 alarm cleared.
EDESC
#
#
#
EVENT xPDUBranchCurrentHighAlarm .1.3.6.1.4.1.318.0.342 "Status Events" Minor
FORMAT APC XPDU [$2]: Branch circuit current $4 above threshold $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Branch circuit current $4 is above threshold $5.
EDESC
#
#
#
EVENT xPDUBranchCurrentHighAlarmCleared .1.3.6.1.4.1.318.0.343 "Status Events" Normal
FORMAT APC XPDU [$2]: Branch circuit current $4 alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Branch circuit high current $3 alarm cleared.
EDESC
#
#
#
EVENT xPDUInternalCommError .1.3.6.1.4.1.318.0.344 "Status Events" Critical
FORMAT APC XPDU [$2]: Communication error., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Internal communication error.
EDESC
#
#
#
EVENT emsHardwareStateAbnormal .1.3.6.1.4.1.318.0.345 "Status Events" Critical
FORMAT APC EMS [$2]: Hardware is in an abnormal state., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Hardware is in an abnormal state.
EDESC
#
#
#
EVENT emsHardwareStateNormal .1.3.6.1.4.1.318.0.346 "Status Events" Normal
FORMAT APC EMS [$2]: Hardware is in its normal state., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Hardware is in its normal state.
EDESC
#
#
#
EVENT ceSevereCondition .1.3.6.1.4.1.318.0.347 "Status Events" Critical
FORMAT APC Custom Event #$2: $1, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Severe condition set: $1
EDESC
#
#
#
EVENT ceSevereConditionCleared .1.3.6.1.4.1.318.0.348 "Status Events" Normal
FORMAT APC Custom Event #$2: $1, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Severe condition cleared: $1
EDESC
#
#
#
EVENT ceWarningCondition .1.3.6.1.4.1.318.0.349 "Status Events" Minor
FORMAT APC Custom Event #$2: $1, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Warning condition set: $1
EDESC
#
#
#
EVENT ceWarningConditionCleared .1.3.6.1.4.1.318.0.350 "Status Events" Normal
FORMAT APC Custom Event #$2: $1, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Warning condition cleared: $1
EDESC
#
#
#
EVENT ceInformationalCondition .1.3.6.1.4.1.318.0.351 "Status Events" Normal
FORMAT APC Custom Event #$2: $1, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Informational condition set: $1
EDESC
#
#
#
EVENT ceInformationalConditionCleared .1.3.6.1.4.1.318.0.352 "Status Events" Normal
FORMAT APC Custom Event #$2: $1, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Informational condition cleared: $1
EDESC
#
#
#
EVENT upsInternalOverTemperature .1.3.6.1.4.1.318.0.353 "Status Events" Minor
FORMAT APC UPS: The internal over temperature condition exists., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The internal over temperature condition exists.
EDESC
#
#
#
EVENT upsInternalOverTemperatureCleared .1.3.6.1.4.1.318.0.354 "Status Events" Normal
FORMAT APC UPS: The internal over temperature condition cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The internal over temperature condition cleared.
EDESC
#
#
#
EVENT upsMpuReset .1.3.6.1.4.1.318.0.355 "Status Events" Normal
FORMAT APC UPS: The MPU has been reset., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The MPU has been reset.
EDESC
#
#
#
EVENT upsOutputSwitchClosed .1.3.6.1.4.1.318.0.356 "Status Events" Normal
FORMAT APC UPS: The Output Switch is closed., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The Output Switch is closed.
EDESC
#
#
#
EVENT upsOutputSwitchOpened .1.3.6.1.4.1.318.0.357 "Status Events" Normal
FORMAT APC UPS: The Output Switch is open., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The Output Switch is open.
EDESC
#
#
#
EVENT upsCalibrationStackChanged .1.3.6.1.4.1.318.0.358 "Status Events" Normal
FORMAT APC UPS: A calibration value in the stack was changed., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A calibration value in the stack was changed.
EDESC
#
#
#
EVENT envMaxTempThresholdViolation .1.3.6.1.4.1.318.0.359 "Status Events" Critical
FORMAT APC ENV [$2]: Over max temp ($3,$4) on Probe $5)., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Over max temp ($3,$4) on Probe $5.
EDESC
#
#
#
EVENT envMaxTempThresholdViolationCleared .1.3.6.1.4.1.318.0.360 "Status Events" Normal
FORMAT APC ENV [$2]: Over max temp ($3,$4) on Probe $5 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Over max temp ($3,$4) on Probe $5 cleared.
EDESC
#
#
#
EVENT envMinTempThresholdViolation .1.3.6.1.4.1.318.0.361 "Status Events" Critical
FORMAT APC ENV [$2]: Under min temp ($3,$4) on Probe $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Under min temp ($3,$4) on Probe $5.
EDESC
#
#
#
EVENT envMinTempThresholdViolationCleared .1.3.6.1.4.1.318.0.362 "Status Events" Normal
FORMAT APC ENV [$2]: Under min temp ($3,$4) on Probe $5 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Under min temp ($3,$4) on Probe $5 cleared.
EDESC
#
#
#
EVENT envMaxHumidityThresholdViolation .1.3.6.1.4.1.318.0.363 "Status Events" Critical
FORMAT APC ENV [$2]: Over max Humidity ($3) on Probe $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Over max Humidity ($3) on Probe $4.
EDESC
#
#
#
EVENT envMaxHumidityThresholdViolationCleared .1.3.6.1.4.1.318.0.364 "Status Events" Normal
FORMAT APC ENV [$2]: Over max Humidity ($3) on Probe $4 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Over max Humidity ($3) on Probe $4 cleared.
EDESC
#
#
#
EVENT envMinHumidityThresholdViolation .1.3.6.1.4.1.318.0.365 "Status Events" Critical
FORMAT APC ENV [$2]: Under min Humidity ($3) on Probe $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Under min Humidity ($3) on Probe $4.
EDESC
#
#
#
EVENT envMinHumidityThresholdViolationCleared .1.3.6.1.4.1.318.0.366 "Status Events" Normal
FORMAT APC ENV [$2]: Under min Humidity ($3) on Probe $4 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Under min Humidity ($3) on Probe $4 cleared.
EDESC
#
#
#
EVENT envSTIncTempRateViolation .1.3.6.1.4.1.318.0.367 "Status Events" Critical
FORMAT APC ENV [$2]: ST inc. temp rate ($3,$4) on Probe $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Short-term inc. temp rate violation. ($3,$4) on Probe $5.
EDESC
#
#
#
EVENT envSTIncTempRateViolationCleared .1.3.6.1.4.1.318.0.368 "Status Events" Normal
FORMAT APC ENV [$2]: ST inc. temp rate ($3,$4) on Probe $5 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Short-term inc. temp rate violation ($3,$4) on Probe $5 cleared.
EDESC
#
#
#
EVENT envSTDecTempRateViolation .1.3.6.1.4.1.318.0.369 "Status Events" Critical
FORMAT APC ENV [$2]: ST dec. temp rate ($3,$4) on Probe $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Short-term dec. temp rate violation. ($3,$4) on Probe $5.
EDESC
#
#
#
EVENT envSTDecTempRateViolationCleared .1.3.6.1.4.1.318.0.370 "Status Events" Normal
FORMAT APC ENV [$2]: ST dec. temp rate ($3,$4) on Probe $5 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Short-term dec. temp rate violation ($3,$4) on Probe $5 cleared.
EDESC
#
#
#
EVENT envLTIncTempRateViolation .1.3.6.1.4.1.318.0.371 "Status Events" Critical
FORMAT APC ENV [$2]: LT inc. temp rate ($3,$4) on Probe $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Long-term inc. temp rate violation. ($3,$4) on Probe $5.
EDESC
#
#
#
EVENT envLTIncTempRateViolationCleared .1.3.6.1.4.1.318.0.372 "Status Events" Normal
FORMAT APC ENV [$2]: LT inc. temp rate ($3,$4) on Probe $5 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Long-term inc. temp rate violation ($3,$4) on Probe $5 cleared.
EDESC
#
#
#
EVENT envLTDecTempRateViolation .1.3.6.1.4.1.318.0.373 "Status Events" Critical
FORMAT APC ENV [$2]: LT dec. temp rate ($3,$4) on Probe $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Long-term dec. temp rate violation. ($3,$4) on Probe $5.
EDESC
#
#
#
EVENT envLTDecTempRateViolationCleared .1.3.6.1.4.1.318.0.374 "Status Events" Normal
FORMAT APC ENV [$2]: LT dec. temp rate ($3,$4) on Probe $5 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Long-term dec. temp rate violation ($3,$4) on Probe $5 cleared.
EDESC
#
#
#
EVENT bmsCriticalCondition .1.3.6.1.4.1.318.0.375 "Status Events" Critical
FORMAT APC BMS: $1, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Critical condition: $1
EDESC
#
#
#
EVENT bmsCriticalConditionCleared .1.3.6.1.4.1.318.0.376 "Status Events" Normal
FORMAT APC BMS: $1, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Critical condition cleared: $1
EDESC
#
#
#
EVENT bmsWarningCondition .1.3.6.1.4.1.318.0.377 "Status Events" Minor
FORMAT APC BMS: $1, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Warning condition set: $1
EDESC
#
#
#
EVENT bmsWarningConditionCleared .1.3.6.1.4.1.318.0.378 "Status Events" Normal
FORMAT APC BMS: $1, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Warning condition cleared: $1
EDESC
#
#
#
EVENT bmsInformationalCondition .1.3.6.1.4.1.318.0.379 "Status Events" Normal
FORMAT APC BMS: $1, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Informational condition set: $1
EDESC
#
#
#
EVENT bmsInformationalConditionCleared .1.3.6.1.4.1.318.0.380 "Status Events" Normal
FORMAT APC BMS: $1, Trap Arguments:($#):$* [APC PowerNet]
SDESC
Informational condition cleared: $1
EDESC
#
#
#
EVENT xATSOutputVoltageLowAlarm .1.3.6.1.4.1.318.0.381 "Status Events" Critical
FORMAT APC XATS [$2]: output voltage $4 below threshold $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output voltage $4 is below threshold $5.
EDESC
#
#
#
EVENT xATSOutputVoltageLowAlarmCleared .1.3.6.1.4.1.318.0.382 "Status Events" Normal
FORMAT APC XATS [$2]: output low voltage $4 alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output low voltage $4 alarm cleared.
EDESC
#
#
#
EVENT xATSOutputVoltageHighAlarm .1.3.6.1.4.1.318.0.383 "Status Events" Critical
FORMAT APC XATS [$2]: output voltage $4 above threshold $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output voltage $4 is above threshold $5.
EDESC
#
#
#
EVENT xATSOutputVoltageHighAlarmCleared .1.3.6.1.4.1.318.0.384 "Status Events" Normal
FORMAT APC XATS [$2]: output high voltage $4 alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output high voltage $4 alarm cleared.
EDESC
#
#
#
EVENT xATSOutputCurrentLowAlarm .1.3.6.1.4.1.318.0.385 "Status Events" Critical
FORMAT APC XATS [$2]: output current $4 below threshold $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output current $4 is below threshold $5.
EDESC
#
#
#
EVENT xATSOutputCurrentLowAlarmCleared .1.3.6.1.4.1.318.0.386 "Status Events" Normal
FORMAT APC XATS [$2]: output low current $4 alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output low current $4 alarm cleared.
EDESC
#
#
#
EVENT xATSOutputCurrentHighAlarm .1.3.6.1.4.1.318.0.387 "Status Events" Critical
FORMAT APC XATS [$2]: Output current $4 above threshold $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output current $4 is above threshold $5.
EDESC
#
#
#
EVENT xATSOutputCurrentHighAlarmCleared .1.3.6.1.4.1.318.0.388 "Status Events" Normal
FORMAT APC XATS [$2]: output high current $4 alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output high current $4 alarm cleared.
EDESC
#
#
#
EVENT xATSOutputFrequencyAlarm .1.3.6.1.4.1.318.0.389 "Status Events" Critical
FORMAT APC XATS [$2]: output frequency $3 outside the threshold range $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output frequency is out-of-range.
EDESC
#
#
#
EVENT xATSOutputFrequencyAlarmCleared .1.3.6.1.4.1.318.0.390 "Status Events" Normal
FORMAT APC XATS [$2]: output frequency in range., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Output frequency in range.
EDESC
#
#
#
EVENT xATSInternalCommError .1.3.6.1.4.1.318.0.391 "Status Events" Critical
FORMAT APC XATS [$2]: Communication error., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Internal communication error.
EDESC
#
#
#
EVENT xATSInternalCommErrorCleared .1.3.6.1.4.1.318.0.392 "Status Events" Normal
FORMAT APC XATS [$2]: Communication error cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
ATS Communication error cleared.
EDESC
#
#
#
EVENT xATSDataCommMismatchError .1.3.6.1.4.1.318.0.393 "Status Events" Critical
FORMAT APC XATS [$2]: Data mismatch error., Trap Arguments:($#):$* [APC PowerNet]
SDESC
ATS data mismatch error.
EDESC
#
#
#
EVENT xATSDataCommMismatchErrorCleared .1.3.6.1.4.1.318.0.394 "Status Events" Normal
FORMAT APC XATS [$2]: Data mismatch error cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
ATS data mismatch error cleared.
EDESC
#
#
#
EVENT xATSGenCommLost .1.3.6.1.4.1.318.0.395 "Status Events" Minor
FORMAT APC XATS [$2]: No communication with generator., Trap Arguments:($#):$* [APC PowerNet]
SDESC
ATS/Generator communication lost.
EDESC
#
#
#
EVENT xATSGenCommEstablished .1.3.6.1.4.1.318.0.396 "Status Events" Normal
FORMAT APC XATS [$2]: Communication with generator established., Trap Arguments:($#):$* [APC PowerNet]
SDESC
ATS/generator communication established.
EDESC
#
#
#
EVENT xATSNeutralPosition .1.3.6.1.4.1.318.0.397 "Status Events" Minor
FORMAT APC XATS [$2]: transferred to the neutral position while in $3 mode., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Transferred to neutral.
EDESC
#
#
#
EVENT xATSSwitchTransferEvent .1.3.6.1.4.1.318.0.398 "Status Events" Normal
FORMAT APC XATS [$2]: $5 transfer to source $4 while in $3 mode., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Source-to-Source transfer.
EDESC
#
#
#
EVENT xATSInternalATSFault .1.3.6.1.4.1.318.0.399 "Status Events" Critical
FORMAT APC XATS [$2]: Internal fault detected $3., Trap Arguments:($#):$* [APC PowerNet]
SDESC
ATS internal fault detected.
EDESC
#
#
#
EVENT xATSInternalATSFaultCleared .1.3.6.1.4.1.318.0.400 "Status Events" Normal
FORMAT APC XATS [$2]: Internal fault cleared $3., Trap Arguments:($#):$* [APC PowerNet]
SDESC
ATS internal fault cleared.
EDESC
#
#
#
EVENT xATSEngineStartAsserted .1.3.6.1.4.1.318.0.401 "Status Events" Normal
FORMAT APC XATS [$2]: Engine Start signal asserted., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Engine Start asserted.
EDESC
#
#
#
EVENT xATSEngineStopAsserted .1.3.6.1.4.1.318.0.402 "Status Events" Normal
FORMAT APC XATS [$2]: Engine Stop signal asserted., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Engine Stop asserted.
EDESC
#
#
#
EVENT xATSStartFailure .1.3.6.1.4.1.318.0.403 "Status Events" Critical
FORMAT APC XATS [$2]: Generator failed to start., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator failed to start.
EDESC
#
#
#
EVENT xATSStopFailure .1.3.6.1.4.1.318.0.404 "Status Events" Minor
FORMAT APC XATS [$2]: Generator failed to stop., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator failed to stop.
EDESC
#
#
#
EVENT xATSNotInAutomaticMode .1.3.6.1.4.1.318.0.405 "Status Events" Critical
FORMAT APC XATS [$2]: XATS is not-in-automatic mode., Trap Arguments:($#):$* [APC PowerNet]
SDESC
ATS not in auto.
EDESC
#
#
#
EVENT xATSNotInAutomaticModeCleared .1.3.6.1.4.1.318.0.406 "Status Events" Normal
FORMAT APC XATS [$2]: XATS in auto mode., Trap Arguments:($#):$* [APC PowerNet]
SDESC
ATS in auto mode.
EDESC
#
#
#
EVENT xATSEpoTripped .1.3.6.1.4.1.318.0.407 "Status Events" Critical
FORMAT APC XATS [$2]: Emergency Power Off (EPO) tripped., Trap Arguments:($#):$* [APC PowerNet]
SDESC
EPO tripped.
EDESC
#
#
#
EVENT xATSEpoReset .1.3.6.1.4.1.318.0.408 "Status Events" Normal
FORMAT APC XATS [$2]: Emergency Power Off (EPO) reset., Trap Arguments:($#):$* [APC PowerNet]
SDESC
EPO armed.
EDESC
#
#
#
EVENT xATSEpoTestMode .1.3.6.1.4.1.318.0.409 "Status Events" Minor
FORMAT APC XATS [$2]: Emergency Power Off (EPO) in test mode., Trap Arguments:($#):$* [APC PowerNet]
SDESC
EPO disabled.
EDESC
#
#
#
EVENT xATSEpoArmed .1.3.6.1.4.1.318.0.410 "Status Events" Normal
FORMAT APC XATS [$2]: Emergency Power Off (EPO) enabled., Trap Arguments:($#):$* [APC PowerNet]
SDESC
EPO armed.
EDESC
#
#
#
EVENT xATSTestInitiated .1.3.6.1.4.1.318.0.411 "Status Events" Normal
FORMAT APC XATS [$2]: $3 test initiated., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Test initiated.
EDESC
#
#
#
EVENT xATSTestCanceled .1.3.6.1.4.1.318.0.412 "Status Events" Normal
FORMAT APC XATS [$2]: $3 test canceled., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Test canceled.
EDESC
#
#
#
EVENT xATSTestFailed .1.3.6.1.4.1.318.0.413 "Status Events" Critical
FORMAT APC XATS [$2]: Initiated test failed., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Initiated test failed.
EDESC
#
#
#
EVENT xATSTestPassed .1.3.6.1.4.1.318.0.414 "Status Events" Normal
FORMAT APC XATS [$2]: Initiated test passed., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Initiated test passed.
EDESC
#
#
#
EVENT xATSInputContactStateAbnormal .1.3.6.1.4.1.318.0.415 "Status Events" Critical
FORMAT APC XATS [$2]: Contact $3 changed to abnormal state $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Input contact $3 has changed to its abnormal state $5.
EDESC
#
#
#
EVENT xATSInputContactStateNormal .1.3.6.1.4.1.318.0.416 "Status Events" Normal
FORMAT APC XATS [$2]: Contact $3 changed to normal state $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Input contact $3 has changed to its normal state $5.
EDESC
#
#
#
EVENT xATSRemoteStartContactMismatch .1.3.6.1.4.1.318.0.417 "Status Events" Critical
FORMAT APC XATS [$2]: Generator/ATS start contact mismatch., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator/ATS start contact mismatch.
EDESC
#
#
#
EVENT xATSRemoteStartContactMismatchCleared .1.3.6.1.4.1.318.0.418 "Status Events" Normal
FORMAT APC XATS [$2]: Generator/ATS start contact mismatch cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator/ATS start contact mismatch cleared.
EDESC
#
#
#
EVENT xATSDoorOpenAlarm .1.3.6.1.4.1.318.0.419 "Status Events" Minor
FORMAT APC XATS [$2]: Panel door is open alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Panel door open alarm.
EDESC
#
#
#
EVENT xATSDoorOpenAlarmCleared .1.3.6.1.4.1.318.0.420 "Status Events" Normal
FORMAT APC XATS [$2]: Panel door open alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Panel door open alarm cleared.
EDESC
#
#
#
EVENT xATSDCBackupAlarm .1.3.6.1.4.1.318.0.421 "Status Events" Minor
FORMAT APC XATS [$2]: DC backup failure., Trap Arguments:($#):$* [APC PowerNet]
SDESC
ATS DC backup failure.
EDESC
#
#
#
EVENT xATSDCBackupAlarmCleared .1.3.6.1.4.1.318.0.422 "Status Events" Normal
FORMAT APC XATS [$2]: DC backup alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
DC backup alarm cleared.
EDESC
#
#
#
EVENT xATSGeneratorLowCoolantLevelAlarm .1.3.6.1.4.1.318.0.423 "Status Events" Critical
FORMAT APC XGEN [$2]: Generator low coolant level alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator low coolant level alarm.
EDESC
#
#
#
EVENT xATSGeneratorLowCoolantLevelAlarmCleared .1.3.6.1.4.1.318.0.424 "Status Events" Normal
FORMAT APC XGEN [$2]: Generator low coolant level alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator low coolant level alarm cleared.
EDESC
#
#
#
EVENT xATSGeneratorVeryLowCoolantLevelAlarm .1.3.6.1.4.1.318.0.425 "Status Events" Critical
FORMAT APC XGEN [$2]: Generator very low coolant level alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator very low coolant level alarm.
EDESC
#
#
#
EVENT xATSGeneratorVeryLowCoolantLevelAlarmCleared .1.3.6.1.4.1.318.0.426 "Status Events" Normal
FORMAT APC XGEN [$2]: Generator very low coolant level alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator very low coolant level alarm cleared.
EDESC
#
#
#
EVENT xATSGeneratorHighCoolantTempAlarm .1.3.6.1.4.1.318.0.427 "Status Events" Critical
FORMAT APC XGEN [$2]: Generator high coolant temperature alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator high coolant temperature alarm.
EDESC
#
#
#
EVENT xATSGeneratorHighCoolantTempAlarmCleared .1.3.6.1.4.1.318.0.428 "Status Events" Normal
FORMAT APC XGEN [$2]: Generator high coolant temperature alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator high coolant temperature alarm cleared.
EDESC
#
#
#
EVENT xATSGeneratorVeryHighCoolantTempAlarm .1.3.6.1.4.1.318.0.429 "Status Events" Critical
FORMAT APC XGEN [$2]: Generator very high coolant temperature alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator very high coolant temperature alarm.
EDESC
#
#
#
EVENT xATSGeneratorVeryHighCoolantTempAlarmCleared .1.3.6.1.4.1.318.0.430 "Status Events" Normal
FORMAT APC XGEN [$2]: Generator very high coolant temperature alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator very high coolant temperature alarm cleared.
EDESC
#
#
#
EVENT xATSGeneratorLowCoolantTempAlarm .1.3.6.1.4.1.318.0.431 "Status Events" Minor
FORMAT APC XGEN [$2]: Generator low coolant temperature alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator low coolant temperature alarm.
EDESC
#
#
#
EVENT xATSGeneratorLowCoolantTempAlarmCleared .1.3.6.1.4.1.318.0.432 "Status Events" Normal
FORMAT APC XGEN [$2]: Generator low coolant temperature alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator low coolant temperature alarm cleared.
EDESC
#
#
#
EVENT xATSGeneratorLowOilLevelAlarm .1.3.6.1.4.1.318.0.433 "Status Events" Critical
FORMAT APC XGEN [$2]: Generator low oil level alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator low oil level alarm.
EDESC
#
#
#
EVENT xATSGeneratorLowOilLevelAlarmCleared .1.3.6.1.4.1.318.0.434 "Status Events" Normal
FORMAT APC XGEN [$2]: Generator low oil level alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator low oil level alarm cleared.
EDESC
#
#
#
EVENT xATSGeneratorLowBatteryVoltDuringCrankAlarm .1.3.6.1.4.1.318.0.435 "Status Events" Critical
FORMAT APC XGEN [$2]: Low battery voltage while cranking alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator low battery volts while cranking alarm.
EDESC
#
#
#
EVENT xATSGeneratorLowBatteryVoltDuringCrankAlarmCleared .1.3.6.1.4.1.318.0.436 "Status Events" Normal
FORMAT APC XGEN [$2]: Low battery voltage while cranking alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator low battery volts while cranking alarm cleared.
EDESC
#
#
#
EVENT xATSGeneratorVeryLowBatteryVoltDuringCrankAlarm .1.3.6.1.4.1.318.0.437 "Status Events" Critical
FORMAT APC XGEN [$2]: Generator v.low battery voltage while cranking alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator v.low battery volts while cranking alarm.
EDESC
#
#
#
EVENT xATSGeneratorVeryLowBatteryVoltDuringCrankAlarmCleared .1.3.6.1.4.1.318.0.438 "Status Events" Normal
FORMAT APC XGEN [$2]: Generator v.low battery voltage while cranking alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator v.low battery volts while cranking alarm cleared.
EDESC
#
#
#
EVENT xATSGeneratorEStop .1.3.6.1.4.1.318.0.439 "Status Events" Critical
FORMAT APC XGEN [$2]: Generator emergency stop engaged., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator emergency stop engaged.
EDESC
#
#
#
EVENT xATSGeneratorEStopCleared .1.3.6.1.4.1.318.0.440 "Status Events" Normal
FORMAT APC XGEN [$2]: Generator emergency stop condition cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator emergency stop condition cleared.
EDESC
#
#
#
EVENT xATSGeneratorHighBatteryVolt .1.3.6.1.4.1.318.0.441 "Status Events" Minor
FORMAT APC XGEN [$2]: Generator high battery voltage., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator high battery volts.
EDESC
#
#
#
EVENT xATSGeneratorHighBatteryVoltCleared .1.3.6.1.4.1.318.0.442 "Status Events" Normal
FORMAT APC XGEN [$2]: Generator high battery voltage condition cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator high battery volts condition cleared.
EDESC
#
#
#
EVENT xATSGeneratorLowBatteryVolt .1.3.6.1.4.1.318.0.443 "Status Events" Critical
FORMAT APC XGEN [$2]: Generator low battery voltage., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator low battery volts.
EDESC
#
#
#
EVENT xATSGeneratorLowBatteryVoltCleared .1.3.6.1.4.1.318.0.444 "Status Events" Normal
FORMAT APC XGEN [$2]: Generator low battery voltage condition cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator low battery volts condition cleared.
EDESC
#
#
#
EVENT xATSGeneratorControlSwitchNotAuto .1.3.6.1.4.1.318.0.445 "Status Events" Critical
FORMAT APC XGEN [$2]: Generator not-in-automatic mode., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator not-in-auto.
EDESC
#
#
#
EVENT xATSGeneratorControlSwitchNotAutoCleared .1.3.6.1.4.1.318.0.446 "Status Events" Normal
FORMAT APC XGEN [$2]: Generator automatic mode restored., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator not-in-auto cleared.
EDESC
#
#
#
EVENT xATSGeneratorLowOilPressure .1.3.6.1.4.1.318.0.447 "Status Events" Critical
FORMAT APC XGEN [$2]: Generator low oil pressure., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator low oil pressure.
EDESC
#
#
#
EVENT xATSGeneratorLowOilPressureCleared .1.3.6.1.4.1.318.0.448 "Status Events" Normal
FORMAT APC XGEN [$2]: Generator low oil pressure condition cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator low oil pressure condition cleared.
EDESC
#
#
#
EVENT xATSGeneratorVeryLowOilPressure .1.3.6.1.4.1.318.0.449 "Status Events" Critical
FORMAT APC XGEN [$2]: Generator v.low oil pressure., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator v.low oil pressure.
EDESC
#
#
#
EVENT xATSGeneratorVeryLowOilPressureCleared .1.3.6.1.4.1.318.0.450 "Status Events" Normal
FORMAT APC XGEN [$2]: Generator v.low oil pressure condition cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator v.low oil pressure condition cleared.
EDESC
#
#
#
EVENT xATSGeneratorOverload .1.3.6.1.4.1.318.0.451 "Status Events" Critical
FORMAT APC XGEN [$2]: Generator is in overload event., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator on overload event.
EDESC
#
#
#
EVENT xATSGeneratorOverloadCleared .1.3.6.1.4.1.318.0.452 "Status Events" Normal
FORMAT APC XGEN [$2]: Generator is in overload event cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator on overload event cleared.
EDESC
#
#
#
EVENT xATSGeneratorLowACVEvent .1.3.6.1.4.1.318.0.453 "Status Events" Critical
FORMAT APC XGEN [$2]: State of the Generator AC voltage., Trap Arguments:($#):$* [APC PowerNet]
SDESC
State of the Generator AC voltage.
EDESC
#
#
#
EVENT xATSGeneratorLowACVEventCleared .1.3.6.1.4.1.318.0.454 "Status Events" Normal
FORMAT APC XGEN [$2]: State of the Generator AC voltage cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
State of the Generator AC voltage cleared.
EDESC
#
#
#
EVENT xATSGeneratorHighACVEvent .1.3.6.1.4.1.318.0.455 "Status Events" Critical
FORMAT APC XGEN [$2]: State of the Generator AC voltage., Trap Arguments:($#):$* [APC PowerNet]
SDESC
State of the Generator AC voltage.
EDESC
#
#
#
EVENT xATSGeneratorHighACVEventCleared .1.3.6.1.4.1.318.0.456 "Status Events" Normal
FORMAT APC XGEN [$2]: State of the Generator AC voltage cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
State of the Generator AC voltage cleared.
EDESC
#
#
#
EVENT xATSGeneratorOverspeed .1.3.6.1.4.1.318.0.457 "Status Events" Critical
FORMAT APC XGEN [$2]: Generator overspeed condition., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator overspeed condition.
EDESC
#
#
#
EVENT xATSGeneratorOverspeedCleared .1.3.6.1.4.1.318.0.458 "Status Events" Normal
FORMAT APC XGEN [$2]: Generator overspeed condition cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator overspeed condition cleared.
EDESC
#
#
#
EVENT xATSGeneratorEngineCold .1.3.6.1.4.1.318.0.459 "Status Events" Critical
FORMAT APC XGEN [$2]: Generator engine is cold, may not start., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator engine is cold.
EDESC
#
#
#
EVENT xATSGeneratorEngineColdCleared .1.3.6.1.4.1.318.0.460 "Status Events" Normal
FORMAT APC XGEN [$2]: Engine is cold to start condition cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Engine is cold to start condition cleared.
EDESC
#
#
#
EVENT xATSGeneratorOutputBreakerOpen .1.3.6.1.4.1.318.0.461 "Status Events" Critical
FORMAT APC XGEN [$2]: Generator output breaker open alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator output breaker open.
EDESC
#
#
#
EVENT xATSGeneratorOutputBreakerOpenCleared .1.3.6.1.4.1.318.0.462 "Status Events" Normal
FORMAT APC XGEN [$2]: Generator output breaker open alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator output breaker open cleared.
EDESC
#
#
#
EVENT xATSGeneratorLowFuelLevelAlarm .1.3.6.1.4.1.318.0.463 "Status Events" Minor
FORMAT APC XGEN [$2]: Low fuel level alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator low fuel level alarm.
EDESC
#
#
#
EVENT xATSGeneratorLowFuelLevelAlarmCleared .1.3.6.1.4.1.318.0.464 "Status Events" Normal
FORMAT APC XGEN [$2]: Low fuel level alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator low fuel level alarm cleared.
EDESC
#
#
#
EVENT xATSGeneratorVeryLowFuelLevelAlarm .1.3.6.1.4.1.318.0.465 "Status Events" Critical
FORMAT APC XGEN [$2]: Very Low fuel level alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator very low fuel level alarm.
EDESC
#
#
#
EVENT xATSGeneratorVeryLowFuelLevelAlarmCleared .1.3.6.1.4.1.318.0.466 "Status Events" Normal
FORMAT APC XGEN [$2]: Very Low fuel level alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator very low fuel level alarm cleared.
EDESC
#
#
#
EVENT xATSGeneratorLowRunTimeAlarm .1.3.6.1.4.1.318.0.467 "Status Events" Minor
FORMAT APC XGEN [$2]: Low run time alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator low run time alarm.
EDESC
#
#
#
EVENT xATSGeneratorLowRunTimeAlarmCleared .1.3.6.1.4.1.318.0.468 "Status Events" Normal
FORMAT APC XGEN [$2]: Low run time alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator low run time alarm.
EDESC
#
#
#
EVENT xATSGeneratorVeryLowRunTimeAlarm .1.3.6.1.4.1.318.0.469 "Status Events" Critical
FORMAT APC XGEN [$2]: Very low run time alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator very low run time alarm.
EDESC
#
#
#
EVENT xATSGeneratorVeryLowRunTimeAlarmCleared .1.3.6.1.4.1.318.0.470 "Status Events" Normal
FORMAT APC XGEN [$2]: Very low run time alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator very low run time alarm.
EDESC
#
#
#
EVENT xATSGeneratorServiceDueAlarm .1.3.6.1.4.1.318.0.471 "Status Events" Minor
FORMAT APC XATS [$2]: Generator scheduled maintenance is due., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator maintenance due.
EDESC
#
#
#
EVENT xATSGeneratorServiceDueAlarmCleared .1.3.6.1.4.1.318.0.472 "Status Events" Normal
FORMAT APC XATS [$2]: Generator service due alarm is cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator service alarm is cleared.
EDESC
#
#
#
EVENT xATSGeneratorShutdown .1.3.6.1.4.1.318.0.473 "Status Events" Critical
FORMAT APC XGEN [$2]: Generator shutdown., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator shutdown
EDESC
#
#
#
EVENT xATSGeneratorShutdownCleared .1.3.6.1.4.1.318.0.474 "Status Events" Normal
FORMAT APC XGEN [$2]: Generator shutdown is cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator shutdown is cleared.
EDESC
#
#
#
EVENT xATSGeneratorBatteryCharger .1.3.6.1.4.1.318.0.475 "Status Events" Critical
FORMAT APC XGEN [$2]: Generator batt. charger is nonfunctional., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator battery charger is nonfunctional
EDESC
#
#
#
EVENT xATSGeneratorBatteryChargerCleared .1.3.6.1.4.1.318.0.476 "Status Events" Normal
FORMAT APC XGEN [$2]: Fault in the generator battery charger is cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Fault in the generator battery charger is cleared.
EDESC
#
#
#
EVENT xATSGeneratorGenericEvent .1.3.6.1.4.1.318.0.477 "Status Events" Minor
FORMAT APC XGEN [$2]: Generator generic event., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator generic event.
EDESC
#
#
#
EVENT xATSGeneratorGenericEventCleared .1.3.6.1.4.1.318.0.478 "Status Events" Normal
FORMAT APC XGEN [$2]: Generic generator event is cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generic generator event is cleared.
EDESC
#
#
#
EVENT xPDUInternalCommErrorCleared .1.3.6.1.4.1.318.0.479 "Status Events" Normal
FORMAT APC XPDU [$2]: Communication error cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
PDU Communication error cleared.
EDESC
#
#
#
EVENT xPDUSystemStateAlarm .1.3.6.1.4.1.318.0.480 "Status Events" Critical
FORMAT APC XPDU [$2]: System state change alarm $3., Trap Arguments:($#):$* [APC PowerNet]
SDESC
PDU state change alarm $3.
EDESC
#
#
#
EVENT xPDUSystemStateAlarmCleared .1.3.6.1.4.1.318.0.481 "Status Events" Normal
FORMAT APC XPDU [$2]: Normal system state change $3., Trap Arguments:($#):$* [APC PowerNet]
SDESC
PDU normal state change $3.
EDESC
#
#
#
EVENT xPDUEpoTestMode .1.3.6.1.4.1.318.0.482 "Status Events" Minor
FORMAT APC XPDU [$2]: Emergency Power Off (EPO) in test mode., Trap Arguments:($#):$* [APC PowerNet]
SDESC
EPO disabled.
EDESC
#
#
#
EVENT xPDUEpoArmed .1.3.6.1.4.1.318.0.483 "Status Events" Normal
FORMAT APC XPDU [$2]: Emergency Power Off (EPO) enabled., Trap Arguments:($#):$* [APC PowerNet]
SDESC
EPO armed.
EDESC
#
#
#
EVENT xPDUFuseBlownAlarm .1.3.6.1.4.1.318.0.484 "Status Events" Critical
FORMAT APC XPDU [$2]: Check fuse $3., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Fuse $3 detected opened.
EDESC
#
#
#
EVENT xPDUFuseBlownAlarmCleared .1.3.6.1.4.1.318.0.485 "Status Events" Normal
FORMAT APC XPDU [$2]: Check fuse $3 alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Fuse $3 alarm cleared.
EDESC
#
#
#
EVENT xPDUBreakerPositionAlarm .1.3.6.1.4.1.318.0.486 "Status Events" Critical
FORMAT APC XPDU [$2]: Breaker $3 alarm $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Breaker $3 position alarm $4.
EDESC
#
#
#
EVENT xPDUBreakerPositionAlarmCleared .1.3.6.1.4.1.318.0.487 "Status Events" Normal
FORMAT APC XPDU [$2]: Breaker position alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Breaker $3 alarm cleared $4.
EDESC
#
#
#
EVENT xPDUBreakerChangeEvent .1.3.6.1.4.1.318.0.488 "Status Events" Normal
FORMAT APC XPDU [$2]: Breaker $3 changed $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Breaker/switch event.
EDESC
#
#
#
EVENT xPDUDataCommMismatchError .1.3.6.1.4.1.318.0.489 "Status Events" Critical
FORMAT APC XPDU [$2]: Data mismatch error., Trap Arguments:($#):$* [APC PowerNet]
SDESC
XPDU data mismatch error.
EDESC
#
#
#
EVENT xPDUDataCommMismatchErrorCleared .1.3.6.1.4.1.318.0.490 "Status Events" Normal
FORMAT APC XPDU [$2]: Data mismatch error cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
XPDU data mismatch error cleared.
EDESC
#
#
#
EVENT xPDUSystemInMaintenanceBypassMode .1.3.6.1.4.1.318.0.491 "Status Events" Minor
FORMAT APC XPDU [$2]: System state changed to maintenance bypass., Trap Arguments:($#):$* [APC PowerNet]
SDESC
PDU state changed to maintenance bypass.
EDESC
#
#
#
EVENT xPDUSystemInUPSOperationalMode .1.3.6.1.4.1.318.0.492 "Status Events" Normal
FORMAT APC XPDU [$2]: System state changed to UPS operational., Trap Arguments:($#):$* [APC PowerNet]
SDESC
PDU state changed to UPS operational.
EDESC
#
#
#
EVENT xATSGeneratorFuelTankRuptureAlarm .1.3.6.1.4.1.318.0.493 "Status Events" Minor
FORMAT APC XGEN [$2]: Generator inner wall rupture alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator inner wall rupture alarm.
EDESC
#
#
#
EVENT xATSGeneratorFuelTankRuptureAlarmCleared .1.3.6.1.4.1.318.0.494 "Status Events" Normal
FORMAT APC XGEN [$2]: Generator inner wall rupture alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator inner wall rupture alarm cleared.
EDESC
#
#
#
EVENT xATSGeneratorGroundFaultAlarm .1.3.6.1.4.1.318.0.495 "Status Events" Critical
FORMAT APC XGEN [$2]: Generator ground fault alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator ground fault alarm.
EDESC
#
#
#
EVENT xATSGeneratorGroundFaultAlarmCleared .1.3.6.1.4.1.318.0.496 "Status Events" Normal
FORMAT APC XGEN [$2]: Generator ground fault alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Generator ground fault alarm cleared.
EDESC
#
#
#
EVENT xATSOutputLoadPoweredByGeneratorAlarm .1.3.6.1.4.1.318.0.497 "Status Events" Minor
FORMAT APC XATS [$2]: System load powered by generator alarm., Trap Arguments:($#):$* [APC PowerNet]
SDESC
System load powered by generator.
EDESC
#
#
#
EVENT xATSOutputLoadPoweredByGeneratorAlarmCleared .1.3.6.1.4.1.318.0.498 "Status Events" Normal
FORMAT APC XATS [$2]: System load powered by generator alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
System load powered by generator alarm cleared.
EDESC
#
#
#
EVENT xAPCControllerFirmwareUpdateTransferStart .1.3.6.1.4.1.318.0.499 "Status Events" Normal
FORMAT APC [$2]: Start update transfer., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Start update transfer.
EDESC
#
#
#
EVENT xAPCControllerFirmwareUpdateTransferComplete .1.3.6.1.4.1.318.0.500 "Status Events" Normal
FORMAT APC [$2]: update transfer complete., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Update transfer complete.
EDESC
#
#
#
EVENT xAPCControllerFirmwareUpdateTransferFailed .1.3.6.1.4.1.318.0.501 "Status Events" Critical
FORMAT APC [$2]: Update transfer failed., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Update transfer failed.
EDESC
#
#
#
EVENT upsPfcInputRelayFailure .1.3.6.1.4.1.318.0.502 "Status Events" Minor
FORMAT APC UPS: The PFC input relay failure exists., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The PFC (Power Factor Correction) input relay failure exists.
EDESC
#
#
#
EVENT upsPfcInputRelayFailureCleared .1.3.6.1.4.1.318.0.503 "Status Events" Normal
FORMAT APC UPS: The PFC input relay failure cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The PFC (Power Factor Correction) input relay failure cleared.
EDESC
#
#
#
EVENT upsInverterOverTemperature .1.3.6.1.4.1.318.0.504 "Status Events" Minor
FORMAT APC UPS: The inverter over temperature condition exists., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The inverter over temperature condition exists.
EDESC
#
#
#
EVENT upsInverterOverTemperatureCleared .1.3.6.1.4.1.318.0.505 "Status Events" Normal
FORMAT APC UPS: The inverter over temperature condition cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The inverter over temperature condition cleared.
EDESC
#
#
#
EVENT upsBatteryOverVoltage .1.3.6.1.4.1.318.0.506 "Status Events" Minor
FORMAT APC UPS: The battery over voltage condition exists., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The battery over voltage condition exists.
EDESC
#
#
#
EVENT upsBatteryOverVoltageCleared .1.3.6.1.4.1.318.0.507 "Status Events" Normal
FORMAT APC UPS: The battery over voltage condition cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The battery over voltage condition cleared.
EDESC
#
#
#
EVENT upsEepromFault .1.3.6.1.4.1.318.0.508 "Status Events" Minor
FORMAT APC UPS: The EEPROM fault exists., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The EEPROM fault exists.
EDESC
#
#
#
EVENT upsEepromFaultCleared .1.3.6.1.4.1.318.0.509 "Status Events" Normal
FORMAT APC UPS: The EEPROM fault cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The EEPROM fault cleared.
EDESC
#
#
#
EVENT aruFanRuntimeAlarm .1.3.6.1.4.1.318.0.510 "Status Events" Minor
FORMAT APC ARU [$4]: Fan [$5] Runhour has Exceeded its Threshold., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Fan Runhour Alarm.
EDESC
#
#
#
EVENT aruFanRuntimeAlarmCleared .1.3.6.1.4.1.318.0.511 "Status Events" Normal
FORMAT APC ARU [$4]: Fan [$5] Runhour Alarm Cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Fan Runhour Alarm Cleared.
EDESC
#
#
#
EVENT aruFanPoorPerformanceAlarm .1.3.6.1.4.1.318.0.512 "Status Events" Minor
FORMAT APC ARU [$4]: Fan [$5] Poor Performance Detected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Fan Health Alarm.
EDESC
#
#
#
EVENT aruFanPoorPerformanceAlarmCleared .1.3.6.1.4.1.318.0.513 "Status Events" Normal
FORMAT APC ARU [$4]: Fan [$5] Performance Restored., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Fan Health Alarm Cleared.
EDESC
#
#
#
EVENT aruRedundantPowerLostAlarm .1.3.6.1.4.1.318.0.514 "Status Events" Minor
FORMAT APC ARU [$4]: Redundant AC Input has been Lost., Trap Arguments:($#):$* [APC PowerNet]
SDESC
AC Redundancy Lost.
EDESC
#
#
#
EVENT aruRedundantPowerLostAlarmCleared .1.3.6.1.4.1.318.0.515 "Status Events" Normal
FORMAT APC ARU [$4]: Redundant AC Input has been Restored., Trap Arguments:($#):$* [APC PowerNet]
SDESC
AC Redundancy Restored.
EDESC
#
#
#
EVENT apcDeviceConfigChange .1.3.6.1.4.1.318.0.516 "Status Events" Normal
FORMAT APC [$2]: Device configuration change., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A device configuration change has been made on a device.
EDESC
#
#
#
EVENT apcEnvSensorConnected .1.3.6.1.4.1.318.0.517 "Status Events" Normal
FORMAT APC ENV [$2]: Sensor $4 Connected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Sensor $4 Connected.
EDESC
#
#
#
EVENT apcEnvSensorDisconnected .1.3.6.1.4.1.318.0.518 "Status Events" Critical
FORMAT APC ENV [$2]: Sensor $4 Disconnected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Sensor $4 Disconnected.
EDESC
#
#
#
EVENT apcEnvMaxTempThresholdViolation .1.3.6.1.4.1.318.0.519 "Status Events" Critical
FORMAT APC ENV [$2]: Over max temp on Sensor $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Over max temp on Sensor $5.
EDESC
#
#
#
EVENT apcEnvMaxTempThresholdViolationCleared .1.3.6.1.4.1.318.0.520 "Status Events" Normal
FORMAT APC ENV [$2]: Over max temp on Sensor $4 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Over max temp on Sensor $4 cleared.
EDESC
#
#
#
EVENT apcEnvHighTempThresholdViolation .1.3.6.1.4.1.318.0.521 "Status Events" Minor
FORMAT APC ENV [$2]: Overtemp on Sensor $4)., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Overtemp on Sensor $4.
EDESC
#
#
#
EVENT apcEnvHighTempThresholdViolationCleared .1.3.6.1.4.1.318.0.522 "Status Events" Normal
FORMAT APC ENV [$2]: Overtemp on Sensor $4 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Overtemp on Sensor $4 cleared.
EDESC
#
#
#
EVENT apcEnvLowTempThresholdViolation .1.3.6.1.4.1.318.0.523 "Status Events" Minor
FORMAT APC ENV [$2]: Undertemp on Sensor $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Undertemp on Sensor $4.
EDESC
#
#
#
EVENT apcEnvLowTempThresholdViolationCleared .1.3.6.1.4.1.318.0.524 "Status Events" Normal
FORMAT APC ENV [$2]: Undertemp on Sensor $4 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Undertemp on Sensor $4 cleared.
EDESC
#
#
#
EVENT apcEnvMinTempThresholdViolation .1.3.6.1.4.1.318.0.525 "Status Events" Critical
FORMAT APC ENV [$2]: Under min temp on Sensor $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Under min temp on Sensor $4.
EDESC
#
#
#
EVENT apcEnvMinTempThresholdViolationCleared .1.3.6.1.4.1.318.0.526 "Status Events" Normal
FORMAT APC ENV [$2]: Under min temp on Sensor $4 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Under min temp on Sensor $4 cleared.
EDESC
#
#
#
EVENT apcEnvSTIncTempRateViolation .1.3.6.1.4.1.318.0.527 "Status Events" Critical
FORMAT APC ENV [$2]: ST inc. temp rate on Sensor $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Short-term inc. temp rate violation. on Sensor $4.
EDESC
#
#
#
EVENT apcEnvSTIncTempRateViolationCleared .1.3.6.1.4.1.318.0.528 "Status Events" Normal
FORMAT APC ENV [$2]: ST inc. temp rate on Sensor $4 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Short-term inc. temp rate violation on Sensor $4 cleared.
EDESC
#
#
#
EVENT apcEnvSTDecTempRateViolation .1.3.6.1.4.1.318.0.529 "Status Events" Critical
FORMAT APC ENV [$2]: ST dec. temp rate on Sensor $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Short-term dec. temp rate violation. on Sensor $4.
EDESC
#
#
#
EVENT apcEnvSTDecTempRateViolationCleared .1.3.6.1.4.1.318.0.530 "Status Events" Normal
FORMAT APC ENV [$2]: ST dec. temp rate on Sensor $4 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Short-term dec. temp rate violation on Sensor $4 cleared.
EDESC
#
#
#
EVENT apcEnvLTIncTempRateViolation .1.3.6.1.4.1.318.0.531 "Status Events" Critical
FORMAT APC ENV [$2]: LT inc. temp rate on Sensor $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Long-term inc. temp rate violation. on Sensor $4.
EDESC
#
#
#
EVENT apcEnvLTIncTempRateViolationCleared .1.3.6.1.4.1.318.0.532 "Status Events" Normal
FORMAT APC ENV [$2]: LT inc. temp rate on Sensor $4 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Long-term inc. temp rate violation on Sensor $4 cleared.
EDESC
#
#
#
EVENT apcEnvLTDecTempRateViolation .1.3.6.1.4.1.318.0.533 "Status Events" Critical
FORMAT APC ENV [$2]: LT dec. temp rate on Sensor $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Long-term dec. temp rate violation. on Sensor $4.
EDESC
#
#
#
EVENT apcEnvLTDecTempRateViolationCleared .1.3.6.1.4.1.318.0.534 "Status Events" Normal
FORMAT APC ENV [$2]: LT dec. temp rate on Sensor $4 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Long-term dec. temp rate violation on Sensor $4 cleared.
EDESC
#
#
#
EVENT apcEnvMaxHumidityThresholdViolation .1.3.6.1.4.1.318.0.535 "Status Events" Critical
FORMAT APC ENV [$2]: Over max Humidity on Sensor $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Over max Humidity on Sensor $4.
EDESC
#
#
#
EVENT apcEnvMaxHumidityThresholdViolationCleared .1.3.6.1.4.1.318.0.536 "Status Events" Normal
FORMAT APC ENV [$2]: Over max Humidity on Sensor $4 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Over max Humidity on Sensor $4 cleared.
EDESC
#
#
#
EVENT apcEnvHighHumidityThresholdViolation .1.3.6.1.4.1.318.0.537 "Status Events" Minor
FORMAT APC ENV [$2]: Over Humidity on Sensor $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Over Humidity on Sensor $4.
EDESC
#
#
#
EVENT apcEnvHighHumidityThresholdViolationCleared .1.3.6.1.4.1.318.0.538 "Status Events" Normal
FORMAT APC ENV [$2]: Over Humidity on Sensor $4 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Over Humidity on Sensor $4 cleared.
EDESC
#
#
#
EVENT apcEnvLowHumidityThresholdViolation .1.3.6.1.4.1.318.0.539 "Status Events" Minor
FORMAT APC ENV [$2]: Under Humidity on Sensor $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Under Humidity on Sensor $4.
EDESC
#
#
#
EVENT apcEnvLowHumidityThresholdViolationCleared .1.3.6.1.4.1.318.0.540 "Status Events" Normal
FORMAT APC ENV [$2]: Under Humidity on Sensor $4 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Under Humidity on Sensor $4 cleared.
EDESC
#
#
#
EVENT apcEnvMinHumidityThresholdViolation .1.3.6.1.4.1.318.0.541 "Status Events" Critical
FORMAT APC ENV [$2]: Under min Humidity on Sensor $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Under min Humidity on Sensor $4.
EDESC
#
#
#
EVENT apcEnvMinHumidityThresholdViolationCleared .1.3.6.1.4.1.318.0.542 "Status Events" Normal
FORMAT APC ENV [$2]: Under min Humidity on Sensor $4 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Under min Humidity on Sensor $4 cleared.
EDESC
#
#
#
EVENT apcBeaconConnected .1.3.6.1.4.1.318.0.543 "Status Events" Normal
FORMAT APC [$2]: Beacon Connected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Beacon Connected.
EDESC
#
#
#
EVENT apcBeaconDisconnected .1.3.6.1.4.1.318.0.544 "Status Events" Critical
FORMAT APC [$2]: Beacon Disconnected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Beacon Disconnected.
EDESC
#
#
#
EVENT apcBeaconOn .1.3.6.1.4.1.318.0.545 "Status Events" Normal
FORMAT APC [$2]: Beacon On., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Beacon On.
EDESC
#
#
#
EVENT apcBeaconOff .1.3.6.1.4.1.318.0.546 "Status Events" Normal
FORMAT APC [$2]: Beacon Off., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Beacon Off.
EDESC
#
#
#
EVENT apcOutletStateAbnormal .1.3.6.1.4.1.318.0.547 "Status Events" Minor
FORMAT APC [$2]: Outlet $4 to abnormal state $6., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Outlet $4 to abnormal state $6.
EDESC
#
#
#
EVENT apcOutletStateNormal .1.3.6.1.4.1.318.0.548 "Status Events" Normal
FORMAT APC [$2]: Outlet $4 to normal state $6., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Outlet $4 to normal state $6.
EDESC
#
#
#
EVENT apcOutputRelayStateAbnormal .1.3.6.1.4.1.318.0.549 "Status Events" Minor
FORMAT APC [$2]: Relay $4 to abnormal state $6., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Relay $4 to abnormal state $6.
EDESC
#
#
#
EVENT apcOutputRelayStateNormal .1.3.6.1.4.1.318.0.550 "Status Events" Normal
FORMAT APC [$2]: Relay $4 to normal state $6., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Relay $4 to normal state $6.
EDESC
#
#
#
EVENT apcHardwareStateAbnormal .1.3.6.1.4.1.318.0.551 "Status Events" Critical
FORMAT APC [$2]: Hardware is in an abnormal state., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Hardware is in an abnormal state.
EDESC
#
#
#
EVENT apcHardwareStateNormal .1.3.6.1.4.1.318.0.552 "Status Events" Normal
FORMAT APC [$2]: Hardware is in its normal state., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Hardware is in its normal state.
EDESC
#
#
#
EVENT apcCriticalDiscreteInputContactStateAbnormal .1.3.6.1.4.1.318.0.553 "Status Events" Critical
FORMAT APC [$2]: Discrete contact $4 to abnormal state $6., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Discrete contact $4 to abnormal state $6.
EDESC
#
#
#
EVENT apcCriticalDiscreteInputContactStateNormal .1.3.6.1.4.1.318.0.554 "Status Events" Normal
FORMAT APC [$2]: Discrete contact $4 to normal state $6., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Discrete contact $4 to normal state $6.
EDESC
#
#
#
EVENT apcWarningDiscreteInputContactStateAbnormal .1.3.6.1.4.1.318.0.555 "Status Events" Minor
FORMAT APC [$2]: Discrete contact $4 to abnormal state $6., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Discrete contact $4 to abnormal state $6.
EDESC
#
#
#
EVENT apcWarningDiscreteInputContactStateNormal .1.3.6.1.4.1.318.0.556 "Status Events" Normal
FORMAT APC [$2]: Discrete contact $4 to normal state $6., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Discrete contact $4 to normal state $6.
EDESC
#
#
#
EVENT apcInformationalDiscreteInputContactStateAbnormal .1.3.6.1.4.1.318.0.557 "Status Events" Normal
FORMAT APC [$2]: Discrete contact $4 to abnormal state $6., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Discrete contact $4 to abnormal state $6.
EDESC
#
#
#
EVENT apcInformationalDiscreteInputContactStateNormal .1.3.6.1.4.1.318.0.558 "Status Events" Normal
FORMAT APC [$2]: Discrete contact $4 to normal state $6., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Discrete contact $4 to normal state $6.
EDESC
#
#
#
EVENT apcAnalogInputMaxThresholdViolation .1.3.6.1.4.1.318.0.559 "Status Events" Critical
FORMAT APC [$2]: Under max threshold on input $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Over max threshold on input $5.
EDESC
#
#
#
EVENT apcAnalogInputMaxThresholdViolationCleared .1.3.6.1.4.1.318.0.560 "Status Events" Normal
FORMAT APC [$2]: Over max threshold on input $5 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Over max threshold on input $5 cleared.
EDESC
#
#
#
EVENT apcAnalogInputHighThresholdViolation .1.3.6.1.4.1.318.0.561 "Status Events" Minor
FORMAT APC [$2]: Over high threshold on input $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Over high threshold on input $5.
EDESC
#
#
#
EVENT apcAnalogInputHighThresholdViolationCleared .1.3.6.1.4.1.318.0.562 "Status Events" Normal
FORMAT APC [$2]: Over high threshold on input $5 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Over high threshold on input $5 cleared.
EDESC
#
#
#
EVENT apcAnalogInputLowThresholdViolation .1.3.6.1.4.1.318.0.563 "Status Events" Minor
FORMAT APC [$2]: Under low threshold on input $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Under low threshold on input $5.
EDESC
#
#
#
EVENT apcAnalogInputLowThresholdViolationCleared .1.3.6.1.4.1.318.0.564 "Status Events" Normal
FORMAT APC [$2]: Under low threshold on input $5 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Under low threshold on input $5 cleared.
EDESC
#
#
#
EVENT apcAnalogInputMinThresholdViolation .1.3.6.1.4.1.318.0.565 "Status Events" Critical
FORMAT APC [$2]: Under min threshold on input $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Under min threshold on input $5.
EDESC
#
#
#
EVENT apcAnalogInputMinThresholdViolationCleared .1.3.6.1.4.1.318.0.566 "Status Events" Normal
FORMAT APC [$2]: Under min threshold on input $5 cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Under min threshold on input $5 cleared.
EDESC
#
#
#
EVENT apcDeviceClearLostComms .1.3.6.1.4.1.318.0.567 "Status Events" Normal
FORMAT APC: Lost communications reset command has been issued., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Lost communications reset command has been issued.
EDESC
#
#
#
EVENT apcDeviceConnected .1.3.6.1.4.1.318.0.568 "Status Events" Normal
FORMAT APC ENV [$2]: Device $4 Connected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Device $4 Connected.
EDESC
#
#
#
EVENT apcDeviceDisconnected .1.3.6.1.4.1.318.0.569 "Status Events" Critical
FORMAT APC [$2]: Device $4 Disconnected., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Device $4 Disconnected.
EDESC
#
#
#
EVENT apcUnregisteredUserAccessDenied .1.3.6.1.4.1.318.0.570 "Status Events" Normal
FORMAT APC Unregistered user's RFID $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Unregistered user's RFID $5.
EDESC
#
#
#
EVENT apcRegisteredUserAccessDenied .1.3.6.1.4.1.318.0.571 "Status Events" Normal
FORMAT APC Access denied, user $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Access denied, user $5.
EDESC
#
#
#
EVENT apcRegisteredUserConfigChange .1.3.6.1.4.1.318.0.572 "Status Events" Normal
FORMAT APC Registered user configuration change., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Registered user configuration change.
EDESC
#
#
#
EVENT apcDoorUnlocked .1.3.6.1.4.1.318.0.573 "Status Events" Normal
FORMAT APC Door unlocked, door access user $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Door unlocked, door access user $5.
EDESC
#
#
#
EVENT apcDoorLocked .1.3.6.1.4.1.318.0.574 "Status Events" Normal
FORMAT APC Door locked, door access user $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Door locked, door access user $5.
EDESC
#
#
#
EVENT apcHandleOpened .1.3.6.1.4.1.318.0.575 "Status Events" Normal
FORMAT APC $4 door handle opened., Trap Arguments:($#):$* [APC PowerNet]
SDESC
$4 door handle opened.
EDESC
#
#
#
EVENT apcHandleClosed .1.3.6.1.4.1.318.0.576 "Status Events" Normal
FORMAT APC $4 door handle closed., Trap Arguments:($#):$* [APC PowerNet]
SDESC
$4 door handle closed.
EDESC
#
#
#
EVENT apcDoorOpened .1.3.6.1.4.1.318.0.577 "Status Events" Normal
FORMAT APC $4 door opened., Trap Arguments:($#):$* [APC PowerNet]
SDESC
$4 door opened.
EDESC
#
#
#
EVENT apcDoorClosed .1.3.6.1.4.1.318.0.578 "Status Events" Normal
FORMAT APC $4 door closed., Trap Arguments:($#):$* [APC PowerNet]
SDESC
$4 door closed.
EDESC
#
#
#
EVENT apcKeyOverrideUnlocked .1.3.6.1.4.1.318.0.580 "Status Events" Minor
FORMAT APC: Key override unlock has occurred on door $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Key override unlock has occurred on door $4.
EDESC
#
#
#
EVENT apcKeyOverrideLocked .1.3.6.1.4.1.318.0.581 "Status Events" Normal
FORMAT APC: Key override lock has occurred on door $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Key override lock has occurred on door $4.
EDESC
#
#
#
EVENT apcForcedEntry .1.3.6.1.4.1.318.0.582 "Status Events" Critical
FORMAT APC: Forced entry has occurred on door $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Forced entry has occurred on door $4.
EDESC
#
#
#
EVENT apcForcedEntryCleared .1.3.6.1.4.1.318.0.583 "Status Events" Normal
FORMAT APC: forced entry has has been cleared on door $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Forced entry has been cleared on door $4.
EDESC
#
#
#
EVENT apcRelockTimeout .1.3.6.1.4.1.318.0.584 "Status Events" Critical
FORMAT APC relock timeout on $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Relock timeout on $4.
EDESC
#
#
#
EVENT apcRelockTimeoutCleared .1.3.6.1.4.1.318.0.585 "Status Events" Normal
FORMAT APC relock timout has been cleared on $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Relock timout has been cleared on $4.
EDESC
#
#
#
EVENT apcDoorSenseDisconnected .1.3.6.1.4.1.318.0.586 "Status Events" Critical
FORMAT APC: A door sensor was disconnected on door $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A door sensor was disconnected on door $4.
EDESC
#
#
#
EVENT apcDoorSenseConnected .1.3.6.1.4.1.318.0.587 "Status Events" Normal
FORMAT APC: A door sensor was connected on door $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A door sensor was connected on door $4.
EDESC
#
#
#
EVENT apcDoorLostComms .1.3.6.1.4.1.318.0.588 "Status Events" Critical
FORMAT APC: Communication was lost with door $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communication was lost with door $4.
EDESC
#
#
#
EVENT apcDoorEstablishedComms .1.3.6.1.4.1.318.0.589 "Status Events" Normal
FORMAT APC: Communication has been established with door $4., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Communication has been established with door $4.
EDESC
#
#
#
EVENT apcRegisteredUserAccessChange .1.3.6.1.4.1.318.0.590 "Status Events" Normal
FORMAT APC Registered user access change., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Registered user access change.
EDESC
#
#
#
EVENT apcUnregisteredUserStatusChange .1.3.6.1.4.1.318.0.591 "Status Events" Normal
FORMAT APC Unregistered user status change., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Unregistered user status change.
EDESC
#
#
#
EVENT apcDeviceClearUserConfigs .1.3.6.1.4.1.318.0.592 "Status Events" Normal
FORMAT APC: User configurations reset command has been issued., Trap Arguments:($#):$* [APC PowerNet]
SDESC
User configurations reset command has been issued.
EDESC
#
#
#
EVENT upsBatteryTempSensorFault .1.3.6.1.4.1.318.0.600 "Status Events" Minor
FORMAT APC UPS: The battery temperature sensor fault exists., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The battery temperature sensor fault exists.
EDESC
#
#
#
EVENT upsBatteryTempSensorFaultCleared .1.3.6.1.4.1.318.0.601 "Status Events" Normal
FORMAT APC UPS: The battery temperature sensor fault cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The battery temperature sensor fault cleared.
EDESC
#
#
#
EVENT upsBatterySoftBusStartFault .1.3.6.1.4.1.318.0.602 "Status Events" Minor
FORMAT APC UPS: A battery bus soft start fault exists., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A battery bus soft start fault exists.
EDESC
#
#
#
EVENT upsBatterySoftBusStartFaultCleared .1.3.6.1.4.1.318.0.603 "Status Events" Normal
FORMAT APC UPS: A battery bus soft start fault exists cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A battery bus soft start fault exists cleared.
EDESC
#
#
#
EVENT apcOutputShortCircuit .1.3.6.1.4.1.318.0.604 "Status Events" Minor
FORMAT APC Device: An output short circuit condition exists., Trap Arguments:($#):$* [APC PowerNet]
SDESC
An output short circuit condition exists.
EDESC
#
#
#
EVENT apcOutputShortCircuitCleared .1.3.6.1.4.1.318.0.605 "Status Events" Normal
FORMAT APC Device: An output short circuit condition cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
An output short circuit condition cleared.
EDESC
#
#
#
EVENT apcOutputRelayFault .1.3.6.1.4.1.318.0.606 "Status Events" Minor
FORMAT APC Device: An output relay (or its driver) fault exists., Trap Arguments:($#):$* [APC PowerNet]
SDESC
An output relay (or its driver) fault exists.
EDESC
#
#
#
EVENT apcOutputRelayFaultCleared .1.3.6.1.4.1.318.0.607 "Status Events" Normal
FORMAT APC Device: An output relay (or its driver) fault cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
An output relay (or its driver) fault cleared.
EDESC
#
#
#
EVENT upsPfcFault .1.3.6.1.4.1.318.0.608 "Status Events" Minor
FORMAT APC UPS: A PFC fault exists., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A PFC fault exists.
EDESC
#
#
#
EVENT upsPfcFaultCleared .1.3.6.1.4.1.318.0.609 "Status Events" Normal
FORMAT APC UPS: The PFC fault cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The PFC fault cleared.
EDESC
#
#
#
EVENT apcDcBusOverVoltage .1.3.6.1.4.1.318.0.610 "Status Events" Minor
FORMAT APC Devcie: DC bus voltage is too high., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The DC bus voltage is too high.
EDESC
#
#
#
EVENT apcDcBusOverVoltageCleared .1.3.6.1.4.1.318.0.611 "Status Events" Normal
FORMAT APC Device: The DC bus voltage is too high cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The DC bus voltage is too high cleared.
EDESC
#
#
#
EVENT upsInverterFault .1.3.6.1.4.1.318.0.612 "Status Events" Minor
FORMAT APC UPS: The inverter fault exists., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The inverter fault exists.
EDESC
#
#
#
EVENT upsInverterFaultCleared .1.3.6.1.4.1.318.0.613 "Status Events" Normal
FORMAT APC UPS: The inverter fault cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The inverter fault cleared.
EDESC
#
#
#
EVENT apcAdConverterFault .1.3.6.1.4.1.318.0.614 "Status Events" Minor
FORMAT APC Device: The A/D converter fault exists., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The A/D converter fault exists.
EDESC
#
#
#
EVENT apcAdConverterFaultCleared .1.3.6.1.4.1.318.0.615 "Status Events" Normal
FORMAT APC Device: The A/D converter fault cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The A/D converter fault cleared.
EDESC
#
#
#
EVENT apcLogicPowerSupplyFault .1.3.6.1.4.1.318.0.616 "Status Events" Minor
FORMAT APC Device: A logic power supply fault exists., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A logic power supply fault exists.
EDESC
#
#
#
EVENT apcLogicPowerSupplyFaultCleared .1.3.6.1.4.1.318.0.617 "Status Events" Normal
FORMAT APC Device: A logic power supply fault cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A logic power supply fault cleared.
EDESC
#
#
#
EVENT apcTransformerDCImbalanceFault .1.3.6.1.4.1.318.0.618 "Status Events" Minor
FORMAT APC Device: The DC component of the tformer's curr is too high., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The DC component of the transformer's current is too high.
EDESC
#
#
#
EVENT apcTransformerDCImbalanceFaultCleared .1.3.6.1.4.1.318.0.619 "Status Events" Normal
FORMAT APC Device: The DC component of the tformer's curr is normal., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The DC component of the transformer's current is normal.
EDESC
#
#
#
EVENT upsBackfeedRelayFault .1.3.6.1.4.1.318.0.620 "Status Events" Minor
FORMAT UPS Device: The backfeed relay (or its driver) has a fault., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The backfeed relay (or its driver) has a fault.
EDESC
#
#
#
EVENT upsBackfeedRelayFaultCleared .1.3.6.1.4.1.318.0.621 "Status Events" Normal
FORMAT UPS Device: The bfeed rly (or its drver) has a flt cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The backfeed relay (or its driver) has a fault cleared.
EDESC
#
#
#
EVENT upsBypassRelayFault .1.3.6.1.4.1.318.0.622 "Status Events" Minor
FORMAT APC Device: A bypass relay (or its driver) has a fault., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A bypass relay (or its driver) has a fault.
EDESC
#
#
#
EVENT upsBypassRelayFaultCleared .1.3.6.1.4.1.318.0.623 "Status Events" Normal
FORMAT APC Device: A bypass relay (or its driver) has a fault cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A bypass relay (or its driver) has a fault cleared.
EDESC
#
#
#
EVENT upsMainRelayFault .1.3.6.1.4.1.318.0.624 "Status Events" Critical
FORMAT APC Device: A main relay (or its driver) has a fault., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A main relay (or its driver) has a fault.
EDESC
#
#
#
EVENT upsMainRelayFaultCleared .1.3.6.1.4.1.318.0.625 "Status Events" Normal
FORMAT APC Device: A main relay (or its driver) has a fault cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A main relay (or its driver) has a fault cleared.
EDESC
#
#
#
EVENT xPDUBranchCurrentMinAlarm .1.3.6.1.4.1.318.0.626 "Status Events" Critical
FORMAT APC XPDU [$2]: Branch circuit current $4 below threshold $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Branch circuit current $4 is below threshold $5.
EDESC
#
#
#
EVENT xPDUBranchCurrentMinAlarmCleared .1.3.6.1.4.1.318.0.627 "Status Events" Normal
FORMAT APC XPDU [$2]: Branch circuit low current $3 alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Branch circuit low current $4 alarm cleared.
EDESC
#
#
#
EVENT xPDUBranchCurrentMaxAlarm .1.3.6.1.4.1.318.0.628 "Status Events" Critical
FORMAT APC XPDU [$2]: Branch circuit current $4 above threshold $5., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Branch circuit current $4 is above threshold $5.
EDESC
#
#
#
EVENT xPDUBranchCurrentMaxAlarmCleared .1.3.6.1.4.1.318.0.629 "Status Events" Normal
FORMAT APC XPDU [$2]: Branch circuit current $4 alarm cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Branch circuit high current $3 alarm cleared.
EDESC
#
#
#
EVENT rPDUOutletLowLoad .1.3.6.1.4.1.318.0.630 "Status Events" Minor
FORMAT APC Rack PDU: Violation of outlet low load threshold., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A Rack PDU has violated the outlet low load threshold.
EDESC
#
#
#
EVENT rPDUOutletLowLoadCleared .1.3.6.1.4.1.318.0.631 "Status Events" Normal
FORMAT APC Rack PDU: Low load condition cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The low load condition on a Rack PDU has been cleared.
EDESC
#
#
#
EVENT rPDUOutletNearOverload .1.3.6.1.4.1.318.0.632 "Status Events" Minor
FORMAT APC Rack PDU: Near an overload condition., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A Rack PDU is near an outlet overload condition.
EDESC
#
#
#
EVENT rPDUOutletNearOverloadCleared .1.3.6.1.4.1.318.0.633 "Status Events" Normal
FORMAT APC Rack PDU: Outlet Near overload condition has cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Rack PDU outlet near overload condition has cleared.
EDESC
#
#
#
EVENT rPDUOutletOverload .1.3.6.1.4.1.318.0.634 "Status Events" Critical
FORMAT APC Rack PDU: Outlet Overload condition., Trap Arguments:($#):$* [APC PowerNet]
SDESC
A Rack PDU is in an outlet overload condition.
EDESC
#
#
#
EVENT rPDUOutletOverloadCleared .1.3.6.1.4.1.318.0.635 "Status Events" Normal
FORMAT APC Rack PDU: Overload condition has cleared., Trap Arguments:($#):$* [APC PowerNet]
SDESC
The outlet overload condition on a Rack PDU has cleared.
EDESC
#
#
#
EVENT apcTestTrap .1.3.6.1.4.1.318.0.636 "Status Events" Normal
FORMAT APC: Test trap., Trap Arguments:($#):$* [APC PowerNet]
SDESC
Test Trap.
EDESC
#
#
#
EVENT baseFanFailureCleared .1.3.6.1.4.1.318.0.637 "Status Events" Normal
FORMAT APC UPS: Base module fan has been repaired, Trap Arguments:($#):$* [APC PowerNet]
SDESC
The base module fan has been repaired.
EDESC
#
#
#
EVENT apcDeviceAlarmStateHeartbeat .1.3.6.1.4.1.318.0.999 "Status Events" Normal
FORMAT APC X., Trap Arguments:($#):$* [APC PowerNet]
SDESC
.
EDESC
#
#
#
EVENT apcDiscoveryAlarmStateTableUpdate .1.3.6.1.4.1.318.0.1000 "Status Events" Normal
FORMAT APC X., Trap Arguments:($#):$* [APC PowerNet]
SDESC
.
EDESC
#
#
#
