-- *****************************************************************
-- CISCO-CATOS-ACL-QOS-MIB.my:  Cisco CatOS Acl Qos MIB
--
-- November 2001, Edward Pham
-- January  2002, Edward Pham
-- August   2002, Edward Pham
-- March    2003, Edward Pham
-- July     2003, Edward Pham
-- September 2003, Edward Pham
-- October  2003, Liwei Lue
-- November 2003, Edward Pham
--
-- Copyright (c) 2001-2007 by cisco Systems, Inc.
-- All rights reserved.
--
-- *****************************************************************

CISCO-CATOS-ACL-QOS-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, 
    OBJECT-TYPE, 
    Counter32,
    Counter64,
    Gauge32,
    Integer32,
    Unsigned32
        FROM SNMPv2-SMI
  
    MODULE-COMPLIANCE,
    OBJECT-GROUP
        FROM SNMPv2-CONF

    TEXTUAL-CONVENTION,
    RowStatus,
    MacAddress,
    DateAndTime,
    TruthValue
        FROM SNMPv2-TC

    ifIndex,
    InterfaceIndex
        FROM IF-MIB

    ciscoMgmt
        FROM CISCO-SMI
 
    VlanIndex 
        FROM CISCO-VTP-MIB

    Dscp,
    QosLayer2Cos,
    Percent,
    QosInterfaceQueueType
        FROM CISCO-QOS-PIB-MIB

    cseFlowDataEntry
        FROM CISCO-SWITCH-ENGINE-MIB

    CounterBasedGauge64
        FROM HCNUM-TC

    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB

    CiscoPortList,
    CiscoIpProtocol
        FROM CISCO-TC

    InetAddressType,
    InetAddress,
    InetPortNumber
        FROM INET-ADDRESS-MIB
    ;


ciscoCatOSAclQosMIB    MODULE-IDENTITY
    LAST-UPDATED    "200711020000Z"
    ORGANIZATION    "Cisco Systems Inc. "
    CONTACT-INFO
        "Cisco Systems
        Customer Service

        Postal: 170 W Tasman Drive
            San Jose, CA 95134
            USA

        Tel: +1 800 553-NETS

        E-mail: cs-wbu@cisco.com"
    DESCRIPTION
        "This MIB module is for Access Control Lists(ACLs) configuration
        of Quality of Service (QoS) as well as Security feature on the
        Cisco Catalyst 5000/6000 series switch running CatOS. It also
        provides QoS configuration and statistics information.
         
        Configuration information available through this MIB includes
        Security and QoS ACL configuration for IP, IPX and Layer 2 
        traffic, QoS and Security configuration parameters. 

        Statistics available through this MIB includes QoS statistics
        for Layer 3 traffic. In addition, detailed, flow-specific
        statistics are also available.

        This MIB module is applied in conjunction with 
        CISCO-QOS-POLICY-CONFIG-MIB. The configuration information 
        available through this MIB takes effect throughout the device 
        when the value of qosPrOperPolicySource object in 
        CISCO-QOS-POLICY-CONFIG-MIB is 'local' or applies to a specific
        interface when the value of qosPrIfOperPolicySource object
        in CISCO-QOS-POLICY-CONFIG-MIB which associates with that 
        interface is 'local' while the value of qosPrOperPolicySource is
        not 'local'.

        The following terms are used throughout this MIB: 

            ACE stands for Access Control Entry. An ACL consists of an 
            ordered set of ACEs. ACE is a filter which is used to 
            identify flows with certain characteristics. It includes
            fields such as ingress/egress ports, L2(layer 2) addresses,
            L3(layer 3) addresses, TCP/UDP port numbers, etc.

            QoS ACE and Security ACE are very similar to each other
            but the actions of the ACEs are different.  
       
            Security ACEs are compared to each packet, and each ACE
            specifies whether packets that match with it are either
            forwarded or dropped.

            ESP: Enscrypted Security Payload.
 
            QoS is the method which attempts to ensure that the network
            requirements of different applications can be met by giving
            preferential forwarding treatment to some traffic. It is
            usually consisted of these steps: classification, policing,
            output scheduling, marking and shaping. Classification 
            identifies the traffic. Policing checks if the traffic 
            conformed to a specified criteria. Output scheduling,
            marking and shaping control how the traffic is transmitted
            to the next hop. 

            A flow is a non-specific term for a microflow or an
            aggregate flow.

            Microflow is a single instance of an application to 
            application flow of packets which is identified by source
            address, source port, destination address, destination port
            and protocol id.

            Aggregate flow is a collection of microflows that are
            treated together as one for the purpose of QoS.

            DSCP (Differentiated Services Code Point) is the six most 
            significant bits of the ToS field in a IP packet header.

            DSCP Mutation: the previous hop(s) and the following hop(s)
            of a device may reside in a different QoS domain. A QoS
            domain refers to the set of QoS rules and conventions
            adopted by an administrative entity. For instance, a set
            of DSCP values may have a different meaning in different
            domains. DSCP mutation allows a DSCP set to be mutated or
            transformed in order to maintain semantic compatibility
            between adjacent domains. The mutation is done via mapping
            tables which maps the old DSCP value from one domain to a
            new DSCP value in the other domain. 

            IP precedence is the three most significant bits of the ToS 
            field in a IP packet header.
            
            Cos (Class of Service) is the three bits in the layer 2
            header that indicates user priority value assigned to this
            packet.

            Trust state is a parameter configured at a physical
            interface or an ACL to determine a DSCP value assigned to
            a packet for QoS purpose.

            In profile packet is a packet that does not cause the
            committed access rate of the packet's flow to be exceeded.

            Out of profile packet is a packet that cause the committed
            access rate of the packet's flow to be exceeded.

        To accomplish classification, the user defines an ACL describing
        the specification of a traffic flow then attaches this ACL to a 
        physical interface or a vlan. When a packet arrives at an
        interface, depending on the configured trust state at that
        interface, it can either be matched against an ACL if the trust
        state is not trusted or get a DSCP assigned and go directly to 
        output scheduling. In the former case, when the packet matches 
        an ACE in the attached ACL, the next step will be policing. At 
        the end of classification process, a packet has a DSCP value 
        assigned. In some platform (e.g. Catalyst 4000) that does not
        support ACL configuration, classification is accomplished by
        matching the Cos value of incoming packet. 

        A packet can be policed at microflow or aggregate flow level.
        Policing is done using the token bucket algorithm. 
        At the end of policing process, if packet does not cause the
        flow to exceed the normal rate, it will continue to the next
        step. Otherwise, the packet is dropped or assigned a 'policed'
        DSCP value. Some platforms support multi-rate policing.  When 
        packet causes the flow to exceed the normal rate but not the
        excess rate, it is assigned a 'policed' DSCP value. When packet
        causes the flow to exceed excess rate, it is either dropped or
        has a 'policed' DSCP value assigned. After policing process,
        the next step is output scheduling.

        Output scheduling is the process of assigning a packet to
        a queue and a threshold according to the packet's Cos value.
        To get its Cos value, a DSCP to Cos mapping will be performed.

        This MIB also defines 'Security ACLs' which some devices support
        as a mean to enforce security. Security ACLs, attached at an
        ingress interface, are compared to each packet arriving at that
        interface. If the packet matches an ACE in the ACLs, it is
        either permitted to go through the device or blocked and
        dropped or redirected to another interface."
    REVISION   "200711020000Z"
    DESCRIPTION
        "Add the following groups:
             caqDownloadClassifierGroup,
             caqIpOperClassifierGroup,
             caqSecurityDownloadAclInfoGroup,
             caqSecurityDownloadIpAceGroup,
             caqIfDownloadAclMapGroup,
             caqIfIpPhoneMapGroup,
             caqArpLoggingSourceGroup,
             caqIpAceTypeGroup." 
    REVISION   "200607150000Z"
    DESCRIPTION
        "Add 'include' enumeration value for caqSecurityAction.

         Add caqQosL3StatsRateGroup,
             caqQosL3StatsPeakGroup,
             caqAggPolicerOctetsRateGroup,
             caqAggPolicerPacketsRateGroup,
             caqAggPolicerOctetsPeakGroup, 
             caqAggPolicerPacketsPeakGroup,
             caqQosPortRateGroup,
             caqQosPortPeakGroup,
             caqSecurityActionDnldAceGroup."
    REVISION   "200507260000Z"
    DESCRIPTION
        "Add 'matchEapoudp' and 'matchUrlRedirect' enum value
         for caqIpProtocolMatchCriteria object."
    REVISION   "200405260000Z"
    DESCRIPTION
        "Add the following groups to support ACL hit count
         configuration and statistics: 

         caqAclFeatureGroup 
         caqAclHitCountGroup 

         Add the following groups to support additional matching
         criteria for MAC ACE and MAC packet classify feature on
         VLAN:

         caqMacAceExtGroup. 
         caqMacPktClassifyVlanGroup." 
    REVISION   "200311260000Z"
    DESCRIPTION
        "Add the following objects to support group name for source
         and destination fields in caqIpAceTable:
         caqIpAceSrcGroup
         caqIpAceDestGroup."
    REVISION   "200310280000Z"
    DESCRIPTION
        "Add caqIfSecurityAclConfigGroup to support port ACL."
    REVISION   "200309300000Z"
    DESCRIPTION
        "Add the dhcpSnooping bit for caqSecurityRateLimitFeatures
         object.
         
         Fix a typo in the DESCRIPTION clause for caqSecurityAction
         object."
    REVISION   "200307010000Z"
    DESCRIPTION
        "Deprecate caqSecurityRedirectPortList object and add
         caqSecurityRedirect2kPortList to support up to 2048
         bridge ports."
    REVISION   "200303050000Z"
    DESCRIPTION
        "Add the following objects and tables:
         caqClassifierMapDirection,
         caqIpAceSecurityId,
         caqDscpRewriteEnabled,
         caqAggPolicerOctets,
         caqAggPolicerNRExceedOctets,
         caqAggPolicerERExceedOctets,
         caqDscpMutationMapTable,
         caqVlanMutationIdMapTable,
         caqQosDefaultActionTable."
    REVISION   "200210100000Z"
    DESCRIPTION
        "Add the caqLoggingGroup, caqArpInspGroup and 
         caqSecurityRateLimitGroup to support security ACL logging,
         security ACL features rate limit and ARP Inspection
         device configuration."
    REVISION   "200201170000Z"
    DESCRIPTION
        "Add the caqIfTrustDeviceGroup and caqQosExcessBurstGroup
         to support Qos information on excess burst size and trusted
         device configuration."
    REVISION   "200110180000Z"
    DESCRIPTION
        "Add the caqPbfObjects group and modify the
         caqSecurityActionTable to support policy based forwarding."
    REVISION   "200102150000Z"
    DESCRIPTION
        "Add the following objects:
         caqAggPolicerName,
         caqAggPolicerPackets,
         caqAggPolicerNRExceedPackets,
         caqAggPolicerERExceedPackets."
    REVISION   "200102070000Z"
    DESCRIPTION
        "Initial version of this MIB module."

    ::= { ciscoMgmt 179 }

--
--
-- Textual Conventions
--
--
CaqAclName ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "31a"
    STATUS  current
    DESCRIPTION
        "A character string for an ACL (Access Control List) name.
        Valid characters are a-z, A-Z,  0-9, '-', '_' and '.'. Some
        devices may require that an AclName contains at least one
        non-numeric character. Acl name is case sensitive."
    SYNTAX     OCTET STRING (SIZE(1..31)) 

CaqPolicerName ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "31a"
    STATUS  current
    DESCRIPTION
        "A character string for a policer name.  Valid characters are 
        a-z, A-Z,  0-9, '-', '_' and '.'. Some devices may require that
        a PolicerName contains at least one non-numeric character.
        Policer name is case sensitive."
    SYNTAX     OCTET STRING (SIZE(1..31)) 

CaqPolicerNameOrEmpty ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "31a"
    STATUS  current
    DESCRIPTION
        "This textual convention is an extension of the PolicerName
        convention. The latter defines a non-empty policer name. This
        extension permits the additional value of empty string. Examples
        of the usage of empty string might include situations where
        there is no policer defined for an ACE." 
    SYNTAX     OCTET STRING (SIZE(0..31)) 

CaqAdjacencyName ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "18a"
    STATUS  current
    DESCRIPTION
        "A character string for an adjacency name.  Valid characters
        are a-z, A-Z,  0-9, '-', '_' and '.'. Some devices may require
        that an AdjacencyName contains at least one non-numeric
        character. Adjacency name is case sensitive."
    SYNTAX     OCTET STRING (SIZE(1..18)) 

--
-- Direction
--
CaqDirection ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "Indicates a particular direction of traffic." 
    SYNTAX  INTEGER {
              ingress(1),
              egress(2)
            }

--
-- IP Precedence
--
CaqIpPrecedence ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "Indicates the IP precedence."
    REFERENCE
        "RFC791 INTERNET PROTOCOL, Chapter 3.1"
    SYNTAX  Unsigned32 (0..7)


--
-- Queue Number 
--
CaqQueueNumber ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "An integer indicates a queue number."
    SYNTAX  Unsigned32 (1..100)

--
-- Threshold Number 
--
CaqThresholdNumber ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "An integer indicates a threshold number."
    SYNTAX  Unsigned32 (1..100)

--
-- HitCountAclType 
--
CaqHitCountAclType ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "An integer indicating the ACL type that 
         supports ACL hit count feature."
    SYNTAX  INTEGER { ipSecurity(1), 
                      ipxSecurity(2), 
                      macSecurity(3) 
                    } 
--
-- Cisco CatOS Acl Qos MIB object definitions
--

ciscoCatOSAclQosMIBObjects OBJECT IDENTIFIER 
    ::= { ciscoCatOSAclQosMIB 1 }

-- Cisco CatOS Acl Qos MIB consists of the following groups
-- [1] Cisco CatOS Acl Qos Global Group (caqGlobalObjects).
-- [2] Cisco CatOS Acl Qos Interface Group (caqInterfaceObjects).
-- [3] Cisco CatOS Acl Qos Acl Group (caqAclObjects).
-- [4] Cisco CatOS Acl Qos Statistics Group (caqQosStatsObjects).
-- [5] Cisco CatOS Acl Qos Extension Group (caqExtObjects).
-- [6] Cisco CatOS Acl Qos Policy-Based Forwarding (PBF)
--     Group (caqPbfObjects).
-- [7] Cisco CatOS Acl Security Logging Group (caqLoggingObjects)
-- [8] Cisco CatOS Acl ARP Inspection Group (caqArpInspObjects)
caqGlobalObjects     OBJECT IDENTIFIER
    ::= { ciscoCatOSAclQosMIBObjects 1 }
caqInterfaceObjects     OBJECT IDENTIFIER
    ::= { ciscoCatOSAclQosMIBObjects 2 }
caqAclObjects     OBJECT IDENTIFIER
    ::= { ciscoCatOSAclQosMIBObjects 3 }
caqQosStatsObjects     OBJECT IDENTIFIER
    ::= { ciscoCatOSAclQosMIBObjects 4 }
caqExtObjects     OBJECT IDENTIFIER
    ::= { ciscoCatOSAclQosMIBObjects 5 }
caqPbfObjects     OBJECT IDENTIFIER
    ::= { ciscoCatOSAclQosMIBObjects 6 }
caqLoggingObjects     OBJECT IDENTIFIER
    ::= { ciscoCatOSAclQosMIBObjects 7 }
caqArpInspObjects     OBJECT IDENTIFIER
    ::= { ciscoCatOSAclQosMIBObjects 8 }
caqAclHitCountObjects     OBJECT IDENTIFIER
    ::= { ciscoCatOSAclQosMIBObjects 9 }
caqDownloadAclObjects     OBJECT IDENTIFIER
    ::= { ciscoCatOSAclQosMIBObjects 10 }

--**********************************************************************
-- Cisco CatOS Acl Qos Global Group
--**********************************************************************

--
-- The caqCosToDscpTable
--

caqCosToDscpTable    OBJECT-TYPE
    SYNTAX        SEQUENCE OF CaqCosToDscpEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "This table contains the mapping of Cos values to DSCP values.
        This map is used to associate the Cos of packets arriving at a
        port to a DSCP where the port's trust state is trustCoS(2). 
        This map is a table of eight Cos values (0 through 7) and their
        corresponding DSCP values. This mapping applies to every port on
        the device."
    ::= { caqGlobalObjects 1 }

caqCosToDscpEntry    OBJECT-TYPE
    SYNTAX        CaqCosToDscpEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "Each row contains the mapping from a CoS value to a DSCP
        value."
    INDEX { caqCosToDscpCos }
    ::= { caqCosToDscpTable 1 }

CaqCosToDscpEntry ::= SEQUENCE {
    caqCosToDscpCos    QosLayer2Cos,
    caqCosToDscpDscp   Dscp
}

caqCosToDscpCos        OBJECT-TYPE
    SYNTAX        QosLayer2Cos
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "The CoS value being mapped to the DSCP value in this device."
    ::= { caqCosToDscpEntry 1 }

caqCosToDscpDscp        OBJECT-TYPE
    SYNTAX        Dscp
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "The DSCP value which the CoS value maps to. The default
        configuration is :

        CoS    DSCP
        0        0
        1        8
        2        16
        3        24
        4        32
        5        40
        6        48
        7        56
        ."
    ::= { caqCosToDscpEntry 2 }

--
-- CaqIpPrecToDscpTable    
--
caqIpPrecToDscpTable    OBJECT-TYPE
    SYNTAX        SEQUENCE OF CaqIpPrecToDscpEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "This table contains the mapping of IP Precedence to DSCP.
        This map is used to associate the IP Precedence of IP packets
        arriving at a port to a DSCP where the port's trust state is 
        trustIpPrec(3).  This map is a table of eight IpPrecedence
        values (0 through 7) and their corresponding DSCP values. 
        This mapping applies to every port on the device."
    ::= { caqGlobalObjects 2 }

caqIpPrecToDscpEntry    OBJECT-TYPE
    SYNTAX        CaqIpPrecToDscpEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "Each row contains the mapping from an IP Precedence value to
        a DSCP value."
    INDEX { caqIpPrecToDscpIpPrec }
    ::= { caqIpPrecToDscpTable 1 }

CaqIpPrecToDscpEntry ::= SEQUENCE {
    caqIpPrecToDscpIpPrec    CaqIpPrecedence,
    caqIpPrecToDscpDscp      Dscp
}

caqIpPrecToDscpIpPrec  OBJECT-TYPE
    SYNTAX        CaqIpPrecedence
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "The IP Precedence value being mapped to the DSCP value in
        this device."
    ::= { caqIpPrecToDscpEntry 1 }

caqIpPrecToDscpDscp  OBJECT-TYPE
    SYNTAX        Dscp
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "The DSCP value which the IP Precedence value maps to. The
        default configuration is the identity function :

        IPPrec    DSCP
        0            0
        1            8
        2            16
        3            24
        4            32
        5            40
        6            48
        7            56
        ."
    ::= { caqIpPrecToDscpEntry 2 }

--
-- caqDscpMappingTable
--

caqDscpMappingTable    OBJECT-TYPE
    SYNTAX        SEQUENCE OF CaqDscpMappingEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "This table always has 64 entries, one for each DSCP value. The
        table contains three mappings from the DSCP value assigned to
        a packet. One mapping is to the egress CoS to be stored in the
        layer-2 frame headers for output on 802.1Q or ISL interfaces.
        The other two mappings are to the remarked (or 'marked down')
        DSCP values which are used when a policer's requires that 
        a packet's DSCP value to be modified. Of these two mappings,
        one is for a Normal Rate policer, and the other is for an 
        Excess Rate policer.  These mappings apply for every port on the
        device."
    ::= { caqGlobalObjects 3 }

caqDscpMappingEntry    OBJECT-TYPE
    SYNTAX        CaqDscpMappingEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "Each row contains the mapping from DSCP value to CoS value
        and policed DSCP."
    INDEX  { caqDscpMappingDscp }
    ::= { caqDscpMappingTable 1 }

CaqDscpMappingEntry ::= SEQUENCE {
    caqDscpMappingDscp           Dscp,
    caqDscpMappingCos            QosLayer2Cos,
    caqDscpMappingNRPolicedDscp  Dscp,
    caqDscpMappingERPolicedDscp  Dscp
}

caqDscpMappingDscp    OBJECT-TYPE
    SYNTAX        Dscp
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "The DSCP value being mapped to the CoS value and policed DSCP
        value in this device."
    ::= { caqDscpMappingEntry 1 }

caqDscpMappingCos    OBJECT-TYPE
    SYNTAX        QosLayer2Cos
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "The CoS value which the DSCP values maps to.

        The default configuration is calculated from the
        formula CoS = DSCP divide by 8.
        That is:
        DSCP 0-7 all map to CoS 0;
        DSCP 8-15 all map to CoS 1;
             ...
        DSCP 32-39 all map to CoS 4;
             ...
        DSCP 56-63 all map to CoS 7."
    ::= { caqDscpMappingEntry 2 }

caqDscpMappingNRPolicedDscp   OBJECT-TYPE
    SYNTAX        Dscp
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "The normal rate policed DSCP value which the DSCP values maps
        to. The normal rate default mapping of DSCP to 'marked down'
        DSCP is the identity function.
        That is:
            63 -> 63
            62 -> 62
                ...
            31 -> 31
                ...
            2 -> 2
            1 -> 1
            0 -> 0."
    ::= { caqDscpMappingEntry 3 }

caqDscpMappingERPolicedDscp   OBJECT-TYPE
    SYNTAX        Dscp
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "The excess rate policed DSCP value which the DSCP values maps
        to. If the value of caqFlowPolicerExcessRateSupport object is
        false(2), this object cannot be instantiated. The excess rate
        default DSCP mapping of DSCP to 'marked down' DSCP is the
        identity function.
        That is:
            63 -> 63
            62 -> 62
                ...
            31 -> 31
                ...
            2 -> 2
            1 -> 1
            0 -> 0."
    ::= { caqDscpMappingEntry 4 }

--
-- Queue assignment table
--

-- The Assignment of packets to queues and thresholds based on
-- their CoS value.

caqCosAssignmentTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqCosAssignmentEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table provides the information for and configuration of
        assigning packets to queues and thresholds based on their CoS
        value."
    ::= { caqGlobalObjects 4 }

caqCosAssignmentEntry OBJECT-TYPE
    SYNTAX      CaqCosAssignmentEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The assignment of packets to a pair of queue and threshold 
        based on their Cos value. The packets assignment also depends 
        on port types. For each port type, there is a set of Cos  
        value (0..7) associated with a pair of queue number and 
        threshold number (q,t). Packets that have their Cos value
        belong to a particular set will be assigned to the pair of
        queue number and threshold number that this set associated
        with." 
    INDEX { caqCosAssignQueueType, caqCosAssignCos }
    ::= { caqCosAssignmentTable 1 }

CaqCosAssignmentEntry ::= SEQUENCE {
    caqCosAssignQueueType           QosInterfaceQueueType,
    caqCosAssignCos                 QosLayer2Cos,
    caqCosAssignQueueNumber         CaqQueueNumber, 
    caqCosAssignThresholdNumber     CaqThresholdNumber 
}

caqCosAssignQueueType  OBJECT-TYPE
    SYNTAX      QosInterfaceQueueType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The queue type of this interface."
    ::= { caqCosAssignmentEntry 1 }

caqCosAssignCos  OBJECT-TYPE
    SYNTAX      QosLayer2Cos
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Indicates the Cos value which is used to match the
         Cos value of packets for queue assignment."
    ::= { caqCosAssignmentEntry 2 }

caqCosAssignQueueNumber OBJECT-TYPE
    SYNTAX      CaqQueueNumber 
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The queue number which the Cos value denoted by 
        caqCosAssignCos will be associated with. This queue number
        must not larger than the queue count defined by 
        caqCosAssignQueueType."
    ::= { caqCosAssignmentEntry 3 }

caqCosAssignThresholdNumber OBJECT-TYPE
    SYNTAX      CaqThresholdNumber 
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The threshold number which the Cos value denoted by 
        caqCosAssignCos will be associated with. This threshold
        number must not larger than the threshold count defined
        by caqCosAssignQueueType."
    ::= { caqCosAssignmentEntry 4 }


--
-- The Queue Threshold Table
--

caqQueueThresholdTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqQueueThresholdEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table maintains threshold parameters for the specified
        queue number and threshold number of a port type."
    ::= { caqGlobalObjects 5 }

caqQueueThresholdEntry       OBJECT-TYPE
    SYNTAX      CaqQueueThresholdEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "For each threshold of a queue, there are parameters to set on
        the threshold. This entry contains the parameters."
    INDEX   { caqQueueThreshQueueType,
              caqQueueThreshQueueIndex,
              caqQueueThreshThresholdIndex }
    ::= { caqQueueThresholdTable 1 }

CaqQueueThresholdEntry ::= SEQUENCE {
    caqQueueThreshQueueType           QosInterfaceQueueType,
    caqQueueThreshQueueIndex          CaqQueueNumber, 
    caqQueueThreshThresholdIndex      CaqThresholdNumber, 
    caqQueueThreshDropAlgorithm       INTEGER,
    caqQueueThreshDropThreshold       Unsigned32, 
    caqQueueThreshMinWredThreshold    Percent,
    caqQueueThreshMaxWredThreshold    Unsigned32 
}

caqQueueThreshQueueType  OBJECT-TYPE
    SYNTAX      QosInterfaceQueueType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Indicates the queue type."
    ::= { caqQueueThresholdEntry 1 }


caqQueueThreshQueueIndex  OBJECT-TYPE
    SYNTAX      CaqQueueNumber 
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Indicates queue number. This queue number must not be larger
        than the queue count defined by caqQueueThreshQueueType."
    ::= { caqQueueThresholdEntry 2 }

caqQueueThreshThresholdIndex   OBJECT-TYPE
    SYNTAX      CaqThresholdNumber 
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Indicates threshold number. This threshold number must not
        be larger than the threshold count defined by 
        caqQueueThreshQueueType."
    ::= { caqQueueThresholdEntry 3 }

caqQueueThreshDropAlgorithm   OBJECT-TYPE
    SYNTAX      INTEGER { tailDrop(1), wred(2) } 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the drop algorithm used at this queue and threshold.
         
         tailDrop(1) indicates that tailDrop is used.
         
         wred(2) indicates that WRED is used."
    ::= { caqQueueThresholdEntry 4 }

caqQueueThreshDropThreshold   OBJECT-TYPE
    SYNTAX      Unsigned32 (1..100) 
    UNITS       "percent"
    MAX-ACCESS  read-write    
    STATUS      current
    DESCRIPTION
        "This object specifies the drop threshold parameter for a
        pair of queue and threshold of an interface queue type when the
        drop algorithm is tail drop. Once the packets in the buffer is
        more than the value of this object, the incoming packets of the
        buffer are dropped. The value is a percentage of the full
        buffer.

        This object is instantiated only if the value of 
        caqQueueThreshDropAlgorithm is tailDrop(1)." 
    ::= { caqQueueThresholdEntry 5 }

caqQueueThreshMinWredThreshold   OBJECT-TYPE
    SYNTAX      Percent
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This object specifies the min WRED threshold parameter of a
        threshold number for the specific port type when WRED drop
        algorithm is used.
        
        WRED (Weighted Random Early Detect) is a mechanism which drops
        packets fairly during congestion so that adaptive applications
        can react to congestion. This object specifies a percentage of
        the buffer size.

        This object is instantiated only if the value of
        caqQueueThreshDropAlgorithm is wred(2)."
    ::= { caqQueueThresholdEntry 6 }

caqQueueThreshMaxWredThreshold   OBJECT-TYPE
    SYNTAX      Unsigned32 (1..100) 
    UNITS       "percent"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This object specifies the max WRED threshold parameter of a
        threshold number for the specific port type when WRED drop
        algorithm is used.

        This object is instantiated only if the value of 
        caqQueueThreshDropAlgorithm is wred(2)." 
    ::= { caqQueueThresholdEntry 7 }

--
-- The Queue Table
--

caqQueueTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqQueueEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table used to configure the WRR (weighted round robin)
        weights for queues and the ratio of memory buffer allocation
        for each queue. It only contains entries for the specific port 
        types which supports either WRR or buffer allocation."
    ::= { caqGlobalObjects 6 }

caqQueueEntry       OBJECT-TYPE
    SYNTAX      CaqQueueEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A set of WRR weight and memory buffer allocation ratio for
        ingress or egress of a specific queue."
    INDEX   { caqQueueDirection,
              caqQueueType,
              caqQueueNumber }
    ::= { caqQueueTable 1 }

CaqQueueEntry ::= SEQUENCE {
    caqQueueDirection         CaqDirection,
    caqQueueType              QosInterfaceQueueType,
    caqQueueNumber            CaqQueueNumber, 
    caqQueueWrrWeight         Unsigned32,
    caqQueueBufferSizeRatio   Unsigned32 
}

caqQueueDirection  OBJECT-TYPE
    SYNTAX      CaqDirection
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Indicates whether this row's queue parameters are to
        be applied for ingress or for egress traffic."
    ::= { caqQueueEntry 1 }

caqQueueType  OBJECT-TYPE
    SYNTAX      QosInterfaceQueueType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Indicates the queue type."
    ::= { caqQueueEntry 2 }


caqQueueNumber  OBJECT-TYPE
    SYNTAX      CaqQueueNumber 
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Indicates queue number."
    ::= { caqQueueEntry 3 }

caqQueueWrrWeight  OBJECT-TYPE
    SYNTAX          Unsigned32  (1..255)
    MAX-ACCESS      read-write    
    STATUS          current
    DESCRIPTION
        "This object is to configure the weight for the specified
        queue type and for the specified direction." 
    ::= { caqQueueEntry 4 }

caqQueueBufferSizeRatio    OBJECT-TYPE
    SYNTAX          Unsigned32 (1..99) 
    UNITS           "percent"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Indicates the percentage of ingress or egress packet buffer
        memory allocated to the specified queue."
    ::= { caqQueueEntry 5 }

--
--  The Dscp Mutation Map Table
--

caqDscpMutationMapTable    OBJECT-TYPE
    SYNTAX        SEQUENCE OF CaqDscpMutationMapEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "The table provides the DSCP mutation mapping configuration
         on the device. This table is only instantiated if DSCP
         Mutation is supported by the device."
    ::= { caqGlobalObjects 7 }

caqDscpMutationMapEntry    OBJECT-TYPE
    SYNTAX        CaqDscpMutationMapEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "Each row contains the mapping from old DSCP value to new
        DSCP value per specific mutation table."
    INDEX  { caqDscpMutationTableId, caqDscpMutationOldDscp }
    ::= { caqDscpMutationMapTable 1 }

CaqDscpMutationMapEntry ::= SEQUENCE {
    caqDscpMutationTableId           Unsigned32,
    caqDscpMutationOldDscp           Dscp, 
    caqDscpMutationNewDscp           Dscp
}

caqDscpMutationTableId    OBJECT-TYPE
    SYNTAX        Unsigned32 
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "The mutation table ID number." 
    ::= { caqDscpMutationMapEntry 1 }

caqDscpMutationOldDscp    OBJECT-TYPE
    SYNTAX        Dscp
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "The old DSCP value."
    ::= { caqDscpMutationMapEntry 2 }

caqDscpMutationNewDscp   OBJECT-TYPE
    SYNTAX        Dscp
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "The new DSCP value which the old DSCP values maps to for
        a specific mutation table. The default mapping of old DSCP to
        new DSCP for mutation purpose is the identity function.
        That is:
            63 -> 63
            62 -> 62
                ...
            31 -> 31
                ...
            2 -> 2
            1 -> 1
            0 -> 0."
    ::= { caqDscpMutationMapEntry 3 }

--
--  The VLAN to Mutation Table Map Table
--

caqVlanMutationIdMapTable    OBJECT-TYPE
    SYNTAX        SEQUENCE OF CaqVlanMutationIdMapEntry 
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "The table provides the VLAN to mutation table mapping
         configuration on the device. This table is only
         instantiated if DSCP Mutation is supported by the 
         device."
    ::= { caqGlobalObjects 8 }

caqVlanMutationIdMapEntry    OBJECT-TYPE
    SYNTAX        CaqVlanMutationIdMapEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "When the first time a VLAN is created in a device supporting
        this table, a corresponding entry of this table will be added.
        The value of caqVlanMutationTableId object in such row will be
        initialized to 0."
    INDEX  { caqVlanMutationIndex } 
    ::= { caqVlanMutationIdMapTable 1 }

CaqVlanMutationIdMapEntry ::= SEQUENCE {
    caqVlanMutationIndex          VlanIndex,
    caqVlanMutationTableId        Unsigned32
}

caqVlanMutationIndex    OBJECT-TYPE
    SYNTAX        VlanIndex 
    MAX-ACCESS    not-accessible 
    STATUS        current
    DESCRIPTION
        "Indicates the VLAN number."
    ::= { caqVlanMutationIdMapEntry 1 }

caqVlanMutationTableId    OBJECT-TYPE
    SYNTAX        Unsigned32
    MAX-ACCESS    read-write 
    STATUS        current
    DESCRIPTION
        "Indicates the mutation table ID number. The value of this
        object should match one of caqDscpMutationTableId object
        value in caqDscpMutationMapTable. 
        
        Mutation table 0 always provides the identity mapping."
    ::= { caqVlanMutationIdMapEntry 2 }

caqDscpRewriteEnabled OBJECT-TYPE
    SYNTAX        TruthValue 
    MAX-ACCESS    read-write 
    STATUS        current
    DESCRIPTION
        "Indicates whether DSCP rewrite is enabled or disabled
        in the device. 

        if true(1), all outgoing packets will have their DSCP
        value rewrited based on the result of classification,
        policing or DSCP mutation configured in the device.
   
        if false(2), all outgoing packets will have their DSCP
        values as when they arrived."
    ::= { caqGlobalObjects 9 }

caqMacPktClassifyVlansLow  OBJECT-TYPE
    SYNTAX        OCTET STRING (SIZE(0..256))
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "A string of octets containing one bit per VLAN for
         VLANs with VlanIndex value of 0 to 2047. The first
         octet corresponds to VLANs with VlanIndex values
         of 0 through 7; the second octet to VLANs 8 through
         15; etc.  The most significant bit of each octet
         corresponds to the lowest value VlanIndex in that octet.

         For each VLAN, if Ethernet packet classify feature is 
         enabled then the bit corresponding to that VLAN is set
         to '1'.

         Note that if the length of this string is less than
         256 octets, any 'missing' octets are assumed to contain
         the value zero. A NMS may omit any zero-valued octets
         from the end of this string in order to reduce SetPDU size,
         and the agent may also omit zero-valued trailing octets,
         to reduce the size of GetResponse PDUs."
    ::= { caqGlobalObjects 10 }

caqMacPktClassifyVlansHigh  OBJECT-TYPE
    SYNTAX        OCTET STRING (SIZE(0..256))
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "A string of octets containing one bit per VLAN for
         VLANs with VlanIndex value of 2048 to 4095. The first
         octet corresponds to VLANs with VlanIndex values
         of 2048 through 2055; the second octet to VLANs 2056
         through 2063; etc.  The most significant bit of each
         octet corresponds to the lowest value VlanIndex in that
         octet.

         For each VLAN, if Ethernet packet classify feature is 
         enabled then the bit corresponding to that VLAN is set
         to '1'.

         Note that if the length of this string is less than
         256 octets, any 'missing' octets are assumed to contain
         the value zero. A NMS may omit any zero-valued octets
         from the end of this string in order to reduce SetPDU size,
         and the agent may also omit zero-valued trailing octets,
         to reduce the size of GetResponse PDUs."
    ::= { caqGlobalObjects 11 }


--*********************************************************************
-- Cisco CatOS Acl Qos Interface Group
--*********************************************************************
--
--

--
-- caqIfConfigTable
--

caqIfConfigTable  OBJECT-TYPE
    SYNTAX        SEQUENCE OF CaqIfConfigEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "This table describes the trust state and the default Cos
        value configured at each physical interface. It also 
        indicates whether an ACL attached to a Qos capable physical
        interface is applied per VLAN or per physical interface if
        the platform supports ACL configuration."
    ::= { caqInterfaceObjects 1 }
 
caqIfConfigEntry  OBJECT-TYPE
    SYNTAX        CaqIfConfigEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "The index of this table is the ifIndex of a
        physical port with QoS capability."
    INDEX { ifIndex }
    ::= { caqIfConfigTable 1 }
 
CaqIfConfigEntry  ::= SEQUENCE {
    caqIfCos                QosLayer2Cos,
    caqIfTrustStateConfig   INTEGER,
    caqIfAclBase            INTEGER,
    caqIfTrustDevice        BITS, 
    caqIfOperTrustState     INTEGER 
}
 

caqIfCos         OBJECT-TYPE
    SYNTAX       QosLayer2Cos 
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
        "This object indicates the default Cos value configured at this
        physical interface. This default value will be assigned to
        packet which does not have a Cos value in its layer-2 header
        when the packet arrives at this interface."  
    ::= { caqIfConfigEntry 1 }

caqIfTrustStateConfig   OBJECT-TYPE
    SYNTAX    INTEGER {
                  untrusted(1),
                  trustCoS(2),
                  trustIpPrec(3),
                  trustDscp(4)
              } 
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This object is used to set the trust state of an interface. 
        (whether the packets arriving at an interface are trusted to
        carry the correct data for classification.)

        If the object is untrusted(1), then the DSCP assigned to the
        packet is the DSCP specified by classification rule obtained
        from the matching ACE (Access Control Entry). ACE is a filter
        that is used to identify flows with certain characteristics. It
        includes fields such as ingress/egress ports, L2 addresses, L3
        addresses , TCP/UDP port number.

        If this object is trustCoS(2), then the DSCP assigned
        to the packet is the layer2 CoS of the packet mapped to a
        DSCP by the CoS-to-DSCP mapping defined in object
        caqCosToDscpDscp.

        When this object is trustIpPrec(3), a DSCP is assigned to
        an IP packet according to the IP-Precedence-to-DSCP mapping
        defined by the values contained in caqIpPrecToDscpTable. For 
        non-IP packets, trustIpPrec(3) has identical behavior as 
        trustCoS(2).

        When this object is trustDscp(4), the DSCP contained in an IP 
        packet is trusted as being the correct value to assign to it.
        For non-IP packets, trustDscp(4) has identical behavior as
        trustCoS(2)."
    DEFVAL { untrusted }
    ::= { caqIfConfigEntry 2 }

caqIfAclBase OBJECT-TYPE
    SYNTAX  INTEGER { vlan(1), port(2) }
    MAX-ACCESS read-write
    STATUS  current
    DESCRIPTION
        "For a given physical interface, this object indicates whether 
        packets arriving at that interface are classified and policed 
        based on port's ACL or based on the ACL of the VLAN which the
        port belongs to. This object is only instantiated if the
        platform support ACL configuration."
    ::= { caqIfConfigEntry 3 }

caqIfTrustDevice OBJECT-TYPE
    SYNTAX  BITS { 
                trustCiscoIPPhone(0) 
            }
    MAX-ACCESS read-write
    STATUS  current
    DESCRIPTION
        "For a given physical interface, this object indicates the
        restriction on trusting only a specific type of device which
        is connected to this interface to carry the correct data for
        classification.

        trustCiscoIPPhone(0) indicates that there is a restriction
        on trusting only ciscoIPPhone to carry the correct data for
        classification. 

        If there is no bits turned on, any device connected to
        this interface is trusted to carry the correct data for
        clarification.
 
        This object is only instantiated if the platform supports
        trust device configuration." 
    ::= { caqIfConfigEntry 4 }

caqIfOperTrustState   OBJECT-TYPE
    SYNTAX    INTEGER {
                  untrusted(1),
                  trustCoS(2),
                  trustIpPrec(3),
                  trustDscp(4)
              } 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object is used to indicate the operational trust state of
        an interface. The operational trust state may or may not be 
        identical to the config trust state denoted by
        caqIfTrustStateConfig. The value of this object depends on the
        runtime conditions such as whether the interface is configured
        to trust a certain type of device as denoted by caqIfTrustDevice
        as well as whether a device of the trusted type is connected to
        the interface. For example, if the interface is configured to
        only trust Cisco IP Phone and the phone is not connected to 
        the interface at runtime, the operational trust state of this
        interface will have the untrusted(1) value even if the
        trustCoS(2) value is configured in caqIfTrustStateConfig.

        This object is only instantiated if the platform supports
        trust device configuration. 

        If the object is untrusted(1), then the DSCP assigned to the
        packet is the DSCP specified by classification rule obtained
        from the matching ACE (Access Control Entry). ACE is a filter
        that is used to identify flows with certain characteristics. It
        includes fields such as ingress/egress ports, L2 addresses, L3
        addresses , TCP/UDP port number.

        If this object is trustCoS(2), then the DSCP assigned
        to the packet is the layer2 CoS of the packet mapped to a
        DSCP by the CoS-to-DSCP mapping defined in object
        caqCosToDscpDscp.

        When this object is trustIpPrec(3), a DSCP is assigned to
        an IP packet according to the IP-Precedence-to-DSCP mapping
        defined by the values contained in caqIpPrecToDscpTable. For 
        non-IP packets, trustIpPrec(3) has identical behavior as 
        trustCoS(2).

        When this object is trustDscp(4), the DSCP contained in an IP 
        packet is trusted as being the correct value to assign to it.
        For non-IP packets, trustDscp(4) has identical behavior as
        trustCoS(2)."
    ::= { caqIfConfigEntry 5 }

--
-- The caqClassifierTable
--

caqClassifierTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqClassifierEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table identifies which ACLs are in use on which
        interfaces. Some devices may impose constraints on the number
        of ACLs that can be attached to each interface; for example a
        constraint that at most three Qos ACLs, one for each type: IP,
        IPX and MAC, and at most three Security ACLs, one for each
        type: IP, IPX and MAC, can be attached to an interface."
    ::= { caqInterfaceObjects 2 }

caqClassifierEntry      OBJECT-TYPE
    SYNTAX      CaqClassifierEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry identifies that a particular ACL is in use on a
        particular interface. An interface can be a physical port
        or a VLAN."
    INDEX { ifIndex, caqClassifierAclType,
            IMPLIED caqClassifierAclName }
    ::= { caqClassifierTable 1 }

CaqClassifierEntry ::= SEQUENCE {
    caqClassifierAclType          INTEGER, 
    caqClassifierAclName          CaqAclName, 
    caqClassifierMapStatus        RowStatus,
    caqClassifierMapDirection     BITS
}

caqClassifierAclType       OBJECT-TYPE
    SYNTAX      INTEGER { 
                         ipQos(1), 
                         ipxQos(2), 
                         macQos(3),
                         ipSecurity(4),
                         ipxSecurity(5),
                         macSecurity(6)
                        } 
    MAX-ACCESS  not-accessible 
    STATUS      current
    DESCRIPTION
        "Indicates the type of ACL attached to this interface.

        ipQos(1) indicates that this ACL is an IP Qos ACL.

        ipxQos(2) indicates that this ACL is an IPX Qos ACL.

        macQos(3) indicates that this ACL is a MAC Qos ACL.

        ipSecurity(4) indicates that this ACL is an IP Security ACL.

        ipxSecurity(5) indicates that this ACL is an IPX Security ACL.

        macSecurity(6) indicates that this ACL is a MAC Security ACL."
    ::= { caqClassifierEntry 1 }

caqClassifierAclName       OBJECT-TYPE
    SYNTAX      CaqAclName 
    MAX-ACCESS  not-accessible 
    STATUS      current
    DESCRIPTION
        "Indicates the ACL name which should exist in the ACL tables
         e.g. in caqIpAceTable. This ACL can be a Qos ACL or a 
         Security ACL." 
    ::= { caqClassifierEntry 2 }

caqClassifierMapStatus     OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The status of this classifier conceptual row entry.
         An entry may not exist in the active state unless the
         ACL name denoted by caqClassifierAclName object in the 
         entry exist and active (i.e. its RowStatus object is 
         active(1)) in an ACL table. 

         Once a row becomes active, value in any other column within
         such row cannot be modified except by setting
         caqClassifierMapStatus to notInService(2) for such row."
    ::= { caqClassifierEntry 3 }

caqClassifierMapDirection     OBJECT-TYPE
    SYNTAX      BITS { ingress(0), egress(1) } 
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates whether this ACL are to be attached to ingress or
         egress direction." 
    DEFVAL { {ingress} }
    ::= { caqClassifierEntry 4 }

caqIfSecurityAclConfigTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF CaqIfSecurityAclConfigEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "A list of the interfaces which support the security
         ACL feature."
    ::= { caqInterfaceObjects 3 }

caqIfSecurityAclConfigEntry    OBJECT-TYPE
    SYNTAX        CaqIfSecurityAclConfigEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "An entry contains configuration information about
         a security ACL mapped to a interface which is capable
         for this feature."
    INDEX { ifIndex }
    ::= { caqIfSecurityAclConfigTable 1 }

CaqIfSecurityAclConfigEntry ::=
    SEQUENCE {
        caqIfSecurityAclBase    INTEGER
    }

caqIfSecurityAclBase OBJECT-TYPE
    SYNTAX    INTEGER {
              port(1),
              vlan(2),
              merge(3)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The security ACL configuration mode for an interface.

         Setting this variable to the value port(1) will cause the 
         packets (L3 forwarded packets and L2 packets) arriving at that
         interface to be filtered based on the ACL mapped to that
         interface.

         Setting this variable to the value vlan(2) will cause the 
         packets (L3 forwarded packets and L2 packets) arriving at that
         access interface to be filtered based on two ACL(the router's
         ACL and the ACL of the VLAN to which the interface belongs).
         If it is a trunking interface, the vlan-tag packets will be 
         filtered based on the ACL of the tag-vlan. 
          
         Setting this variable to the value merge(3) will merge the
         physical interface ACL, the VLAN ACL and the router ACL 
         together to emulate the logical serial model shown below.

                                 L3 only
         Port ACL -> VLAN ACL -> Router ACL -> Router ACL -> VLAN ACL
         physical    ingress     ingress       egress        egress
         interface"
   ::= { caqIfSecurityAclConfigEntry 1 }


--
-- The caqIpOperClassifierTable
--

caqIpOperClassifierTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqIpOperClassifierEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table identifies which operational IP ACLs are in use 
        on which interfaces." 
    ::= { caqInterfaceObjects 4 }

caqIpOperClassifierEntry      OBJECT-TYPE
    SYNTAX      CaqIpOperClassifierEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in this table identifies operational IP ACLs that
        are currently in use on a particular interface. An interface
        can be a physical port or a VLAN."
    INDEX { ifIndex, caqIpOperAclFeature }
    ::= { caqIpOperClassifierTable 1 }

CaqIpOperClassifierEntry ::= SEQUENCE {
    caqIpOperAclFeature        INTEGER,
    caqIpOperAclName           SnmpAdminString, 
    caqIpOperAclMapSource      BITS 
}

caqIpOperAclFeature       OBJECT-TYPE
    SYNTAX      INTEGER {
                    ingressIpQos(1),
                    egressIpQos(2),
                    ipSecurity(3)
                } 
    MAX-ACCESS  not-accessible 
    STATUS      current
    DESCRIPTION
        "An index indicates the feature to which the operational
        IP ACLs mapped at this interface are applied.

        'ingressIpQos' indicates the ACL mapped at this interface
        is used to classify ingress IP traffic for QoS feature.

        'egressIpQos' indicates the ACL mapped at this interface
        is used to classify egress IP traffic for QoS feature.
          
        'ipSecurity' indicates the ACL mapped at this interface
        is used to classify IP traffic for security feature."
    ::= { caqIpOperClassifierEntry 1 }

caqIpOperAclName       OBJECT-TYPE
    SYNTAX      SnmpAdminString
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
        "This object indicates the name of an operational IP ACL 
         which is mapped at this interface to classify IP traffic
         for feature denoted by caqIpOperAclFeature object." 
    ::= { caqIpOperClassifierEntry 2 }

caqIpOperAclMapSource     OBJECT-TYPE
    SYNTAX      BITS {
                    configured(0),
                    dot1x(1),
                    macAuth(2),
                    webAuth(3),
                    eou(4)     
                } 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates the sources that map the operational
         IP ACLs at this interface.

         'configured' indicates that the ACL mapping is introduced
         by manual configuration through CLI or an NMS application. 

         'dot1x' indicates that the ACL mapping is introduced by
         the operation of 802.1x feature. 

         'macAuth' indicates that the ACL mapping is introduced by
         the operation of Mac Authentication Bypass feature.

         'webAuth' indicates that the ACL mapping is introduced by
         the operation of Web Authentication feature. 

         'eou' indicates that the ACL mapping is introduced by
         the operation of Extensible Authentication Protocol over
         UDP (EOU) feature."
    ::= { caqIpOperClassifierEntry 3 }

--
-- The caqDownloadClassifierTable
--

caqDownloadClassifierTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqDownloadClassifierEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table identifies ACLs assignment to capable
        interface which is downloaded using different 
        security features."  
    ::= { caqInterfaceObjects 5 }

caqDownloadClassifierEntry      OBJECT-TYPE
    SYNTAX      CaqDownloadClassifierEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry identifies ACLs assignment on a capable
        physical interface."
    INDEX { ifIndex, caqDownloadAclFeature }
    ::= { caqDownloadClassifierTable 1 }

CaqDownloadClassifierEntry ::= SEQUENCE {
    caqDownloadAclFeature        INTEGER,
    caqDownloadClassifierAclName CaqAclName, 
    caqDownloadMapSource         INTEGER, 
    caqDownloadAclType           INTEGER 
}

caqDownloadAclFeature       OBJECT-TYPE
    SYNTAX      INTEGER {
                    ingressIpQos(1),
                    egressIpQos(2),
                    ipSecurity(3)
                } 
    MAX-ACCESS  not-accessible 
    STATUS      current
    DESCRIPTION
        "This object indicates the feature that ACLs mapped
        at this interface is used for.

        'ingressIpQos' indicates the ACL mapped at this interface
        is used to classify ingress IP traffic for QoS feature.

        'egressIpQos' indicates the ACL mapped at this interface
        is used to classify egress IP traffic for QoS feature.
          
        'ipSecurity' indicates the ACL mapped at this interface
        is used to classify IP traffic for security feature."
    ::= { caqDownloadClassifierEntry 1 }

caqDownloadClassifierAclName       OBJECT-TYPE
    SYNTAX      CaqAclName 
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
        "This object indicates the ACL name mapped to this
        interface to classify traffic for a specific feature
        denoted by the corresponding caqDownloadAclFeature."
    ::= { caqDownloadClassifierEntry 2 }

caqDownloadMapSource     OBJECT-TYPE
    SYNTAX      INTEGER {
                    dot1x(1),
                    macAuth(2)
                } 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates the source that maps the ACLs at this
        interface.

         'dot1x' indicates that the ACL mapping is introduced by
         the operation of 802.1x feature. 

         'macAuth' indicates that the ACL mapping is introduced by
         the operation of Mac Authentication Bypass feature."
    ::= { caqDownloadClassifierEntry 3 }

caqDownloadAclType     OBJECT-TYPE
    SYNTAX      INTEGER { pacl(1), vacl(2) } 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates the type of the ACL.

         'pacl' indicates this is a port-based ACL.
         'vacl' indicates this is a VLAN-based ACL."
    ::= { caqDownloadClassifierEntry 4 }

--**********************************************************************
-- Cisco CatOS Acl Qos Acl Group
--**********************************************************************
--
--

caqAclCapabilities  OBJECT-TYPE
    SYNTAX        BITS { 
                         ipQos(0), 
                         ipxQos(1), 
                         macQos(2),
                         ipSecurity(3), 
                         ipxSecurity(4), 
                         macSecurity(5) } 
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Indicates what ACL capabilities are supported on the device.
        An ACL belongs to one of the following types: IP, IPX and MAC.
        Furthermore, an ACL can be used for either QoS or Security
        feature.

        If ipQos(0) bit is turned on, caqIpAceTable can be instantiated
        for Qos feature, otherwise it can not.

        If ipxQos(1) bit is turned on, caqIpxAceTable can be
        instantiated for Qos feature, otherwise it can not.

        If macQos(2) bit is turned on, caqMacAceTable can be
        instantiated for Qos feature, otherwise it can not.

        If ipSecurity(3) bit is turned on, caqIpAceTable can be
        instantiated for Security feature, otherwise it can not.

        If ipxSecurity(4) bit is turned on, caqIpxAceTable can be
        instantiated for Security feature, otherwise it can not.

        If macSecurity(5) bit is turned on, caqMacAceTable can be
        instantiated for Security feature, otherwise it can not."
    ::= { caqAclObjects 1 }


--
-- caqIpAceTable
--

caqIpAceTable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqIpAceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains a list of IP ACEs. Each ACE consists of
        a filter specification and behavior associated with it which
        describes what action to carry out on packets which match.

        An ACL is defined as the set of ACEs of the same type (all
        QoS, or all Security).  Within a feature (qos or security),
        each ACE is named by a combination of an AclName and an ACE
        index, such that all the ACEs which are named using the same
        AclName are part of the same ACL."
    ::= { caqAclObjects 2 }

caqIpAceEntry    OBJECT-TYPE
    SYNTAX      CaqIpAceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry defines an ACE, consisting of a set of match
        criteria. For a packet to match an entry, it has to match
        all the criteria specified in that entry."
    INDEX {  caqIpAceFeature, caqIpAclName, caqIpAceIndex }
    ::= { caqIpAceTable 1 }

CaqIpAceEntry ::= SEQUENCE {
    caqIpAceFeature                INTEGER,
    caqIpAclName                   CaqAclName,
    caqIpAceIndex                  Unsigned32,
    caqIpAceMatchedAction          Unsigned32, 
    caqIpAceProtocolType           Unsigned32, 
    caqIpAceAddrType               InetAddressType,
    caqIpAceSrcIp                  InetAddress,
    caqIpAceSrcIpMask              InetAddress,
    caqIpAceSrcPortOp              INTEGER,
    caqIpAceSrcPort                Unsigned32,
    caqIpAceSrcPortRange           Unsigned32,
    caqIpAceDestIp                 InetAddress,
    caqIpAceDestIpMask             InetAddress,
    caqIpAceDestPortOp             INTEGER,
    caqIpAceDestPort               Unsigned32,
    caqIpAceDestPortRange          Unsigned32,
    caqIpAceTosMatchCriteria       INTEGER,
    caqIpAceIpPrec                 CaqIpPrecedence,
    caqIpAceDscp                   Dscp,
    caqIpAceProtocolMatchCriteria  INTEGER,
    caqIpAceIcmpType               Unsigned32,
    caqIpAceIcmpCode               Unsigned32,
    caqIpAceIgmpType               Unsigned32,
    caqIpAceOrderPosition          Unsigned32,
    caqIpAceBeforePosition         Unsigned32,
    caqIpAceStatus                 RowStatus,
    caqIpAceSecurityId             Unsigned32,
    caqIpAceSrcGroup               SnmpAdminString,
    caqIpAceDestGroup              SnmpAdminString,
    caqIpAceType                   INTEGER
}

caqIpAceFeature       OBJECT-TYPE
    SYNTAX      INTEGER { qos(1), security(2) } 
    MAX-ACCESS  not-accessible 
    STATUS      current
    DESCRIPTION
        "Indicates whether this entry is a Qos ACL or Security ACL.
        ACEs belongs to the same ACL should have the same value
        for this object." 
    ::= { caqIpAceEntry 1 }

caqIpAclName  OBJECT-TYPE
    SYNTAX      CaqAclName
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The name of an ACL. Within a feature (qos or security), the
        name is unique across all of the ACL tables that identifies
        the list to which the entry belongs in the device." 
    ::= { caqIpAceEntry 2 }

caqIpAceIndex       OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The index of an ACE within an ACL." 
    ::= { caqIpAceEntry 3 }

caqIpAceMatchedAction      OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535) 
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the action to be taken if a packet matches this ACE.
        If the value of this ACE's caqIpAceFeature object is: 'qos(1)',
        then this object contains the index of an active row in
        caqQosActionSelectTable.  If the value of this ACE's
        caqIpAceFeature object is: 'security(2)', then this object
        contains the index of an active row in caqSecurityActionTable."
    ::= { caqIpAceEntry 4 }

caqIpAceProtocolType        OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255) 
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The protocol number field in the IP header used to indicate
        the higher layer protocol as specified in RFC 1700. A value 
        value of 0 matches every IP packet. 

        For example :
        0 is IP, 1 is ICMP, 2 is IGMP, 4 is IP in IP encapsulation,
        6 is TCP, 9 is IGRP, 17 is UDP, 47 is GRE, 50 is ESP, 51 is AH,
        88 is IGRP, 89 is OSPF, 94 is KA9Q/NOS compatible IP over IP,
        103 is PIMv2, 108 is PCP."
    REFERENCE
        "RFC 1700, Assigned Numbers."
    DEFVAL { 0 } -- IP
    ::= { caqIpAceEntry 5 }

caqIpAceAddrType        OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The type of IP address used by this ACE entry."
    ::= { caqIpAceEntry 6 } 

caqIpAceSrcIp           OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The specified source IP address. The packet's source address is
        AND-ed with the value of caqIpAceSrcIpMask and then compared
        against the value of this object. If this object value is
        0.0.0.0, and the value of caqIpAceSrcIpMask object in the same
        entry is 255.255.255.255, this entry matches any source IP
        address." 
    ::= { caqIpAceEntry 7 }

caqIpAceSrcIpMask           OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The specified source IP address mask."
    ::= { caqIpAceEntry 8 }

caqIpAceSrcPortOp       OBJECT-TYPE
    SYNTAX      INTEGER { noOperator(1), lt(2), gt(3),
                          eq(4), neq(5), range(6) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates how a packet's source TCP/UDP port number is
        to be compared.

        If the caqIpAceProtocolType object in the same row does not
        indicate TCP or UDP, this object has to be 'noOperator(1)' and
        cannot be changed while this row is active, i.e., the value of
        caqIpAceStatus in the same row has the value 'active(1)'.
  
        'noOperator(1)', which is the default value, means that no
        comparison is to be made with the source TCP/UDP port number.

        lt(2) means less than, gt(3) means greater than, eq(4)
        means equal, neq(5) means not equal. Those 4 operators
        are using the caqIpAceSrcPort object as an operand which
        is the only one needed. 

        range(6) means that it compares the port value between two 
        numbers, so this operator needs 2 operands. One operand is 
        the starting port number of the range which is caqIpAceSrcPort 
        object, and the other operand is the ending port number of the 
        range which the caqIpAceSrcPortRange object is in."
    DEFVAL { noOperator }
    ::= { caqIpAceEntry 9 }

caqIpAceSrcPort     OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The source port number of the TCP or UDP protocol. If the
        caqIpAceSrcPortOp object in the same row is range(6), this
        object will be the starting port number of the port range.
        This object cannot be configured if caqIpAceStatus in the 
        same row is active(1) or caqIpAceSrcPortOp in the same row
        is noOperator(1)."
    ::= { caqIpAceEntry 10 }

caqIpAceSrcPortRange    OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The source port number of the TCP or UDP protocol. If the
        caqIpAceSrcPortOp object in the same row is range(6), this
        object will be the ending port number of the port range.
        This object cannot be configured if caqIpAceStatus in the 
        same row is active(1) or caqIpAceSrcPortOp in the same row
        is not range(6)."
    ::= { caqIpAceEntry 11 }

caqIpAceDestIp          OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The specified destination IP address. The packet's destination
        address is AND-ed with the value of caqIpAceDestIpMask and then
        compared against the value of this object. If this object value
        is 0.0.0.0 and the value of caqIpAceDestIpMask object in the
        same entry is 255.255.255.255, this entry matches any
        destination IP address." 
    DEFVAL { '00000000'H } -- 0.0.0.0
    ::= { caqIpAceEntry 12 }

caqIpAceDestIpMask  OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The specified destination IP address mask."
    DEFVAL  { 'FFFFFFFF'H } -- 255.255.255.255
    ::= { caqIpAceEntry 13 }

caqIpAceDestPortOp      OBJECT-TYPE
    SYNTAX      INTEGER { noOperator(1), lt(2), gt(3),
                          eq(4), neq(5), range(6) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates how a packet's destination TCP/UDP port number is
        to be compared.

        If the caqIpAceProtocolType object in the same row does not
        indicate TCP or UDP, this object has to be 'noOperator(1)' and
        cannot be changed while this row is active, i.e., the value of
        caqIpAceStatus in the same row has the value 'active(1)'.

        'noOperator(1)', which is the default value, means that no
        comparison is to be made with the destination TCP/UDP port
        number.

        lt(2) means less than.
        
        gt(3) means greater than.
 
        eq(4) means equal. 
        
        neq(5) means not equal. Those 4 operators are using the 
        caqIpAceDestPort object as an operand which is the only one
        needed. 

        range(6) means that it compares the port value between two
        numbers, so this operator needs 2 operands. One operand is the
        starting port number of the range which is caqIpAceDestPort
        object, and the other operand is the ending port number
        of the range which the caqIpAceDestPortRange object is in."
    DEFVAL { noOperator }
    ::= { caqIpAceEntry 14 }

caqIpAceDestPort        OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The destination port number of the TCP or UDP protocol.
        If the caqIpAceDestPortOp object in the same row is range(6),
        this object will be the starting port number of the port range.
        This object cannot be configured if caqIpAceStatus in the 
        same row is active(1) or caqIpAceDestPortOp in the same row
        is noOperator(1)."
    ::= { caqIpAceEntry 15 }

caqIpAceDestPortRange   OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The destination port number of the TCP or UDP protocol.
        If the caqIpAceDestPortOp object in the same row is range(6),
        this object will be the ending port number of the port range.
        This object cannot be configured if caqIpAceStatus in the 
        same row is active(1) or caqIpAceDestPortOp in the same row
        is not range(6)."
    ::= { caqIpAceEntry 16 }

caqIpAceTosMatchCriteria     OBJECT-TYPE
    SYNTAX        INTEGER {
                    none(1), 
                    matchDscp(2),
                    matchIpPrec(3)
                  }
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "Indicates what field of Tos octet in the packet header
         to be matched. 
         
         none(1) means that there is no need to match the ToS octet.

         matchDscp(2) means that the DSCP value of packet header need
         to be matched. If this value is specified, the caqIpAceDscp
         object in the same row should be configured.  

         matchIpPrec(3) means that the IpPrecedence value of packet
         header need to be matched. If this value is specifed, the 
         caqIpAceIpPrec object in the same row should be configured."
    DEFVAL { none }
    ::= { caqIpAceEntry 17 }
 
caqIpAceIpPrec    OBJECT-TYPE
    SYNTAX      CaqIpPrecedence
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the IP precedence value to be matched against.
        This object could not be configured when the status of the
        entry, caqIpAceStatus, is active(1).  
        
        The value of this object is ignored whenever the value of 
        caqIpAceTosMatchCritial object is not matchIpPrec(3)."
    DEFVAL { 0 }
    ::= { caqIpAceEntry 18 }

caqIpAceDscp       OBJECT-TYPE
    SYNTAX      Dscp
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the Dscp value to be matched against.
        This object could not be configured when the status of the
        entry, caqIpAceStatus, is active(1).  Packets can be matched
        the DSCP level from 0 to 63. 

        The value of this object is ignored whenever the value of 
        caqIpAceTosMatchCritial object is not matchDscp(2)."
    DEFVAL { 0 }
    ::= { caqIpAceEntry 19 }

caqIpAceProtocolMatchCriteria     OBJECT-TYPE
    SYNTAX        INTEGER {
                    none(1), 
                    matchIgmpType(2),
                    matchIcmpType(3),
                    matchIcmpTypeAndCode(4),
                    matchEstablished(5),
                    matchSecurityId(6),
                    matchEapoudp(7),
                    matchUrlRedirect(8)
                  }
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "Indicates what field in the packet header for ICMP or IGMP
         or TCP protocol or IPv4 ESP (Enscrypted Security Payload)
         to be matched. 
         
         none(1) = no comparison is to be done for ICMP/IGMP/TCP/ESP.

         matchIgmpType(2) means that the Type field of IGMP protocol
         packet header needs to be matched. If this value is specified,
         the caqIpAceIgmpType object in the same row should be
         configured.  

         matchIcmpType(3) means that the Type field of ICMP protocol
         packet header needs to be matched. If this value is specified,
         the caqIpAceIcmpType object in the same row should be
         configured.

         matchIcmpTypeAndCode(4) means that both the Type and Code
         fields of ICMP protocol packet header need to be matched.
         If this value is specified, the caqIpAceIcmpType and
         caqIpAceIcmpCode object in the same row should be configured.
         
         matchEstablished(5) means that a match occurs if the TCP packet
         has the ACK or RST bits set. The non matching case is that of
         the intial TCP packet to form a connection.

         matchSecurityId(6) means that the Security Association
         Identifier field of IPv4 ESP packet header needs to be matched.
         If this value is specified, the caqIpAceSecurityId object in
         the same row should be configured.

         matchEapoudp(7) means that this ACE needs to be matched
         against the criteria for EAP (Extensible Authentication
         Protocol) over UDP purpose. 

         matchUrlRedirect(8) means that this ACE needs to be matched
         against the criteria for URL redirection purpose."
    DEFVAL { none }
    ::= { caqIpAceEntry 20 }

caqIpAceIcmpType        OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the message type of ICMP packets. The type is
        a number from 0 to 255. 

        The value of this object is ignored whenever the value of 
        caqIpAceProtocolMatchCritial object is not matchIcmpType(3) or
        matchIcmpTypeAndCode(4)."
    DEFVAL { 0 }
    ::= { caqIpAceEntry 21 }

caqIpAceIcmpCode        OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the message code of ICMP packets. The code is
        a number from 0 to 255. 

        The value of this object is ignored whenever the value of 
        caqIpAceProtocolMatchCritial object is not
        matchIcmpTypeAndCode(4)."
    DEFVAL { 0 }
    ::= { caqIpAceEntry 22 }

caqIpAceIgmpType        OBJECT-TYPE
    SYNTAX      Unsigned32 (0..15)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the message type of IGMP packets. The code is
        a number from 0 to 15.

        The value of this object is ignored whenever the value of 
        caqIpAceProtocolMatchCritial object is not matchIgmpType(2)."
    DEFVAL { 0 }
    ::= { caqIpAceEntry 23 }

caqIpAceOrderPosition     OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The ordering position of this ACE in the ACL. If this entry
        is not in active(1) state, this object has value of 0."
    ::= { caqIpAceEntry 24 }

caqIpAceBeforePosition       OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object is to control the position of an ACE in the ACL.
        Indicates the order position of a new ACE before an active ACE 
        which is already in the ACL. It means that the new ACE will 
        replace the position of the ACE which the object specifies.

        For example, if there are 6 ACEs in an ACL, so the positions
        of those 6 ACEs will be 1, 2, 3, 4, 5, 6. If the user would
        like to add a new ACE and specifies 4 to be the value of
        this object, the old ACEs in positions, 4, 5, 6 will become
        5, 6, 7 while the entry containing the new ACE is active.
        Be careful, for example, if the user would like to move an ACE
        whose position is 2 to before the ACE whose position is 5. He
        put the status of that entry to in-active and the position order
        will be 1, 2, 3, 4, 5.  The old ACEs in positions 3, 4, 5, 6
        becomes 2, 3, 4, 5. So, the user has to specify the object to 4,
        because the ACE in old position 5 has been moved to position 4.

        If not specified, the default value 0 will be used. And the
        new ACE is appended to the end of the ACL. 0 will be always
        returned if the status of this row is active. If the entry
        is from active(1) to notInService(2), this object should have 
        default value."
    DEFVAL { 0 }
    ::= { caqIpAceEntry 25 }

caqIpAceStatus      OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The status of this IP ACE conceptual row entry. This object is 
        used to manage creation, deletion and modification of rows in
        this table. 
       
        An entry may not exist in the active state unless all objects
        in the entry have an appropriate value. Especially, it cannot
        be in active state unless the caqIpAceMatchedAction object in
        the entry point to an active entry (i.e its RowStatus object is
        active(1)) in the caqQosActionSelectTable or
        caqSecurityActionTable. Once a row becomes active, value in any 
        other column within such row cannot be modified.

        If this row is the only ACE in an ACL and the value of its
        caqIpAclName object matches the value of caqClassifierAclName
        object in any active entry of the caqClassifierTable, removing
        this entry will also remove the associated entry in the 
        caqClassifierTable.

        If the value of caqIpAceType in this row is 'systemGenerated', 
        this row cannot be deleted or modified." 
    ::= { caqIpAceEntry 26 }

caqIpAceSecurityId        OBJECT-TYPE
    SYNTAX      Unsigned32 (0 |4..233)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the Security Association Identifier of IPv4 ESP
        packets. 

        The value of this object is ignored whenever the value of 
        caqIpAceProtocolMatchCritial object is not matchSecurityId(6)."
    DEFVAL { 0 }
    ::= { caqIpAceEntry 27 }

caqIpAceSrcGroup        OBJECT-TYPE
    SYNTAX      SnmpAdminString 
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the source group name which the source IP address
         in the IP packet header belongs to. If this object is 
         configured, the value of caqIpAceProtocolType object in the
         same row will have the value of 0." 
    DEFVAL { "" }
    ::= { caqIpAceEntry 28 }

caqIpAceDestGroup        OBJECT-TYPE
    SYNTAX      SnmpAdminString 
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the destination group name which the destination
         IP address in the IP packet header belongs to. If this object
         is configured, the value of caqIpAceProtocolType object in
         the same row will have the value of 0."
    DEFVAL { "" }
    ::= { caqIpAceEntry 29 }

caqIpAceType        OBJECT-TYPE
    SYNTAX      INTEGER { configured(1), systemGenerated(2) } 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the ACE type." 
    ::= { caqIpAceEntry 30 }

--
-- caqIpxAceTable
--

caqIpxAceTable   OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqIpxAceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains a list of IPX ACEs. Each ACE consists of
        a filter specification and behavior associated with it which
        describes what action to carry out on packets which match.

        An ACL is defined as the set of ACEs of the same type (all
        QoS, or all Security).  Within each feature (qos or security),
        each ACE is named by a combination of an AclName and an ACE
        index, such that all the ACEs which are named using the same
        AclName are part of the same ACL. This table is instantiated
        only if the ipxQos bit or ipxSecurity bit of caqAclCapabilities
        object is turned on."
    ::= { caqAclObjects 3 }

caqIpxAceEntry   OBJECT-TYPE
    SYNTAX      CaqIpxAceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry of caqIpxAceTable consists of a set of match
        creteria. For a IPX flow to match an entry, it has to match
        all the conditions specified in that entry."
    INDEX { caqIpxAceFeature, caqIpxAclName , caqIpxAceIndex }
    ::= { caqIpxAceTable 1 }

CaqIpxAceEntry ::= SEQUENCE {
    caqIpxAceFeature            INTEGER,
    caqIpxAclName               CaqAclName,
    caqIpxAceIndex              Unsigned32,
    caqIpxAceMatchedAction      Unsigned32, 
    caqIpxAceSrcNet             OCTET STRING, 
    caqIpxAceDestMatchCriteria  BITS,
    caqIpxAceProtocolType       Unsigned32,
    caqIpxAceDestNet            OCTET STRING, 
    caqIpxAceDestNode           OCTET STRING,
    caqIpxAceDestNetMask        OCTET STRING, 
    caqIpxAceDestNodeMask       OCTET STRING,
    caqIpxAceOrderPosition      Unsigned32,
    caqIpxAceBeforePosition     Unsigned32,
    caqIpxAceStatus             RowStatus
}

caqIpxAceFeature       OBJECT-TYPE
    SYNTAX      INTEGER { qos(1), security(2) } 
    MAX-ACCESS  not-accessible 
    STATUS      current
    DESCRIPTION
        "Indicates whether this entry is a Qos ACL or Security ACL.
        ACEs belongs to the same ACL should have the same value
        for this object." 
    ::= { caqIpxAceEntry 1 }

caqIpxAclName  OBJECT-TYPE
    SYNTAX      CaqAclName
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The name of an ACL. Within a feature (qos or security), this
        name is unique across all of the ACL tables that identifies
        the list to which the entry belongs in the device." 
    ::= { caqIpxAceEntry 2 }

caqIpxAceIndex      OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The index of an IPX ACE within an ACL." 
    ::= { caqIpxAceEntry 3 }

caqIpxAceMatchedAction     OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535) 
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the action to be taken if a packet matches this ACE.
        If the value of this ACE's caqIpxAceFeature object is: 'qos(1)',
        then this object contains the index of an active row in
        caqQosActionSelectTable.  If the value of this ACE's
        caqIpxAceFeature object is: 'security(2)', then this object
        contains the index of an active row in caqSecurityActionTable."
    ::= { caqIpxAceEntry 4 }

caqIpxAceSrcNet     OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(4)) 
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the source network from which the packet is
        being sent. This is a 32-bits value that uniquely identifies
        network cable segment in IPX protocol. 
        A network number of 0xFFFFFFFF matches all networks."
    ::= { caqIpxAceEntry 5 }

caqIpxAceDestMatchCriteria        OBJECT-TYPE
    SYNTAX    BITS {
                   matchProtocol(0),
                   matchIpxDestNet(1),
                   matchIpxDestNode(2),
                   matchIpxDestNetMask(3),
                   matchIpxDestNodeMask(4)
              }
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "Indicate which matches to be checked for the
        destination network of the flow.

        matchProtocol(0) means that the flow protocol
        will be matched against the value specified by
        caqIpxAceProtocolType object in the same row.

        matchIpxDestNet(1)  means that the flow destination
        network will be matched against the value specified
        by caqIpxAceDestNet object in the same row.

        matchIpxDestNode(2) means that the flow destination node
        will be matched against the value specified by 
        caqIpxAceDestNode object in the same row.
        If this option bit is on, the matchIpxDestNet(1) bit has
        to be on also.

        matchIpxDestNetMask(3) means that the packet's flow destination
        network will be AND-ed with the value specified by 
        caqIpxAceDestNetMask object in the same row and then compared
        against the value of caqIpxAceDestNet object.

        matchIpxDestNodeMask(4) means that the packet's flow
        destination node will be AND-ed with the value specified by
        caqIpxAceDestNodeMask object in the same row and then compared
        against the value of caqIpxAceDestNode object."
    DEFVAL { { } }
    ::= { caqIpxAceEntry 6 }

caqIpxAceProtocolType        OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The protocol number field in the IPX header used to indicate
        the higher layer protocol.  It can be any, ncp, netbios, rip,
        sap or an integer between 0 to 255."
    REFERENCE
        "RFC 1700, Assigned Numbers."
    ::= { caqIpxAceEntry 7 }

caqIpxAceDestNet        OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(4)) 
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Number of the destination network to which the packet
        is being sent. This is a 32-bit value that uniquely identifies
        the IPX network cable segment in IPX protocol.  A network
        number of 0xFFFFFFFF matches all networks.

        The value of this object is ignored whenever the
        matchIpxDestNet(1) and matchIpxDestNetMask(3) bits of
        caqIpxAceDestMatchCriteria object are not on."
    ::= { caqIpxAceEntry 8 }

caqIpxAceDestNode       OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (6))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Node on the destination network to which the packet is being
        sent. This is a 48 bits value.

        The value of this object is ignored whenever the
        matchIpxDestNode(2) and matchIpxDestNodeMask(4) bits of
        caqIpxAceDestMatchCriteria object are not on."
    ::= { caqIpxAceEntry 9 }

caqIpxAceDestNetMask        OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(4)) 
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Mask to be applied to the destination net. This is an
        32-bit value that has the same format as destination net.

        The value of this object is ignored whenever the
        matchIpxDestNetMask(3) bit of caqIpxAceDestMatchCriteria
        object is not on."
    ::= { caqIpxAceEntry 10 }

caqIpxAceDestNodeMask       OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (6))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Mask to be applied to the destination node.  This is a 48-bit
        value.

        The value of this object is ignored whenever the
        matchIpxDestNodeMask(4) bit of caqIpxAceDestMatchCriteria
        object is not on."
    ::= { caqIpxAceEntry 11 }

caqIpxAceOrderPosition     OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The ordering position of this ACE in the ACL. If this entry
        is not in active(1) state, this object has value of 0."
    ::= { caqIpxAceEntry 12 }

caqIpxAceBeforePosition       OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object is to control the position of an ACE in the ACL.
        Specifies the order position of a new ACE before an active ACE 
        which is already in the ACL. It means that the new ACE will 
        replace the position of the ACE which the object specifies.

        For example, if there are 6 ACEs in an ACL, so the positions
        of those 6 ACEs will be 1, 2, 3, 4, 5, 6. If the user would
        like to add a new ACE and he specifies 4 to be the value of
        this object, the old ACEs in positions, 4, 5, 6 will become
        5, 6, 7 while the entry containing the new ACE is active.
        The removing is similar. Be careful, for example, if the
        user would like to move an ACE whose position is 2 to before
        the ACE whose position is 5. He put the status of that entry
        to in-active and the position order will be 1, 2, 3, 4, 5.
        The old ACEs in positions 3, 4, 5, 6 becomes 2, 3, 4, 5. So,
        the user has to specify the object to 4, because the ACE in
        old position 5 has been moved to position 4.

        If not specified, the default value 0 will be used. And the
        new ACE is appended to the end of the ACL. 0 will be always
        returned if the status of this row is active. If the entry
        is from active(1) to notInService(2), this object should be 
        default value."
    DEFVAL { 0 }
    ::= { caqIpxAceEntry 13 }


caqIpxAceStatus     OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The status of this IPX ACE conceptual row entry. This object
        is used to manage creation, deletion and modification of rows
        in this table. 
       
        An entry may not exist in the active state unless all objects 
        in the entry have an appropriate value. Especially, it cannot
        be in active state unless the caqIpxAceMatchedAction object in
        the entry point to an active entry (i.e its RowStatus object is 
        active(1)) in the caqQosActionSelectTable or 
        caqSecurityActionTable. Once a row becomes active, value in any 
        other column within such row cannot be modified.

        If this row is the only ACE in an ACL and the value of its
        caqIpxAclName object matches the value of caqClassifierAclName
        object in any active entry of the caqClassifierTable, removing
        this entry will also remove the associated entry in the 
        caqClassifierTable." 
    ::= { caqIpxAceEntry 14 }

--
-- caqMacAceTable
--

caqMacAceTable   OBJECT-TYPE
    SYNTAX  SEQUENCE OF CaqMacAceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains a list of MAC ACEs. Each ACE consists of
        a filter specification and behavior associated with it which
        describes what action to carry out on packets which match.

        An ACL is defined as the set of ACEs of the same type (all
        QoS, or all Security).  Within a feature (qos or security), each
        ACE is named by a combination of an AclName and an ACE index,
        such that all the ACEs which are named using the same AclName
        are part of the same ACL. This table is instantiated only if
        the macQos bit or macSecurity bit of caqAclCapabilities object
        is turned on."
    ::= { caqAclObjects 4 }

caqMacAceEntry   OBJECT-TYPE
    SYNTAX      CaqMacAceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry of caqMacAceTable consist of a set of match
        criteria. For a layer 2 flow to match an entry, it has to
        match all the conditions specified in that entry."
    INDEX { caqMacAceFeature, caqMacAclName, caqMacAceIndex }
    ::= { caqMacAceTable 1 }

CaqMacAceEntry ::= SEQUENCE {
    caqMacAceFeature        INTEGER,
    caqMacAclName           CaqAclName,
    caqMacAceIndex          Unsigned32,
    caqMacAceMatchedAction  Unsigned32, 
    caqMacAceSrcMac         MacAddress,
    caqMacAceSrcMacMask     MacAddress,
    caqMacAceDestMac        MacAddress,
    caqMacAceDestMacMask    MacAddress,
    caqMacAceEthertype      Unsigned32,
    caqMacAceOrderPosition  Unsigned32,
    caqMacAceBeforePosition Unsigned32,
    caqMacAceStatus         RowStatus,
    caqMacAceMatchCriteria  BITS,
    caqMacAceCos            QosLayer2Cos,
    caqMacAceVlan           VlanIndex
}

caqMacAceFeature       OBJECT-TYPE
    SYNTAX      INTEGER { qos(1), security(2) } 
    MAX-ACCESS  not-accessible 
    STATUS      current
    DESCRIPTION
        "Indicates whether this entry is a Qos ACL or Security ACL." 
    ::= { caqMacAceEntry 1 }

caqMacAclName  OBJECT-TYPE
    SYNTAX      CaqAclName
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The name of an ACL. Within a feature (qos or security), this
        name is unique across all the ACL tables that identifies the
        list to which the entry belongs in the device." 
    ::= { caqMacAceEntry 2 }

caqMacAceIndex      OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The index of an Mac ACE within an ACL." 
    ::= { caqMacAceEntry 3 }

caqMacAceMatchedAction        OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535) 
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the action to be taken if a packet matches this ACE.
        If the value of this ACE's caqMacAceFeature object is: 'qos(1)',
        then this object contains the index of an active row in
        caqQosActionSelectTable.  If the value of this ACE's
        caqMacAceFeature object is: 'security(2)', then this object
        contains the index of an active row in caqSecurityActionTable."
    ::= { caqMacAceEntry 4 }

caqMacAceSrcMac     OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the 48 bits source MAC address. The packet's source
        address is AND-ed with the value of caqMacAceSrcMacMask and then
        compared against the value of this object. If this object value
        is 00-00-00-00-00-00, and the value of caqMacAceSrcMacMask
        object in the same entry is ff-ff-ff-ff-ff-ff, this entry
        matches any source Mac address." 
    ::= { caqMacAceEntry 5 }

caqMacAceSrcMacMask OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the 48 bit source MAC address mask."
    ::= { caqMacAceEntry 6 }

caqMacAceDestMac        OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the 48 bits destination MAC address. The packet's
        destination  address is AND-ed with the value of
        caqMacAceDestMacMask and then compared against the value of
        this object. If this object value is 00-00-00-00-00-00, and the
        value of caqMacAceDestMacMask object in the same entry is
        ff-ff-ff-ff-ff-ff, this entry matches any destionation Mac
        address." 
    ::= { caqMacAceEntry 7 }

caqMacAceDestMacMask    OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the 48 bit destination MAC address mask."
    ::= { caqMacAceEntry 8 }

caqMacAceEthertype  OBJECT-TYPE
    SYNTAX      Unsigned32 ('0000'H..'FFFF'H)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This 16-bit hexadecimal number indicates the matched Ethernet
        type. 0x0000 means any Ethernet type will be matched."
    REFERENCE
        "RFC 1700, Assigned Numbers."
    DEFVAL { '0000'H }
    ::= { caqMacAceEntry 9 }

caqMacAceOrderPosition     OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The ordering position of this ACE in the ACL. If this entry
        is not in active(1) state, this object has value of 0."
    ::= { caqMacAceEntry 10 }

caqMacAceBeforePosition       OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object is to control the position of an ACE in the ACL.
        Specifies the order position of a new ACE before a ACE which
        is already in the ACL. It means that the new ACE will replace
        the position of the ACE which the object specifies.

        For example, if there are 6 ACEs in an ACL, so the positions
        of those 6 ACEs will be 1, 2, 3, 4, 5, 6. If the user would
        like to add a new ACE and he specifies 4 to be the value of
        this object, the old ACEs in positions, 4, 5, 6 will become
        5, 6, 7 while the entry containing the new ACE is active.
        The removing is similar. Be careful, for example, if the
        user would like to move an ACE whose position is 2 to before
        the ACE whose position is 5. He put the status of that entry
        to in-active and the position order will be 1, 2, 3, 4, 5.
        The old ACEs in positions 3, 4, 5, 6 becomes 2, 3, 4, 5. So,
        the user has to specify the object to 4, because the ACE in
        old position 5 has been moved to position 4.

        If not specified, the default value 0 will be used. And the
        new ACE is appended to the end of the ACL. 0 will be always
        returned if the status of this row is active. If the entry
        is from active to notInService, this object should has default
        value."
    DEFVAL { 0 }
    ::= { caqMacAceEntry 11 }

caqMacAceStatus     OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The status of this MAC ACE conceptual row entry. This object
        is used to manage creation, deletion and modification of rows
        in this table. 
       
        An entry may not exist in the active state unless all objects 
        in the entry have an appropriate value. Especially, it cannot
        be in active state unless the caqMacAceMatchedAction object in
        the entry point to an active entry (i.e its RowStatus object is 
        active(1)) in the caqQosActionSelectTable or 
        caqSecurityActionTable. Once a row becomes active, value in any 
        other column within such row cannot be modified.

        If this row is the only ACE in an ACL and the value of its
        caqMacAclName object matches the value of caqClassifierAclName
        object in any active entry of the caqClassifierTable, removing
        this entry will also remove the associated entry in the 
        caqClassifierTable." 
    ::= { caqMacAceEntry 12 }

caqMacAceMatchCriteria        OBJECT-TYPE
    SYNTAX    BITS {
                   matchCos(0),
                   matchVlan(1)
              }
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "Indicates which field in the packet header to be matched. 

        matchCos(0) means that the packet Cos value  
        will be matched against the value specified by
        caqMacAceCos object in the same row.

        matchVlan(1) means that the packet VLAN value 
        will be matched against the value specified by
        caqMacAceVlan object in the same row."
    DEFVAL { { } }
    ::= { caqMacAceEntry 13 }

caqMacAceCos        OBJECT-TYPE
    SYNTAX      QosLayer2Cos 
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the packet Cos value to be matched.

         The value of this object is ignored whenever the
         matchCos(0) bit of caqMacAceMatchCriteria object
         is not on." 
    ::= { caqMacAceEntry 14 }

caqMacAceVlan        OBJECT-TYPE
    SYNTAX      VlanIndex 
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the packet VLAN number to be matched.
     
         The value of this object is ignored whenever the
         matchVlan(1) bit of caqMacAceMatchCriteria object
         is not on." 
    ::= { caqMacAceEntry 15 }

--
--  Flow policing capability
--

caqFlowPolicingCpb   OBJECT-TYPE
    SYNTAX      BITS { 
                      microFlow(0),
                      aggregate(1)
                     }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the flow policing capability of the device.

         microFlow(0) indicates that microflow can be policed.

         aggregate(1) indicates that aggregate flow can be policed."
    ::= { caqAclObjects 5 } 

--
-- caqQosActionSelectTable
--

caqQosActionSelectTable       OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqQosActionSelectEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table describes the actions of ACEs.  Once an ACE is
        matched, it follows its MatchedAction object to an entry of this
        table to get an action for the matching ACE. 
        An action includes policer information as well as an DSCP 
        associated with trust state information of the matching ACE." 
    ::= { caqAclObjects 6 }

caqQosActionSelectEntry       OBJECT-TYPE
    SYNTAX      CaqQosActionSelectEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "An entry of an ACE action. It links to the entries of
        caqFlowPolicerTable with caqQosActionSelectMicroflow, 
        caqQosActionSelectAggregate objects."
    INDEX { caqQosActionSelectIndex }
    ::= { caqQosActionSelectTable 1 }

CaqQosActionSelectEntry   ::= SEQUENCE {
    caqQosActionSelectIndex       Unsigned32,
    caqQosActionSelectTrust       INTEGER,
    caqQosActionSelectDscp        Dscp,
    caqQosActionSelectMicroflow   CaqPolicerNameOrEmpty, 
    caqQosActionSelectAggregate   CaqPolicerNameOrEmpty, 
    caqQosActionSelectStatus      RowStatus
}

caqQosActionSelectIndex       OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The index of this table for indicating an ACE Action for QoS."
    ::= { caqQosActionSelectEntry 1 }

caqQosActionSelectTrust       OBJECT-TYPE
    SYNTAX    INTEGER { noTrust(1), trustCos(2),
                        trustIpPrec(3), trustDscp(4) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Determines if the packets matching the ACE should be trusted
        or if a specific DSCP should be assigned to it.

        If trustCos(2) is specified, the final DSCP value should refer
        to caqCosToDscpDscp object in caqCosToDscpTable to transfer
        layer 2 CoS value to DSCP value.

        If trustIpPrec(3) is specified, the final DSCP value should
        refer to caqIpPrecToDscpDscp object in caqIpPrecToDscpTable
        to transfer IP Precedence value to DSCP value.

        If trustDscp(4) is specified, the final DSCP value is the one
        which packets carry.

        If noTrust(1) is specified, the final DSCP value will have the
        value of caqQosActionSelectDscp object. That is, if an instance
        of this object is noTrust(1), the caqQosActionSelectStatus
        object can not become 'active(1)' until a value has been
        assigned to the corresponding instance of
        caqQosActionSelectDscp."
    ::= { caqQosActionSelectEntry 2 }

caqQosActionSelectDscp    OBJECT-TYPE
    SYNTAX      Dscp
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object is only instantiated when the
        caqQosActionSelectTrust object in the same entry has been set
        to noTrust(1)."
    ::= { caqQosActionSelectEntry 4 }

caqQosActionSelectMicroflow OBJECT-TYPE
    SYNTAX      CaqPolicerNameOrEmpty 
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates a policer name. The value of this object either
        matches the value of caqFlowPolicerName object of an active
        entry in caqFlowPolicerTable or has an empty string value. The
        ACE uses this object to link to a policer flow entry.  If there
        is no microflow policer defined for the ACE pointed to this
        entry, this object should be an empty string. If the
        microflow(0) bit of caqFlowPolicingCpb object is turned off,
        this object should also be an empty string. Otherwise it should
        match the value of caqFlowPolicerName of an entry in the 
        caqFlowPolicerTable which has its RowStatus value to be
        active(1) and the type of the policer should be microflow(1)."
    ::= { caqQosActionSelectEntry 5 }

caqQosActionSelectAggregate OBJECT-TYPE
    SYNTAX      CaqPolicerNameOrEmpty 
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates a policer name. The value of this object either
        matches the value of caqFlowPolicerName object of an active
        entry in caqFlowPolicerTable or has an empty string value. 
        The ACE uses this object to link to a policer flow entry. 
        If there is no aggregate policer defined for the ACE pointed
        to this entry, this object should be an empty string. If the
        aggregate(1) bit of caqFlowPolicingCpb object is turned off, 
        this object should also be an an empty string. Otherwise
        it should match the value of caqFlowPolicerName of an entry in
        the caqFlowPolicerTable which has its RowStatus value to be
        active(1) and the type of the policer should be aggregate(2)."
    ::= { caqQosActionSelectEntry 6 }

caqQosActionSelectStatus  OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The status of this Qos Action Select conceptual row entry. This
        object is used to manage creation, deletion and modification of 
        rows in this table. 
       
        An entry may not exist in the active state unless all objects 
        in the entry have an appropriate value. Once a row becomes
        active, value in any other column within such row cannot be
        modified.

        If this row is pointed to by an active entry in the ACL tables, 
        this object cannot be changed from active(1) to any other
        value."
    ::= { caqQosActionSelectEntry 7 }

caqFlowPolicerExcessRateSupport      OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Indicates whether the device supports excess rate
         configuration."
    ::= { caqAclObjects 7 }


--
-- Flow Policing Table
--

caqFlowPolicerTable  OBJECT-TYPE
    SYNTAX        SEQUENCE OF CaqFlowPolicerEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "This table defines the flow policing rules. A flow policing
        rule comprises a rate, burst size and drop-or-mark indication."
    ::= { caqAclObjects 8 }

caqFlowPolicerEntry  OBJECT-TYPE
    SYNTAX        CaqFlowPolicerEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "The attributes defining a flow policing rule."
    INDEX { IMPLIED caqFlowPolicerName }
    ::= { caqFlowPolicerTable 1 }

CaqFlowPolicerEntry ::= SEQUENCE {
    caqFlowPolicerName                  CaqPolicerName,
    caqFlowPolicerType                  INTEGER,
    caqFlowPolicerNormalRateRequest     Integer32,
    caqFlowPolicerNormalRateGrant       Integer32,
    caqFlowPolicerNormalRateAction      INTEGER,
    caqFlowPolicerExcessRateRequest     Integer32,
    caqFlowPolicerExcessRateGrant       Integer32,
    caqFlowPolicerExcessRateAction      INTEGER,
    caqFlowPolicerBurstSizeRequest      Integer32,
    caqFlowPolicerBurstSizeGrant        Integer32,
    caqFlowPolicerStatus                RowStatus,
    caqFlowPolicerExcessBurstRequest    Unsigned32,
    caqFlowPolicerExcessBurstGrant      Unsigned32
}

caqFlowPolicerName      OBJECT-TYPE
    SYNTAX        CaqPolicerName
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "The name of a policer.  This name has to be unique to identify
        a microflow or an aggregate policer in the device."
    ::= { caqFlowPolicerEntry 1 }

caqFlowPolicerType  OBJECT-TYPE
    SYNTAX   INTEGER {
                 microflow(1),
                 aggregate(2)
             }
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "The type of this policer."
    ::= { caqFlowPolicerEntry 2 }

caqFlowPolicerNormalRateRequest  OBJECT-TYPE
    SYNTAX       Integer32 (0 | 32..8000000)
    UNITS        "kbps"
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "The requested average rate of the flow.  The base unit of this
        object is 1 kilo-bits per second.  0 may be specified for a
        rate which causes all packets to be out-of-profile.
        Out-of-profile indicates that a packet causes the committed
        access rate of the packet's flow to be exceeded.  Committed
        access rate is the bandwidth that has been committed to a
        specific flow or group of flows.  The committed rate can be
        enforced by policing or by shaping."
    ::= { caqFlowPolicerEntry 3 }

caqFlowPolicerNormalRateGrant  OBJECT-TYPE
    SYNTAX       Integer32 
    UNITS        "kbps"
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The granted average rate of the flow.  The base unit of this
        object is 1 kilo-bits per second. If the status of this row is
        not active, the value of this object will be the same as
        caqFlowPolicerNormalRateRequest's value.

        If the QoS function is enabled and the policy source is from
        local configuration, this MIB object is from the runtime
        hardware information.  Due to hardware granularity, the
        granted value may not be the same as the value specified
        by caqFlowPolicerNormalRateRequest object. It will be the
        closest value to the requested one that the hardware can
        support."
    ::= { caqFlowPolicerEntry 4 }

caqFlowPolicerNormalRateAction    OBJECT-TYPE
    SYNTAX    INTEGER { drop(1), policedDscp(2) }
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "The action for those normal rate out-of-profile packets. The
        action is to drop the packets or mark down its DSCP to the 
        value of caqDscpMappingNRPolicedDscp defined in 
        caqDscpMappingTable.

        If the caqFlowPolicerExcessRateSupport is true(1), this object
        cannot be set to drop(1). Setting the value of
        caqFlowPolicerExcessRateRequest object equal to the value of
        caqFlowPolicerNormalRateRequest object together with setting the
        value of caqFlowPolicerExcessRateAction object to drop(1) will
        effectively drop the packet at normal rate."
    ::= { caqFlowPolicerEntry 5 }

caqFlowPolicerExcessRateRequest  OBJECT-TYPE
    SYNTAX       Integer32 (0 | 32..8000000)
    UNITS        "kbps"
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "The requested excess rate of the flow.  The base unit of this
        object is 1 kilo-bits per second.  0 may be specified for a
        rate which causes all packets to be out-of-profile.
        Out-of-profile indicates that a packet causes the committed
        access rate of the packet's flow to be exceeded.  Committed
        access rate is the bandwidth that has been committed to a
        specific flow or group of flows.  The committed rate can be
        enforced by policing or by shaping.
        
        If the caqFlowPolicerExcessRateSupport is false(2), this object
        cannot be instantiated."
    ::= { caqFlowPolicerEntry 6 }

caqFlowPolicerExcessRateGrant  OBJECT-TYPE
    SYNTAX       Integer32 
    UNITS        "kbps"
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The granted excess rate of the flow.  The base unit of this
        object is 1 kilo-bits per second. If the status of this row is
        not active, the value of this object will be the same as
        caqFlowPolicerExcessRateRequest's value.

        If the QoS function is enabled and the policy source is from
        local configuration, this MIB object is from the runtime
        hardware information. Due to hardware granularity, the
        granted value may not be the same as the value specified
        by caqFlowPolicerExcessRateRequest object. It will be the
        closest value to the requested one that the hardware can
        support.

        If the caqFlowPolicerExcessRateSupport is false(2), this object
        cannot be instantiated."
    ::= { caqFlowPolicerEntry 7 }

caqFlowPolicerExcessRateAction    OBJECT-TYPE
    SYNTAX    INTEGER { drop(1), policedDscp(2) }
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "The action for those excess rate out-of-profile packets. The
        action is to drop the packets or mark down its DSCP value to 
        value of caqDscpMappingERPolicedDscp defined in 
        caqDscpMappingTable.

        If the caqFlowPolicerExcessRateSupport is false(2), this object
        cannot be instantiated."
    ::= { caqFlowPolicerEntry 8 }

caqFlowPolicerBurstSizeRequest  OBJECT-TYPE
    SYNTAX       Integer32 (1..32000)
    UNITS        "kilo-bits"
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "The requested burst rate of the flow. The base unit of this
        object is 1 kilo-bits."
    ::= { caqFlowPolicerEntry 9 }

caqFlowPolicerBurstSizeGrant  OBJECT-TYPE
    SYNTAX       Integer32 
    UNITS        "kilo-bits"
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The granted burst rate of the flow. The base unit of this
        object is 1 kilo-bits. If the status of this row is not
        active, the value of this object will be the same as
        caqFlowPolicerBurstSizeRequest's value.

        If the QoS function is enabled and the policy source is from
        local configuration, this MIB object is from the runtime
        hardware information. Due to hardware granularity, the
        granted value may not be the same as the value specified
        by caqFlowPolicerBurstSizeRequest object. It will be the
        closest value to the requested one that the hardware can
        support."
    ::= { caqFlowPolicerEntry 10 }

caqFlowPolicerStatus        OBJECT-TYPE
    SYNTAX        RowStatus
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "The status of this flow policer conceptual row entry. This 
        object is used to manage creation, deletion and modification of 
        rows in this table. 
       
        An entry may not exist in the active state unless all objects 
        in the entry have an appropriate value. Once a row becomes 
        active, value in any other column within such row cannot be 
        modified.

        If this row is pointed to by an active entry in the
        caqQosActionSelectTable, this object cannot be changed from 
        active(1) to any other value."
    ::= { caqFlowPolicerEntry 11 }

caqFlowPolicerExcessBurstRequest  OBJECT-TYPE
    SYNTAX       Unsigned32 (1..32000)
    UNITS        "kilo-bits"
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "The requested excess burst size of the flow.

        If the caqFlowPolicerExcessBurstSupport is false(2), this
        object cannot be instantiated."
    ::= { caqFlowPolicerEntry 12 }

caqFlowPolicerExcessBurstGrant  OBJECT-TYPE
    SYNTAX       Unsigned32 (1..32000)
    UNITS        "kilo-bits"
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The granted excess burst size of the flow. If the status of
        this row is not active, the value of this object will be the
        same as caqFlowPolicerExcessBurstRequest's value.

        If the QoS function is enabled and the policy source is from
        local configuration, this MIB object is from the runtime
        hardware information. Due to hardware granularity, the
        granted value may not be the same as the value specified
        by caqFlowPolicerExcessBurstRequest object. It will be the
        closest value to the requested one that the hardware can
        support.

        If the caqFlowPolicerExcessBurstSupport is false(2), this
        object cannot be instantiated."
    ::= { caqFlowPolicerEntry 13 }

--
-- caqSecurityActionTable
--

caqSecurityActionTable       OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqSecurityActionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table describes the actions of Security ACEs. Once an ACE
        is matched and it can go through an entry of this table to find
        the Security action."
    ::= { caqAclObjects 9 }

caqSecurityActionEntry       OBJECT-TYPE
    SYNTAX      CaqSecurityActionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry of a Security ACE action.  It provides the action for
        for the traffic matching Security ACEs."
    INDEX { caqSecurityActionIndex }
    ::= { caqSecurityActionTable 1 }

CaqSecurityActionEntry   ::= SEQUENCE {
    caqSecurityActionIndex       Unsigned32,
    caqSecurityAction            INTEGER,
    caqSecurityRedirectPortList  OCTET STRING,
    caqSecurityCapture           TruthValue,
    caqSecurityActionStatus      RowStatus,
    caqSecurityAdjIndex          Unsigned32,
    caqSecurityArpMacAddress     MacAddress,
    caqSecurityRedirect2kPortList  OCTET STRING,
    caqSecurityDownloadedAceFeature  INTEGER
}

caqSecurityActionIndex       OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The index of this table for indicating a Security ACE action
        entry."
    ::= { caqSecurityActionEntry 1 }

caqSecurityAction            OBJECT-TYPE
    SYNTAX    INTEGER {
                  permit(1),
                  deny(2),
                  redirect(3),
                  redirectWithAdj(4),
                  denyWithLog(5),
                  denyArpInspection(6),
                  denyArpInspWithLog(7),
                  permitArpInspection(8),
                  include(9)
              }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Determines the action that the device will take if the traffic
        matches the ACE.

        If permit(1) is specified, the matched traffic will be allowed
        through the device.

        If deny(2) is specified, the matched traffic will be blocked and
        dropped.

        If redirect(3) is specified, the matched traffic will be
        redirected to physical port(s) which should be configured
        in the caqSecurityRedirectPortList object. Redirect means
        taking packet coming in and putting it out of port(s)
        as is.

        If redirectWithAdj(4) is specified, the matched traffic will
        be redirected to the VLAN configured in the adjacency entry
        denoted by caqSecurityAdjIndex.

        If denyWithLog(5) is specified, the matched traffic will be
        blocked, dropped and logged. 

        If denyArpInspection(6) is specified, the matched ARP traffic
        will be blocked and dropped.

        If denyArpInspWithLog(7) is specified, the matched ARP traffic
        will be blocked, dropped and logged.

        If permitArpInspection(8) is specified, the matched ARP
        traffic will be allowed through the device.

        if include(9) is specified, the matched trafic will be
        regulated according to the downloaded ACE type denoted
        by caqSecurityDownloadedAceFeature object."
    ::= { caqSecurityActionEntry 2 }

caqSecurityRedirectPortList      OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(0..128))
    MAX-ACCESS  read-create
    STATUS      deprecated 
    DESCRIPTION
        "Indicates the set of physical port(s) that matched
        traffic is redirected to. Each octet within the value of
        this object specifies a set of eight ports, with the first
        octet specifying ports 1 through 8, the second octet
        specifying ports 9 through 16, etc. Within each octet, the
        most significant bit represents the lowest numbered port,
        and the least significant bit represents the highest numbered
        port. Thus, each port is represented by a single bit within
        the value of this object. If that bit has a value of '1' then
        that port is included in the set of redirect ports; the port
        is not included if its bit has a value of '0'. The value of
        this object is ignored whenever the value of caqSecurityAction
        object in the same row is not redirect(3)."
    ::= { caqSecurityActionEntry 3 }

caqSecurityCapture      OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates whether the matched traffic is to be captured.
        Capture means the packet is not only switched normally but also
        a copy of the switched packet is transmitted on the capture
        port(s). Traffic which is dropped cannot be captured; only
        traffic that is forwarded to its appropriate destination, can
        also be forwarded to a capture port. Redirected traffic 
        cannot be captured.

        Packets are only output on a capture port if they are on
        a VLAN which is carried on that port.  To capture traffic
        from many vlans, the capture port(s) should be a trunk
        carrying the required vlans.

        The capturing destination port(s) should be configured in
        caqSecurityAclCaptureIfTable."
    DEFVAL { false }
    ::= { caqSecurityActionEntry 4 }

caqSecurityActionStatus  OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The status of this Security ACE action conceptual row entry.
        This object is used to manage creation, deletion and 
        modification of rows in this table. 
       
        An entry may not exist in the active state unless all objects 
        in the entry have appropriate value. If the value of
        caqSecurityAction object in the same row is redirectWithAdj(4),
        user must use the value of the index object of an active entry
        in caqAdjacencyTable to configure the caqSecurityAdjIndex
        object. Once a row becomes active, value in any other column
        within such row cannot be modified.

        If this row is pointed to by an active entry in the ACL tables,
        this object cannot be changed from active(1) to any other
        value."
    ::= { caqSecurityActionEntry 5 }

caqSecurityAdjIndex  OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535) 
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the index of an active adjacency entry in 
        caqAdjacencyTable. The value of this object is ignored whenever
        the value of caqSecurityAction object in the same row is not
        redirectWithAdj(4)." 
    DEFVAL { 0 }
    ::= { caqSecurityActionEntry 6 }

caqSecurityArpMacAddress  OBJECT-TYPE
    SYNTAX      MacAddress 
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the 48 bits Mac address used in ARP packet.
        The value of this object is ignored whenever the value of
        caqSecurityAction object in the same row is not one of
        the following values denyArpInspection(6), denyArpInspWithLog(7)
        and permitArpInspection(8)." 
    DEFVAL { 'FFFFFFFFFFFF'H } 
    ::= { caqSecurityActionEntry 7 }

caqSecurityRedirect2kPortList      OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(0..256))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the set of physical port(s) that matched
        traffic is redirected to. Each octet within the value of
        this object specifies a set of eight ports, with the first
        octet specifying ports 1 through 8, the second octet
        specifying ports 9 through 16, etc. Within each octet, the
        most significant bit represents the lowest numbered port,
        and the least significant bit represents the highest numbered
        port. Thus, each port is represented by a single bit within
        the value of this object. If that bit has a value of '1' then
        that port is included in the set of redirect ports; the port
        is not included if its bit has a value of '0'. The value of
        this object is ignored whenever the value of caqSecurityAction
        object in the same row is not redirect(3). This object can
        accommodate up to 2048 ports.
     
        A port number is the value of dot1dBasePort for the port in
        the BRIDGE-MIB (RFC 1493)."
    ::= { caqSecurityActionEntry 8 }

caqSecurityDownloadedAceFeature  OBJECT-TYPE
    SYNTAX      INTEGER {
                    notApplicable(1), 
                    dot1x(2),
                    macAuth(3),
                    webAuth(4),
                    eou(5),
                    ipPhone(6)
                } 
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the feature type of the downloaded ACE.

        'notApplicable' indicates that this security action
        entry is not applied to any downloaded ACE.

        'dot1x' indicates that this security action entry is
        applied to downloaded ACE for 802.1x feature.

        'macAuth' indicates that this security action entry is
        applied to downloaded ACE for Mac Authentication
        Bypass feature.

        'webAuth' indicates that this security action entry is
        applied to downloaded ACE for Web-Proxy Authentication
        feature.

        'eou' indicates that this security action entry is
        applied to downloaded ACE for Extensible Authentication
        Protocol over UDP (EOU) feature.

        'ipPhone' indicates that this security action entry is
        applied to downloaded ACE for IP Phone feature. 

        The value of this object is 'notApplicable' whenever the
        value of caqSecurityAction object in the same row is not
        'include'. When an entry of this table is created with
        'include' value specified for caqSecurityAction, 'notApplicable'
        cannot be used for this object value."
    DEFVAL { notApplicable } 
    ::= { caqSecurityActionEntry 9 }
--
-- caqSecurityAclCaptureIfTable
--

caqSecurityAclCaptureIfTable  OBJECT-TYPE
    SYNTAX        SEQUENCE OF CaqSecurityAclCaptureIfEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "This table contains all the physical ports which are capable
        of being capture interfaces on which captured packets are
        output."
    ::= { caqAclObjects 10 }

caqSecurityAclCaptureIfEntry  OBJECT-TYPE
    SYNTAX        CaqSecurityAclCaptureIfEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "The index of this table is the ifIndex value of a
        physical port which is capable of being a capture interface
        on which captured packets are output." 
    INDEX { ifIndex }
    ::= { caqSecurityAclCaptureIfTable 1 }

CaqSecurityAclCaptureIfEntry ::= SEQUENCE {
    caqSecurityAclCaptureEnable   TruthValue
}

caqSecurityAclCaptureEnable  OBJECT-TYPE
    SYNTAX     TruthValue
    MAX-ACCESS read-write
    STATUS  current
    DESCRIPTION
        "An interface can be a destination of captured traffic which 
        matched any Security ACL. 

        This object is to specify whether to enable or disable this
        interface as a destination of captured traffic."
    DEFVAL { false }
    ::= { caqSecurityAclCaptureIfEntry 1 }

--
-- Excess Burst Capability Object
--

caqFlowPolicerExcessBurstSupport      OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Indicates whether the device supports excess burst 
         size configuration."
    ::= { caqAclObjects 11 }

--
--  Security Acl Feature Rate Limit objects
--
caqSecurityRateLimitFeatures   OBJECT-TYPE 
    SYNTAX       BITS {
                        arpInspection(0),
                        dot1xDHCP(1),
                        dhcpSnooping(2)
                      } 
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Indicates the features which implement rate limit
         on their traffic flows using the rate limit value
         denoted by caqSecurityAclRateLimit object. This 
         rate limit value is shared among all features denoted
         by this object."  
    ::= { caqAclObjects 12 }

caqSecurityAclRateLimit   OBJECT-TYPE
    SYNTAX       Unsigned32
    UNITS        "packet per second"
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
        "Indicates the maximum rate of all traffic flows
         subjected to rate limiting imposed by all features
         denoted by caqSecurityRateLimitFeatures object."  
    ::= { caqAclObjects 13 }

--
--  The caqQosDefaultAction table
--

caqQosDefaultActionTable  OBJECT-TYPE
    SYNTAX        SEQUENCE OF CaqQosDefaultActionEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "This table contains the QoS default action taken by the
        device for traffic which is not matched by a specific
        QoS ACE." 
    ::= { caqAclObjects 14 }

caqQosDefaultActionEntry  OBJECT-TYPE
    SYNTAX        CaqQosDefaultActionEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "The entries in this table are corresponding to the type of
        traffic as well as its direction and contain the default
        DSCP value, trust state and policers information. The number
        of entry in this table depends on what type of traffic
        supported by the device." 
    INDEX { caqQosTrafficDirection, caqQosTrafficType }
    ::= { caqQosDefaultActionTable 1 }

CaqQosDefaultActionEntry ::= SEQUENCE {
    caqQosTrafficDirection       CaqDirection,
    caqQosTrafficType            INTEGER,
    caqQosDefaultTrustState      INTEGER,
    caqQosDefaultDscp            Dscp,
    caqQosDefaultMicroflow       CaqPolicerNameOrEmpty,
    caqQosDefaultAggregate       CaqPolicerNameOrEmpty
}

caqQosTrafficDirection    OBJECT-TYPE
    SYNTAX     CaqDirection 
    MAX-ACCESS not-accessible 
    STATUS     current
    DESCRIPTION
        "Indicates whether this row's parameters are to
        be applied for ingress or for egress traffic."
    ::= { caqQosDefaultActionEntry 1 }

caqQosTrafficType    OBJECT-TYPE
    SYNTAX     INTEGER { 
                          mac(1),
                          ip(2),
                          ipx(3)
                       }
    MAX-ACCESS not-accessible 
    STATUS     current
    DESCRIPTION
        "Indicates whether this row's parameters are to
        be applied for Ethernet, IP or IPX traffic."
    ::= { caqQosDefaultActionEntry 2 }

caqQosDefaultTrustState       OBJECT-TYPE
    SYNTAX    INTEGER { 
                        noTrust(1), 
                        trustCos(2),
                        trustIpPrec(3),
                        trustDscp(4)
                      }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Indicates the default assigned trust state.     

        If trustCos(2) is specified, the default DSCP value of an
        unmatched packet should refer to caqCosToDscpDscp
        object in caqCosToDscpTable to transfer layer 2 CoS value to
        DSCP value.

        If trustIpPrec(3) is specified, the default DSCP value of an
        unmatched packet should refer to caqIpPrecToDscpDscp
        object in caqIpPrecToDscpTable to transfer IP Precedence value
        to DSCP value.

        If trustDscp(4) is specified, the default DSCP value of an
        unmatched packet is the one which packets carry.

        If noTrust(1) is specified, the default DSCP value of an
        unmatched packet will have the value of caqQosDefaultDscp
        object."
    ::= { caqQosDefaultActionEntry 3 }

caqQosDefaultDscp    OBJECT-TYPE
    SYNTAX      Dscp
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This object is only instantiated when the
        caqQosDefaultTrust object in the same entry has been set
        to noTrust(1)."
    ::= { caqQosDefaultActionEntry 4 }

caqQosDefaultMicroflow OBJECT-TYPE
    SYNTAX      CaqPolicerNameOrEmpty 
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Indicates a microflow policer name. The value of
        this object either matches the value of caqFlowPolicerName
        object of an active entry in caqFlowPolicerTable or has an
        empty string value.
        If there is no default microflow policer defined for unmatched
        traffic, this object should be an empty string. If the
        microflow(0) bit of caqFlowPolicingCpb object is turned off,
        this object should also be an empty string. Otherwise it should
        match the value of caqFlowPolicerName of an entry in the 
        caqFlowPolicerTable which has its RowStatus value to be
        active(1) and the type of the policer should be microflow(1)."
    ::= { caqQosDefaultActionEntry 5 }

caqQosDefaultAggregate OBJECT-TYPE
    SYNTAX      CaqPolicerNameOrEmpty 
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Indicates an aggregate policer name. The value of this object
        either matches the value of caqFlowPolicerName object of an
        active entry in caqFlowPolicerTable or has an empty string
        value. If there is no default aggregate policer defined for
        unmatched traffic, this object should be an empty string. If
        the aggregate(1) bit of caqFlowPolicingCpb object is turned
        off, this object should also be an an empty string. Otherwise
        it should match the value of caqFlowPolicerName of an entry in
        the caqFlowPolicerTable which has its RowStatus value to be
        active(1) and the type of the policer should be aggregate(2)."
    ::= { caqQosDefaultActionEntry 6 }

--
--  Acl Feature support 
--

caqAclFeatureCpb      OBJECT-TYPE
    SYNTAX        BITS { vlanAclHitCount(0), portAclHitCount (1) } 
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Indicates the set of features that the device supports
         related to ACLs configured in the device. 

         vlanAclHitCount(0) indicates that the device supports 
         ACL hit count feature for ACLs attached to VLAN interfaces.

         portAclHitCount(1) indicates that the device supports 
         ACL hit count feature for ACLs attached to physical 
         interfaces."
    ::= { caqAclObjects 15 }

--
--  The caqQosStatsObjects
--

caqL3PacketsDropByPolicer  OBJECT-TYPE
     SYNTAX     Counter64
     MAX-ACCESS read-only
     STATUS     current
     DESCRIPTION
         "Indicates the number of Layer 3 packets dropped due to
          policing."
     ::= { caqQosStatsObjects 1 }

caqTosChangedIpPackets  OBJECT-TYPE
     SYNTAX     Counter64
     MAX-ACCESS read-only
     STATUS     current
     DESCRIPTION
         "Indicates the number of IP packets have the Tos value
          changed."
     ::= { caqQosStatsObjects 2 }

caqCosChangedIpPackets  OBJECT-TYPE
     SYNTAX     Counter64
     MAX-ACCESS read-only
     STATUS     current
     DESCRIPTION
         "Indicates the number of IP packets have the Cos value
          changed."
     ::= { caqQosStatsObjects 3 }

caqCosChangedNonIpPackets  OBJECT-TYPE
     SYNTAX     Counter64
     MAX-ACCESS read-only
     STATUS     current
     DESCRIPTION
         "Indicates the number of non IP packets have the Cos 
          value changed."
     ::= { caqQosStatsObjects 4 }

--
--  The Port Statistics Table
--

caqPortStatsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqPortStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table containing QoS statistics counters per physical
        interface."
    ::= { caqQosStatsObjects 5 }

caqPortStatsEntry OBJECT-TYPE
    SYNTAX      CaqPortStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry contains QoS statistics maintained by the switching
        engine."
    INDEX  { ifIndex,
             caqPortStatsDirection,
             caqPortStatsQueueNumber,
             caqPortStatsThresholdNumber  }
    ::= { caqPortStatsTable 1 }

CaqPortStatsEntry ::= SEQUENCE {
    caqPortStatsDirection       CaqDirection,
    caqPortStatsQueueNumber     CaqQueueNumber, 
    caqPortStatsThresholdNumber CaqThresholdNumber, 
    caqPortStatsDropPkts        Counter64,
    caqPortStatsDropPktsAveRate     Gauge32,
    caqPortStatsDropPktsPeakRate  Gauge32
}

caqPortStatsDirection OBJECT-TYPE
    SYNTAX      CaqDirection
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Indicates traffic direction of an physical interface."
    ::= { caqPortStatsEntry 1 }

caqPortStatsQueueNumber  OBJECT-TYPE
    SYNTAX      CaqQueueNumber 
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Indicates the queue number of the interface for which
        statistics are collected. For example : if the port type of
        this interface is 1P2Q2T, this object can be 1, 2, 3." 
    ::= { caqPortStatsEntry 2 }

caqPortStatsThresholdNumber  OBJECT-TYPE
    SYNTAX       CaqThresholdNumber 
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "Indicates the threshold number of a queue on the interface for
        which statistics are collected. For example : if the port type
        of this interface is 1P2Q2T, this object can be 1, 2."
    ::= { caqPortStatsEntry 3 }

caqPortStatsDropPkts  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets have been received then dropped from the
        interface because they exceeded the threshold value configured
        at this queue and threshold of this interface."
    ::= { caqPortStatsEntry 4 }

caqPortStatsDropPktsAveRate OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS      "packets per second"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The five minute linearly-decayed moving average of packets
        have been received then dropped from the interface because
        they exceeded the threshold value configured at this queue
        and threshold of this interface."
    ::= { caqPortStatsEntry 5 }

caqPortStatsDropPktsPeakRate  OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS      "packets per second"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The peak rate of packets have been received then dropped from
        the interface because they exceeded the threshold value
        configured at this queue and threshold of this interface over
        the past five minutes."
    ::= { caqPortStatsEntry 6 }

--
--  The Flow specific Statistics Table
--

caqFlowStatsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqFlowStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table containing QoS statistics counter per flow."
    ::= { caqQosStatsObjects 6 }

caqFlowStatsEntry OBJECT-TYPE
    SYNTAX      CaqFlowStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry contains the number of out of profile packet
         per flow maintained by the switching engine." 
    AUGMENTS { cseFlowDataEntry }
    ::= { caqFlowStatsTable 1 }

CaqFlowStatsEntry ::= SEQUENCE {
    caqFlowStatsOutOfProfilePackets    Counter64
}

caqFlowStatsOutOfProfilePackets OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates the number of out-of-profile packets in
         this flow."
    ::= { caqFlowStatsEntry 1 }

--
--  The Aggregate Policer Statistics Table
--

caqAggPolicerStatsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqAggPolicerStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table containing QoS statistics counter per aggregate
         policer."
    ::= { caqQosStatsObjects 7 }

caqAggPolicerStatsEntry OBJECT-TYPE
    SYNTAX      CaqAggPolicerStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry contains the number of packet policed and the
         number of out of profile packets per aggregate policer." 
    INDEX { IMPLIED caqAggPolicerName }
    ::= { caqAggPolicerStatsTable 1 }

CaqAggPolicerStatsEntry ::= SEQUENCE {
    caqAggPolicerName                 CaqPolicerName,
    caqAggPolicerPackets              Counter64,
    caqAggPolicerNRExceedPackets      Counter64,
    caqAggPolicerERExceedPackets      Counter64,
    caqAggPolicerOctets               Counter64,
    caqAggPolicerNRExceedOctets       Counter64,
    caqAggPolicerERExceedOctets       Counter64,
    caqAggPolicerOctetsRate           CounterBasedGauge64, 
    caqAggPolicerNRExceedOctetsRate   CounterBasedGauge64,
    caqAggPolicerERExceedOctetsRate   CounterBasedGauge64,
    caqAggPolicerOctetsPeakRate       CounterBasedGauge64, 
    caqAggPolicerPacketsRate          CounterBasedGauge64,
    caqAggPolicerNRExceedPacketsRate  CounterBasedGauge64,
    caqAggPolicerERExceedPacketsRate  CounterBasedGauge64,
    caqAggPolicerPacketsPeakRate      CounterBasedGauge64
}

caqAggPolicerName      OBJECT-TYPE
    SYNTAX        CaqPolicerName
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "The name of a policer.  This name has to be unique to identify
        an aggregate policer in the device."
    ::= { caqAggPolicerStatsEntry 1 }

caqAggPolicerPackets OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates the number of packets is policed by this aggregate 
         policer. This object is only instantiated if such info is
         available in the device."
    ::= { caqAggPolicerStatsEntry 2 }

caqAggPolicerNRExceedPackets OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates the number of packets exceeded the normal rate of
         this aggregate policer. This object in only instantiated if
         such info is available in the device."
    ::= { caqAggPolicerStatsEntry 3 }

caqAggPolicerERExceedPackets OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates the number of packets exceeded the excess rate of
         this policer. This object is only instantiated if such info
         is available in the device and if excess rate is supported
         by the device as indicated by caqFlowPolicerExcessRateSupport
         object."
    ::= { caqAggPolicerStatsEntry 4 }

caqAggPolicerOctets OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates the number of octets is policed by this aggregate 
         policer. This object is only instantiated if such info is
         available in the device."
    ::= { caqAggPolicerStatsEntry 5 }

caqAggPolicerNRExceedOctets OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates the number of octets exceeded the normal rate of
         this aggregate policer. This object is only instantiated if
         such info is available in the device."
    ::= { caqAggPolicerStatsEntry 6 }

caqAggPolicerERExceedOctets OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates the number of octets exceeded the excess rate of
         this policer. This object is only instantiated if such info
         is available in the device and if excess rate is supported
         by the device as indicated by caqFlowPolicerExcessRateSupport
         object."
    ::= { caqAggPolicerStatsEntry 7 }

caqAggPolicerOctetsRate OBJECT-TYPE
    SYNTAX      CounterBasedGauge64
    UNITS       "kbps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates five minute linearly-decayed moving average of
         octets policed by this aggregate policer.
         This object is only instantiated if such info is available in
         the device."
    ::= { caqAggPolicerStatsEntry 8 }

caqAggPolicerNRExceedOctetsRate OBJECT-TYPE
    SYNTAX      CounterBasedGauge64
    UNITS       "kbps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates five minute linearly-decayed moving average of
         octets exceeded the normal rate of this aggregate policer.
         This object is only instantiated if such info is available in
         the device."
    ::= { caqAggPolicerStatsEntry 9 }

caqAggPolicerERExceedOctetsRate OBJECT-TYPE
    SYNTAX      CounterBasedGauge64
    UNITS       "kbps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates five minute linearly-decayed moving average of
         octets exceeded the excess rate of this policer. This object
         is only instantiated if such info is available in the device
         and if excess rate is supported by the device as indicated by
         caqFlowPolicerExcessRateSupport object."
    ::= { caqAggPolicerStatsEntry 10 }

caqAggPolicerOctetsPeakRate OBJECT-TYPE
    SYNTAX      CounterBasedGauge64
    UNITS      "kbps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates peak rate of octets is policed by this aggregate 
         policer over the past five minute. This object is only
         instantiated if such info is available in the device."
    ::= { caqAggPolicerStatsEntry 11 }

caqAggPolicerPacketsRate OBJECT-TYPE
    SYNTAX      CounterBasedGauge64
    UNITS       "packets per second"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates five minute linearly-decayed moving average of
         packets policed by this aggregate policer.
         This object is only instantiated if such info is available in
         the device."
    ::= { caqAggPolicerStatsEntry 12 }

caqAggPolicerNRExceedPacketsRate OBJECT-TYPE
    SYNTAX      CounterBasedGauge64
    UNITS       "packets per second"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates five minute linearly-decayed moving average of
         packets exceeded the normal rate of this aggregate policer.
         This object is only instantiated if such info is available in
         the device."
    ::= { caqAggPolicerStatsEntry 13 }

caqAggPolicerERExceedPacketsRate OBJECT-TYPE
    SYNTAX      CounterBasedGauge64
    UNITS       "packets per second" 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates five minute linearly-decayed moving average of
         packets exceeded the excess rate of this policer. This object
         is only instantiated if such info is available in the device
         and if excess rate is supported by the device as indicated by
         caqFlowPolicerExcessRateSupport object."
    ::= { caqAggPolicerStatsEntry 14 }

caqAggPolicerPacketsPeakRate OBJECT-TYPE
    SYNTAX      CounterBasedGauge64
     UNITS      "packets per second"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates peak rate of packets is policed by this aggregate 
         policer over the past five minutes. This object is only
         instantiated if such info is available in the device."
    ::= { caqAggPolicerStatsEntry 15 }

caqL3PacketsDropByPolicerAveRate  OBJECT-TYPE
     SYNTAX     CounterBasedGauge64
     UNITS      "packets per second"
     MAX-ACCESS read-only
     STATUS     current
     DESCRIPTION
         "Indicates five minute linearly-decayed moving average of 
          Layer 3 packets dropped due to policing."
     ::= { caqQosStatsObjects 8 }

caqL3PacketsDropByPolicerPeakRate  OBJECT-TYPE
     SYNTAX     CounterBasedGauge64
     UNITS      "packets per second"
     MAX-ACCESS read-only
     STATUS     current
     DESCRIPTION
         "Indicates the peak rate of Layer 3 packets dropped due to
          policing over the past five minutes."
     ::= { caqQosStatsObjects 9 }

caqTosChangedIpPacketsAveRate  OBJECT-TYPE
     SYNTAX     CounterBasedGauge64
     UNITS      "packets per second"
     MAX-ACCESS read-only
     STATUS     current
     DESCRIPTION
         "Indicates five minute linearly-decayed moving average of
          IP packets have the Tos value change."
     ::= { caqQosStatsObjects 10 }

caqTosChangedIpPacketsPeakRate  OBJECT-TYPE
     SYNTAX     CounterBasedGauge64
     UNITS      "packets per second"
     MAX-ACCESS read-only
     STATUS     current
     DESCRIPTION
         "Indicates the peak rate of IP packets have the Tos value
          change over the past five minute."
     ::= { caqQosStatsObjects 11 }

caqCosChangedIpPacketsAveRate  OBJECT-TYPE
     SYNTAX     CounterBasedGauge64
     UNITS      "packets per second"
     MAX-ACCESS read-only
     STATUS     current
     DESCRIPTION
         "Indicates five minute linearly-decayed moving average of
          IP packets have the Cos value change."
     ::= { caqQosStatsObjects 12 }

caqCosChangedIpPacketsPeakRate  OBJECT-TYPE
     SYNTAX     CounterBasedGauge64
     UNITS      "packets per second"
     MAX-ACCESS read-only
     STATUS     current
     DESCRIPTION
         "Indicates the peak rate of IP packets have the Cos value
          change over the past five minutes."
     ::= { caqQosStatsObjects 13 }

caqCosChangedNonIpPacketsAveRate  OBJECT-TYPE
     SYNTAX     CounterBasedGauge64
     UNITS      "packets per second"
     MAX-ACCESS read-only
     STATUS     current
     DESCRIPTION
         "Indicates five minute linearly-decayed moving average of
          non IP packets have the Cos value change."
     ::= { caqQosStatsObjects 14 }

caqCosChangedNonIpPacketPeakRate  OBJECT-TYPE
     SYNTAX     CounterBasedGauge64
     UNITS      "packets per second"
     MAX-ACCESS read-only
     STATUS     current
     DESCRIPTION
         "Indicates the peak rate of non IP packets have the Cos 
          value change over the past five minutes."
     ::= { caqQosStatsObjects 15 }


--*********************************************************************
-- Cisco CatOS Acl Qos Extension Group
--*********************************************************************


--
-- caqBridgedPolicerTable
--



caqBridgedPolicerTable        OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqBridgedPolicerEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table provides configuration information for each
        (existing) VLAN on whether or not bridged packets are policed
        at the microflow level on that VLAN. This configuration is
        useful in situations in which there are insufficient resources
        to police bridged packets at the microflow level on all VLANs.
        This configuration has no effect on aggregate policing." 
    ::= { caqExtObjects 1 }

caqBridgedPolicerEntry    OBJECT-TYPE
    SYNTAX      CaqBridgedPolicerEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A conceptual row in the caqBridgedPolicerTable 
        to control if bridged packets are policed at microflow
        level on a particular VLAN." 
    INDEX   { caqBridgedFlowVlanIndex }
    ::= { caqBridgedPolicerTable 1 }

CaqBridgedPolicerEntry ::= SEQUENCE {
    caqBridgedFlowVlanIndex  VlanIndex,
    caqBridgedFlowEnabled    TruthValue
}

caqBridgedFlowVlanIndex    OBJECT-TYPE
    SYNTAX      VlanIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The VLAN-id of this VLAN."
    ::= { caqBridgedPolicerEntry 1 }

caqBridgedFlowEnabled    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Enable or Disable this function. If this objects is set to
         true, the bridged packets will be policed at microflow level.
         If it is set to false, bridged packets won't be policed at
         microflow level. This value has no effect on aggregate
         policing. The default is false."
    DEFVAL { false }
    ::= { caqBridgedPolicerEntry 2 }


--
-- caqCosMacVlanRouterTable
--

caqCosMacVlanRouterTable  OBJECT-TYPE
    SYNTAX       SEQUENCE OF CaqCosMacVlanRouterEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "This table is used either to assign a Cos value to frames
       on a specific VLAN and which have a specific destination MAC
       address and/or to indicate if the configured destination MAC
       address is of a router. This table is applied only for platform
       that supports these features." 
    ::= { caqExtObjects 2 }

caqCosMacVlanRouterEntry   OBJECT-TYPE
    SYNTAX       CaqCosMacVlanRouterEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "The Cos value to be assigned to frames on a specific VLAN and
        which have a specific destination MAC address and/or the
        configured destination MAC address is of a router."
    INDEX { caqCosMacAddress, caqCosVlanNumber }
    ::= { caqCosMacVlanRouterTable 1 }

CaqCosMacVlanRouterEntry  ::= SEQUENCE {
    caqCosMacAddress      MacAddress,
    caqCosVlanNumber      VlanIndex,
    caqMacAddressCpb      BITS,
    caqCosValue           QosLayer2Cos,
    caqCosMacVlanRouterStatus   RowStatus
}

caqCosMacAddress     OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Indicates the destination MAC address to match against the
        flow."
    ::= { caqCosMacVlanRouterEntry 1 }

caqCosVlanNumber     OBJECT-TYPE
    SYNTAX      VlanIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Indicates the VLAN number."
    ::= { caqCosMacVlanRouterEntry 2 }

caqMacAddressCpb     OBJECT-TYPE
    SYNTAX      BITS { 
                       routerMac(0),
                       cosVlanMac(1)
                     }
    MAX-ACCESS  read-create 
    STATUS      current
    DESCRIPTION
        "Indicates the capability of the destination MAC address denoted
        by caqCosMacAddress object in the same row. 

        routerMac(0) means that it is a router Mac address.

        cosVlanMac(1) means that a Cos value is assigned to frames
        on a specific VLAN and which has this MAC address as its
        destination."
    ::= { caqCosMacVlanRouterEntry 3 }

caqCosValue     OBJECT-TYPE
    SYNTAX      QosLayer2Cos
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the Cos value. This object is only instantiated
        if the cosVlanMac bit in caqMacAddressCpb object is turned
        on."
    ::= { caqCosMacVlanRouterEntry 4 }

caqCosMacVlanRouterStatus     OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The status of this conceptual row entry. This object is 
        used to manage creation, deletion and modification of rows in 
        this table. 
       
        An entry may not exist in the active state unless all objects 
        in the entry have an appropriate value. Once a row becomes
        active, value in any other column within such row cannot be
        modified except by setting caqCosMacVlanRouterStatus to
        notInService(2) for such row."
    ::= { caqCosMacVlanRouterEntry 5 }


--*********************************************************************
-- Cisco CatOS Acl Qos PBF Group
--*********************************************************************

caqPbfStatus     OBJECT-TYPE
    SYNTAX       INTEGER {
                   macAddrOk(1),
                   macAddrNotSet(2),
                   msfcPresent(3)
                 }
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Indicates the status of policy-based forwarding (PBF) engine.
         
        macAddrOk(1) indicates that the MAC address of the PBF engine
        is set successfully and PBF engine is operational.

        macAddrNotSet(2) indicates that the MAC address of the PBF
        engine is not set and PBF engine is not operational.

        msfcPresent(3) indicates that there is a Multiplayer Switch
        Feature Card (MSFC) present in the device thus the PBF engine
        is not operational."
    ::= { caqPbfObjects 1 }

caqPbfMacAddress     OBJECT-TYPE
    SYNTAX       MacAddress 
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
        "Indicates the PBF engine MAC address. When the value of
        caqPbfStatus is msfcPresent(3), this object cannot be configured
        and its previously configured value is ignored." 
    ::= { caqPbfObjects 2 }

--
-- The Adjacency Table.
-- 

caqAdjacencyTable  OBJECT-TYPE
    SYNTAX       SEQUENCE OF CaqAdjacencyEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "This table contains a list of adjacencies to use in
        policy-based forwarding (PBF). PBF is a feature that
        makes possible forwarding between two different VLANs
        without having a router."  
    ::= { caqPbfObjects 3 }

caqAdjacencyEntry   OBJECT-TYPE
    SYNTAX       CaqAdjacencyEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "An entry defines an adjacency. Each adjacency consists
        of a destination VLAN, source and destination MAC address as
        well as adjacency name and MTU configuration."
    INDEX { caqAdjIndex }
    ::= { caqAdjacencyTable 1 }

CaqAdjacencyEntry  ::= SEQUENCE {
    caqAdjIndex          Unsigned32,
    caqAdjDstVlanNumber  VlanIndex,
    caqAdjDstMacAddress  MacAddress,
    caqAdjSrcMacAddress  MacAddress, 
    caqAdjName           CaqAdjacencyName, 
    caqAdjMtu            Unsigned32,
    caqAdjHitCount       Counter64,
    caqAdjStatus         RowStatus
}

caqAdjIndex     OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Indicates the index of this adjacency." 
    ::= { caqAdjacencyEntry 1 }

caqAdjDstVlanNumber  OBJECT-TYPE
    SYNTAX        VlanIndex 
    MAX-ACCESS    read-create 
    STATUS        current
    DESCRIPTION
        "Indicates the destination VLAN number of this adjacency." 
    ::= { caqAdjacencyEntry 2 }

caqAdjDstMacAddress     OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create 
    STATUS      current
    DESCRIPTION
        "Indicates the adjacency destination MAC address."
    ::= { caqAdjacencyEntry 3 }

caqAdjSrcMacAddress     OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-create 
    STATUS      current
    DESCRIPTION
        "Indicates the adjacency source MAC address. If this object
        is not configured, it will contain the MAC address of the
        PBF engine which is denoted by caqPbfMacAddress object."
    ::= { caqAdjacencyEntry 4 }

caqAdjName      OBJECT-TYPE
    SYNTAX      CaqAdjacencyName 
    MAX-ACCESS  read-create 
    STATUS      current
    DESCRIPTION
        "Indicates the adjacency name. The adjacency name should be
        unique among all entries in this table."
    ::= { caqAdjacencyEntry 5 }

caqAdjMtu       OBJECT-TYPE
    SYNTAX      Unsigned32 (576..18190)
    UNITS       "bytes"
    MAX-ACCESS  read-create 
    STATUS      current
    DESCRIPTION
        "Indicates the adjacency MTU."
    DEFVAL { 9216 }
    ::= { caqAdjacencyEntry 6 }

caqAdjHitCount     OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
        "Indicates the number of packets that have matched this
        adjacency's criteria. The value of this object is cleared when
        this row is derefenced by entries in caqSecurityActionTable."
    ::= { caqAdjacencyEntry 7 }

caqAdjStatus    OBJECT-TYPE
    SYNTAX      RowStatus 
    MAX-ACCESS  read-create 
    STATUS      current
    DESCRIPTION
        "Indicates the status of this adjacency conceptual entry.
        This object is used to manage creation, deletion and
        modification of rows in this table.

        An entry may not exist in the active state unless all objects
        in the entry have an appropriate value. Once a row becomes
        active, value in any other column within such row cannot be
        modified.

        This object cannot be changed from active(1) to any other value
        if the following two conditions are met:
        - There is an active entry in caqSecurityActionTable with
          caqSecurityAdjIndex equal to caqAdjIndex.
        - That entry has caqSecurityAction set to redirectWithAdj(4)." 
    ::= { caqAdjacencyEntry 8 }

--*********************************************************************
-- Cisco CatOS Acl Security Logging Group
--*********************************************************************

caqAclLogMaxFlow     OBJECT-TYPE
    SYNTAX       Unsigned32 (256..2048)
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
        "Indicates the maximum number of traffic flow will be logged
        by the device." 
    ::= { caqLoggingObjects 1 }

caqAclSecurityLoggingRateLimit   OBJECT-TYPE
    SYNTAX       Unsigned32 (500..5000)
    UNITS        "packet per second"
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
        "Indicates the redirect rate of traffic flow subjected 
         to security ACL logging."  
    ::= { caqLoggingObjects 2 }

caqAclRouterAclRateLimit   OBJECT-TYPE
    SYNTAX       Unsigned32 (1..1000)
    UNITS        "packet per second"
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
        "Indicates the redirect rate of traffic flow subjected 
         to router ACL logging."  
    ::= { caqLoggingObjects 3 }

--
-- caqIpFlowLoggingTable
--

caqIpFlowLoggingTable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqIpFlowLoggingEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains a list of IP flows that describes the 
        IP traffic denied and logged by the device." 
    ::= { caqLoggingObjects 4 }

caqIpFlowLoggingEntry    OBJECT-TYPE
    SYNTAX      CaqIpFlowLoggingEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry describes an IP flow, consisting of a set of data 
        such as source and destination address, source and destination
        port as well as protocol specific information. To keep the
        table from overflow, each entry contains a TTL (Time to Live)
        object. An entry will be removed from this table when its TTL
        value reaches zero."
    INDEX { caqIpFlowLoggingIndex }
    ::= { caqIpFlowLoggingTable 1 }

CaqIpFlowLoggingEntry ::= SEQUENCE {
    caqIpFlowLoggingIndex          Unsigned32,
    caqIpFlowVlan                  VlanIndex,
    caqIpFlowIfIndex               InterfaceIndex, 
    caqIpFlowProtocolType          Unsigned32,
    caqIpFlowAddrType              InetAddressType,
    caqIpFlowSrcIp                 InetAddress,
    caqIpFlowSrcPort               Integer32,
    caqIpFlowDestIp                InetAddress,
    caqIpFlowDestPort              Integer32,
    caqIpFlowIcmpType              Integer32,
    caqIpFlowIcmpCode              Integer32,
    caqIpFlowIgmpType              Integer32,
    caqIpFlowArpOpcode             INTEGER,
    caqIpFlowArpSrcMacAddr         MacAddress,
    caqIpFlowArpHeaderSrcMacAddr   MacAddress, 
    caqIpFlowPacketsCount          Counter32,
    caqIpFlowLoggingTTL            Unsigned32,
    caqIpFlowArpLoggingSource      INTEGER,
    caqIpFlowArpAclName            SnmpAdminString, 
    caqIpFlowArpAceNumber          Unsigned32
}

caqIpFlowLoggingIndex       OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The index of this table for indicating a logged IP flow." 
    ::= { caqIpFlowLoggingEntry 1 }

caqIpFlowVlan      OBJECT-TYPE
    SYNTAX      VlanIndex 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the VLAN number which this logged IP flow belongs." 
    ::= { caqIpFlowLoggingEntry 2 }

caqIpFlowIfIndex      OBJECT-TYPE
    SYNTAX      InterfaceIndex 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the ifIndex of the interface where this logged
        IP flow arrived."
    ::= { caqIpFlowLoggingEntry 3 }

caqIpFlowProtocolType        OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The protocol number field in the IP header of this logged
         IP flow as specified in RFC 1700."
    REFERENCE
        "RFC 1700, Assigned Numbers."
    ::= { caqIpFlowLoggingEntry 4 }

caqIpFlowAddrType        OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the address type for addresses specified in
        caqIpFlowSrcIp and caqIpFlowDestIp of this logged IP
        flow."
    ::= { caqIpFlowLoggingEntry 5 } 

caqIpFlowSrcIp           OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the source address of this logged IP flow."
    ::= { caqIpFlowLoggingEntry 6 }

caqIpFlowSrcPort     OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the source port number of this logged IP flow
        when its protocol field is TCP or UDP. The value of this
        object is -1 if the flow is not UDP or TCP traffic." 
    ::= { caqIpFlowLoggingEntry 7 }

caqIpFlowDestIp          OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the destination address of this logged IP flow."
    ::= { caqIpFlowLoggingEntry 8 }

caqIpFlowDestPort        OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the destination port number of this logged IP flow
        when its protocol field is TCP or UDP. The value of this
        object is -1 if the flow is not UDP or TCP traffic." 
    ::= { caqIpFlowLoggingEntry 9 }

caqIpFlowIcmpType        OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the message type of ICMP packets. The value of this
        object is -1 if the flow is not ICMP traffic." 
    ::= { caqIpFlowLoggingEntry 10 }

caqIpFlowIcmpCode        OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the message code of ICMP packets. The value of this
        object is -1 if the flow is not ICMP traffic." 
    ::= { caqIpFlowLoggingEntry 11 }

caqIpFlowIgmpType        OBJECT-TYPE
    SYNTAX      Integer32 (-1 | 0..15)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the message type of IGMP packets. The value of this
        object is -1 if the flow is not IGMP traffic." 
    ::= { caqIpFlowLoggingEntry 12 }

caqIpFlowArpOpcode  OBJECT-TYPE
    SYNTAX      INTEGER { 
                          notApplicable(1), 
                          request(2), 
                          reply(3) 
                        }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the ARP opcode value of this ARP flow.
         
         If the value of this object is notApplicable(1), this flow
         is not ARP traffic.

         If the value of this object is request(2), this flow
         is ARP request traffic.
         
         If the value of this object is reply(3), this flow
         is ARP reply traffic."
         
    ::= { caqIpFlowLoggingEntry 13 }

caqIpFlowArpSrcMacAddr  OBJECT-TYPE
    SYNTAX      MacAddress 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the Ethernet Source Address value of this ARP
        flow.  This object is ignored if the flow is not ARP
        traffic."  
    ::= { caqIpFlowLoggingEntry 14 }

caqIpFlowArpHeaderSrcMacAddr  OBJECT-TYPE
    SYNTAX      MacAddress 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the Ethernet Source Address value included in the
        ARP header of this ARP flow. This object is ignored if the
        flow is not ARP traffic."  
    ::= { caqIpFlowLoggingEntry 15 }

caqIpFlowPacketsCount      OBJECT-TYPE
    SYNTAX      Counter32 
    UNITS       "packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of packets that belong to this IP flow." 
    ::= { caqIpFlowLoggingEntry 16 }

caqIpFlowLoggingTTL  OBJECT-TYPE
    SYNTAX      Unsigned32 
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the TTL (Time to Live) of this entry. The entry 
        is removed when its value of this object reaches 0."  
    ::= { caqIpFlowLoggingEntry 17 }

caqIpFlowArpLoggingSource  OBJECT-TYPE
    SYNTAX      INTEGER { 
                          notApplicable(1), 
                          dai(2), 
                          acl(3) 
                }  
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the source that triggered the logging of this 
        ARP flow. This object value is 'notApplicable' if the
        flow is not ARP traffic.

        'dai' indicates the logging source is Dynamic Arp Inspection
        feature.

        'acl' indicates the logging source is a configured security
        access control list (ACL)." 
    ::= { caqIpFlowLoggingEntry 18 }

caqIpFlowArpAclName  OBJECT-TYPE
    SYNTAX      SnmpAdminString 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the security ACL name which triggered the 
        logging of this ARP flow. This object is ignored if
        the value of caqIpFlowArpLoggingSource object in the
        same row is not 'acl'." 
    ::= { caqIpFlowLoggingEntry 19 }

caqIpFlowArpAceNumber  OBJECT-TYPE
    SYNTAX      Unsigned32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the ACE number within the ACL denoted by 
        caqIpFlowArpAclName object which triggered the logging 
        of this ARP flow. This object is ignored if the value of
        caqIpFlowArpLoggingSource object in the same row is not 'acl'."
    ::= { caqIpFlowLoggingEntry 20 }

--*********************************************************************
--*********************************************************************
-- Cisco CatOS Acl ARP Inspection Group
--*********************************************************************
caqAclArpInspMatchMac   OBJECT-TYPE
    SYNTAX       INTEGER {
                     disable(1),
                     enable(2),
                     drop(3),
                     dropAndLog(4)
                 } 
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
        "Indicates whether for ARP packets MAC address matching of
        ethernet header and the source MAC address specified in ARP
        header is enabled. It also indicates the action taken when
        the addresses do not match. 
        
        If this object value is disable(1), the device will not check
        for matching of source MAC address in ethernet header with the
        sender MAC address in ARP header for ARP packets. 

        If this object value is enable(2), the device will check
        for matching of source MAC address in ethernet header with the
        sender MAC address in ARP header for ARP packets. A syslog
        message is generated if the MAC addresses check fails. 

        If this object value is drop(3), the device will check for
        MAC addresses matching and ARP packets whose MAC addresses
        do not match will be dropped. 

        If this object value is dropAndLog(4), the device will check
        for MAC addresses matching and ARP packets whose MAC addresses
        do not match will be dropped and logged into
        caqIpFlowLoggingTable." 
    ::= { caqArpInspObjects 2 }

caqAclArpInspAddrValidation   OBJECT-TYPE
    SYNTAX       INTEGER {
                     disable(1),
                     enable(2),
                     drop(3),
                     dropAndLog(4)
                 } 
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
        "Indicates whether for ARP packets checking for valid source MAC
        and source IP address specified in ARP header is enabled. It
        also indicates the action taken when the addresses are not
        valid. 
        
        If this object value is disable(1), the device will not check
        for valid MAC and IP address for ARP packets. 

        If this object value is enable(2), the device will check
        for valid MAC and IP address for ARP packets. A syslog
        message is generated if the addresses check fails. 

        If this object value is drop(3), the device will check for
        valid MAC and IP addresses. ARP packets whose have illegal MAC
        and IP addresses will be dropped. 

        If this object value is dropAndLog(4), the device will check
        for valid MAC and IP addresses. ARP packets whose have invalid
        MAC and IP addresses will be dropped and logged into
        caqIpFlowLoggingTable." 
    ::= { caqArpInspObjects 3 }

caqArpInspGlobalForwardedPkts  OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates the total number of packets subjected to
        ARP Inspection is forwarded."
    ::= { caqArpInspObjects 4 }

caqArpInspGlobalDroppedPkts  OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates the total number of packets subjected to
        ARP Inspection is dropped."
    ::= { caqArpInspObjects 5 }

caqRARPForwardedPkts  OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates the total number of packets subjected to
        Reverse ARP (RARP) Inspection is forwarded."
    ::= { caqArpInspObjects 6 }

caqMatchedMacFailedPkts  OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates the total number of packets subjected to
        ARP Inspection whose MAC address specified in the ethernet
        header and the source MAC address specified in ARP
        header does not match."
    ::= { caqArpInspObjects 7 }

caqAddrValidationFailedPkts  OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates the total number of ARP packets that have 
        invalid source MAC address or invalid source IP address
        specified in the ARP header." 
    ::= { caqArpInspObjects 8 }

caqArpInspIpDroppedPkts  OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates the total number of IP packets dropped by 
         ARP Inspection because of invalid IP address."
    ::= { caqArpInspObjects 9 }

--
--
--  The Arp Inspection Statistics Table
--

caqArpInspStatsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqArpInspStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table containing ARP Inspection statistics counter per ACL."
    ::= { caqArpInspObjects 10 }

caqArpInspStatsEntry OBJECT-TYPE
    SYNTAX      CaqArpInspStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry contains the numbers of packet permitted or denied 
         per ACL." 
    INDEX { IMPLIED caqArpInspAclName }
    ::= { caqArpInspStatsTable 1 }

CaqArpInspStatsEntry ::= SEQUENCE {
    caqArpInspAclName             CaqAclName,
    caqArpInspForwardedPackets    Counter64,
    caqArpInspDroppedPackets      Counter64
}

caqArpInspAclName      OBJECT-TYPE
    SYNTAX        CaqAclName
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "The name of an ACL that contains ACE used for ARP Inspection."
    ::= { caqArpInspStatsEntry 1 }

caqArpInspForwardedPackets OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates the number of packets subjected to ARP Inspection
         is forwarded by this ACL." 
    ::= { caqArpInspStatsEntry 2 }

caqArpInspDroppedPackets OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Indicates the number of packets subjected to ARP Inspection
         is dropped by this ACL." 
    ::= { caqArpInspStatsEntry 3 }

--
-- caqIfArpInspConfigTable
--

caqIfArpInspConfigTable  OBJECT-TYPE
    SYNTAX        SEQUENCE OF CaqIfArpInspConfigEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "This table contains the configuration of several threshold
        values related to ARP Inspection at each physical interface."   
    ::= { caqArpInspObjects 11 }

caqIfArpInspConfigEntry  OBJECT-TYPE
    SYNTAX        CaqIfArpInspConfigEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "Each entry contains the configuration for drop threshold
        and shutdown threshold for ARP Inspection at each physical 
        interface that supports this feature. Some of the
        interfaces (but not limited to) for which this feature
        might be applicable are: ifType = ethernetCsmacd(6)."
    INDEX { ifIndex }
    ::= { caqIfArpInspConfigTable 1 }

CaqIfArpInspConfigEntry  ::= SEQUENCE {
    caqIfArpInspDropThreshold     Unsigned32,
    caqIfArpInspShutdownThreshold Unsigned32 
}

caqIfArpInspDropThreshold  OBJECT-TYPE
    SYNTAX        Unsigned32 (0..5000)
    UNITS         "packet per second"
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "Indicates the drop threshold value where excess packets of
        a traffic flow subjected to ARP Inspection will be dropped
        if its rate is greater than this threshold value. If the value
        of this object is 0, no rate limit is applied for dropping
        ARP traffic at this interface."
    ::= { caqIfArpInspConfigEntry 1 }

caqIfArpInspShutdownThreshold  OBJECT-TYPE
    SYNTAX        Unsigned32 (0..5000)
    UNITS         "packet per second"
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "Indicates the threshold value where the interface will be
        shutdown if traffic rate subjected to ARP Inspection is greater
        than this threshold value. If the value of this object is 0,
        no ARP traffic rate limit is applied for shutting down the
        interface."
    ::= { caqIfArpInspConfigEntry 2 }

--
--  caqAclHitCountObjects group
--

caqAclHitCountVlansLow  OBJECT-TYPE
    SYNTAX        OCTET STRING (SIZE(0..256))
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "A string of octets containing one bit per VLAN for
         VLANs with VlanIndex value of 0 to 2047. The first
         octet corresponds to VLANs with VlanIndex values
         of 0 through 7; the second octet to VLANs 8 through
         15; etc.  The most significant bit of each octet
         corresponds to the lowest value VlanIndex in that octet.

         For each VLAN, if ACL hit count feature is enabled then
         the bit corresponding to that VLAN is set to '1'.

         Note that if the length of this string is less than
         256 octets, any 'missing' octets are assumed to contain
         the value zero. A NMS may omit any zero-valued octets
         from the end of this string in order to reduce SetPDU size,
         and the agent may also omit zero-valued trailing octets,
         to reduce the size of GetResponse PDUs.

         This object is only instantiated when the vlanAclHitCount(0)
         bit is set to '1' in the caqAclFeatureCpb object."
    ::= { caqAclHitCountObjects 1 }

caqAclHitCountVlansHigh  OBJECT-TYPE
    SYNTAX        OCTET STRING (SIZE(0..256))
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "A string of octets containing one bit per VLAN for
         VLANs with VlanIndex value of 2048 to 4095. The first
         octet corresponds to VLANs with VlanIndex values
         of 2048 through 2055; the second octet to VLANs 2056
         through 2063; etc.  The most significant bit of each
         octet corresponds to the lowest value VlanIndex in that
         octet.

         For each VLAN, if ACL hit count feature is enabled then
         the bit corresponding to that VLAN is set to '1'.

         Note that if the length of this string is less than
         256 octets, any 'missing' octets are assumed to contain
         the value zero. A NMS may omit any zero-valued octets
         from the end of this string in order to reduce SetPDU size,
         and the agent may also omit zero-valued trailing octets,
         to reduce the size of GetResponse PDUs.

         This object is only instantiated when the vlanAclHitCount(0)
         bit is set to '1' in the caqAclFeatureCpb object."
    ::= { caqAclHitCountObjects 2 }

caqAclHitCountPortList OBJECT-TYPE
    SYNTAX      CiscoPortList
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Indicates the set of physical port(s), in bridge port
        number, where ACL hit count feature is enabled. 

        For each port, if ACL hit count feature is enabled then 
        the bit corresponding to that port is set to '1'.

        This object is only instantiated when the portAclHitCount(1)
        bit is set to '1' in the caqAclFeatureCpb object."
    ::= { caqAclHitCountObjects 3 }

--
-- The caqAclHitCountTable
--

caqAclHitCountTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqAclHitCountEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table provides the hit count configuration on 
        ACLs which support this feature."
    ::= { caqAclHitCountObjects 4 }

caqAclHitCountEntry      OBJECT-TYPE
    SYNTAX      CaqAclHitCountEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry indicates whether the hit count feature is enabled
        on a particular ACL as well as its statistic collection mode." 
    INDEX { caqAclHitCountAclType,
            IMPLIED caqAclHitCountAclName }
    ::= { caqAclHitCountTable 1 }

CaqAclHitCountEntry ::= SEQUENCE {
    caqAclHitCountAclType          CaqHitCountAclType, 
    caqAclHitCountAclName          CaqAclName, 
    caqAclHitCountEnable           TruthValue
}

caqAclHitCountAclType       OBJECT-TYPE
    SYNTAX      CaqHitCountAclType
    MAX-ACCESS  not-accessible 
    STATUS      current
    DESCRIPTION
        "Indicates the type of ACL.

        ipSecurity(1) indicates that this ACL is an IP Security ACL.

        ipxSecurity(2) indicates that this ACL is an IPX Security ACL.

        macSecurity(3) indicates that this ACL is a MAC Security ACL."
    ::= { caqAclHitCountEntry 1 }

caqAclHitCountAclName       OBJECT-TYPE
    SYNTAX      CaqAclName 
    MAX-ACCESS  not-accessible 
    STATUS      current
    DESCRIPTION
        "Indicates the ACL name which should exist in the ACL tables
         e.g. in caqIpAceTable. This ACL must be matching the type
         specified in caqAclHitCountAclType in the same row." 
    ::= { caqAclHitCountEntry 2 }

caqAclHitCountEnable     OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Indicates whether this ACL hit count is enabled."
    ::= { caqAclHitCountEntry 3 }

--
-- The caqAceHitCountTable
--

caqAceHitCountTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqAceHitCountEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table provides the hit count configuration on 
        ACEs which support this feature."
    ::= { caqAclHitCountObjects 5 }

caqAceHitCountEntry      OBJECT-TYPE
    SYNTAX      CaqAceHitCountEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry indicates whether the hit count feature is enabled
        on a particular ACE as well as its hit count statistic." 
    INDEX { caqAceHitCountAclType,
            caqAceHitCountAclName,
            caqAceHitCountAceIndex }
    ::= { caqAceHitCountTable 1 }

CaqAceHitCountEntry ::= SEQUENCE {
    caqAceHitCountAclType          CaqHitCountAclType, 
    caqAceHitCountAclName          CaqAclName, 
    caqAceHitCountAceIndex         Unsigned32, 
    caqAceHitCountEnable           TruthValue,
    caqAceIngressHitCount          Counter64,
    caqAceEgressHitCount           Counter64
}

caqAceHitCountAclType       OBJECT-TYPE
    SYNTAX      CaqHitCountAclType
    MAX-ACCESS  not-accessible 
    STATUS      current
    DESCRIPTION
        "Indicates the type of ACL.

        ipSecurity(1) indicates that this ACL is an IP Security ACL.

        ipxSecurity(2) indicates that this ACL is an IPX Security ACL.

        macSecurity(3) indicates that this ACL is a MAC Security ACL."
    ::= { caqAceHitCountEntry 1 }

caqAceHitCountAclName       OBJECT-TYPE
    SYNTAX      CaqAclName 
    MAX-ACCESS  not-accessible 
    STATUS      current
    DESCRIPTION
        "Indicates the ACL name which should exist in the ACL tables
         e.g. in caqIpAceTable. This ACL must be matching the type
         specified in caqAceHitCountAclType in the same row." 
    ::= { caqAceHitCountEntry 2 }

caqAceHitCountAceIndex      OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The index of an ACE within an ACL."
    ::= { caqAceHitCountEntry 3 }

caqAceHitCountEnable     OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Indicates whether this ACE hit count is enabled."
    ::= { caqAceHitCountEntry 4 }

caqAceIngressHitCount        OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates number of hit count for this ACE for
        ingress traffic."
    ::= { caqAceHitCountEntry 5 }

caqAceEgressHitCount        OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates number of hit count for this ACE for
        egress traffic."
    ::= { caqAceHitCountEntry 6 }

--
-- The caqAclIfHitCountTable
--

caqIfAclHitCountTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqIfAclHitCountEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table provides the ACL hit count statistics at
         an interface. An interface can be a physical port if
         the bit portAclHitCount(1) is set in the object
         caqAclFeatureCpb or a VLAN if the bit vlanAclHitCount(0)
         is set in the object caqAclFeatureCpb."
    ::= { caqAclHitCountObjects 6 }

caqIfAclHitCountEntry      OBJECT-TYPE
    SYNTAX      CaqIfAclHitCountEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry indicates the number of hit count at each
         ACE belonged to an ACL which supports hit count collection
         at an interface where the ACL is attached."
    INDEX { ifIndex,
            caqIfAclHitCountAclType,
            caqIfAclHitCountAclName,
            caqIfAclHitCountAceIndex }
    ::= { caqIfAclHitCountTable 1 }

CaqIfAclHitCountEntry ::= SEQUENCE {
    caqIfAclHitCountAclType      CaqHitCountAclType, 
    caqIfAclHitCountAclName      CaqAclName, 
    caqIfAclHitCountAceIndex     Unsigned32, 
    caqIfAclIngressHitCount      Counter64,
    caqIfAclEgressHitCount       Counter64
}

caqIfAclHitCountAclType       OBJECT-TYPE
    SYNTAX      CaqHitCountAclType
    MAX-ACCESS  not-accessible 
    STATUS      current
    DESCRIPTION
        "Indicates the type of ACL.

        ipSecurity(1) indicates that this ACL is an IP Security ACL.

        ipxSecurity(2) indicates that this ACL is an IPX Security ACL.

        macSecurity(3) indicates that this ACL is a MAC Security ACL."
    ::= { caqIfAclHitCountEntry 1 }

caqIfAclHitCountAclName       OBJECT-TYPE
    SYNTAX      CaqAclName 
    MAX-ACCESS  not-accessible 
    STATUS      current
    DESCRIPTION
        "Indicates the ACL name which should exist in the ACL tables
         e.g. in caqIpAceTable. This ACL must be matching the type
         specified in caqIfAclHitCountAclType in the same row." 
    ::= { caqIfAclHitCountEntry 2 }

caqIfAclHitCountAceIndex       OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The index of an ACE within an ACL." 
    ::= { caqIfAclHitCountEntry 3 }


caqIfAclIngressHitCount     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of hit count of this ACE for
        ingress traffic on this interface." 
    ::= { caqIfAclHitCountEntry 4 }

caqIfAclEgressHitCount     OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of hit count of this ACE for
        egress traffic on this interface." 
    ::= { caqIfAclHitCountEntry 5 }

--
-- The caqDownloadAclInfoTable
--

caqDownloadAclInfoTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqDownloadAclInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table provides the management information for 
        downloaded ACLs."
    ::= { caqDownloadAclObjects 1 }

caqDownloadAclInfoEntry      OBJECT-TYPE
    SYNTAX      CaqDownloadAclInfoEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry is populated for each downloaded ACL in 
         the device." 
    INDEX { IMPLIED caqDownloadAclName }
    ::= { caqDownloadAclInfoTable 1 }

CaqDownloadAclInfoEntry ::= SEQUENCE {
    caqDownloadAclName             SnmpAdminString, 
    caqDownloadAclUserCount        Unsigned32,
    caqDownloadAclDownloadTime     DateAndTime 
}

caqDownloadAclName       OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE (1..255))
    MAX-ACCESS  not-accessible 
    STATUS      current
    DESCRIPTION
        "This object indicates the name of a downloaded ACL." 
    ::= { caqDownloadAclInfoEntry 1 }

caqDownloadAclUserCount     OBJECT-TYPE
    SYNTAX      Unsigned32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates the number of users (i.e., 
        authenticated hosts) who are using this downloaded ACL." 
    ::= { caqDownloadAclInfoEntry 2 }

caqDownloadAclDownloadTime     OBJECT-TYPE
    SYNTAX      DateAndTime 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates the time when this ACL is downloaded
         to the device." 
    ::= { caqDownloadAclInfoEntry 3 }

--
-- caqIpDownloadAceTable
--

caqIpDownloadAceTable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqIpDownloadAceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains a list of downloaded IP ACEs for 
        security purpose. Each ACE consists of a filter specification
        and behavior associated with it which describes what action
        to carry out on packets which match.

        An ACL is defined as the set of ACEs. Each ACE is named by
        a combination of an AclName and an ACE index, such that all
        the ACEs which are named using the same AclName are part of
        the same ACL."
    ::= { caqDownloadAclObjects 2 }

caqIpDownloadAceEntry    OBJECT-TYPE
    SYNTAX      CaqIpDownloadAceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry defines an ACE, consisting of a set of match
        criteria. For a packet to match an entry, it has to match
        all the criteria specified in that entry."
    INDEX { caqIpDownloadAclName, caqIpDownloadAceIndex }
    ::= { caqIpDownloadAceTable 1 }

CaqIpDownloadAceEntry ::= SEQUENCE {
    caqIpDownloadAclName                   SnmpAdminString,
    caqIpDownloadAceIndex                  Unsigned32,
    caqIpDownloadAceMatchedAction          INTEGER, 
    caqIpDownloadAceProtocolType           CiscoIpProtocol,
    caqIpDownloadAceAddrType               InetAddressType,
    caqIpDownloadAceSrcIp                  InetAddress,
    caqIpDownloadAceSrcIpMask              InetAddress,
    caqIpDownloadAceSrcPortOp              INTEGER,
    caqIpDownloadAceSrcPort                InetPortNumber,
    caqIpDownloadAceSrcPortRange           InetPortNumber,
    caqIpDownloadAceDestIp                 InetAddress,
    caqIpDownloadAceDestIpMask             InetAddress,
    caqIpDownloadAceDestPortOp             INTEGER,
    caqIpDownloadAceDestPort               InetPortNumber,
    caqIpDownloadAceDestPortRange          InetPortNumber,
    caqIpDownloadAceTosMatchCriteria       INTEGER,
    caqIpDownloadAceIpPrec                 CaqIpPrecedence,
    caqIpDownloadAceDscp                   Dscp,
    caqIpDnldAcePrtocolMatchCriteria       INTEGER,
    caqIpDownloadAceIcmpType               Unsigned32,
    caqIpDownloadAceIcmpCode               Unsigned32
}

caqIpDownloadAclName  OBJECT-TYPE
    SYNTAX      SnmpAdminString
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The name of a downloaded IP ACL."
    ::= { caqIpDownloadAceEntry 1 }

caqIpDownloadAceIndex       OBJECT-TYPE
    SYNTAX      Unsigned32 
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The index of an ACE within a downloaded ACL." 
    ::= { caqIpDownloadAceEntry 2 }

caqIpDownloadAceMatchedAction      OBJECT-TYPE
    SYNTAX    INTEGER {
                  permit(1),
                  deny(2),
                  denyAndLog(3),
                  permitAndCapture(4)
              }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the action to be taken if a packet matches this ACE.

        If 'permit' is specified, the matched packet will be allowed
        through the device.

        If 'deny' is specified, the matched packet will be blocked and
        dropped.

        If 'denyAndLog' is specified, the matched packet will be
        blocked, dropped and logged.

        If 'permitAndCapture' is specified, the matched packet will be
        allowed, and a copy of it will be forwarded to capture port(s)."
    ::= { caqIpDownloadAceEntry 3 }

caqIpDownloadAceProtocolType        OBJECT-TYPE
    SYNTAX      CiscoIpProtocol 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The protocol number field in the IP header used to indicate
        the higher layer protocol as specified in RFC 1700. A value 
        value of 0 matches every IP packet. 

        For example :
        0 is IP, 1 is ICMP, 2 is IGMP, 4 is IP in IP encapsulation,
        6 is TCP, 9 is IGRP, 17 is UDP, 47 is GRE, 50 is ESP, 51 is AH,
        88 is IGRP, 89 is OSPF, 94 is KA9Q/NOS compatible IP over IP,
        103 is PIMv2, 108 is PCP."
    REFERENCE
        "RFC 1700, Assigned Numbers."
    ::= { caqIpDownloadAceEntry 4 }

caqIpDownloadAceAddrType        OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The type of IP address used by this ACE entry."
    ::= { caqIpDownloadAceEntry 5 } 

caqIpDownloadAceSrcIp           OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The specified source IP address. The packet's source address
        is AND-ed with the value of caqIpDownloadAceSrcIpMask and then
        compared against the value of this object. If this object value
        is 0.0.0.0, and the value of caqIpDownloadAceSrcIpMask object
        in the same entry is 255.255.255.255, this entry matches any
        source IP address." 
    ::= { caqIpDownloadAceEntry 6 }

caqIpDownloadAceSrcIpMask           OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The specified source IP address mask."
    ::= { caqIpDownloadAceEntry 7 }

caqIpDownloadAceSrcPortOp       OBJECT-TYPE
    SYNTAX      INTEGER { noOperator(1), lt(2), gt(3),
                          eq(4), neq(5), range(6) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates how a packet's source TCP/UDP port number is
        to be compared.

        'noOperator', which is the default value, means that no
        comparison is to be made with the source TCP/UDP port number.

        'lt' means less than, 'gt' means greater than, 'eq'
        means equal, 'neq' means not equal. Those 4 operators
        are using the caqIpDownloadAceSrcPort object as an operand
        which is the only one needed. 

        'range' means that it compares the port value between two 
        numbers, so this operator needs 2 operands. One operand is 
        the starting port number of the range which is
        caqIpDownloadAceSrcPort object, and the other operand is the
        ending port number of the range which the
        caqIpDownloadAceSrcPortRange object is in."
    ::= { caqIpDownloadAceEntry 8 }

caqIpDownloadAceSrcPort     OBJECT-TYPE
    SYNTAX      InetPortNumber 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The source port number of the TCP or UDP protocol. If the
        caqIpDownloadAceSrcPortOp object in the same row is 'range',
        this object will be the starting port number of the port
        range."
    ::= { caqIpDownloadAceEntry 9 }

caqIpDownloadAceSrcPortRange    OBJECT-TYPE
    SYNTAX      InetPortNumber 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The source port number of the TCP or UDP protocol. If the
        caqIpDownloadAceSrcPortOp object in the same row is 'range',
        this object will be the ending port number of the port range,
        otherwise the value of this object is ignored."
    ::= { caqIpDownloadAceEntry 10 }

caqIpDownloadAceDestIp          OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The specified destination IP address. The packet's destination
        address is AND-ed with the value of caqIpDownloadAceDestIpMask
        and then compared against the value of this object. If this
        object value is 0.0.0.0 and the value of
        caqIpDownloadAceDestIpMask object in the same entry is
        255.255.255.255, this entry matches any destination IP
        address." 
    ::= { caqIpDownloadAceEntry 11 }

caqIpDownloadAceDestIpMask  OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The specified destination IP address mask."
    ::= { caqIpDownloadAceEntry 12 }

caqIpDownloadAceDestPortOp      OBJECT-TYPE
    SYNTAX      INTEGER { noOperator(1), lt(2), gt(3),
                          eq(4), neq(5), range(6) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates how a packet's destination TCP/UDP port number is
        to be compared.

        'noOperator', which is the default value, means that no
        comparison is to be made with the destination TCP/UDP port
        number.

        'lt' means less than.
        
        'gt' means greater than.
 
        'eq' means equal. 
        
        'neq' means not equal. Those 4 operators are using the 
        caqIpDownloadAceDestPort object as an operand which is the
        only one needed. 

        'range' means that it compares the port value between two
        numbers, so this operator needs 2 operands. One operand is the
        starting port number of the range which is
        caqIpDownloadAceDestPort object, and the other operand is the
        ending port number of the range which the
        caqIpDownloadAceDestPortRange object is in."
    ::= { caqIpDownloadAceEntry 13 }

caqIpDownloadAceDestPort        OBJECT-TYPE
    SYNTAX      InetPortNumber 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The destination port number of the TCP or UDP protocol.
        If the caqIpDownloadAceDestPortOp object in the same row is
        'range' this object will be the starting port number of the
        port range."
    ::= { caqIpDownloadAceEntry 14 }

caqIpDownloadAceDestPortRange   OBJECT-TYPE
    SYNTAX      InetPortNumber 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The destination port number of the TCP or UDP protocol.
        If the caqIpDownloadAceDestPortOp object in the same row is
        'range', this object will be the ending port number of the
        port range, otherwise this object value is ignored."
    ::= { caqIpDownloadAceEntry 15 }

caqIpDownloadAceTosMatchCriteria     OBJECT-TYPE
    SYNTAX        INTEGER {
                    none(1), 
                    matchDscp(2),
                    matchIpPrec(3)
                  }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Indicates what field of Tos octet in the packet header
         to be matched. 
         
         'none' means that there is no need to match the ToS octet.

         'matchDscp' means that the DSCP value of packet header need
         to be matched. If this value is specified, the 
         caqIpDownloadAceDscp object in the same row should have 
         valid value. 

         'matchIpPrec' means that the IpPrecedence value of packet
         header need to be matched. If this value is specifed, the 
         caqIpDownloadAceIpPrec object in the same row should have
         a valid value." 
    ::= { caqIpDownloadAceEntry 16 }
 
caqIpDownloadAceIpPrec    OBJECT-TYPE
    SYNTAX      CaqIpPrecedence
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies the IP precedence value to be matched against.
        
        The value of this object is ignored whenever the value of 
        caqIpDownloadAceTosMatchCritial object is not 'matchIpPrec'."
    ::= { caqIpDownloadAceEntry 17 }

caqIpDownloadAceDscp       OBJECT-TYPE
    SYNTAX      Dscp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies the Dscp value to be matched against.
        Packets can be matched to DSCP value from 0 to 63. 

        The value of this object is ignored whenever the value of 
        caqIpDownloadAceTosMatchCritial object is not 'matchDscp'."
    ::= { caqIpDownloadAceEntry 18 }

caqIpDnldAcePrtocolMatchCriteria  OBJECT-TYPE
    SYNTAX        INTEGER {
                    none(1), 
                    matchIcmpType(2),
                    matchIcmpTypeAndCode(3),
                    matchEstablished(4)
                  }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Indicates what field in the packet header for ICMP or IGMP
         or TCP protocol to be matched. 
         
         'none' means no comparison is to be done for ICMP/TCP.

         'matchIcmpType' means that the Type field of ICMP protocol
         packet header needs to be matched. If this value is specified,
         the caqIpDownloadAceIcmpType object in the same row should
         have a valid value. 

         'matchIcmpTypeAndCode' means that both the Type and Code
         fields of ICMP protocol packet header need to be matched.
         If this value is specified, the caqIpDownloadAceIcmpType and
         caqIpDownloadAceIcmpCode object in the same row should have
         valid values. 
         
         'matchEstablished' means that a match occurs if the TCP packet
         has the ACK or RST bits set. The non matching case is that of
         the intial TCP packet to form a connection."
    ::= { caqIpDownloadAceEntry 19 }

caqIpDownloadAceIcmpType        OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the message type of ICMP packets. The type is
        a number from 0 to 255. 

        The value of this object is ignored whenever the value of 
        caqIpDnldAcePrtocolMatchCriteria object is not 'matchIcmpType'
        or 'matchIcmpTypeAndCode'."
    ::= { caqIpDownloadAceEntry 20 }

caqIpDownloadAceIcmpCode        OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the message code of ICMP packets. The code is
        a number from 0 to 255. 

        The value of this object is ignored whenever the value of 
        caqIpDnldAcePrtocolMatchCriteria object is not
        'matchIcmpTypeAndCode'."
    ::= { caqIpDownloadAceEntry 21 }

--
-- The caqIfDownloadAclTable
--

caqIfDownloadAclTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqIfDownloadAclEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table provides the management information for 
        physical interface where downloaded ACLs are applied."
    ::= { caqDownloadAclObjects 3 }

caqIfDownloadAclEntry      OBJECT-TYPE
    SYNTAX      CaqIfDownloadAclEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry is populated for each interface that utilies
         downloaded ACLs in the device." 
    INDEX { ifIndex, IMPLIED caqDownloadAclName }
    ::= { caqIfDownloadAclTable 1 }

CaqIfDownloadAclEntry ::= SEQUENCE {
    caqIfDownloadAclFeature          INTEGER,
    caqIfDownloadAclAddressType      InetAddressType,
    caqIfDownloadAclHostAddress      InetAddress
}

caqIfDownloadAclFeature   OBJECT-TYPE
    SYNTAX      INTEGER {
                    dot1x(1),
                    eou(2),
                    macAuth(3),
                    webAuth(4)
                } 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates the security feature running at this
        interface and trigger the download of this ACL.

        'dot1x' indicates that the 802.1x feature is running at this
        interface and trigger the download of this ACL.

        'eou' indicates that the Extensible Authentication Protocol
        over UDP (EOU) feature is running at this interface and trigger
        the download of this ACL.

        'macAuth' indicates that the Mac Authentication Bypass
        feature is running at this interface and trigger the download
        of this ACL.

        'webAuth' indicates that the Web Authentication feature is
        running at this interface and trigger the download of this ACL."
    ::= { caqIfDownloadAclEntry 1 }

caqIfDownloadAclAddressType  OBJECT-TYPE
    SYNTAX      InetAddressType 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates the type of IP address of the host."
    ::= { caqIfDownloadAclEntry 2 }

caqIfDownloadAclHostAddress  OBJECT-TYPE
    SYNTAX      InetAddress 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates IP address of the host connected
        to this interface. The type of this address is determined
        by the value of caqIfDownloadAclAddressType object." 
    ::= { caqIfDownloadAclEntry 3 }

--
-- The caqIfIpPhoneMapTable
--

caqIfIpPhoneMapTable      OBJECT-TYPE
    SYNTAX      SEQUENCE OF CaqIfIpPhoneMapEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table provides the management information for 
        the mapping of IP Phone to interface that utilizes
        downloaded ACL."
    ::= { caqDownloadAclObjects 4 }

caqIfIpPhoneMapEntry      OBJECT-TYPE
    SYNTAX      CaqIfIpPhoneMapEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry is populated for each interface that has
         an IP Phone connected to and utilizes downloaded ACL."
    INDEX { ifIndex }
    ::= { caqIfIpPhoneMapTable 1 }

CaqIfIpPhoneMapEntry ::= SEQUENCE {
    caqIfIpPhoneAddressType      InetAddressType,
    caqIfIpPhoneHostAddress      InetAddress
}

caqIfIpPhoneAddressType  OBJECT-TYPE
    SYNTAX      InetAddressType 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates the type of IP address of the
        IP Phone connected to this interface." 
    ::= { caqIfIpPhoneMapEntry 1 }

caqIfIpPhoneHostAddress  OBJECT-TYPE
    SYNTAX      InetAddress 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates the IP address of the IP Phone.
        The type of this address is determined by the value of
        the caqIfIpPhoneAddressType object."
    ::= { caqIfIpPhoneMapEntry 2 }

--
-- Notifications
--

caqMIBNotifications   OBJECT IDENTIFIER ::= { ciscoCatOSAclQosMIB 2 }

-- no notifications defined


--
-- Conformance
--

caqMIBConformance OBJECT IDENTIFIER ::= { ciscoCatOSAclQosMIB 3 }

caqMIBCompliances OBJECT IDENTIFIER
    ::= { caqMIBConformance 1 }

caqMIBGroups      OBJECT IDENTIFIER
    ::= { caqMIBConformance 2 }


-- Compliance

caqMIBCompliance MODULE-COMPLIANCE
        STATUS deprecated 
        DESCRIPTION
            "The compliance statement for the  CISCO-CATOS-ACL-QOS-MIB."
        MODULE        
        MANDATORY-GROUPS { caqIfConfigGroup, 
                           caqAclCpbGroup,
                           caqFlowPolicingCpbGroup,
                           caqQueueAssignmentGroup,
                           caqQueueGroup }

        GROUP caqQosStatsGroup
        DESCRIPTION
            "This group is mandatory only for the platform 
            which support QoS statistics information." 

        GROUP caqQosMappingGroup
        DESCRIPTION
            "This group is mandatory only for the platform 
            which support mapping between Cos, IpPrecedence
            and DSCP." 

        GROUP caqIfAclConfigGroup
        DESCRIPTION
            "This group is mandatory only for the platform 
            which support ACL configuration."

        GROUP caqIpAceGroup
        DESCRIPTION
            "This group is mandatory only in agents for which the 
            ipQos bit or ipSecurity bit of caqAclCapabilities is
            turned on."

        GROUP caqIpxAceGroup
        DESCRIPTION
            "This group is mandatory only in agents for which the 
            ipxQos bit or ipxSecurity bit of caqAclCapabilities is
            turned on."

        GROUP caqMacAceGroup
        DESCRIPTION
            "This group is mandatory only in agents for which the 
            macQos bit or macSecurity bit of caqAclCapabilities is
            turned on."

        GROUP caqPolicingGroup
        DESCRIPTION
            "This group is mandatory only for the platform
            which supports flow policing."

        GROUP caqActionGroup
        DESCRIPTION
            "This group is mandatory only for the platform
            which supports flow classification."

        GROUP caqSecurityGroup
        DESCRIPTION
            "This group is mandatory only for the platform
            which supports security feature."

        GROUP caqQosBridgedFlowPolicerGroup
        DESCRIPTION
            "This group is mandatory only for the platform
            which supports enabling or disabling bridged packets
            policing."

        GROUP caqQosMacVlanGroup
        DESCRIPTION
            "This group is mandatory only for the platform
            which support flow classification based on MAC address
            and VLAN pair."

        GROUP caqQosExcessRateGroup
        DESCRIPTION
            "This group is mandatory in agents for which the value of
            caqFlowPolicerExcessRateSupport is 'true'."

        OBJECT caqIpAceSrcIp
        SYNTAX InetAddress (SIZE(4))
        DESCRIPTION
         "An implementation is only required to support IPv4 addresses."

        OBJECT caqIpAceSrcIpMask
        SYNTAX InetAddress (SIZE(4))
        DESCRIPTION
         "An implementation is only required to support IPv4 addresses."

        OBJECT caqIpAceDestIp
        SYNTAX InetAddress (SIZE(4))
        DESCRIPTION
         "An implementation is only required to support IPv4 addresses."

        OBJECT caqIpAceDestIpMask
        SYNTAX InetAddress (SIZE(4))
        DESCRIPTION
         "An implementation is only required to support IPv4 addresses."
        ::= { caqMIBCompliances 1 }

                     
caqMIBCompliance2 MODULE-COMPLIANCE
        STATUS deprecated 
        DESCRIPTION
            "The compliance statement for the  CISCO-CATOS-ACL-QOS-MIB."
        MODULE        
        MANDATORY-GROUPS { caqIfConfigGroup, 
                           caqAclCpbGroup,
                           caqFlowPolicingCpbGroup,
                           caqQueueAssignmentGroup,
                           caqQueueGroup }

        GROUP caqQosStatsGroup
        DESCRIPTION
            "This group is mandatory only for the platform 
            which support QoS statistics information." 

        GROUP caqQosMappingGroup
        DESCRIPTION
            "This group is mandatory only for the platform 
            which support mapping between Cos, IpPrecedence
            and DSCP." 

        GROUP caqIfAclConfigGroup
        DESCRIPTION
            "This group is mandatory only for the platform 
            which support ACL configuration."

        GROUP caqIpAceGroup
        DESCRIPTION
            "This group is mandatory only in agents for which the 
            ipQos bit or ipSecurity bit of caqAclCapabilities is
            turned on."

        GROUP caqIpxAceGroup
        DESCRIPTION
            "This group is mandatory only in agents for which the 
            ipxQos bit or ipxSecurity bit of caqAclCapabilities is
            turned on."

        GROUP caqMacAceGroup
        DESCRIPTION
            "This group is mandatory only in agents for which the 
            macQos bit or macSecurity bit of caqAclCapabilities is
            turned on."

        GROUP caqPolicingGroup
        DESCRIPTION
            "This group is mandatory only for the platform
            which supports flow policing."

        GROUP caqActionGroup
        DESCRIPTION
            "This group is mandatory only for the platform
            which supports flow classification."

        GROUP caqSecurityGroup
        DESCRIPTION
            "This group is mandatory only for the platform
            which supports security feature."

        GROUP caqQosBridgedFlowPolicerGroup
        DESCRIPTION
            "This group is mandatory only for the platform
            which supports enabling or disabling bridged packets
            policing."

        GROUP caqQosMacVlanGroup
        DESCRIPTION
            "This group is mandatory only for the platform
            which support flow classification based on MAC address
            and VLAN pair."

        GROUP caqLoggingGroup
        DESCRIPTION
            "Implementation of this group is optional."

        GROUP caqArpInspGroup 
        DESCRIPTION
            "Implementation of this group is optional."

        OBJECT caqIpAceSrcIp
        SYNTAX InetAddress (SIZE(4))
        DESCRIPTION
         "An implementation is only required to support IPv4 addresses."

        OBJECT caqIpAceSrcIpMask
        SYNTAX InetAddress (SIZE(4))
        DESCRIPTION
         "An implementation is only required to support IPv4 addresses."

        OBJECT caqIpAceDestIp
        SYNTAX InetAddress (SIZE(4))
        DESCRIPTION
         "An implementation is only required to support IPv4 addresses."

        OBJECT caqIpAceDestIpMask
        SYNTAX InetAddress (SIZE(4))
        DESCRIPTION
         "An implementation is only required to support IPv4 addresses."
        ::= { caqMIBCompliances 2 }

                     
caqMIBCompliance3 MODULE-COMPLIANCE
        STATUS deprecated 
        DESCRIPTION
            "The compliance statement for the  CISCO-CATOS-ACL-QOS-MIB."
        MODULE        
        MANDATORY-GROUPS { caqIfConfigGroup, 
                           caqAclCpbGroup,
                           caqFlowPolicingCpbGroup,
                           caqQueueAssignmentGroup,
                           caqQueueGroup }

        GROUP caqQosStatsGroup
        DESCRIPTION
            "This group is mandatory only for the platform 
            which support QoS statistics information." 

        GROUP caqQosMappingGroup
        DESCRIPTION
            "This group is mandatory only for the platform 
            which support mapping between Cos, IpPrecedence
            and DSCP." 

        GROUP caqIfAclConfigGroup
        DESCRIPTION
            "This group is mandatory only for the platform 
            which support ACL configuration."

        GROUP caqIpAceGroup
        DESCRIPTION
            "This group is mandatory only in agents for which the 
            ipQos bit or ipSecurity bit of caqAclCapabilities is
            turned on."

        GROUP caqIpxAceGroup
        DESCRIPTION
            "This group is mandatory only in agents for which the 
            ipxQos bit or ipxSecurity bit of caqAclCapabilities is
            turned on."

        GROUP caqMacAceGroup
        DESCRIPTION
            "This group is mandatory only in agents for which the 
            macQos bit or macSecurity bit of caqAclCapabilities is
            turned on."

        GROUP caqPolicingGroup
        DESCRIPTION
            "This group is mandatory only for the platform
            which supports flow policing."

        GROUP caqActionGroup
        DESCRIPTION
            "This group is mandatory only for the platform
            which supports flow classification."

        GROUP caqSecurityGroup2
        DESCRIPTION
            "This group is mandatory only for the platform
            which supports security feature."

        GROUP caqQosBridgedFlowPolicerGroup
        DESCRIPTION
            "This group is mandatory only for the platform
            which supports enabling or disabling bridged packets
            policing."

        GROUP caqQosMacVlanGroup
        DESCRIPTION
            "This group is mandatory only for the platform
            which support flow classification based on MAC address
            and VLAN pair."

        GROUP caqLoggingGroup
        DESCRIPTION
            "Implementation of this group is optional."

        GROUP caqArpInspGroup 
        DESCRIPTION
            "Implementation of this group is optional."

        OBJECT caqIpAceSrcIp
        SYNTAX InetAddress (SIZE(4))
        DESCRIPTION
         "An implementation is only required to support IPv4 addresses."

        OBJECT caqIpAceSrcIpMask
        SYNTAX InetAddress (SIZE(4))
        DESCRIPTION
         "An implementation is only required to support IPv4 addresses."

        OBJECT caqIpAceDestIp
        SYNTAX InetAddress (SIZE(4))
        DESCRIPTION
         "An implementation is only required to support IPv4 addresses."

        OBJECT caqIpAceDestIpMask
        SYNTAX InetAddress (SIZE(4))
        DESCRIPTION
         "An implementation is only required to support IPv4 addresses."
        ::= { caqMIBCompliances 3 }


caqMIBCompliance4 MODULE-COMPLIANCE
        STATUS current 
        DESCRIPTION
            "The compliance statement for the  CISCO-CATOS-ACL-QOS-MIB."
        MODULE        
        MANDATORY-GROUPS { caqIfConfigGroup, 
                           caqAclCpbGroup,
                           caqFlowPolicingCpbGroup,
                           caqQueueAssignmentGroup,
                           caqQueueGroup }

        GROUP caqQosStatsGroup
        DESCRIPTION
            "This group is mandatory only for the platform 
            which support QoS statistics information." 

        GROUP caqQosMappingGroup
        DESCRIPTION
            "This group is mandatory only for the platform 
            which support mapping between Cos, IpPrecedence
            and DSCP." 

        GROUP caqIfAclConfigGroup
        DESCRIPTION
            "This group is mandatory only for the platform 
            which support ACL configuration."

        GROUP caqIpAceGroup
        DESCRIPTION
            "This group is mandatory only in agents for which the 
            ipQos bit or ipSecurity bit of caqAclCapabilities is
            turned on."

        GROUP caqIpxAceGroup
        DESCRIPTION
            "This group is mandatory only in agents for which the 
            ipxQos bit or ipxSecurity bit of caqAclCapabilities is
            turned on."

        GROUP caqMacAceGroup
        DESCRIPTION
            "This group is mandatory only in agents for which the 
            macQos bit or macSecurity bit of caqAclCapabilities is
            turned on."

        GROUP caqPolicingGroup
        DESCRIPTION
            "This group is mandatory only for the platform
            which supports flow policing."

        GROUP caqActionGroup
        DESCRIPTION
            "This group is mandatory only for the platform
            which supports flow classification."

        GROUP caqSecurityGroup2
        DESCRIPTION
            "This group is mandatory only for the platform
            which supports security feature."

        GROUP caqQosBridgedFlowPolicerGroup
        DESCRIPTION
            "This group is mandatory only for the platform
            which supports enabling or disabling bridged packets
            policing."

        GROUP caqQosMacVlanGroup
        DESCRIPTION
            "This group is mandatory only for platform which
            supports flow classification based on MAC address
            and VLAN pair."

        GROUP caqLoggingGroup
        DESCRIPTION
            "Implementation of this group is optional."

        GROUP caqArpInspGroup 
        DESCRIPTION
            "Implementation of this group is optional."

        GROUP caqQosStatsGroup2
        DESCRIPTION
            "This group is mandatory only for platform which
            supports QoS statistics information per aggregate
            policer." 

        GROUP caqSecurityPBFGroup 
        DESCRIPTION
            "This group is mandatory only for platform which
             supports PBF configuration and statistics
            information." 

        GROUP caqQosExcessBurstGroup 
        DESCRIPTION
            "This group is mandatory only for platform which
            supports Qos information on excess burst size." 

        GROUP caqIfTrustDeviceGroup 
        DESCRIPTION
            "This group is mandatory only for platform which
            supports trusted device configuration and operational
            state."

        GROUP caqSecurityRateLimitGroup 
        DESCRIPTION
            "This group is mandatory only for platform which
            supports security acl feature rate limit configuration
            state." 

        GROUP caqDscpMutationGroup 
        DESCRIPTION
            "This group is mandatory only for platform which
            supports DSCP mutation configuration information." 

        GROUP caqQosDefaultActionGroup 
        DESCRIPTION
            "This group is mandatory only for platform which
            supports default Qos action configuration on the device." 

        GROUP caqIfAclConfigGroup2 
        DESCRIPTION
            "This group is mandatory only for platform which
            supports additional ACL attachment configuration on
            the device."

        GROUP caqIpEspGroup 
        DESCRIPTION
            "Implementation of this group is optional."

        GROUP caqDscpRewriteGroup 
        DESCRIPTION
            "This group is mandatory only for platform which
            supports configuration of DSCP rewrite feature on
            the device." 

        GROUP caqAggPolicerOctetStatsGroup 
        DESCRIPTION
            "This group is mandatory only for platform which
            supports QoS statistics information per aggregate
            policer in unit of octet." 

        GROUP caqIfSecurityAclConfigGroup 
        DESCRIPTION
            "This group is mandatory only for platform which
            supports security ACL information applied at 
            physical interface on the device." 

        GROUP caqIpAceExtGroup 
        DESCRIPTION
            "This group is mandatory only for platform which
            supports source and destination group information to
            configure IP ACL on the device." 

        GROUP caqAclHitCountGroup 
        DESCRIPTION
            "This group is mandatory only for platform which
            supports ACL hit count configuration and statistics
            on the device." 

        GROUP caqMacAceExtGroup
        DESCRIPTION
            "This group is mandatory only for platform which
            supports addtional matching criteria such as the VLAN, 
            Cos information to configure MAC ACE on the device."

        GROUP caqMacPktClassifyVlanGroup 
        DESCRIPTION
            "This group is mandatory only for platform which
            supports VLAN configuration for MAC packet classify
            feature on the device."

        GROUP caqAclFeatureGroup 
        DESCRIPTION
            "This group is mandatory only for platform which
            supports device capability related to feature using
            ACL configured on the device."

        GROUP caqPortAclHitCountGroup 
        DESCRIPTION
            "This group is mandatory only for platform which
            supports security ACL information applied at
            physical interface on the device." 

        GROUP caqVlanAclHitCountGroup 
        DESCRIPTION
            "This group is mandatory only for platform which
            supports security ACL information applied at
            VLAN interface on the device." 

        OBJECT caqIpAceSrcIp
        SYNTAX InetAddress (SIZE(4))
        DESCRIPTION
         "An implementation is only required to support IPv4 addresses."

        OBJECT caqIpAceSrcIpMask
        SYNTAX InetAddress (SIZE(4))
        DESCRIPTION
         "An implementation is only required to support IPv4 addresses."

        OBJECT caqIpAceDestIp
        SYNTAX InetAddress (SIZE(4))
        DESCRIPTION
         "An implementation is only required to support IPv4 addresses."

        OBJECT caqIpAceDestIpMask
        SYNTAX InetAddress (SIZE(4))
        DESCRIPTION
         "An implementation is only required to support IPv4 addresses."
        ::= { caqMIBCompliances 4 }
                     
--
-- Units of Conformance
--

caqIfConfigGroup OBJECT-GROUP
    OBJECTS {
      caqIfTrustStateConfig,
      caqIfCos
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the Qos configuration 
        information at each physical interface on the device."
    ::= { caqMIBGroups 1 }

caqIfAclConfigGroup OBJECT-GROUP
    OBJECTS {
      caqIfAclBase,
      caqClassifierMapStatus
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the ACL information on
        the device."
    ::= { caqMIBGroups 2 }

caqAclCpbGroup OBJECT-GROUP
    OBJECTS {
      caqAclCapabilities 
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the ACL information on
        the device."
    ::= { caqMIBGroups 3 } 

caqIpAceGroup OBJECT-GROUP
    OBJECTS {
      caqIpAceMatchedAction,
      caqIpAceProtocolType,
      caqIpAceAddrType,
      caqIpAceSrcIp,
      caqIpAceSrcIpMask,
      caqIpAceSrcPortOp,
      caqIpAceSrcPort,
      caqIpAceSrcPortRange,
      caqIpAceDestIp,
      caqIpAceDestIpMask,
      caqIpAceDestPortOp,
      caqIpAceDestPort,
      caqIpAceDestPortRange,
      caqIpAceTosMatchCriteria,
      caqIpAceProtocolMatchCriteria,
      caqIpAceIpPrec,
      caqIpAceDscp,
      caqIpAceIcmpType,
      caqIpAceIcmpCode,
      caqIpAceIgmpType,
      caqIpAceOrderPosition,
      caqIpAceBeforePosition,
      caqIpAceStatus
    }
    STATUS current
    DESCRIPTION
          "A collection of objects providing the IP ACE
          information."
    ::= { caqMIBGroups 4 }

caqIpxAceGroup OBJECT-GROUP
    OBJECTS {
      caqIpxAceMatchedAction,
      caqIpxAceSrcNet,
      caqIpxAceDestMatchCriteria,
      caqIpxAceDestNet,
      caqIpxAceProtocolType,
      caqIpxAceDestNode,
      caqIpxAceDestNetMask,
      caqIpxAceDestNodeMask,
      caqIpxAceOrderPosition,
      caqIpxAceBeforePosition,
      caqIpxAceStatus
    }
    STATUS current
    DESCRIPTION
          "A collection of objects providing the IPX ACE
          information."
    ::= { caqMIBGroups 5 }

caqMacAceGroup OBJECT-GROUP
    OBJECTS {
      caqMacAceMatchedAction,
      caqMacAceSrcMac,
      caqMacAceSrcMacMask,
      caqMacAceDestMac,
      caqMacAceDestMacMask,
      caqMacAceEthertype,
      caqMacAceOrderPosition,
      caqMacAceBeforePosition,
      caqMacAceStatus
    }
    STATUS current
    DESCRIPTION
          "A collection of objects providing the MAC ACE
          information."
    ::= { caqMIBGroups 6 }

caqActionGroup OBJECT-GROUP
    OBJECTS {
      caqQosActionSelectTrust,
      caqQosActionSelectDscp,
      caqQosActionSelectMicroflow,
      caqQosActionSelectAggregate,
      caqQosActionSelectStatus
    }
    STATUS current
    DESCRIPTION
          "A collection of objects providing the ACE action
          information."
    ::= { caqMIBGroups 7 }

caqPolicingGroup OBJECT-GROUP
    OBJECTS {
      caqFlowPolicerType,
      caqFlowPolicerExcessRateSupport,
      caqFlowPolicerNormalRateRequest,
      caqFlowPolicerNormalRateGrant,
      caqFlowPolicerBurstSizeRequest,
      caqFlowPolicerBurstSizeGrant,
      caqFlowPolicerNormalRateAction,
      caqFlowPolicerStatus
    }
    STATUS current
    DESCRIPTION
          "A collection of objects providing the microflow and
          aggregate flow configuration."
    ::= { caqMIBGroups 8 }

caqQosExcessRateGroup OBJECT-GROUP
    OBJECTS {
      caqFlowPolicerExcessRateRequest,
      caqFlowPolicerExcessRateGrant,
      caqFlowPolicerExcessRateAction
    }
    STATUS current
    DESCRIPTION
          "A collection of objects providing Qos 
          information on excess rate."
    ::= { caqMIBGroups 9 }

caqQosMappingGroup OBJECT-GROUP
    OBJECTS {
      caqCosToDscpDscp,
      caqIpPrecToDscpDscp,
      caqDscpMappingCos,
      caqDscpMappingNRPolicedDscp,
      caqDscpMappingERPolicedDscp
    }
    STATUS current
    DESCRIPTION
          "A collection of objects providing Qos mapping
          information."
    ::= { caqMIBGroups 10 }

caqQueueAssignmentGroup OBJECT-GROUP
    OBJECTS {
      caqCosAssignQueueNumber,
      caqCosAssignThresholdNumber
    }
    STATUS current
    DESCRIPTION
          "A collection of objects providing the queue assignment
          information."
    ::= { caqMIBGroups 11 }

caqQueueGroup OBJECT-GROUP
    OBJECTS {
      caqQueueThreshDropAlgorithm,
      caqQueueThreshDropThreshold,
      caqQueueThreshMinWredThreshold,
      caqQueueThreshMaxWredThreshold,
      caqQueueWrrWeight,
      caqQueueBufferSizeRatio
    }
    STATUS current
    DESCRIPTION
          "A collection of objects providing the queue 
          information."
    ::= { caqMIBGroups 12 }

caqQosBridgedFlowPolicerGroup OBJECT-GROUP
    OBJECTS {
      caqBridgedFlowEnabled
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the information on 
        bridged packet policing." 
    ::= { caqMIBGroups 13 }

caqQosMacVlanGroup OBJECT-GROUP
    OBJECTS {
      caqMacAddressCpb,
      caqCosValue,
      caqCosMacVlanRouterStatus
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the classification 
        information based on Mac address and vlan." 
    ::= { caqMIBGroups 14 }

caqQosStatsGroup OBJECT-GROUP
    OBJECTS {
      caqL3PacketsDropByPolicer,
      caqTosChangedIpPackets,
      caqCosChangedIpPackets,
      caqCosChangedNonIpPackets,
      caqPortStatsDropPkts,
      caqFlowStatsOutOfProfilePackets
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the QoS statistics
        information."
    ::= { caqMIBGroups 15 }

caqSecurityGroup OBJECT-GROUP
    OBJECTS {
       caqSecurityAction,
       caqSecurityCapture,
       caqSecurityRedirectPortList,
       caqSecurityActionStatus,
       caqSecurityAclCaptureEnable
    }
    STATUS deprecated 
    DESCRIPTION
        "A collection of objects providing the security information."
    ::= { caqMIBGroups 16 }

caqFlowPolicingCpbGroup OBJECT-GROUP
    OBJECTS {
      caqFlowPolicingCpb 
    }
    STATUS current
    DESCRIPTION
        "A collection of object providing the flow policing capability
         information." 
    ::= { caqMIBGroups 17 }

caqQosStatsGroup2 OBJECT-GROUP
    OBJECTS {
      caqAggPolicerPackets,
      caqAggPolicerNRExceedPackets,
      caqAggPolicerERExceedPackets
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the QoS statistics
        information per aggregate policer."
    ::= { caqMIBGroups 18 }

caqSecurityPBFGroup OBJECT-GROUP
    OBJECTS {
      caqPbfStatus,
      caqPbfMacAddress,
      caqAdjDstVlanNumber,
      caqAdjDstMacAddress,
      caqAdjSrcMacAddress,
      caqAdjName,
      caqAdjMtu,
      caqAdjHitCount,
      caqAdjStatus,
      caqSecurityAdjIndex
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the PBF configuration 
        and statistics information."
    ::= { caqMIBGroups 19 }

caqQosExcessBurstGroup OBJECT-GROUP
    OBJECTS {
      caqFlowPolicerExcessBurstSupport,
      caqFlowPolicerExcessBurstRequest,
      caqFlowPolicerExcessBurstGrant
    }
    STATUS current
    DESCRIPTION
          "A collection of objects providing Qos information on
          excess burst size."
    ::= { caqMIBGroups 20 }

caqIfTrustDeviceGroup OBJECT-GROUP
    OBJECTS {
      caqIfTrustDevice,
      caqIfOperTrustState
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the trusted device
        configuration and operational state."
    ::= { caqMIBGroups 21 }

caqLoggingGroup OBJECT-GROUP
    OBJECTS {
      caqAclLogMaxFlow,
      caqAclSecurityLoggingRateLimit,
      caqAclRouterAclRateLimit,
      caqIpFlowVlan,
      caqIpFlowIfIndex,
      caqIpFlowProtocolType,
      caqIpFlowAddrType,
      caqIpFlowSrcIp,
      caqIpFlowSrcPort,
      caqIpFlowDestIp,
      caqIpFlowDestPort,
      caqIpFlowIcmpType,
      caqIpFlowIcmpCode,
      caqIpFlowIgmpType,
      caqIpFlowArpOpcode,
      caqIpFlowArpSrcMacAddr,
      caqIpFlowArpHeaderSrcMacAddr,
      caqIpFlowPacketsCount,
      caqIpFlowLoggingTTL
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the security logging 
        configuration and statistics."
    ::= { caqMIBGroups 22 }

caqArpInspGroup OBJECT-GROUP
    OBJECTS {
      caqSecurityArpMacAddress,
      caqAclArpInspMatchMac,
      caqAclArpInspAddrValidation,
      caqArpInspGlobalForwardedPkts,
      caqArpInspGlobalDroppedPkts,
      caqRARPForwardedPkts,
      caqMatchedMacFailedPkts,
      caqAddrValidationFailedPkts,
      caqArpInspIpDroppedPkts, 
      caqArpInspForwardedPackets,
      caqArpInspDroppedPackets,
      caqIfArpInspDropThreshold,
      caqIfArpInspShutdownThreshold
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the ARP Inspection 
        configuration and statistics."
    ::= { caqMIBGroups 23 }

caqSecurityRateLimitGroup OBJECT-GROUP
    OBJECTS {
      caqSecurityRateLimitFeatures,
      caqSecurityAclRateLimit
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the security acl
        feature rate limit configuration state."
    ::= { caqMIBGroups 24 }

caqDscpMutationGroup OBJECT-GROUP
    OBJECTS {
      caqDscpMutationNewDscp,
      caqVlanMutationTableId
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the DSCP mutation 
        configuration information."
    ::= { caqMIBGroups 25 }

caqQosDefaultActionGroup OBJECT-GROUP
    OBJECTS {
      caqQosDefaultTrustState,
      caqQosDefaultDscp,
      caqQosDefaultMicroflow,
      caqQosDefaultAggregate
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the default Qos action 
        configuration on the device."
    ::= { caqMIBGroups 26 }

caqIfAclConfigGroup2 OBJECT-GROUP
    OBJECTS {
      caqClassifierMapDirection
    }
    STATUS current
    DESCRIPTION
        "A collection of object providing the additional ACL attachment
        configuration on the device."
    ::= { caqMIBGroups 27 }

caqIpEspGroup OBJECT-GROUP
    OBJECTS {
      caqIpAceSecurityId
    }
    STATUS current
    DESCRIPTION
        "A collection of object providing the Ip ESP traffic matching 
        configuration on the device."
    ::= { caqMIBGroups 28 }

caqDscpRewriteGroup OBJECT-GROUP
    OBJECTS {
      caqDscpRewriteEnabled       
    }
    STATUS current
    DESCRIPTION
        "A collection of object providing the configuration of
        DSCP rewrite feature on the device."
    ::= { caqMIBGroups 29 }

caqAggPolicerOctetStatsGroup OBJECT-GROUP
    OBJECTS {
      caqAggPolicerOctets,
      caqAggPolicerNRExceedOctets,
      caqAggPolicerERExceedOctets
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the QoS statistics
        information per aggregate policer in unit of octet."
    ::= { caqMIBGroups 30 }

caqSecurityGroup2 OBJECT-GROUP
    OBJECTS {
       caqSecurityAction,
       caqSecurityCapture,
       caqSecurityRedirect2kPortList,
       caqSecurityActionStatus,
       caqSecurityAclCaptureEnable
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the security information."
    ::= { caqMIBGroups 31 }

caqIfSecurityAclConfigGroup OBJECT-GROUP
    OBJECTS {
      caqIfSecurityAclBase
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the security ACL 
         information on the device."
    ::= { caqMIBGroups 32 }

caqIpAceExtGroup OBJECT-GROUP
    OBJECTS {
      caqIpAceSrcGroup,
      caqIpAceDestGroup
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the source and destination
         group information to configure IP ACL on the device."
    ::= { caqMIBGroups 33 }

caqAclHitCountGroup OBJECT-GROUP
    OBJECTS {
      caqAclHitCountEnable, 
      caqAceHitCountEnable, 
      caqAceIngressHitCount, 
      caqAceEgressHitCount, 
      caqIfAclIngressHitCount,
      caqIfAclEgressHitCount
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the ACL hit count 
         configuration and statistics on the device."
    ::= { caqMIBGroups 34 }

caqMacAceExtGroup OBJECT-GROUP
    OBJECTS {
      caqMacAceMatchCriteria,
      caqMacAceVlan,
      caqMacAceCos
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing addtional matching
         criteria such as the VLAN, Cos information to configure
         MAC ACE on the device."
    ::= { caqMIBGroups 35 }

caqMacPktClassifyVlanGroup OBJECT-GROUP
    OBJECTS {
      caqMacPktClassifyVlansLow, 
      caqMacPktClassifyVlansHigh 
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the VLAN
         configuration for MAC packet classify feature 
         on the device."
    ::= { caqMIBGroups 36 }

caqAclFeatureGroup OBJECT-GROUP
    OBJECTS {
      caqAclFeatureCpb
    }
    STATUS current
    DESCRIPTION
        "A collection of object providing what feature
         related to ACL that the device is capable of."
    ::= { caqMIBGroups 37 }

caqPortAclHitCountGroup OBJECT-GROUP
    OBJECTS {
      caqAclHitCountPortList
    }
    STATUS current
    DESCRIPTION
        "A collection of object providing the set of physical
         ports where ACL hit count feature is enabled." 
    ::= { caqMIBGroups 38 }

caqVlanAclHitCountGroup OBJECT-GROUP
    OBJECTS {
      caqAclHitCountVlansLow,
      caqAclHitCountVlansHigh
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the set of VLANs 
         where ACL hit count feature is enabled." 
    ::= { caqMIBGroups 39 }

caqQosL3StatsRateGroup OBJECT-GROUP
    OBJECTS {
      caqL3PacketsDropByPolicerAveRate,       
      caqTosChangedIpPacketsAveRate,
      caqCosChangedNonIpPacketsAveRate,
      caqCosChangedIpPacketsAveRate
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the five minute 
         linearly-decayed moving average QoS statistics for Layer 3
         traffic."
    ::= { caqMIBGroups 40 }

caqQosL3StatsPeakGroup OBJECT-GROUP
    OBJECTS {
      caqCosChangedNonIpPacketPeakRate,
      caqCosChangedIpPacketsPeakRate,
      caqL3PacketsDropByPolicerPeakRate,
      caqTosChangedIpPacketsPeakRate      
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the peak rate QoS
         statistics over past five minute period for Layer 3 traffic." 
    ::= { caqMIBGroups 41 }

caqAggPolicerOctetsRateGroup OBJECT-GROUP
    OBJECTS {
      caqAggPolicerOctetsRate,
      caqAggPolicerNRExceedOctetsRate,
      caqAggPolicerERExceedOctetsRate
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the five minute 
         linearly-decayed octets moving average rate per aggregate
         policer."
    ::= { caqMIBGroups 42 }

caqAggPolicerPacketsRateGroup OBJECT-GROUP
    OBJECTS {
      caqAggPolicerPacketsRate,
      caqAggPolicerNRExceedPacketsRate,
      caqAggPolicerERExceedPacketsRate
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the five minute 
         linearly-decayed packets moving average rate per aggregate
         policer."
    ::= { caqMIBGroups 43 }

caqAggPolicerOctetsPeakGroup OBJECT-GROUP
    OBJECTS {
      caqAggPolicerOctetsPeakRate
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the peak rate of octets
         over past five minute period per aggregate policer." 
    ::= { caqMIBGroups 44 }

caqAggPolicerPacketsPeakGroup OBJECT-GROUP
    OBJECTS {
      caqAggPolicerPacketsPeakRate
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the peak rate of packets
         over past five minute period per aggregate policer." 
    ::= { caqMIBGroups 45 }

caqQosPortRateGroup OBJECT-GROUP
    OBJECTS {
      caqPortStatsDropPktsAveRate
    }
    STATUS current
    DESCRIPTION
        "A collection of object providing the five minute
         linearly-decayed packets drop rate per interface." 
    ::= { caqMIBGroups 46 }

caqQosPortPeakGroup OBJECT-GROUP
    OBJECTS {
      caqPortStatsDropPktsPeakRate    
    }
    STATUS current
    DESCRIPTION
        "A collection of object providing the peak rate of packets
         over past five minute period per interface." 
    ::= { caqMIBGroups 47 }

caqSecurityActionDnldAceGroup OBJECT-GROUP
    OBJECTS {
      caqSecurityDownloadedAceFeature
    }
    STATUS current
    DESCRIPTION
        "A collection of object providing feature type of downloaded
         ACE." 
    ::= { caqMIBGroups 48 }

caqSecurityDownloadAclInfoGroup OBJECT-GROUP
    OBJECTS {
        caqDownloadAclUserCount,
        caqDownloadAclDownloadTime 
    }
    STATUS current
    DESCRIPTION
        "A collection of object providing downloaded ACL information."
    ::= { caqMIBGroups 49 }

caqSecurityDownloadIpAceGroup OBJECT-GROUP
    OBJECTS {
        caqIpDownloadAceMatchedAction,
        caqIpDownloadAceProtocolType,
        caqIpDownloadAceAddrType,
        caqIpDownloadAceSrcIp,
        caqIpDownloadAceSrcIpMask,
        caqIpDownloadAceSrcPortOp,
        caqIpDownloadAceSrcPort,
        caqIpDownloadAceSrcPortRange,
        caqIpDownloadAceDestIp,
        caqIpDownloadAceDestIpMask,
        caqIpDownloadAceDestPortOp,
        caqIpDownloadAceDestPort,
        caqIpDownloadAceDestPortRange,
        caqIpDownloadAceTosMatchCriteria,
        caqIpDownloadAceIpPrec,
        caqIpDownloadAceDscp,
        caqIpDnldAcePrtocolMatchCriteria,
        caqIpDownloadAceIcmpType,
        caqIpDownloadAceIcmpCode
    }
    STATUS current
    DESCRIPTION
        "A collection of object providing download IP ACE information."
    ::= { caqMIBGroups 50 }

caqIfDownloadAclMapGroup OBJECT-GROUP
    OBJECTS {
        caqIfDownloadAclFeature,
        caqIfDownloadAclAddressType, 
        caqIfDownloadAclHostAddress     
    }
    STATUS current
    DESCRIPTION
        "A collection of object providing mapping information of
        downloaded ACL to capable interface."
    ::= { caqMIBGroups 51 }

caqIfIpPhoneMapGroup OBJECT-GROUP
    OBJECTS {
        caqIfIpPhoneAddressType, 
        caqIfIpPhoneHostAddress     
    }
    STATUS current
    DESCRIPTION
        "A collection of object providing mapping information
        of IP phone to capable interface where downloaded ACL
        is utilized." 
    ::= { caqMIBGroups 52 }

caqIpAceTypeGroup OBJECT-GROUP
    OBJECTS {
        caqIpAceType 
    }
    STATUS current
    DESCRIPTION
        "A collection of object providing the type of an Ip ACE."
    ::= { caqMIBGroups 53 }

caqIpOperClassifierGroup OBJECT-GROUP
    OBJECTS {
        caqIpOperAclName,
        caqIpOperAclMapSource
    }
    STATUS current
    DESCRIPTION
        "A collection of objects provides the operational mapping
         of IP ACLs to each applicable interface." 
    ::= { caqMIBGroups 54 }

caqDownloadClassifierGroup OBJECT-GROUP
    OBJECTS {
        caqDownloadClassifierAclName,
        caqDownloadMapSource,
        caqDownloadAclType
    }
    STATUS current
    DESCRIPTION
        "A collection of objects provides the mapping of ACLs to each
        applicable interface downloaded by security features." 
    ::= { caqMIBGroups 55 }

caqArpLoggingSourceGroup OBJECT-GROUP
    OBJECTS {
        caqIpFlowArpLoggingSource,
        caqIpFlowArpAclName,
        caqIpFlowArpAceNumber
    }
    STATUS current
    DESCRIPTION
        "A collection of objects provides the logging source of
        ARP flow."
    ::= { caqMIBGroups 56 }

END



