-- ***********************************************
-- PAN-COMMON-MIB.my
--
-- MIB for the common MIB objects implemented by all
-- Palo Alto devices.
-- ***********************************************

PAN-COMMON-MIB DEFINITIONS ::= BEGIN

	IMPORTS
		MODULE-IDENTITY, OBJECT-IDENTITY,
		OBJECT-TYPE, NOTIFICATION-TYPE,
		Integer32
			FROM SNMPv2-SMI
--		MODULE-COMPLIANCE, OBJECT-GROUP
--			FROM SNMPv2-CONF
		TEXTUAL-CONVENTION
            		FROM SNMPv2-TC
		DisplayString, TruthValue
			FROM SNMPv2-TC
		TcChassisType
			FROM PAN-GLOBAL-TC
		panModules, panCommonMib
			FROM PAN-GLOBAL-REG;

	panCommonMibModule MODULE-IDENTITY
		LAST-UPDATED			"201409040000Z"
		ORGANIZATION			"Palo Alto Networks"
		CONTACT-INFO			"
					Customer Support
					Palo Alto Networks
					4401 Great America Pkwy
					Santa Clara, CA 95054-1211

					+1 866-898-9087
					support at paloaltonetworks dot com"

		DESCRIPTION				"
			A MIB module containing definitions of managed objects
			implemented by all Palo Alto Networks' products."
        REVISION                "201406300000Z"
        DESCRIPTION             "
            Rev 2.3
                        Added entries for Log Collector."
        REVISION                "201409040000Z"
        DESCRIPTION             "
            Rev 2.2
                        Added entries for Wildfire content versions.
                        Added entry for new platform PA 3060."
		REVISION				"201403060000Z"
		DESCRIPTION				"
			Rev 2.1
                        Fixed a capitalization error with PanVsysEntry."
		REVISION				"201303010000Z"
		DESCRIPTION				"
			Rev 2.0
                        Updated with panGlobalProtect and panVsysTable."
        REVISION                "201102091610Z"
		DESCRIPTION				"
			Rev 1.0
			Initial version of MIB module PAN-COMMON-MIB."

		::= { panModules 3 }

	panCommonConfMib OBJECT-IDENTITY
		STATUS					current
		DESCRIPTION				"
			Sub-tree for MIB conformance statements."
		::= { panCommonMib 1 }

	panCommonObjs OBJECT-IDENTITY
		STATUS					current
		DESCRIPTION				"
			Sub-tree for common MIB objects."
		::= { panCommonMib 2 }

	panCommonEvents OBJECT-IDENTITY
		STATUS					current
		DESCRIPTION				"
			Sub-tree for common MIB events."
		::= { panCommonMib 3 }

	-- Top level groups

	panSys OBJECT-IDENTITY
		STATUS					current
		DESCRIPTION				"
			Sub-tree for common system objects."
		::= { panCommonObjs 1 }

	panChassis OBJECT-IDENTITY
		STATUS					current
		DESCRIPTION				"
			Sub-tree for common chassis information."
		::= { panCommonObjs 2 }

	panSession OBJECT-IDENTITY
		STATUS					current
		DESCRIPTION				"
			Sub-tree for common session information."
		::= { panCommonObjs 3 }

	panMgmt OBJECT-IDENTITY
		STATUS					current
		DESCRIPTION				"
			Sub-tree for common Management plane information."
		::= { panCommonObjs 4 }

	panGlobalProtect OBJECT-IDENTITY
		STATUS					current
		DESCRIPTION				"
			Sub-tree for common GlobalProtect information."
		::= { panCommonObjs 5 }

	panLogCollector OBJECT-IDENTITY
		STATUS					current
		DESCRIPTION				"
			Sub-tree for common Log Collector information."
		::= { panCommonObjs 6 }

    panDeviceLogging OBJECT-IDENTITY
        STATUS					current
        DESCRIPTION				"
            Sub-tree for common Device information."
        ::= { panCommonObjs 7 }

    panGlobalCounters OBJECT-IDENTITY
        STATUS                  current
        DESCRIPTION             "
            Sub-tree for common Global counters."
        ::= { panSys 19 }

	----------------------------------------------------------------------
	-- System objects

	panSysSwVersion OBJECT-TYPE
		SYNTAX      DisplayString
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Full software version. The first two components of the full
			version are the major and minor versions. The third component
			indicates the maintenance release number and the fourth,
			the build number."
		::= { panSys 1 }

	panSysHwVersion OBJECT-TYPE
		SYNTAX      DisplayString
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Hardware version of the unit."
		::= { panSys 2 }

	panSysSerialNumber OBJECT-TYPE
		SYNTAX      DisplayString
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"The serial number of the unit. If not available,
			an empty string is returned."
		::= { panSys 3 }

	panSysTimeZoneOffset OBJECT-TYPE
		SYNTAX      Integer32
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"The offset in seconds from UTC of the system's time zone.
			Values are negative for locations west of UTC and positive
			for locations east of UTC."
		::= { panSys 4 }

	panSysDaylightSaving OBJECT-TYPE
		SYNTAX      TruthValue
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Whether daylight savings are in currently in effect for the
			system's time zone."
		::= { panSys 5 }

	panSysVpnClientVersion OBJECT-TYPE
		SYNTAX      DisplayString
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Currently installed VPN client package version.  If
			package is not installed, 0.0.0 is returned."
		::= { panSys 6 }

	panSysAppVersion OBJECT-TYPE
		SYNTAX      DisplayString
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Currently installed application definition version.  If 
			no application definition is found, 0 is returned."
		::= { panSys 7 }

	panSysAvVersion OBJECT-TYPE
		SYNTAX      DisplayString
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Currently installed antivirus version.  If no antivirus 
			is found, 0 is returned."
		::= { panSys 8 }

	panSysThreatVersion OBJECT-TYPE
		SYNTAX      DisplayString 
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Currently installed threat definition version.  If no
			threat definition is found, 0 is returned."
		::= { panSys 9 }

	panSysUrlFilteringVersion OBJECT-TYPE
		SYNTAX      DisplayString 
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Currently installed URL filtering version.  If no URL
			filtering is installed, 0 is returned."
		::= { panSys 10 }

	panSysHAState OBJECT-TYPE
		SYNTAX      DisplayString 
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Current high-availability state."
		::= { panSys 11 }

	panSysHAPeerState OBJECT-TYPE
		SYNTAX      DisplayString
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Current peer high-availability state."
		::= { panSys 12 }

	panSysHAMode OBJECT-TYPE
		SYNTAX      DisplayString 
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Current high-availability mode (disabled, 
			active-passive, or active-active)."
		::= { panSys 13 }

	panSysUrlFilteringDatabase OBJECT-TYPE
		SYNTAX      DisplayString
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Current installed URL filtering database
			(surfcontrol, brightcloud, etc)"
		::= { panSys 14 }

	panSysGlobalProtectClientVersion OBJECT-TYPE
		SYNTAX      DisplayString
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Currently installed global-protect client package version. 
			If package is not installed, 0.0.0 is returned."
		::= { panSys 15 }

	panSysOpswatDatafileVersion OBJECT-TYPE
		SYNTAX      DisplayString
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Currently installed opswat database version. 
			If package is not installed, 0 is returned."
		::= { panSys 16 }

        panSysWildfireVersion OBJECT-TYPE
                SYNTAX      DisplayString
                MAX-ACCESS  read-only
                STATUS      current
                DESCRIPTION
                        "Currently installed wildfire content version.  If no wildfire content 
                         is found, 0 is returned."
                ::= { panSys 17 }

        panSysWildfirePrivateCloudVersion OBJECT-TYPE
                SYNTAX      DisplayString
                MAX-ACCESS  read-only
                STATUS      current
                DESCRIPTION
                        "Currently installed wildfire private cloud content version.  If no wpc
                        is found, 0 is returned."
                ::= { panSys 18 }

        panSysAppReleaseDate OBJECT-TYPE
                SYNTAX      DisplayString
                MAX-ACCESS  read-only
                STATUS      current
                DESCRIPTION
                        "Currently installed application definition release date.  If 
                        no release date is found, unknown is returned."
                ::= { panSys 20 }

        panSysThreatReleaseDate OBJECT-TYPE
                SYNTAX      DisplayString
                MAX-ACCESS  read-only
                STATUS      current
                DESCRIPTION
                        "Currently installed threat release date.  If
                        no release date is found, unknown is returned."
                ::= { panSys 21 }

        panSysAvReleaseDate OBJECT-TYPE
                SYNTAX      DisplayString
                MAX-ACCESS  read-only
                STATUS      current
                DESCRIPTION
                        "Currently installed antivirus release date.  If
                        no release date is found, unknown is returned."
                ::= { panSys 22 }

        panSysWfReleaseDate OBJECT-TYPE
                SYNTAX      DisplayString
                MAX-ACCESS  read-only
                STATUS      current
                DESCRIPTION
                        "Currently installed WildFire release date.  If
                        no release date is found, unknown is returned."
                ::= { panSys 23 }

	----------------------------------------------------------------------
	-- Chassis

	panChassisType OBJECT-TYPE
		SYNTAX      DisplayString
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Chassis type for this Palo Alto device."
		::= { panChassis 1 }

	panMSeriesMode OBJECT-TYPE
		SYNTAX      DisplayString
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Series Mode for this Palo Alto device."
		::= { panChassis 2 }


	----------------------------------------------------------------------
	-- Session

	panSessionUtilization OBJECT-TYPE
		SYNTAX      Integer32
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Session table utilization percentage. Values should
			be between 0 and 100."
		::= { panSession 1 }

	panSessionMax OBJECT-TYPE
		SYNTAX      Integer32
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Total number of sessions supported."
		::= { panSession 2 }

	panSessionActive OBJECT-TYPE
		SYNTAX      Integer32
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Total number of active sessions."
		::= { panSession 3 }

	panSessionActiveTcp OBJECT-TYPE
		SYNTAX      Integer32
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Total number of active TCP sessions."
		::= { panSession 4 }

	panSessionActiveUdp OBJECT-TYPE
		SYNTAX      Integer32
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Total number of active UDP sessions."
		::= { panSession 5 }

	panSessionActiveICMP OBJECT-TYPE
		SYNTAX      Integer32
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Total number of active ICMP sessions."
		::= { panSession 6 }

	panSessionActiveSslProxy OBJECT-TYPE
		SYNTAX      Integer32
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Total number of active SSL proxy sessions."
		::= { panSession 7 }

	panSessionSslProxyUtilization OBJECT-TYPE
		SYNTAX      Integer32
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"SSL proxy Session utilization percentage. Values should
			be between 0 and 100."
		::= { panSession 8 }

	panVsysTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF PanVsysEntry
        MAX-ACCESS      not-accessible
		STATUS			current
		DESCRIPTION
			"VSYS table"
		::= { panSession 9 }
        
    panZoneTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF PanZoneEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION             "    
            Sub-tree for the current active connectionsPerSecond (CPS) values
            for each zone present."
        ::= { panSession 10 }

    panIfTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF PanIfEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION             "    
            Sub-tree for the current active connectionsPerSecond (CPS) values
            for each interface present."
        ::= { panSession 11 }


	----------------------------------------------------------------------
	-- VsysTable 

    panVsysEntry OBJECT-TYPE
		SYNTAX          PanVsysEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
            "Entries are created when the Vsys's are added to the
            entVsysTable."
    INDEX           { panVsysId }
    ::= { panVsysTable 1 }

    PanVsysEntry ::= SEQUENCE {
        panVsysId                       Integer32,
	    panVsysName                     DisplayString,
	    panVsysSessionUtilizationPct    Integer32,
    	panVsysActiveSessions           Integer32,
    	panVsysMaxSessions              Integer32,
        panVsysActiveTcpCps             Unsigned32,    
        panVsysActiveUdpCps             Unsigned32,    
        panVsysActiveOtherIpCps         Unsigned32 
       }
       
	panVsysId OBJECT-TYPE
		SYNTAX      Integer32
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Vsys id"
		::= { panVsysEntry 1 }

	panVsysName OBJECT-TYPE
		SYNTAX      DisplayString
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"User assigned vsys name (empty string if not available)"
		::= { panVsysEntry 2 }

	panVsysSessionUtilizationPct OBJECT-TYPE
		SYNTAX      Integer32
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Vsys utilization percentage, if session limit is configured.
            If session limit is not configured, this value is '0'"
		::= { panVsysEntry 3 }

	panVsysActiveSessions OBJECT-TYPE
		SYNTAX      Integer32
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Active sessions on this Vsys"
		::= { panVsysEntry 4 }

	panVsysMaxSessions OBJECT-TYPE
		SYNTAX      Integer32
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Max sessions on this Vsys, if session limit is configured.
            If session limit is not configured, this value is '0'"
		::= { panVsysEntry 5 }

    panVsysActiveTcpCps OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Number of active Tcp Connections per second for thie vSys."
        ::= { panVsysEntry 6 }

    panVsysActiveUdpCps OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Number of active Udp Connections per second for thie vSys."
        ::= { panVsysEntry 7 }

    panVsysActiveOtherIpCps OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Number of active Other IP Connections per second for thie vSys."
        ::= { panVsysEntry 8 }

	----------------------------------------------------------------------
	-- Mgmt

	panMgmtPanoramaConnected OBJECT-TYPE
		SYNTAX      DisplayString
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Current Connection status to Panorama Server (connected, not-connected)"
		::= { panMgmt 1 }

	panMgmtPanorama2Connected OBJECT-TYPE
		SYNTAX      DisplayString
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Current Connection status to Panorama2 Server (connected, not-connected)"
		::= { panMgmt 2 }

	----------------------------------------------------------------------
	-- GlobalProtect 

	panGPGatewayUtilization OBJECT-IDENTITY
		STATUS					current
		DESCRIPTION
			"GlobalProtect gateway utilization"
		::= { panGlobalProtect 1 }

	----------------------------------------------------------------------
	-- GlobalProtect gateway utilization 

	panGPGWUtilizationPct OBJECT-TYPE
		SYNTAX      Integer32
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"GlobalProtect Gateway utilization percentage"
		::= { panGPGatewayUtilization 1 }

	panGPGWUtilizationMaxTunnels OBJECT-TYPE
		SYNTAX      Integer32
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Max tunnels allowed"
		::= { panGPGatewayUtilization 2 }

	panGPGWUtilizationActiveTunnels OBJECT-TYPE
		SYNTAX      Integer32
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
			"Number of active tunnels"
		::= { panGPGatewayUtilization 3 }
 
    --------------------------------------------------------------------
    -- Device Logging MIB
    panDeviceLoggingLogRate OBJECT-IDENTITY
        STATUS                  current
        DESCRIPTION             "
            Sub-tree for Device Logging Rate statistics."
        ::= { panDeviceLogging 1 }

    panDeviceLoggingLogTypeStatTable OBJECT-TYPE
        SYNTAX                  SEQUENCE OF PanDeviceLoggingLogTypeStatEntry
        MAX-ACCESS              not-accessible
        STATUS                  current
        DESCRIPTION             "
            Sub-tree for the statistics for different log types on the Device."
        ::= { panDeviceLogging 2 }

    panDeviceLoggingLogUsageTable OBJECT-TYPE
        SYNTAX                  SEQUENCE OF PanDeviceLoggingLogUsageEntry
        MAX-ACCESS              not-accessible
        STATUS                  current
        DESCRIPTION             "
            Sub-tree for Log Usage and days retained for different log types on the Device.
            Log Disk Usage is avaiable as MB (in use)."
        ::= { panDeviceLogging 3 }

    panDeviceLoggingExtFwd OBJECT-IDENTITY
        STATUS                  current
        DESCRIPTION             "
            Sub-tree for tracking dropped logs as ther are forwarded from device."
        ::= { panDeviceLogging 4 }

    panDeviceLoggingCollectorConnectionTable OBJECT-TYPE
        SYNTAX                  SEQUENCE OF PanDeviceLoggingCollectorConnectionEntry
        MAX-ACCESS              not-accessible
        STATUS                  current
        DESCRIPTION             "
            Sub-tree for tracking various log collection entities connected to  device."
        ::= { panDeviceLogging 5 }


    ---------------------------------------------------------------------------
    -- panDeviceLoggingLogRate

    panDeviceIncomingLogRate OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The incoming rate in logs/s on the Device."
        ::= { panDeviceLoggingLogRate 1 }
 
    panDeviceWriteLogRate OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The write rate in logs/s on the Device."
        ::= { panDeviceLoggingLogRate 2 }

    ---------------------------------------------------------------------------
    -- panDeviceLoggingLogTypeStatTable

    panDeviceLoggingLogTypeStatEntry OBJECT-TYPE
        SYNTAX          PanDeviceLoggingLogTypeStatEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
            "Entries are created when the panLcLogUsage are added to the panLcLogUsageTable."
    INDEX           { panDeviceLoggingDevice, panDeviceLoggingLogType }
    ::= { panDeviceLoggingLogTypeStatTable  1 }
    
    PanDeviceLoggingLogTypeStatEntry ::= SEQUENCE {
        panDeviceLoggingDevice                      DisplayString,
        panDeviceLoggingDeviceIndex                 Integer32,
        panDeviceLoggingLogType                     DisplayString,
        panDeviceLoggingLogLastLogCreated           TimeStamp,
        panDeviceLoggingLogLastLogFwded             TimeStamp,
        panDeviceLoggingLogLastSeqNumberFwded       Counter64,
        panDeviceLoggingLogLastSeqNumberAck         Counter64,
        panDeviceLoggingLogTotalLogsFwded           Counter64
    }

    panDeviceLoggingDevice OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Device Information (Name or Serial Number)."
        ::= { panDeviceLoggingLogTypeStatEntry 1 }
    
    panDeviceLoggingDeviceIndex OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Index as mentioned in panDeviceLoggingCollectorConnection table."
        ::= { panDeviceLoggingLogTypeStatEntry 2 }

    panDeviceLoggingLogType OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Type of log."
        ::= { panDeviceLoggingLogTypeStatEntry 3 }

    panDeviceLoggingLogLastLogCreated OBJECT-TYPE
        SYNTAX      TimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Time of the last log creation."
        ::= { panDeviceLoggingLogTypeStatEntry 4 }

    panDeviceLoggingLogLastLogFwded OBJECT-TYPE
        SYNTAX      TimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Time at which last log was forwarded."
        ::= { panDeviceLoggingLogTypeStatEntry 5 }

    panDeviceLoggingLogLastSeqNumberFwded OBJECT-TYPE
        SYNTAX      Counter64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Sequence number of the last log that was forwarded."
        ::= { panDeviceLoggingLogTypeStatEntry 6 }

    panDeviceLoggingLogLastSeqNumberAck OBJECT-TYPE
        SYNTAX      Counter64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Sequence number of the last log that was acknowledged."
        ::= { panDeviceLoggingLogTypeStatEntry 7 }

    panDeviceLoggingLogTotalLogsFwded OBJECT-TYPE
        SYNTAX      Counter64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Total number of logs forwarded."
        ::= { panDeviceLoggingLogTypeStatEntry 8 }

    --------------------------------------------------------------------
    -- PanDeviceLoggingLogUsageEntry
    
    panDeviceLoggingLogUsageEntry OBJECT-TYPE
        SYNTAX          PanDeviceLoggingLogUsageEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
            "Entries are created when the panDeviceLoggingLogUsage are added to the panDeviceLoggingLogUsageTable."
    INDEX           { panDeviceLoggingLogUsageLogType }
    ::= { panDeviceLoggingLogUsageTable  1 } 

    PanDeviceLoggingLogUsageEntry ::= SEQUENCE {
        panDeviceLoggingLogUsageLogType              DisplayString,
        panDeviceLoggingDiskUsageDiskSpacePct        FloatValue,
        panDeviceLoggingDiskUsageRetention           Unsigned32,
        panDeviceLoggingDiskQuotaPct                 FloatValue,
        panDeviceLoggingDiskQuota                    FloatValue 
       }

    panDeviceLoggingLogUsageLogType OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Log type for Device. "
        ::= { panDeviceLoggingLogUsageEntry 1 }

    panDeviceLoggingDiskUsageDiskSpacePct OBJECT-TYPE
        SYNTAX      FloatValue
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Disk Usage (MB) for particular log type for Device. "
        ::= { panDeviceLoggingLogUsageEntry 2 }

    panDeviceLoggingDiskUsageRetention OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Log Rentention for particular log type for Device. "
        ::= { panDeviceLoggingLogUsageEntry 3 }
   
    panDeviceLoggingDiskQuotaPct OBJECT-TYPE
        SYNTAX      FloatValue
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Disk Quota percentage for particular log type for Device. "
        ::= { panDeviceLoggingLogUsageEntry 4 }

    panDeviceLoggingDiskQuota OBJECT-TYPE
        SYNTAX      FloatValue
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Disk Quota for particular log type for Device. "
        ::= { panDeviceLoggingLogUsageEntry 5 }

    ----------------------------------------------------------------------
    -- panDeviceLoggingExtFwd

    panDeviceLoggingExtFwdCount OBJECT-TYPE
        SYNTAX      Counter64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Total count for logs forwarded."
        ::= { panDeviceLoggingExtFwd 1 }
 
     panDeviceLoggingExtFwdQueueDrop OBJECT-TYPE
         SYNTAX      Counter64
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "Counter for logs dropped due to queue being full."
         ::= { panDeviceLoggingExtFwd 2 }

    panDeviceLoggingExtFwdStatsSendErr OBJECT-TYPE
        SYNTAX      Counter64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Counter for logs discarded due to sending error."
        ::= { panDeviceLoggingExtFwd 3 }

     panDeviceLoggingExtFwdStatsTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF PanDeviceLoggingExtFwdStatsEntry
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "This table shows the status of logs as they are forwarded via syslog, Traps, email and
             http/https from this Device."
        ::= { panDeviceLoggingExtFwd 4 }

   --------------------------------------------------------------------
   -- panDeviceLoggingExtFwdStatsTable
    panDeviceLoggingExtFwdStatsEntry OBJECT-TYPE
        SYNTAX          PanDeviceLoggingExtFwdStatsEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
            "Entries are created when panDeviceLoggingExtFwdStats are added to panDeviceLoggingExtFwdStatsTable."
    INDEX       { panDeviceLoggingExtFwdStatsTableType }
    ::= { panDeviceLoggingExtFwdStatsTable  1 }

    PanDeviceLoggingExtFwdStatsEntry ::= SEQUENCE {
        panDeviceLoggingExtFwdStatsTableType                 DisplayString,
        panDeviceLoggingExtFwdStatsTableEnqueueCount         Counter64,
        panDeviceLoggingExtFwdStatsTableSendCount            Counter64,
        panDeviceLoggingExtFwdStatsTableDropCount            Counter64,
        panDeviceLoggingExtFwdStatsTableQueueDepth           Counter64,
        panDeviceLoggingExtFwdStatsTable1minAvgSendRate      Unsigned32
    }

     panDeviceLoggingExtFwdStatsTableType OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Name of method used to forward logs."
        ::= { panDeviceLoggingExtFwdStatsEntry 1 }

    panDeviceLoggingExtFwdStatsTableEnqueueCount OBJECT-TYPE
       SYNTAX      Counter64
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "Counter for number of logs enqueued."
       ::= { panDeviceLoggingExtFwdStatsEntry 2 }

    panDeviceLoggingExtFwdStatsTableSendCount OBJECT-TYPE
       SYNTAX      Counter64
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "Counter for number of logs sent."
       ::= { panDeviceLoggingExtFwdStatsEntry 3 }

    panDeviceLoggingExtFwdStatsTableDropCount OBJECT-TYPE
       SYNTAX      Counter64
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "Counter for number of logs dropped."
       ::= { panDeviceLoggingExtFwdStatsEntry 4 }

    panDeviceLoggingExtFwdStatsTableQueueDepth OBJECT-TYPE
       SYNTAX      Counter64
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "Counter for depth of queue."
       ::= { panDeviceLoggingExtFwdStatsEntry 5 }

    panDeviceLoggingExtFwdStatsTable1minAvgSendRate OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
          "Counter for depth of queue."
      ::= { panDeviceLoggingExtFwdStatsEntry 6 }

    -------------------------------------------------------------------
    -- panDeviceLoggingCollectorConnectionTable

    panDeviceLoggingCollectorConnectionEntry    OBJECT-TYPE
        SYNTAX          PanDeviceLoggingCollectorConnectionEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
            "Entries are created when the panDeviceLogging are added to the panDeviceLoggingCollectorConnectionTable."
    INDEX           { panDeviceLoggingCollectorConnectionIP }
    ::= { panDeviceLoggingCollectorConnectionTable  1 }  
    
    PanDeviceLoggingCollectorConnectionEntry  ::= SEQUENCE {
        panDeviceLoggingCollectorConnectionType         DisplayString,
        panDeviceLoggingCollectorConnectionIP           DisplayString,
        panDeviceLoggingCollectorConnectionHostname     DisplayString,
        panDeviceLoggingCollectorConnectionStatus       DisplayString
    }
    
    panDeviceLoggingCollectorConnectionType OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Type of log collection entity (CMS/LC)."
        ::= { panDeviceLoggingCollectorConnectionEntry 1 }

    panDeviceLoggingCollectorConnectionIP OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "IP of log collection entity (CMS/LC) for non-7K and Gryphon.
             Will display connection ID for 7K and Gryphon."
        ::= { panDeviceLoggingCollectorConnectionEntry 2 }

    panDeviceLoggingCollectorConnectionHostname OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Hostname of log collection entity (CMS/LC)."
        ::= { panDeviceLoggingCollectorConnectionEntry 3 }    
    
    panDeviceLoggingCollectorConnectionStatus OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Connection status of log collection entity (CMS/LC)."
        ::= { panDeviceLoggingCollectorConnectionEntry 4 }

	----------------------------------------------------------------------
	-- LogCollector

    panLcStat OBJECT-IDENTITY
        STATUS                  current
        DESCRIPTION             "
            Sub-tree for the Log collection statistics."
        ::= { panLogCollector 1 }

    FloatValue ::= TEXTUAL-CONVENTION
        DISPLAY-HINT  "d-2"
        STATUS         current
        DESCRIPTION
             " This data type is used to represent Float values."
        SYNTAX        OCTET STRING (SIZE(0..64))

	----------------------------------------------------------------------
	-- LogCollector Stats
 
    panLcLogRate OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The write rate in logs/s on the Log Collection"
        ::= { panLcStat 1 }

    panLcLogDuration OBJECT-IDENTITY
        STATUS                  deprecated
        DESCRIPTION             "
            Sub-tree for the Log Duration on the Log Collector. Log
            Duration is Expressed in Days of storage."
        ::= { panLcStat 2 }

    panLcDiskUsageTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF PanLcDiskUsageEntry
        MAX-ACCESS      not-accessible
        STATUS          deprecated
        DESCRIPTION             "
            Sub-tree for the Log Disk Usage on the Log Collector. Log
            Disk Usage is available as MB in use."
        ::= { panLcStat 3 }

    panLcLogUsageTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF PanLcLogUsageEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION             "
            Sub-tree for the Log Usage and data retention on the Log Collector(non localDB). 
            Log Disk Usage is available as MB in use."
        ::= { panLcStat 4 }

    panLocalLogUsageTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF PanLocalLogUsageEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION             "
            Sub-tree for the Log Usage and data retention on the Log Collector(localDB). 
            Log Disk Usage is available as MB in use."
        ::= { panLcStat 5 }

    panLcLogDurationTraffic OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      deprecated
        DESCRIPTION
            "The Log duration (in days) for the traffic logs on the Log Collector"
        ::= { panLcLogDuration 1 }

    panLcLogDurationConfig OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      deprecated
        DESCRIPTION
            "The Log duration (in days) for the config logs on the Log Collector"
        ::= { panLcLogDuration 2 }

    panLcLogDurationSystem OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      deprecated
        DESCRIPTION
            "The Log duration (in days) for the system logs on the Log Collector"
        ::= { panLcLogDuration 3 }

    panLcLogDurationThreat OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      deprecated
        DESCRIPTION
            "The Log duration (in days) for the threat logs on the Log Collector"
        ::= { panLcLogDuration 4 }

    panLcLogDurationAppstat OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      deprecated
        DESCRIPTION
            "The Log duration (in days) for the appstat logs on the Log Collector"
        ::= { panLcLogDuration 5 }

    panLcLogDurationTrsum OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      deprecated
        DESCRIPTION
            "The Log duration (in days) for the trsum logs on the Log Collector"
        ::= { panLcLogDuration 6 }

    panLcLogDurationThsum OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      deprecated
        DESCRIPTION
            "The Log duration (in days) for the thsum logs on the Log Collector"
        ::= { panLcLogDuration 7 }

    panLcLogDurationEvent OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      deprecated
        DESCRIPTION
            "The Log duration (in days) for the event logs on the Log Collector"
        ::= { panLcLogDuration 8 }

    panLcLogDurationAlarm OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      deprecated
        DESCRIPTION
            "The Log duration (in days) for the alarm logs on the Log Collector"
        ::= { panLcLogDuration 9 }

    panLcLogDurationHipmatch OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      deprecated
        DESCRIPTION
            "The Log duration (in days) for the hipmatch logs on the Log Collector"
        ::= { panLcLogDuration 10 }

    panLcLogDurationUserid OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      deprecated
        DESCRIPTION
            "The Log duration (in days) for the userid logs on the Log Collector"
        ::= { panLcLogDuration 11 }

    panLcDiskUsageEntry OBJECT-TYPE
        SYNTAX          PanLcDiskUsageEntry
        MAX-ACCESS      not-accessible
        STATUS          deprecated
        DESCRIPTION
            "Entries are created when the panLcDiskUsage are added to the
            panLcDiskUsageTable."
    INDEX           { panLcDiskUsageId }
    ::= { panLcDiskUsageTable 1 }

    PanLcDiskUsageEntry ::= SEQUENCE {
        panLcDiskUsageId                Integer32,
        panLcDiskUsage                  Unsigned32
       }

    panLocalLogUsageEntry OBJECT-TYPE
        SYNTAX          PanLocalLogUsageEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
            "Entries are created when the panLocalLogUsage are added to the panLocalLogUsageTable."
    INDEX           { panLcLogType }
    ::= { panLocalLogUsageTable  1 }  

    PanLocalLogUsageEntry ::= SEQUENCE {
        panLocalLogType                      DisplayString,
        panLocalDiskUsageDiskSpace           FloatValue,
        panLocalDiskUsageRetention           Unsigned32,
        panLocalDiskQuota                    FloatValue,
        panLocalDiskQuotaPct                 FloatValue
       }    

    panLocalLogType OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Log type for Log Collector. "
        ::= { panLocalLogUsageEntry 1 }

    panLocalDiskUsageDiskSpace OBJECT-TYPE
        SYNTAX      FloatValue
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Disk Usage (in MB) for particular log type for Log Collector. "
        ::= { panLocalLogUsageEntry 2 }

    panLocalDiskUsageRetention OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Log Rentention for particular log type for Log Collector. "
        ::= { panLocalLogUsageEntry 3 }

    panLocalDiskQuota OBJECT-TYPE
        SYNTAX      FloatValue 
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Disk Quota (in GB) for particular log type for Log Collector. "
        ::= { panLocalLogUsageEntry 4 }

    panLocalDiskQuotaPct OBJECT-TYPE
        SYNTAX      FloatValue 
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Disk Quota Percentage for particular log type for Log Collector. "
        ::= { panLocalLogUsageEntry 5 }


    panLcLogUsageEntry OBJECT-TYPE
        SYNTAX          PanLcLogUsageEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
            "Entries are created when the panLcLogUsage are added to the panLcLogUsageTable."
    INDEX           { panLcLogType }
    ::= { panLcLogUsageTable  1 }

    PanLcLogUsageEntry ::= SEQUENCE {
        panLcLogType                      DisplayString,
        panLcDiskUsageDiskSpacePct        FloatValue,
        panLcDiskUsageRetention           Unsigned32,
        panLcDiskQuotaPct                 FloatValue
       }

    panLcLogType OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Log type for Log Collector. "
        ::= { panLcLogUsageEntry 1 }

    panLcDiskUsageDiskSpacePct OBJECT-TYPE
        SYNTAX      FloatValue
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Disk Usage Percentage for particular log type for Log Collector
             aggregated over all disks. "
        ::= { panLcLogUsageEntry 2 }

    panLcDiskUsageRetention OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Log Rentention for particular log type for Log Collector. "
        ::= { panLcLogUsageEntry 3 }
    
    panLcDiskQuotaPct OBJECT-TYPE
        SYNTAX      FloatValue
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Disk Quota Percentage for particular log type for Log Collector
             aggregated over all disks. "
        ::= { panLcLogUsageEntry 4 }
    
    panLcDiskUsageId OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      deprecated
        DESCRIPTION
            "The Log disk id"
        ::= { panLcDiskUsageEntry 1 }

    panLcDiskUsage OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      deprecated
        DESCRIPTION
            "The Log disk usage on the Log Collector"
        ::= { panLcDiskUsageEntry 2 }

    panLcIsRedundancyMember OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "True value indicates this Log Collector is part of a Collector Group with Redundancy is enabled"
        ::= { panLogCollector 2 }

    panLcLogFwdStatsTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF PanLcLogFwdStatsEntry
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "This table shows the status of logs as they are forwarded via syslog, Traps, email and 
             http/https from this Log Collector."
        ::= { panLogCollector 3 }
    ------------------------------------------------------------------
    -- panLcLogFwdStatsTable
        
    panLcLogFwdStatsEntry OBJECT-TYPE
        SYNTAX          PanLcLogFwdStatsEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION    
            "Entries are created when panLcLogFwdStats are added to panLcLogFwdStatsTable."
    INDEX       { panLcLogFwdStatsTableType }
    ::= { panLcLogFwdStatsTable  1 }
    
    PanLcLogFwdStatsEntry ::= SEQUENCE {
        panLcLogFwdStatsTableType             DisplayString,
        panLcLogFwdStatsTableEnqueueCount     Counter64,
        panLcLogFwdStatsTableSendCount        Counter64,
        panLcLogFwdStatsTableDropCount        Counter64,
        panLcLogFwdStatsTableQueueDepth       Counter64
    }

     panLcLogFwdStatsTableType OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Name of method used to forward logs."
        ::= { panLcLogFwdStatsEntry 1 } 

    panLcLogFwdStatsTableEnqueueCount OBJECT-TYPE
       SYNTAX      Counter64
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "Counter for number of logs enqueued."
       ::= { panLcLogFwdStatsEntry 2 } 
    
    panLcLogFwdStatsTableSendCount OBJECT-TYPE
       SYNTAX      Counter64
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "Counter for number of logs sent."
       ::= { panLcLogFwdStatsEntry 3 } 

    panLcLogFwdStatsTableDropCount OBJECT-TYPE
       SYNTAX      Counter64
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "Counter for number of logs dropped."
       ::= { panLcLogFwdStatsEntry 4 } 
    
    panLcLogFwdStatsTableQueueDepth OBJECT-TYPE
       SYNTAX      Counter64
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "Counter for depth of queue."
       ::= { panLcLogFwdStatsEntry 5 } 
  
    -- panLcLoggingConnectedDeviceTable

    panLcLoggingConnectedDeviceTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF PanLcLoggingConnectedDeviceEntry
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "This table shows the details of all devices logging to this Log Collector."
        ::= { panLogCollector 4 }

    panLcLoggingConnectedDeviceEntry OBJECT-TYPE
         SYNTAX          PanLcLoggingConnectedDeviceEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "Entries are created when panLcLoggingConnectedDevice are added to panLcLoggingConnectedDeviceTable."
     INDEX       { panLcLoggingConnectedDeviceConnectionId }
     ::= { panLcLoggingConnectedDeviceTable  1 }

    PanLcLoggingConnectedDeviceEntry ::= SEQUENCE {
         panLcLoggingConnectedDeviceName                DisplayString,
         panLcLoggingConnectedDeviceConnectionId        DisplayString,
         panLcLoggingConnectedIdLogRate                 Unsigned32
     }

    panLcLoggingConnectedDeviceName OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Name of the device being polled."
        ::= { panLcLoggingConnectedDeviceEntry 1 }

    panLcLoggingConnectedDeviceConnectionId OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Connection id of the device being polled."
        ::= { panLcLoggingConnectedDeviceEntry 2 }

    panLcLoggingConnectedIdLogRate OBJECT-TYPE
        SYNTAX      Unsigned32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Logging rate for the connection."
        ::= { panLcLoggingConnectedDeviceEntry 3 }

    -- panLcLoggingDeviceTable 

     panLcLoggingDeviceTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF PanLcLoggingDeviceEntry
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "This table shows the details of logs forwarded by devices logging to this Log Collector."
        ::= { panLogCollector 5 }
     
     panLcLoggingDeviceEntry  OBJECT-TYPE
         SYNTAX          PanLcLoggingDeviceEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "Entries are created when panLcLoggingDevice are added to panLcLoggingDeviceTable."
     INDEX       { panLcLoggingDeviceConnectionId,
                   panLcLoggingLogType }
     ::= { panLcLoggingDeviceTable  1 }

     PanLcLoggingDeviceEntry ::= SEQUENCE {
         panLcLoggingDeviceConnectionId        DisplayString,
         panLcLoggingLogType                   DisplayString,
         panLcLogTypeLastLogRecd               TimeStamp,
         panLcLogTypeLastSeqNumRecd            Counter64,
         panLcLogTypeLastLogGen                TimeStamp
     }
    
    panLcLoggingDeviceConnectionId OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Connection id of the device being polled."
        ::= { panLcLoggingDeviceEntry 1 }

    panLcLoggingLogType OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Log Type of the log being polled."
        ::= { panLcLoggingDeviceEntry 2 }
        
    panLcLogTypeLastLogRecd  OBJECT-TYPE
        SYNTAX      TimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Time at which the last log was received."
        ::= { panLcLoggingDeviceEntry 3 }

    panLcLogTypeLastSeqNumRecd  OBJECT-TYPE
        SYNTAX      Counter64
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Last sequence number received for a type of log."
        ::= { panLcLoggingDeviceEntry 4 }

    panLcLogTypeLastLogGen  OBJECT-TYPE
        SYNTAX      TimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "Time at which the last log was generated."
        ::= { panLcLoggingDeviceEntry 5 }

    ----------------------------------------------------------------------
	-- Events

	panCommonEventObjs OBJECT-IDENTITY
		STATUS					current
		DESCRIPTION				"
			Branch for objects meant only to be sent in event varbinds."
		::= { panCommonEvents 1 }

	panCommonEventEvents OBJECT-IDENTITY
		STATUS					current
		DESCRIPTION				"
			Branch for the events themselves."
		::= { panCommonEvents 2 }

	panCommonEventEventsV2 OBJECT-IDENTITY
		STATUS					current
		DESCRIPTION				"
			Branch for SNMPv2 events. The OIDs for SNMPv2 events should
			have a zero as the next-to-last sub-identifier (as specified
			in RFC1902)."
		::= { panCommonEventEvents 0 }

	-- Objects sent only in events

	panCommonEventDescr OBJECT-TYPE
		SYNTAX					DisplayString
		MAX-ACCESS				accessible-for-notify
		STATUS					current
		DESCRIPTION
			"String that provides a textual description of the event."
		::= { panCommonEventObjs 1 }

	-- Event descriptions

	panCommonEventLog NOTIFICATION-TYPE
		OBJECTS { panCommonEventDescr }
		STATUS  current
		DESCRIPTION
			"A config/system/firewall/threat log"
		::= { panCommonEventEventsV2 1 }

	----------------------------------------------------------------------
	-- GlobalCounters 

	panAhoSw OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"The total usage of software for AHO"
		::= { panGlobalCounters 1 }

	panDfaSw OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"The total number of dfa match using software"
		::= { panGlobalCounters 2 }

	panFlowHostServiceAllow OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Device management session allowed"
		::= { panGlobalCounters 3 }

	panHaPathmonSent OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"HA path-monitoring packets sent"
		::= { panGlobalCounters 4 }
        
	panAhoFpga OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"The total requests to FPGA for AHO"
		::= { panGlobalCounters 5 }

	panDfaFpga OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"The total requests to FPGA for DFA"
		::= { panGlobalCounters 6 }

	panFpgaPkt OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"The packets held because of requests to FPGA"
		::= { panGlobalCounters 7 }

	panGlobalCountersDOSCounters OBJECT-IDENTITY
		STATUS					current
		DESCRIPTION
			"Sub-tree for Global DOS counters"
		::= { panGlobalCounters 8 }

	panGlobalCountersDropCounters OBJECT-IDENTITY
		STATUS					current
		DESCRIPTION
			"Sub-tree for Global Drop counters"
		::= { panGlobalCounters 9 }

	panGlobalCountersIPFragmentationCounters OBJECT-IDENTITY
		STATUS					current
		DESCRIPTION
			"Sub-tree for Global IPFragmentation counters"
		::= { panGlobalCounters 10 }

	panGlobalCountersTCPState OBJECT-IDENTITY
		STATUS					current
		DESCRIPTION
			"Sub-tree for Global TCPState counters"
		::= { panGlobalCounters 11 }

    panGlobalCountersTunnelInspect OBJECT-IDENTITY
        STATUS                  current
        DESCRIPTION
            "Sub-tree for Global Tunnel (GRE, IPSEC and GTP) counters"
        ::= { panGlobalCounters 12 }


	----------------------------------------------------------------------
    -- Global DOS Counters

	panFlowDosAgMaxSessLimit OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Session limit reached for aggregate profile, drop session"
		::= { panGlobalCountersDOSCounters 1 }

	panFlowDosBlkNumEntries OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Number of entries in DOS block table"
		::= { panGlobalCountersDOSCounters 2 }

	panFlowDosClMaxSessLimit OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Session limit reached for classified profile, drop session"
		::= { panGlobalCountersDOSCounters 3 }
        
	panFlowDosClSyncookieAckErr OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"TCP SYN cookies: Invalid ACKs received, classified profile"
		::= { panGlobalCountersDOSCounters 4 }

	panFlowDosClSyncookieAckRcv OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"TCP SYN cookies: ACKs to cookies received, classified profile"
		::= { panGlobalCountersDOSCounters 5 }

	panFlowDosClSyncookieBlkDur OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packets dropped: Flagged for blocking and under block duration for cl"
		::= { panGlobalCountersDOSCounters 6 }

	panFlowDosClSyncookieMax OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packet dropped: SYN cookies maximum threshold reached, classified pro"
		::= { panGlobalCountersDOSCounters 7 }

	panFlowDosClSyncookieSent OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"TCP SYN cookies: cookies sent, classified profile"
		::= { panGlobalCountersDOSCounters 8 }

	panFlowMeterVsysThrottle OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Session metering: sessions throttled by vsys configuration"
		::= { panGlobalCountersDOSCounters 9 }


	panFlowPolicyDeny OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Session setup: denied by policy"
		::= { panGlobalCountersDOSCounters 10 }

	panFlowPolicyNat OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Session setup: source NAT IP/port allocation error"
		::= { panGlobalCountersDOSCounters 11 }

	panFlowScanDrop OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Session setup: denied by scan detection"
		::= { panGlobalCountersDOSCounters 12 }

	panFlowDosDropIpBlocked OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packets dropped: Flagged for blocking and under block duration by oth"
		::= { panGlobalCountersDOSCounters 13 }

	panFlowDosRedIcmp OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packets dropped: Zone protection protocol 'icmp' RED"
		::= { panGlobalCountersDOSCounters 14 }

	panFlowDosRedIcmp6 OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packets dropped: Zone protection protocol 'icmpv6' RED"
		::= { panGlobalCountersDOSCounters 15 }


	panFlowDosRedIp OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packets dropped: Zone protection protocol 'other-ip' RED"
		::= { panGlobalCountersDOSCounters 16 }

	panFlowDosRedTcp OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packets dropped: Zone protection protocol 'tcp-syn' RED"
		::= { panGlobalCountersDOSCounters 17 }

	panFlowDosRedUdp OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packets dropped: Zone protection protocol 'udp' RED"
		::= { panGlobalCountersDOSCounters 18 }

	panFlowDosRuleAgBlkDur OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packets dropped: Flagged for blocking and under block duration for ag"
		::= { panGlobalCountersDOSCounters 19 }

	panFlowDosRuleAgRedAct OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packets dropped: Activate aggregate RED threshold reached, random ear"
		::= { panGlobalCountersDOSCounters 20 }

	panFlowDosRuleAgRedMax OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packets dropped: Maximal aggregate RED threshold reached"
		::= { panGlobalCountersDOSCounters 21 }

	panFlowDosRuleDeny OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packets dropped: Denied action by DoS policy"
		::= { panGlobalCountersDOSCounters 22 }

	panFlowDosRuleDrop OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packets dropped: Rate limited or IP blocked"
		::= { panGlobalCountersDOSCounters 23 }

	panFlowDosRuleDropAggr OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packets dropped: due to aggregate rate limiting"
		::= { panGlobalCountersDOSCounters 24 }

	panFlowDosRuleDropClBlkDur OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packets dropped: Flagged for blocking and under block duration for cl"
		::= { panGlobalCountersDOSCounters 25 }

	panFlowDosRuleDropClRedAct OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packets dropped: Activate classified RED threshold reached, random ea"
		::= { panGlobalCountersDOSCounters 26 }

	panFlowDosRuleDropClRedMax OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packets dropped: Maximal classified RED threshold reached"
		::= { panGlobalCountersDOSCounters 27 }

	panFlowDosRuleDropClassified OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packets dropped: due to classified rate limiting"
		::= { panGlobalCountersDOSCounters 28 }

	panFlowDosSyncookieBlkDur OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packets dropped: Flagged for blocking and under block duration for ag"
		::= { panGlobalCountersDOSCounters 29 }

	panFlowDosSyncookieMax OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packet dropped: SYN cookies maximum threshold reached, aggregate prof"
		::= { panGlobalCountersDOSCounters 30 }

	panFlowDosZoneRedAct OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packets dropped: Activate zone RED threshold reached, random early dr"
		::= { panGlobalCountersDOSCounters 31 }

	panFlowDosZoneRedMax OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packets dropped: Maximal zone RED threshold reached"
		::= { panGlobalCountersDOSCounters 32 }
        
    panFlowDosBlkSwEntries OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
        STATUS					current
        DESCRIPTION
            "Number of entries in DOS Software block table"
        ::= { panGlobalCountersDOSCounters 33 }
    
    panFlowDosBlkHwEntries OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
        STATUS                  current
        DESCRIPTION
            "Number of entries in DOS Hardware block table"
        ::= { panGlobalCountersDOSCounters 34 } 


 -------------------------------------------------------------------------------------------------------
 -- Pan Global Drop Counters

	panFlowFwdL3TtlZero OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packets dropped: IP TTL reaches zero"
		::= { panGlobalCountersDropCounters 1 }

	panFlowMeterHostThrottle OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Session metering: sessions throttled by management session threshold"
		::= { panGlobalCountersDropCounters 2 }

	panFlowHostServiceDeny OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Device management session denied"
		::= { panGlobalCountersDropCounters 3 }
        
	panFlowHostServiceUnknown OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Session discarded: unknown application to control plane"
		::= { panGlobalCountersDropCounters 4 }

	panPktAllocFailure OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packet allocation error"
		::= { panGlobalCountersDropCounters 5 }

	panPktAllocFailureCos OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packet allocation error due to QoS control"
		::= { panGlobalCountersDropCounters 6 }

	panSessionDiscard OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Session set to discard by security policy check"
		::= { panGlobalCountersDropCounters 7 }

 ------------------------------------------------------------------------------------------------------
 -- Pan Global IPFragmentation Counters

	panFlowIpfragFragErr OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Packet dropped: IP fragmentation error"
		::= { panGlobalCountersIPFragmentationCounters 1 }

	panFlowIpfragRecv OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"IP fragments received"
		::= { panGlobalCountersIPFragmentationCounters 2 }

------------------------------------------------------------------------------------------------------
-- Pan Global TCP State Counters

	panTcpAllocWqeFailed OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"wqe allocation failure in tcp"
		::= { panGlobalCountersTCPState 1 }

	panTcpDeny OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"session denied because of failure in tcp reassembly"
		::= { panGlobalCountersTCPState 2 }

	panTcpDropOutOfWnd OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"out-of-window packets dropped"
		::= { panGlobalCountersTCPState 3 }
        
	panTcpDropPacket OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"packets dropped because of failure in tcp reassembly"
		::= { panGlobalCountersTCPState 4 }

	panFlowActionClose OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"TCP sessions closed via injecting RST"
		::= { panGlobalCountersTCPState 5 }

	panFlowActionReset OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"TCP clients reset via responding RST"
		::= { panGlobalCountersTCPState 6 }

	panFlowTcpNonSyn OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"Non-SYN TCP packets without session match"
		::= { panGlobalCountersTCPState 7 }


	panTcpExceedSegLimit OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
		STATUS					current
		DESCRIPTION
			"packets dropped due to the limitation on global tcp out-of-order pack"
		::= { panGlobalCountersTCPState 8 }

    ------------------------------------------------------------------------------------------------------
    -- Pan Global Tunnel State Counters

    panFlowTciGreDecapSuccess OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
        STATUS                  current
        DESCRIPTION
            "Total GRE sessions tunnel inspected"
        ::= { panGlobalCountersTunnelInspect 1 }
    
    panFlowTciGreDecapFailed OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
        STATUS                  current
        DESCRIPTION
            "Total GRE sessions for failed tunnel inspected"
        ::= { panGlobalCountersTunnelInspect 2 }

    panFlowTciGreDecapUnknown OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
        STATUS                  current
        DESCRIPTION
            "Total unknown tunnel inspection packets in GRE tunnel [passed|dropped]"
        ::= { panGlobalCountersTunnelInspect 3 }

    panFlowTciIpsecDecapSuccess OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
        STATUS                  current
        DESCRIPTION
            "Total Ipsec sessions tunnel inspected"
        ::= { panGlobalCountersTunnelInspect 4 }

    panFlowTciIpsecDecapFailed OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
        STATUS                  current
        DESCRIPTION
            "Total IPSEC sessions for failed tunnel inspected"
        ::= { panGlobalCountersTunnelInspect 5 }

    panFlowTciIpsecDecapUnknown OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
        STATUS                  current
        DESCRIPTION
            "Total unknown tunnel inspection packets in IPSEC tunnel [passed|dropped]"
        ::= { panGlobalCountersTunnelInspect 6 }

    panFlowTciGtpDecapSuccess OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
        STATUS                  current
        DESCRIPTION
            "Total GTP sessions tunnel inspected"
        ::= { panGlobalCountersTunnelInspect 7 }

    panFlowTciGtpDecapFailed OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
        STATUS                  current
        DESCRIPTION
            "Total GTP sessions for failed tunnel inspected"
        ::= { panGlobalCountersTunnelInspect 8 }

    panFlowTciGtpDecapUnknown OBJECT-TYPE
        SYNTAX                  Counter64
        MAX-ACCESS              read-only
        STATUS                  current
        DESCRIPTION
            "Total unknown tunnel inspection packets in GTP tunnel[passed|dropped]"
        ::= { panGlobalCountersTunnelInspect 9 }

    ---------------------------------------------------------------
    -- panIfTable

    panIfEntry OBJECT-TYPE
        SYNTAX          PanIfEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
            "Entries are created when panIfCPS are added to the panIfCPSTable."
    INDEX           { ifIndex  }
    ::= { panIfTable 1 }

    PanIfEntry  ::= SEQUENCE {
        ifIndex                 Unsigned32,
        ifDescr                 DisplayString,
        panIfActiveTcpCps       Unsigned32,
        panIfActiveUdpCps       Unsigned32,
        panIfActiveOtherIpCps   Unsigned32
    }

    ifIndex OBJECT-TYPE
        SYNTAX              Unsigned32
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION
            "Index of the interface"
        ::= { panIfEntry 1 }
    
    ifDescr OBJECT-TYPE
        SYNTAX              DisplayString
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION
            "Description (name) of the interface"
        ::= { panIfEntry 2 }
    
    panIfActiveTcpCps OBJECT-TYPE
        SYNTAX              Unsigned32
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION
            "Number of active TCP connections per second for this interface."
        ::= { panIfEntry 3 }
    
    panIfActiveUdpCps OBJECT-TYPE
        SYNTAX              Unsigned32
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION
            "Number of active UDP connections per second for this interface."
        ::= { panIfEntry 4 }
    
    panIfActiveOtherIpCps OBJECT-TYPE
        SYNTAX              Unsigned32
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION
            "Number of active Other IP connections per second for this interface."
        ::= { panIfEntry 5 }
    
   ---------------------------------------------------------------
    -- panZoneTable

    panZoneEntry OBJECT-TYPE
        SYNTAX          PanZoneEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
            "Entries are created when panZoneCPS are added to the panZoneCPSTable."
    INDEX           { ifIndex  }
    ::= { panZoneTable 1 }

    PanZoneEntry  ::= SEQUENCE {
        panZoneName               DisplayString,
        panZoneActiveTcpCps       Unsigned32,
        panZoneActiveUdpCps       Unsigned32,
        panZoneActiveOtherIpCps   Unsigned32
    }

    panZoneName OBJECT-TYPE
        SYNTAX              DisplayString
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION
            "Zone name for the interface"
        ::= { panZoneEntry 1 }

    panZoneActiveTcpCps OBJECT-TYPE
        SYNTAX              Unsigned32
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION
            "Number of active TCP connections per second for this zone."
        ::= { panZoneEntry 2 }

    panZoneActiveUdpCps OBJECT-TYPE
        SYNTAX              Unsigned32
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION
            "Number of active UDP connections per second for this zone."
        ::= { panZoneEntry 3 }

    panZoneActiveOtherIpCps OBJECT-TYPE
        SYNTAX              Unsigned32
        MAX-ACCESS          read-only
        STATUS              current
        DESCRIPTION
            "Number of active Other IP connections per second for this zone."
        ::= { panZoneEntry 4 }
    

--------------------------------------------------------------------------------------------------------
END
