MIKROTIK-MIB DEFINITIONS ::= BEGIN

IMPORTS
MODULE-IDENTITY, OBJECT-TYPE, Integer32, Counter32, Gauge32, IpAddress,
Counter64, enterprises, NOTIFICATION-TYPE FROM SNMPv2-SMI
TEXTUAL-CONVENTION, DisplayString, MacAddress, DateAndTime FROM SNMPv2-TC
TimeTicks FROM SNMPv2-SMI
OBJECT-GROUP FROM SNMPv2-CONF
NOTIFICATION-GROUP FROM SNMPv2-CONF;

mikrotikExperimentalModule MODULE-IDENTITY
  LAST-UPDATED "201404100000Z"
  ORGANIZATION "MikroTik"
  CONTACT-INFO "@mikrotik.com"
  DESCRIPTION ""
  REVISION "201404100000Z"
  DESCRIPTION ""
  ::= { mikrotik 1 }

mikrotik OBJECT IDENTIFIER ::= { enterprises 14988 }
mtXMetaInfo OBJECT IDENTIFIER ::= { mikrotikExperimentalModule 2 }
mtXRouterOsGroups OBJECT IDENTIFIER ::= { mtXMetaInfo 1 }

mtXRouterOs OBJECT IDENTIFIER ::= { mikrotikExperimentalModule 1 }
mtxrWireless OBJECT IDENTIFIER ::= { mtXRouterOs 1 }
mtxrQueues OBJECT IDENTIFIER ::= { mtXRouterOs 2 }
mtxrHealth OBJECT IDENTIFIER ::= { mtXRouterOs 3 }
mtxrLicense OBJECT IDENTIFIER ::= { mtXRouterOs 4 }
mtxrHotspot OBJECT IDENTIFIER ::= { mtXRouterOs 5 }
mtxrDHCP OBJECT IDENTIFIER ::= { mtXRouterOs 6 }
mtxrSystem OBJECT IDENTIFIER ::= { mtXRouterOs 7 }
mtxrScripts OBJECT IDENTIFIER ::= { mtXRouterOs 8 }
mtxrTraps OBJECT IDENTIFIER ::= { mtXRouterOs 9 }
mtxrNstremeDual OBJECT IDENTIFIER ::= { mtXRouterOs 10 }
mtxrNeighbor OBJECT IDENTIFIER ::= { mtXRouterOs 11 }
mtxrGps OBJECT IDENTIFIER ::= { mtXRouterOs 12 }
mtxrWirelessModem OBJECT IDENTIFIER ::= { mtXRouterOs 13 }
mtxrInterfaceStats OBJECT IDENTIFIER ::= { mtXRouterOs 14 }
mtxrPOE OBJECT IDENTIFIER ::= { mtXRouterOs 15 }
mtxrLTEModem OBJECT IDENTIFIER ::= { mtXRouterOs 16 }

ObjectIndex ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "x"
    STATUS current
    DESCRIPTION "Internal "
    SYNTAX Integer32 (0..2147483647)
-- Note that actually in RouterOs index values can be in range 0..4294967294,
-- this can sometimes make them negative. Any of the following syntaxes would
-- be more appropriate, but since Integer32 is used for InterfaceIndex in
-- IF-MIB, where it can also take negative values in RouterOs, it is used
-- here for consistency.
-- Also note that ObjectIndex value is not related to item numbers that are
-- used by console and shown by console print command.
--
-- SYNTAX Integer32 (-2147483648..2147483647)
-- SYNTAX Unsigned32 (0..4294967295)

Voltage ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d-1"
    STATUS current
    DESCRIPTION ""
    SYNTAX Integer32 (-2147483648..2147483647)

Temperature ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d-1"
    STATUS current
    DESCRIPTION ""
    SYNTAX Integer32 (-2147483648..2147483647)

Power ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d-1"
    STATUS current
    DESCRIPTION ""
    SYNTAX Integer32 (-2147483648..2147483647)


mtxrWlStatTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrWlStatEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWireless 1 }

mtxrWlStatEntry OBJECT-TYPE
    SYNTAX MtxrWlStatEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "Wireless station mode interface"
    INDEX { mtxrWlStatIndex }
    ::= { mtxrWlStatTable 1 }

MtxrWlStatEntry ::= SEQUENCE {
    mtxrWlStatIndex ObjectIndex,
    mtxrWlStatTxRate Gauge32,
    mtxrWlStatRxRate Gauge32,
    mtxrWlStatStrength Integer32,
    mtxrWlStatSsid DisplayString,
    mtxrWlStatBssid MacAddress,
    mtxrWlStatFreq Integer32,
    mtxrWlStatBand DisplayString
}

mtxrWlStatIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlStatEntry 1 }

mtxrWlStatTxRate OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "bits per second"
    ::= { mtxrWlStatEntry 2 }

mtxrWlStatRxRate OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "bits per second"
    ::= { mtxrWlStatEntry 3 }

mtxrWlStatStrength OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "dBm"
    ::= { mtxrWlStatEntry 4 }

mtxrWlStatSsid OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlStatEntry 5 }

mtxrWlStatBssid OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlStatEntry 6 }

mtxrWlStatFreq OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "megahertz"
    ::= { mtxrWlStatEntry 7 }

mtxrWlStatBand OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlStatEntry 8 }

mtxrWlRtabTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrWlRtabEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWireless 2 }

mtxrWlRtabEntry OBJECT-TYPE
    SYNTAX MtxrWlRtabEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "Wireless registration table. It is indexed by remote
        mac-address and local interface index"
    INDEX { mtxrWlRtabAddr, mtxrWlRtabIface }
    ::= { mtxrWlRtabTable 1 }

MtxrWlRtabEntry ::= SEQUENCE {
    mtxrWlRtabAddr MacAddress,
    mtxrWlRtabIface ObjectIndex,
    mtxrWlRtabStrength Integer32,
    mtxrWlRtabTxBytes Counter32,
    mtxrWlRtabRxBytes Counter32,
    mtxrWlRtabTxPackets Counter32,
    mtxrWlRtabRxPackets Counter32,
    mtxrWlRtabTxRate Gauge32,
    mtxrWlRtabRxRate Gauge32,
    mtxrWlRtabRouterOSVersion DisplayString,
    mtxrWlRtabUptime TimeTicks,
    mtxrWlRtabSignalToNoise Integer32,
    mtxrWlRtabTxStrengthCh0 Integer32,
    mtxrWlRtabRxStrengthCh0 Integer32,
    mtxrWlRtabTxStrengthCh1 Integer32,
    mtxrWlRtabRxStrengthCh1 Integer32,
    mtxrWlRtabTxStrengthCh2 Integer32,
    mtxrWlRtabRxStrengthCh2 Integer32
}

mtxrWlRtabAddr OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 1 }

mtxrWlRtabIface OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 2 }

mtxrWlRtabStrength OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "dBm"
    ::= { mtxrWlRtabEntry 3 }

mtxrWlRtabTxBytes OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 4 }

mtxrWlRtabRxBytes OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 5 }

mtxrWlRtabTxPackets OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 6 }

mtxrWlRtabRxPackets OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 7 }

mtxrWlRtabTxRate OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "bits per second"
    ::= { mtxrWlRtabEntry 8 }

mtxrWlRtabRxRate OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "bits per second"
    ::= { mtxrWlRtabEntry 9 }

mtxrWlRtabRouterOSVersion OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "RouterOS version"
    ::= { mtxrWlRtabEntry 10 }

mtxrWlRtabUptime OBJECT-TYPE
    SYNTAX TimeTicks
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "uptime"
    ::= { mtxrWlRtabEntry 11 }

mtxrWlRtabSignalToNoise OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Measured in dB, if value does not exist it is indicated with 0"
    ::= { mtxrWlRtabEntry 12 }

mtxrWlRtabTxStrengthCh0 OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 13 }

mtxrWlRtabRxStrengthCh0 OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 14 }

mtxrWlRtabTxStrengthCh1 OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 15 }

mtxrWlRtabRxStrengthCh1 OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 16 }

mtxrWlRtabTxStrengthCh2 OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 17 }

mtxrWlRtabRxStrengthCh2 OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlRtabEntry 18 }

mtxrWlRtabEntryCount OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Wireless registration table entry count"
    ::= { mtxrWireless 4 }

mtxrWlApTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrWlApEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWireless 3 }

mtxrWlApEntry OBJECT-TYPE
    SYNTAX MtxrWlApEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "Wireless access point mode interface"
    INDEX { mtxrWlApIndex }
    ::= { mtxrWlApTable 1 }

MtxrWlApEntry ::= SEQUENCE {
    mtxrWlApIndex ObjectIndex,
    mtxrWlApTxRate Gauge32,
    mtxrWlApRxRate Gauge32,
    mtxrWlApSsid DisplayString,
    mtxrWlApBssid MacAddress,
    mtxrWlApClientCount Counter32,
    mtxrWlApFreq Integer32,
    mtxrWlApBand DisplayString,
    mtxrWlApNoiseFloor Integer32,
    mtxrWlApOverallTxCCQ Counter32,
    mtxrWlApAuthClientCount Counter32
}

mtxrWlApIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlApEntry 1 }

mtxrWlApTxRate OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "bits per second"
    ::= { mtxrWlApEntry 2 }

mtxrWlApRxRate OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "bits per second"
    ::= { mtxrWlApEntry 3 }

mtxrWlApSsid OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlApEntry 4 }

mtxrWlApBssid OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlApEntry 5 }

mtxrWlApClientCount OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlApEntry 6 }

mtxrWlApFreq OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "megahertz"
    ::= { mtxrWlApEntry 7 }

mtxrWlApBand OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlApEntry 8 }

mtxrWlApNoiseFloor OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlApEntry 9 }

mtxrWlApOverallTxCCQ OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlApEntry 10 }

mtxrWlApAuthClientCount OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrWlApEntry 11 }

mtxrQueueSimpleTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrQueueSimpleEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueues 1 }

mtxrQueueSimpleEntry OBJECT-TYPE
    SYNTAX MtxrQueueSimpleEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "Simple queue"
    INDEX { mtxrQueueSimpleIndex }
    ::= { mtxrQueueSimpleTable 1 }

MtxrQueueSimpleEntry ::= SEQUENCE {
    mtxrQueueSimpleIndex ObjectIndex,
    mtxrQueueSimpleName DisplayString,
    mtxrQueueSimpleSrcAddr IpAddress,
    mtxrQueueSimpleSrcMask IpAddress,
    mtxrQueueSimpleDstAddr IpAddress,
    mtxrQueueSimpleDstMask IpAddress,
    mtxrQueueSimpleIface ObjectIndex,
    mtxrQueueSimpleBytesIn Counter64,
    mtxrQueueSimpleBytesOut Counter64,
    mtxrQueueSimplePacketsIn Counter32,
    mtxrQueueSimplePacketsOut Counter32,
    mtxrQueueSimplePCQQueuesIn Counter32,
    mtxrQueueSimplePCQQueuesOut Counter32,
    mtxrQueueSimpleDroppedIn Counter32,
    mtxrQueueSimpleDroppedOut Counter32
}

mtxrQueueSimpleIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 1 }

mtxrQueueSimpleName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 2 }

mtxrQueueSimpleSrcAddr OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 3 }

mtxrQueueSimpleSrcMask OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 4 }

mtxrQueueSimpleDstAddr OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 5 }

mtxrQueueSimpleDstMask OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 6 }

mtxrQueueSimpleIface OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "interface index"
    ::= { mtxrQueueSimpleEntry 7 }

mtxrQueueSimpleBytesIn OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 8 }

mtxrQueueSimpleBytesOut OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 9 }

mtxrQueueSimplePacketsIn OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 10 }

mtxrQueueSimplePacketsOut OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 11 }

mtxrQueueSimplePCQQueuesIn OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 12 }

mtxrQueueSimplePCQQueuesOut OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 13 }

mtxrQueueSimpleDroppedIn OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 14 }

mtxrQueueSimpleDroppedOut OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueSimpleEntry 15 }

mtxrQueueTreeTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrQueueTreeEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueues 2 }

mtxrQueueTreeEntry OBJECT-TYPE
    SYNTAX MtxrQueueTreeEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "Tree queue"
    INDEX { mtxrQueueTreeIndex }
    ::= { mtxrQueueTreeTable 1 }

MtxrQueueTreeEntry ::= SEQUENCE {
    mtxrQueueTreeIndex ObjectIndex,
    mtxrQueueTreeName DisplayString,
    mtxrQueueTreeFlow DisplayString,
    mtxrQueueTreeParentIndex ObjectIndex,
    mtxrQueueTreeBytes Counter32,
    mtxrQueueTreePackets Counter32,
    mtxrQueueTreeHCBytes Counter64,
    mtxrQueueTreePCQQueues Counter32,
    mtxrQueueTreeDropped Counter32
}

mtxrQueueTreeIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueTreeEntry 1 }

mtxrQueueTreeName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueTreeEntry 2 }

mtxrQueueTreeFlow OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "flowmark"
    ::= { mtxrQueueTreeEntry 3 }

mtxrQueueTreeParentIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "index of parent tree queue or parent interface"
    ::= { mtxrQueueTreeEntry 4 }

mtxrQueueTreeBytes OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueTreeEntry 5 }

mtxrQueueTreePackets OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueTreeEntry 6 }

mtxrQueueTreeHCBytes OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueTreeEntry 7 }

mtxrQueueTreePCQQueues OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueTreeEntry 8 }

mtxrQueueTreeDropped OBJECT-TYPE
    SYNTAX Counter32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrQueueTreeEntry 9 }

mtxrHlCoreVoltage OBJECT-TYPE
    SYNTAX Voltage
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "core voltage"
    ::= { mtxrHealth 1 }

mtxrHlThreeDotThreeVoltage OBJECT-TYPE
    SYNTAX Voltage
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "3.3V voltage"
    ::= { mtxrHealth 2 }

mtxrHlFiveVoltage OBJECT-TYPE
    SYNTAX Voltage
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "5V voltage"
    ::= { mtxrHealth 3 }

mtxrHlTwelveVoltage OBJECT-TYPE
    SYNTAX Voltage
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "12V voltage"
    ::= { mtxrHealth 4 }

mtxrHlSensorTemperature OBJECT-TYPE
    SYNTAX Temperature
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "temperature at sensor chip"
    ::= { mtxrHealth 5 }

mtxrHlCpuTemperature OBJECT-TYPE
    SYNTAX Temperature
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "temperature near cpu"
    ::= { mtxrHealth 6 }

mtxrHlBoardTemperature OBJECT-TYPE
    SYNTAX Temperature
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHealth 7 }

mtxrHlVoltage OBJECT-TYPE
    SYNTAX Voltage
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHealth 8 }

mtxrHlActiveFan OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHealth 9 }

mtxrHlTemperature OBJECT-TYPE
    SYNTAX Temperature
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHealth 10 }

mtxrHlProcessorTemperature OBJECT-TYPE
    SYNTAX Temperature
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHealth 11 }

mtxrHlPower OBJECT-TYPE
    SYNTAX Power
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Watts"
    ::= { mtxrHealth 12 }

mtxrHlCurrent OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "mA"
    ::= { mtxrHealth 13 }

mtxrHlProcessorFrequency OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Mhz"
    ::= { mtxrHealth 14 }

mtxrLicSoftwareId OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "software id"
    ::= { mtxrLicense 1 }

mtxrLicUpgrUntil OBJECT-TYPE
    SYNTAX DateAndTime
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "current key allows upgrading until this date"
    ::= { mtxrLicense 2 }

mtxrLicLevel OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "current key level"
    ::= { mtxrLicense 3 }

mtxrLicVersion OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "software version"
    ::= { mtxrLicense 4 }

mtxrLicUpgradableTo OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "upgradable to"
    ::= { mtxrLicense 5 }

-- ACTIVE USERS ***************************************************************

mtxrHotspotActiveUsersTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrHotspotActiveUsersTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspot 1 }

mtxrHotspotActiveUsersTableEntry OBJECT-TYPE
    SYNTAX MtxrHotspotActiveUsersTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    INDEX { mtxrHotspotActiveUserIndex }
    ::= { mtxrHotspotActiveUsersTable 1 }

MtxrHotspotActiveUsersTableEntry ::= SEQUENCE {
	mtxrHotspotActiveUserIndex ObjectIndex,
	mtxrHotspotActiveUserServerID Integer32,
	mtxrHotspotActiveUserName DisplayString,
	mtxrHotspotActiveUserDomain DisplayString,
	mtxrHotspotActiveUserIP IpAddress,
	mtxrHotspotActiveUserMAC MacAddress,
	mtxrHotspotActiveUserConnectTime Integer32,
	mtxrHotspotActiveUserValidTillTime Integer32,
	mtxrHotspotActiveUserIdleStartTime Integer32,
	mtxrHotspotActiveUserIdleTimeout Integer32,
	mtxrHotspotActiveUserPingTimeout Integer32,
	mtxrHotspotActiveUserBytesIn Counter64,
	mtxrHotspotActiveUserBytesOut Counter64,
	mtxrHotspotActiveUserPacketsIn Counter64,
	mtxrHotspotActiveUserPacketsOut Counter64,
	mtxrHotspotActiveUserLimitBytesIn Counter64,
	mtxrHotspotActiveUserLimitBytesOut Counter64,
	mtxrHotspotActiveUserAdvertStatus Integer32,
	mtxrHotspotActiveUserRadius Integer32,
	mtxrHotspotActiveUserBlockedByAdvert Integer32
}

mtxrHotspotActiveUserIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 1 }

mtxrHotspotActiveUserServerID OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 2 }

mtxrHotspotActiveUserName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 3 }

mtxrHotspotActiveUserDomain OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 4 }

mtxrHotspotActiveUserIP OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 5 }

mtxrHotspotActiveUserMAC OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 6 }

mtxrHotspotActiveUserConnectTime OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 7 }

mtxrHotspotActiveUserValidTillTime OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 8 }

mtxrHotspotActiveUserIdleStartTime OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 9 }

mtxrHotspotActiveUserIdleTimeout OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 10 }

mtxrHotspotActiveUserPingTimeout OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 11 }

mtxrHotspotActiveUserBytesIn OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 12 }

mtxrHotspotActiveUserBytesOut OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 13 }

mtxrHotspotActiveUserPacketsIn OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 14 }

mtxrHotspotActiveUserPacketsOut OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 15 }

mtxrHotspotActiveUserLimitBytesIn OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 16 }

mtxrHotspotActiveUserLimitBytesOut OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 17 }

mtxrHotspotActiveUserAdvertStatus OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 18 }

mtxrHotspotActiveUserRadius OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 19 }

mtxrHotspotActiveUserBlockedByAdvert OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrHotspotActiveUsersTableEntry 20 }

mtxrDHCPLeaseCount OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrDHCP 1 }

-- SYSTEM ********************************************************************

mtxrSystemReboot OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION "set non zero to reboot"
    ::= { mtxrSystem 1 }

mtxrUSBPowerReset OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION "switches off usb power for specified amout of seconds"
    ::= { mtxrSystem 2 }

mtxrSerialNumber OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "RouterBOARD serial number"
    ::= { mtxrSystem 3 }

mtxrFirmwareVersion OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "Current firmware version"
    ::= { mtxrSystem 4 }

-- SCRIPTS ********************************************************************

mtxrScriptTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrScriptTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrScripts 1 }

mtxrScriptTableEntry OBJECT-TYPE
    SYNTAX MtxrScriptTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    INDEX { mtxrScriptIndex }
    ::= { mtxrScriptTable 1 }

MtxrScriptTableEntry ::= SEQUENCE {
	mtxrScriptIndex ObjectIndex,
	mtxrScriptName DisplayString,
	mtxrScriptRunCmd Integer32
}

mtxrScriptIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrScriptTableEntry 1 }

mtxrScriptName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrScriptTableEntry 2 }

mtxrScriptRunCmd OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION "set non zero to run"
    ::= { mtxrScriptTableEntry 3 }

-- Dual Nstreme ***************************************************************

mtxrDnStatTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrDnStatEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrNstremeDual 1 }

mtxrDnStatEntry OBJECT-TYPE
    SYNTAX MtxrDnStatEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "Nstreme Dual interface"
    INDEX { mtxrDnStatIndex }
    ::= { mtxrDnStatTable 1 }

MtxrDnStatEntry ::= SEQUENCE {
    mtxrDnStatIndex ObjectIndex,
    mtxrDnStatTxRate Gauge32,
    mtxrDnStatRxRate Gauge32,
    mtxrDnStatTxStrength Integer32,
    mtxrDnStatRxStrength Integer32,
    mtxrDnConnected Integer32
}	

mtxrDnStatIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrDnStatEntry 1 }

mtxrDnStatTxRate OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "bits per second"
    ::= { mtxrDnStatEntry 2 }

mtxrDnStatRxRate OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "bits per second"
    ::= { mtxrDnStatEntry 3 }

mtxrDnStatTxStrength OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "dBm"
    ::= { mtxrDnStatEntry 4 }

mtxrDnStatRxStrength OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "dBm"
    ::= { mtxrDnStatEntry 5 }

mtxrDnConnected OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "0 - not connected, connected otherwise"
    ::= { mtxrDnStatEntry 6 }

-- NEIGHBOR *******************************************************************

mtxrNeighborTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrNeighborTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrNeighbor 1 }

mtxrNeighborTableEntry OBJECT-TYPE
    SYNTAX MtxrNeighborTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    INDEX { mtxrNeighborIndex }
    ::= { mtxrNeighborTable 1 }

MtxrNeighborTableEntry ::= SEQUENCE {
	mtxrNeighborIndex ObjectIndex,
	mtxrNeighborIpAddress IpAddress,
	mtxrNeighborMacAddress MacAddress,
	mtxrNeighborVersion DisplayString,
	mtxrNeighborPlatform DisplayString,
	mtxrNeighborIdentity DisplayString,
	mtxrNeighborSoftwareID DisplayString,
        mtxrNeighborInterfaceID ObjectIndex
}

mtxrNeighborIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrNeighborTableEntry 1 }

mtxrNeighborIpAddress OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrNeighborTableEntry 2 }

mtxrNeighborMacAddress OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrNeighborTableEntry 3 }

mtxrNeighborVersion OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrNeighborTableEntry 4 }

mtxrNeighborPlatform OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrNeighborTableEntry 5 }

mtxrNeighborIdentity OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrNeighborTableEntry 6 }

mtxrNeighborSoftwareID OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrNeighborTableEntry 7 }

mtxrNeighborInterfaceID OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrNeighborTableEntry 8 }

-- GROUPS *********************************************************************

mtxrWirelessGroup OBJECT-GROUP OBJECTS {
        mtxrWlStatTxRate,
	mtxrWlStatRxRate,
	mtxrWlStatStrength,
	mtxrWlStatSsid,
        mtxrWlStatBssid,
	mtxrWlStatFreq,
	mtxrWlStatBand,
	mtxrWlRtabStrength,
	mtxrWlRtabTxBytes,
        mtxrWlRtabRxBytes,
	mtxrWlRtabTxPackets,
	mtxrWlRtabRxPackets,
        mtxrWlRtabTxRate,
	mtxrWlRtabRxRate,
	mtxrWlRtabEntryCount,
        mtxrWlRtabRouterOSVersion,
        mtxrWlRtabUptime,
        mtxrWlRtabSignalToNoise,
        mtxrWlRtabTxStrengthCh0,
        mtxrWlRtabRxStrengthCh0,
        mtxrWlRtabTxStrengthCh1,
        mtxrWlRtabRxStrengthCh1,
        mtxrWlRtabTxStrengthCh2,
        mtxrWlRtabRxStrengthCh2,
        mtxrWlApTxRate,
	mtxrWlApRxRate,
	mtxrWlApSsid,
        mtxrWlApBssid,
        mtxrWlApClientCount,
        mtxrWlApBand,
        mtxrWlApFreq,
        mtxrWlApNoiseFloor,
        mtxrWlApOverallTxCCQ,
        mtxrWlApAuthClientCount
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 1 }

mtxrQueueGroup OBJECT-GROUP OBJECTS {
        mtxrQueueSimpleName, mtxrQueueSimpleSrcAddr, mtxrQueueSimpleSrcMask,
        mtxrQueueSimpleDstAddr, mtxrQueueSimpleDstMask, mtxrQueueSimpleIface,
        mtxrQueueSimpleBytesIn, mtxrQueueSimpleBytesOut,
        mtxrQueueSimplePacketsIn, mtxrQueueSimplePacketsOut, mtxrQueueTreeName,
        mtxrQueueSimplePCQQueuesIn,
        mtxrQueueSimplePCQQueuesOut,
        mtxrQueueSimpleDroppedIn,
        mtxrQueueSimpleDroppedOut,
        mtxrQueueTreeFlow, mtxrQueueTreeParentIndex, mtxrQueueTreeBytes,
        mtxrQueueTreePackets,
        mtxrQueueTreeHCBytes,
        mtxrQueueTreePCQQueues,
        mtxrQueueTreeDropped
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 2 }

mtxrHealthGroup OBJECT-GROUP OBJECTS {
        mtxrHlCoreVoltage, mtxrHlThreeDotThreeVoltage, mtxrHlFiveVoltage,
        mtxrHlTwelveVoltage, mtxrHlSensorTemperature, mtxrHlCpuTemperature,
        mtxrHlBoardTemperature, mtxrHlVoltage, mtxrHlActiveFan, 
	mtxrHlTemperature, mtxrHlProcessorTemperature,
        mtxrHlCurrent, mtxrHlPower,
        mtxrHlProcessorFrequency
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 3 }

mtxrLincenseGroup OBJECT-GROUP OBJECTS {
        mtxrLicSoftwareId, mtxrLicUpgrUntil, mtxrLicLevel, mtxrLicVersion, mtxrLicUpgradableTo
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 4 }

mtxrHotspotActiveUserGroup OBJECT-GROUP OBJECTS {
	mtxrHotspotActiveUserServerID,
	mtxrHotspotActiveUserName,
	mtxrHotspotActiveUserDomain,
	mtxrHotspotActiveUserIP,
	mtxrHotspotActiveUserMAC,
	mtxrHotspotActiveUserConnectTime,
	mtxrHotspotActiveUserValidTillTime,
	mtxrHotspotActiveUserIdleStartTime,
	mtxrHotspotActiveUserIdleTimeout,
	mtxrHotspotActiveUserPingTimeout,
	mtxrHotspotActiveUserBytesIn,
	mtxrHotspotActiveUserBytesOut,
	mtxrHotspotActiveUserPacketsIn,
	mtxrHotspotActiveUserPacketsOut,
	mtxrHotspotActiveUserLimitBytesIn,
	mtxrHotspotActiveUserLimitBytesOut,
	mtxrHotspotActiveUserAdvertStatus,
	mtxrHotspotActiveUserRadius,
	mtxrHotspotActiveUserBlockedByAdvert
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 5 }

mtxrScriptGroup OBJECT-GROUP OBJECTS {
	mtxrScriptName, mtxrScriptRunCmd
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 8 }

mtxrNstremeDualGroup OBJECT-GROUP OBJECTS {
	mtxrDnStatTxRate, mtxrDnStatRxRate,
	mtxrDnStatTxStrength, mtxrDnStatRxStrength, mtxrDnConnected
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 10 }

mtxrNeighborGroup OBJECT-GROUP OBJECTS {
	mtxrNeighborIpAddress,
	mtxrNeighborMacAddress,
	mtxrNeighborVersion,
	mtxrNeighborPlatform,
	mtxrNeighborIdentity,
	mtxrNeighborSoftwareID,
	mtxrNeighborInterfaceID
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 11 }

mtxrDHCPGroup OBJECT-GROUP OBJECTS {
        mtxrDHCPLeaseCount
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 12 }

mtxrSystemGroup OBJECT-GROUP OBJECTS {
        mtxrSystemReboot,
        mtxrUSBPowerReset,
        mtxrSerialNumber,
        mtxrFirmwareVersion
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 13 }

mtxrTrapGroup NOTIFICATION-GROUP NOTIFICATIONS {
        mtxrTrap,
        mtxrTemperatureException
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 14 }

mtxrGPSGroup OBJECT-GROUP OBJECTS {
        mtxrDate,
        mtxrLongtitude,
        mtxrLatitude,
        mtxrAltitude,
        mtxrSpeed,
        mtxrSattelites,
        mtxrValid
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 15 }

mtxrWirelessModemGroup OBJECT-GROUP OBJECTS {
        mtxrWirelessModemSignalStrength,
        mtxrWirelessModemSignalECIO
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 16 }

mtxrInterfaceStatsGroup OBJECT-GROUP OBJECTS {
        mtxrInterfaceStatsName,
        mtxrInterfaceStatsDriverRxBytes,
        mtxrInterfaceStatsDriverRxPackets,
        mtxrInterfaceStatsDriverTxBytes,
        mtxrInterfaceStatsDriverTxPackets,

        mtxrInterfaceStatsTxRx64,
        mtxrInterfaceStatsTxRx65To127,
        mtxrInterfaceStatsTxRx128To255,
        mtxrInterfaceStatsTxRx256To511,
        mtxrInterfaceStatsTxRx512To1023,
        mtxrInterfaceStatsTxRx1024To1518,
        mtxrInterfaceStatsTxRx1519ToMax,

        mtxrInterfaceStatsRxBytes,
        mtxrInterfaceStatsRxPackets,
        mtxrInterfaceStatsRxTooShort,
        mtxrInterfaceStatsRx64,
        mtxrInterfaceStatsRx65To127,
        mtxrInterfaceStatsRx128To255,
        mtxrInterfaceStatsRx256To511,
        mtxrInterfaceStatsRx512To1023,
        mtxrInterfaceStatsRx1024To1518,
        mtxrInterfaceStatsRx1519ToMax,
        mtxrInterfaceStatsRxTooLong,
        mtxrInterfaceStatsRxBroadcast,
        mtxrInterfaceStatsRxPause,
        mtxrInterfaceStatsRxMulticast,
        mtxrInterfaceStatsRxFCSError,
        mtxrInterfaceStatsRxAlignError,
        mtxrInterfaceStatsRxFragment,
        mtxrInterfaceStatsRxOverflow,
        mtxrInterfaceStatsRxControl,
        mtxrInterfaceStatsRxUnknownOp,
        mtxrInterfaceStatsRxLengthError,
        mtxrInterfaceStatsRxCodeError,
        mtxrInterfaceStatsRxCarrierError,
        mtxrInterfaceStatsRxJabber,
        mtxrInterfaceStatsRxDrop,

        mtxrInterfaceStatsTxBytes,
        mtxrInterfaceStatsTxPackets,
        mtxrInterfaceStatsTxTooShort,
        mtxrInterfaceStatsTx64,
        mtxrInterfaceStatsTx65To127,
        mtxrInterfaceStatsTx128To255,
        mtxrInterfaceStatsTx256To511,
        mtxrInterfaceStatsTx512To1023,
        mtxrInterfaceStatsTx1024To1518,
        mtxrInterfaceStatsTx1519ToMax,
        mtxrInterfaceStatsTxTooLong,
        mtxrInterfaceStatsTxBroadcast,
        mtxrInterfaceStatsTxPause,
        mtxrInterfaceStatsTxMulticast,
        mtxrInterfaceStatsTxUnderrun,
        mtxrInterfaceStatsTxCollision,
        mtxrInterfaceStatsTxExcessiveCollision,
        mtxrInterfaceStatsTxMultipleCollision,
        mtxrInterfaceStatsTxSingleCollision,
        mtxrInterfaceStatsTxExcessiveDeferred,
        mtxrInterfaceStatsTxDeferred,
        mtxrInterfaceStatsTxLateCollision,
        mtxrInterfaceStatsTxTotalCollision,
        mtxrInterfaceStatsTxPauseHonored,
        mtxrInterfaceStatsTxDrop,
        mtxrInterfaceStatsTxJabber,
        mtxrInterfaceStatsTxFCSError,
        mtxrInterfaceStatsTxControl,
        mtxrInterfaceStatsTxFragment
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 17 }

mtxrPOEGroup OBJECT-GROUP OBJECTS {
        mtxrPOEName,
        mtxrPOEStatus,
        mtxrPOEVoltage,
        mtxrPOECurrent,
        mtxrPOEPower
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 18 }

mtxrLTEModemGroup OBJECT-GROUP OBJECTS {
        mtxrLTEModemInterfaceIndex,
        mtxrLTEModemSignalRSRP
    }
    STATUS current
    DESCRIPTION ""
    ::= { mtXRouterOsGroups 19 }

-- TRAPS **********************************************************************

mtxrNotifications OBJECT IDENTIFIER ::= { mtxrTraps 0 }

mtxrTrap NOTIFICATION-TYPE
    STATUS  current
    DESCRIPTION "Mikrotik trap OID"
    ::= { mtxrNotifications 1 }

mtxrTemperatureException NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "Mikrotik CPU temperature exception trap"
    ::= { mtxrNotifications 2 }

-- GPS ************************************************************************

mtxrDate OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "UNIX time"
    ::= { mtxrGps 1 }

mtxrLongtitude OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "longtitude"
    ::= { mtxrGps 2 }

mtxrLatitude OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "latitude"
    ::= { mtxrGps 3 }

mtxrAltitude OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "altitude"
    ::= { mtxrGps 4 }

mtxrSpeed OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "speed"
    ::= { mtxrGps 5 }

mtxrSattelites OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "visible sattelite count"
    ::= { mtxrGps 6 }

mtxrValid OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "is the data valid"
    ::= { mtxrGps 7 }

-- Wireless Modem ************************************************************

mtxrWirelessModemSignalStrength OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "signal strength in dBm (if first ppp-client modem supports)"
    ::= { mtxrWirelessModem 1 }

mtxrWirelessModemSignalECIO OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "signal EC/IO in dB (if first ppp-client modem supports)"
    ::= { mtxrWirelessModem 2 }

-- Interface Stats ************************************************************

mtxrInterfaceStatsTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrInterfaceStatsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "Extended interface statistics.
    Some interfaces may have only parts of this table
    with unavailable values set to zero."
    ::= { mtxrInterfaceStats 1 }

mtxrInterfaceStatsEntry OBJECT-TYPE
    SYNTAX MtxrInterfaceStatsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    INDEX { mtxrInterfaceStatsIndex }
    ::= { mtxrInterfaceStatsTable 1 }

MtxrInterfaceStatsEntry ::= SEQUENCE {
    mtxrInterfaceStatsIndex ObjectIndex,
    mtxrInterfaceStatsName DisplayString,

    mtxrInterfaceStatsDriverRxBytes Counter64,
    mtxrInterfaceStatsDriverRxPackets Counter64,
    mtxrInterfaceStatsDriverTxBytes Counter64,
    mtxrInterfaceStatsDriverTxPackets Counter64,

    mtxrInterfaceStatsTxRx64 Counter64,
    mtxrInterfaceStatsTxRx65To127 Counter64,
    mtxrInterfaceStatsTxRx128To255 Counter64,
    mtxrInterfaceStatsTxRx256To511 Counter64,
    mtxrInterfaceStatsTxRx512To1023 Counter64,
    mtxrInterfaceStatsTxRx1024To1518 Counter64,
    mtxrInterfaceStatsTxRx1519ToMax Counter64,

    mtxrInterfaceStatsRxBytes Counter64,
    mtxrInterfaceStatsRxPackets Counter64,
    mtxrInterfaceStatsRxTooShort Counter64,
    mtxrInterfaceStatsRx64 Counter64,
    mtxrInterfaceStatsRx65To127 Counter64,
    mtxrInterfaceStatsRx128To255 Counter64,
    mtxrInterfaceStatsRx256To511 Counter64,
    mtxrInterfaceStatsRx512To1023 Counter64,
    mtxrInterfaceStatsRx1024To1518 Counter64,
    mtxrInterfaceStatsRx1519ToMax Counter64,
    mtxrInterfaceStatsRxTooLong Counter64,
    mtxrInterfaceStatsRxBroadcast Counter64,
    mtxrInterfaceStatsRxPause Counter64,
    mtxrInterfaceStatsRxMulticast Counter64,
    mtxrInterfaceStatsRxFCSError Counter64,
    mtxrInterfaceStatsRxAlignError Counter64,
    mtxrInterfaceStatsRxFragment Counter64,
    mtxrInterfaceStatsRxOverflow Counter64,
    mtxrInterfaceStatsRxControl Counter64,
    mtxrInterfaceStatsRxUnknownOp Counter64,
    mtxrInterfaceStatsRxLengthError Counter64,
    mtxrInterfaceStatsRxCodeError Counter64,
    mtxrInterfaceStatsRxCarrierError Counter64,
    mtxrInterfaceStatsRxJabber Counter64,
    mtxrInterfaceStatsRxDrop Counter64,

    mtxrInterfaceStatsTxBytes Counter64,
    mtxrInterfaceStatsTxPackets Counter64,
    mtxrInterfaceStatsTxTooShort Counter64,
    mtxrInterfaceStatsTx64 Counter64,
    mtxrInterfaceStatsTx65To127 Counter64,
    mtxrInterfaceStatsTx128To255 Counter64,
    mtxrInterfaceStatsTx256To511 Counter64,
    mtxrInterfaceStatsTx512To1023 Counter64,
    mtxrInterfaceStatsTx1024To1518 Counter64,
    mtxrInterfaceStatsTx1519ToMax Counter64,
    mtxrInterfaceStatsTxTooLong Counter64,
    mtxrInterfaceStatsTxBroadcast Counter64,
    mtxrInterfaceStatsTxPause Counter64,
    mtxrInterfaceStatsTxMulticast Counter64,
    mtxrInterfaceStatsTxUnderrun Counter64,
    mtxrInterfaceStatsTxCollision Counter64,
    mtxrInterfaceStatsTxExcessiveCollision Counter64,
    mtxrInterfaceStatsTxMultipleCollision Counter64,
    mtxrInterfaceStatsTxSingleCollision Counter64,
    mtxrInterfaceStatsTxExcessiveDeferred Counter64,
    mtxrInterfaceStatsTxDeferred Counter64,
    mtxrInterfaceStatsTxLateCollision Counter64,
    mtxrInterfaceStatsTxTotalCollision Counter64,
    mtxrInterfaceStatsTxPauseHonored Counter64,
    mtxrInterfaceStatsTxDrop Counter64,
    mtxrInterfaceStatsTxJabber Counter64,
    mtxrInterfaceStatsTxFCSError Counter64,
    mtxrInterfaceStatsTxControl Counter64,
    mtxrInterfaceStatsTxFragment Counter64
}

mtxrInterfaceStatsIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 1 }

mtxrInterfaceStatsName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 2 }

mtxrInterfaceStatsDriverRxBytes OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 11 }

mtxrInterfaceStatsDriverRxPackets OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 12 }

mtxrInterfaceStatsDriverTxBytes OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 13 }

mtxrInterfaceStatsDriverTxPackets OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 14 }

mtxrInterfaceStatsTxRx64 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 15 }

mtxrInterfaceStatsTxRx65To127 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 16 }

mtxrInterfaceStatsTxRx128To255 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 17 }

mtxrInterfaceStatsTxRx256To511 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 18 }

mtxrInterfaceStatsTxRx512To1023 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 19 }

mtxrInterfaceStatsTxRx1024To1518 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 20 }

mtxrInterfaceStatsTxRx1519ToMax OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 21 }

mtxrInterfaceStatsRxBytes OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 31 }
 
mtxrInterfaceStatsRxPackets OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 32 }

mtxrInterfaceStatsRxTooShort OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 33 }

mtxrInterfaceStatsRx64 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 34 }

mtxrInterfaceStatsRx65To127 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 35 }

mtxrInterfaceStatsRx128To255 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 36 }

mtxrInterfaceStatsRx256To511 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 37 }

mtxrInterfaceStatsRx512To1023 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 38 }

mtxrInterfaceStatsRx1024To1518 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 39 }

mtxrInterfaceStatsRx1519ToMax OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 40 }

mtxrInterfaceStatsRxTooLong OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 41 }

mtxrInterfaceStatsRxBroadcast OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 42 }

mtxrInterfaceStatsRxPause OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 43 }

mtxrInterfaceStatsRxMulticast OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 44 }

mtxrInterfaceStatsRxFCSError OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 45 }

mtxrInterfaceStatsRxAlignError OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 46 }

mtxrInterfaceStatsRxFragment OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 47 }

mtxrInterfaceStatsRxOverflow OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 48 }

mtxrInterfaceStatsRxControl OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 49 }

mtxrInterfaceStatsRxUnknownOp OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 50 }

mtxrInterfaceStatsRxLengthError OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 51 }

mtxrInterfaceStatsRxCodeError OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 52 }

mtxrInterfaceStatsRxCarrierError OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 53 }

mtxrInterfaceStatsRxJabber OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 54 }

mtxrInterfaceStatsRxDrop OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 55 }

mtxrInterfaceStatsTxBytes OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 61 }

mtxrInterfaceStatsTxPackets OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 62 }

mtxrInterfaceStatsTxTooShort OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 63 }

mtxrInterfaceStatsTx64 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 64 }

mtxrInterfaceStatsTx65To127 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 65 }

mtxrInterfaceStatsTx128To255 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 66 }

mtxrInterfaceStatsTx256To511 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 67 }

mtxrInterfaceStatsTx512To1023 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 68 }

mtxrInterfaceStatsTx1024To1518 OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 69 }

mtxrInterfaceStatsTx1519ToMax OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 70 }

mtxrInterfaceStatsTxTooLong OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 71 }

mtxrInterfaceStatsTxBroadcast OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 72 }

mtxrInterfaceStatsTxPause OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 73 }

mtxrInterfaceStatsTxMulticast OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 74 }

mtxrInterfaceStatsTxUnderrun OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 75 }

mtxrInterfaceStatsTxCollision OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 76 }

mtxrInterfaceStatsTxExcessiveCollision OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 77 }

mtxrInterfaceStatsTxMultipleCollision OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 78 }

mtxrInterfaceStatsTxSingleCollision OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 79 }

mtxrInterfaceStatsTxExcessiveDeferred OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 80 }

mtxrInterfaceStatsTxDeferred OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 81 }

mtxrInterfaceStatsTxLateCollision OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 82 }

mtxrInterfaceStatsTxTotalCollision OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 83 }

mtxrInterfaceStatsTxPauseHonored OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 84 }

mtxrInterfaceStatsTxDrop OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 85 }

mtxrInterfaceStatsTxJabber OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 86 }

mtxrInterfaceStatsTxFCSError OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 87 }

mtxrInterfaceStatsTxControl OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 88 }

mtxrInterfaceStatsTxFragment OBJECT-TYPE
    SYNTAX Counter64
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrInterfaceStatsEntry 89 }

-- POE ************************************************************************

mtxrPOETable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrPOEEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "Power Over Ethernet"
    ::= { mtxrPOE 1 }

mtxrPOEEntry OBJECT-TYPE
    SYNTAX MtxrPOEEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    INDEX { mtxrPOEInterfaceIndex }
    ::= { mtxrPOETable 1 }

MtxrPOEEntry ::= SEQUENCE {
    mtxrPOEInterfaceIndex ObjectIndex,
    mtxrPOEName DisplayString,
    mtxrPOEStatus Integer32,
    mtxrPOEVoltage Voltage,
    mtxrPOECurrent Integer32,
    mtxrPOEPower Power
}

mtxrPOEInterfaceIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrPOEEntry 1 }

mtxrPOEName OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrPOEEntry 2 }

mtxrPOEStatus OBJECT-TYPE
    SYNTAX INTEGER {
        disabled(1),
        waitingForLoad(2),
        poweredOn(3),
        overload(4)
    }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION ""
    ::= { mtxrPOEEntry 3 }

mtxrPOEVoltage OBJECT-TYPE
    SYNTAX Voltage
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "V"
    ::= { mtxrPOEEntry 4 }

mtxrPOECurrent OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "mA"
    ::= { mtxrPOEEntry 5 }

mtxrPOEPower OBJECT-TYPE
    SYNTAX Power
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "W"
    ::= { mtxrPOEEntry 6 }

-- LTE Modem ************************************************************

mtxrLTEModemTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MtxrLTEModemEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION "LTE Modems"
    ::= { mtxrLTEModem 1 }

mtxrLTEModemEntry OBJECT-TYPE
    SYNTAX MtxrLTEModemEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    INDEX { mtxrLTEModemInterfaceIndex }
    ::= { mtxrLTEModemTable 1 }

MtxrLTEModemEntry ::= SEQUENCE {
    mtxrLTEModemInterfaceIndex ObjectIndex,
    mtxrLTEModemSignalRSRP Integer32
}

mtxrLTEModemInterfaceIndex OBJECT-TYPE
    SYNTAX ObjectIndex
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION ""
    ::= { mtxrLTEModemEntry 1 }

mtxrLTEModemSignalRSRP OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION "dBm"
    ::= { mtxrLTEModemEntry 2 }

-- ***************************************************************************
END

