MIMOSA-NETWORKS-BFIVE-MIB DEFINITIONS ::= BEGIN

--  Copyright (C) 2017, Mimosa Networks, Inc. All Rights Reserved.
--
--  Mimosa Networks MIB
--  Revision: 1.02
--  Date: April 28, 2017
--
--  Mimosa Networks, Inc.
--  469 El Camino Real Ste 100
--  Santa Clara, CA 95050
--  support@mimosa.co
--
--  This MIB defines the MIB specification for Mimosa Network's Products
--
--  Mimosa reserves the right to make changes to this MIB specification as
--  well as other information related to this specification without prior
--  notice.  The user of this specification should consult Mimosa Networks,
--  to determine if any such changes have been made.
--
--  Current MIBs are available from Mimosa Networks at the following URLs:
--
--		http://help.mimosa.co
--
--  In no event shall Mimosa Networks, Inc. be liable for any indirect,
--  consequential, special or incidental damages whatsoever (including
--  but not limited to lost profits or lost revenue) arising out of or
--  related to this specification or the information contained in it.
--  This non-liability extends to even if Mimosa Networks Inc. has been
--  advised of, known, or should have known, the potential for such damages.

--  Mimosa Networks, Inc. hereby grants end-users, and other parties a
--  a non-exclusive license to use this MIB specification in order to
--  manage products of Mimosa Networks, Inc.


IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE,
    NOTIFICATION-TYPE, Integer32,
    Counter32, Counter64, Unsigned32,
    TimeTicks, IpAddress                  FROM SNMPv2-SMI

    DisplayString , MacAddress,
    RowStatus, TruthValue,
    PhysAddress, TEXTUAL-CONVENTION       FROM SNMPv2-TC

    MODULE-COMPLIANCE, OBJECT-GROUP,
    NOTIFICATION-GROUP 	                  FROM SNMPv2-CONF

    ifIndex                               FROM IF-MIB
    mimosaWireless,
    mimosaConformanceGroup                FROM MIMOSA-NETWORKS-BASE-MIB;

mimosaB5Module MODULE-IDENTITY
    LAST-UPDATED "201506030000Z"
    ORGANIZATION "Mimosa Networks
    			  www.mimosa.co"
    CONTACT-INFO
    	"postal:
    	Mimosa Networks, Inc.
		469 El Camino Real Ste 100
		Santa Clara, CA 95050
        email: support@mimosa.co"
    DESCRIPTION
		"Mimosa device MIB definitions"
	REVISION	"201704280000Z"
    DESCRIPTION
		"Compatible with Firmware 1.4.5"
    ::= { mimosaConformanceGroup 1 }

mimosaGeneral       OBJECT IDENTIFIER ::= { mimosaWireless 1 }
mimosaLocInfo       OBJECT IDENTIFIER ::= { mimosaWireless 2 }
mimosaWanInfo       OBJECT IDENTIFIER ::= { mimosaWireless 3 }
mimosaTdmaInfo      OBJECT IDENTIFIER ::= { mimosaWireless 4 }
mimosaMgmtInfo      OBJECT IDENTIFIER ::= { mimosaWireless 5 }
mimosaRfInfo        OBJECT IDENTIFIER ::= { mimosaWireless 6 }
mimosaPerfInfo      OBJECT IDENTIFIER ::= { mimosaWireless 7 }
mimosaServices      OBJECT IDENTIFIER ::= { mimosaWireless 8 }


-- *****************************************************************
-- ***                   Mimosa Textual Conventions              ***
-- *****************************************************************
DecimalOne ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d-1"
    STATUS       current
    DESCRIPTION  "Fixed point, one decimal"
    SYNTAX       Integer32

DecimalTwo ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d-2"
    STATUS       current
    DESCRIPTION  "Fixed point, two decimals"
    SYNTAX       Integer32

DecimalFive ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d-5"
    STATUS       current
    DESCRIPTION  "Fixed point, five decimals"
    SYNTAX       Integer32

-- *****************************************************************
-- ***       Mimosa General variables are specified below.    ***
-- *****************************************************************

mimosaDeviceName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..64))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The name of the local Mimosa device. This unique identifier could
         be the same as the sysName object."
    ::= { mimosaGeneral 1 }

mimosaSerialNumber OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..64))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The unique serial number of the Mimosa device."
    ::= { mimosaGeneral 2 }

mimosaFirmwareVersion OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..64))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The version of the currently installed and/or running firmware
         on the Mimosa device."
    ::= { mimosaGeneral 3 }

mimosaFirmwareBuildDate OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..64))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The creation date of the currently installed and/or running
         firmware on the Mimosa device."
    ::= { mimosaGeneral 4 }

mimosaLastRebootTime OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..64))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The last time the Mimosa device rebooted."
    ::= { mimosaGeneral 5 }

mimosaUnlockCode OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..64))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The code used to unlock the Mimosa device."
    ::= { mimosaGeneral 6 }

mimosaLEDBrightness OBJECT-TYPE
    SYNTAX  INTEGER {
                auto(1),
                low(2),
                medium(3),
                high(4)
            }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the intensity of the status indicator lights on the
         device exterior. The Auto option adjusts the amount of light
         based upon ambient conditions. Manual options include Low,
         Medium, and High."
    ::= { mimosaGeneral 7 }

mimosaInternalTemp OBJECT-TYPE
    SYNTAX       DecimalOne
    UNITS        "C" 
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The internal temperature of the Mimosa device."
    ::= { mimosaGeneral 8 }

mimosaRegulatoryDomain OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..64))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The country in which the Mimosa device has been configured to run."
    ::= { mimosaGeneral 9 }


-- **********************************************************************
-- ***     Mimosa Device Location variables are specified below.      ***
-- **********************************************************************

mimosaLongitude OBJECT-TYPE
    SYNTAX       DecimalFive
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The Longitude of the Mimosa device location, in 5 decimal points."
    ::= { mimosaLocInfo 1 }

mimosaLatitude OBJECT-TYPE
    SYNTAX       DecimalFive
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The Latitude of the Mimosa device location, in 5 decimal points."
    ::= { mimosaLocInfo 2 }

mimosaAltitude OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "meters" 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The Altitude of the Mimosa device location in meters."
    ::= { mimosaLocInfo 3 }

mimosaSatelliteSNR OBJECT-TYPE
    SYNTAX       DecimalOne
    UNITS        "dB"
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The average Signal to Noise Ratio (SNR) amongst all of the satellites
         detected by the Mimosa device. Display is in 1 decimal point."
    ::= { mimosaLocInfo 4 }

mimosaSatelliteStrength OBJECT-TYPE
    SYNTAX  INTEGER {
                good(1),
                bad(2)
            }
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Strength of the satellites based on the number of satellites available.
         It is considered good if more than 2 satellites are available."
    ::= { mimosaLocInfo 5 }

mimosaGPSSatellites OBJECT-TYPE
    SYNTAX       Integer32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Total number of GPS satellites detected."
    ::= { mimosaLocInfo 6 }

mimosaGlonassSatellites OBJECT-TYPE
    SYNTAX       Integer32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Total number of GLONASS satellites detected."
    ::= { mimosaLocInfo 7 }

mimosaClockAccuracy OBJECT-TYPE
    SYNTAX       DecimalTwo
    UNITS        "PPB"
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "Timing signal accuracy measured in parts per billion (PPB) by the
         Mimosa device. Display is in 2 decimal points."
    ::= { mimosaLocInfo 8 }


-- **********************************************************************
-- ***  Mimosa Device TDMA Information variables are specified below. ***
-- **********************************************************************

mimosaWirelessMode OBJECT-TYPE
    SYNTAX  INTEGER {
                accessPoint(1),
                station(2)
            }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Describes wherger the Mimosa device acts as an access point or station."
    ::= { mimosaTdmaInfo 1 }

mimosaWirelessProtocol OBJECT-TYPE
    SYNTAX  INTEGER {
                tdma(1),
                csma(2)
            }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Describes the wireless protocol configured on the Mimosa device. 
	     Both TDMA and CSMA are supported. TDMA is a deterministic protocol
         where each device is assigned a time slot during which it is allowed
         to transmit. This allows for collocated radios to utilize the same
         channel and avoid Tx/Rx collisions and interference."
    ::= { mimosaTdmaInfo 2 }

mimosaTDMAMode OBJECT-TYPE
    SYNTAX  INTEGER {
                a(1),
                b(2)
            }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies the TDMA Gender of the radio (A or B)."
    ::= { mimosaTdmaInfo 3 }

mimosaTDMAWindow OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "ms"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies the length of the transmit time slot in milliseconds."
    ::= { mimosaTdmaInfo 4 }

mimosaTrafficSplit OBJECT-TYPE
    SYNTAX  INTEGER {
                symmetric(1),
                asymmetric(2),
                auto(3)
            }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The radio can be configured to allocate bandwidth symmetrically (50/50)
         or asymmetrically (75/25 or 25/75) in environments where traffic
         direction is expected to be heavier in one direction than the other.
         With an asymmetrical split, the local radio is represented first in the
         slash notation, (local/remote). For example, in the (75/25) split, the
         local radio gets 75, while the remote radio gets 25. If Auto is selected
         the radio will automatically determine, based upon traffic flow, which
         ratio will be used. The radio will continue to evaluate the flow and
         adjust accordingly."
    ::= { mimosaTdmaInfo 5 }


-- **********************************************************************
-- *** Mimosa Device Radio Information variables are specified below. ***
-- **********************************************************************

mimosaChainTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF MimosaChainEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A list of RF chain entries, which is part of MIMO tables. MIMO stands
         for Multiple In Multiple Out."
    ::= { mimosaRfInfo 1 }

mimosaChainEntry OBJECT-TYPE
    SYNTAX      MimosaChainEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry containing chain information applicable to a particular
         RF chain."
    INDEX   { mimosaChain }
    ::= { mimosaChainTable 1 }

MimosaChainEntry ::=
    SEQUENCE {
        mimosaChain        Integer32,
        mimosaTxPower      DecimalOne,
        mimosaRxPower      DecimalOne,
        mimosaRxNoise      DecimalOne,
        mimosaSNR          DecimalOne,
        mimosaCenterFreq   Integer32,
        mimosaPolarization INTEGER
    }

mimosaChain OBJECT-TYPE
    SYNTAX      Integer32 (0..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An index which is used to access a particular entry in the chain table."
    ::= { mimosaChainEntry 1 }

mimosaTxPower OBJECT-TYPE
    SYNTAX      DecimalOne
    UNITS       "dBm"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies the transmit power of the given RF chain. A value of -8 means
         this particular TxChain is not a valid entry."
    ::= { mimosaChainEntry 2 }

mimosaRxPower OBJECT-TYPE
    SYNTAX      DecimalOne
    UNITS       "dBm"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies the receive power of the given RF chain. A value of -100
         means this particular RxChain is not a valid entry (SNR must be -100)."
    ::= { mimosaChainEntry 3 }

mimosaRxNoise OBJECT-TYPE
    SYNTAX      DecimalOne
    UNITS       "dBm"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies the received noise level for the given RF chain."
    ::= { mimosaChainEntry 4 }

mimosaSNR OBJECT-TYPE
    SYNTAX      DecimalOne
    UNITS       "dB"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the Signal to Noise Ratio (SNR) for the given RF chain.
         A value of -100 means this particular RxChain is not a valid entry."
    ::= { mimosaChainEntry 5 }

mimosaCenterFreq OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "MHz"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The center frequency for the given RF chain. A value of 0 means this
         particular Chain is not a valid entry."
    ::= { mimosaChainEntry 6 }

mimosaPolarization OBJECT-TYPE
    SYNTAX  INTEGER {
                horizontal(1),
                vertical(2)
            }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The ploarization of the given RF chain. It could be horizontal or
         vertical."
    ::= { mimosaChainEntry 7 }


mimosaStreamTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF MimosaStreamEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A list of data stream entries, which are part of MIMO tables. MIMO
         stands for Multiple In Multiple Out."
    ::= { mimosaRfInfo 2 }

mimosaStreamEntry OBJECT-TYPE
    SYNTAX      MimosaStreamEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The entry containing information applicable to a particular stream."
    INDEX   { mimosaStream }
    ::= { mimosaStreamTable 1 }

MimosaStreamEntry ::=
    SEQUENCE {
        mimosaStream       Integer32,
        mimosaTxPhy        Integer32,
        mimosaTxMCS        Integer32,
        mimosaTxWidth      Integer32,
	mimosaRxPhy        Integer32,
        mimosaRxMCS        Integer32,
        mimosaRxWidth      Integer32,
	mimosaRxEVM        DecimalOne
   }

mimosaStream OBJECT-TYPE
    SYNTAX      Integer32 (0..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The index used to access a particular entry in the stream table."
    ::= { mimosaStreamEntry 1 }

mimosaTxPhy OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "Mbps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies the transmit rate of the given data stream."
    ::= { mimosaStreamEntry 2 }

mimosaTxMCS OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies the transmit MCS of the given data stream. A value of
         -1 means this particular TxStream is not a valid entry."
    ::= { mimosaStreamEntry 3 }

mimosaTxWidth OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "MHz"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies the channel width based on MCS. A value of 
	 -1 means this particular TxWidth is not a valid entry"
    ::= { mimosaStreamEntry 4 }

mimosaRxPhy OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "Mbps"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies the receive rate of the given data stream."
    ::= { mimosaStreamEntry 5 }

mimosaRxMCS OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies the receive MCS of the given data stream. A value of
         -1 means this particular RxStream is not a valid entry."
    ::= { mimosaStreamEntry 6 }

mimosaRxWidth OBJECT-TYPE
    SYNTAX      Integer32
    UNITS	"MHz"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies the receive Rx Width of the given data stream. A value of
         -1 means this particular RxWidth is not a valid entry."
    ::= { mimosaStreamEntry 7 }

mimosaRxEVM OBJECT-TYPE
    SYNTAX      DecimalOne
    UNITS       "dB"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies the receive Error Vector Magnitude (EVM) of the given data
         stream."
    ::= { mimosaStreamEntry 8 }

mimosaChannelTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF MimosaChannelEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "A list of RF channel entries on the Mimosa device."
    ::= { mimosaRfInfo 3 }

mimosaChannelEntry OBJECT-TYPE
    SYNTAX      MimosaChannelEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The entry containing management information applicable to a particular
         channel."
    INDEX   { mimosaChannel }
    ::= { mimosaChannelTable 1 }

MimosaChannelEntry ::=
    SEQUENCE {
        mimosaChannel            Integer32,
        mimosaChannelMode        INTEGER,
        mimosaChannelWidth       Integer32,
        mimosaChannelTxPower     DecimalOne,
        mimosaChannelCenterFreq  Integer32
    }

mimosaChannel OBJECT-TYPE
    SYNTAX      Integer32 (0..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The index used to access a particular entry in the RF channel table."
    ::= { mimosaChannelEntry 1 }

mimosaChannelMode OBJECT-TYPE
    SYNTAX  INTEGER {
                transmit(1),
                receive(2),
                bidirectional(3)
            }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
	"Specifies the mode for the given channel. The transmit or receive
	 values indicate Frequency Diversity (FD) mode is in use. The
	 bidirectional value means that the channel is used for both transmit
	 and receive in all other single or dual channel modes."
    ::= { mimosaChannelEntry 2 }

mimosaChannelWidth OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "MHz"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies the channel width of the given channel."
    ::= { mimosaChannelEntry 3 }

mimosaChannelTxPower OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "dBm"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies the transmit power level on the channel. If Channel Width
         is set to 1xN MHz, Channel 2 is not be used. In Frequency Diversity mode,
         Power 1 and Power 2 represent transmit power on the local and remote
         sides, respectively."
    ::= { mimosaChannelEntry 4 }

mimosaChannelCenterFreq OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "MHz"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies the center frequency of the channel used on the link. In all
         modes, the center frequency represents the absolute center of the
         selected channel width without any offset, and the center can be moved
         in 5 MHz increments.

         A value of 0 means this particular channel is not a valid entry."
    ::= { mimosaChannelEntry 5 }

mimosaAntennaGain OBJECT-TYPE
    SYNTAX       Integer32
    UNITS        "dBi"
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The antenna gain on the Mimosa device."
    ::= { mimosaRfInfo 4 }

mimosaTotalTxPower OBJECT-TYPE
    SYNTAX      DecimalOne
    UNITS        "dBm"
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The total transmit power for all the channels on the Mimosa device."
    ::= { mimosaRfInfo 5 }

mimosaTotalRxPower OBJECT-TYPE
    SYNTAX      DecimalOne
    UNITS        "dBm"
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The total receive power for all the channels on the Mimosa device."
    ::= { mimosaRfInfo 6 }

mimosaTargetSignalStrength OBJECT-TYPE
    SYNTAX      Integer32
    UNITS        "dB"
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The calculated target receive signal strength based on device coordinates and settings."
    ::= { mimosaRfInfo 7 }


-- **********************************************************************
-- ***  Mimosa Device WAN Information variables are specified below.  ***
-- **********************************************************************

mimosaWanSsid OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..64))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The wireless link name used by both radios. Both AP and Station must
         use the same SSID to communicate with each other."
    ::= { mimosaWanInfo 1 }

mimosaWanMac OBJECT-TYPE
    SYNTAX      PhysAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The MAC address used for the wireless link."
    ::= { mimosaWanInfo 2 }

mimosaWanStatus OBJECT-TYPE
    SYNTAX  INTEGER {
                connected(1),
                disconnected(2)
            }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The wireless link status between the Mimosa devices."
    ::= { mimosaWanInfo 3 }

mimosaWanUpTime OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The wireless link up time since last reboot."
    ::= { mimosaWanInfo 4 }


-- ****************************************************************************
-- *** Mimosa Device Performance Information variables are specified below. ***
-- ****************************************************************************

mimosaPhyTxRate OBJECT-TYPE
    SYNTAX      DecimalTwo
    UNITS       "kbps" 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The transmit packet rate at the physical level over a 5 second interval."
    ::= { mimosaPerfInfo 1 }

mimosaPhyRxRate OBJECT-TYPE
    SYNTAX      DecimalTwo
    UNITS       "kbps" 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The receive packet rate at the physical level over a 5 second interval."
    ::= { mimosaPerfInfo 2 }

mimosaPerTxRate OBJECT-TYPE
    SYNTAX      DecimalTwo
    UNITS       "%"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The trasnmit Packet Error Rate (PER) over a 5 second interval. It is
         caluculated as packets with errors versuss packets without errors."
    ::= { mimosaPerfInfo 3 }

mimosaPerRxRate OBJECT-TYPE
    SYNTAX      DecimalTwo
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The receive Packet Error Rate (PER) over a 5 second interval. It is
         caluculated as packets with errors versuss packets without errors."
    ::= { mimosaPerfInfo 4 }


-- ****************************************************************************
-- *** Mimosa Device Management  Information variables are specified below. ***
-- ****************************************************************************

mimosaNetworkMode OBJECT-TYPE
    SYNTAX  INTEGER {
                enabled(1),
                disabled(2),
                auto(3)
            }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies the mode for the local 2.4 GHz wireless network operation.
         If Auto is selected, the 2.4 GHz management network is turned on for a
         limited time (defined in Console Timeout ) after boot and then turned
         off if there is no activity. If a user associates with the radio within
         the timeout period, they will not be disconnected."
    ::= { mimosaMgmtInfo 1 }

mimosaRecoverySsid OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The recovery SSID that allows the device to be reset to factory
         defaults. This is available for 10 minutes after device boot. Disabling
         the 2.4 GHz management network will not impact availability of this
         option. The serial number of the device must be known in order to
         perform the factory reset."
    ::= { mimosaMgmtInfo 2 }

mimosaLocalSsid OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The SSID for managing the local 2.4 GHz wireless interface."
    ::= { mimosaMgmtInfo 3 }

mimosaLocalChannel OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
	"The channel used for the local 2.4 GHz wireless interface."
    ::= { mimosaMgmtInfo 4 }

mimosaConsoleTimeout OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "min"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
	"The amount inactivity on the 2.4 GHz wireless interface before
         turning it off in Auto mode."
    ::= { mimosaMgmtInfo 5 }

mimosaMaxClients OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
	"The maximum number of wireless clients that can simultaneously access
         the 2.4 GHz management interface."
    ::= { mimosaMgmtInfo 6 }

mimosaLocalMac OBJECT-TYPE
    SYNTAX      PhysAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The MAC address used for 2.4 GHz wireless link."
    ::= { mimosaMgmtInfo 7 }

mimosaLocalIpAddr OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IP address assigned to the 2.4 GHz wireless link."
    ::= { mimosaMgmtInfo 8 }

mimosaLocalNetMask OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IP netmask assigned to the 2.4 GHz wireless link."
    ::= { mimosaMgmtInfo 9 }

mimosaLocalGateway OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IP address of the gateway for the 2.4 GHz wireless link."
    ::= { mimosaMgmtInfo 10 }

mimosaFlowControl OBJECT-TYPE
    SYNTAX      INTEGER {
                    enabled(1),
                    disabled(2)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies whether Flow Control is enabled on the Mimosa device."
    ::= { mimosaMgmtInfo 11 }
 


-- *************************************************************************
-- *** Mimosa Device Services Information variables are specified below. ***
-- *************************************************************************

mimosaHttpsEnabled OBJECT-TYPE
    SYNTAX  INTEGER {
                enabled(1),
                disabled(2)
            }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies whether HTTPS is enabled on the Mimosa device."
    ::= { mimosaServices 1 }

mimosaMgmtVlanEnabled OBJECT-TYPE
    SYNTAX  INTEGER {
                enabled(1),
                disabled(2)
            }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies whether the Management VLAN is enabled on the Mimosa device."
    ::= { mimosaServices 2 }

mimosaMgmtCloudEnabled OBJECT-TYPE
    SYNTAX  INTEGER {
                enabled(1),
                disabled(2)
            }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies whether the Management Cloud is enabled on the Mimosa device."
    ::= { mimosaServices 3 }

mimosaRestMgmtEnabled OBJECT-TYPE
    SYNTAX  INTEGER {
                enabled(1),
                disabled(2)
            }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies whether the REST management is enabled on the Mimosa device."
    ::= { mimosaServices 4 }

mimosaPingWatchdogEnabled OBJECT-TYPE
    SYNTAX  INTEGER {
                enabled(1),
                disabled(2)
            }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies whether the IP Ping watchdog is enabled on the Mimosa device.
         This is used to reset the device if a configured IP address is
         not reached in certain number of retries."
    ::= { mimosaServices 5 }

mimosaSyslogEnabled OBJECT-TYPE
    SYNTAX  INTEGER {
                enabled(1),
                disabled(2)
            }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies whether the Syslog client is enabled on the Mimosa device.
         Syslog client sends the log messages to configured syslog server."
    ::= { mimosaServices 6 }

mimosaNtpMode OBJECT-TYPE
    SYNTAX  INTEGER {
                custom(1),
                standard(2)
            }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies whether the NTP client is configured to use standard servers
         from NIST, NTP organizations or custom NTP server."
    ::= { mimosaServices 7 }

mimosaNtpServer OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..64))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies the name or address of the custom NTP server."
    ::= { mimosaServices 8 }

END

