-- *****************************************************************
-- CISCO-CAT6K-CROSSBAR-MIB.my
--   
-- Mar 2001, Padma Pullela
-- Nov. 2002, Padma Pullela/Lilian Jiang
-- March  2003, Padma Pullela
-- June  2004, Padma Pullela
--   

-- Copyright (c) 2001-2002, 2003-2009 by cisco Systems, Inc.
-- All rights reserved.
-- *****************************************************************

CISCO-CAT6K-CROSSBAR-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Counter32,
    Unsigned32,
    Gauge32,
    NOTIFICATION-TYPE
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP,
    NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    TEXTUAL-CONVENTION,
    TruthValue,
    DisplayString,
    DateAndTime,
    TimeStamp
        FROM SNMPv2-TC
    entPhysicalName,
    entPhysicalVendorType,
    entPhysicalIndex,
    entPhysicalDescr
        FROM ENTITY-MIB
    Percent
        FROM CISCO-QOS-PIB-MIB
    ciscoMgmt
        FROM CISCO-SMI;


ciscoCat6kCrossbarMIB MODULE-IDENTITY
    LAST-UPDATED    "200902150000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service
            Postal: 170 W Tasman Drive
            San Jose, CA  95134
            USA
            Tel: +1 800 553-NETS

            E-mail: cs-cat6000@cisco.com"
    DESCRIPTION
        "The Catalyst 6000 Crossbar MIB provides instrumentation for
        configuration and operation of the crossbar switching fabric
        module, and additional functionalities for switching bus 
        and internal bus, etc.
        "
    REVISION        "200902150000Z"
    DESCRIPTION
        "Added cc6kxbarErrRcvryPersLinkResGroup and
         cc6kxbarErrRcvryChResyncGroup,
         cc6kxbarTMSwBusUtilGroup, 
         cc6kxbarTMSwBusUtilNotifControlGroup,
         cc6kxbarTMSwBusUtilNotifObjectGroup,
         cc6kxbarTMSwBusUtilNotifGroup,
         cc6kxbarTMChUtilGroup,
         cc6kxbarTMChUtilNotifControlGroup,
         cc6kxbarTMChUtilNotifObjectGroup,
         cc6kxbarTMChUtilNotifGroup.

         Added two new enumerations 'pfc4' and 'pfc4xl' 
         in cc6kxbarSysCapPfcOperMode.

         Added DISPLAY-HINT in TEXTUAL-CONVENTION
         of ModuleSlotNumber and FabricChannelNumber."
    REVISION        "200712180000Z"
    DESCRIPTION
        "Added cc6kxbarSysCapPfcOperModeGroup,
         cc6kxbarSysCapSwitchResGroup, cc6kxbarChannelUtilGroup1,
         cc6kxbarSwBusGroup1, cc6kxbarErrorGroup,
         cc6kxbarErrRcvryThresholdGroup and 
         cc6kxbarErrRcvrySwitchoverGroup."
    REVISION        "200612190000Z"
    DESCRIPTION
        "Added cc6kxbarDcefOnlyModeAllowedGroup,
        cc6kxbarForceBusModeGroup,
        cc6kxbarFlowCtrlNotifCtrlGroup,
        cc6kxbarFlowCtrlBusThreshGroup,
        cc6kxbarFlowCtrlBusThrNotifGroup 
        and cc6kxbarBusOnlyModeOperGroup."
    REVISION        "200411190000Z"
    DESCRIPTION
        "Added cc6kxbarIntBusCRCErrGroup."
    REVISION        "200408110000Z"
    DESCRIPTION
        "Added cc6kxbarIntBusNotifControlGroup and
        cc6kxbarIntBusCRCErrNotifGroup."
    REVISION        "200406110000Z"
    DESCRIPTION
        "Added cc6kxbarTruncatedModeOper Object and changed the
        description of cc6kxbarTruncatedModeAllowed and 
        cc6kxbarMinFabricPresent."
    REVISION        "200309290000Z"
    DESCRIPTION
        "Changed the description of cc6kxbarTruncatedModeAllowed and
        cc6kxbarMinFabricPresent. Removed default value for 
        cc6kxbarTruncatedModeAllowed."
    REVISION        "200304020000Z"
    DESCRIPTION
        "Changed the SYNTAX and description of cc6kxbarMinFabricPresent
        and  description of cc6kxbarTruncatedModeAllowed."
    REVISION        "200212050000Z"
    DESCRIPTION
        "Added cc6kxbarModuleChannelSpeed, cc6kxbarSwBusSwitchingStatus,
        cc6kxbarSwBusFailureDuration, cc6kxbarSwBusNotifEnable 
        objects and cc6kxbarSwBusStallNotif notification."
    REVISION        "200106250000Z"
    DESCRIPTION
        "Initial version of this MIB module."
          ::= { ciscoMgmt 217 }


ciscoCat6kXbarMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoCat6kCrossbarMIB 1 }

cc6kxbarConfiguration  OBJECT IDENTIFIER
    ::= { ciscoCat6kXbarMIBObjects 1 }

cc6kxbarStatus  OBJECT IDENTIFIER
    ::= { ciscoCat6kXbarMIBObjects 2 }

cc6kxbarStatistics  OBJECT IDENTIFIER
    ::= { ciscoCat6kXbarMIBObjects 3 }

cc6kxbarSwBusObjects  OBJECT IDENTIFIER
    ::= { ciscoCat6kXbarMIBObjects 4 }

cc6kxbarIntBusObjects  OBJECT IDENTIFIER
    ::= { ciscoCat6kXbarMIBObjects 5 }

cc6kxbarFlowCtrlObjects  OBJECT IDENTIFIER
    ::= { ciscoCat6kXbarMIBObjects 6 }

cc6kxbarSystemCapacityObjects OBJECT IDENTIFIER 
    ::= { ciscoCat6kXbarMIBObjects 7 }

cc6kxbarErrorRecoveryObjects OBJECT IDENTIFIER
    ::= { ciscoCat6kXbarMIBObjects 8 }

cc6kxbarTrafficMonitorObjects OBJECT IDENTIFIER
    ::= { ciscoCat6kXbarMIBObjects 9 }

cc6kxbarTrafficMonitorSwBusObjects OBJECT IDENTIFIER 
    ::= { cc6kxbarTrafficMonitorObjects 1}

cc6kxbarTrafficMonitorChObjects  OBJECT IDENTIFIER 
    ::= { cc6kxbarTrafficMonitorObjects 2}


-- Textual Conventions

ModuleSlotNumber ::= TEXTUAL-CONVENTION
    DISPLAY-HINT    "d"
    STATUS          current
    DESCRIPTION     "Slot number of the module."
    SYNTAX          Unsigned32

FabricChannelNumber ::= TEXTUAL-CONVENTION
    DISPLAY-HINT    "d" 
    STATUS          current
    DESCRIPTION     "Fabric channel number."
    SYNTAX          Unsigned32

ChannelStatus ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION     "Status of the Channel."
    SYNTAX          INTEGER  {
                        ok(1),
                        syncError(2),
                        heartbeatError(3),
                        crcError(4),
                        bufferError(5),
                        timeoutError(6),
                        unused(7)
                    }

-- Configuration objects
cc6kxbarFallbackMode OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "cc6kxbarFallbackMode controls system fallback to bus-mode
        after loss of switching fabric module.
        'true'  - When the last fabric card is removed
                  system will adjust the supervisor and
                  line cards switching mode automatically without
                  resetting the system. With this feature enabled,
                  the switch might lose traffic while it's
                  changing the switching mode.
        'false'  - All the ports in the system will be
                  disabled when the last fabric card is removed."
    DEFVAL          { true } 
    ::= { cc6kxbarConfiguration 1 }

cc6kxbarBusOnlyModeAllowed OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Indicates whether bus mode is administratively enabled on
        the device or not." 
    ::= { cc6kxbarConfiguration 2 }

cc6kxbarTruncatedModeAllowed OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Indicates whether truncated mode is
        administratively enabled on the device or not." 
    ::= { cc6kxbarConfiguration 3 }

cc6kxbarMinFabricPresent OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object indicates the minimum number
        of switching fabric capable modules to be present in the 
        system, for any switching fabric capable module to be in
        'crossbarmode' indicated by  cc6kxbarModuleModeSwitchingMode,
        when cc6kxbarTruncatedModeOper is 'false'." 
    ::= { cc6kxbarConfiguration 4 }

cc6kxbarLcdBannerTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF Cc6kxbarLcdBannerEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "cc6kxbarLcdBannerTable configures the Lcd banner of the
        fabric module."
    ::= { cc6kxbarConfiguration 5 }

cc6kxbarLcdBannerEntry OBJECT-TYPE
    SYNTAX          Cc6kxbarLcdBannerEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in cc6kxbarLcdBannerTable.
        Entries are created by the agent based on the
        size of the lcd banner."
    INDEX           { cc6kxbarLcdBannerIndex } 
    ::= { cc6kxbarLcdBannerTable 1 }

Cc6kxbarLcdBannerEntry ::= SEQUENCE {
        cc6kxbarLcdBannerIndex   Unsigned32,
        cc6kxbarLcdBannerBanner  DisplayString,
        cc6kxbarLcdBannerMaxSize Unsigned32
}

cc6kxbarLcdBannerIndex OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Object which specifies a unique entry in the
        table." 
    ::= { cc6kxbarLcdBannerEntry 1 }

cc6kxbarLcdBannerBanner OBJECT-TYPE
    SYNTAX          DisplayString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Message that would be displayed on the fabric card LCD.
        The size of cc6kxbarLcdBannerBanner should be less than 
        or equal to the cc6kxbarLcdBannerMaxSize value." 
    ::= { cc6kxbarLcdBannerEntry 2 }

cc6kxbarLcdBannerMaxSize OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Maximum size of the associated cc6kxbarLcdBannerBanner
        object." 
    ::= { cc6kxbarLcdBannerEntry 3 }
 


cc6kxbarTruncatedModeOper OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Indicates if the truncated mode is
        operationally enabled on the device or not.
        'true' - With the fabric module present in the system,
                 cc6kxbarModuleModeSwitchingMode will be
                 'crossbarmode' for all the fabric capable
                  modules.
        'false'- With the cc6kxbarMinFabricPresent fabric capable 
                 modules and the fabric module  present in the system,
                 cc6kxbarModuleModeSwitchingMode
                 will be 'crossbarmode' for fabric capable modules." 
    ::= { cc6kxbarConfiguration 6 }

cc6kxbarDcefOnlyModeAllowed OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Indicates whether the dcef mode is enabled on the standby
        supervisor or not.
        'true' - Setting cc6kxbarDcefOnlyModeAllowed to 'true'
                 makes the  cc6kxbarModuleModeSwitchingMode of
                 all the active modules to 'dcefmode'.
                 With the active fabric module present in the system,
                 with the switch being in stateful switchover mode,
                 with all the cards that has no distributed Cisco
                 Express forwarding  switching support being
                 powered down and on some platforms with standby
                 supervisor ports being shutdown, changing
                 cc6kxbarDcefOnlyModeAllowed to 'true' will make the
                 standby supervisor module reloaded and booted up
                 as distributed forwarding module.
        'false'- Setting cc6kxbarDcefOnlyModeAllowed to 'false'
                 makes the cc6kxbarModuleModeSwitchingMode of the
                 standby supervisor module to the default value.
                 Changing cc6kxbarDcefOnlyModeAllowed  to 'false'
                 will make the standby supervisor reloaded and booted 
                 up with the default cc6kxbarModuleModeSwitchingMode." 
    ::= { cc6kxbarConfiguration 7 }

cc6kxbarForceBusMode OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Indicates whether some affected modules are forced to be in
        'busmode' or not.
        'true' - Setting cc6kxbarForceBusMode to 'true' makes the
                 cc6kxbarModuleModeSwitchingMode of all
                 the affected modules to 'busmode'. Changing the
                 cc6kxbarForceBusMode to 'true' will make all the
                 affected modules reloaded and booted up as
                 non fabric capable modules.
        'false'- Setting cc6kxbarForceBusMode to 'false' makes the
                 cc6kxbarModuleModeSwitchingMode of all the affected
                 modules to the default value. Changing
                 cc6kxbarForceBusMode to 'false' will make all the
                 affected modules reloaded and booted up with the
                 default cc6kxbarModuleModeSwitchingMode." 
    ::= { cc6kxbarConfiguration 8 }

cc6kxbarBusOnlyModeOper OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Indicates if the bus mode is operationally enabled on the
        device or not.

        'true' - Modules are allowed to run in 'busmode'.
        'false' - None of the modules are allowed to run in 'busmode'
                 i.e., All the non-fabric capable modules will
                 be powered off.  Absence of fabric module results
                 in all the fabric capable modules being powered
                 off." 
    ::= { cc6kxbarConfiguration 9 }

-- Status objects
cc6kxbarFabricActiveSlot OBJECT-TYPE
    SYNTAX          ModuleSlotNumber
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "cc6kxbarFabricActiveSlot indicates the slot number of the
        active switching fabric module. A value of zero indicates 
        that the active switching fabric module is either powered 
        down or not present in the chassis." 
    ::= { cc6kxbarStatus 1 }

cc6kxbarFabricBackupSlot OBJECT-TYPE
    SYNTAX          ModuleSlotNumber
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "cc6kxbarFabricBackupSlot indicates the slot number of the
        backup switching fabric module. A value of zero indicates 
        that the backup switching fabric module is either powered
        down or not present in the chassis." 
    ::= { cc6kxbarStatus 2 }

cc6kxbarModuleModeTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF Cc6kxbarModuleModeEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "cc6kxbarModuleModeTable indicates the switching mode of each
        module in the system."
    ::= { cc6kxbarStatus 3 }

cc6kxbarModuleModeEntry OBJECT-TYPE
    SYNTAX          Cc6kxbarModuleModeEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in cc6kxbarModuleModeTable. The agent creates
        an entry when a non switching fabric module 
        is inserted in the chassis.
        The agent destroys an entry when a non switching fabric
        module is power down or reset or removed from the chassis."
    INDEX           { cc6kxbarModuleModeModule } 
    ::= { cc6kxbarModuleModeTable 1 }

Cc6kxbarModuleModeEntry ::= SEQUENCE {
        cc6kxbarModuleModeModule        ModuleSlotNumber,
        cc6kxbarModuleModeSwitchingMode INTEGER 
}

cc6kxbarModuleModeModule OBJECT-TYPE
    SYNTAX          ModuleSlotNumber
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION     "The module slot number." 
    ::= { cc6kxbarModuleModeEntry 1 }

cc6kxbarModuleModeSwitchingMode OBJECT-TYPE
    SYNTAX          INTEGER  {
                        busmode(1),
                        crossbarmode(2),
                        dcefmode(3)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "cc6kxbarModuleModeSwitchingMode indicates switching mode
        of the cc6kxbarModuleModeModule.
        'busmode'     -  Modules  in this mode don't use fabric.
                         Backplane is used for both lookup and data
                         forwarding.
        'crossbarmode' -  Modules in this mode use backplane 
                          for forwarding decision and fabric for data 
                          forwarding
        'dcefmode'    -  Modules in this mode use fabric for data 
                         forwarding and local forwarding is enabled." 
    ::= { cc6kxbarModuleModeEntry 2 }
 


cc6kxbarModuleChannelTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF Cc6kxbarModuleChannelEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "cc6kxbarModuleChannelTable shows the operational status
        of fabric channels. This table will be instantiated only when 
        cc6kxbarFabricActiveSlot has a valid value other than zero."
    ::= { cc6kxbarStatus 4 }

cc6kxbarModuleChannelEntry OBJECT-TYPE
    SYNTAX          Cc6kxbarModuleChannelEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION     "An entry in cc6kxbarModuleChannelTable."
    INDEX           {
                        cc6kxbarModuleChannelModule,
                        cc6kxbarModuleChannelChannel
                    } 
    ::= { cc6kxbarModuleChannelTable 1 }

Cc6kxbarModuleChannelEntry ::= SEQUENCE {
        cc6kxbarModuleChannelModule    ModuleSlotNumber,
        cc6kxbarModuleChannelChannel   FabricChannelNumber,
        cc6kxbarModuleChannelModStatus ChannelStatus,
        cc6kxbarModuleChannelFabStatus ChannelStatus,
        cc6kxbarModuleChannelSpeed     Gauge32
}

cc6kxbarModuleChannelModule OBJECT-TYPE
    SYNTAX          ModuleSlotNumber
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION     "The module slot number." 
    ::= { cc6kxbarModuleChannelEntry 1 }

cc6kxbarModuleChannelChannel OBJECT-TYPE
    SYNTAX          FabricChannelNumber
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Fabric channel number of the  cc6kxbarModuleChannelModule." 
    ::= { cc6kxbarModuleChannelEntry 2 }

cc6kxbarModuleChannelModStatus OBJECT-TYPE
    SYNTAX          ChannelStatus
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The status of the fabric channel at the
        cc6kxbarModuleChannelModule." 
    ::= { cc6kxbarModuleChannelEntry 3 }

cc6kxbarModuleChannelFabStatus OBJECT-TYPE
    SYNTAX          ChannelStatus
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The status of the fabric channel at the
        cc6kxbarFabricActiveSlot." 
    ::= { cc6kxbarModuleChannelEntry 4 }

cc6kxbarModuleChannelSpeed OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The speed in mega bits per second of the
        cc6kxbarModuleChannelChannel for cc6kxbarModuleChannelModule." 
    ::= { cc6kxbarModuleChannelEntry 5 }
 

-- Statistics Objects

cc6kxbarStatisticsTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF Cc6kxbarStatisticsEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "cc6kxbarStatisticsTable gives the
        fabric channel counters and utilization
        information.  This table will be instantiated when 
        cc6kxbarFabricActiveSlot has a valid value other than
        zero."
    ::= { cc6kxbarStatistics 1 }

cc6kxbarStatisticsEntry OBJECT-TYPE
    SYNTAX          Cc6kxbarStatisticsEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION     "An entry in cc6kxbarStatisticsTable."
    INDEX           {
                        cc6kxbarStatisticsModule,
                        cc6kxbarStatisticsChannel
                    } 
    ::= { cc6kxbarStatisticsTable 1 }

Cc6kxbarStatisticsEntry ::= SEQUENCE {
        cc6kxbarStatisticsModule         ModuleSlotNumber,
        cc6kxbarStatisticsChannel        FabricChannelNumber,
        cc6kxbarStatisticsInErrors       Counter32,
        cc6kxbarStatisticsOutErrors      Counter32,
        cc6kxbarStatisticsOutDropped     Counter32,
        cc6kxbarStatisticsInUtil         Percent,
        cc6kxbarStatisticsOutUtil        Percent,
        cc6kxbarStatisticsPeakInUtil     Percent,
        cc6kxbarStatisticsPeakTmInUtil   DateAndTime,
        cc6kxbarStatisticsPeakOutUtil    Percent,
        cc6kxbarStatisticsPeakTmOutUtil  DateAndTime
}

cc6kxbarStatisticsModule OBJECT-TYPE
    SYNTAX          ModuleSlotNumber
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION     "The module slot number." 
    ::= { cc6kxbarStatisticsEntry 1 }

cc6kxbarStatisticsChannel OBJECT-TYPE
    SYNTAX          FabricChannelNumber
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Fabric channel number associated with the
        cc6kxbarStatisticsModule." 
    ::= { cc6kxbarStatisticsEntry 2 }

cc6kxbarStatisticsInErrors OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of error packets received on
        cc6kxbarStatisticsChannel for cc6kxbarStatisticsModule
        since this entry was last initialized." 
    ::= { cc6kxbarStatisticsEntry 3 }

cc6kxbarStatisticsOutErrors OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of error packets transmitted on
        cc6kxbarStatisticsModule through the 
        cc6kxbarStatisticsChannel since this entry was 
        last initialized." 
    ::= { cc6kxbarStatisticsEntry 4 }

cc6kxbarStatisticsOutDropped OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of  dropped packets transmitted on the
        cc6kxbarStatisticsChannel for cc6kxbarStatisticsModule
        since this entry was last initialized." 
    ::= { cc6kxbarStatisticsEntry 5 }

cc6kxbarStatisticsInUtil OBJECT-TYPE
    SYNTAX          Percent
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Input utilization of the cc6kxbarStatisticsChannel for
        cc6kxbarStatisticsModule." 
    ::= { cc6kxbarStatisticsEntry 6 }

cc6kxbarStatisticsOutUtil OBJECT-TYPE
    SYNTAX          Percent
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Output utilization of the cc6kxbarStatisticsChannel for
        cc6kxbarStatisticsModule." 
    ::= { cc6kxbarStatisticsEntry 7 }
 
cc6kxbarStatisticsPeakInUtil  OBJECT-TYPE
    SYNTAX Percent
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Indicates the peak value of cc6kxbarStatisticsInUtil of the 
         cc6kxbarStatisticsChannel for cc6kxbarStatisticsModule."
    ::= {cc6kxbarStatisticsEntry 8}

cc6kxbarStatisticsPeakTmInUtil   OBJECT-TYPE
    SYNTAX DateAndTime 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Indicates the time of most recent change in the corresponding 
         instance value of cc6kxbarStatisticsPeakInUtil."
    ::= {cc6kxbarStatisticsEntry 9}

cc6kxbarStatisticsPeakOutUtil   OBJECT-TYPE
    SYNTAX Percent
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Indicates the peak value of cc6kxbarStatisticsOutUtil of the 
         cc6kxbarStatisticsChannel for cc6kxbarStatisticsModule."
    ::= {cc6kxbarStatisticsEntry 10}

cc6kxbarStatisticsPeakTmOutUtil   OBJECT-TYPE
    SYNTAX DateAndTime 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Indicates the time of most recent change in the corresponding
         instance value of cc6kxbarStatisticsPeakOutUtil."
    ::= {cc6kxbarStatisticsEntry 11}

cc6kxbarErrorTable OBJECT-TYPE
    SYNTAX SEQUENCE OF Cc6kxbarErrorEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "cc6kxbarErrorTable provides the fabric channel error 
         information. This table will be instantiated only when 
         cc6kxbarFabricActiveSlot has a valid value other than zero."
    ::= { cc6kxbarStatistics 2 }

cc6kxbarErrorEntry OBJECT-TYPE
    SYNTAX Cc6kxbarErrorEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "An entry in cc6kxbarErrorTable for a specific fabric channel
         on a specific module."  
    INDEX { cc6kxbarErrorModule, cc6kxbarErrorChannel }
    ::= { cc6kxbarErrorTable 1 }

Cc6kxbarErrorEntry ::= SEQUENCE {
    cc6kxbarErrorModule         ModuleSlotNumber,
    cc6kxbarErrorChannel        FabricChannelNumber,
    cc6kxbarErrorModuleCrc      Gauge32,
    cc6kxbarErrorModuleHbeat    Gauge32,
    cc6kxbarErrorModuleSync     Gauge32,
    cc6kxbarErrorModuleDDRSync  Gauge32,
    cc6kxbarErrorChannelSync    Gauge32,
    cc6kxbarErrorChannelBuffer  Gauge32,
    cc6kxbarErrorChannelTimeout Gauge32
    }

cc6kxbarErrorModule  OBJECT-TYPE
    SYNTAX ModuleSlotNumber
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The module slot number."
    ::= { cc6kxbarErrorEntry 1 }

cc6kxbarErrorChannel OBJECT-TYPE
    SYNTAX FabricChannelNumber
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Fabric channel number associated with the  
         cc6kxbarErrorModule."
    ::= { cc6kxbarErrorEntry 2 }

cc6kxbarErrorModuleCrc  OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Indicates the total number of CRC error packets for the
         cc6kxbarErrorChannel of the cc6kxbarErrorModule." 
    ::= { cc6kxbarErrorEntry 3 }

cc6kxbarErrorModuleHbeat  OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Indicates the total number of heartbeat misses detected 
         for the cc6kxbarErrorChannel of the cc6kxbarErrorModule."
    ::= { cc6kxbarErrorEntry 4 }

cc6kxbarErrorModuleSync  OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Indicates the total number of times cc6kxbarErrorModule could 
         not sync to the active switching fabric module."
    ::= { cc6kxbarErrorEntry 5 }

cc6kxbarErrorModuleDDRSync  OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Indicates the total number of DDR(Double Data Rate) channel
         sync errors for the cc6kxbarErrorChannel of the 
         cc6kxbarErrorModule."
    ::= { cc6kxbarErrorEntry 6 }

cc6kxbarErrorChannelSync  OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Indicates the total number of sync errors received at
         cc6kxbarErrorChannel." 
    ::= { cc6kxbarErrorEntry 7 }

cc6kxbarErrorChannelBuffer  OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Indicates the total number of times the memory buffer for
         cc6kxbarErrorChannel of the cc6kxbarErrorModule is full." 
    ::= { cc6kxbarErrorEntry 8 }

cc6kxbarErrorChannelTimeout  OBJECT-TYPE
    SYNTAX Gauge32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Indicates the total number of timeouts for input from
         the cc6kxbarErrorChannel of the cc6kxbarErrorModule." 
    ::= { cc6kxbarErrorEntry 9 }

-- Switching Bus Objects
cc6kxbarSwBusSwitchingStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        normal(1),
                        stalled(2),
                        isolated(3)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Indicates the current switching status of the
        switching bus on the system. 

        normal -- the switching bus is under normal 
                  packet switching operation.

        stalled -- the switching bus has stopped packet 
                   switching but is still attached to
                   the system, i.e., the switching bus
                   is stalled. 

        isolated -- the switching bus has stopped packet 
                   switching and is detached from 
                   the system, i.e., the switching bus 
                   is isolated.

        The object is only instantiated on systems which 
        support switching bus switching detection feature." 
    ::= { cc6kxbarSwBusObjects 1 }

cc6kxbarSwBusFailureDuration OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Indicates the failure duration of the switching
        bus since the switching bus has transitioned 
        out of the normal(1) state as monitored by  
        cc6kxbarSwBusSwitchingStatus. If the object 
        value of cc6kxbarSwBusSwitchingStatus is 
        normal(1), then the object value of 
        cc6kxbarSwBusFailureDuration should be zero.

        The object is only instantiated on systems which
        support switching bus switching detection feature." 
    ::= { cc6kxbarSwBusObjects 2 }

cc6kxbarSwBusNotifEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Indicates whether or not the notification
        cc6kxbarSwBusStatusChangeNotif should be generated 
        when there is change in the switching status of the 
        switching bus as monitored by 
        cc6kxbarSwBusSwitchingStatus.

        The object is only instantiated on systems which
        support switching bus switching detection feature." 
    ::= { cc6kxbarSwBusObjects 3 }

cc6kxbarSwBusUtilization OBJECT-TYPE
        SYNTAX          Percent
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
             "Indicates the percentage of bandwidth utilization
              of the switching bus."
        ::= { cc6kxbarSwBusObjects 4 }

cc6kxbarSwBusPeakUtilization OBJECT-TYPE
        SYNTAX          Percent
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
             "Indicates the peak percentage value of bandwidth 
              utilization of the switching bus since the system 
              started."
        ::= { cc6kxbarSwBusObjects 5 }

cc6kxbarSwBusPeakTimeUtil OBJECT-TYPE
        SYNTAX          DateAndTime
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
             "Indicates the time at which the peak percentage value 
              of bandwidth utilization of the switching bus value 
              occurred."
        ::= { cc6kxbarSwBusObjects 6 }

-- Internal Bus Objects
cc6kxbarIntBusNotifEnable OBJECT-TYPE
    SYNTAX          BITS {
                        intBusCRCErrExcd(0),
                        intBusCRCErrRcvrd(1)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Indicates whether the generation of a specified
        notification for internal bus is enabled or not. 
        If a bit corresponding to a notification is set to 
        1, then that notification can be generated.

        intBusCRCErrExcd -- the cc6kxbarIntBusCRCErrExcdNotif 
                            notification.

        intBusCRCErrRcvrd -- the cc6kxbarIntBusCRCErrRcvrdNotif
                            notification.
        " 
    ::= { cc6kxbarIntBusObjects 1 }

cc6kxbarIntBusCRCErrTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF Cc6kxbarIntBusCRCErrEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table containing internal bus CRC error information
        on a list of physical entities (such as modules)."
    ::= { cc6kxbarIntBusObjects 2 }

cc6kxbarIntBusCRCErrEntry OBJECT-TYPE
    SYNTAX          Cc6kxbarIntBusCRCErrEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry containing internal bus CRC error information
        on a physical entity (such as a module)."
    INDEX           { entPhysicalIndex } 
    ::= { cc6kxbarIntBusCRCErrTable 1 }

Cc6kxbarIntBusCRCErrEntry ::= SEQUENCE {
        cc6kxbarIntBusCRCErrExcdStatus TruthValue,
        cc6kxbarIntBusCRCErrExcdCount  Unsigned32
}

cc6kxbarIntBusCRCErrExcdStatus OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Indicates whether the internal bus CRC error
        on a physical entity is currently exceeding the fatal 
        threshold or not." 
    ::= { cc6kxbarIntBusCRCErrEntry 1 }

cc6kxbarIntBusCRCErrExcdCount OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Indicates the number of times the internal bus CRC
        error on a physical entity has exceeded the fatal 
        threshold." 
    ::= { cc6kxbarIntBusCRCErrEntry 2 }
 


-- Flow Control Objects
cc6kxbarFlowCtrlNotifEnable OBJECT-TYPE
    SYNTAX          BITS {
                        busThreshExcd(0)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Specifies whether the generation of a specified
        notification for flow control feature is enabled or
        not. If a bit corresponding to a notification is set
        to one, then that notification can be generated.

        busThreshExcd -- the cc6kxbarFlowCtrlBusThrExcdNotif
                            notification.
        " 
    ::= { cc6kxbarFlowCtrlObjects 1 }

cc6kxbarFlowCtrlBusFIFOThrMode OBJECT-TYPE
    SYNTAX          INTEGER  {
                        off(1),
                        on(2),
                        auto(3)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Specifies the mode configuration of the system bus
        flow control FIFO threshold.

        off -- the flow control FIFO threshold is set to the
              original value defined by the system.

        on -- the flow control FIFO threshold is set to the
              lower value defined by the system.

        auto -- the system starts monitoring the system bus
              flow control FIFO threshold and will change the
              flow control FIFO threshold from the original
              value to the lower value when the system detects
              the first occurrence of the threshold exceeding
              on a physical entity (such as a module) over
              the system allowed limit." 
    ::= { cc6kxbarFlowCtrlObjects 2 }

cc6kxbarFlowCtrlBusFIFOThrValue OBJECT-TYPE
    SYNTAX          INTEGER  {
                        original(1),
                        lower(2)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Indicates the current value of the system bus flow
        control FIFO threshold, whether it is the original
        value or the lower value." 
    ::= { cc6kxbarFlowCtrlObjects 3 }

cc6kxbarFlowCtrlBusFIFOTransTime OBJECT-TYPE
    SYNTAX          TimeStamp
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Indicates the value of sysUpTime at the time
        that the system bus flow control FIFO threshold
        is transitioned to lower value when the object value 
        of  cc6kxbarFlowCtrlBusFIFOThrValue is 'lower'. This
        object will take on the value of zero when the object
        value of cc6kxbarFlowCtrlBusFIFOThrValue is 
        'original'." 
    ::= { cc6kxbarFlowCtrlObjects 4 }

-- System Capacity Objects

cc6kxbarSysCapPfcOperMode OBJECT-TYPE
        SYNTAX          INTEGER {
                                  unknown(1),
                                  pfc3a(2),
                                  pfc3b(3),
                                  pfc3bxl(4),
                                  pfc3cst1(5),
                                  pfc3cxlst1(6),
                                  pfc3c(7),
                                  pfc3cxl(8),
                                  pfc4(9),
                                  pfc4xl(10)   
                        }
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
             "Indicates the operating mode of the policy feature
             card (PFC).

             unknown -- unknown.

             pfc3a -- Policy feature card 3A.

             pfc3b -- Policy feature card 3B.

             pfc3bxl -- Policy feature card 3B XL.

             pfc3cst1 -- Policy feature card 3C ST1.

             pfc3cxlst1 -- Policy feature card 3C XL ST1.

             pfc3c -- Policy feature card 3C.

             pfc3cxl -- Policy feature card 3C XL.  

             pfc4 -- Policy feature card 4.

             pfc4xl -- Policy feature card 4 XL.
             "
        ::= { cc6kxbarSystemCapacityObjects 1 }

cc6kxbarSysCapSwitchResTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF Cc6kxbarSysCapSwitchResEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A cc6kxbarSysCapSwitchResTable entry lists 
        the capacity information of the switching 
        resources for ENTITY-MIB entPhysicalTable entries 
        of manageable components with type entPhysicalClass 
        module(9).
        "
    ::= { cc6kxbarSystemCapacityObjects 2 } 

cc6kxbarSysCapSwitchResEntry OBJECT-TYPE
    SYNTAX  Cc6kxbarSysCapSwitchResEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A cc6kxbarSysCapSwitchResEntry entry lists 
        the capacity information of the switching 
        resources for ENTITY-MIB entPhysicalTable entries
        of manageable components with type entPhysicalClass 
        module(9).

        Entries are created by the agent at the system power-up
        or module insertion.
      
        Entries are deleted by the agent upon module removal.
        "
    INDEX   { entPhysicalIndex } 
    ::= { cc6kxbarSysCapSwitchResTable 1 }

Cc6kxbarSysCapSwitchResEntry ::= SEQUENCE {
    cc6kxbarSysCapSwitchResSeries   INTEGER,
    cc6kxbarSysCapSwitchResCefMode  INTEGER 
}  

cc6kxbarSysCapSwitchResSeries OBJECT-TYPE
    SYNTAX        INTEGER {
                            unknown(1),
                            supervisor(2),
                            classic(3),
                            fabric(4),
                            dcef720(5),
                            cef720(6),
                            dcef256(7),
                            cef256(8) 
                  }                        
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Indicates the module series for traffic forwarding options. 

        unknown -- unknown.

        supervisor -- supervisor module.

        classic -- classic module.

        fabric -- fabric module.
 
        dcef720 -- dCEF720 module.

        cef720 -- CEF720 module.

        dcef256 -- dCEF256 module.

        cef256 -- CEF256 module. 
        "
    ::= { cc6kxbarSysCapSwitchResEntry 1 }

cc6kxbarSysCapSwitchResCefMode OBJECT-TYPE
    SYNTAX        INTEGER {
                            notApplicable(1),
                            dcef(2),
                            cef(3)
                  }                        
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Indicates the Cisco Express Forwarding (CEF) mode of 
        the module.  

        notApplicable -- not applicable for this module.

        dcef -- distributed CEF.

        cef -- CEF. 
        "
    ::= { cc6kxbarSysCapSwitchResEntry 2 }

-- Fabric Error Recovery Objects 

cc6kxbarErrRcvryThreshLink OBJECT-TYPE
    SYNTAX        Unsigned32 (1..4294967295)
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "Specifies the threshold on fabric link errors occurring 
        in a channel for the fabric error recovery feature." 
    ::= { cc6kxbarErrorRecoveryObjects 1 }

cc6kxbarErrRcvryThreshPersLink OBJECT-TYPE
    SYNTAX        Unsigned32 (1..4294967295)
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "Specifies the threshold on persistent fabric link errors
        occurring in a channel for the fabric error recovery feature."
    ::= { cc6kxbarErrorRecoveryObjects 2 }

cc6kxbarErrRcvrySwitchoverEnable OBJECT-TYPE
    SYNTAX        TruthValue 
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "Specifies whether the switchover to the standby fabric module 
        is enabled or not on the detection of excessive fabric link 
        errors occurring in a channel for the fabric error recovery 
        feature."
    ::= { cc6kxbarErrorRecoveryObjects 3 }

cc6kxbarErrRcvryPersLinkResync OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "Specifies whether the system will resync the channel or not
        on the detection of excessive persistent fabric link errors
        in a channel for the fabric error recovery feature." 
    ::= { cc6kxbarErrorRecoveryObjects 4 }
    
cc6kxbarErrRcvryChResyncCount OBJECT-TYPE
    SYNTAX        Unsigned32 (1..4294967295)
    MAX-ACCESS    read-write 
    STATUS        current
    DESCRIPTION
        "Specifies the consecutive number of times of
        channel resync within the time interval as specified
        by cc6kxbarErrRcvryChResyncInterval, over which  
        the channel resync is considered as failure 
        for the fabric error recovery feature."  
    ::= { cc6kxbarErrorRecoveryObjects 5 }

cc6kxbarErrRcvryChResyncInterval OBJECT-TYPE
    SYNTAX        Unsigned32 (1..4294967295)
    UNITS         "milliseconds"
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "Specifies the time interval for the consecutive
        counting of channel resync for the fabric error
        recovery feature."
    ::= { cc6kxbarErrorRecoveryObjects 6 }

--Traffic Monitor Objects

cc6kxbarTMSwBusUtilEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Specifies whether the traffic monitor feature is 
         enabled on the switching bus or not."
    ::= { cc6kxbarTrafficMonitorSwBusObjects 1 }

cc6kxbarTMSwBusUtilInterval OBJECT-TYPE
    SYNTAX        Unsigned32 (1..4294967295)
    UNITS         "seconds"
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "Specifies the interval at the end of which 
         the switching bus traffic utilization is compared 
         against cc6kxbarTMSwBusUtilThreshold."
    ::= { cc6kxbarTrafficMonitorSwBusObjects 2 }

cc6kxbarTMSwBusUtilThreshold OBJECT-TYPE
    SYNTAX        Percent
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "Specifies the threshold of the switching bus 
         traffic utilization."
    ::= { cc6kxbarTrafficMonitorSwBusObjects 3 }

cc6kxbarTMSwBusUtilLogCount OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Indicates the number of times the following
         events are logged for the switching bus:

         1. the switching bus traffic utilization has 
         risen above the configured threshold (as 
         specified by cc6kxbarTMSwBusUtilThreshold),
         or has kept staying above the configured 
         threshold at a logging interval (as specified
         by cc6kxbarTMSwBusUtilLogInterval).

         2. the switching bus traffic utilization
         has fallen below the configured threshold."
    ::= { cc6kxbarTrafficMonitorSwBusObjects 4 }

cc6kxbarTMSwBusUtilLastLogTime OBJECT-TYPE
    SYNTAX        DateAndTime
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Indicates the last logging time of the 
         events as counted in cc6kxbarTMSwBusUtilLogCount.  

         This object will contain 0-1-1,00:00:00.0 when
         the value of cc6kxbarTMSwBusUtilLogCount is zero."
    ::= { cc6kxbarTrafficMonitorSwBusObjects 5 }

cc6kxbarTMSwBusUtilLogInterval OBJECT-TYPE
    SYNTAX        Unsigned32 (1..4294967295)
    UNITS         "seconds"
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "Specifies the logging interval if the switching
         bus traffic utilization keeps staying above the
         cc6kxbarTMSwBusUtilThreshold."
    ::= { cc6kxbarTrafficMonitorSwBusObjects 6 }

cc6kxbarTMSwBusUtilUtilization OBJECT-TYPE
    SYNTAX        Percent
    MAX-ACCESS    accessible-for-notify
    STATUS        current
    DESCRIPTION
        "The switching bus traffic utilization included 
         in the notification currently being sent."  
    ::= { cc6kxbarTrafficMonitorSwBusObjects 7 }

cc6kxbarTMSwBusUtilNotifEnable OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
        "Specifies whether the generation of 
         c6kxbarTMSwBusUtilAboveNotif and 
         c6kxbarTMSwBusUtilBelowNotif notifications
         is enabled or not.
 
         When this object is 'true', the generation of
         cc6kxbarTMSwBusUtilAboveNotif and 
         c6kxbarTMSwBusUtilBelowNotif notifications is
         enabled. When this object is 'false', the 
         generation of cc6kxbarTMSwBusUtilAboveNotif and 
         c6kxbarTMSwBusUtilBelowNotif notifications 
         is disabled."
    ::= { cc6kxbarTrafficMonitorSwBusObjects 8 }

cc6kxbarTMChUtilTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF Cc6kxbarTMChUtilEntry 
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "cc6kxbarTrafficMntrChUtilTable provides the 
         information on the traffic utilization of each 
         fabric channel associated with each module slot
         for a given traffic direction in the chassis."  
    ::= { cc6kxbarTrafficMonitorChObjects 1 }

cc6kxbarTMChUtilEntry OBJECT-TYPE
    SYNTAX        Cc6kxbarTMChUtilEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "An entry in cc6kxbarTMChUtilTable. Each traffic
         direction for each fabric channel associated with
         each module slot in the chassis will have an 
         entry in this table." 
    INDEX         { 
                      cc6kxbarTMChUtilModule, 
                      cc6kxbarTMChUtilChannel, 
                      cc6kxbarTMChUtilDirection 
                  } 
    ::= { cc6kxbarTMChUtilTable 1 }

Cc6kxbarTMChUtilEntry ::= SEQUENCE {
     cc6kxbarTMChUtilModule          ModuleSlotNumber,
     cc6kxbarTMChUtilChannel         FabricChannelNumber,
     cc6kxbarTMChUtilDirection       INTEGER,
     cc6kxbarTMChUtilEnable          TruthValue,
     cc6kxbarTMChUtilInterval        Unsigned32,
     cc6kxbarTMChUtilThreshold       Percent,
     cc6kxbarTMChUtilLogCount        Counter32,
     cc6kxbarTMChUtilLastLogTime     DateAndTime 
}

cc6kxbarTMChUtilModule  OBJECT-TYPE
    SYNTAX        ModuleSlotNumber
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "Indicates the module slot number in the chassis."  
    ::= { cc6kxbarTMChUtilEntry 1 }

cc6kxbarTMChUtilChannel OBJECT-TYPE
    SYNTAX        FabricChannelNumber
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "Indicates the fabric channel number associated with
         the corresponding cc6kxbarTMChUtilModule." 
    ::= { cc6kxbarTMChUtilEntry 2 }

cc6kxbarTMChUtilDirection OBJECT-TYPE
    SYNTAX        INTEGER {
                              ingress(1),
                              egress(2)
                           }
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
         "Indicates the direction of traffic to be monitored."
    ::= { cc6kxbarTMChUtilEntry 3 }

cc6kxbarTMChUtilEnable OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
        "Specifies whether the traffic monitor feature is
         enabled on a fabric channel for a given traffic
         direction or not." 
    ::= { cc6kxbarTMChUtilEntry 4 }

cc6kxbarTMChUtilInterval OBJECT-TYPE
    SYNTAX        Unsigned32 (1..4294967295)
    UNITS         "seconds"
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "Specifies the interval at the end of which the
         traffic utilization on a fabric channel for a 
         given traffic direction is compared against 
         its corresponding cc6kxbarTMChUtilThreshold."
    ::= { cc6kxbarTMChUtilEntry 5 }

cc6kxbarTMChUtilThreshold OBJECT-TYPE
    SYNTAX        Percent
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "Specifies the threshold of the traffic utilization
         on a fabric channel for a given traffic direction."
    ::= { cc6kxbarTMChUtilEntry 6 }

cc6kxbarTMChUtilLogCount OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Indicates the number of times the following
         events are logged on a fabric channel
         for a given direction.
    
         1. the traffic utilization on a fabric channel 
         for a given traffic direction has risen above its 
         corresponding configured threshold (as specified 
         by cc6kxbarTMChUtilThreshold), or has kept 
         staying above the configured threshold at a 
         logging interval (as specified by 
         cc6kxbarTMChUtilLogInterval).
    
         2. the traffic utilization on a fabric channel
         for a given traffic direciton has fallen below 
         its corresponding configured threshold."
    ::= { cc6kxbarTMChUtilEntry 7 }

cc6kxbarTMChUtilLastLogTime OBJECT-TYPE
    SYNTAX        DateAndTime
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Indicates the last logging time of the 
         events as counted in the corresponding
         cc6kxbarTMChUtilLogCount on a fabric channel 
         for a given traffic direction.

         This object will contain 0-1-1,00:00:00.0 when
         the corresponding cc6kxbarTMChUtilLogCount is zero."
         ::= { cc6kxbarTMChUtilEntry 8 }

cc6kxbarTMChUtilLogInterval OBJECT-TYPE
    SYNTAX        Unsigned32 (1..4294967295)
    UNITS         "seconds"
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "Specifies the logging interval if the traffic 
         utilization for a fabric channel on a given
         traffic direction keeps staying above its 
         corresponding cc6kxbarTMChUtilThreshold." 
    ::= { cc6kxbarTrafficMonitorChObjects 2 }

cc6kxbarTMChUtilUtilization OBJECT-TYPE
    SYNTAX          Percent
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
       "The traffic utilization on a fabric channel
        for a given traffic direciton included in the 
        notification currently being sent."
    ::= { cc6kxbarTrafficMonitorChObjects 3 }

cc6kxbarTMChUtilNotifEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
       "Specifies whether the generation of 
        cc6kxbarTMChUtilAboveNotif and cc6kxbarTMChUtilBelowNotif
        notifications is enabled or not.

        When this object is 'true', the generation of
        cc6kxbarTMChUtilAboveNotif and cc6kxbarTMChUtilBelowNotif
        notifications is enabled. When this object is 'false', 
        the generation of cc6kxbarTMChUtilAboveNotif and 
        cc6kxbarTMChUtilBelowNotif notifications is disabled."
        ::= { cc6kxbarTrafficMonitorChObjects 4 }

-- Notifications
ciscoCat6kXbarMIBNotifs  OBJECT IDENTIFIER
    ::= { ciscoCat6kCrossbarMIB 0 }



cc6kxbarSwBusStatusChangeNotif NOTIFICATION-TYPE
    OBJECTS         {
                        cc6kxbarSwBusSwitchingStatus,
                        cc6kxbarSwBusFailureDuration
                    }
    STATUS          current
    DESCRIPTION
        "A cc6kxbarSwBusStatusChangeNotif notification
        is sent by the the device when there is change
        in switching status of the switching bus as 
        monitored by cc6kxbarSwBusSwitchingStatus."
   ::= { ciscoCat6kXbarMIBNotifs 1 }


cc6kxbarIntBusCRCErrExcdNotif NOTIFICATION-TYPE
    OBJECTS         {
                        entPhysicalName,
                        entPhysicalVendorType
                    }
    STATUS          current
    DESCRIPTION
        "A cc6kxbarIntBusCRCThreshExcdNotif notification
        is sent by the system when the system has
        detected that the internal bus CRC error on
        a physical entity (such as a module) as specified
        by entPhysicalName has exceeded the fatal threshold."
   ::= { ciscoCat6kXbarMIBNotifs 2 }


cc6kxbarIntBusCRCErrRcvrdNotif NOTIFICATION-TYPE
    OBJECTS         {
                        entPhysicalName,
                        entPhysicalVendorType
                    }
    STATUS          current
    DESCRIPTION
        "A cc6kxbarIntBusCRCErrRcvrdNotif notification
        is sent by the system when the system has
        recovered as the internal bus CRC error on
        a physical entity (such as a module) as
        specified by entPhysicalName has fallen below
        the normal threshold."
   ::= { ciscoCat6kXbarMIBNotifs 3 }


cc6kxbarFlowCtrlBusThrExcdNotif NOTIFICATION-TYPE
    OBJECTS         {
                        entPhysicalName,
                        entPhysicalVendorType
                    }
    STATUS          current
    DESCRIPTION
        "A cc6kxbarFlowCtrlBusThrExcdNotif notification
        is sent by the system when the system detects the
        first occurrence of the system bus flow control FIFO
        threshold exceeding on a physical entity
        (such as a module) over the system allowed limit
        when the object value of
        cc6kxbarFlowCtrlBusFIFOThrMode is 'auto'."
   ::= { ciscoCat6kXbarMIBNotifs 4 }

cc6kxbarTMSwBusUtilAboveNotif NOTIFICATION-TYPE
    OBJECTS         {
                        cc6kxbarTMSwBusUtilUtilization,
                        cc6kxbarTMSwBusUtilThreshold,
                        cc6kxbarTMSwBusUtilInterval,
                        entPhysicalDescr
                    }
    STATUS          current
    DESCRIPTION
        "This notification is sent when the switching bus 
         traffic utilization has risen above the configured 
         threshold (as specified by 
         cc6kxbarTMSwBusUtilThreshold), or has kept staying
         above the configured threshold at a logging interval 
         (as specified by cc6kxbarTMSwBusUtilLogInterval).
         The varbind entPhysicalDescr specifies the physical 
         entity (such as chassis) for which the 
         cc6kxbarTMSwBusUtilAboveNotif is sent."
   ::= { ciscoCat6kXbarMIBNotifs 5 }

cc6kxbarTMSwBusUtilBelowNotif NOTIFICATION-TYPE
    OBJECTS         {
                        cc6kxbarTMSwBusUtilUtilization,
                        cc6kxbarTMSwBusUtilThreshold,
                        cc6kxbarTMSwBusUtilInterval,
                        entPhysicalDescr
                    }
    STATUS          current
    DESCRIPTION
        "This notification is sent when the switching bus 
         traffic utilization has fallen below the configured 
         threshold (as specified by 
         cc6kxbarTMSwBusUtilThreshold). The varbind 
         entPhysicalDescr specifies the physical entity 
         (such as chassis) for which the 
         cc6kxbarTMSwBusUtilBelowNotif is sent." 
    ::= { ciscoCat6kXbarMIBNotifs 6 }

cc6kxbarTMChUtilAboveNotif NOTIFICATION-TYPE
    OBJECTS         {
                        cc6kxbarTMChUtilUtilization,
                        cc6kxbarTMChUtilThreshold,
                        cc6kxbarTMChUtilInterval,
                        entPhysicalDescr
                    }
    STATUS          current
    DESCRIPTION
        "This notification is sent when the traffic 
         utilization on a fabric channel for a given 
         traffic direction has risen above its 
         corresponding configured threshold (as 
         specified by cc6kxbarTMChUtilThreshold), or has 
         kept staying above the configured threshold at a 
         logging interval (as specified by 
         cc6kxbarTMChUtilLogInterval). The varbind 
         entPhysicalDescr specifies the physical entity 
         (such as chassis) for which the 
         cc6kxbarTMChUtilAboveNotif is sent."
   ::= { ciscoCat6kXbarMIBNotifs 7 }

cc6kxbarTMChUtilBelowNotif NOTIFICATION-TYPE
    OBJECTS         {
                        cc6kxbarTMChUtilUtilization,
                        cc6kxbarTMChUtilThreshold,
                        cc6kxbarTMChUtilInterval,
                        entPhysicalDescr
                    }
    STATUS          current
    DESCRIPTION
        "This notification is sent when the traffic 
         utilization on a fabric channel for a given 
         traffic direction has fallen below its 
         corresponding configured threshold (as 
         specified by cc6kxbarTMChUtilThreshold). The 
         varbind entPhysicalDescr specifies the 
         physical entity (such as chassis) for which
         the cc6kxbarTMChUtilBelowNotif is sent."
    ::= { ciscoCat6kXbarMIBNotifs 8 }

-- Conformance and Compliance
cc6kxbarMIBConformance  OBJECT IDENTIFIER
    ::= { ciscoCat6kCrossbarMIB 3 }

cc6kxbarMIBCompliances  OBJECT IDENTIFIER
    ::= { cc6kxbarMIBConformance 1 }

cc6kxbarMIBGroups  OBJECT IDENTIFIER
    ::= { cc6kxbarMIBConformance 2 }


-- Conformance
cc6kxbarMIBCompliance MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for
        the CISCO-CAT6K-CROSSBAR-MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cc6kxbarModuleStatusGroup,
                        cc6kxbarChannelStatusGroup,
                        cc6kxbarChannelStatisticsGroup
                    }

    GROUP           cc6kxbarFallbackGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support fallback mode feature."

    GROUP           cc6kxbarBusOnlyAllowedGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support busonly  mode feature."
    ::= { cc6kxbarMIBCompliances 2 }

cc6kxbarMIBComplianceVer1 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for
        the CISCO-CAT6K-CROSSBAR-MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cc6kxbarModuleStatusGroupVer1,
                        cc6kxbarChannelStatusGroup,
                        cc6kxbarChannelStatisticsGroupVer1
                    }

    GROUP           cc6kxbarFallbackGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support fallback mode feature."

    GROUP           cc6kxbarBusOnlyAllowedGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support bus only mode feature."

    GROUP           cc6kxbarLcdBannerGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support lcd banner feature."

    GROUP           cc6kxbarChannelUtilGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support Input and Output traffic utilization on the 
        fabric channel."

    GROUP           cc6kxbarChannelSpeedGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support fabric channel speed feature."

    GROUP           cc6kxbarSwBusGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        switching bus switching detection feature."

    GROUP           cc6kxbarSwBusNotifGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        switching bus switching detection notification 
        feature."
    ::= { cc6kxbarMIBCompliances 3 }

cc6kxbarMIBComplianceVer2 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for
        the CISCO-CAT6K-CROSSBAR-MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cc6kxbarModuleStatusGroupVer1,
                        cc6kxbarChannelStatusGroup,
                        cc6kxbarChannelStatisticsGroupVer1
                    }

    GROUP           cc6kxbarFallbackGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support fallback mode feature."

    GROUP           cc6kxbarBusOnlyAllowedGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support bus only mode feature."

    GROUP           cc6kxbarLcdBannerGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support lcd banner feature."

    GROUP           cc6kxbarChannelUtilGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support Input and Output traffic utilization on the 
        fabric channel."

    GROUP           cc6kxbarChannelSpeedGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support fabric channel speed feature."

    GROUP           cc6kxbarSwBusGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        switching bus switching detection feature."

    GROUP           cc6kxbarSwBusNotifGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        switching bus switching detection notification 
        feature."

    GROUP           cc6kxbarTruncatedOperGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        operational truncated mode."
    ::= { cc6kxbarMIBCompliances 4 }

cc6kxbarMIBComplianceVer3 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for
        the CISCO-CAT6K-CROSSBAR-MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cc6kxbarModuleStatusGroupVer1,
                        cc6kxbarChannelStatusGroup,
                        cc6kxbarChannelStatisticsGroupVer1
                    }

    GROUP           cc6kxbarFallbackGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support fallback mode feature."

    GROUP           cc6kxbarBusOnlyAllowedGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support bus only mode feature."

    GROUP           cc6kxbarLcdBannerGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support lcd banner feature."

    GROUP           cc6kxbarChannelUtilGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support Input and Output traffic utilization on the 
        fabric channel."

    GROUP           cc6kxbarChannelSpeedGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support fabric channel speed feature."

    GROUP           cc6kxbarSwBusGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        switching bus switching detection feature."

    GROUP           cc6kxbarSwBusNotifGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        switching bus switching detection notification 
        feature."

    GROUP           cc6kxbarTruncatedOperGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        operational truncated mode."

    GROUP           cc6kxbarIntBusNotifControlGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        internal bus notifications."

    GROUP           cc6kxbarIntBusCRCErrNotifGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        internal bus CRC error notifications."
    ::= { cc6kxbarMIBCompliances 5 }

cc6kxbarMIBComplianceVer4 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for
        the CISCO-CAT6K-CROSSBAR-MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cc6kxbarModuleStatusGroupVer1,
                        cc6kxbarChannelStatusGroup,
                        cc6kxbarChannelStatisticsGroupVer1
                    }

    GROUP           cc6kxbarFallbackGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support fallback mode feature."

    GROUP           cc6kxbarBusOnlyAllowedGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support bus only mode feature."

    GROUP           cc6kxbarLcdBannerGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support lcd banner feature."

    GROUP           cc6kxbarChannelUtilGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support Input and Output traffic utilization on the 
        fabric channel."

    GROUP           cc6kxbarChannelSpeedGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support fabric channel speed feature."

    GROUP           cc6kxbarSwBusGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        switching bus switching detection feature."

    GROUP           cc6kxbarSwBusNotifGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        switching bus switching detection notification 
        feature."

    GROUP           cc6kxbarTruncatedOperGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        operational truncated mode."

    GROUP           cc6kxbarIntBusNotifControlGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        internal bus notifications."

    GROUP           cc6kxbarIntBusCRCErrNotifGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        internal bus CRC error notifications."

    GROUP           cc6kxbarIntBusCRCErrGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        internal bus CRC error status."
    ::= { cc6kxbarMIBCompliances 6 }

cc6kxbarMIBComplianceVer5 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for
        the CISCO-CAT6K-CROSSBAR-MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cc6kxbarModuleStatusGroupVer1,
                        cc6kxbarChannelStatusGroup,
                        cc6kxbarChannelStatisticsGroupVer1
                    }

    GROUP           cc6kxbarFallbackGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support fallback mode feature."

    GROUP           cc6kxbarBusOnlyAllowedGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support bus only mode feature."

    GROUP           cc6kxbarLcdBannerGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support lcd banner feature."

    GROUP           cc6kxbarChannelUtilGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support Input and Output traffic utilization on the 
        fabric channel."

    GROUP           cc6kxbarChannelSpeedGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support fabric channel speed feature."

    GROUP           cc6kxbarSwBusGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        switching bus switching detection feature."

    GROUP           cc6kxbarSwBusNotifGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        switching bus switching detection notification 
        feature."

    GROUP           cc6kxbarTruncatedOperGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        operational truncated mode."

    GROUP           cc6kxbarIntBusNotifControlGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        internal bus notifications."

    GROUP           cc6kxbarIntBusCRCErrNotifGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        internal bus CRC error notifications."

    GROUP           cc6kxbarIntBusCRCErrGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        internal bus CRC error status."

    GROUP           cc6kxbarDcefOnlyModeAllowedGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        dcef only mode feature."

    GROUP           cc6kxbarForceBusModeGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        force bus mode feature."

    GROUP           cc6kxbarFlowCtrlNotifCtrlGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        the system flow control notification control."

    GROUP           cc6kxbarFlowCtrlBusThreshGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        the system bus flow control FIFO threshold configuration."

    GROUP           cc6kxbarFlowCtrlBusThrNotifGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        the system bus flow control FIFO threshold exceeding
        notification."

    GROUP           cc6kxbarBusOnlyModeOperGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        operational bus mode."
    ::= { cc6kxbarMIBCompliances 7 }

cc6kxbarMIBComplianceVer6 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for
        the CISCO-CAT6K-CROSSBAR-MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cc6kxbarModuleStatusGroupVer1,
                        cc6kxbarChannelStatusGroup,
                        cc6kxbarChannelStatisticsGroupVer1
                    }

    GROUP           cc6kxbarFallbackGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support fallback mode feature."

    GROUP           cc6kxbarBusOnlyAllowedGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support bus only mode feature."

    GROUP           cc6kxbarLcdBannerGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support lcd banner feature."

    GROUP           cc6kxbarChannelUtilGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support Input and Output traffic utilization on the 
        fabric channel."

    GROUP           cc6kxbarChannelSpeedGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support fabric channel speed feature."

    GROUP           cc6kxbarSwBusGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        switching bus switching detection feature."

    GROUP           cc6kxbarSwBusNotifGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        switching bus switching detection notification 
        feature."

    GROUP           cc6kxbarTruncatedOperGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        operational truncated mode."

    GROUP           cc6kxbarIntBusNotifControlGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        internal bus notifications."

    GROUP           cc6kxbarIntBusCRCErrNotifGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        internal bus CRC error notifications."

    GROUP           cc6kxbarIntBusCRCErrGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        internal bus CRC error status."

    GROUP           cc6kxbarDcefOnlyModeAllowedGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        dcef only mode feature."

    GROUP           cc6kxbarForceBusModeGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        force bus mode feature."

    GROUP           cc6kxbarFlowCtrlNotifCtrlGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        the system flow control notification control."

    GROUP           cc6kxbarFlowCtrlBusThreshGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        the system bus flow control FIFO threshold configuration."

    GROUP           cc6kxbarFlowCtrlBusThrNotifGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        the system bus flow control FIFO threshold exceeding
        notification."

    GROUP           cc6kxbarBusOnlyModeOperGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        operational bus mode."

    GROUP           cc6kxbarSysCapPfcOperModeGroup
    DESCRIPTION
        "This group is mandatory only for platforms which
        support the system information of PFC operational mode."
 
    GROUP           cc6kxbarSysCapSwitchResGroup
    DESCRIPTION
        "This group is mandatory only for platforms which
        support the capacity information of switching 
        resources in the system."

    GROUP cc6kxbarChannelUtilGroup1
    DESCRIPTION
         "This group is mandatory only for those platforms which
          support peak input and output traffic utilization on the
          fabric channel."

    GROUP cc6kxbarSwBusGroup1
    DESCRIPTION
        "This group is mandatory only for platforms which support
         switching bus utilization."

    GROUP cc6kxbarErrorGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
         support error statistics on the fabric channel."

    GROUP cc6kxbarErrRcvryThresholdGroup
    DESCRIPTION
       "This group is mandatory for platforms which provide
        the configuration of thresholds on fabric link errors
        for the fabric error recovery feature."

    GROUP cc6kxbarErrRcvrySwitchoverGroup
    DESCRIPTION
       "This group is mandatory for platforms which provide
        the configuration of fabric switchover on excessive fabric 
        link errors for the fabric error recovery feature."

    ::= { cc6kxbarMIBCompliances 8 }

cc6kxbarMIBComplianceVer7 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for
        the CISCO-CAT6K-CROSSBAR-MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cc6kxbarModuleStatusGroupVer1,
                        cc6kxbarChannelStatusGroup,
                        cc6kxbarChannelStatisticsGroupVer1
                    }

    GROUP           cc6kxbarFallbackGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support fallback mode feature."

    GROUP           cc6kxbarBusOnlyAllowedGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support bus only mode feature."

    GROUP           cc6kxbarLcdBannerGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support lcd banner feature."

    GROUP           cc6kxbarChannelUtilGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support Input and Output traffic utilization on the 
        fabric channel."

    GROUP           cc6kxbarChannelSpeedGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
        support fabric channel speed feature."

    GROUP           cc6kxbarSwBusGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        switching bus switching detection feature."

    GROUP           cc6kxbarSwBusNotifGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        switching bus switching detection notification 
        feature."

    GROUP           cc6kxbarTruncatedOperGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        operational truncated mode."

    GROUP           cc6kxbarIntBusNotifControlGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        internal bus notifications."

    GROUP           cc6kxbarIntBusCRCErrNotifGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        internal bus CRC error notifications."

    GROUP           cc6kxbarIntBusCRCErrGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        internal bus CRC error status."

    GROUP           cc6kxbarDcefOnlyModeAllowedGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        dcef only mode feature."

    GROUP           cc6kxbarForceBusModeGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        force bus mode feature."

    GROUP           cc6kxbarFlowCtrlNotifCtrlGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        the system flow control notification control."

    GROUP           cc6kxbarFlowCtrlBusThreshGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        the system bus flow control FIFO threshold configuration."

    GROUP           cc6kxbarFlowCtrlBusThrNotifGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        the system bus flow control FIFO threshold exceeding
        notification."

    GROUP           cc6kxbarBusOnlyModeOperGroup
    DESCRIPTION
        "This group is mandatory only for platforms which support
        operational bus mode."

    GROUP           cc6kxbarSysCapPfcOperModeGroup
    DESCRIPTION
        "This group is mandatory only for platforms which
        support the system information of PFC operational mode."
 
    GROUP           cc6kxbarSysCapSwitchResGroup
    DESCRIPTION
        "This group is mandatory only for platforms which
        support the capacity information of switching 
        resources in the system."

    GROUP cc6kxbarChannelUtilGroup1
    DESCRIPTION
         "This group is mandatory only for those platforms which
          support peak input and output traffic utilization on the
          fabric channel."

    GROUP cc6kxbarSwBusGroup1
    DESCRIPTION
        "This group is mandatory only for platforms which support
         switching bus utilization."

    GROUP cc6kxbarErrorGroup
    DESCRIPTION
        "This group is mandatory only for those platforms which
         support error statistics on the fabric channel."

    GROUP cc6kxbarErrRcvryThresholdGroup
    DESCRIPTION
       "This group is mandatory for platforms which provide
        the configuration of thresholds on fabric link errors
        for the fabric error recovery feature."

    GROUP cc6kxbarErrRcvrySwitchoverGroup
    DESCRIPTION
       "This group is mandatory for platforms which provide
        the configuration of fabric switchover on excessive fabric 
        link errors for the fabric error recovery feature."

    GROUP cc6kxbarErrRcvryPersLinkResGroup
    DESCRIPTION
        "This group is mandatory for platforms which provide
        the configuration of channel resync on excessive 
        persistent fabric link errors for the fabric error 
        recovery feature."

    GROUP cc6kxbarErrRcvryChResyncGroup
    DESCRIPTION
       "This group is mandatory for platforms which provide
        the configuration of channel resync threshold for the 
        fabric error recovery feature."

    GROUP cc6kxbarTMSwBusUtilGroup
    DESCRIPTION
       "This group is mandatory for platforms which provide  
        the configuration for traffic monitor feature on the 
        switching bus."

    GROUP cc6kxbarTMSwBusUtilNotifControlGroup
    DESCRIPTION
       "This group is mandatory for platforms which provide
        the notification control for traffic monitor 
        notifications on the switching bus."

    GROUP cc6kxbarTMSwBusUtilNotifObjectGroup
    DESCRIPTION
       "This group is mandatory for platforms which support 
        traffic monitor notifications on the switching bus."

    GROUP cc6kxbarTMSwBusUtilNotifGroup
    DESCRIPTION
         "This group is mandatory for platforms which support
         traffic monitor notifications on the switching bus." 

    GROUP cc6kxbarTMChUtilGroup
    DESCRIPTION
       "This group is mandatory for platforms which provide
        the configuration for traffic monitor feature on  
        fabric channels."

    GROUP cc6kxbarTMChUtilNotifControlGroup
    DESCRIPTION
       "This group is mandatory for platforms which provide
        the notification control for traffic monitor 
        notifications on fabric channels."

    GROUP cc6kxbarTMChUtilNotifObjectGroup
    DESCRIPTION
       "This group is mandatory for platforms which support 
        traffic monitor notifications on fabric channels."

    GROUP cc6kxbarTMChUtilNotifGroup
    DESCRIPTION
         "This group is mandatory for platforms which support
         traffic monitor notifications on fabric channels." 

    ::= { cc6kxbarMIBCompliances 9 }

-- Units of Conformance
cc6kxbarModuleStatusGroup OBJECT-GROUP
    OBJECTS         {
                        cc6kxbarLcdBannerMaxSize,
                        cc6kxbarLcdBannerBanner,
                        cc6kxbarTruncatedModeAllowed,
                        cc6kxbarMinFabricPresent,
                        cc6kxbarFabricActiveSlot,
                        cc6kxbarFabricBackupSlot,
                        cc6kxbarModuleModeSwitchingMode
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects providing
        configuration and operation of the crossbar 
        switching fabric module and switching capable 
        module."
    ::= { cc6kxbarMIBGroups 1 }

cc6kxbarChannelStatusGroup OBJECT-GROUP
    OBJECTS         {
                        cc6kxbarModuleChannelModStatus,
                        cc6kxbarModuleChannelFabStatus
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing
        status and configuration of the fabric channel."
    ::= { cc6kxbarMIBGroups 2 }

cc6kxbarChannelStatisticsGroup OBJECT-GROUP
    OBJECTS         {
                        cc6kxbarStatisticsInErrors,
                        cc6kxbarStatisticsOutErrors,
                        cc6kxbarStatisticsOutDropped,
                        cc6kxbarStatisticsInUtil,
                        cc6kxbarStatisticsOutUtil
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects providing statistics for
        the fabric channel."
    ::= { cc6kxbarMIBGroups 3 }

cc6kxbarFallbackGroup OBJECT-GROUP
    OBJECTS         { cc6kxbarFallbackMode }
    STATUS          current
    DESCRIPTION
        "This object controls system fallback to bus-mode
        after loss of switching fabric module."
    ::= { cc6kxbarMIBGroups 4 }

cc6kxbarBusOnlyAllowedGroup OBJECT-GROUP
    OBJECTS         { cc6kxbarBusOnlyModeAllowed }
    STATUS          current
    DESCRIPTION
        "This object determines the value of
        cc6kxbarModuleModeSwitchingMode of each module."
    ::= { cc6kxbarMIBGroups 5 }

cc6kxbarModuleStatusGroupVer1 OBJECT-GROUP
    OBJECTS         {
                        cc6kxbarTruncatedModeAllowed,
                        cc6kxbarMinFabricPresent,
                        cc6kxbarFabricActiveSlot,
                        cc6kxbarFabricBackupSlot,
                        cc6kxbarModuleModeSwitchingMode
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing
        configuration and operation of the crossbar 
        switching fabric module and switching capable 
        module."
    ::= { cc6kxbarMIBGroups 6 }

cc6kxbarChannelStatisticsGroupVer1 OBJECT-GROUP
    OBJECTS         {
                        cc6kxbarStatisticsInErrors,
                        cc6kxbarStatisticsOutErrors,
                        cc6kxbarStatisticsOutDropped
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing statistics for
        the fabric channel."
    ::= { cc6kxbarMIBGroups 7 }

cc6kxbarLcdBannerGroup OBJECT-GROUP
    OBJECTS         {
                        cc6kxbarLcdBannerMaxSize,
                        cc6kxbarLcdBannerBanner
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing configuration of
        the lcd Banner of the fabric module."
    ::= { cc6kxbarMIBGroups 8 }

cc6kxbarChannelUtilGroup OBJECT-GROUP
    OBJECTS         {
                        cc6kxbarStatisticsInUtil,
                        cc6kxbarStatisticsOutUtil
                    }
    STATUS          current
    DESCRIPTION
        "These object determines Input and Output Utilization of the
        fabric channel."
    ::= { cc6kxbarMIBGroups 9 }

cc6kxbarChannelSpeedGroup OBJECT-GROUP
    OBJECTS         { cc6kxbarModuleChannelSpeed }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing the
        speed of the fabric channel."
    ::= { cc6kxbarMIBGroups 10 }

cc6kxbarSwBusGroup OBJECT-GROUP
    OBJECTS         {
                        cc6kxbarSwBusSwitchingStatus,
                        cc6kxbarSwBusFailureDuration,
                        cc6kxbarSwBusNotifEnable
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects for the switching bus switching
        detection feature."
    ::= { cc6kxbarMIBGroups 11 }

cc6kxbarSwBusNotifGroup NOTIFICATION-GROUP
   NOTIFICATIONS    { cc6kxbarSwBusStatusChangeNotif }
    STATUS          current
    DESCRIPTION
        "A collection of notifications for the switching
        bus switching detection feature."
    ::= { cc6kxbarMIBGroups 12 }

cc6kxbarTruncatedOperGroup OBJECT-GROUP
    OBJECTS         { cc6kxbarTruncatedModeOper }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing the
        operational truncated mode."
    ::= { cc6kxbarMIBGroups 13 }

cc6kxbarIntBusNotifControlGroup OBJECT-GROUP
    OBJECTS         { cc6kxbarIntBusNotifEnable }
    STATUS          current
    DESCRIPTION
        "A collection of objects to control the notification
        generation for internal bus."
    ::= { cc6kxbarMIBGroups 14 }

cc6kxbarIntBusCRCErrNotifGroup NOTIFICATION-GROUP
   NOTIFICATIONS    {
                        cc6kxbarIntBusCRCErrExcdNotif,
                        cc6kxbarIntBusCRCErrRcvrdNotif
                    }
    STATUS          current
    DESCRIPTION
        "A collection of notifications for the
        internal bus CRC error."
    ::= { cc6kxbarMIBGroups 15 }

cc6kxbarIntBusCRCErrGroup OBJECT-GROUP
    OBJECTS         {
                        cc6kxbarIntBusCRCErrExcdStatus,
                        cc6kxbarIntBusCRCErrExcdCount
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects to indicate the internal bus
        CRC error information on a physical entity."
    ::= { cc6kxbarMIBGroups 16 }

cc6kxbarDcefOnlyModeAllowedGroup OBJECT-GROUP
    OBJECTS         { cc6kxbarDcefOnlyModeAllowed }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing the configuration
        and information about the dcef only mode feature."
    ::= { cc6kxbarMIBGroups 17 }

cc6kxbarForceBusModeGroup OBJECT-GROUP
    OBJECTS         { cc6kxbarForceBusMode }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing the configuration
        and information about the force bus mode feature."
    ::= { cc6kxbarMIBGroups 18 }

cc6kxbarFlowCtrlNotifCtrlGroup OBJECT-GROUP
    OBJECTS         { cc6kxbarFlowCtrlNotifEnable }
    STATUS          current
    DESCRIPTION
        "A collection of objects to control the notification
        generation for the system flow control feature."
    ::= { cc6kxbarMIBGroups 19 }

cc6kxbarFlowCtrlBusThreshGroup OBJECT-GROUP
    OBJECTS         {
                        cc6kxbarFlowCtrlBusFIFOThrMode,
                        cc6kxbarFlowCtrlBusFIFOThrValue,
                        cc6kxbarFlowCtrlBusFIFOTransTime
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing configuration
        information about the system bus flow control FIFO
        threshold."
    ::= { cc6kxbarMIBGroups 20 }

cc6kxbarFlowCtrlBusThrNotifGroup NOTIFICATION-GROUP
   NOTIFICATIONS    { cc6kxbarFlowCtrlBusThrExcdNotif }
    STATUS          current
    DESCRIPTION
        "A collection of notifications for the system bus
        flow control FIFO threshold exceeding."
    ::= { cc6kxbarMIBGroups 21 }

cc6kxbarBusOnlyModeOperGroup OBJECT-GROUP
    OBJECTS         { cc6kxbarBusOnlyModeOper }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing the
        operational bus mode."
    ::= { cc6kxbarMIBGroups 22 }

cc6kxbarSysCapPfcOperModeGroup OBJECT-GROUP
      OBJECTS { cc6kxbarSysCapPfcOperMode }
      STATUS  current
      DESCRIPTION
          "A collection of objects providing the system 
           information of PFC operational mode."
      ::= { cc6kxbarMIBGroups 23 }

cc6kxbarSysCapSwitchResGroup OBJECT-GROUP
      OBJECTS { 
                  cc6kxbarSysCapSwitchResSeries,
                  cc6kxbarSysCapSwitchResCefMode 
              }
      STATUS  current
      DESCRIPTION
          "A collection of objects providing the capacity 
           information of switching resources in the system."
      ::= { cc6kxbarMIBGroups 24 }

cc6kxbarChannelUtilGroup1 OBJECT-GROUP
    OBJECTS {
         cc6kxbarStatisticsPeakInUtil,
         cc6kxbarStatisticsPeakTmInUtil,
         cc6kxbarStatisticsPeakOutUtil,
         cc6kxbarStatisticsPeakTmOutUtil
    }
    STATUS  current
    DESCRIPTION
        "A collection of objects providing the information about peak
         input and output utilization of a specific fabric channel on 
         a specific module."
      ::= { cc6kxbarMIBGroups 25 }

cc6kxbarSwBusGroup1 OBJECT-GROUP
    OBJECTS {
         cc6kxbarSwBusUtilization,
         cc6kxbarSwBusPeakUtilization,
         cc6kxbarSwBusPeakTimeUtil
    }
    STATUS  current
    DESCRIPTION
        "A collection of objects providing the information about
         switching bus utilization."
      ::= { cc6kxbarMIBGroups 26 }

cc6kxbarErrorGroup OBJECT-GROUP
    OBJECTS {
         cc6kxbarErrorModuleCrc,
         cc6kxbarErrorModuleHbeat,
         cc6kxbarErrorModuleSync,
         cc6kxbarErrorModuleDDRSync,
         cc6kxbarErrorChannelSync,
         cc6kxbarErrorChannelBuffer,
         cc6kxbarErrorChannelTimeout
    }
    STATUS  current
    DESCRIPTION
        "A collection of objects providing error statistics for
         a specific fabric channel on a specific module."
      ::= { cc6kxbarMIBGroups 27 }

cc6kxbarErrRcvryThresholdGroup OBJECT-GROUP
    OBJECTS {
         cc6kxbarErrRcvryThreshLink,
         cc6kxbarErrRcvryThreshPersLink
    }
    STATUS  current
    DESCRIPTION
        "A collection of objects providing the configuration
         of thresholds on fabric link errors for the fabric
         error recovery feature." 
      ::= { cc6kxbarMIBGroups 28 }

cc6kxbarErrRcvrySwitchoverGroup  OBJECT-GROUP
    OBJECTS { cc6kxbarErrRcvrySwitchoverEnable }
    STATUS  current
    DESCRIPTION
        "A collection of objects providing the configuration  
         of fabric switchover on excessive fabric link errors
         for the fabric error recovery feature." 
      ::= { cc6kxbarMIBGroups 29 }

cc6kxbarErrRcvryPersLinkResGroup  OBJECT-GROUP
    OBJECTS { cc6kxbarErrRcvryPersLinkResync }
    STATUS  current
    DESCRIPTION
        "A collection of objects providing the configuration
         of channel resync on excessive persistent fabric link
         errors for the fabric error recovery feature."
    ::= { cc6kxbarMIBGroups 30 }

cc6kxbarErrRcvryChResyncGroup OBJECT-GROUP
    OBJECTS {
         cc6kxbarErrRcvryChResyncCount,
         cc6kxbarErrRcvryChResyncInterval
    }
    STATUS  current
    DESCRIPTION
        "A collection of objects providing the configuration
         for channel resync threshold for the fabric error
         recovery feature."
    ::= { cc6kxbarMIBGroups 31 }

cc6kxbarTMSwBusUtilGroup OBJECT-GROUP
    OBJECTS {
        cc6kxbarTMSwBusUtilEnable,
        cc6kxbarTMSwBusUtilInterval,
        cc6kxbarTMSwBusUtilThreshold,
        cc6kxbarTMSwBusUtilLogCount,
        cc6kxbarTMSwBusUtilLastLogTime,
        cc6kxbarTMSwBusUtilLogInterval
    }
    STATUS  current
    DESCRIPTION
        "A collection of objects providing configuration
         information for traffic monitor feature on 
         the switching bus."
    ::= { cc6kxbarMIBGroups 32 }

cc6kxbarTMSwBusUtilNotifControlGroup OBJECT-GROUP
    OBJECTS {
        cc6kxbarTMSwBusUtilNotifEnable
    }
    STATUS  current
    DESCRIPTION
        "A collection of objects to control the traffic monitor
         notification generation on the switching bus."
    ::= { cc6kxbarMIBGroups 33 }

cc6kxbarTMSwBusUtilNotifObjectGroup OBJECT-GROUP
    OBJECTS {
        cc6kxbarTMSwBusUtilUtilization
    }
    STATUS  current
    DESCRIPTION
        "A collection of objects included in the traffic monitor
         notifications on the switching bus."
    ::= { cc6kxbarMIBGroups 34 }

cc6kxbarTMSwBusUtilNotifGroup NOTIFICATION-GROUP
    NOTIFICATIONS {
         cc6kxbarTMSwBusUtilAboveNotif,
         cc6kxbarTMSwBusUtilBelowNotif
    }
    STATUS  current
    DESCRIPTION
         "A collection of traffic monitor notifications on the
          switching bus."  
    ::= { cc6kxbarMIBGroups 35 }

cc6kxbarTMChUtilGroup OBJECT-GROUP
    OBJECTS {
        cc6kxbarTMChUtilEnable,         
        cc6kxbarTMChUtilInterval,      
        cc6kxbarTMChUtilThreshold,    
        cc6kxbarTMChUtilLogCount,  
        cc6kxbarTMChUtilLastLogTime,
        cc6kxbarTMChUtilLogInterval  
    }
    STATUS  current
    DESCRIPTION
        "A collection of objects providing the configuration
         information for traffic monitor feature on fabric 
         channels."
    ::= { cc6kxbarMIBGroups 36 }

cc6kxbarTMChUtilNotifControlGroup OBJECT-GROUP
    OBJECTS {
        cc6kxbarTMChUtilNotifEnable
    }
    STATUS  current
    DESCRIPTION
        "A collection of objects to control the traffic monitor 
         notification generation on fabric channels. "
    ::= { cc6kxbarMIBGroups 37 }

cc6kxbarTMChUtilNotifObjectGroup OBJECT-GROUP
    OBJECTS {
        cc6kxbarTMChUtilUtilization
    }
    STATUS  current
    DESCRIPTION
        "A collection of objects included in the traffic monitor
         notifications on fabric channels."
    ::= { cc6kxbarMIBGroups 38 }

cc6kxbarTMChUtilNotifGroup NOTIFICATION-GROUP
    NOTIFICATIONS {
        cc6kxbarTMChUtilAboveNotif,
        cc6kxbarTMChUtilBelowNotif 
    }
    STATUS  current
    DESCRIPTION
        "A collection of traffic monitor notifications on 
         fabric channels."
    ::= { cc6kxbarMIBGroups 39 }

END



