#-MIBFILE: cpqsinfo.mib

CPQSINFO-MIB DEFINITIONS ::= BEGIN


compaq OBJECT IDENTIFIER ::= { enterprises 232 }
DisplayString ::=
	OCTET STRING

PhysAddress ::=
	OCTET STRING

mib-2 OBJECT IDENTIFIER ::= { mgmt 1 }
system OBJECT IDENTIFIER ::= { mib-2 1 }
sysName OBJECT IDENTIFIER ::= { system 5 }
cpqHostOs OBJECT IDENTIFIER ::= { compaq 11 }
cpqHoComponent OBJECT IDENTIFIER ::= { cpqHostOs 2 }
cpqHoTrapInfo OBJECT IDENTIFIER ::= { cpqHoComponent 11 }
cpqHoTrapFlags OBJECT IDENTIFIER ::= { cpqHoTrapInfo 1 }
cpqSystemInfo OBJECT IDENTIFIER ::= { compaq 2 }

cpqSiMibRev OBJECT IDENTIFIER ::= { cpqSystemInfo 1 }

cpqSiComponent OBJECT IDENTIFIER ::= { cpqSystemInfo 2 }

cpqSiInterface OBJECT IDENTIFIER ::= { cpqSiComponent 1 }

cpqSiAsset OBJECT IDENTIFIER ::= { cpqSiComponent 2 }

cpqSiSecurity OBJECT IDENTIFIER ::= { cpqSiComponent 3 }

cpqSiSystemBoard OBJECT IDENTIFIER ::= { cpqSiComponent 4 }

cpqSiBoardRev OBJECT IDENTIFIER ::= { cpqSiComponent 5 }

cpqSiRackServer OBJECT IDENTIFIER ::= { cpqSiComponent 6 }

cpqSiVideo OBJECT IDENTIFIER ::= { cpqSiComponent 7 }

cpqSiMonitor OBJECT IDENTIFIER ::= { cpqSiComponent 8 }

cpqSiHotPlugSlot OBJECT IDENTIFIER ::= { cpqSiComponent 9 }

cpqSiSystemBattery OBJECT IDENTIFIER ::= { cpqSiComponent 10 }

cpqSiDockingStation OBJECT IDENTIFIER ::= { cpqSiComponent 11 }

cpqSiFru OBJECT IDENTIFIER ::= { cpqSiComponent 12 }

cpqSiRackEnclosure OBJECT IDENTIFIER ::= { cpqSiComponent 13 }

cpqSiServerBlade OBJECT IDENTIFIER ::= { cpqSiComponent 14 }

cpqSiRack OBJECT IDENTIFIER ::= { cpqSiComponent 15 }

cpqSiMP OBJECT IDENTIFIER ::= { cpqSiComponent 16 }

cpqSiOsCommon OBJECT IDENTIFIER ::= { cpqSiInterface 4 }

cpqSiMibRevMajor OBJECT-TYPE
	SYNTAX INTEGER (1..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The major revision level of the MIB.

A change in the major revision level represents a major change
in the architecture of the MIB.  A change in the major revision
level may indicate a significant change in the information
supported and/or the meaning of the supported information,
correct interpretation of data may require a MIB document with
the same major revision level."
	::= { cpqSiMibRev 1 }


cpqSiMibRevMinor OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The minor revision level of the MIB.

A change in the minor revision level may represent some minor
additional support, no changes to any pre-existing information
has occurred."
	::= { cpqSiMibRev 2 }


cpqSiMibCondition OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	ok(2),
	degraded(3),
	failed(4)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The overall condition.

This object represents the overall status of the server
information represented by this MIB."
	::= { cpqSiMibRev 3 }


cpqSiOsCommonPollFreq OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The Insight Agent's polling frequency.

The frequency, in seconds, at which the Insight Agent requests
information from the device driver.  A frequency of zero (0)
indicates that the Insight Agent retrieves the information upon
request of a management station, it does not poll the device
driver at a specific interval.

If the poll frequency is zero (0) all attempts to write to this
object will fail.  If the poll frequency is non-zero,
setting this value will change the polling frequency of the
Insight Agent.  Setting the poll frequency to zero (0) will
always fail, an agent may also choose to fail any request to
change the poll frequency to a value that would severely impact
system performance."
	::= { cpqSiOsCommon 1 }


cpqSiOsCommonModuleTable OBJECT-TYPE
	SYNTAX SEQUENCE OF CpqSiOsCommonModuleEntry
	ACCESS read-only
	STATUS optional
	DESCRIPTION "A table of software modules that provide an interface to the
device this MIB describes."
	::= { cpqSiOsCommon 2 }


cpqSiOsCommonModuleEntry OBJECT-TYPE
	SYNTAX CpqSiOsCommonModuleEntry
	ACCESS read-only
	STATUS optional
	DESCRIPTION "A description of a software module that provides an interface
to the device this MIB describes."
	INDEX { cpqSiOsCommonModuleIndex  }

	::= { cpqSiOsCommonModuleTable 1 }

cpqSiOsCommonModuleEntry ::=
	SEQUENCE {
		cpqSiOsCommonModuleIndex INTEGER,
		cpqSiOsCommonModuleName DisplayString,
		cpqSiOsCommonModuleVersion DisplayString,
		cpqSiOsCommonModuleDate OCTET STRING,
		cpqSiOsCommonModulePurpose DisplayString
		}

cpqSiOsCommonModuleIndex OBJECT-TYPE
	SYNTAX INTEGER (0..255)
	ACCESS read-only
	STATUS optional
	DESCRIPTION "A unique index for this module description."
	::= { cpqSiOsCommonModuleEntry 1 }


cpqSiOsCommonModuleName OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS optional
	DESCRIPTION "The module name."
	::= { cpqSiOsCommonModuleEntry 2 }


cpqSiOsCommonModuleVersion OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..5))
	ACCESS read-only
	STATUS optional
	DESCRIPTION "The module version in XX.YY format.

Where XX is the major version number and YY is the minor version
number.  This field will be a null (size 0) string if the agent
cannot provide the module version."
	::= { cpqSiOsCommonModuleEntry 3 }


cpqSiOsCommonModuleDate OBJECT-TYPE
	SYNTAX OCTET STRING (SIZE(7))
	ACCESS read-only
	STATUS optional
	DESCRIPTION "The module date.

field  octets  contents                  range
=====  ======  =======                  =====
1      1-2   year                      0..65536
2       3    month                     1..12
3       4    day                       1..31
4       5    hour                      0..23
5       6    minute                    0..59 
6       7    second                    0..60
(use 60 for leap-second)


This field will be set to year = 0 if the agent cannot provide
the module date.  The hour, minute, and second field will be set
to zero (0) if they are not relevant.  The year field is set
with the most significant octet first."
	::= { cpqSiOsCommonModuleEntry 4 }


cpqSiOsCommonModulePurpose OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS optional
	DESCRIPTION "The purpose of the module described in this entry."
	::= { cpqSiOsCommonModuleEntry 5 }


cpqSiSysSerialNum OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The serial number of the physical system unit.

The string will be empty if the system does not report the
serial number function."
	::= { cpqSiAsset 1 }


cpqSiFormFactor OBJECT-TYPE
	SYNTAX INTEGER {
	unknown(1),
	portable(2),
	laptop(3),
	desktop(4),
	tower(5),
	mini-tower(6),
	rack-mount(7)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The form factor of the system. Setting this variable to
unknown will fail."
	::= { cpqSiAsset 2 }


cpqSiAssetTag OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The customer changeable identifier that is set to the system
serial number at the time of manufacture.

The string will be empty if the system does not report this
function."
	::= { cpqSiAsset 3 }


cpqSiOwnershipTag OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..79))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This is a customer changeable identifier that will be
displayed by ROM at POST.  This is an 80 byte standard
ASCII character string and is Administrator Password
protected.

An example could be:
Property of Hewlett-Packard Company

The string should be NULL terminated.  This item will be
empty if the system does not report this function."
	::= { cpqSiAsset 4 }


cpqSiSysServiceNum OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The service number of the system unit.

The string will be empty if the system does not report the
system service number."
	::= { cpqSiAsset 5 }


cpqSiSysProductId OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The product id string of the system unit.

The string will be empty if the system does not report the
product id."
	::= { cpqSiAsset 6 }


cpqSiAssetTagMaxLength OBJECT-TYPE
	SYNTAX INTEGER
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION " Maximum allowed size in bytes of the asset tag."
	::= { cpqSiAsset 7 }


cpqSiVirtualSystemTable OBJECT-TYPE
	SYNTAX SEQUENCE OF CpqSiVirtualSystemEntry
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "A table of virtual system information entries."
	::= { cpqSiAsset 8 }


cpqSiVirtualSystemEntry OBJECT-TYPE
	SYNTAX CpqSiVirtualSystemEntry
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "A virtual system information table entry."
	INDEX { cpqSiVirtualSystemIndex  }

	::= { cpqSiVirtualSystemTable 1 }

cpqSiVirtualSystemEntry ::=
	SEQUENCE {
		cpqSiVirtualSystemIndex INTEGER,
		cpqSiVirtualSystemSerialNumber DisplayString,
		cpqSiVirtualSystemUUID DisplayString
		}

cpqSiVirtualSystemIndex OBJECT-TYPE
	SYNTAX INTEGER (0..255)
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "The unique index of the virtual system information entry."
	::= { cpqSiVirtualSystemEntry 1 }


cpqSiVirtualSystemSerialNumber OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "The HP Virtual Serial Number for the computer system package.  The Virtual
Serial Number is the system serial number exposed to the operating
system when running in an HP Virtual Connect environment.  The Virtual
Serial Number presented here will correspond to the Virtual UUID at the
same index location."
	::= { cpqSiVirtualSystemEntry 2 }


cpqSiVirtualSystemUUID OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "The HP Virtual UUID for the computer system package.  The Virtual
UUID is the UUID number exposed to the operating system when running
in an HP Virtual Connect environment.  The Virtual UUID presented
here will correspond to the Virtual serial number at the same index
location."
	::= { cpqSiVirtualSystemEntry 3 }


cpqSiPowerOnPassword OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	disabled(2),
	enabled(3)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The state of the power on password feature."
	::= { cpqSiSecurity 1 }


cpqSiNetServerMode OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	disabled(2),
	enabled(3)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The state of the network server mode feature."
	::= { cpqSiSecurity 2 }


cpqSiQuickLockPassword OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	disabled(2),
	enabled(3)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The state of the quicklock password feature."
	::= { cpqSiSecurity 3 }


cpqSiQuickBlank OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	disabled(2),
	enabled(3)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The state of the quick blank screen feature."
	::= { cpqSiSecurity 4 }


cpqSiDisketteBootControl OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	disabled(2),
	enabled(3)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The state of the diskette boot control feature."
	::= { cpqSiSecurity 5 }


cpqSiSerialPortAControl OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	disabled(2),
	enabled(3)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The state of the access control for the primary serial port
interface embedded in the system board."
	::= { cpqSiSecurity 6 }


cpqSiSerialPortBControl OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	disabled(2),
	enabled(3)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The state of the access control for the secondary serial port
interface embedded in the system board."
	::= { cpqSiSecurity 7 }


cpqSiParallelPortControl OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	disabled(2),
	enabled(3)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The state of the access control for the parallel port interface
embedded in the system board."
	::= { cpqSiSecurity 8 }


cpqSiFloppyDiskControl OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	disabled(2),
	enabled(3)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The state of the access control for the floppy diskette
interface embedded in the system board."
	::= { cpqSiSecurity 9 }


cpqSiFixedDiskControl OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	disabled(2),
	enabled(3)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The state of the access control for the fixed disk interface
embedded in the system board."
	::= { cpqSiSecurity 10 }


cpqSiHoodRemovedTime OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Last detection of hood removed by Smart Hood Sensor."
	::= { cpqSiSecurity 11 }


cpqSiHoodSensorConfiguration OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	disabled(2),
	notifyUser(3),
	adminPasswordProtected(4)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This is the current configuration of the Smart Cover
sensor.

The following values are currently defined:

other(1)
Smart Cover sensor is not supported on this system or cannot
be determined by the Insight Agent.  You may need to upgrade
your software.

disabled(2)
Smart Cover sensor will not detect a hood removal and
cpqSiHoodRemovedTime will not be updated.

notifyUser(3)
Smart Cover sensor will detect a hood removal and will display
a message at POST for the user.

adminPasswordProtected(4)
Smart Cover sensor will detect a hood removal and will display
a message at POST for the user to enter the Admin Password.
The system will not boot until proper password is entered."
	::= { cpqSiSecurity 12 }


cpqSiSmartCoverLockStatus OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	unlocked(2),
	locked(3)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This is the current status of the Smart Cover
Lock. The following values are currently defined:

other(1)
Smart Cover Lock is not supported on this system or cannot
be determined by the Insight Agent.  You may need to upgrade
your software.

unlocked(2)
Smart Cover Lock is not locked.  The status will be set to
unlocked due to one of the following:
1. The system hood is removed, or
2. There is no administrator password set, or
3. The administrator manually sets status to unlock.

locked(3)
Smart Cover Lock is locked. The administrator password is
required to unlock the hood."
	::= { cpqSiSecurity 13 }


cpqSiUSBPortControl OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	disabled(2),
	enabled(3),
	legacydisabled(4),
	externalportdisabled(5)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The state of the access control for the Universal
Serial Bus interface(s) embedded in the system
board.

other(1)
If Status could not be determined.

disabled(2)
USB interface is disable.

enabled(3)
USB interface is enable.

legacydisabled(4)
Legacy USB interface is disabled.

externalportdisabled(5)
External USB Ports are disabled."
	::= { cpqSiSecurity 14 }


cpqSiProductId OBJECT-TYPE
	SYNTAX INTEGER (1..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The machine product ID.

This value indicates the product type of the system board
in this system.  The value 127 will be given if the machine ID
cannot be determined.  A value of 127 will also be used for the
special case of a machine containing neither EISA nor ISA slots."
	::= { cpqSiSystemBoard 1 }


cpqSiProductName OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The machine product name.

The name of the machine used in this system."
	::= { cpqSiSystemBoard 2 }


cpqSiAuxiliaryInput OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	disabled(2),
	enabled(3)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The state of the auxiliary input (pointing) device."
	::= { cpqSiSystemBoard 4 }


cpqSiMemModuleTable OBJECT-TYPE
	SYNTAX SEQUENCE OF CpqSiMemModuleEntry
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "A table of memory module descriptions."
	::= { cpqSiSystemBoard 5 }


cpqSiMemModuleEntry OBJECT-TYPE
	SYNTAX CpqSiMemModuleEntry
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "A memory module description."
	INDEX { cpqSiMemBoardIndex , cpqSiMemModuleIndex }

	::= { cpqSiMemModuleTable 1 }

cpqSiMemModuleEntry ::=
	SEQUENCE {
		cpqSiMemBoardIndex INTEGER,
		cpqSiMemModuleIndex INTEGER,
		cpqSiMemModuleSize INTEGER,
		cpqSiMemModuleType INTEGER,
		cpqSiMemModuleSpeed INTEGER,
		cpqSiMemModuleTechnology INTEGER,
		cpqSiMemModuleManufacturer DisplayString,
		cpqSiMemModulePartNo DisplayString,
		cpqSiMemModuleDate OCTET STRING,
		cpqSiMemModuleSerialNo DisplayString,
		cpqSiMemModuleECCStatus INTEGER,
		cpqSiMemModuleHwLocation DisplayString,
		cpqSiMemModuleFrequency INTEGER,
		cpqSiMemModuleCellTablePtr INTEGER,
		cpqSiMemModuleCellStatus INTEGER,
		cpqSiMemModulePartNoMfgr DisplayString,
		cpqSiMemModuleSerialNoMfgr DisplayString
		}

cpqSiMemBoardIndex OBJECT-TYPE
	SYNTAX INTEGER (0..255)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The slot in which the memory board or cartridge is installed.

A value of 0 indicates memory installed directly on the
system board."
	::= { cpqSiMemModuleEntry 1 }


cpqSiMemModuleIndex OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The memory module number."
	::= { cpqSiMemModuleEntry 2 }


cpqSiMemModuleSize OBJECT-TYPE
	SYNTAX INTEGER (0..2147483647)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Module memory size in kilobytes.  A kilobyte of memory is
defined as 1024 bytes.

A size of 0 indicates the module is not present."
	::= { cpqSiMemModuleEntry 3 }


cpqSiMemModuleType OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	board(2),
	cpqSingleWidthModule(3),
	cpqDoubleWidthModule(4),
	simm(5),
	pcmcia(6),
	compaq-specific(7),
	dimm(8),
	smallOutlineDimm(9),
	rimm(10),
	srimm(11),
	fb-dimm(12)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Type of memory module installed.  The value other(1) will be
given if the type is not known.  The value board(2) will be
given if the memory module is permanently mounted (not modular)
on a system board or memory expansion board."
	::= { cpqSiMemModuleEntry 4 }


cpqSiMemModuleSpeed OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS optional
	DESCRIPTION "Module memory speed in nanoseconds.  The value zero (0) will
be given if the module speed cannot be determined."
	::= { cpqSiMemModuleEntry 5 }


cpqSiMemModuleTechnology OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	fastPageMode(2),
	edoPageMode(3),
	burstEdoPageMode(4),
	synchronous(5),
	rdram(6)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Technology type of memory module installed.  The value other(1)
will be given if the technology is not known."
	::= { cpqSiMemModuleEntry 6 }


cpqSiMemModuleManufacturer OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The memory module's manufacturer name.

This field will be a null (size 0) string if the manufacturer
name is not available."
	::= { cpqSiMemModuleEntry 7 }


cpqSiMemModulePartNo OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The memory module's manufacturer part number.

This field will be a null (size 0) string if the manufacturer
part number is not available."
	::= { cpqSiMemModuleEntry 8 }


cpqSiMemModuleDate OBJECT-TYPE
	SYNTAX OCTET STRING (SIZE(7))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The memory module date of manufacture.

field  octets  contents                  range
=====  ======  ======================    ========
1     1-2    year                      0..65536
2       3    month                     1..12
3       4    day                       1..31
4       5    hour                      0..23
5       6    minute                    0..59
6       7    second                    0..60
(use 60 for leap-second)

This field will be set to year = 0 if the date of manufacture
is not available.  The hour, minute, and second fields will
always be set to 0."
	::= { cpqSiMemModuleEntry 9 }


cpqSiMemModuleSerialNo OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The memory module's serial number.

This field will be a null (size 0) string if the serial number
is not available."
	::= { cpqSiMemModuleEntry 10 }


cpqSiMemModuleECCStatus OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	ok(2),
	degraded(3),
	degradedModuleIndexUnknown(4)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This provides the current status of the correctable memory
errors for this memory module.

The following status values are supported:

other(1):
ECC is not supported on this memory module.

ok(2):
The correctable error count is below threshold.

degraded(3):
The correctable error count has exceeded threshold.

degradedModuleIndexUnknown(4):
The correctable error count has exceeded threshold.
The module index not available."
	::= { cpqSiMemModuleEntry 11 }


cpqSiMemModuleHwLocation OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "A text description of the hardware location, on complex
multi SBB hardware only, for the memory module.
A NULL string indicates that the hardware location could not
be determined or is irrelevant."
	::= { cpqSiMemModuleEntry 12 }


cpqSiMemModuleFrequency OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The memory module frequency in MHz.  The value zero (0) will
be given if the module frequency cannot be determined."
	::= { cpqSiMemModuleEntry 13 }


cpqSiMemModuleCellTablePtr OBJECT-TYPE
	SYNTAX INTEGER (0..15)
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "Index for the cell in cpqSeCellTable where the memory board is
installed."
	::= { cpqSiMemModuleEntry 14 }


cpqSiMemModuleCellStatus OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	ok(2),
	deconfigured(3)
	}
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "This provides the current status for this memory module.

The following status values are supported:

other(1):
The memory module status is not available

ok(2):
The memory module is active

deconfigured(3):
The memory module is not ready"
	::= { cpqSiMemModuleEntry 15 }


cpqSiMemModulePartNoMfgr OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "The memory module's manufacturer's part number.

This field will be a null (size 0) string if the manufacturer
part number is not available."
	::= { cpqSiMemModuleEntry 16 }


cpqSiMemModuleSerialNoMfgr OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "The memory module's manufacturer's serial number.

This field will be a null (size 0) string if the manufacturer
serial number is not available."
	::= { cpqSiMemModuleEntry 17 }


cpqSiSystemId OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The System ID.

This value indicates the system ID of the system board
in this system.  This ID replaces the product ID used in
older machines (cpqSiProductId).  A value of 7Eh for the
cpqSiProductId indicates that the cpqSiSystemId should be
used to identify the system.  A value of zero (0)
indicates that the system ID function is not supported on this
machine.  In this case, the cpqSiProductId should be used to
identify the system."
	::= { cpqSiSystemBoard 6 }


cpqSiSystemCpuId OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The System ID : CPU Component.

This value indicates the CPU type of the system board
in this system.  A value of zero (0) indicates that the CPU
type cannot be determined."
	::= { cpqSiSystemBoard 7 }


cpqSiFlashRomSupport OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	notSupported(2),
	supported(3)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This value indicates if this system supports flash upgradable
system ROM."
	::= { cpqSiSystemBoard 8 }


cpqSiQuickTestRomDate OBJECT-TYPE
	SYNTAX OCTET STRING (SIZE(7))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This value indicates the date of the current quick test ROM
image.

field  octets  contents                  range
=====  ======  =======                  =====
1      1-2   year                      0..65536
2       3    month                     1..12
3       4    day                       1..31
4       5    hour                      0..23
5       6    minute                    0..59
6       7    second                    0..60
(use 60 for leap-second)


This field will be set to year = 0 if quick test ROM is not
present.  The hour, minute, and second field will be set
to zero (0) if they are not relevant.  The year field is set
with the most significant octet first."
	::= { cpqSiSystemBoard 9 }


cpqSiReboot OBJECT-TYPE
	SYNTAX INTEGER {
	notAvailable(1),
	available(2),
	defaultOnlyAvailable(3),
	rebootToCpqUtils(2693),
	rebootToDefault(8115),
	autoShutdown(9037)
	}
	ACCESS read-only
	STATUS optional
	DESCRIPTION "This object may contain the following values:
notAvailable(1)
the system does not support the reboot functionality.
Setting this object to notAvailable(1) has no effect.

available(2)
the system supports the both reboot to functionalities.
Setting this object to available(2) has no effect.

defaultOnlyAvailable(3)
the system supports the only the default reboot functionality.
Setting this object to available(3) has no effect.

rebootToCpqUtils(2693)
the system will reboot to the System Utilities if
the reboot functionality is available.  If possible,
the agent will attempt to gracefully shutdown the
operating system before performing the reboot.
If this functionality is unavailable on this system
then all sets will have no effect.

rebootToDefault(8115)
the system will reboot and allow the default boot
process to occur if the reboot functionality is
available.  If possible, the agent will attempt to
gracefully shutdown the operating system before
performing the reboot.  If this functionality is
unavailable on this system then all sets will have
no effect.

autoShutdown(9037)
If possible, the agent will attempt to gracefully
shutdown the operating system. The agent will not
preform a reboot.

"
	::= { cpqSiSystemBoard 10 }


cpqSiProcMicroPatchTable OBJECT-TYPE
	SYNTAX SEQUENCE OF CpqSiProcMicroPatchEntry
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This table lists the set of processor microcode patches that
the system ROM contains. During post, the ROM will apply the
appropriate patches to the CPU microcode. Scan this table to
ensure that a patch is being applied to a processor."
	::= { cpqSiSystemBoard 11 }


cpqSiProcMicroPatchEntry OBJECT-TYPE
	SYNTAX CpqSiProcMicroPatchEntry
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "An entry describing one microcode patch contained in the system
ROM."
	INDEX { cpqSiProcMicroPatchIndex  }

	::= { cpqSiProcMicroPatchTable 1 }

cpqSiProcMicroPatchEntry ::=
	SEQUENCE {
		cpqSiProcMicroPatchIndex INTEGER,
		cpqSiProcMicroPatchId INTEGER,
		cpqSiProcMicroPatchDate OCTET STRING,
		cpqSiProcMicroPatchFamily OCTET STRING
		}

cpqSiProcMicroPatchIndex OBJECT-TYPE
	SYNTAX INTEGER (1..255)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Index into the microcode patch table."
	::= { cpqSiProcMicroPatchEntry 1 }


cpqSiProcMicroPatchId OBJECT-TYPE
	SYNTAX INTEGER
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The ID of this particular CPU microcode patch."
	::= { cpqSiProcMicroPatchEntry 2 }


cpqSiProcMicroPatchDate OBJECT-TYPE
	SYNTAX OCTET STRING (SIZE(7))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This value indicates the date of this CPU microcode patch.

field  octets  contents                  range
=====  ======  =======                  =====
1      1-2   year                      0..65536
2       3    month                     1..12
3       4    day                       1..31
4       5    hour                      0..23
5       6    minute                    0..59
6       7    second                    0..60
(use 60 for leap-second)

NOTE: Year is stored in packed BCD. The most significant
part is in the second octet. For example:
1995 would be stored as 0x95 0x19.

The hour, minute, and second field will be set to zero (0)
if they are not relevant.  The year field is set with the
most significant octet first."
	::= { cpqSiProcMicroPatchEntry 3 }


cpqSiProcMicroPatchFamily OBJECT-TYPE
	SYNTAX OCTET STRING (SIZE(3))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The valid family/model/step of the processor that this CPU
microcode patch applies to.

field  octets  contents                  range
=====  ======  =======                  =====
1       1    CPU Step                  0..255
2       2    CPU Model                 0..255
3       3    CPU Family                0..255 "
	::= { cpqSiProcMicroPatchEntry 4 }


cpqSiPowerMgmtStatus OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	disabled(2),
	enabled(3)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The state of power management."
	::= { cpqSiSystemBoard 12 }


cpqSiRebootFlags OBJECT-TYPE
	SYNTAX INTEGER
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The Reboot Flags.

This is a collection of flags used to indicate the re-boot
options available. This integer is a bitmap, with each bit
indicating the availability of an option. If the bit is set
to 1, the option is available; otherwise it is not. Multiple
options are allowed.

NOTE:   bit 31 is the most significant bit, bit 0 is the least
significant.


Status   This is a collection of flags.  Each bit has the
following meaning when it is on (1):

Bit 31:     Execute Set
Bit 30-6:   RESERVED
Bit 5:      Boot to ROM Based Setup
Bit 4:      RESERVED
Bit 3:      Boot to OS
Bit 2:      Boot to Utils
Bit 1:      Warm Boot
Bit 0:      Cold Boot"
	::= { cpqSiSystemBoard 13 }


cpqSiMemErrorIndex OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Placeholder for memory module number for ECC traps.
Represents the number of the memory module for which an ECC status
change has occurred. Set to 65535 if module number not available."
	::= { cpqSiSystemBoard 14 }


cpqSiMemECCCondition OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	ok(2),
	degraded(3)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This provides the current condition of the correctable memory
errors for the entire memory.

The following status values are supported:

other(1) :
ECC is not supported.

ok(2)    :
The correctable error count is below threshold.

degraded(3) :
The correctable error count has exceeded threshold."
	::= { cpqSiSystemBoard 15 }


cpqSiMemConfigChangeData OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..383))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Text string for the memory configuration change trap."
	::= { cpqSiSystemBoard 16 }


cpqSiServerSystemId OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..8))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "A Server System ID.

This value is used to uniquely identify systems via a unique
ID on systems that do not support the EISA bus."
	::= { cpqSiSystemBoard 17 }


cpqSiPowerScheme OBJECT-TYPE
	SYNTAX INTEGER {
	unsupported(1),
	other(2),
	power-saver(3),
	balanced(4),
	high-performance(5),
	user-defined(6)
	}
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "The current active power plan or power scheme of the system."
	::= { cpqSiSystemBoard 18 }


cpqSiPowerSchemeName OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "The name of current active power plan or power scheme of the
system. When cpqSiPowerScheme has a value of user-defined(6), the 
user defined name can be populated here."
	::= { cpqSiSystemBoard 19 }


cpqSiCurrentPerformanceStatePointer OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "Pointer to cpqSiPerfStateIndex in cpqSiPerfStateTable to indicate the current performance state of the system."
	::= { cpqSiSystemBoard 20 }


cpqSiMinPerformanceState OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "The slowest performance state by the selected power state policy."
	::= { cpqSiSystemBoard 21 }


cpqSiMaxPerformanceState OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "The fastest performance state supported by the selected power state policy."
	::= { cpqSiSystemBoard 22 }


cpqSiPerfStateTable OBJECT-TYPE
	SYNTAX SEQUENCE OF CpqSiPerfStateEntry
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "A table of supported performance states of the system."
	::= { cpqSiSystemBoard 23 }


cpqSiPerfStateEntry OBJECT-TYPE
	SYNTAX CpqSiPerfStateEntry
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "An entry describing a supported performance state of the system."
	INDEX { cpqSiPerfStateIndex  }

	::= { cpqSiPerfStateTable 1 }

cpqSiPerfStateEntry ::=
	SEQUENCE {
		cpqSiPerfStateIndex INTEGER,
		cpqSiPerfState INTEGER,
		cpqSiPerfStateCpuFrequency INTEGER,
		cpqSiPerfStateCpuPower INTEGER
		}

cpqSiPerfStateIndex OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "Index into the performance state table. cpqSiCurrentPerformanceStatePointer should point to one of these values."
	::= { cpqSiPerfStateEntry 1 }


cpqSiPerfState OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "Performance state number. A unique number assigned to a performance state instance."
	::= { cpqSiPerfStateEntry 2 }


cpqSiPerfStateCpuFrequency OBJECT-TYPE
	SYNTAX INTEGER (0..2147483647)
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "The processor frequency in megahertz for this performance state instance."
	::= { cpqSiPerfStateEntry 3 }


cpqSiPerfStateCpuPower OBJECT-TYPE
	SYNTAX INTEGER (0..2147483647)
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "The processor power setting in milliwatts for this performance state instance."
	::= { cpqSiPerfStateEntry 4 }


cpqSiTPMmodule OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	absent(2),
	presentEnabled(3),
	presentDisabled(4)
	}
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "This field will be populated if TPM module is present in the system board.
other(1)
No record of TPM exist.
absent(2)
TPM module is not present in the system.
presentEnabled(3)
TPM module is present in the system and currently enabled.
presentDisabled(4)
TPM module is present in the system and currently not enabled."
	::= { cpqSiSystemBoard 24 }


cpqSiCurRevDate OBJECT-TYPE
	SYNTAX DisplayString (SIZE(8))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The current board revision configuration date in MM/DD/YY
format.  This is the date that the EISA Configuration Utility
was used to define the current configuration.  This value will
contain 'N/A' if this system does not support this feature."
	::= { cpqSiBoardRev 1 }


cpqSiPrevRevDate OBJECT-TYPE
	SYNTAX DisplayString (SIZE(8))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The previous board revision configuration date in MM/DD/YY
format.  This is the date that the EISA Configuration Utility
was used to define the previous configuration.  This value will
contain 'N/A' if this system does not support this feature."
	::= { cpqSiBoardRev 2 }


cpqSiBoardRevTable OBJECT-TYPE
	SYNTAX SEQUENCE OF CpqSiBoardRevEntry
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "A table of board revision descriptions."
	::= { cpqSiBoardRev 3 }


cpqSiBoardRevEntry OBJECT-TYPE
	SYNTAX CpqSiBoardRevEntry
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "A board revision description."
	INDEX { cpqSiBoardRevSlotIndex , cpqSiBoardRevIndex }

	::= { cpqSiBoardRevTable 1 }

cpqSiBoardRevEntry ::=
	SEQUENCE {
		cpqSiBoardRevSlotIndex INTEGER,
		cpqSiBoardRevIndex INTEGER,
		cpqSiBoardRevId DisplayString,
		cpqSiBoardRevCur DisplayString,
		cpqSiBoardRevPrev DisplayString,
		cpqSiBoardRevHwLocation DisplayString
		}

cpqSiBoardRevSlotIndex OBJECT-TYPE
	SYNTAX INTEGER (0..255)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The slot in which the board described in this entry resides.
Zero (0) indicates the system board."
	::= { cpqSiBoardRevEntry 1 }


cpqSiBoardRevIndex OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "A number that uniquely specifies which board in a specific slot
is described in this entry.  Zero (0) indicates the main board
in this slot.  Any other number indicates a daughter board or a
component of the main board."
	::= { cpqSiBoardRevEntry 2 }


cpqSiBoardRevId OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..16))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "A description of the board type.  The defined types are:

Type
==============
System Board
Processor n     (n = the processor number)
Memory n        (n = the memory board number)
Slot n          (n = the slot the board occupies)

Other types may be defined at a later date."
	::= { cpqSiBoardRevEntry 3 }


cpqSiBoardRevCur OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..8))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The current revision for the board described in this entry.
This value will be N/A if there is no current revision
information."
	::= { cpqSiBoardRevEntry 4 }


cpqSiBoardRevPrev OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..8))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The revision for the board described in this entry prior to the
current configuration.  This value will be N/A if there is no
previous revision information."
	::= { cpqSiBoardRevEntry 5 }


cpqSiBoardRevHwLocation OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "A text description of the hardware location, on complex
multi SBB hardware only, for the board.
A NULL string indicates that the hardware location could not
be determined or is irrelevant."
	::= { cpqSiBoardRevEntry 6 }


cpqSiFirmwareRevTable OBJECT-TYPE
	SYNTAX SEQUENCE OF CpqSiFirmwareRevEntry
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "A table of firmware revision descriptions."
	::= { cpqSiBoardRev 4 }


cpqSiFirmwareRevEntry OBJECT-TYPE
	SYNTAX CpqSiFirmwareRevEntry
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "A firmware revision description."
	INDEX { cpqSiFirmwareRevIndex  }

	::= { cpqSiFirmwareRevTable 1 }

cpqSiFirmwareRevEntry ::=
	SEQUENCE {
		cpqSiFirmwareRevIndex INTEGER,
		cpqSiFirmwareRevDesc DisplayString,
		cpqSiFirmwareRevString DisplayString,
		cpqSiFirmwareRevCellTablePtr INTEGER,
		cpqSiFirmwareLocation DisplayString,
		cpqSiFirmwareStatus INTEGER
		}

cpqSiFirmwareRevIndex OBJECT-TYPE
	SYNTAX INTEGER
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Locally-unique index for this entry."
	::= { cpqSiFirmwareRevEntry 1 }


cpqSiFirmwareRevDesc OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Description, e.g. SRM console, ARC console, System BIOS, etc."
	::= { cpqSiFirmwareRevEntry 2 }


cpqSiFirmwareRevString OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Version number, possibly of the form Vx.y or Vx.y-z."
	::= { cpqSiFirmwareRevEntry 3 }


cpqSiFirmwareRevCellTablePtr OBJECT-TYPE
	SYNTAX INTEGER
	ACCESS read-only
	STATUS optional
	DESCRIPTION "Index for the cell in cpqSeCellTable where this firmware is located"
	::= { cpqSiFirmwareRevEntry 4 }


cpqSiFirmwareLocation OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "Description of which board the firmware is located in."
	::= { cpqSiFirmwareRevEntry 5 }


cpqSiFirmwareStatus OBJECT-TYPE
	SYNTAX INTEGER {
	unknown(1),
	active(2),
	inactive(3)
	}
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "The current status for this firmware."
	::= { cpqSiFirmwareRevEntry 6 }


cpqSiFirmwareCfgTable OBJECT-TYPE
	SYNTAX SEQUENCE OF CpqSiFirmwareCfgEntry
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Table of soft switches and symbols maintained by the
firmware.  May be operating system and/or option-specific
and will certainly be system-specific.  This list is
intended to be easily extensible and support arbitrary
datatypes.  It includes such switches as powerup options,
default dump device, etc.
Note - the string comparison for svrFwSymbolName is case
insensitive."
	::= { cpqSiBoardRev 5 }


cpqSiFirmwareCfgEntry OBJECT-TYPE
	SYNTAX CpqSiFirmwareCfgEntry
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Each entry represents one variable or symbol maintained by
or stored by some instance of firmware in the system."
	INDEX { cpqSiFirmwareCfgName  }

	::= { cpqSiFirmwareCfgTable 1 }

cpqSiFirmwareCfgEntry ::=
	SEQUENCE {
		cpqSiFirmwareCfgName DisplayString,
		cpqSiFirmwareCfgValue DisplayString
		}

cpqSiFirmwareCfgName OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The firmware configuration symbol name as visible from the
console."
	::= { cpqSiFirmwareCfgEntry 1 }


cpqSiFirmwareCfgValue OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The firmware configuration symbol value.  Null if none
or unknown."
	::= { cpqSiFirmwareCfgEntry 2 }


cpqSiRackServerShutdownRole OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	master(2),
	slave(3)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This entry describes this system's role in a rack-mounted
uninterruptible power supply family. The master both
communicates with the UPS and derives its power from the
UPS.  The slave derives its power from the UPS, but does
not communicate with it."
	::= { cpqSiRackServer 1 }


cpqSiRackServerMasterName OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..48))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This entry describes the name of the master server in a
rack-mounted uninterruptible power supply family. A slave
system would communicate with this server to derive UPS
status."
	::= { cpqSiRackServer 2 }


cpqSiVideoEdidRaw OBJECT-TYPE
	SYNTAX OCTET STRING (SIZE(128))
	ACCESS read-only
	STATUS optional
	DESCRIPTION "The raw value returned from the video EDID function."
	::= { cpqSiVideo 1 }


cpqSiVideoDesc OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS optional
	DESCRIPTION "The manufacturer and model description of the video display."
	::= { cpqSiVideo 2 }


cpqSiVideoSerialNumber OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..32))
	ACCESS read-only
	STATUS optional
	DESCRIPTION "The serial number of the video display."
	::= { cpqSiVideo 3 }


cpqSiVideoManufactureDate OBJECT-TYPE
	SYNTAX OCTET STRING (SIZE(7))
	ACCESS read-only
	STATUS optional
	DESCRIPTION "The date of manufacture of the video display in the following
format:

field  octets  contents                  range
=====  ======  =======                  =====
1      1-2   year                      0..65536
2       3    month                     1..12
3       4    day                       1..31
4       5    hour                      0..23
5       6    minute                    0..59
6       7    second                    0..60
(use 60 for leap-second)

This field will be set to year = 0 if the agent cannot provide
the date.  The date information that is given resolves to a year
and week, so the hour, minute, and second field will be set to 0,
the month and day fields will give the monday of the week of
manufacture."
	::= { cpqSiVideo 4 }


cpqSiVideoHeight OBJECT-TYPE
	SYNTAX INTEGER (0..255)
	ACCESS read-only
	STATUS optional
	DESCRIPTION "The maximum image height of the video display in centimeters"
	::= { cpqSiVideo 5 }


cpqSiVideoWidth OBJECT-TYPE
	SYNTAX INTEGER (0..255)
	ACCESS read-only
	STATUS optional
	DESCRIPTION "The maximum image width of the video display in centimeters"
	::= { cpqSiVideo 6 }


cpqSiVideoMaxHorPixel OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS optional
	DESCRIPTION "The number of horizontal pixels in the highest resolution video
mode supported."
	::= { cpqSiVideo 7 }


cpqSiVideoMaxVertPixel OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS optional
	DESCRIPTION "The number of vertical pixels in the highest resolution video
mode supported."
	::= { cpqSiVideo 8 }


cpqSiVideoMaxRefreshRate OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS optional
	DESCRIPTION "The video refresh rate in Hz of the highest resolution video
mode supported."
	::= { cpqSiVideo 9 }


cpqSiMonitorOverallCondition OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	ok(2),
	degraded(3),
	failed(4)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This value specifies the overall condition of the system's
monitor(s).

The following conditions are supported:

other(1)
The monitor does not support fault reporting or condition is
unknown.

ok(2)
The monitor is operating OK.

degraded(3)
The monitor has detected a fault.  The monitor is still useable
but action should be taken to return the monitor to ok.

failed(4)
The monitor has detected a fault.  The monitor will not
be useable. Action should be taken to replace the monitor."
	::= { cpqSiMonitor 1 }


cpqSiMonitorTable OBJECT-TYPE
	SYNTAX SEQUENCE OF CpqSiMonitorEntry
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "A table of all video monitor descriptions connected to this
system."
	::= { cpqSiMonitor 2 }


cpqSiMonitorEntry OBJECT-TYPE
	SYNTAX CpqSiMonitorEntry
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "A video monitor description."
	INDEX { cpqSiMonitorIndex  }

	::= { cpqSiMonitorTable 1 }

cpqSiMonitorEntry ::=
	SEQUENCE {
		cpqSiMonitorIndex INTEGER,
		cpqSiMonitorEdidRaw OCTET STRING,
		cpqSiMonitorDesc DisplayString,
		cpqSiMonitorSerialNumber DisplayString,
		cpqSiMonitorManufactureDate OCTET STRING,
		cpqSiMonitorHeight INTEGER,
		cpqSiMonitorWidth INTEGER,
		cpqSiMonitorMaxHorPixel INTEGER,
		cpqSiMonitorMaxVertPixel INTEGER,
		cpqSiMonitorMaxRefreshRate INTEGER,
		cpqSiMonitorManufacturer DisplayString,
		cpqSiMonitorThermalCondition INTEGER,
		cpqSiMonitorOperationalCondition INTEGER,
		cpqSiMonitorStatus INTEGER
		}

cpqSiMonitorIndex OBJECT-TYPE
	SYNTAX INTEGER (0..15)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "A unique index for each video display connected to the system."
	::= { cpqSiMonitorEntry 1 }


cpqSiMonitorEdidRaw OBJECT-TYPE
	SYNTAX OCTET STRING (SIZE(128))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The raw value returned from the video EDID function."
	::= { cpqSiMonitorEntry 2 }


cpqSiMonitorDesc OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The manufacturer and model description of the video display."
	::= { cpqSiMonitorEntry 3 }


cpqSiMonitorSerialNumber OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..32))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The serial number of the video display."
	::= { cpqSiMonitorEntry 4 }


cpqSiMonitorManufactureDate OBJECT-TYPE
	SYNTAX OCTET STRING (SIZE(7))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The date of manufacture of the video display in the following
format:

field  octets  contents                  range
=====  ======  =======                  =====
1      1-2   year                      0..65536
2       3    month                     1..12
3       4    day                       1..31
4       5    hour                      0..23
5       6    minute                    0..59
6       7    second                    0..60
(use 60 for leap-second)

This field will be set to year = 0 if the agent cannot provide
the date.  The date information that is given resolves to a year
and week, so the hour, minute, and second field will be set to 0,
the month and day fields will give the monday of the week of
manufacture."
	::= { cpqSiMonitorEntry 5 }


cpqSiMonitorHeight OBJECT-TYPE
	SYNTAX INTEGER (0..255)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The maximum image height of the video display in centimeters"
	::= { cpqSiMonitorEntry 6 }


cpqSiMonitorWidth OBJECT-TYPE
	SYNTAX INTEGER (0..255)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The maximum image width of the video display in centimeters"
	::= { cpqSiMonitorEntry 7 }


cpqSiMonitorMaxHorPixel OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The number of horizontal pixels in the highest resolution video
mode supported."
	::= { cpqSiMonitorEntry 8 }


cpqSiMonitorMaxVertPixel OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The number of vertical pixels in the highest resolution video mode
supported."
	::= { cpqSiMonitorEntry 9 }


cpqSiMonitorMaxRefreshRate OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The video refresh rate in Hz of the highest resolution video mode
supported."
	::= { cpqSiMonitorEntry 10 }


cpqSiMonitorManufacturer OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The manufacturer of the video display."
	::= { cpqSiMonitorEntry 11 }


cpqSiMonitorThermalCondition OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	ok(2),
	degraded(3)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This provides the condition of the monitor's internal temperature.

This value will be one of the following:

other(1)
Monitor thermal fault reporting is not supported by this monitor
or the Insight Agent does not recognize the status.  You may
need to upgrade your software.

ok(2)
The internal temperature is within normal limits.

degraded(3)
The internal temperature is outside normal operating range."
	::= { cpqSiMonitorEntry 12 }


cpqSiMonitorOperationalCondition OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	ok(2),
	degraded(3),
	failed(4)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This provides the condition of the monitor's operational features.

This condition value will be one of the following:

other(1)
Monitor operational fault reporting is not supported by this
monitor or the Insight Agent does not recognize the status.
You may need to upgrade your software.

ok(2)
The monitor is operating within normal limits.

degraded(3)
The monitor is not functioning within normal operating limits.
At least one of the operational features has become degraded.

failed(4)
The monitor is not functioning within normal operating limits.
At least one of the operational features has failed causing the
monitor to not be usable.  The monitor should be replaced."
	::= { cpqSiMonitorEntry 13 }


cpqSiMonitorStatus OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	unknown(2),
	ok(3),
	thermalDegraded(4),
	operationalFailure(5)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This provides the status of the monitor's fault reporting features.

This status value will be one of the following:

other(1)
Monitor fault reporting is not supported by this monitor or the
Insight Agent does not recognize the status. You may need to
upgrade your software.

unknown(2)
The monitor status is unknown because the monitor is
either in power saving mode or it has been turned off.

ok(3)
The monitor is operating within normal limits.

thermalDegraded(4)
The monitor's internal temperature is not functioning within
normal operating limits.

operationalFailure(5)
The monitor is not functioning within normal operating limits.
At least one of the operational features has failed.
The monitor should be replaced."
	::= { cpqSiMonitorEntry 14 }


cpqSiHotPlugSlotSupported OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	notSupported(2),
	supported(3)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This value specifies if this system supports the Hot
Pluggable Slot feature."
	::= { cpqSiHotPlugSlot 1 }


cpqSiHotPlugSlotCondition OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	ok(2),
	degraded(3),
	failed(4)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This value specifies the overall condition of the Hot Plug
Slot feature.

The Hot Plug condition is set as follows:

other(1)
When Hot Plug Slots are not supported or condition is unknown.

ok(2)
If there are no hot plug slots with a condition of degraded
or failed.

degraded(3)
If there are degraded slot entries but none failed.

failed(4)
If there are failed slot entries."
	::= { cpqSiHotPlugSlot 2 }


cpqSiHotPlugSlotChangeCount OBJECT-TYPE
	SYNTAX INTEGER
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This value will be incremented each time a hot plug event
occurs resulting in a change in the hot plug slot table."
	::= { cpqSiHotPlugSlot 3 }


cpqSiHotPlugSlotTable OBJECT-TYPE
	SYNTAX SEQUENCE OF CpqSiHotPlugSlotEntry
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "A list of Hot Plug Slot information entries."
	::= { cpqSiHotPlugSlot 4 }


cpqSiHotPlugSlotEntry OBJECT-TYPE
	SYNTAX CpqSiHotPlugSlotEntry
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "A description of a Hot Plug Slot."
	INDEX { cpqSiHotPlugSlotChassis , cpqSiHotPlugSlotIndex }

	::= { cpqSiHotPlugSlotTable 1 }

cpqSiHotPlugSlotEntry ::=
	SEQUENCE {
		cpqSiHotPlugSlotChassis INTEGER,
		cpqSiHotPlugSlotIndex INTEGER,
		cpqSiHotPlugSlotBoardPresent INTEGER,
		cpqSiHotPlugSlotPowerState INTEGER,
		cpqSiHotPlugSlotBoardCondition INTEGER,
		cpqSiHotPlugSlotErrorStatus INTEGER,
		cpqSiHotPlugSlotHwLocation DisplayString
		}

cpqSiHotPlugSlotChassis OBJECT-TYPE
	SYNTAX INTEGER (0..255)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The Chassis where this hot plug slot resides."
	::= { cpqSiHotPlugSlotEntry 1 }


cpqSiHotPlugSlotIndex OBJECT-TYPE
	SYNTAX INTEGER (0..255)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The slot within the chassis for this hot plug slot."
	::= { cpqSiHotPlugSlotEntry 2 }


cpqSiHotPlugSlotBoardPresent OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	present(2),
	absent(3),
	presentButSuspended(4)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This value indicates whether a board is present(2) in or
absent(3) from the slot.  A value of other(1) indicates
the information could not be obtained."
	::= { cpqSiHotPlugSlotEntry 3 }


cpqSiHotPlugSlotPowerState OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	powerOn(2),
	powerOff(3)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This value is set to powerOn(2) when power is being supplied
to the slot and powerOff(3) when power is not being supplied.
A value of other(1) indicates the information could not be
obtained."
	::= { cpqSiHotPlugSlotEntry 4 }


cpqSiHotPlugSlotBoardCondition OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	ok(2),
	degraded(3),
	failed(4)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This value specifies the condition of the hot plug slot.

The hot plug condition is set as follows:

other(1)
When the condition could not be determined.

ok(2)
The slot is powered up and operating normally.

degraded(3)
If the board in the slot is not fully functioning.

failed(4)
If the slot is failed for any reason.  See the status code
for more information on the failure."
	::= { cpqSiHotPlugSlotEntry 5 }


cpqSiHotPlugSlotErrorStatus OBJECT-TYPE
	SYNTAX INTEGER {
	noError(1),
	generalError(2),
	wrongRevision(3),
	wrongBoard(4),
	cannotConfig(5),
	powerFault(6),
	unexpectedPowerLoss(7),
	wrongSpeed(8),
	functionalFailure(9)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This value specifies the status of the hot plug slot.

The hot plug slot status is set as follows:

noError(1)
The slot is operating normally.

generalError(2)
A general error occurred.

wrongRevision(3)
The revision of the replacement adapter was different from
the original adapter.

wrongBoard(4)
The model of the replacement adapter was different from the
original adapter.

cannotConfig(5)
The adapter could not be configured.

powerFault(6)
A power fault occurred for the slot.

unexpectedPowerLoss(7)
Power was unexpectedly lost from the slot.

wrongSpeed(8)
The adapter cannot be run at the current bus speed.

functionlFailure(9)
The adapter is not functioning correctly.  This may
be caused by a cabling problem."
	::= { cpqSiHotPlugSlotEntry 6 }


cpqSiHotPlugSlotHwLocation OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "A text description of the hardware location, on complex
multi SBB hardware only, for the hot plug slot.
A NULL string indicates that the hardware location could not
be determined or is irrelevant."
	::= { cpqSiHotPlugSlotEntry 7 }


cpqSiSystemBatteryOverallCondition OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	ok(2),
	degraded(3),
	failed(4)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This value specifies the overall condition of all of the
system batteries.

The following conditions are supported:

other(1)
The system does not use system batteries or the battery
condition is unknown.

ok(2)
All System Batteries are operating OK.

degraded(3)
One or more of the System Batteries has degraded.  The
degraded battery will continue to function but should be
replaced.

failed(4)
One of more of the System Batteries has failed.  The failed
battery is no longer usable. Action should be taken to replace
the battery."
	::= { cpqSiSystemBattery 1 }


cpqSiSysBatteryTable OBJECT-TYPE
	SYNTAX SEQUENCE OF CpqSiSysBatteryEntry
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "A table of System Batteries."
	::= { cpqSiSystemBattery 2 }


cpqSiSysBatteryEntry OBJECT-TYPE
	SYNTAX CpqSiSysBatteryEntry
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "A system battery description."
	INDEX { cpqSiSysBatteryIndex  }

	::= { cpqSiSysBatteryTable 1 }

cpqSiSysBatteryEntry ::=
	SEQUENCE {
		cpqSiSysBatteryIndex INTEGER,
		cpqSiSysBatteryModel DisplayString,
		cpqSiSysBatterySerialNum DisplayString,
		cpqSiSysBatteryAssetTag DisplayString,
		cpqSiSysBatteryManufacturer DisplayString,
		cpqSiSysBatteryDate OCTET STRING,
		cpqSiSysBatterySmartVersion DisplayString,
		cpqSiSysBatteryCondition INTEGER,
		cpqSiSysBatteryStatus INTEGER,
		cpqSiSysBatteryChemistry INTEGER,
		cpqSiSysBatteryRemainingCap INTEGER,
		cpqSiSysBatteryFirmwareRevision INTEGER,
		cpqSiSysBatteryHardwareRevision INTEGER,
		cpqSiSysBatteryFullCap INTEGER,
		cpqSiSysBatteryDesignCap INTEGER,
		cpqSiSysBatteryHwLocation DisplayString
		}

cpqSiSysBatteryIndex OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "A unique index for this battery entry."
	::= { cpqSiSysBatteryEntry 1 }


cpqSiSysBatteryModel OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The model name for  this battery."
	::= { cpqSiSysBatteryEntry 2 }


cpqSiSysBatterySerialNum OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The serial number for this battery."
	::= { cpqSiSysBatteryEntry 3 }


cpqSiSysBatteryAssetTag OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This is the customer changeable battery identifier that is set
to this system battery's serial number at the time of
manufacture.

The string will be empty if the battery does support
this function."
	::= { cpqSiSysBatteryEntry 4 }


cpqSiSysBatteryManufacturer OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The battery's manufacturer's name.

The string will be empty if the battery does support
this function."
	::= { cpqSiSysBatteryEntry 5 }


cpqSiSysBatteryDate OBJECT-TYPE
	SYNTAX OCTET STRING (SIZE(7))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The battery's manufacture date.

field  octets  contents                  range
=====  ======  =======                  =====
1      1-2   year                      0..65536
2       3    month                     1..12
3       4    day                       1..31
4       5    hour                      0..23
5       6    minute                    0..59
6       7    second                    0..60
(use 60 for leap-second)

This field will be set to year = 0 if the agent cannot provide
the module date.  The hour, minute, and second field will be set
to zero (0) if they are not relevant.  The year field is set
with the most significant octet first.

The string will be empty if the battery does support
this function."
	::= { cpqSiSysBatteryEntry 6 }


cpqSiSysBatterySmartVersion OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The Smart Battery Data Specification version number supported by this
battery.

The string will be empty if the system battery does support
this function."
	::= { cpqSiSysBatteryEntry 7 }


cpqSiSysBatteryCondition OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	ok(2),
	degraded(3),
	failed(4)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This provides the current condition of this system battery.

The following status values are supported:

other(1)
The battery does not support condition monitoring or
the Insight Agent cannot determine condition.

ok(2)
The battery is operating normally.  No user action is
required.

degraded(3)
The battery is degraded.  The battery is still usable
but should be replaced.

failed(4)
The battery has failed.  The battery is no longer
usable and should be replaced soon."
	::= { cpqSiSysBatteryEntry 8 }


cpqSiSysBatteryStatus OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	ok(2),
	capacityDegraded(3),
	chargeFault(4),
	batteryFailure(5)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This provides the current status of the battery.

The following status values are supported:

other(1):
This battery does not support status reporting.

ok(2):
The battery is operating ok.

User Action: No action required.

capacityDegraded(3):
Significant battery degradation has occurred.
The battery can no longer be fully recharged.

User Action:
If using multiple batteries, run the Power
Conservation Utility to identify the battery
location.  Contact your System Administrator or
Authorized Reseller to order a replacement
battery.

chargeFault(4):
One or more batteries are not functioning properly.

User Action:
Make sure all batteries are operating in the
recommended temperature range.  Check for foreign
objects in the battery slots.  Remove and reinsert all
batteries to resume normal battery operation.
Contact your System Administrator or Authorized
Reseller if you are still experiencing problems.

batteryFailure(5):
The battery has failed and must be replaced.

User Action:
Contact your System Administrator or Authorized
Reseller to order a replacement battery.  Recycle your
old battery. For proper disposal information, refer
to the documentation that came with your computer."
	::= { cpqSiSysBatteryEntry 9 }


cpqSiSysBatteryChemistry OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	unknown(2),
	lead-Acid(3),
	nickel-Cadmium(4),
	nickel-Metal-Hydride(5),
	lithium-Ion(6),
	zinc-Air(7),
	lithium-Polymer(8)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The chemistry of the battery."
	::= { cpqSiSysBatteryEntry 10 }


cpqSiSysBatteryRemainingCap OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This is a percentage of the battery's remaining capacity
from its design capacity.

If this attribute is not supported, 65535 is returned."
	::= { cpqSiSysBatteryEntry 11 }


cpqSiSysBatteryFirmwareRevision OBJECT-TYPE
	SYNTAX INTEGER (0..255)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This is the revision level of the firmware on the battery.

If this attribute is not supported, 255 is returned."
	::= { cpqSiSysBatteryEntry 12 }


cpqSiSysBatteryHardwareRevision OBJECT-TYPE
	SYNTAX INTEGER (0..255)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This is the revision level of the hardware on the battery.

If this attribute is not supported, 255 is returned."
	::= { cpqSiSysBatteryEntry 13 }


cpqSiSysBatteryFullCap OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This is the mWatt-Hours of the battery's Full capacity on
the current charge.

If this attribute is not supported, 65535 is returned."
	::= { cpqSiSysBatteryEntry 14 }


cpqSiSysBatteryDesignCap OBJECT-TYPE
	SYNTAX INTEGER (0..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This is the mWatt-Hours of the battery's design capacity as
specified by the manufacturer.

If this attribute is not supported, 65535 is returned."
	::= { cpqSiSysBatteryEntry 15 }


cpqSiSysBatteryHwLocation OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "A text description of the hardware location, on complex
multi SBB hardware only, for the battery.
A NULL string indicates that the hardware location could not
be determined or is irrelevant."
	::= { cpqSiSysBatteryEntry 16 }


cpqSiDockingStationStatus OBJECT-TYPE
	SYNTAX INTEGER {
	notSupported(1),
	docked(2),
	undocked(3)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This value specifies the connection of the computer
system to a docking station.

The following connection states are supported:

notSupported(1)
This system does not interface to a docking station.

docked(2)
This system is connected to a docking station.

undocked(3)
This system is not connect to a docking station."
	::= { cpqSiDockingStation 1 }


cpqSiDockingStationSerialNum OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The serial number of the docking station.

The string will be empty if the docking station does not support a
serial or the system does not interface to a docking station."
	::= { cpqSiDockingStation 2 }


cpqSiDockingStationModel OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The model name of the docking station.

The string will be empty if the docking station does not report the
model name or the system does not interface to a docking station."
	::= { cpqSiDockingStation 3 }


cpqSiDockingStationAssetTag OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This is a customer changeable identifier that is set to the docking
station serial number at the time of manufacture.

The string will be empty if the docking station does not report an
asset tag or the system does not interface to a docking station."
	::= { cpqSiDockingStation 4 }


cpqSiFruTable OBJECT-TYPE
	SYNTAX SEQUENCE OF CpqSiFruEntry
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Table of Field Replaceable Units of system, providing
inventory and asset control information.  This table is
referenced from logical hardware descriptions elsewhere in
the MIB."
	::= { cpqSiFru 1 }


cpqSiFruEntry OBJECT-TYPE
	SYNTAX CpqSiFruEntry
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Each entry represents a Field Replaceable Unit (FRU) of hardware."
	INDEX { cpqSiFruIndex  }

	::= { cpqSiFruTable 1 }

cpqSiFruEntry ::=
	SEQUENCE {
		cpqSiFruIndex INTEGER,
		cpqSiFruType INTEGER,
		cpqSiFruDescr DisplayString,
		cpqSiFruVendor DisplayString,
		cpqSiFruPartNumber DisplayString,
		cpqSiFruRevision DisplayString,
		cpqSiFruFirmwareRevision DisplayString,
		cpqSiFruSerialNumber DisplayString,
		cpqSiFruAssetNo DisplayString,
		cpqSiFruClass INTEGER,
		cpqSiFruSlotNumber DisplayString,
		cpqSiFruSubAssemblyNumber INTEGER,
		cpqSiFruAssemblyNumber INTEGER,
		cpqSiFruChassisNumber INTEGER,
		cpqSiFruPositionNumber INTEGER,
		cpqSiFruCabinetIDNumber INTEGER,
		cpqSiFruSiteLocation INTEGER,
		cpqSiFruDiagStatus INTEGER,
		cpqSiFruExtendedDiagStatus INTEGER,
		cpqSiFruCellTablePtr INTEGER,
		cpqSiFruIOCTablePtr INTEGER,
		cpqSiFruFileId DisplayString,
		cpqSiFruScanRev DisplayString
		}

cpqSiFruIndex OBJECT-TYPE
	SYNTAX INTEGER
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "A locally-unique index value."
	::= { cpqSiFruEntry 1 }


cpqSiFruType OBJECT-TYPE
	SYNTAX INTEGER {
	unknown(1),
	other(2),
	motherBoard(3),
	processor(4),
	memoryCard(5),
	memoryModule(6),
	peripheralDevice(7),
	systemBusBridge(8),
	powerSupply(9),
	chassis(10),
	fan(11),
	ioCard(12)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "General category of the type of FRU that this is."
	::= { cpqSiFruEntry 2 }


cpqSiFruDescr OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "More detailed description of FRU type, if known."
	::= { cpqSiFruEntry 3 }


cpqSiFruVendor OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Manufacturer name or ID."
	::= { cpqSiFruEntry 4 }


cpqSiFruPartNumber OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Number by which this unit is orderable."
	::= { cpqSiFruEntry 5 }


cpqSiFruRevision OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Version number of this unit. If artwork level is available, it will
appear as 'Artwork: XXX' following FRU version portion."
	::= { cpqSiFruEntry 6 }


cpqSiFruFirmwareRevision OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The revision of the firmware, if any.  Otherwise null."
	::= { cpqSiFruEntry 7 }


cpqSiFruSerialNumber OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The serial number of this unit's instance."
	::= { cpqSiFruEntry 8 }


cpqSiFruAssetNo OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The asset number for this unit. This string may be limited."
	::= { cpqSiFruEntry 9 }


cpqSiFruClass OBJECT-TYPE
	SYNTAX INTEGER {
	unknown(1),
	other(2),
	currentBoardInSlot(3),
	priorBoardInSlot(4),
	parentBoard(5),
	priorParentBoard(6),
	priorParentSystem(7)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Represents the status category of the unit."
	::= { cpqSiFruEntry 10 }


cpqSiFruSlotNumber OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Physical slot number of FRU."
	::= { cpqSiFruEntry 11 }


cpqSiFruSubAssemblyNumber OBJECT-TYPE
	SYNTAX INTEGER
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Subassembly containing this FRU.  From FRU V5.0."
	::= { cpqSiFruEntry 12 }


cpqSiFruAssemblyNumber OBJECT-TYPE
	SYNTAX INTEGER
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Assembly containing this FRU.  From FRU V5.0."
	::= { cpqSiFruEntry 13 }


cpqSiFruChassisNumber OBJECT-TYPE
	SYNTAX INTEGER
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Chassis containing this FRU.  From FRU V5.0."
	::= { cpqSiFruEntry 14 }


cpqSiFruPositionNumber OBJECT-TYPE
	SYNTAX INTEGER
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Position in Chassis to help locate FRU.  From FRU V5.0."
	::= { cpqSiFruEntry 15 }


cpqSiFruCabinetIDNumber OBJECT-TYPE
	SYNTAX INTEGER
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Cabinet number containing this FRU.  From FRU V5.0."
	::= { cpqSiFruEntry 16 }


cpqSiFruSiteLocation OBJECT-TYPE
	SYNTAX INTEGER
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Site code for system containing this FRU.  From FRU V5.0."
	::= { cpqSiFruEntry 17 }


cpqSiFruDiagStatus OBJECT-TYPE
	SYNTAX INTEGER {
	unknown(1),
	ok(2),
	degraded(3),
	failed(4),
	disabled(5)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Use system status values to describe current state of the
FRU."
	::= { cpqSiFruEntry 18 }


cpqSiFruExtendedDiagStatus OBJECT-TYPE
	SYNTAX INTEGER
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Diagnostic Status value returned by Device Specific 
diagnostics.  Usually through a diagnostic status register
on the device.  See product manual for bit descriptions."
	::= { cpqSiFruEntry 19 }


cpqSiFruCellTablePtr OBJECT-TYPE
	SYNTAX INTEGER
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "Index for the cell in cpqSeCellTable where this FRU is physically located."
	::= { cpqSiFruEntry 20 }


cpqSiFruIOCTablePtr OBJECT-TYPE
	SYNTAX INTEGER
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "Index for the I/O Chassis in cpqSeIOCTablePtr where this FRU is physically located"
	::= { cpqSiFruEntry 21 }


cpqSiFruFileId OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "This represents the FRU file identifier"
	::= { cpqSiFruEntry 22 }


cpqSiFruScanRev OBJECT-TYPE
	SYNTAX DisplayString (SIZE(0..255))
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "This represents FRU scan revision"
	::= { cpqSiFruEntry 23 }


cpqSiRackEnclosureMgrTable OBJECT-TYPE
	SYNTAX SEQUENCE OF CpqSiRackEnclosureMgrEntry
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "Table of possible rack and/or enclosure based systems."
	::= { cpqSiRackEnclosure 1 }


cpqSiRackEnclosureMgrEntry OBJECT-TYPE
	SYNTAX CpqSiRackEnclosureMgrEntry
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "A entry for a rack and/or enclosure based system."
	INDEX { cpqSiRackEnclosureMgrIndex  }

	::= { cpqSiRackEnclosureMgrTable 1 }

cpqSiRackEnclosureMgrEntry ::=
	SEQUENCE {
		cpqSiRackEnclosureMgrIndex INTEGER,
		cpqSiRackEnclosureMgrType INTEGER,
		cpqSiRackEnclosureMgrIpAddr DisplayString,
		cpqSiRackEnclosureMgrWebLink DisplayString,
		cpqSiRackEnclosureMgrCondition INTEGER,
		cpqSiRackEnclosureMgrSerialNumber DisplayString,
		cpqSiRackEnclosureMgrModel DisplayString,
		cpqSiRackEnclosureMgrName DisplayString,
		cpqSiRackEnclosureMgrFwRev DisplayString,
		cpqSiRackEnclosureMgrProductID DisplayString,
		cpqSiRackEnclosureMgrUUID DisplayString
		}

cpqSiRackEnclosureMgrIndex OBJECT-TYPE
	SYNTAX INTEGER
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "A locally-unique index value."
	::= { cpqSiRackEnclosureMgrEntry 1 }


cpqSiRackEnclosureMgrType OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	noEnclosureManagement(2),
	enclosureManagement(3),
	onboardAdminManagement(4)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "This value specifies the type of enclosure management.

other(1)
When the type not be determined.

noEnclosureManagement(2)
The server is part of a rack/enclosure managed system, but there
is no dedicated enclosure manager.

enclosureManagement(3)
The server is part of a rack/enclosure managed system with a
dedicated enclosure manager.

onboardAdminManagement(4)
The server is part of a rack/enclosure managed system with a
onboard Administrator."
	::= { cpqSiRackEnclosureMgrEntry 2 }


cpqSiRackEnclosureMgrIpAddr OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The IP address of the rack enclosure manager.

The string will be empty if the enclosure does not report the
information or it could not be determined."
	::= { cpqSiRackEnclosureMgrEntry 3 }


cpqSiRackEnclosureMgrWebLink OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The web link to the enclosure managers web based management
information for the enclosure.

The string will be empty if the enclosure does not report the
information or it could not be determined."
	::= { cpqSiRackEnclosureMgrEntry 4 }


cpqSiRackEnclosureMgrCondition OBJECT-TYPE
	SYNTAX INTEGER {
	other(1),
	ok(2),
	degraded(3),
	failed(4)
	}
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The overall condition of the Enclosure.  For more detailed
status information, follow the cpqSiEnclosureMgrWebLink through
the Web Management Agent interface.

other(1)
This is the default condition for systems when
cpqSiRackEnclosureMgrType has a value of
noEnclosureManagement(2).

When cpqSiRackEnclosureMgrType has a value of
enclosureManagement(3), this indicates the status of the
enclosure manager could not be determined.

ok(2)
The enclosure manager is in an ok state.  Follow the
cpqSiRackEnclosureMgrWebLink link in the Web Management Agents
to manage the enclosure.

degraded(3)
The enclosure manager is in a degraded state.  Follow the
cpqSiRackEnclosureMgrWebLink link in the Web Management Agents
to manage the enclosure.

failed(4)
The enclosure manager is in a failed state.  Follow the
cpqSiRackEnclosureMgrWebLink link in the Web Management Agents
to manage the enclosure."
	::= { cpqSiRackEnclosureMgrEntry 5 }


cpqSiRackEnclosureMgrSerialNumber OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION "The serial number of the enclosure.

The string will be empty if the enclosure does not report the
information or it could not be determined."
	::= { cpqSiRackEnclosureMgrEntry 6 }


cpqSiRackEnclosureMgrModel OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "The model name of the enclosure.
The string will be empty if it could not be determined."
	::= { cpqSiRackEnclosureMgrEntry 7 }


cpqSiRackEnclosureMgrName OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "The name of the enclosure. This name logically groups together the 
Blade servers installed in the same enclosure and it is shared 
with the other servers in the enclosure.
The string will be empty if it could not be determined."
	::= { cpqSiRackEnclosureMgrEntry 8 }


cpqSiRackEnclosureMgrFwRev OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "The Firmware revision of the Enclosure Manager/Onboard Administrator.
The string will be empty if it could not be determined."
	::= { cpqSiRackEnclosureMgrEntry 9 }


cpqSiRackEnclosureMgrProductID OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "The Enclosure product identifier. The string will be empty 
if it could not be determined."
	::= { cpqSiRackEnclosureMgrEntry 10 }


cpqSiRackEnclosureMgrUUID OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "The Enclosure unique identifier. The string will be empty 
if it could not be determined."
	::= { cpqSiRackEnclosureMgrEntry 11 }


cpqSiServerBladeEnclosureBayNumber OBJECT-TYPE
	SYNTAX INTEGER
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "This value specifies the enclosure bay number occupied by the blade.
In case of a blade occupying multiple bays, this will be the lowest
enclosure bay number of all the bay numbers occupied by this balde"
	::= { cpqSiServerBlade 1 }


cpqSiServerBladeHeight OBJECT-TYPE
	SYNTAX INTEGER {
	unknown(1),
	halfHeightBlade(2),
	fullHeightBlade(3)
	}
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "Blade height is the Blade length.

unknown(1)
This indicates it could not be determined.

halfHeightBlade(2)
This indicates a half-height server Blade.

fullHeightBlade(3)
This indicates a full-height server Blade."
	::= { cpqSiServerBlade 2 }


cpqSiServerBladeWidth OBJECT-TYPE
	SYNTAX INTEGER {
	unknown(1),
	singleWide(2),
	doubleWide(3)
	}
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "Width of the Blade in terms of Enclosure Bays. This pertain to the
Blade side that connects to the enclosure backplane."
	::= { cpqSiServerBlade 3 }


cpqSiRackName OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "The rack name. This name is used to logically group together 
enclosures in a rack and it is shared with other enclosures 
in the rack. 
The string will be empty if it could not be determined."
	::= { cpqSiRack 1 }


cpqSiRackUUID OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "The rack unique identifier. The string will be empty 
if it could be determined."
	::= { cpqSiRack 2 }


cpqSiMPHostName OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "The host name of the Management Processor.
The string will be empty if it could not be determined."
	::= { cpqSiMP 1 }


cpqSiMPHealthStatus OBJECT-TYPE
	SYNTAX INTEGER {
	unknown(1),
	ok(2),
	degraded(3),
	failed(4)
	}
	ACCESS read-only
	STATUS obsolete
	DESCRIPTION "The health status of the Management Processor."
	::= { cpqSiMP 2 }


cpqSiHoodRemoved TRAP-TYPE
      ENTERPRISE compaq
      VARIABLES { sysName, cpqHoTrapFlags }
      --#SUMMARY "Hood is removed from unit."
      --#ARGUMENTS {}
      --#SEVERITY MAJOR
      --#TIMEINDEX 99
      --#STATE DEGRADED
      --#TYPE "System hood is removed (2001)"
      --#ENABLE true
      --#CATEGORY "Proliant System and Environmental Events"
DESCRIPTION "System hood is removed.  The hood status has been set to removed.  The system's hood is not in a properly installed state. This situation may result in improper cooling of the system due to air flow changes caused by the missing hood.  User Action: Replace the cover (hood), ensure the system's cover is properly installed. Verify the system is in working order."
      ::= 2001

cpqSiMonitorConditionOK TRAP-TYPE
      ENTERPRISE compaq
      VARIABLES { sysName, cpqHoTrapFlags, cpqSiMonitorIndex }
      --#SUMMARY "The monitor's condition has been set to OK."
      --#ARGUMENTS {}
      --#SEVERITY INFORMATIONAL
      --#TIMEINDEX 99
      --#STATE OPERATIONAL
      --#MSG_FORMATTER "$V3V#Monitor Index: #"
      --#TYPE "Monitor Condition OK (2002)"
      --#ENABLE true
      --#CATEGORY "Proliant System and Environmental Events"
DESCRIPTION "Fault reporting features have returned to within their normal operating range for the monitor indicated by cpqSiMonitorIndex. The monitor's condition has been set to OK.  User Action:  None."
      ::= 2002

cpqSiMonitorConditionDegraded TRAP-TYPE
      ENTERPRISE compaq
      VARIABLES { sysName, cpqHoTrapFlags, cpqSiMonitorIndex }
      --#SUMMARY "The monitor's condition has been set to degraded."
      --#ARGUMENTS {}
      --#SEVERITY MINOR
      --#TIMEINDEX 99
      --#STATE DEGRADED
      --#MSG_FORMATTER "$V3V#Monitor Index: #"
      --#TYPE "Monitor Condition Degraded (2003)"
      --#ENABLE true
      --#CATEGORY "Proliant System and Environmental Events"
DESCRIPTION "A fault reporting feature has exceeded normal limits for the monitor indicated by the cpqSiMonitorIndex. The monitor's condition is degraded due to the internal temperature exceeding normal operating limits.  The monitor is still useable, but action should be taken to return the condition to OK.  User Action: Physically check for obstructions to air flow around the monitor.  Check the thermostat in the room that the system occupies.  Allow the monitor to cool by turning off the monitor for 5 minutes then turn the monitor back on.  After the monitor cools, another alarm indicating an improving condition, such as Monitor OK, will be issued."
      ::= 2003

cpqSiMonitorConditionFailed TRAP-TYPE
      ENTERPRISE compaq
      VARIABLES { sysName, cpqHoTrapFlags, cpqSiMonitorIndex }
      --#SUMMARY "The monitor's condition has been set to failed."
      --#ARGUMENTS {}
      --#SEVERITY CRITICAL
      --#TIMEINDEX 99
      --#STATE NONOPERATIONAL
      --#MSG_FORMATTER "$V3V#Monitor Index: #"
      --#TYPE "Monitor Condition Failed (2004)"
      --#ENABLE true
      --#CATEGORY "Proliant System and Environmental Events"
DESCRIPTION "A fault reporting feature has exceeded normal limits in the monitor indicated by the cpqSiMonitorIndex. The monitor's condition has been set to failed due to an operational feature exceeding normal operating limits.  The monitor will not be useable and should be replaced.  User Action: Make a note of the monitor model number and serial number.  Replace the monitor.  Refer to the appropriate Maintenance and Service Guide for detailed information on a component replacement."
      ::= 2004

cpqSiCorrMemErrStatusDegraded TRAP-TYPE
      ENTERPRISE compaq
      VARIABLES { sysName, cpqHoTrapFlags, cpqSiMemErrorIndex }
      --#SUMMARY "The Memory Module %d ECC status has been set to degraded."
      --#ARGUMENTS {3}
      --#SEVERITY MINOR
      --#TIMEINDEX 99
      --#STATE DEGRADED
      --#MSG_FORMATTER "$V3V#Memory Module Number: #"
      --#TYPE "Excessive Correctable Memory Errors (2005)"
      --#ENABLE true
      --#CATEGORY "Proliant System and Environmental Events"
DESCRIPTION "Correctable memory error count has exceeded the threshold for the memory module indicated by the 'cpqSiMemErrorIndex' variable. The appropriate cpqSiMemModuleECCStatus has been set to degraded.  User Action: For Desktops, the System Administrator should run the F10 Diagnostics on this system and select RAM LONG TEST. If it is determined that a module needs replacing, schedule maintenance for the system and replace the failed memory module.  Refer to the appropriate Maintenance and Service Guide for detailed information on a component replacement."
      ::= 2005

cpqSiCorrMemErrStatusOk TRAP-TYPE
      ENTERPRISE compaq
      VARIABLES { sysName, cpqHoTrapFlags, cpqSiMemErrorIndex }
      --#SUMMARY "The Memory Module %d ECC status has been set to OK."
      --#ARGUMENTS {3}
      --#SEVERITY INFORMATIONAL
      --#TIMEINDEX 99
      --#STATE OPERATIONAL
      --#MSG_FORMATTER "$V3V#Memory Module Number: #"
      --#TYPE "Correctable Memory Errors Count OK (2006)"
      --#ENABLE true
      --#CATEGORY "Proliant System and Environmental Events"
DESCRIPTION "Correctable memory error count is now below the threshold for the memory module indicated by the 'cpqSiMemErrorIndex' variable. The appropriate cpqSiMemModuleECCStatus has been set to ok.  User Action: None."
      ::= 2006

cpqSiMemConfigChange TRAP-TYPE
      ENTERPRISE compaq
      VARIABLES { sysName, cpqHoTrapFlags, cpqSiMemConfigChangeData }
      --#SUMMARY "The system's memory configuration has changed."
      --#ARGUMENTS {}
      --#SEVERITY INFORMATIONAL
      --#TIMEINDEX 99
      --#STATE OPERATIONAL
      --#MSG_FORMATTER "$V3V#Details: #"
      --#TYPE "Memory modules have changed (2007)"
      --#ENABLE true
      --#CATEGORY "Proliant System and Environmental Events"
DESCRIPTION "A memory configuration change has occurred. CpqSiMemConfigChangeData will indicate which memory modules slots have changed.  User Action: You may want to verify a valid reason for a memory configuration to have occurred. If system issuing the alert is a Desktop running NT, the memory configuration change information is also logged in the NT System Log."
      ::= 2007

cpqSiHotPlugSlotBoardRemoved TRAP-TYPE
      ENTERPRISE compaq
      VARIABLES { sysName, cpqHoTrapFlags, cpqSiHotPlugSlotChassis, cpqSiHotPlugSlotIndex }
      --#SUMMARY "Hot Plug Slot Board Removed from Chassis %d, Slot %d."
      --#ARGUMENTS {2,3}
      --#SEVERITY INFORMATIONAL
      --#TIMEINDEX 99
      --#STATE OPERATIONAL
      --#MSG_FORMATTER "$V3V#Chassis Number: # $V4V#Slot Number: #"
      --#TYPE "Hot Plug Slot Board Removed (2008)"
      --#ENABLE true
      --#CATEGORY "Proliant System and Environmental Events"
DESCRIPTION "Hot Plug Slot Board Removed.  A Hot Plug Slot Board has been removed from the specified chassis and slot.  User Action: None."
      ::= 2008

cpqSiHotPlugSlotBoardInserted TRAP-TYPE
      ENTERPRISE compaq
      VARIABLES { sysName, cpqHoTrapFlags, cpqSiHotPlugSlotChassis, cpqSiHotPlugSlotIndex }
      --#SUMMARY "Hot Plug Slot Board Inserted into Chassis %d, Slot %d."
      --#ARGUMENTS {2,3}
      --#SEVERITY INFORMATIONAL
      --#TIMEINDEX 99
      --#STATE OPERATIONAL
      --#MSG_FORMATTER "$V3V#Chassis Number: # $V4V#Slot Number: #"
      --#TYPE "Hot Plug Slot Board Inserted (2009)"
      --#ENABLE true
      --#CATEGORY "Proliant System and Environmental Events"
DESCRIPTION "Hot Plug Slot Board Inserted.  A Hot Plug Slot Board has been inserted into the specified chassis and slot.  User Action: None."
      ::= 2009

cpqSiHotPlugSlotPowerUpFailed TRAP-TYPE
      ENTERPRISE compaq
      VARIABLES { sysName, cpqHoTrapFlags, cpqSiHotPlugSlotChassis, cpqSiHotPlugSlotIndex, cpqSiHotPlugSlotErrorStatus }
      --#SUMMARY "Hot Plug Slot Board Failed in Chassis %d, Slot %d, Error %d."
      --#ARGUMENTS {2,3,4}
      --#SEVERITY CRITICAL
      --#TIMEINDEX 99
      --#STATE FAILED
      --#MSG_FORMATTER "$V3V#Chassis Number: # $V4V#Slot Number: # $V5V#Hot Plug Error Status: #"
      --#TYPE "Hot Plug Slot Board Failed (2010)"
      --#ENABLE true
      --#CATEGORY "Proliant System and Environmental Events"
DESCRIPTION "Hot Plug Slot Board Failed Power-Up.  A Hot Plug Slot Board has failed to power-up in the specified chassis and slot.  User Action: Insure the board and all cables are installed correctly and the board type and revision are the same as the replaced board."
      ::= 2010

cpqSiSysBatteryFailure TRAP-TYPE
      ENTERPRISE compaq
      VARIABLES { sysName, cpqHoTrapFlags, cpqSiSysBatteryIndex, cpqSiSysBatterySerialNum }
      --#SUMMARY "Battery %d has failed."
      --#ARGUMENTS {2}
      --#SEVERITY MAJOR
      --#TIMEINDEX 99
      --#STATE DEGRADED
      --#MSG_FORMATTER "$V3V#Battery Index: # $V4V#Battery Serial Number: #"
      --#TYPE "Battery Failure (2011)"
      --#ENABLE true
      --#CATEGORY "Proliant System and Environmental Events"
DESCRIPTION "The battery indicated by cpqSiSysBatteryIndex has failed and must be replaced.  User Action:  Contact your System Administrator or Authorized Reseller to order a replacement battery. Recycle your old battery. For proper disposal information, refer to the documentation that came with your computer."
      ::= 2011

cpqSiSysBatteryChargingDegraded TRAP-TYPE
      ENTERPRISE compaq
      VARIABLES { sysName, cpqHoTrapFlags, cpqSiSysBatteryIndex, cpqSiSysBatterySerialNum }
      --#SUMMARY "Battery %d has degraded charging capacity."
      --#ARGUMENTS {2}
      --#SEVERITY MAJOR
      --#TIMEINDEX 99
      --#STATE DEGRADED
      --#MSG_FORMATTER "$V3V#Battery Index: # $V4V#Battery Serial Number: #"
      --#TYPE "Battery Charging Degradation (2012)"
      --#ENABLE true
      --#CATEGORY "Proliant System and Environmental Events"
DESCRIPTION "Significant battery degradation has occurred with battery indicated by cpqSiSysBatteryIndex.  The battery can no longer be fully recharged.  User Action: If using multiple batteries, run the Power Conservation Utility to identify the battery location.  Contact your System Administrator or Authorized Reseller to order a replacement battery."
      ::= 2012

cpqSiSysBatteryCalibrationError TRAP-TYPE
      ENTERPRISE compaq
      VARIABLES { sysName, cpqHoTrapFlags, cpqSiSysBatteryIndex, cpqSiSysBatterySerialNum }
      --#SUMMARY "Battery %d has calibration error."
      --#ARGUMENTS {2}
      --#SEVERITY MAJOR
      --#TIMEINDEX 99
      --#STATE DEGRADED
      --#MSG_FORMATTER "$V3V#Battery Index: # $V4V#Battery Serial Number: #"
      --#TYPE "Battery Calibration Error (2013)"
      --#ENABLE true
      --#CATEGORY "Proliant System and Environmental Events"
DESCRIPTION "Calibration is needed with battery indicated by cpqSiSysBatteryIndex.  The battery can not correctly indicate capacity.  User Action: Run the Power Conservation Utility.  Contact your System Administrator or Authorized Reseller to order a replacement battery."
      ::= 2013

END

