
ATM2-MIB DEFINITIONS ::= BEGIN

-- From file: "atm2.mi2"
-- Compile options "4 G A M"

IMPORTS
    Gauge32, Counter32, Integer32
            FROM SNMPv2-SMI-v1
    OBJECT-TYPE
            FROM RFC-1212
    TRAP-TYPE
            FROM RFC-1215
    ifIndex
	    FROM RFC1213-MIB
    TruthValue, RowStatus, TimeStamp, DisplayString
            FROM SNMPv2-TC-v1
    InterfaceIndex
            FROM IF-MIB
    atmMIB, atmMIBObjects
	    FROM ATM-TC-MIB
    atmVpCrossConnectIndex, atmVpCrossConnectLowIfIndex, atmVpCrossConnectLowVpi,
    atmVpCrossConnectHighIfIndex, atmVpCrossConnectHighVpi
	    FROM ATM-MIB
    atmVcCrossConnectIndex, atmVcCrossConnectLowIfIndex, atmVcCrossConnectLowVpi, 
    atmVcCrossConnectLowVci, atmVcCrossConnectHighIfIndex, atmVcCrossConnectHighVpi,
    atmVcCrossConnectHighVci
	    FROM ATM-MIB
    atmInterfaceConfEntry, atmVplEntry, atmVplVpi, 
    atmVplOperStatus, atmVclEntry, atmVclVpi, atmVclVci, 
    atmVclOperStatus, atmVpCrossConnectEntry, 
    atmVcCrossConnectEntry
            FROM ATM-MIB
    AtmAddr, AtmSigDescrParamIndex, AtmInterfaceType, 
    AtmIlmiNetworkPrefix, AtmVcIdentifier, AtmVpIdentifier, 
    AtmTrafficDescrParamIndex
            FROM ATM-TC-MIB;


  atm2MIB OBJECT IDENTIFIER ::= { atmMIBObjects 14}

--atm2MIB OBJECT IDENTIFIER ::= { experimental XX }
-- MODULE-IDENTITY
--  LastUpdated
--    9612051200Z
--  OrgName
--    IETF AToMMIB Working Group
--  ContactInfo
--              Faye Ly
--      Postal:  3Com Networks Inc.
--               Santa Clara, CA 95052
--               US
--      Tel:     +1 408 764 6576
--      Fax:     +1 408 495 2599
--      E-Mail:  faye@3com.com
--    
--               Michael Noto
--      Postal:  Network Equipment Technologies
--               800 Saginaw Drive RM 21.1.111
--               Redwood City, CA 94063
--               US
--      Tel:     +1 415 569 7143
--      Fax:     +1 908 758 4177
--      E-mail:  mike_noto@net.com
--    
--               Andrew Smith
--      Postal:  Extreme Networks
--               1601 S. De Anza Blvd, #220
--               Cupertino, CA 95014
--               US
--      Tel:     +1 408 342 0985
--      Fax:     +1 408 342 0989
--      E-Mail:  ansmith@ix.netcom.com
--    
--               Ethan Mickey Spiegel
--      Postal:  Cisco Systems
--               170 W. Tasman Drive
--               San Jose, CA 95134-1706
--      Tel:     +1 408 526 6408
--      Fax:     +1 408 526 6488
--      E-Mail:  mspiegel@cisco.com
--    
--               Kaj Tesink
--      Postal:  Bell Communications Research
--               331 Newman Springs Road
--               Red Bank, NJ 07701
--               US
--      Tel:     +1 908 758 5254
--      Fax:     +1 908 758 4177
--      E-mail:  kaj@cc.bellcore.com
--  Descr
--    This MIB Module is a supplement to the
--    ATM-MIB [1].

atm2MIBObjects  OBJECT IDENTIFIER ::= { atm2MIB 1 }
atm2MIBTraps    OBJECT IDENTIFIER ::= { atm2MIB 2 }
atmPvcTraps     OBJECT IDENTIFIER ::= { atm2MIBTraps 1 }
atmPvcTrapsPrefix OBJECT IDENTIFIER ::= { atmPvcTraps 0 }
atm2MIBConformance OBJECT IDENTIFIER ::= { atm2MIB 3 }
atm2MIBGroups   OBJECT IDENTIFIER ::= { atm2MIBConformance 1 }
atm2MIBCompliances OBJECT IDENTIFIER ::= { atm2MIBConformance 2 }

atmSvcVpCrossConnectTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AtmSvcVpCrossConnectEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "The ATM SVPC Cross Connect table.  A
        bi-directional VP cross-connect between two
        switched VPLs is modeled as one entry in this
        table.  A Soft PVPC cross-connect, between a
        soft permanent VPL and a switched VPL, is
        also modeled as one entry in this table."
    ::= { atm2MIBObjects 1 }

atmSvcVpCrossConnectEntry OBJECT-TYPE
    SYNTAX AtmSvcVpCrossConnectEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "An entry in the ATM SVPC Cross Connect table.
        This entry is used to model a bi-directional
        ATM VP cross-connect between two VPLs."
    INDEX { atmSvcVpCrossConnectIndex, atmSvcVpCrossConnectLowIfIndex, atmSvcVpCrossConnectLowVpi, atmSvcVpCrossConnectHighIfIndex, atmSvcVpCrossConnectHighVpi }
    ::= { atmSvcVpCrossConnectTable 1 }

AtmSvcVpCrossConnectEntry ::= SEQUENCE {
    atmSvcVpCrossConnectIndex INTEGER,
    atmSvcVpCrossConnectLowIfIndex InterfaceIndex,
    atmSvcVpCrossConnectLowVpi AtmVpIdentifier,
    atmSvcVpCrossConnectHighIfIndex InterfaceIndex,
    atmSvcVpCrossConnectHighVpi AtmVpIdentifier,
    atmSvcVpCrossConnectCreationTime TimeStamp,
    atmSvcVpCrossConnectRowStatus RowStatus
    }

atmSvcVpCrossConnectIndex OBJECT-TYPE
    SYNTAX INTEGER(1..2147483647)
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "A unique value to identify this SVPC cross-connect."
    ::= { atmSvcVpCrossConnectEntry 1 }

atmSvcVpCrossConnectLowIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
--    Rsyntax Integer32
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "The value of this object is equal to MIB II's
        ifIndex value of the ATM interface port for this
        SVPC cross-connect.  The term low implies
        that this ATM interface has the numerically lower
        ifIndex value than the other ATM interface
        identified in the same atmSvcVpCrossConnectEntry."
    ::= { atmSvcVpCrossConnectEntry 2 }

atmSvcVpCrossConnectLowVpi OBJECT-TYPE
    SYNTAX AtmVpIdentifier
--    Rsyntax INTEGER(0..4095)
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "The value of this object is equal to the VPI
        value associated with the SVPC cross-connect
        at the ATM interface that is identified by
        atmSvcVpCrossConnectLowIfIndex.  The VPI value
        cannot exceed the number supported by the
        atmInterfaceMaxVpiBits at the low ATM interface
        port."
    ::= { atmSvcVpCrossConnectEntry 3 }

atmSvcVpCrossConnectHighIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
--    Rsyntax Integer32
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "The value of this object is equal to MIB II's
         ifIndex value of the ATM interface port for
         this SVC VP cross-connect.  The term high
         implies that this ATM interface has the
         numerically higher ifIndex value than the
         other ATM interface identified in the same
         atmSvcVpCrossConnectEntry."
    ::= { atmSvcVpCrossConnectEntry 4 }

atmSvcVpCrossConnectHighVpi OBJECT-TYPE
    SYNTAX AtmVpIdentifier
--    Rsyntax INTEGER(0..4095)
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "The value of this object is equal to the VPI
         value associated with the SVPC cross-connect
         at the ATM interface that is identified by
         atmSvcVpCrossConnectHighIfIndex.  The VPI value
         cannot exceed the number supported by the
         atmInterfaceMaxVpiBits at the high ATM interface
         port."
    ::= { atmSvcVpCrossConnectEntry 5 }

atmSvcVpCrossConnectCreationTime OBJECT-TYPE
    SYNTAX TimeStamp
--    Rsyntax TimeTicks
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The value of MIB II's sysUpTime object
         at the time this bi-directional SVPC
         cross-connect was created.  If the current
         state was entered prior to the last
         re-initialization of the agent, then this
         object contains a zero value."
    ::= { atmSvcVpCrossConnectEntry 6 }

atmSvcVpCrossConnectRowStatus OBJECT-TYPE
    SYNTAX RowStatus
--    Rsyntax INTEGER {
--        active(1),
--        notInService(2),
--        notReady(3),
--        createAndGo(4),
--        createAndWait(5),
--        destroy(6)
--        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "This object is used to delete rows in the
        atmSvcVpCrossConnectTable."
    ::= { atmSvcVpCrossConnectEntry 7 }

atmSvcVcCrossConnectTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AtmSvcVcCrossConnectEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "The ATM SVCC Cross Connect table.  A
         bi-directional VC cross-connect between two
         switched VCLs is modeled as one entry in
         this table.  A Soft PVCC cross-connect,
         between a soft permanent VCL and a switched
         VCL, is also modeled as one entry in this
         table."
    ::= { atm2MIBObjects 2 }

atmSvcVcCrossConnectEntry OBJECT-TYPE
    SYNTAX AtmSvcVcCrossConnectEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "An entry in the ATM SVCC Cross Connect table.
         This entry is used to model a bi-directional ATM
         VC cross-connect between two VCLs."
    INDEX { atmSvcVcCrossConnectIndex, atmSvcVcCrossConnectLowIfIndex, atmSvcVcCrossConnectLowVpi, atmSvcVcCrossConnectLowVci, atmSvcVcCrossConnectHighIfIndex, atmSvcVcCrossConnectHighVpi, atmSvcVcCrossConnectHighVci }
    ::= { atmSvcVcCrossConnectTable 1 }

AtmSvcVcCrossConnectEntry ::= SEQUENCE {
    atmSvcVcCrossConnectIndex INTEGER,
    atmSvcVcCrossConnectLowIfIndex InterfaceIndex,
    atmSvcVcCrossConnectLowVpi AtmVpIdentifier,
    atmSvcVcCrossConnectLowVci AtmVcIdentifier,
    atmSvcVcCrossConnectHighIfIndex InterfaceIndex,
    atmSvcVcCrossConnectHighVpi AtmVpIdentifier,
    atmSvcVcCrossConnectHighVci AtmVcIdentifier,
    atmSvcVcCrossConnectCreationTime TimeStamp,
    atmSvcVcCrossConnectRowStatus RowStatus
    }

atmSvcVcCrossConnectIndex OBJECT-TYPE
    SYNTAX INTEGER(1..2147483647)
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "A unique value to identify this SVCC cross-connect."
    ::= { atmSvcVcCrossConnectEntry 1 }

atmSvcVcCrossConnectLowIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
--    Rsyntax Integer32
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "The value of this object is equal to MIB II's
         ifIndex value of the ATM interface port for this
         SVCC cross-connect.  The term low implies that
         this ATM interface has the numerically lower
         ifIndex value than the other ATM interface
         identified in the same atmSvcVcCrossConnectEntry."
    ::= { atmSvcVcCrossConnectEntry 2 }

atmSvcVcCrossConnectLowVpi OBJECT-TYPE
    SYNTAX AtmVpIdentifier
--    Rsyntax INTEGER(0..4095)
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "The value of this object is equal to the VPI
         value associated with the SVCC cross-connect
         at the ATM interface that is identified by
         atmSvcVcCrossConnectLowIfIndex.  The VPI value
         cannot exceed the number supported by the
         atmInterfaceMaxVpiBits at the low ATM interface
         port."
    ::= { atmSvcVcCrossConnectEntry 3 }

atmSvcVcCrossConnectLowVci OBJECT-TYPE
    SYNTAX AtmVcIdentifier
--    Rsyntax INTEGER(0..65535)
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "The value of this object is equal to the VCI
         value associated with the SVCC cross-connect
         at the ATM interface that is identified by
         atmSvcVcCrossConnectLowIfIndex.  The VCI value
         cannot exceed the number supported by the
         atmInterfaceMaxVciBits at the low ATM interface
         port."
    ::= { atmSvcVcCrossConnectEntry 4 }

atmSvcVcCrossConnectHighIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
--    Rsyntax Integer32
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "The value of this object is equal to MIB II's
         ifIndex value for the ATM interface port for
         this SVCC cross-connect.  The term high implies
         that this ATM interface has the numerically
         higher ifIndex value than the other ATM interface
         identified in the same atmSvcVcCrossConnectEntry."
    ::= { atmSvcVcCrossConnectEntry 5 }

atmSvcVcCrossConnectHighVpi OBJECT-TYPE
    SYNTAX AtmVpIdentifier
--    Rsyntax INTEGER(0..4095)
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "The value of this object is equal to the VPI
         value associated with the SVCC cross-connect
         at the ATM interface that is identified by
         atmSvcVcCrossConnectHighIfIndex.  The VPI value
         cannot exceed the number supported by the
         atmInterfaceMaxVpiBits at the high ATM interface
         port."
    ::= { atmSvcVcCrossConnectEntry 6 }

atmSvcVcCrossConnectHighVci OBJECT-TYPE
    SYNTAX AtmVcIdentifier
--    Rsyntax INTEGER(0..65535)
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "The value of this object is equal to the VCI
         value associated with the SVCC cross-connect
         at the ATM interface that is identified by
         atmSvcVcCrossConnectHighIfIndex.  The VCI value
         cannot exceed the number supported by the
         atmInterfaceMaxVciBits at the high ATM interface
         port."
    ::= { atmSvcVcCrossConnectEntry 7 }

atmSvcVcCrossConnectCreationTime OBJECT-TYPE
    SYNTAX TimeStamp
--    Rsyntax TimeTicks
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The value of MIB II's sysUpTime object
         at the time this bi-directional SVCC
         cross-connect was created.  If the current
         state was entered prior to the last
         re-initialization of the agent, then this
         object contains a zero value."
    ::= { atmSvcVcCrossConnectEntry 8 }

atmSvcVcCrossConnectRowStatus OBJECT-TYPE
    SYNTAX RowStatus
--    Rsyntax INTEGER {
--        active(1),
--        notInService(2),
--        notReady(3),
--        createAndGo(4),
--        createAndWait(5),
--        destroy(6)
--        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "This object is used to delete rows in the
        atmSvcVcCrossConnectTable."
    ::= { atmSvcVcCrossConnectEntry 9 }

atmSigStatTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AtmSigStatEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "This table contains ATM interface signalling monitoring
         , one entry per ATM signalling interface."
    ::= { atm2MIBObjects 3 }

atmSigStatEntry OBJECT-TYPE
    SYNTAX AtmSigStatEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "This list contains signalling statistics variables."
    INDEX { ifIndex }
    ::= { atmSigStatTable 1 }

AtmSigStatEntry ::= SEQUENCE {
    atmSigSSCOPConEvents Counter32,
    atmSigSSCOPErrdPdus Counter32,
    atmSigDetectSetupAttempts Counter32,
    atmSigEmitSetupAttempts Counter32,
    atmSigDetectUnavailRoutes Counter32,
    atmSigEmitUnavailRoutes Counter32,
    atmSigDetectUnavailResrcs Counter32,
    atmSigEmitUnavailResrcs Counter32,
    atmSigDetectCldPtyEvents Counter32,
    atmSigEmitCldPtyEvents Counter32,
    atmSigDetectMsgErrors Counter32,
    atmSigEmitMsgErrors Counter32,
    atmSigDetectClgPtyEvents Counter32,
    atmSigEmitClgPtyEvents Counter32,
    atmSigDetectTimerExpireds Counter32,
    atmSigEmitTimerExpireds Counter32,
    atmSigDetectRestarts Counter32,
    atmSigEmitRestarts Counter32,
    atmSigInEstabls Counter32,
    atmSigOutEstabls Counter32
    }

atmSigSSCOPConEvents OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "SSCOP Connection Events Counter.  This
        counter counts the sum of the following errors:
        
        1) SSCOP Connection Disconnect Counter
        
        The abnormal occurrence of this event is
        characterized by the expiry of Timer_NO_RESPONSE.
        (This event is communicated to the layer management
        with MAA-ERROR code P.  See ITU-T Q.2110 [13].)
        
        2) SSCOP Connection Initiation Failure
        
        This condition indicates the inability to establish
        an SSCOP connection.  This event occurs whenever the
        number of expiries of the connection control timer
        (Timer_CC) exceeds the MaxCC or upon receipt of a
        connection reject message BGREJ PDU.  (This event is
        communicated to layer management with MAA-ERROR
        code O.  See ITU-T Q.2110.)
        
        3) SSCOP Connection Re-Establ/Resynch
        
        This event occurs upon receipt of a BGN PDU or RESYNC
        PDU."
    ::= { atmSigStatEntry 1 }

atmSigSSCOPErrdPdus OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "SSCOP Errored PDUs Counter.  This counter counts the
        sum of the following errors:
        
        1) Invalid PDUs.
           These are defined in SSCOP and consist of PDUs
           with incorrect length (MAA-ERROR code U),
           undefined PDU type code or not 32-bit aligned.
        
        2) PDUs that result in MAA error codes and are
           discarded
           See Errors A-M and Q-T defined in ITU-T Q.2110 [13]."
    ::= { atmSigStatEntry 2 }

atmSigDetectSetupAttempts OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "Call Setup Attempts Counter.  This counter counts
        the number of call setup attempts(both successful
        and unsuccessful) detected on this interface."
    ::= { atmSigStatEntry 3 }

atmSigEmitSetupAttempts OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "Call Setup Attempts Counter.  This counter counts the
        number of call setup attempts(both successful and
        unsuccessful) transmitted on this interface."
    ::= { atmSigStatEntry 4 }

atmSigDetectUnavailRoutes OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "Number of Route Unavailability detected on this
        interface. This counter is incremented when a RELEASE,
        RELEASE COMPLETE (only when not preceded by a RELEASE
        mesg for the same call), ADD PARTY REJECT, or STATUS
        message that contains one of the following cause code
        values is received (Note: These cause values apply to
        both UNI3.0 and UNI3.1):
        
        
        Cause Value            Meaning
        
           1            unallocated (unassigned) number
           2            no route to specified transit network
           3            no route to destination
        
        NOTE:  For this counter, RELEASE COMPLETE
        messages that are a reply to a previous RELEASE
        message and contain the same cause value, are
        redundant (for counting purposes) and should not
        be counted."
    ::= { atmSigStatEntry 5 }

atmSigEmitUnavailRoutes OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "Number of Route Unavailability transmitted from this
        interface. This counter is incremented when a RELEASE,
        RELEASE COMPLETE (only when not preceded by a RELEASE
        mesg for the same call), ADD PARTY REJECT, or STATUS
        message that contains one of the following cause code
        values is transmitted (Note: These cause values apply
        to both UNI3.0 and UNI3.1):
        
        
        Cause Value            Meaning
        
           1            unallocated (unassigned) number
           2            no route to specified transit network
           3            no route to destination
        
        NOTE:  For this counter, RELEASE COMPLETE
        messages that are a reply to a previous RELEASE
        message and contain the same cause value, are
        redundant (for counting purposes) and should not
        be counted."
    ::= { atmSigStatEntry 6 }

atmSigDetectUnavailResrcs OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "Number of Resource Unavailability detected on this
        interfrace.  This counter is incremented when a
        RELEASE, RELEASE COMPLETE (only when not preceded by a
        RELEASE mesg for the same call), ADD PARTY REJECT, or
        STATUS message that contains one of the following cause
        code values is received (Note: These cause values apply
        to both UNI3.0 and UNI3.1 unless otherwise stated):
        
        Cause Value          Meaning
        
           35          requested VPCI/VCI not available
           37          user cell rate not available (UNI3.1
                       only)
           38          network out of order
           41          temporary failure
           45          no VPCI/VCI available
           47          resource unavailable, unspecified
           49          Quality of Service unavailable
           51          user cell rate not available (UNI3.0
                       only)
           58          bearer capability not presently
                       available
           63          Service or option not available,
                       unspecified
           92          too many pending add party requests
        
        NOTE:  For this counter, RELEASE COMPLETE
        messages that are a reply to a previous RELEASE
        message and contain the same cause value, are
        redundant (for counting purposes) and should not
        be counted."
    ::= { atmSigStatEntry 7 }

atmSigEmitUnavailResrcs OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "Number of Resource Unavailability transmitted from
        this interfrace.  This counter is incremented when a
        RELEASE, RELEASE COMPLETE (only when not preceded by a
        RELEASE mesg for the same call), ADD PARTY REJECT, or
        STATUS message that contains one of the following cause
        code values is transmitted (Note: These cause values
        apply to both UNI3.0 and UNI3.1 unless otherwise
        stated):
        
        Cause Value          Meaning
        
           35          requested VPCI/VCI not available
           37          user cell rate not available (UNI3.1
                       only)
           38          network out of order
           41          temporary failure
           45          no VPCI/VCI available
           47          resource unavailable, unspecified
           49          Quality of Service unavailable
           51          user cell rate not available (UNI3.0
                       only)
           58          bearer capability not presently
                       available
           63          Service or option not available,
                       unspecified
           92          too many pending add party requests
        
        NOTE:  For this counter, RELEASE COMPLETE
        messages that are a reply to a previous RELEASE
        message and contain the same cause value, are
        redundant (for counting purposes) and should not
        be counted."
    ::= { atmSigStatEntry 8 }

atmSigDetectCldPtyEvents OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "Number of Called Party Responsible For Unsuccessful
        Call detected on this interface. This counter is
        incremented when a RELEASE, RELEASE COMPLETE (only when
        not preceded by a RELEASE mesg for the same call), ADD
        PARTY REJECT, or STATUS message that contains one of
        the following cause code values is received (Note:
        These cause values apply to both UNI3.0 and UNI3.1):
        
        Cause Value         Meaning
        
           17           user busy
           18           no user responding
           21           call rejected
           22           number changed
           23           user rejects all calls with calling
                        line id restriction (CLIR)
           27           destination out of order
           31           normal, unspecified
           88           incompatible destination
        
        NOTE:  For this counter, RELEASE COMPLETE
        messages that are a reply to a previous RELEASE
        message and contain the same cause value, are
        redundant (for counting purposes) and should not
        be counted.
        
        Note: Cause Value #30 'response to STATUS ENQUIRY'
        was not included in this memo since it did not apply
        to a hard failure."
    ::= { atmSigStatEntry 9 }

atmSigEmitCldPtyEvents OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "Number of Called Party Responsible For Unsuccessful Call
        transmitted from this interface. This counter is
        incremented when a RELEASE, RELEASE COMPLETE (only
        when not preceded by a RELEASE mesg for the same call),
        ADD PARTY REJECT, or STATUS message that contains one
        of the following cause code values is
        transmitted (Note: These cause values apply to both
        UNI3.0 and UNI3.1):
        
        Cause Value         Meaning
        
           17           user busy
           18           no user responding
           21           call rejected
           22           number changed
           23           user rejects all calls with calling
                        line id restriction (CLIR)
           27           destination out of order
           31           normal, unspecified
           88           incompatible destination
        
        NOTE:  For this counter, RELEASE COMPLETE
        messages that are a reply to a previous RELEASE
        message and contain the same cause value, are
        redundant (for counting purposes) and should not
        be counted.
        
        Note: Cause Value #30 'response to STATUS ENQUIRY'
        was not included in this memo since it did not apply
        to a hard failure."
    ::= { atmSigStatEntry 10 }

atmSigDetectMsgErrors OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "Number of Incorrect Messages detected on this
        interface.  The Incorrect Messages Counter reflects any
        sort of incorrect information in a message.  This
        includes:
        
        - RELEASE, RELEASE COMPLETE, ADD PARTY REJECT,
          and STATUS messages transmitted, that contain any of
          the Cause values listed below.
        
        - Ignored messages.  These messages are dropped
          because the message was so damaged that it could
          not be further processed.  A list of dropped
          messages is compiled below:
        
           1.  Message with invalid protocol discriminator
        
           2.  Message with errors in the call reference I.E.
                - Bits 5-8 of the first octet not equal to
                  '0000'
                - Bits 1-4 of the first octet indicating a
                  length other than 3 octets
                - RELEASE COMPLETE message received with a
                  call reference that does not relate to a
                  call active or in progress
                - SETUP message received with call reference
                  flag incorrectly set to 1
                - SETUP message received with a call
                  reference for a call that is already
                  active or in progress.
        
           3.  Message too short
        
        
        The following cause values are monitored by this
        counter (Note: These cause values apply to both UNI3.0
        and UNI3.1 unless otherwise stated):
        
        Cause Value     Meaning
        
           10     VPCI/VCI unacceptable (UNI3.0 only)
           36     VPCI/VCI assignment failure (UNI3.1 only)
           81     invalid call reference value
           82     identified channel does not exist
           89     invalid endpoint reference
           96     mandatory information element is missing
           97     message type non-existent or not
                  implemented
           99     information element non-existent or not
                  implemented
           100    invalid information element contents
           101    message not compatible with call state
           104    incorrect message length
           111    protocol error, unspecified
        
           NOTE:  For this counter, RELEASE COMPLETE
           messages that are a reply to a previous RELEASE
           message and contain the same cause value, are
           redundant (for counting purposes) and should not
           be counted."
    ::= { atmSigStatEntry 11 }

atmSigEmitMsgErrors OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "Number of Incorrect Messages transmitted on this
        interface.  The Incorrect Messages Counter reflects any
        sort of incorrect information in a message.  This
        includes:
        
        
        - RELEASE, RELEASE COMPLETE, ADD PARTY REJECT,
          and STATUS messages transmitted or
          received, that contain any of the Cause values
          listed below.
        
        - Ignored messages.  These messages are dropped
          because the message was so damaged that it could
          not be further processed.  A list of dropped
          messages is compiled below:
        
           1.  Message with invalid protocol discriminator
        
           2.  Message with errors in the call reference I.E.
                - Bits 5-8 of the first octet not equal to
                  '0000'
                - Bits 1-4 of the first octet indicating a
                  length other than 3 octets
                - RELEASE COMPLETE message received with a
                  call reference that does not relate to a
                  call active or in progress
                - SETUP message received with call reference
                  flag incorrectly set to 1
                - SETUP message received with a call
                  reference for a call that is already
                  active or in progress.
        
           3.  Message too short
        
        
        The following cause values are monitored by this
        counter (Note: These cause values apply to both UNI3.0
        and UNI3.1 unless otherwise stated):
        
        Cause Value     Meaning
        
           10     VPCI/VCI unacceptable (UNI3.0 only)
           36     VPCI/VCI assignment failure (UNI3.1 only)
           81     invalid call reference value
           82     identified channel does not exist
           89     invalid endpoint reference
           96     mandatory information element is missing
           97     message type non-existent or not
                  implemented
           99     information element non-existent or not
                  implemented
           100    invalid information element contents
           101    message not compatible with call state
           104    incorrect message length
           111    protocol error, unspecified
        
           NOTE:  For this counter, RELEASE COMPLETE
           messages that are a reply to a previous RELEASE
           message and contain the same cause value, are
           redundant (for counting purposes) and should not
           be counted."
    ::= { atmSigStatEntry 12 }

atmSigDetectClgPtyEvents OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "Number of Calling Party Events detected on this
        interface.  This counter monitors error events that
        occur due to the originating user doing something
        wrong. This counter is incremented when a RELEASE,
        RELEASE COMPLETE (only when not preceded by a RELEASE
        mesg for the same call), ADD PARTY REJECT, or STATUS
        message that contains one of the following cause code
        values is received (Note: These cause values apply to
        both UNI3.0 and UNI3.1):
        
        Cause Value     Meaning
        
           28     invalid number format (address incomplete)
           43     access information discarded
           57     bearer capability not authorized
           65     bearer capability not implemented
           73     unsupported combination of traffic
                  parameters
           78     AAL parameters cannot be supported (UNI3.1
                  only)
           91     invalid transit network selection
           93     AAL parameters cannot be supported (UNI3.0
                  only)
        
           NOTE:  For this counter, RELEASE COMPLETE
           messages that are a reply to a previous RELEASE
           message and contain the same cause value, are
           redundant (for counting purposes) and should not
           be counted."
    ::= { atmSigStatEntry 13 }

atmSigEmitClgPtyEvents OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "Number of Calling Party Events transmitted from this
        interface.  This counter monitors error events that
        occur due to the originating user doing something
        wrong. This counter is incremented when a RELEASE,
        RELEASE COMPLETE (only when not preceded by a RELEASE
        mesg for the same call), ADD PARTY REJECT, or STATUS
        message that contains one of the following cause code
        values is transmitted (Note: These cause values apply
        to both UNI3.0 and UNI3.1):
        
        Cause Value     Meaning
        
           28     invalid number format (address incomplete)
           43     access information discarded
           57     bearer capability not authorized
           65     bearer capability not implemented
           73     unsupported combination of traffic
                  parameters
           78     AAL parameters cannot be supported (UNI3.1
                  only)
           91     invalid transit network selection
           93     AAL parameters cannot be supported (UNI3.0
                  only)
        
           NOTE:  For this counter, RELEASE COMPLETE
           messages that are a reply to a previous RELEASE
           message and contain the same cause value, are
           redundant (for counting purposes) and should not
           be counted."
    ::= { atmSigStatEntry 14 }

atmSigDetectTimerExpireds OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "Number of Timer Expiries detected on this interface.
        The Timer Expiries Counter provides a count of network
        timer expiries, and to some extent, host or switch
        timer expiries.  The conditions for incrementing this
        counter are:
           - Expiry of any network timer
        
           - Receipt of a RELEASE or RELEASE COMPLETE
             message with Cause #102, 'recovery on
             timer expiry'.
        
        NOTE:  For this counter, RELEASE COMPLETE messages
        that are a reply to a previous RELEASE message and
        contain the same cause value, are redundant (for
        counting purposes) and should not be counted."
    ::= { atmSigStatEntry 15 }

atmSigEmitTimerExpireds OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "Number of Timer Expiries transmitted from this
        interface.  The Timer Expiries Counter provides a count
        of network timer expiries, and to some extent, host or
        switch timer expiries.  The conditions for incrementing
        this counter are:
           - Expiry of any network timer
        
           - Receipt of a RELEASE or RELEASE COMPLETE
             message with Cause #102, 'recovery on
             timer expiry'.
        
        NOTE:  For this counter, RELEASE COMPLETE messages
        that are a reply to a previous RELEASE message and
        contain the same cause value, are redundant (for
        counting purposes) and should not be counted."
    ::= { atmSigStatEntry 16 }

atmSigDetectRestarts OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "Number of Restart Activity errors detected on this
        interface.  The Restart Activity Counter provides a
        count of host, switch, or network restart activity.
        This counter is incremented when receiving a RESTART
        message."
    ::= { atmSigStatEntry 17 }

atmSigEmitRestarts OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "Number of Restart Activity errors transmitted from
        this interface.  The Restart Activity Counter provides
        a count of host, switch, or network restart activity.
        This counter is incremented when transmitting a RESTART
        message."
    ::= { atmSigStatEntry 18 }

atmSigInEstabls OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "Number of SVC VCCs established at this signalling
        entity for incoming connections."
    ::= { atmSigStatEntry 19 }

atmSigOutEstabls OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "Number of SVC VCCs established at this signalling
        entity for outgoing connections."
    ::= { atmSigStatEntry 20 }

atmSigSupportTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AtmSigSupportEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "This table contains ATM local interface configuration
        parameters, one entry per ATM signalling interface."
    ::= { atm2MIBObjects 4 }

atmSigSupportEntry OBJECT-TYPE
    SYNTAX AtmSigSupportEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "This list contains signalling configuration parameters
        and state variables."
    INDEX { ifIndex }
    ::= { atmSigSupportTable 1 }

AtmSigSupportEntry ::= SEQUENCE {
    atmSigSupportClgPtyNumDel INTEGER,
    atmSigSupportClgPtySubAddr INTEGER,
    atmSigSupportCldPtySubAddr INTEGER,
    atmSigSupportHiLyrInfo INTEGER,
    atmSigSupportLoLyrInfo INTEGER,
    atmSigSupportBlliRepeatInd INTEGER,
    atmSigSupportAALInfo INTEGER,
    atmSigSupportPrefCarrier OCTET STRING
    }

atmSigSupportClgPtyNumDel OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "This object indicates whether the Calling Party Number
        Information Element is transferred to the called party
        address.  The value of this object can be:
          - enabled(1)  This Information Element is transferred
                        to the called party
        
          - disabled(2) This Information Element is NOT
                        transferred to the called party."
    ::= { atmSigSupportEntry 1 }

atmSigSupportClgPtySubAddr OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "This object indicates whether to accept and transfer
        the Calling Party Subaddress Information Element from
        the calling party to the called party.  Calling party
        subaddress information shall only be transferred to the
        called party if calling party number delivery is
        enabled (i.e., atmSigSupportClgPtyNumDel =
        'enabled(1)'.  The value of this object can be:
          - enabled(1)  This Information Element is transferred
                        to the called party
        
          - disabled(2) This Information Element is NOT
                        transferred to the called party."
    ::= { atmSigSupportEntry 2 }

atmSigSupportCldPtySubAddr OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "This object indicates whether to accept, transfer, and
        deliver the Called Party Subaddress Information Element
        from the calling party to the called party.  The value
        of this object can be:
          - enabled(1)  This Information Element is transferred
                        to the called party
        
          - disabled(2) This Information Element is NOT
                        transferred to the called party."
    ::= { atmSigSupportEntry 3 }

atmSigSupportHiLyrInfo OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "This object indicates whether to accept, transfer, and
        deliver the Broadband High Layer Information Element
        from the calling party to the called party.  The value
        of this object can be:
          - enabled(1)  This Information Element is transferred
                        to the called party
        
          - disabled(2) This Information Element is NOT
                        transferred to the called party."
    ::= { atmSigSupportEntry 4 }

atmSigSupportLoLyrInfo OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "This object indicates whether to accept, transfer, and
        deliver the Broadband Low Layer Information Element
        from the calling party to the called party.  The value
        of this object can be:
          - enabled(1)  This Information Element is transferred
                        to the called party
        
          - disabled(2) This Information Element is NOT
                        transferred to the called party."
    ::= { atmSigSupportEntry 5 }

atmSigSupportBlliRepeatInd OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "This object indicates whether to accept, transfer, and
        deliver the Broadband Repeat Indicator with two or
        three instances of the Broadband Low Layer Information
        Element for low layer information selection from the
        calling party to the called party.  This object shall
        only be transferred if atmSigSupportLoLyrInfo =
        'enabled(1)'.  The value of this object can be:
          - enabled(1)  This Information Element is transferred
                        to the called party
        
          - disabled(2) This Information Element is NOT
                        transferred to the called party."
    ::= { atmSigSupportEntry 6 }

atmSigSupportAALInfo OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "This object indicates whether to accept, transfer, and
        deliver the ATM Adaptation Layer Parameters Information
        Element from the calling party to the called party.
        The value of this object can be:
          - enabled(1)  This Information Element is transferred
                        to the called party
        
          - disabled(2) This Information Element is NOT
                        transferred to the called party."
    ::= { atmSigSupportEntry 7 }

atmSigSupportPrefCarrier OBJECT-TYPE
    SYNTAX OCTET STRING
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "This parameter identifies the carrier to which
        intercarrier calls originated from this interface are
        routed when transit network selection information is
        not provided by the calling party.  If a Carrier
        Identification Code (CIC) is used the parameter shall
        contain the CIC.  For three-digit CICs, the first octet
        shall be '0' and the CIC is contained in the three
        following octets.  If the preferred carrier feature is
        not supported the value is a zero-length string."
    ::= { atmSigSupportEntry 8 }

atmSigDescrParamTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AtmSigDescrParamEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "A table contains signalling capabilities of VCLs
        except the Traffic Descriptor.  Traffic
        descriptors are described in the
        atmTrafficDescrParamTable."
    REFERENCE
        "ATM Forum User-Network Interface Specification,
        Version 3.1, Section 5.4.5 Variable Length
        Information Elements."
    ::= { atm2MIBObjects 5 }

atmSigDescrParamEntry OBJECT-TYPE
    SYNTAX AtmSigDescrParamEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "Each entry in this table represents a set of
        signalling capabilities that can be applied to a
        VCL. There is no requirement for unique entries,
        except that the index must be unique.  Objects
        atmSigDescrParamRowStatus is required during
        creation."
    INDEX { atmSigDescrParamIndex }
    ::= { atmSigDescrParamTable 1 }

AtmSigDescrParamEntry ::= SEQUENCE {
    atmSigDescrParamIndex AtmSigDescrParamIndex,
    atmSigDescrParamAalType INTEGER,
    atmSigDescrParamAalSscsType INTEGER,
    atmSigDescrParamBhliType INTEGER,
    atmSigDescrParamBhliInfo OCTET STRING,
    atmSigDescrParamBbcConnConf INTEGER,
    atmSigDescrParamBlliLayer2 INTEGER,
    atmSigDescrParamBlliLayer3 INTEGER,
    atmSigDescrParamBlliPktSize INTEGER,
    atmSigDescrParamBlliSnapId INTEGER,
    atmSigDescrParamBlliOuiPid OCTET STRING,
    atmSigDescrParamRowStatus RowStatus
    }

atmSigDescrParamIndex OBJECT-TYPE
    SYNTAX AtmSigDescrParamIndex
--    Rsyntax INTEGER(0..2147483647)
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "The value of this object is used by the
        atmVclExtTable to identify a row in this table."
    ::= { atmSigDescrParamEntry 1 }

atmSigDescrParamAalType OBJECT-TYPE
    SYNTAX INTEGER {
        other(1),
        aal1(2),
        aal34(3),
        aal5(4),
        userDefined(5)
        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "The AAL type. The value of this object is set to
        other(1) when not defined."
    DEFVAL { other }
    ::= { atmSigDescrParamEntry 2 }

atmSigDescrParamAalSscsType OBJECT-TYPE
    SYNTAX INTEGER {
        other(1),
        assured(2),
        nonassured(3),
        frameRelay(4),
        null(5)
        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "The SSCS type used by this entry."
    DEFVAL { other }
    ::= { atmSigDescrParamEntry 3 }

atmSigDescrParamBhliType OBJECT-TYPE
    SYNTAX INTEGER {
        other(1),
        iso(2),
        user(3),
        hiProfile(4),
        vendorSpecific(5)
        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "The Broadband high layer type."
    DEFVAL { other }
    ::= { atmSigDescrParamEntry 4 }

atmSigDescrParamBhliInfo OBJECT-TYPE
    SYNTAX OCTET STRING(SIZE(0..7))
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "The Broadband high layer information.  When
        atmSigDescrParamBhliType is set to iso(2), the
        value of this object is a zero length string.
        When atmSigDescrParamBhliType is set to
        hiProfile(4), the value of this object is a length
        of 4 octet string containing user to user profile
        identifier.  When atmSigDescrParamBhliType is set
        to    vendorSpecific(4), the value of this object
        is a length of 7 octet string.  The most
        significant 3 octets consist of a globally-
        administered OUI, the least significant 4 octets
        are the vender administered application OUI."
    DEFVAL { ''h }
    ::= { atmSigDescrParamEntry 5 }

atmSigDescrParamBbcConnConf OBJECT-TYPE
    SYNTAX INTEGER {
        ptp(1),
        ptmp(2)
        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "The Broadband bearer capability user plane
        connection configuration parameter."
    ::= { atmSigDescrParamEntry 6 }

atmSigDescrParamBlliLayer2 OBJECT-TYPE
    SYNTAX INTEGER {
        other(1),
        iso1745(2),
        q921(3),
        x25linklayer(4),
        x25multilink(5),
        lapb(6),
        hdlcArm(7),
        hdlcNrm(8),
        hdlcAbm(9),
        iso88022(10),
        x75slp(11),
        q922(12),
        userDef(13),
        iso7776(14)
        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "The Broadband low layer information, protocol
        type of layer 2.  The value of this object is
        other(1) if layer 2 protocol is not used."
    DEFVAL { other }
    ::= { atmSigDescrParamEntry 7 }

atmSigDescrParamBlliLayer3 OBJECT-TYPE
    SYNTAX INTEGER {
        other(1),
        x25pkt(2),
        isoiec8208(3),
        x223iso8878(4),
        isoiec8473(5),
        t70(6),
        tr9577(7),
        userDef(8)
        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "The Broadband low layer information, protocol
        type of layer 3.  The value of this object is
        other(1) if layer 3 protocol is not used."
    DEFVAL { other }
    ::= { atmSigDescrParamEntry 8 }

atmSigDescrParamBlliPktSize OBJECT-TYPE
    SYNTAX INTEGER {
        other(1),
        s16(2),
        s32(3),
        s64(4),
        s128(5),
        s256(6),
        s512(7),
        s1024(8),
        s2048(9),
        s4096(10)
        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "The default packet size defined in B-LLI."
    DEFVAL { other }
    ::= { atmSigDescrParamEntry 9 }

atmSigDescrParamBlliSnapId OBJECT-TYPE
    SYNTAX INTEGER {
        other(1),
        true(2),
        false(3)
        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "The SNAP ID used for Broadband low layer protocol
        layer 3.  The value of this object is other(1) if
        atmSigDescrParamBlliLayer3 is set to other(1)."
    DEFVAL { other }
    ::= { atmSigDescrParamEntry 10 }

atmSigDescrParamBlliOuiPid OBJECT-TYPE
    SYNTAX OCTET STRING(SIZE(0..5))
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "The OUI/PID encoding for Broadband low layer
        protocol layer 3.  The value of this object is a
        zero length string if atmSigDescrParamBlliLayer3
        is set to none(1).  When used, it is always 5
        octets with the most significant octet as the OUI
        Octet 1 and the least significant octet as the PID
        Octet 2."
    DEFVAL { ''h }
    ::= { atmSigDescrParamEntry 11 }

atmSigDescrParamRowStatus OBJECT-TYPE
    SYNTAX RowStatus
--    Rsyntax INTEGER {
--        active(1),
--        notInService(2),
--        notReady(3),
--        createAndGo(4),
--        createAndWait(5),
--        destroy(6)
--        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "This object is used to create and delete rows in
        the atmSigDescrParamTable. Writable values are:
        -'createAndWait' which allows manager to create an
        entry first and fill in the parameters later.
        -'active' which allows manager to set the entry to
        be available to users.  -'destroy' which allows
        manager to delete an entry from this table.
        Readable values are: -'createAndWait' which means
        the entry is created but not available to be used.
        -'active' means it is active and ready to be used
        by agent or manager."
    ::= { atmSigDescrParamEntry 12 }

atmIfRegisteredAddrTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AtmIfRegisteredAddrEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "This table contains a list of ATM addresses that can
        be used for calls to and from a given interface by a
        switch or service.  The ATM addresses are either
        registered by the endsystem via ILMI or statically
        configured.  This table does not expose PNNI
        reachability information.  ILMI registered addresses
        cannot be deleted using this table.  This table only
        applies to switches and network services."
    ::= { atm2MIBObjects 6 }

atmIfRegisteredAddrEntry OBJECT-TYPE
    SYNTAX AtmIfRegisteredAddrEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "An entry in the ATM Interface Registered Address
        table."
    INDEX { ifIndex, atmIfRegAddrAddress }
    ::= { atmIfRegisteredAddrTable 1 }

AtmIfRegisteredAddrEntry ::= SEQUENCE {
    atmIfRegAddrAddress AtmAddr,
    atmIfRegAddrAddressSource INTEGER,
    atmIfRegAddrOrgScope INTEGER,
    atmIfRegAddrRowStatus RowStatus
    }

atmIfRegAddrAddress OBJECT-TYPE
    SYNTAX AtmAddr
--    Rsyntax OCTET STRING(SIZE(0 | 8 | 20))
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "An address registered for a given switch or service
        interface."
    ::= { atmIfRegisteredAddrEntry 1 }

atmIfRegAddrAddressSource OBJECT-TYPE
    SYNTAX INTEGER {
        other(1),
        static(2),
        dynamic(3)
        }
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The type of address source for a given ATM Address.
        The value dynamic(3) is indicated when ILMI is used."
    ::= { atmIfRegisteredAddrEntry 2 }

atmIfRegAddrOrgScope OBJECT-TYPE
    SYNTAX INTEGER {
        localNetwork(1),
        localNetworkPlusOne(2),
        localNetworkPlusTwo(3),
        siteMinusOne(4),
        intraSite(5),
        sitePlusOne(6),
        organizationMinusOne(7),
        intraOrganization(8),
        organizationPlusOne(9),
        communityMinusOne(10),
        intraCommunity(11),
        communityPlusOne(12),
        regional(13),
        interRegional(14),
        global(15)
        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "This object indicates the organizational scope for the
        referenced address.  The information of the referenced
        address shall not be distributed outside the indicated
        scope.   Refer to Annex 5.3 of ATM Forum UNI Signalling
        4.0 for guidelines regarding the use of organizational
        scopes.
        
        This value cannot be configured for ILMI-registered
        addresses.
        The default values for organizational scope are
        localNetwork(1) for ATM group addresses, and global(15)
        for individual addresses."
    ::= { atmIfRegisteredAddrEntry 3 }

atmIfRegAddrRowStatus OBJECT-TYPE
    SYNTAX RowStatus
--    Rsyntax INTEGER {
--        active(1),
--        notInService(2),
--        notReady(3),
--        createAndGo(4),
--        createAndWait(5),
--        destroy(6)
--        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "This object is used to create and delete rows in the
        atmIfRegisteredAddrTable.  Rows created dynamically
        (e.g., ILMI-registered addresses) cannot be deleted
        using this object."
    ::= { atmIfRegisteredAddrEntry 4 }

atmVclAddrTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AtmVclAddrEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "This table provides a mapping between the
        atmVclTable and the ATM called party/calling party
        address. This table can be used to retrieve the
        calling party and called party ATM address pair
        for a given Vcl. Note that there can be more than
        one pair of calling party and called party ATM
        addresses for a VCL in a point to multi-point
        call."
    ::= { atm2MIBObjects 7 }

atmVclAddrEntry OBJECT-TYPE
    SYNTAX AtmVclAddrEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "Each entry in this table represents a binding
        between a VCL and an ATM address associated with
        this call. This ATM address can be either the
        called party address or the calling party address.
        There can be more than one pair of calling/called
        party ATM addresses associated with the VCL entry
        for point to multi-point calls. Objects
        atmVclAddrAddr, atmVclAddrType, and
        atmVclAddrRowStatus are required during row
        creation."
    INDEX { ifIndex, atmVclVpi, atmVclVci, atmVclAddrAddr }
    ::= { atmVclAddrTable 1 }

AtmVclAddrEntry ::= SEQUENCE {
    atmVclAddrAddr AtmAddr,
    atmVclAddrType INTEGER,
    atmVclAddrRowStatus RowStatus
    }

atmVclAddrAddr OBJECT-TYPE
    SYNTAX AtmAddr
--    Rsyntax OCTET STRING(SIZE(0 | 8 | 20))
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "An ATM address on one end of the VCL.  For SVCs,
        the agent supplies the value of this object at
        creation time.  For PVCs, manager can supply the
        value of this object during or after the PVC
        creation."
    ::= { atmVclAddrEntry 1 }

atmVclAddrType OBJECT-TYPE
    SYNTAX INTEGER {
        callingParty(1),
        calledParty(2)
        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "The type of ATM Address represented by the object
        atmVclAddrAddr.  Choices are either the calling
        party ATM address or the called party ATM
        address."
    ::= { atmVclAddrEntry 2 }

atmVclAddrRowStatus OBJECT-TYPE
    SYNTAX RowStatus
--    Rsyntax INTEGER {
--        active(1),
--        notInService(2),
--        notReady(3),
--        createAndGo(4),
--        createAndWait(5),
--        destroy(6)
--        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "This object is used to create or destroy an entry
        from this table."
    ::= { atmVclAddrEntry 3 }

atmAddrVclTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AtmAddrVclEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "This table provides an alternative way to
        retrieve the atmVclTable.  This table can be used
        to retrieve the indexing to the atmVclTable by an
        ATM address."
    ::= { atm2MIBObjects 8 }

atmAddrVclEntry OBJECT-TYPE
    SYNTAX AtmAddrVclEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "Each entry in this table represents an entry in
        the atmVclTable of the ATM MIB [1] by it's ATM
        address.  The ATM address is either the calling or
        called party ATM address of the call.  Entries in
        this table are read only.  They show up when
        entries are created in the atmVclAddrTable."
    INDEX { atmVclAddrAddr, atmAddrVclAtmIfIndex, atmAddrVclVpi, atmAddrVclVci }
    ::= { atmAddrVclTable 1 }

AtmAddrVclEntry ::= SEQUENCE {
    atmAddrVclAtmIfIndex InterfaceIndex,
    atmAddrVclVpi AtmVpIdentifier,
    atmAddrVclVci AtmVcIdentifier,
    atmAddrVclAddrType INTEGER
    }

atmAddrVclAtmIfIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
--    Rsyntax Integer32
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "The interface index of the ATM interface where
        this VCL pertains to.  This object combined with
        the atmAddrVclVpi and atmAddrVclVci objects serves
        as an index to the atmVclTable."
    ::= { atmAddrVclEntry 1 }

atmAddrVclVpi OBJECT-TYPE
    SYNTAX AtmVpIdentifier
--    Rsyntax INTEGER(0..4095)
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "The VPI value of the VCL.  This object combined
        with the atmAddrVclAtmIfIndex and atmAddrVclVci
        objects serves as an index to the atmVclTable."
    ::= { atmAddrVclEntry 2 }

atmAddrVclVci OBJECT-TYPE
    SYNTAX AtmVcIdentifier
--    Rsyntax INTEGER(0..65535)
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "The VCI value of the VCL.  This object combined
        with the atmAddrVclAtmIfIndex and atmAddrVclVpi
        objects serves as an index to the atmVclTable."
    ::= { atmAddrVclEntry 3 }

atmAddrVclAddrType OBJECT-TYPE
    SYNTAX INTEGER {
        callingParty(1),
        calledParty(2)
        }
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The type of ATM Address represented by the object
        atmVclAddrAddr.  Choices are either calling party
        address or called party address."
    ::= { atmAddrVclEntry 4 }

atmVplStatTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AtmVplStatEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "This table contains all statistic counters per
        VPL.  It is used to monitor the usage of the VPL
        in terms of incoming cells and outgoing cells."
    ::= { atm2MIBObjects 9 }

atmVplStatEntry OBJECT-TYPE
    SYNTAX AtmVplStatEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "Each entry in this table represents a VPL."
    INDEX { ifIndex, atmVplVpi }
    ::= { atmVplStatTable 1 }

AtmVplStatEntry ::= SEQUENCE {
    atmVplStatTotalCellIns Counter32,
    atmVplStatClp0CellIns Counter32,
    atmVplStatTotalDiscards Counter32,
    atmVplStatClp0Discards Counter32,
    atmVplStatTotalCellOuts Counter32,
    atmVplStatClp0CellOuts Counter32,
    atmVplStatTaggedOuts Counter32
    }

atmVplStatTotalCellIns OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The total number of valid ATM cells received by
        this VPL including both CLP=0 and CLP=1 cells.
        The cells are counted prior to the application of
        the traffic policing."
    ::= { atmVplStatEntry 1 }

atmVplStatClp0CellIns OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The number of valid ATM cells received by this
        VPL with CLP=0.  The cells are counted prior to
        the application of the traffic policing."
    ::= { atmVplStatEntry 2 }

atmVplStatTotalDiscards OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The total number of valid ATM cells discarded by
        the traffic policing entity. This includes cells
        orginally received with CLP=0 and CLP=1."
    ::= { atmVplStatEntry 3 }

atmVplStatClp0Discards OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The total number of valid ATM cells received with
        CLP=0 an  discarded by the traffic policing
        entity."
    ::= { atmVplStatEntry 4 }

atmVplStatTotalCellOuts OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The total number of valid ATM cells transmitted
        by this VPL.  This includes both CLP=0 and CLP=1
        cells."
    ::= { atmVplStatEntry 5 }

atmVplStatClp0CellOuts OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The total number of valid ATM cells transmitted
        with CLP=0 by this VPL."
    ::= { atmVplStatEntry 6 }

atmVplStatTaggedOuts OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The total number of valid ATM cells tagged by the
        traffic policing entity from CLP=0 to CLP=1 and
        transmitted by this VPL."
    ::= { atmVplStatEntry 7 }

atmVplLogicalPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AtmVplLogicalPortEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "Indicates whether the VPL is an ATM Logical Port
        interface (ifType=80)."
    ::= { atm2MIBObjects 10 }

atmVplLogicalPortEntry OBJECT-TYPE
    SYNTAX AtmVplLogicalPortEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "An entry with information about the ATM Logical
        Port interface."
    INDEX { ifIndex, atmVplVpi }
-- Augments atmVplEntry FROM ATM-MIB
    ::= { atmVplLogicalPortTable 1 }

AtmVplLogicalPortEntry ::= SEQUENCE {
    atmVplLogicalPortDef INTEGER,
    atmVplLogicalPortIndex InterfaceIndex
    }

atmVplLogicalPortDef OBJECT-TYPE
    SYNTAX INTEGER {
        notLogicalIf(1),
        isLogicalIf(2)
        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "Indicates whether the VPC at this VPL interface
        is an ATM Logical Port interface."
    DEFVAL { notLogicalIf }
    ::= { atmVplLogicalPortEntry 1 }

atmVplLogicalPortIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
--    Rsyntax Integer32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The ifTable index of the ATM logical port
        interface associated with this VPL. Only valid if
        the value of atmVplLogicalPortDef is isLogicalIf,
        and the VPL row is active."
    ::= { atmVplLogicalPortEntry 2 }

atmVclStatTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AtmVclStatEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "This table contains all statistic counters per
        VCL.  It is used to monitor the usage of the VCL
        in terms of incoming cells and outgoing cells."
    ::= { atm2MIBObjects 11 }

atmVclStatEntry OBJECT-TYPE
    SYNTAX AtmVclStatEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "Each entry in this table represents a VCL."
    INDEX { ifIndex, atmVclVpi, atmVclVci }
    ::= { atmVclStatTable 1 }

AtmVclStatEntry ::= SEQUENCE {
    atmVclStatTotalCellIns Counter32,
    atmVclStatClp0CellIns Counter32,
    atmVclStatTotalDiscards Counter32,
    atmVclStatClp0Discards Counter32,
    atmVclStatTotalCellOuts Counter32,
    atmVclStatClp0CellOuts Counter32,
    atmVclStatTaggedOuts Counter32
    }

atmVclStatTotalCellIns OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The total number of valid ATM cells received by
        this VCL including both CLP=0 and CLP=1 cells.
        The cells are counted prior to the application of
        the traffic policing."
    ::= { atmVclStatEntry 1 }

atmVclStatClp0CellIns OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The number of valid ATM cells received by this
        VCL with CLP=0.  The cells are counted prior to
        the application of the traffic policing."
    ::= { atmVclStatEntry 2 }

atmVclStatTotalDiscards OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The total number of valid ATM cells discarded by
        the traffic policing entity. This includes cells
        orginally received with CLP=0 and CLP=1."
    ::= { atmVclStatEntry 3 }

atmVclStatClp0Discards OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The total number of valid ATM cells received with
        CLP=0 an  discarded by the traffic policing
        entity."
    ::= { atmVclStatEntry 4 }

atmVclStatTotalCellOuts OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The total number of valid ATM cells transmitted
        by this VCL.  This includes both CLP=0 and CLP=1
        cells."
    ::= { atmVclStatEntry 5 }

atmVclStatClp0CellOuts OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The total number of valid ATM cells transmitted
        with CLP=0 by this VCL."
    ::= { atmVclStatEntry 6 }

atmVclStatTaggedOuts OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The total number of valid ATM cells tagged by the
        traffic policing entity from CLP=0 to CLP=1 and
        transmitted by this VCL."
    ::= { atmVclStatEntry 7 }

atmAal5VclStatTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AtmAal5VclStatEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "This table provides a collection of objects
        providing AAL5 configuration and performance
        statistics of a VCL."
    ::= { atm2MIBObjects 12 }

atmAal5VclStatEntry OBJECT-TYPE
    SYNTAX AtmAal5VclStatEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "Each entry in this table represents a VCL."
    INDEX { ifIndex, atmVclVpi, atmVclVci }
    ::= { atmAal5VclStatTable 1 }

AtmAal5VclStatEntry ::= SEQUENCE {
    atmAal5VclInPkts Counter32,
    atmAal5VclOutPkts Counter32,
    atmAal5VclInOctets Counter32,
    atmAal5VclOutOctets Counter32
    }

atmAal5VclInPkts OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The number of AAL5 CPCS PDUs received on the AAL5
        VCC at the interface identified by the ifIndex."
    ::= { atmAal5VclStatEntry 1 }

atmAal5VclOutPkts OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The number of AAL5 CPCS PDUs transmitted on the
        AAL5 VCC at the interface identified by the
        ifIndex."
    ::= { atmAal5VclStatEntry 2 }

atmAal5VclInOctets OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The number of octets contained in AAL5 CPCS PDUs
        received on the AAL5 VCC at the interface
        identified by the ifIndex."
    ::= { atmAal5VclStatEntry 3 }

atmAal5VclOutOctets OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The number of octets contained in AAL5 CPCS PDUs
        transmitted on the AAL5 VCC at the interface
        identified by the ifIndex."
    ::= { atmAal5VclStatEntry 4 }

atmVclGenTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AtmVclGenEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "General Information for each VC."
    ::= { atm2MIBObjects 13 }

atmVclGenEntry OBJECT-TYPE
    SYNTAX AtmVclGenEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "An entry with general information
        about the ATM VC."
    INDEX { ifIndex, atmVclVpi, atmVclVci }
-- Augments atmVclEntry FROM ATM-MIB
    ::= { atmVclGenTable 1 }

AtmVclGenEntry ::= SEQUENCE {
    atmVclGenSigDescrIndex AtmSigDescrParamIndex
    }

atmVclGenSigDescrIndex OBJECT-TYPE
    SYNTAX AtmSigDescrParamIndex
--    Rsyntax INTEGER(0..2147483647)
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "The value of this object identifies the
        row in the ATM Signalling Descriptor
        Parameter Table which applies to this
        VCL."
    ::= { atmVclGenEntry 1 }

atmInterfaceExtTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AtmInterfaceExtEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "This table contains ATM interface
        configuration and monitoring information not
        defined in the atmInterfaceConfTable from the
        ATM-MIB [1].  This includes the type of
        connection setup procedures, ILMI information,
        and information on the VPI/VCI range."
    ::= { atm2MIBObjects 14 }

atmInterfaceExtEntry OBJECT-TYPE
    SYNTAX AtmInterfaceExtEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "An entry extends the
        atmInterfaceConfEntry defined in [1].  Each
        entry corresponds to an ATM
        interface."
    INDEX { ifIndex }
-- Augments atmInterfaceConfEntry FROM ATM-MIB
    ::= { atmInterfaceExtTable 1 }

AtmInterfaceExtEntry ::= SEQUENCE {
    atmIntfConfigType AtmInterfaceType,
    atmIntfActualType AtmInterfaceType,
    atmIntfConfigSide INTEGER,
    atmIntfActualSide INTEGER,
    atmIntfIlmiFsmState INTEGER,
    atmIntfIlmiEstablishConPollIntvl Integer32,
    atmIntfIlmiCheckConPollIntvl Integer32,
    atmIntfIlmiConPollInactFactor Integer32,
    atmIntfIlmiPublicPrivateIndctr INTEGER,
    atmInterfaceConfMaxSvpcVpi INTEGER,
    atmInterfaceCurrentMaxSvpcVpi INTEGER,
    atmInterfaceConfMaxSvccVpi INTEGER,
    atmInterfaceCurrentMaxSvccVpi INTEGER,
    atmInterfaceConfMinSvccVci INTEGER,
    atmInterfaceCurrentMinSvccVci INTEGER,
    atmIntfSigVccRxTrafficDescrIndex AtmTrafficDescrParamIndex,
    atmIntfSigVccTxTrafficDescrIndex AtmTrafficDescrParamIndex,
    atmIntfPvcFailures Counter32,
    atmIntfCurrentlyFailingPVpls Gauge32,
    atmIntfCurrentlyFailingPVcls Gauge32,
    atmIntfPvcFailuresTrapEnable TruthValue,
    atmIntfPvcNotificationInterval INTEGER
    }

atmIntfConfigType OBJECT-TYPE
    SYNTAX AtmInterfaceType
--    Rsyntax INTEGER {
--        other(1),
--        autoConfig(2),
--        ituDss2(3),
--        atmfUni3Dot0(4),
--        atmfUni3Dot1(5),
--        atmfUni4Dot0(6),
--        atmfIispUni3Dot0(7),
--        atmfIispUni3Dot1(8),
--        atmfIispUni4Dot0(9),
--        atmfPnni1Dot0(10),
--        atmfBici2Dot0(11),
--        atmfUniPvcOnly(12),
--        atmfNniPvcOnly(13)
--        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "The type of connection setup procedures
        configured for the ATM interface.  Setting this
        variable to a value of 'other' is not allowed."
    DEFVAL { autoConfig }
    ::= { atmInterfaceExtEntry 1 }

atmIntfActualType OBJECT-TYPE
    SYNTAX AtmInterfaceType
--    Rsyntax INTEGER {
--        other(1),
--        autoConfig(2),
--        ituDss2(3),
--        atmfUni3Dot0(4),
--        atmfUni3Dot1(5),
--        atmfUni4Dot0(6),
--        atmfIispUni3Dot0(7),
--        atmfIispUni3Dot1(8),
--        atmfIispUni4Dot0(9),
--        atmfPnni1Dot0(10),
--        atmfBici2Dot0(11),
--        atmfUniPvcOnly(12),
--        atmfNniPvcOnly(13)
--        }
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The type of connection setup procedures
        currently being used on the interface.  This may
        reflect a manually configured value for the
        interface type, or may be determined by other
        means such as auto-configuration.  A value of
        `autoConfig' indicates that auto-configuration
        was requested but has not yet been completed."
    ::= { atmInterfaceExtEntry 2 }

atmIntfConfigSide OBJECT-TYPE
    SYNTAX INTEGER {
        other(1),
        user(2),
        network(3)
        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "The configured role of the managed entity as one
        side of the ATM interface.  This value does not
        apply when the object atmIntfConfigType is set to
        `autoConfig', `atmfPnni1Dot0', or
        `atmfBici2Dot0'."
    ::= { atmInterfaceExtEntry 3 }

atmIntfActualSide OBJECT-TYPE
    SYNTAX INTEGER {
        other(1),
        user(2),
        network(3),
        symmetric(4)
        }
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The current role used by the managed entity to
        represent one side of the ATM interface."
    ::= { atmInterfaceExtEntry 4 }

atmIntfIlmiFsmState OBJECT-TYPE
    SYNTAX INTEGER {
        stopped(1),
        linkFailing(2),
        establishing(3),
        configuring(4),
        retrievingNetworkPrefixes(5),
        registeringNetworkPrefixes(6),
        retrievingAddresses(7),
        registeringAddresses(8),
        verifying(9)
        }
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "Indicates the state of the ILMI Finite State Machine
        associated with this interface."
    REFERENCE
        "ATM Forum ILMI 4.0 Specification, Appendix 1"
    ::= { atmInterfaceExtEntry 7 }

atmIntfIlmiEstablishConPollIntvl OBJECT-TYPE
    SYNTAX Integer32
--  SYNTAX Integer32(1..65535)
--  Units
--    seconds
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "The amount of time S between successive transmissions
        of ILMI messages on this interface for the purpose of
        detecting establishment of ILMI connectivity."
    REFERENCE
        "ATM Forum ILMI 4.0 Section 8.3.1"
    DEFVAL { 1 }
    ::= { atmInterfaceExtEntry 8 }

atmIntfIlmiCheckConPollIntvl OBJECT-TYPE
    SYNTAX Integer32
--  SYNTAX Integer32(0..65535)
--  Units
--    seconds
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "The amount of time T between successive transmissions
        of ILMI messages on this interface for the purpose of
        detecting loss of ILMI connectivity.  The distinguished
        value zero disables ILMI connectivity procedures on
        this interface."
    REFERENCE
        "ATM Forum ILMI 4.0 Section 8.3.1"
    DEFVAL { 5 }
    ::= { atmInterfaceExtEntry 9 }

atmIntfIlmiConPollInactFactor OBJECT-TYPE
    SYNTAX Integer32
--  SYNTAX Integer32(0..65535)
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "The number K of consecutive polls on this interface
        for which no ILMI response message is received before
        ILMI connectivity is declared lost."
    REFERENCE
        "ATM Forum ILMI 4.0 Section 8.3.1"
    DEFVAL { 4 }
    ::= { atmInterfaceExtEntry 10 }

atmIntfIlmiPublicPrivateIndctr OBJECT-TYPE
    SYNTAX INTEGER {
        other(1),
        public(2),
        private(3)
        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "Specifies whether this end of the interface is
        advertised in ILMI as a device of the `public' or
        `private' type."
    DEFVAL { private }
    ::= { atmInterfaceExtEntry 11 }

atmInterfaceConfMaxSvpcVpi OBJECT-TYPE
    SYNTAX INTEGER(0..4095)
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "The maximum VPI that the signalling stack on the ATM
        interface is configured to support for allocation to
        switched virtual path connections."
    ::= { atmInterfaceExtEntry 12 }

atmInterfaceCurrentMaxSvpcVpi OBJECT-TYPE
    SYNTAX INTEGER(0..4095)
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The maximum VPI that the signalling stack on the ATM
        interface may currently allocate to switched virtual
        path connections.  This value is the minimum of
        atmInterfaceConfMaxSvpcVpi, and the
        atmInterfaceMaxSvpcVpi of the interface's UNI/NNI peer.
        
        If the interface does not negotiate with its peer to
        determine the maximum VPI that can be allocated to
        SVPCs on the interface, then the value of this object
        must equal atmInterfaceConfMaxSvpcVpi. "
    ::= { atmInterfaceExtEntry 13 }

atmInterfaceConfMaxSvccVpi OBJECT-TYPE
    SYNTAX INTEGER(0..4095)
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "The maximum VPI that the signalling stack on the ATM
        interface is configured to support for allocation to
        switched virtual channel connections."
    ::= { atmInterfaceExtEntry 14 }

atmInterfaceCurrentMaxSvccVpi OBJECT-TYPE
    SYNTAX INTEGER(0..4095)
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The maximum VPI that the signalling stack on the ATM
        interface may currently allocate to switched virtual
        channel connections.  This value is the minimum of
        atmInterfaceConfMaxSvccVpi, and the
        atmInterfaceConfMaxSvccVpi of the interface's UNI/NNI
        peer.
        
        If the interface does not negotiate with its peer to
        determine the maximum VPI that can be allocated to
        SVCCs on the interface, then the value of this object
        must equal atmInterfaceConfMaxSvccVpi."
    ::= { atmInterfaceExtEntry 15 }

atmInterfaceConfMinSvccVci OBJECT-TYPE
    SYNTAX INTEGER(0..65535)
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "The minimum VCI that the signalling stack on the ATM
        interface is configured to support for allocation to
        switched virtual channel connections."
    ::= { atmInterfaceExtEntry 16 }

atmInterfaceCurrentMinSvccVci OBJECT-TYPE
    SYNTAX INTEGER(0..65535)
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The minimum VCI that the signalling stack on the ATM
        interface may currently allocate to switched virtual
        channel connections.  This value is the maximum of
        atmInterfaceConfMinSvccVci, and the
        atmInterfaceConfMinSvccVci of the interface's UNI/NNI
        peer.
        
        If the interface does not negotiate with its peer to
        determine the minimum VCI that can be allocated to
        SVCCs on the interface, then the value of this object
        must equal atmInterfaceConfMinSvccVci."
    ::= { atmInterfaceExtEntry 17 }

atmIntfSigVccRxTrafficDescrIndex OBJECT-TYPE
    SYNTAX AtmTrafficDescrParamIndex
--    Rsyntax INTEGER(0..2147483647)
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "This object identifies the row in the
        atmTrafficDescrParamTable used during ILMI
        auto-configuration to specify the advertised
        signalling VCC traffic parameters for the
        receive direction.
        
        The traffic descriptor resulting from ILMI auto-
        configuration of the signalling VCC is indicated
        in the atmVclTable."
    ::= { atmInterfaceExtEntry 18 }

atmIntfSigVccTxTrafficDescrIndex OBJECT-TYPE
    SYNTAX AtmTrafficDescrParamIndex
--    Rsyntax INTEGER(0..2147483647)
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "This object identifies the row in the
        atmTrafficDescrParamTable used during ILMI
        auto-configuration to specify the advertised
        signalling VCC traffic parameters for the
        transmit direction.
        
        The traffic descriptor resulting from ILMI auto-
        configuration of the signalling VCC is indicated
        in the atmVclTable."
    ::= { atmInterfaceExtEntry 19 }

atmIntfPvcFailures OBJECT-TYPE
    SYNTAX Counter32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The number of times the operational status of a PVPL
        or PVCL on this interface has gone down."
    ::= { atmInterfaceExtEntry 20 }

atmIntfCurrentlyFailingPVpls OBJECT-TYPE
    SYNTAX Gauge32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The current number of VPLs on this interface for which
        there is an active row in the atmVplTable having an
        atmVplConnKind value of `pvc' and an atmVplOperStatus
        with a value other than `up'."
    ::= { atmInterfaceExtEntry 21 }

atmIntfCurrentlyFailingPVcls OBJECT-TYPE
    SYNTAX Gauge32
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The current number of VCLs on this interface for which
        there is an active row in the atmVclTable having an
        atmVclConnKind value of `pvc' and an atmVclOperStatus
        with a value other than `up'."
    ::= { atmInterfaceExtEntry 22 }

atmIntfPvcFailuresTrapEnable OBJECT-TYPE
    SYNTAX TruthValue
--    Rsyntax INTEGER {
--        true(1),
--        false(2)
--        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "Allows the generation of traps in response to PVCL or
        PVPL failures on this interface."
    DEFVAL { false }
    ::= { atmInterfaceExtEntry 23 }

atmIntfPvcNotificationInterval OBJECT-TYPE
    SYNTAX INTEGER(1..3600)
--  Units
--    seconds
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "The minimum interval between the sending of
        atmIntfPvcFailuresTrap notifications for this
        interface."
    DEFVAL { 30 }
    ::= { atmInterfaceExtEntry 24 }

atmIlmiSrvcRegTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AtmIlmiSrvcRegEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "This table contains a list of all the ATM network
        services known by this device.
        
        The characteristics of these services are made
        available through the ILMI, using the ILMI general-
        purpose service registry MIB.
        
        These services may be made available to all ATM
        interfaces (atmIlmiSrvcRegIndex = 0) or to some
        specific ATM interfaces only (atmIlmiSrvcRegIndex = ATM
        interface index)."
    ::= { atm2MIBObjects 15 }

atmIlmiSrvcRegEntry OBJECT-TYPE
    SYNTAX AtmIlmiSrvcRegEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "Information about a single service provider that is
        available to the user-side of an adjacent device
        through the ILMI."
    INDEX { atmIlmiSrvcRegIndex, atmIlmiSrvcRegServiceID, atmIlmiSrvcRegAddressIndex }
    ::= { atmIlmiSrvcRegTable 1 }

AtmIlmiSrvcRegEntry ::= SEQUENCE {
    atmIlmiSrvcRegIndex InterfaceIndex,
    atmIlmiSrvcRegServiceID OBJECT IDENTIFIER,
    atmIlmiSrvcRegAddressIndex INTEGER,
    atmIlmiSrvcRegATMAddress AtmAddr,
    atmIlmiSrvcRegParm1 OCTET STRING,
    atmIlmiSrvcRegRowStatus RowStatus
    }

atmIlmiSrvcRegIndex OBJECT-TYPE
    SYNTAX InterfaceIndex
--    Rsyntax Integer32
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "The ATM interface where the service defined in this
        entry can be made available to an ATM device attached
        to this interface.
        
        The value of 0 has a special meaning: when an ATM
        service is defined in an entry whose
        atmIlmiSrvcRegIndex is zero, the ATM service is
        available to ATM devices connected to any ATM
        interface.  (default value(s)).
        
        When the user-side of an adjacent device queries the
        content of the ILMI service registry MIB (using the
        ILMI protocol), the local network-side responds with
        the ATM services defined in atmIlmiSrvcRegTable
        entries, provided that these entries are indexed by:
                    - the corresponding interface number (atmIlmiSrvcRegIndex equal
                      to the number of the interface that the adjacent device is
                      connected to)
                    - zero (atmIlmiSrvcRegIndex=0)."
    ::= { atmIlmiSrvcRegEntry 1 }

atmIlmiSrvcRegServiceID OBJECT-TYPE
    SYNTAX OBJECT IDENTIFIER
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "This is the service identifier which uniquely
        identifies the type of service at the address provided
        in the table.  The object identifiers for the LAN
        Emulation Configuration Server (LECS) and the ATM Name
        Server (ANS) are defined in the ATM Forum ILMI Service
        Registry MIB."
    ::= { atmIlmiSrvcRegEntry 2 }

atmIlmiSrvcRegAddressIndex OBJECT-TYPE
    SYNTAX INTEGER(1..2147483647)
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "An arbitrary integer to differentiate multiple rows
        containing different ATM addresses for the same service
        on the same interface.  This number needs NOT to be the
        same as the corresponding ILMI atmfSrvcRegAddressIndex
        MIB object."
    ::= { atmIlmiSrvcRegEntry 3 }

atmIlmiSrvcRegATMAddress OBJECT-TYPE
    SYNTAX AtmAddr
--    Rsyntax OCTET STRING(SIZE(0 | 8 | 20))
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "This is the full address of the service. The user-side of the
        adjacent device may use this address to establish a connection
        with the service."
    ::= { atmIlmiSrvcRegEntry 4 }

atmIlmiSrvcRegParm1 OBJECT-TYPE
    SYNTAX OCTET STRING(SIZE(1..255))
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "An octet string used according to the value of
        atmIlmiSrvcRegServiceID."
    ::= { atmIlmiSrvcRegEntry 5 }

atmIlmiSrvcRegRowStatus OBJECT-TYPE
    SYNTAX RowStatus
--    Rsyntax INTEGER {
--        active(1),
--        notInService(2),
--        notReady(3),
--        createAndGo(4),
--        createAndWait(5),
--        destroy(6)
--        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "This object is used to create or destroy an entry from
        this table."
    ::= { atmIlmiSrvcRegEntry 6 }

atmIlmiNetworkPrefixTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AtmIlmiNetworkPrefixEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "A table specifying per interface network prefix(es)
        supplied by the network side of the UNI during ILMI
        address registration.  When no network prefixes are
        specified for a particular interface, one or more
        network prefixes based on the switch address(es) may be
        used for ILMI address registration."
    ::= { atm2MIBObjects 16 }

atmIlmiNetworkPrefixEntry OBJECT-TYPE
    SYNTAX AtmIlmiNetworkPrefixEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "Information about a single network prefix supplied by
        the network side of the UNI during ILMI address
        registration.  Note that the index variable
        atmIlmiNetPrefixPrefix is a variable-length string, and
        as such the rule for variable-length strings in section
        7.7 of RFC 1902 applies."
    INDEX { ifIndex, atmIlmiNetPrefixPrefix }
    ::= { atmIlmiNetworkPrefixTable 1 }

AtmIlmiNetworkPrefixEntry ::= SEQUENCE {
    atmIlmiNetPrefixPrefix AtmIlmiNetworkPrefix,
    atmIlmiNetPrefixRowStatus RowStatus
    }

atmIlmiNetPrefixPrefix OBJECT-TYPE
    SYNTAX AtmIlmiNetworkPrefix
--    Rsyntax OCTET STRING(SIZE(8 | 13))
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "The network prefix specified for use in ILMI address
        registration."
    ::= { atmIlmiNetworkPrefixEntry 1 }

atmIlmiNetPrefixRowStatus OBJECT-TYPE
    SYNTAX RowStatus
--    Rsyntax INTEGER {
--        active(1),
--        notInService(2),
--        notReady(3),
--        createAndGo(4),
--        createAndWait(5),
--        destroy(6)
--        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "Used to create, delete, activate and de-activate
        network prefixes used in ILMI address registration."
    ::= { atmIlmiNetworkPrefixEntry 2 }

atmSwitchAddressTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AtmSwitchAddressEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "This table contains one or more ATM endsystem
        addresses on a per switch basis.  These addresses are
        used to identify the switch.  When no ILMI network
        prefixes are configured for certain interfaces, network
        prefixes based on the switch address(es) may be used
        for ILMI address registration."
    ::= { atm2MIBObjects 17 }

atmSwitchAddressEntry OBJECT-TYPE
    SYNTAX AtmSwitchAddressEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "An entry in the ATM Switch Address table."
    INDEX { atmSwitchAddressIndex }
    ::= { atmSwitchAddressTable 1 }

AtmSwitchAddressEntry ::= SEQUENCE {
    atmSwitchAddressIndex Integer32,
    atmSwitchAddressAddress OCTET STRING,
    atmSwitchAddressRowStatus RowStatus
    }

atmSwitchAddressIndex OBJECT-TYPE
    SYNTAX Integer32
--  SYNTAX Integer32(1..65535)
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "An arbitrary index used to enumerate the ATM endsystem
        addresses for this switch."
    ::= { atmSwitchAddressEntry 1 }

atmSwitchAddressAddress OBJECT-TYPE
    SYNTAX OCTET STRING(SIZE(13 .. 20))
--  SYNTAX OCTET STRING(SIZE(13 | 20))
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "An ATM endsystem address or address prefix used to
        identify this switch.  When no ESI or SEL field is
        specified, the switch may generate the ESI and SEL
        fields automatically to obtain a complete 20-byte ATM
        endsystem address."
    ::= { atmSwitchAddressEntry 2 }

atmSwitchAddressRowStatus OBJECT-TYPE
    SYNTAX RowStatus
--    Rsyntax INTEGER {
--        active(1),
--        notInService(2),
--        notReady(3),
--        createAndGo(4),
--        createAndWait(5),
--        destroy(6)
--        }
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "Used to create, delete, activate, and de-
        activate
        addresses used to identify this switch."
    ::= { atmSwitchAddressEntry 3 }

atmVpCrossConnectXTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AtmVpCrossConnectXEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "This table contains one row per VP Cross Connect
        represented in the atmVpCrossConnectTable."
    ::= { atm2MIBObjects 18 }

atmVpCrossConnectXEntry OBJECT-TYPE
    SYNTAX AtmVpCrossConnectXEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "Information about a particular ATM VP Cross Connect.
        
        Each entry provides an two objects that name the Cross
        Connect.  One is assigned by the Service User and the
        other by the Service Provider."
    INDEX { atmVpCrossConnectIndex, atmVpCrossConnectLowIfIndex, atmVpCrossConnectLowVpi, atmVpCrossConnectHighIfIndex, atmVpCrossConnectHighVpi }
-- Augments atmVpCrossConnectEntry FROM ATM-MIB
    ::= { atmVpCrossConnectXTable 1 }

AtmVpCrossConnectXEntry ::= SEQUENCE {
    atmVpCrossConnectUserName DisplayString,
    atmVpCrossConnectProviderName DisplayString 
    }

atmVpCrossConnectUserName OBJECT-TYPE
    SYNTAX DisplayString
--  Rsyntax OCTET STRING(0..255)
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "This is a service user assigned textual representation
        of a VPC PVC."
    ::= { atmVpCrossConnectXEntry 1 }

atmVpCrossConnectProviderName OBJECT-TYPE
    SYNTAX DisplayString
--  Rsyntax OCTET STRING(0..255)
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "This is a system supplied textual representation of
        VPC PVC.  It is assigned by the service provider."
    ::= { atmVpCrossConnectXEntry 2 }

atmVcCrossConnectXTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AtmVcCrossConnectXEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "This table contains one row per VC Cross Connect
        represented in the atmVcCrossConnectTable."
    ::= { atm2MIBObjects 19 }

atmVcCrossConnectXEntry OBJECT-TYPE
    SYNTAX AtmVcCrossConnectXEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "Information about a particular ATM VC Cross Connect.
        
        Each entry provides an two objects that name the Cross
        Connect.  One is assigned by the Service User and the
        other by the Service Provider."
    INDEX { atmVcCrossConnectIndex, atmVcCrossConnectLowIfIndex, atmVcCrossConnectLowVpi, atmVcCrossConnectLowVci, atmVcCrossConnectHighIfIndex, atmVcCrossConnectHighVpi, atmVcCrossConnectHighVci }
-- Augments atmVcCrossConnectEntry FROM ATM-MIB
    ::= { atmVcCrossConnectXTable 1 }

AtmVcCrossConnectXEntry ::= SEQUENCE {
    atmVcCrossConnectUserName DisplayString,
    atmVcCrossConnectProviderName DisplayString
    }

atmVcCrossConnectUserName OBJECT-TYPE
    SYNTAX DisplayString
--  Rsyntax OCTET STRING(0..255) 
    ACCESS read-write
    STATUS mandatory
    DESCRIPTION
        "This is a service user assigned textual representation
        of a VCC PVC."
    ::= { atmVcCrossConnectXEntry 1 }

atmVcCrossConnectProviderName OBJECT-TYPE
    SYNTAX DisplayString
--  Rsyntax OCTET STRING(0..255)
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "This is a system supplied textual representation of
        VCC PVC.  It is assigned by the service provider."
    ::= { atmVcCrossConnectXEntry 2 }

atmCurrentlyFailingPVplTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AtmCurrentlyFailingPVplEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "A table indicating all VPLs for which there is an
        active row in the atmVplTable having an atmVplConnKind
        value of `pvc' and an atmVplOperStatus with a value
        other than `up'."
    ::= { atm2MIBObjects 20 }

atmCurrentlyFailingPVplEntry OBJECT-TYPE
    SYNTAX AtmCurrentlyFailingPVplEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "Each entry in this table represents a VPL for which
        the atmVplRowStatus is `active', the atmVplConnKind is
        `pvc', and the atmVplOperStatus is other than `up'."
    INDEX { ifIndex, atmVplVpi }
    ::= { atmCurrentlyFailingPVplTable 1 }

AtmCurrentlyFailingPVplEntry ::= SEQUENCE {
    atmCurrentlyFailingPVplTimeStamp TimeStamp
    }

atmCurrentlyFailingPVplTimeStamp OBJECT-TYPE
    SYNTAX TimeStamp
--    Rsyntax TimeTicks
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The time at which this PVPL began to fail."
    ::= { atmCurrentlyFailingPVplEntry 1 }

atmCurrentlyFailingPVclTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AtmCurrentlyFailingPVclEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "A table indicating all VCLs for which there is an
        active row in the atmVclTable having an atmVclConnKind
        value of `pvc' and an atmVclOperStatus with a value
        other than `up'."
    ::= { atm2MIBObjects 21 }

atmCurrentlyFailingPVclEntry OBJECT-TYPE
    SYNTAX AtmCurrentlyFailingPVclEntry
    ACCESS not-accessible
    STATUS mandatory
    DESCRIPTION
        "Each entry in this table represents a VCL for which
        the atmVclRowStatus is `active', the atmVclConnKind is
        `pvc', and the atmVclOperStatus is other than `up'."
    INDEX { ifIndex, atmVclVpi, atmVclVci }
    ::= { atmCurrentlyFailingPVclTable 1 }

AtmCurrentlyFailingPVclEntry ::= SEQUENCE {
    atmCurrentlyFailingPVclTimeStamp TimeStamp
    }

atmCurrentlyFailingPVclTimeStamp OBJECT-TYPE
    SYNTAX TimeStamp
--    Rsyntax TimeTicks
    ACCESS read-only
    STATUS mandatory
    DESCRIPTION
        "The time at which this PVCL began to fail."
    ::= { atmCurrentlyFailingPVclEntry 1 }

atmIntfPvcFailuresTrap TRAP-TYPE
-- Reverse mappable trap
    ENTERPRISE atmPvcTraps
    VARIABLES {
        ifIndex, atmIntfPvcFailures, atmIntfCurrentlyFailingPVpls, 
        atmIntfCurrentlyFailingPVcls }
--  Status
--    mandatory
    DESCRIPTION
        "A notification indicating that one or more PVPLs or
        PVCLs on this interface has failed since the last
        atmPvcFailuresTrap was sent.  If this trap has not been
        sent for the last atmIntfPvcNotificationInterval, then
        it will be sent on the next increment of
        atmIntfPvcFailures."
    ::= 1

atmSwitchServcHostGroup OBJECT IDENTIFIER ::= { atm2MIBGroups 1 }
-- OBJECT-GROUP
--  Status
--    mandatory
--  Descr
--    A collection of objects providing information
--     for a Switch/Service/Host that implements
--     ATM interfaces.
--  objects
--    atmSigSSCOPConEvents, atmSigSSCOPErrdPdus, 
--    atmSigDetectSetupAttempts, atmSigEmitSetupAttempts, 
--    atmSigDetectUnavailRoutes, atmSigEmitUnavailRoutes, 
--    atmSigDetectUnavailResrcs, atmSigEmitUnavailResrcs, 
--    atmSigDetectCldPtyEvents, atmSigEmitCldPtyEvents, 
--    atmSigDetectMsgErrors, atmSigEmitMsgErrors, 
--    atmSigDetectClgPtyEvents, atmSigEmitClgPtyEvents, 
--    atmSigDetectTimerExpireds, atmSigEmitTimerExpireds, 
--    atmSigDetectRestarts, atmSigEmitRestarts, atmSigInEstabls, 
--    atmSigOutEstabls, atmVclStatTotalCellIns, 
--    atmVclStatClp0CellIns, atmVclStatTotalDiscards, 
--    atmVclStatClp0Discards, atmVclStatTotalCellOuts, 
--    atmVclStatClp0CellOuts, atmVclStatTaggedOuts, 
--    atmVplStatTotalCellIns, atmVplStatClp0CellIns, 
--    atmVplStatTotalDiscards, atmVplStatClp0Discards, 
--    atmVplStatTotalCellOuts, atmVplStatClp0CellOuts, 
--    atmVplStatTaggedOuts, atmVplLogicalPortDef, 
--    atmVplLogicalPortIndex, atmInterfaceConfMaxSvpcVpi, 
--    atmInterfaceCurrentMaxSvpcVpi, atmInterfaceConfMaxSvccVpi, 
--    atmInterfaceCurrentMaxSvccVpi, atmInterfaceConfMinSvccVci, 
--    atmInterfaceCurrentMinSvccVci, 
--    atmIntfSigVccRxTrafficDescrIndex, 
--    atmIntfSigVccTxTrafficDescrIndex, atmIntfPvcFailures, 
--    atmIntfCurrentlyFailingPVpls, atmIntfCurrentlyFailingPVcls, 
--    atmIntfPvcNotificationInterval, atmIntfPvcFailuresTrapEnable, 
--    atmIntfConfigType, atmIntfActualType, atmIntfConfigSide, 
--    atmIntfActualSide, atmIntfIlmiFsmState, 
--    atmIntfIlmiEstablishConPollIntvl, 
--    atmIntfIlmiCheckConPollIntvl, atmIntfIlmiConPollInactFactor, 
--    atmIntfIlmiPublicPrivateIndctr

atmSwitchServcGroup OBJECT IDENTIFIER ::= { atm2MIBGroups 2 }
-- OBJECT-GROUP
--  Status
--    mandatory
--  Descr
--    A collection of objects providing information
--     for a Switch/Service that implements ATM interfaces.
--  objects
--    atmIlmiSrvcRegATMAddress, atmIlmiSrvcRegParm1, 
--    atmIlmiSrvcRegRowStatus, atmIlmiNetPrefixRowStatus, 
--    atmSigSupportClgPtyNumDel, atmSigSupportClgPtySubAddr, 
--    atmSigSupportCldPtySubAddr, atmSigSupportHiLyrInfo, 
--    atmSigSupportLoLyrInfo, atmSigSupportBlliRepeatInd, 
--    atmSigSupportAALInfo, atmSigSupportPrefCarrier, 
--    atmSvcVpCrossConnectCreationTime, 
--    atmSvcVpCrossConnectRowStatus, 
--    atmSvcVcCrossConnectCreationTime, 
--    atmSvcVcCrossConnectRowStatus, atmIfRegAddrAddressSource, 
--    atmIfRegAddrOrgScope, atmIfRegAddrRowStatus

atmServcGroup OBJECT IDENTIFIER ::= { atm2MIBGroups 4 }
-- OBJECT-GROUP
--  Status
--    mandatory
--  Descr
--    A collection of objects providing information
--     for an ATM Network Service.
--  objects
--    atmVpCrossConnectUserName, atmVpCrossConnectProviderName, 
--    atmVcCrossConnectUserName, atmVcCrossConnectProviderName

atmHostGroup OBJECT IDENTIFIER ::= { atm2MIBGroups 5 }
-- OBJECT-GROUP
--  Status
--    mandatory
--  Descr
--    A collection of objects providing information
--     for a Host that implements ATM interfaces.
--  objects
--    atmAal5VclInPkts, atmAal5VclOutPkts, atmAal5VclInOctets, 
--    atmAal5VclOutOctets, atmVclAddrType, atmVclAddrRowStatus, 
--    atmAddrVclAddrType, atmVclGenSigDescrIndex, 
--    atmSigDescrParamAalType, atmSigDescrParamAalSscsType, 
--    atmSigDescrParamBhliType, atmSigDescrParamBhliInfo, 
--    atmSigDescrParamBbcConnConf, atmSigDescrParamBlliLayer2, 
--    atmSigDescrParamBlliLayer3, atmSigDescrParamBlliPktSize, 
--    atmSigDescrParamBlliSnapId, atmSigDescrParamBlliOuiPid, 
--    atmSigDescrParamRowStatus

atm2MIBCompliance OBJECT IDENTIFIER ::= { atm2MIBCompliances 1 }
-- MODULE-COMPLIANCE
--  Status
--    mandatory
--  Descr
--    The compliance statement for SNMP entities which
--    represent ATM interfaces.  The compliance statements
--    are used to determine if a particular group or object
--    applies to hosts, networks/switches, or both.
--  Module
--    >>current<<
--   MandGroup
--    atmSwitchServcHostGroup
--   ObjVar
--    atmVclStatTotalCellIns
--   ObjVar
--    atmVclStatClp0CellIns
--   ObjVar
--    atmVclStatTotalDiscards
--   ObjVar
--    atmVclStatClp0Discards
--   ObjVar
--    atmVclStatTotalCellOuts
--   ObjVar
--    atmVclStatClp0CellOuts
--   ObjVar
--    atmVclStatTaggedOuts
--   ObjVar
--    atmVplStatTotalCellIns
--   ObjVar
--    atmVplStatClp0CellIns
--   ObjVar
--    atmVplStatTotalDiscards
--   ObjVar
--    atmVplStatClp0Discards
--   ObjVar
--    atmVplStatTotalCellOuts
--   ObjVar
--    atmVplStatClp0CellOuts
--   ObjVar
--    atmVplStatTaggedOuts
--   ObjVar
--    atmVplLogicalPortDef
--   ObjVar
--    atmIntfSigVccRxTrafficDescrIndex
--   ObjVar
--    atmIntfSigVccTxTrafficDescrIndex
--   OptGroup
--    atmSwitchServcGroup
--   ObjVar
--    atmIfRegAddrRowStatus
--   ObjVar
--    atmSigSupportClgPtyNumDel
--   ObjVar
--    atmSigSupportClgPtySubAddr
--   ObjVar
--    atmSigSupportCldPtySubAddr
--   ObjVar
--    atmSigSupportHiLyrInfo
--   ObjVar
--    atmSigSupportLoLyrInfo
--   ObjVar
--    atmSigSupportBlliRepeatInd
--   ObjVar
--    atmSigSupportAALInfo
--   ObjVar
--    atmSigSupportPrefCarrier
--   ObjVar
--    atmSvcVpCrossConnectRowStatus
--   ObjVar
--    atmSvcVcCrossConnectRowStatus
--   OptGroup
--    atmServcGroup
--   OptGroup
--    atmHostGroup
--   ObjVar
--    atmVclAddrType
--   ObjVar
--    atmVclAddrRowStatus
--   ObjVar
--    atmVclGenSigDescrIndex
--   ObjVar
--    atmSigDescrParamAalType
--   ObjVar
--    atmSigDescrParamAalSscsType
--   ObjVar
--    atmSigDescrParamBhliType
--   ObjVar
--    atmSigDescrParamBhliInfo
--   ObjVar
--    atmSigDescrParamBbcConnConf
--   ObjVar
--    atmSigDescrParamBlliLayer2
--   ObjVar
--    atmSigDescrParamBlliLayer3
--   ObjVar
--    atmSigDescrParamBlliPktSize
--   ObjVar
--    atmSigDescrParamBlliSnapId
--   ObjVar
--    atmSigDescrParamBlliOuiPid
--   ObjVar
--    atmSigDescrParamRowStatus


END
