--
-- Juniper Enterprise Specific MIB: PFE MIB
-- 
-- Copyright (c) 2006, Juniper Networks, Inc.
-- All rights reserved.
--
-- The contents of this document are subject to change without notice.
--

JUNIPER-PFE-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Counter32, Integer32
        FROM SNMPv2-SMI
    DisplayString
        FROM SNMPv2-TC
    jnxPfeMibRoot
        FROM JUNIPER-SMI;

jnxPfeMib MODULE-IDENTITY
    LAST-UPDATED "201002070000Z" -- Sun Feb 07 00:00:00 2010 UTC
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
            "        Juniper Technical Assistance Center
                     Juniper Networks, Inc.
                     1194 N. Mathilda Avenue
                     Sunnyvale, CA 94089
                     E-mail: support@juniper.net"

    DESCRIPTION
            "The MIB provides PFE specific data."

    REVISION      "201002070000Z"
    DESCRIPTION
               "Added new notification types."
    --REVISION      "201001070000Z"
    --DESCRIPTION
    --         "Added new notification types."
    --REVISION      "200607240000Z"
    --DESCRIPTION
    --           "Initial revision."
    ::= { jnxPfeMibRoot 1 }

    --
    -- This branch contains all PFE Notification statistics data.
    --
    jnxPfeNotification   OBJECT IDENTIFIER ::= { jnxPfeMib 1 }


    --
    -- This table provide global PFE notification stats for each PFE slot,
    -- exposing the data provided by the 'show pfe statistics notification'
    -- cli command.
    --
    jnxPfeNotifyGlTable OBJECT-TYPE
	SYNTAX          SEQUENCE OF JnxPfeNotifyGlEntry
	MAX-ACCESS      not-accessible
	STATUS          current
	DESCRIPTION
		"This table provides global PFE notification statistics."
	::= { jnxPfeNotification 1 }

    jnxPfeNotifyGlEntry OBJECT-TYPE
	SYNTAX          JnxPfeNotifyGlEntry
	MAX-ACCESS      not-accessible
	STATUS          current
	DESCRIPTION
		""
        INDEX { jnxPfeNotifyGlSlot }
	::= { jnxPfeNotifyGlTable 1 }

    JnxPfeNotifyGlEntry ::=
	SEQUENCE {
	    jnxPfeNotifyGlSlot          Integer32,
            jnxPfeNotifyGlParsed        Counter32,
            jnxPfeNotifyGlAged          Counter32,
            jnxPfeNotifyGlCorrupt       Counter32,
            jnxPfeNotifyGlIllegal       Counter32,
            jnxPfeNotifyGlSample        Counter32,
            jnxPfeNotifyGlGiants        Counter32,
            jnxPfeNotifyGlTtlExceeded   Counter32,
            jnxPfeNotifyGlTtlExcErrors  Counter32,
            jnxPfeNotifyGlSvcOptAsp     Counter32,
            jnxPfeNotifyGlSvcOptRe      Counter32,
            jnxPfeNotifyGlPostSvcOptOut Counter32,
            jnxPfeNotifyGlOptTtlExp     Counter32,
            jnxPfeNotifyGlDiscSample    Counter32,
            jnxPfeNotifyGlRateLimited   Counter32,
            jnxPfeNotifyGlPktGetFails   Counter32,
            jnxPfeNotifyGlDmaFails      Counter32,
            jnxPfeNotifyGlDmaTotals     Counter32,
            jnxPfeNotifyGlUnknowns      Counter32
	}

    jnxPfeNotifyGlSlot OBJECT-TYPE
        SYNTAX      Integer32 (0..2147483647)
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "The PFE slot number for this set of global PFE notification
                statistics."
        ::= { jnxPfeNotifyGlEntry 1 }

    jnxPfeNotifyGlParsed OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Count of notifications reported by the routing chip."
        ::= { jnxPfeNotifyGlEntry 2 }

    jnxPfeNotifyGlAged OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Count of notifications that are dropped due to the fact 
                that the they have been in the system for too long and 
                hence not valid anymore."
        ::= { jnxPfeNotifyGlEntry 3 }

    jnxPfeNotifyGlCorrupt OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Count of notifications dropped due to the fact that they 
                have an invalid notification result format. This counter
                is valid for Internet Processor-I and Internet Processor-II 
                only."
        ::= { jnxPfeNotifyGlEntry 4 }

    jnxPfeNotifyGlIllegal OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Count of notifications dropped due to the fact that they 
                have an illegal notification type."
        ::= { jnxPfeNotifyGlEntry 5 }

    jnxPfeNotifyGlSample OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Count of sample notifications reported by the routing chip."
        ::= { jnxPfeNotifyGlEntry 6 }

    jnxPfeNotifyGlGiants OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Count of notifications dropped that are larger than the 
                supported DMA size."
        ::= { jnxPfeNotifyGlEntry 7 }

    jnxPfeNotifyGlTtlExceeded OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Count of options/TTL-expired notifications that need to be 
                sent to service interfaces as transit packets. This counter 
                is valid for Internet Processor-I and Internet Processor-II
                only."
        ::= { jnxPfeNotifyGlEntry 8 }

    jnxPfeNotifyGlTtlExcErrors OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Count of options/TTL-expired packet notifications that could 
                not be sent as transit packets because the output interface 
                could not be determined.  This counter is valid for Internet 
                Processor-I and Internet Processor-II only."
        ::= { jnxPfeNotifyGlEntry 9 }

    jnxPfeNotifyGlSvcOptAsp OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Count of IP options packets that are sent out to a Services 
                PIC."
        ::= { jnxPfeNotifyGlEntry 10 }

    jnxPfeNotifyGlSvcOptRe OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Count of IP options packets that are sent out to the Routing
                Engine."
        ::= { jnxPfeNotifyGlEntry 11 }

    jnxPfeNotifyGlPostSvcOptOut OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Count of notifications that were re-injected by the services 
                PIC after it had processed the associated packets.  These 
                notifications now need to be forwarded out to their actual 
                destination.  This counter is valid for Internet Processor-I 
                and Internet Processor-II only."
        ::= { jnxPfeNotifyGlEntry 12 }

    jnxPfeNotifyGlOptTtlExp OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Count of TTL-expired transit packets."
        ::= { jnxPfeNotifyGlEntry 13 }

    jnxPfeNotifyGlDiscSample OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Count of sample notifications that are dropped as they refer 
                to discarded packets in PFE."
        ::= { jnxPfeNotifyGlEntry 14 }

    jnxPfeNotifyGlRateLimited OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Count of notifications ignored because of PFE software 
                throttling."
        ::= { jnxPfeNotifyGlEntry 15 }

    jnxPfeNotifyGlPktGetFails OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Count of notifications where we could not allocate memory 
                for DMA."
        ::= { jnxPfeNotifyGlEntry 16 }

    jnxPfeNotifyGlDmaFails OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Count of notifications where the DMA of associated packets 
                failed for miscellaneous reasons.  Valid for T-series Internet 
                Processor only."
        ::= { jnxPfeNotifyGlEntry 17 }

    jnxPfeNotifyGlDmaTotals OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Count of notifications for which the packet DMA completed.  
                Valid for T-series Internet Processor only."
        ::= { jnxPfeNotifyGlEntry 18 }

    jnxPfeNotifyGlUnknowns OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Count of notifications that could not be resolved to a known 
                next hop destination. Valid for T-series Internet Processor 
                only."
        ::= { jnxPfeNotifyGlEntry 19 }

    --
    -- This table provides Type specific PFE notification stats for each PFE 
    -- slot, exposing the data provided by the 'show pfe statistics 
    -- notification' cli command.
    --
    jnxPfeNotifyTypeTable OBJECT-TYPE
	SYNTAX          SEQUENCE OF JnxPfeNotifyTypeEntry
	MAX-ACCESS      not-accessible
	STATUS          current
	DESCRIPTION
		"This provides type-specific PFE notification stats"
	::= { jnxPfeNotification 2 }

    jnxPfeNotifyTypeEntry OBJECT-TYPE
	SYNTAX          JnxPfeNotifyTypeEntry
	MAX-ACCESS      not-accessible
	STATUS          current
	DESCRIPTION
		""
        INDEX { jnxPfeNotifyGlSlot, jnxPfeNotifyTypeId }
	::= { jnxPfeNotifyTypeTable 1 }

    JnxPfeNotifyTypeEntry ::=
	SEQUENCE {
	    jnxPfeNotifyTypeId       INTEGER,
            jnxPfeNotifyTypeDescr    DisplayString,
            jnxPfeNotifyTypeParsed   Counter32, 
            jnxPfeNotifyTypeInput    Counter32, 
            jnxPfeNotifyTypeFailed   Counter32, 
            jnxPfeNotifyTypeIgnored  Counter32
	}

    jnxPfeNotifyTypeId  OBJECT-TYPE
        SYNTAX INTEGER {
                   illegal       (1),
                   unclassified  (2),
                   option        (3),
                   nextHop       (4),
                   discard       (5),
                   sample        (6),
                   redirect      (7),
                   dontFragment  (8),
                   cfdf          (9),
                   poison        (10),
                   unknown       (11),
                   specialMemPkt (12), 
                   autoConfig    (13),
                   reject        (14)
               }
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "This identifies the PFE notification type for this row's stats.
            Below is a description of each notification type:
                1.  illegal       Packets with invalid notification type.

                2.  unclassified  Packets that did not have a key lookup 
                                  performed on them.

                3.  option        Packets which have L3 options present.  

                4.  nextHop       Packets that are destined to the host.

                5.  discard       Used when a discarded packet is sent to the 
                                  route processor.

                6.  sample        Unused.

                7.  redirect      This is used when a packet is being sent out 
                                  on the interface it came in on.

                8.  dontFragment  This is used that a packet needs to be 
                                   fragmented but the DF (don't fragment) bit
                                   is set.

                9.  cfdf           When an MTU exceeded indication is 
                                   triggered by the CF chip and the packet has 
                                   DF (don't fragment) set.

                10. poison         Packets that resolved to a poisoned next 
                                   hop index.

                11. unknown       Packets of unknown notification type.
  
                12. specialMemPkt Packets with special memory pkt type notification used in diagnostics.  

                13. autoconfig    Packets with autoconfig PFE notification type used for dynamic VLANs.  

                14. reject        Packets of reject PFE notification type."  
    ::= { jnxPfeNotifyTypeEntry 1 }

    jnxPfeNotifyTypeDescr OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..64))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The description of the Pfe Notification type for this entry."
        ::= { jnxPfeNotifyTypeEntry 2 }

    jnxPfeNotifyTypeParsed OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Count of successful parsing of notifications."
        ::= { jnxPfeNotifyTypeEntry 3 }

    jnxPfeNotifyTypeInput OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Count of notifications whose associated packets were DMA'ed 
                into route processor memory."
        ::= { jnxPfeNotifyTypeEntry 4 }

    jnxPfeNotifyTypeFailed OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Count of failures in parsing the notifications."
        ::= { jnxPfeNotifyTypeEntry 5 }

    jnxPfeNotifyTypeIgnored OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Count of notifications where the notification type in the 
                message does not match any of the valid types."
        ::= { jnxPfeNotifyTypeEntry 6 }

END