-- *******************************************************************
-- CISCO-LWAPP-MESH-MIB.my
-- February,2007 Devesh Pujari
--   
-- Copyright (c) 2006, 2007 by Cisco Systems, Inc.
-- All rights reserved.
-- *******************************************************************

CISCO-LWAPP-MESH-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Unsigned32,
    Integer32,
    Gauge32,
    NOTIFICATION-TYPE
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP,
    NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    TruthValue,
    TimeStamp,
    MacAddress,
    TimeInterval
        FROM SNMPv2-TC
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    cLApSysMacAddress,
    cLApName
        FROM CISCO-LWAPP-AP-MIB
    CLDot11Channel
        FROM CISCO-LWAPP-TC-MIB
    ciscoMgmt
        FROM CISCO-SMI;


-- ********************************************************************
-- *  MODULE IDENTITY
-- ********************************************************************

ciscoLwappMeshMIB MODULE-IDENTITY
    LAST-UPDATED    "200703090000Z"
    ORGANIZATION    "Cisco Systems Inc."
    CONTACT-INFO
            "Cisco Systems,
            Customer Service
            Postal: 170 West Tasman Drive
            San Jose, CA  95134
            USA
            Tel: +1 800 553-NETS

            Email: cs-wnbu-snmp@cisco.com"
    DESCRIPTION
        "This MIB is intended to be implemented on all those
        devices operating as Central Controllers (CC) that
        terminate the Light Weight Access Point Protocol
        (LWAPP) tunnel from Light-weight  Access Points.

        This MIB represents information used in Wireless Mesh
        Network. MAP APs associates directly with RAP APs or 
        with another MAP AP. Each association of AP (MAP-MAP 
        or RAP-MAP) with another AP forms parent-child 
        relationship. 

        The deployment of the controller 
        (referred to as CC in the diagram), mesh nodes 
        (RAP and MAP) LWAPP APs, client(MS) and NMS appear 
        as follows.

         +.......+                 +.......+
         +       +                 +       +
         +  NMS  +                 +  NMS  +
         +       +                 +       +
         +.......+                 +.......+
            .                         .
         .    .                     .   .
        .         .                .        .
        .            .             .            .
        +......+     +......+     +......+           +......+
        +      +     +      +     +      +           +      +
        +  CC  +     +  CC  +     +  CC  +           +  CC  +
        +      +     +      +     +      +           +      +
        +......+     +......+     +......+           +......+
        ..            .             .                 .
        ..            .             .                 .
        .  .            .             .                 .
        .    .            .             .                 .
        .      .            .             .                 .
        .        .            .             .                 .
        +......+ +......+     +......+      +......+          +......+
        +      + +      +     +      +      +      +          +      +
        +  RAP + +  RAP +     +  RAP  +     +  RAP +          +  RAP +
        +      + +      +     +      +      +      +          +      +
        +......+ +......+     +......+      +......+          +......+
        .        .              .             .                 .
        .        .              .             .                 .
        .        .              .             .                 .
        .          .              .             .                 .
        .           .              .             .                 .
        +......+ +......+     +......+      +......+          +......+
        +      + +      +     +      +      +      +          +      +
        +  MAP + +  MS  +     +  MAP +      +  MAP +          +  MAP +
        +      + +      +     +      +      +      +          +      +
        +......+ +......+     +......+      +......+          +......+
        .                    .                          ..    . 
        . .                  .                     ..        .
        .   .                .                  ..            .
        .     .              .              .                .
        +......+ +......+     +......+      +......+.         +......+
        +      + +      +     +      +      +      +          +      +
        +  MAP + +  MAP +     +  MAP +      +  MAP +          +  MS  +
        +      + +      +     +      +      +      +          +      +
        +......+ +......+     +......+      +......+          +......+




        The LWAPP tunnel exists between the controller and
        the APs. The MNs communicate with the APs through
        the protocol defined by the 802.11 standard.

        LWAPP APs, upon bootup, discover and join one of the
        controllers and the controller pushes the 
        configuration, that includes the WLAN parameters to 
        the LWAPP APs. 
        The APs encapsulate all the 802.11 frames from
        wireless clients inside LWAPP frames and forward
        the LWAPP frames to the controller.

                           GLOSSARY

        Access Point ( AP )

        An entity that contains an 802.11 medium access
        control ( MAC ) and physical layer ( PHY ) interface
        and provides access to the distribution services via
        the wireless medium for associated clients.
        LWAPP APs encapsulate all the 802.11 frames in
        LWAPP frames and sends them to the controller to which
        it is logically connected.

        Central Controller ( CC )

        The central entity that terminates the LWAPP protocol
        tunnel from the LWAPP APs. Throughout this MIB,
        this entity is also referred to as 'controller'.

        Mobile Station ( MS )

        A roaming 802.11 wireless device in a wireless
        network associated with an access point. Mobile Station
        and client are used interchangeably. 

        Network Management System ( NMS )

        The station from which the administrator manages the
        wired and wireless networks.

        Mesh Node

        A mesh node is defined as a physical or logical entity
        in the mesh network participating in forming the mesh 
        backhaul. RAP and MAP are two types of mesh nodes 
        supported in mesh network.

        Root AP (RAP)

        The AP forming the bridge between a wired and a mesh
        network with an Ethernet interface to the wired 
        network and a 802.11 radio interface to the mesh 
        network

        Mesh AP (MAP).

        The AP extending wireless coverage similar to a 
        repeater in a mesh network and consists of a 802.11 
        uplink and a 802.11 downlink. On a single-radio 
        backhaul, both uplink and downlink exist on the same 
        radio and are logical links only. On a multi-radio 
        backhaul, they may exist on different radios.

        Mesh Network

        Network starting with the wireless backhaul downlink
        of the RAP and all the entities below except any 
        attached network to the Ethernet link of MAPs. A mesh 
        network below a single RAP is also referred to as a 
        'Mesh Sector'.A mesh network consists of mesh nodes. 
        A single mesh network is always augmented to a single 
        wired network.

        Mesh Link

        A logical 802.11 link between two mesh nodes. A single 
        link is point-to-point. All point-to-multipoint links 
        are considered as multiple mesh links. Often referred 
        to as mesh backhaul link.

        Mesh Backhaul

        A mesh backhaul consists of mesh nodes and mesh links 
        terminating at a RAP. This necessarily creates a one-
        to-one relationship between a 'mesh network', 'mesh
        sector' and a 'mesh backhaul' where these terms can be 
        used interchangeably.

        SNR

        Signal to Noise ratio on the 802.11 radio.

        Bridged network 

        The bridged network is defined as the network(s)
        attached to the Ethernet port of any MAP. There can be
        multiple such networks attached to a single mesh 
        network.

        Mesh Node Roaming

        A mesh node may change its parent mesh node naturally 
        when the RF/network condition changes. Child Mesh node 
        will re-associate and re-authenticate to new parent 
        mesh node. Mesh Security supports two types of mesh 
        node roaming.
           Intra-controller - LWAPP session is not lost.
           Inter-controller - LWAPP session is lost.

        REFERENCE

        [1] Wireless LAN Medium Access Control ( MAC ) and
        Physical Layer ( PHY ) Specifications.

        [2] Draft-obara-capwap-lwapp-00.txt, IETF Light 
        Weight Access Point Protocol"
    REVISION        "200703090000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoMgmt 616 }


ciscoLwappMeshMIBNotifs  OBJECT IDENTIFIER
    ::= { ciscoLwappMeshMIB 0 }

ciscoLwappMeshMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoLwappMeshMIB 1 }

ciscoLwappMeshMIBConform  OBJECT IDENTIFIER
    ::= { ciscoLwappMeshMIB 2 }

ciscoLwappMeshConfig  OBJECT IDENTIFIER
    ::= { ciscoLwappMeshMIBObjects 1 }

ciscoLwappMeshGlobalConfig  OBJECT IDENTIFIER
    ::= { ciscoLwappMeshMIBObjects 2 }

ciscoLwappMeshNeighborsStatus  OBJECT IDENTIFIER
    ::= { ciscoLwappMeshMIBObjects 3 }

ciscoLwappMeshNotifControlConfig  OBJECT IDENTIFIER
    ::= { ciscoLwappMeshMIBObjects 4 }

ciscoLwappMeshMIBNotifObjects  OBJECT IDENTIFIER
    ::= { ciscoLwappMeshMIBObjects 5 }

-- ********************************************************************
-- * Mesh Node configuration
-- ********************************************************************

clMeshNodeTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF ClMeshNodeEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents information about the 802.11
        LWAPP Access Points that have joined the controller
        as part of a mesh network."
    ::= { ciscoLwappMeshConfig 1 }

clMeshNodeEntry OBJECT-TYPE
    SYNTAX          ClMeshNodeEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry represents a conceptual row in this table.
        An entry is created when MAP joins the controller. 
        The entry is removed when the mesh node lose their 
        association with the controller due to loss of 
        communication with controller or when a mesh node 
        is reset."
    INDEX           { cLApSysMacAddress } 
    ::= { clMeshNodeTable 1 }

ClMeshNodeEntry ::= SEQUENCE {
        clMeshNodeRole                 INTEGER ,
        clMeshNodeGroupName            SnmpAdminString,
        clMeshNodeBackhaul             INTEGER ,
        clMeshNodeBackhaulDataRate     Unsigned32,
        clMeshNodeEthernetBridge       TruthValue,
        clMeshNodeEthernetLinkStatus   INTEGER ,
        clMeshNodePublicSafetyBackhaul TruthValue,
        clMeshNodeParentMacAddress     MacAddress,
        clMeshNodeHeaterStatus         INTEGER ,
        clMeshNodeInternalTemp         Integer32,
        clMeshNodeType                 INTEGER ,
        clMeshNodeHops                 Gauge32
}

clMeshNodeRole OBJECT-TYPE
    SYNTAX          INTEGER  {
                        map(1),
                        rap(2)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the role of mesh AP which has
        joined the controller. See glossary section above 
        for detail about MAP and RAP." 
    ::= { clMeshNodeEntry 1 }

clMeshNodeGroupName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..10))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the group name of the mesh
        sector. MAP AP will join the mesh sector which has the 
        same group name configured on RAP AP." 
    ::= { clMeshNodeEntry 2 }

clMeshNodeBackhaul OBJECT-TYPE
    SYNTAX          INTEGER  {
                        dot11a(1),
                        dot11b(2),
                        dot11g(3)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents 802.11 interface type of the
        backhaul link. See Mesh Link in glossary section for
        more detail on backhaul link.
            dot11a - 802.11a radio is used as backhaul link.
            dot11b - 802.11b radio is used as backhaul link.
            dot11g - 802.11g radio is used as backhaul link." 
    ::= { clMeshNodeEntry 3 }

clMeshNodeBackhaulDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "Kbps"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the rate at which packets are sent
        on the backhaul link." 
    ::= { clMeshNodeEntry 4 }

clMeshNodeEthernetBridge OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "A value of 'true' indicates ethernet bridging is enable
        on this mesh node. A value of 'false indicates ethernet 
        bridging is not enable on this mesh node. Ethernet bridging 
        can be enabled on RAP or MAP." 
    ::= { clMeshNodeEntry 5 }

clMeshNodeEthernetLinkStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        up(1),
                        down(2)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents if the link is up or down on
        the ethernet port of the RAP or MAP.
            up   - ethernet link is up.
            down - ethernet link is down." 
    ::= { clMeshNodeEntry 6 }

clMeshNodePublicSafetyBackhaul OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "4.9Ghz considered to be public safety band and is
        limited to some service providers. A value of true
        indicates that 4.9 Ghz can be used on backhaul link 
        by selecting channel on the 802.11a backhaul radio." 
    ::= { clMeshNodeEntry 7 }

clMeshNodeParentMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the MAC address of a parent
        mesh node. In case of RAP this object will 
        return 0000000000000." 
    ::= { clMeshNodeEntry 8 }

clMeshNodeHeaterStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        on(1),
                        off(2)
                    }
    UNITS           "Percent"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the heater status of the
        mesh node.
            on  - heater is in operation
            off - heater is not operation." 
    ::= { clMeshNodeEntry 9 }

clMeshNodeInternalTemp OBJECT-TYPE
    SYNTAX          Integer32
    UNITS           "degree Celsius"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the internal temperature
        of mesh node in celsius." 
    ::= { clMeshNodeEntry 10 }

clMeshNodeType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        indoor(1),
                        outdoor(2)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the type of mesh node.
        indoor  - Mesh node which is manufactured to be used 
                  inside the building. 
        outdoor - Mesh node which can be used outside building 
                  in open environment." 
    ::= { clMeshNodeEntry 11 }

clMeshNodeHops OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "hops"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the number of hops a MAP mesh node
        is from RAP. When the clMeshNodeRole is set to 'RAP' this 
        object will return a value of zero." 
    ::= { clMeshNodeEntry 12 }
 


-- ********************************************************************
-- * Mesh Network global configuration
-- ********************************************************************

clMeshNodeRange OBJECT-TYPE
    SYNTAX          Unsigned32 (150..132000 )
    UNITS           "feet"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the optimal distance in feet
        between RAP and MAP for backhaul link without 
        degrading SNR value."
    DEFVAL          { 12000 } 
    ::= { ciscoLwappMeshGlobalConfig 1 }

clMeshBackhaulClientAccess OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents if client access is to be
        enable on backhaul link. If AP has two radios,802.11a 
        and 802.11bg, then radio which is used as backhaul link 
        does not have client access. A value of 'true' indicates
        client access is present on backhaul link. If AP has only 
        one radio then same radio is used for backhaul and client 
        access."
    DEFVAL          { false } 
    ::= { ciscoLwappMeshGlobalConfig 2 }

clMeshMacFilterList OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "If this object is 'true' then any mesh node joining
        controller will be authenticated against this list.
        If this object is 'false' then mesh node can join 
        controller even if mesh node MAC address is not 
        in MAC filter list."
    DEFVAL          { true } 
    ::= { ciscoLwappMeshGlobalConfig 3 }

clMeshMeshNodeAuthFailureThreshold OBJECT-TYPE
    SYNTAX          Unsigned32 (1..30 )
    UNITS           "failures"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the authorization failure
        threshold value. When the number of failures exceeds 
        this value then 'ciscoLwappMeshAuthFailure' 
        notification is  raised."
    DEFVAL          { 5 } 
    ::= { ciscoLwappMeshGlobalConfig 4 }

clMeshMeshChildAssociationFailuresThreshold OBJECT-TYPE
    SYNTAX          Unsigned32 (10..30 )
    UNITS           "failures"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the number of failed association
        to controller occurred through a parent mesh node. 
        When this values exceeds then 
        'ciscoLwappMeshChildExcludedParent' notification is  
        raised."
    DEFVAL          { 10 } 
    ::= { ciscoLwappMeshGlobalConfig 5 }

clMeshMeshChildExcludedParentInterval OBJECT-TYPE
    SYNTAX          TimeInterval (18000..96000 )
    UNITS           "hundredths-seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the time interval during which
        a child mesh node will exclude a parent mesh node.
        During this interval child will not try to associate 
        the controller through the parent mesh node."
    DEFVAL          { 48000 } 
    ::= { ciscoLwappMeshGlobalConfig 6 }

clMeshSNRThresholdAbate OBJECT-TYPE
    SYNTAX          Unsigned32 (3..50 )
    UNITS           "db"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the abate threshold value of
        SNR. This threshold value is use to determine if the 
        SNR value seen by the child mesh node has reached 
        acceptable level and is use to trigger the
        'ciscoLwappMeshAbateSNR' notification."
    DEFVAL          { 16 } 
    ::= { ciscoLwappMeshGlobalConfig 7 }

clMeshSNRThresholdOnset OBJECT-TYPE
    SYNTAX          Unsigned32 (3..50 )
    UNITS           "db"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the onset threshold value of
        SNR. This threshold value is use to determine if the 
        SNR value seen by the child mesh node has reached 
        below unacceptable level and is use to trigger the
        'ciscoLwappMeshOnsetSNR' notification."
    DEFVAL          { 12 } 
    ::= { ciscoLwappMeshGlobalConfig 8 }

clMeshSNRCheckTimeInterval OBJECT-TYPE
    SYNTAX          TimeInterval (18000..96000 )
    UNITS           "hundredths-seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the time interval after which
        SNR value is checked by child mesh node."
    DEFVAL          { 18000 } 
    ::= { ciscoLwappMeshGlobalConfig 9 }

clMeshExcessiveParentChangeThreshold OBJECT-TYPE
    SYNTAX          Unsigned32 (1..20 )
    UNITS           "occcurences"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the threshold for the number
        of times a child mesh node changes its parent. If number 
        of parent change exceeds this value with in the time 
        interval defined by object 
        'clMeshExcessiveParentChangeInterval' then 
        the 'ciscoLwappMeshExcessiveParentChange' notification 
        is raised."
    DEFVAL          { 5 } 
    ::= { ciscoLwappMeshGlobalConfig 10 }

clMeshExcessiveParentChangeInterval OBJECT-TYPE
    SYNTAX          TimeInterval (180000..360000 )
    UNITS           "hundredths-seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the time interval during which
        number of times a child mesh node changes its parent 
        change is counted. 
        If number of parent change exceeds the value defined by 
        the object 'clMeshExcessiveParentChangeThreshold' with in 
        this time interval then the 
        'ciscoLwappMeshExcessiveParentChange' notification 
        is raised."
    DEFVAL          { 360000 } 
    ::= { ciscoLwappMeshGlobalConfig 11 }

clMeshBackgroundScan OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "A value of 'true' indicates the MAP mesh node
        scans its neighbors on different channel other than 
        only its current channel on backhaul link. This scanning 
        helps MAP mesh node to quickly determine its new parent 
        on different channels."
    DEFVAL          { true } 
    ::= { ciscoLwappMeshGlobalConfig 12 }

clMeshAuthenticationMode OBJECT-TYPE
    SYNTAX          INTEGER  {
                        none(1),
                        eap(2),
                        psk(3)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents authentication mode of RAP and
        MAP mesh nodes in controller.
            none - no authentication is done.
            psk  - pre shared key. Keys provided during manufacturing
                   will be used for authentication of mesh node.
            eap  - extensible authentication protocol is used to 
                   authenticate mesh node. A value of 'eap' indicates, 
                   authentication can happen by local-auth in controller 
                   or by RADIUS server configured in controller."
    DEFVAL          { psk } 
    ::= { ciscoLwappMeshGlobalConfig 13 }
-- ********************************************************************
-- *    NEIGHBOR STATUS
-- ********************************************************************

clMeshNeighborTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF ClMeshNeighborEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents information about neighbors
        of any mesh node. Neighbor AP can be on same or
        different mesh sector. Any mesh node is neighbor of a 
        mesh node, if it can detect 802.11 signals on any 
        channels. Child or parent mesh node also considers as 
        neighbors."
    ::= { ciscoLwappMeshNeighborsStatus 1 }

clMeshNeighborEntry OBJECT-TYPE
    SYNTAX          ClMeshNeighborEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An (conceptual) entry in this table is created when
        mesh node detects neighbor mesh nodes. 
        Entries are removed when the mesh node does not detect
        AP as neighbor."
    INDEX           {
                        cLApSysMacAddress,
                        clMeshNeighborMacAddress
                    } 
    ::= { clMeshNeighborTable 1 }

ClMeshNeighborEntry ::= SEQUENCE {
        clMeshNeighborMacAddress MacAddress,
        clMeshNeighborType       BITS,
        clMeshNeighborLinkSnr    Integer32,
        clMeshNeighborChannel    CLDot11Channel,
        clMeshNeighborUpdate     TimeStamp
}

clMeshNeighborMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents MAC address of neighbor
        mesh node." 
    ::= { clMeshNeighborEntry 1 }

clMeshNeighborType OBJECT-TYPE
    SYNTAX          BITS {
                        parent(0),
                        neighbor(1),
                        excluded(2),
                        child(3),
                        beacon(4),
                        default(5)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents type of neighbor mesh node.
        parent   - Neighbor mesh node is a parent mesh node 
                   of this mesh node.
        neighbor - Its a neighbor mesh node. It can be on 
                   same or different mesh-sector.
        excluded - Neighbor mesh node is excluded by this 
                   mesh node.
        child    - Neighbor mesh node is child of this mesh node.
        beacon   - Neighbor mesh node found by passive scanning.
        Default  - Neighbor mesh node connected using a mismatched 
                   bridge group name" 
    ::= { clMeshNeighborEntry 2 }

clMeshNeighborLinkSnr OBJECT-TYPE
    SYNTAX          Integer32
    UNITS           "dB"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the SNR value seen by this mesh
        node from neighbor mesh node." 
    ::= { clMeshNeighborEntry 3 }

clMeshNeighborChannel OBJECT-TYPE
    SYNTAX          CLDot11Channel
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the channel on which neighbor
        mesh node is operating." 
    ::= { clMeshNeighborEntry 4 }

clMeshNeighborUpdate OBJECT-TYPE
    SYNTAX          TimeStamp
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents when the neighbor table was last
        updated. This value is represented as a instance of 
        sysUp time." 
    ::= { clMeshNeighborEntry 5 }
 


-- ********************************************************************
-- *    Notification control flags
-- ********************************************************************

clMeshAuthFailureNotifEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object controls the generation of
        'ciscoLwappMeshAuthFailure' notification.       
        A value of 'true' indicates notification will 
        be generated.
        A value of 'false' indicates notification will 
        be not be generated."
    DEFVAL          { true } 
    ::= { ciscoLwappMeshNotifControlConfig 1 }

clMeshChildExcludedParentNotifEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object controls the generation of
        'ciscoLwappMeshChildExcludedParent' notification.       
        A value of 'true' indicates notification will 
        be generated.
        A value of 'false' indicates notification will 
        be not be generated."
    DEFVAL          { true } 
    ::= { ciscoLwappMeshNotifControlConfig 2 }

clMeshParentChangeNotifEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object controls the generation of
        'ciscoLwappMeshParentChange' notification.       
        A value of 'true' indicates notification will 
        be generated.
        A value of 'false' indicates notification will 
        be not be generated."
    DEFVAL          { true } 
    ::= { ciscoLwappMeshNotifControlConfig 3 }

clMeshChildMovedNotifEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object controls the generation of
        'ciscoLwappMeshChildMoved' notification.       
        A value of 'true' indicates notification will 
        be generated.
        A value of 'false' indicates notification will 
        be not be generated."
    DEFVAL          { true } 
    ::= { ciscoLwappMeshNotifControlConfig 4 }

clMeshExcessiveParentChangeNotifEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object controls the generation of
        'ciscoLwappMeshExcessiveParentChange' notification.       
        A value of 'true' indicates notification will 
        be generated.
        A value of 'false' indicates notification will 
        be not be generated."
    DEFVAL          { true } 
    ::= { ciscoLwappMeshNotifControlConfig 5 }

clMeshPoorSNRNotifEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object controls the generation of
        'ciscoLwappMeshOnsetSNR' and 
        'ciscoLwappMeshAbateSNR' notifications.       
        A value of 'true' indicates notification will 
        be generated.
        A value of 'false' indicates notification will 
        be not be generated."
    DEFVAL          { true } 
    ::= { ciscoLwappMeshNotifControlConfig 6 }

clMeshConsoleLoginNotifEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object controls the generation of
        'ciscoLwappMeshConsoleLogin' notification.       
        A value of 'true' indicates notification will 
        be generated.
        A value of 'false' indicates notification will 
        be not be generated."
    DEFVAL          { true } 
    ::= { ciscoLwappMeshNotifControlConfig 7 }

-- ********************************************************************
-- *    NOTIFICATION objects
-- ********************************************************************

clMeshNodeMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object specifies the MAC address
        of a LWAPP AP." 
    ::= { ciscoLwappMeshMIBNotifObjects 1 }

clMeshAuthFailureReason OBJECT-TYPE
    SYNTAX          INTEGER  {
                        notInMacFilterList(1),
                        securityFailure(2)
                    }
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object specifies the failure reason when
        a mesh node failed to authenticate through a 
        controller to an Authentication Server.
           notInMacFilterList - MAC address of a mesh node
                       is not configured in MAC filter list.
           securityFailure    - Authentication server sent
                                rejection for the mesh node." 
    ::= { ciscoLwappMeshMIBNotifObjects 2 }

clMeshPreviousParentMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object specifies the MAC address
        of previous parent Mesh Node." 
    ::= { ciscoLwappMeshMIBNotifObjects 3 }

clMeshConsoleLoginStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        success(1),
                        failure(2)
                    }
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object specifies the status of console login
        at MAP mesh node." 
    ::= { ciscoLwappMeshMIBNotifObjects 4 }

-- ********************************************************************
-- *    NOTIFICATION TYPE objects
-- ********************************************************************

ciscoLwappMeshAuthFailure NOTIFICATION-TYPE
    OBJECTS         {
                        clMeshNodeMacAddress,
                        clMeshAuthFailureReason
                    }
    STATUS          current
    DESCRIPTION
        "A mesh node can fail to authorize if the MAC address
        of mesh node is not in the MAC filter list or security 
        failure by authentication server. Reason is specified by 
        'clMeshAuthFailureReason'. This notification is sent by 
        the agent when number of failures exceeds threshold 
        defined by object 'clMeshMeshNodeAuthFailureThreshold'. 
        Object 'clMeshAuthFailureNotifEnabled' controls the 
        generation of this notification."
   ::= { ciscoLwappMeshMIBNotifs 1 }

ciscoLwappMeshChildExcludedParent NOTIFICATION-TYPE
    OBJECTS         {
                        clMeshNodeParentMacAddress,
                        clMeshPreviousParentMacAddress,
                        cLApName
                    }
    STATUS          current
    DESCRIPTION
        "This notification will be sent by agent when child
        mesh node exceeds threshold limit of number of 
        discovery response timeouts defined by object 
        'clMeshMeshChildAssociationFailuresThreshold'. The 
        child mesh node will not try to associate excluded 
        parent mesh node for the interval defined by object 
        'clMeshMeshChildExcludedParentInterval'.

        The child mesh node will remember the excluded parent 
        MAC address and when it joins the network it will 
        inform the controller.  
        'cLApName' specifies child mesh node name. Child MAC 
        address is sent as part of index. Object 
        'clMeshChildExcludedParentNotifEnabled' controls the 
        generation of this notification."
   ::= { ciscoLwappMeshMIBNotifs 2 }

ciscoLwappMeshParentChange NOTIFICATION-TYPE
    OBJECTS         {
                        clMeshNodeParentMacAddress,
                        clMeshPreviousParentMacAddress,
                        cLApName
                    }
    STATUS          current
    DESCRIPTION
        "This notification is sent by the agent when a child
        mesh node changes its parent. Child mesh node will 
        remember its previous parent and when it joins the 
        network it will inform controller about change 
        of its parent. 'cLApName' specifies child mesh node 
        name. Child mesh node MAC address is sent as part of 
        index. Object 'clMeshParentChangeNotifEnabled' controls 
        the generation of this notification."
   ::= { ciscoLwappMeshMIBNotifs 3 }

ciscoLwappMeshChildMoved NOTIFICATION-TYPE
    OBJECTS         {
                        clMeshNeighborType,
                        cLApName
                    }
    STATUS          current
    DESCRIPTION
        "This notification is sent by the agent when a parent
        mesh node loses connection with its child mesh node. 
        'cLApName' specifies parent mesh node name. Parent and 
        child MAC address are sent as part of index. Object 
        'clMeshChildMovedNotifEnabled' controls 
        the generation of this notification."
   ::= { ciscoLwappMeshMIBNotifs 4 }

ciscoLwappMeshExcessiveParentChange NOTIFICATION-TYPE
    OBJECTS         {
                        clMeshNeighborType,
                        cLApName
                    }
    STATUS          current
    DESCRIPTION
        "This notification is sent by the agent when child
        mesh node changes its parent frequently. Each 
        mesh node keeps count of number of parent changes 
        in fixed time. If it exceeds the threshold defined 
        by 'clMeshExcessiveParentChangeThreshold' then child 
        mesh node informs the controller. 'cLApName' specifies 
        child mesh node name. Child and Parent MAC address are 
        sent as part of index. Object 
        'clMeshExcessiveParentChangeNotifEnabled' controls 
        the generation of this notification."
   ::= { ciscoLwappMeshMIBNotifs 5 }

ciscoLwappMeshOnsetSNR NOTIFICATION-TYPE
    OBJECTS         {
                        clMeshNeighborLinkSnr,
                        cLApName
                    }
    STATUS          current
    DESCRIPTION
        "This notification is sent by the agent when child
        mesh node detects lower SNR on backhaul link then 
        defined by object 'clMeshSNRThresholdOnset'. SNR 
        value is checked after interval defined by object 
        'clMeshSNRCheckTimeInterval'. 
        'ciscoLwappMeshAbateSNR' notification will be sent 
        to clear this notification. 'cLApName' specifies 
        child mesh node name. Child and parent MAC address 
        are sent as part of index. Object 
        'clMeshPoorSNRNotifEnabled' controls the generation 
        of this notification."
   ::= { ciscoLwappMeshMIBNotifs 6 }

ciscoLwappMeshAbateSNR NOTIFICATION-TYPE
    OBJECTS         {
                        clMeshNeighborLinkSnr,
                        cLApName
                    }
    STATUS          current
    DESCRIPTION
        "This notification is sent by the agent to clear
        'ciscoLwappMeshOnsetSNR' notification when child mesh 
        node detects SNR on backhaul link is higher then
        the object defined by 'clMeshSNRThresholdAbate'. SNR 
        value is checked after interval defined by object 
        'clMeshSNRCheckTimeInterval'. 
        'cLApName' specifies child mesh node name.
        Child and parent MAC address are sent as part of index.
        Object 'clMeshPoorSNRNotifEnabled' controls the 
        generation of this notification."
   ::= { ciscoLwappMeshMIBNotifs 7 }

ciscoLwappMeshConsoleLogin NOTIFICATION-TYPE
    OBJECTS         {
                        clMeshNodeMacAddress,
                        clMeshConsoleLoginStatus,
                        cLApName
                    }
    STATUS          current
    DESCRIPTION
        "This notification is sent by the agent when login on
        MAP console is successful or failure after three
        attempts. 'cLApName' specifies mesh node name.
        Object 'clMeshPoorSNRNotifEnabled' controls the 
        generation of this notification."
   ::= { ciscoLwappMeshMIBNotifs 8 }
-- ********************************************************************
-- *    Compliance statements
-- ********************************************************************

ciscoLwappMeshMIBCompliances  OBJECT IDENTIFIER
    ::= { ciscoLwappMeshMIBConform 1 }

ciscoLwappMeshMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoLwappMeshMIBConform 2 }


ciscoLwappMeshMIBCompliance MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappMeshMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappMeshConfigGroup,
                        ciscoLwappMeshNeighborStatusGroup,
                        ciscoLwappMeshNotifControlGroup,
                        ciscoLwappMeshNotifObjsGroup,
                        ciscoLwappMeshNotifsGroup
                    }
    ::= { ciscoLwappMeshMIBCompliances 1 }

-- ********************************************************************
-- *    Units of conformance
-- ********************************************************************

ciscoLwappMeshConfigGroup OBJECT-GROUP
    OBJECTS         {
                        clMeshNodeRole,
                        clMeshNodeGroupName,
                        clMeshNodeBackhaul,
                        clMeshNodeBackhaulDataRate,
                        clMeshNodeEthernetBridge,
                        clMeshNodeEthernetLinkStatus,
                        clMeshNodePublicSafetyBackhaul,
                        clMeshNodeParentMacAddress,
                        clMeshNodeHeaterStatus,
                        clMeshNodeInternalTemp,
                        clMeshNodeType,
                        clMeshNodeHops,
                        clMeshNodeRange,
                        clMeshBackhaulClientAccess,
                        clMeshMacFilterList,
                        clMeshMeshNodeAuthFailureThreshold,
                        clMeshMeshChildAssociationFailuresThreshold,
                        clMeshMeshChildExcludedParentInterval,
                        clMeshSNRThresholdAbate,
                        clMeshSNRThresholdOnset,
                        clMeshSNRCheckTimeInterval,
                        clMeshExcessiveParentChangeThreshold,
                        clMeshExcessiveParentChangeInterval,
                        clMeshBackgroundScan,
                        clMeshAuthenticationMode
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the
        global and mesh node specific configuration
        and monitor parameters."
    ::= { ciscoLwappMeshMIBGroups 1 }

ciscoLwappMeshNeighborStatusGroup OBJECT-GROUP
    OBJECTS         {
                        clMeshNeighborType,
                        clMeshNeighborLinkSnr,
                        clMeshNeighborChannel,
                        clMeshNeighborUpdate
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the
        neighbor status of any mesh node."
    ::= { ciscoLwappMeshMIBGroups 2 }

ciscoLwappMeshNotifControlGroup OBJECT-GROUP
    OBJECTS         {
                        clMeshAuthFailureNotifEnabled,
                        clMeshChildExcludedParentNotifEnabled,
                        clMeshParentChangeNotifEnabled,
                        clMeshChildMovedNotifEnabled,
                        clMeshExcessiveParentChangeNotifEnabled,
                        clMeshPoorSNRNotifEnabled,
                        clMeshConsoleLoginNotifEnabled
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the flags
        to control the generation of notification."
    ::= { ciscoLwappMeshMIBGroups 3 }

ciscoLwappMeshNotifObjsGroup OBJECT-GROUP
    OBJECTS         {
                        clMeshNodeMacAddress,
                        clMeshAuthFailureReason,
                        clMeshPreviousParentMacAddress,
                        clMeshConsoleLoginStatus
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the information
        carried by the mesh network related notifications sent
        by the agent to a network management station."
    ::= { ciscoLwappMeshMIBGroups 4 }

ciscoLwappMeshNotifsGroup NOTIFICATION-GROUP
   NOTIFICATIONS    {
                        ciscoLwappMeshAuthFailure,
                        ciscoLwappMeshChildExcludedParent,
                        ciscoLwappMeshParentChange,
                        ciscoLwappMeshChildMoved,
                        ciscoLwappMeshExcessiveParentChange,
                        ciscoLwappMeshOnsetSNR,
                        ciscoLwappMeshAbateSNR,
                        ciscoLwappMeshConsoleLogin
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the mesh network
        related notifications sent by the agent to a network 
        management station."
    ::= { ciscoLwappMeshMIBGroups 5 }

END



