-- *****************************************************************
-- CISCO-IP-CAPABILITY.my: Cisco IP-MIB AGENT-CAPABILITIES
--   
-- June 2005, Gayathri Velayutham.
--   
-- Copyright (c) 2005-2008 by cisco Systems Inc.
-- All rights reserved.
--   
-- *****************************************************************

CISCO-IP-CAPABILITY DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY
        FROM SNMPv2-SMI
    AGENT-CAPABILITIES
        FROM SNMPv2-CONF
    ciscoAgentCapability
        FROM CISCO-SMI;


ciscoIpCapability MODULE-IDENTITY
    LAST-UPDATED    "200808110000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 W. Tasman Drive
            San Jose, CA  95134-1706
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-ipv6@cisco.com"
    DESCRIPTION
        "The capabilities description of IP-MIB."
    REVISION        "200808110000Z"
    DESCRIPTION
        "Added newline at the end of the MIB file."
    REVISION        "200711050000Z"
    DESCRIPTION
        "Added cIpCapc4710aceVA1R700 agent capabilities
        for ACE 4710 Application Control Engine Appliance."
    REVISION        "200611030000Z"
    DESCRIPTION
        "Added capability for Cisco TelePresence System (CTS) and
        Cisco TelePresence Manager (CTM) platforms."
    REVISION        "200605270000Z"
    DESCRIPTION
        "Added capability statement
        cIpCapACSWV03R000"
    REVISION        "200602170000Z"
    DESCRIPTION
        "Added ipv4 Object Groups to the initial
        Agent Capability"
    REVISION        "200507250000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoAgentCapability 445 }



cIpCapV320CRS1 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS XR 3.2.0 for CRS-1"
    STATUS          current
    DESCRIPTION
        "IP-MIB capabilities."

    SUPPORTS        IP-MIB
    INCLUDES        {
                        ipv6GeneralGroup2,
                        ipv6IfGroup,
                        ipSystemStatsGroup,
                        ipIfStatsGroup,
                        ipAddressPrefixGroup,
                        ipAddressGroup,
                        ipNetToPhysicalGroup,
                        ipv6RouterAdvertGroup,
                        icmpStatsGroup,
                        ipGroup,
                        icmpGroup
                    }
    VARIATION       ipSystemStatsIPVersion
    SYNTAX          INTEGER  {
                        ipv6(2)
                    }
    DESCRIPTION
        "This object is supported for ipv6 only."

    VARIATION       ipIfStatsIPVersion
    SYNTAX          INTEGER  {
                        ipv6(2)
                    }
    DESCRIPTION
        "This object is supported for ipv6 only."

    VARIATION       ipAddressPrefixType
    SYNTAX          INTEGER  {
                        ipv6(2)
                    }
    DESCRIPTION
        "This object is supported for ipv6 only."

    VARIATION       ipAddressAddrType
    SYNTAX          INTEGER  {
                        ipv6(2),
                        ipv6z(4)
                    }
    DESCRIPTION
        "This object is supported for ipv6 only."

    VARIATION       ipNetToPhysicalNetAddressType
    SYNTAX          INTEGER  {
                        ipv6(2)
                    }
    DESCRIPTION
        "This object is supported for ipv6 only.For
        linklocal address, both Net and Physical
        address are  the same.Hence, ipv6z (4) is
        redundant and not supported."

    VARIATION       icmpStatsIPVersion
    SYNTAX          INTEGER  {
                        ipv6(2)
                    }
    DESCRIPTION
        "This object is supported  for ipv6 only."

    VARIATION       icmpMsgStatsIPVersion
    SYNTAX          INTEGER  {
                        ipv6(2)
                    }
    DESCRIPTION
        "This object is supported  for ipv6 only ."

    VARIATION       ipv6IpDefaultHopLimit
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported by the platform."

    VARIATION       ipSystemStatsInOctets
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipSystemStatsInNoRoutes
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipSystemStatsInDiscards
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipSystemStatsOutNoRoutes
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipSystemStatsOutForwDatagrams
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipSystemStatsOutTransmits
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipSystemStatsOutOctets
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipSystemStatsInMcastPkts
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipSystemStatsInMcastOctets
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipSystemStatsOutMcastPkts
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipSystemStatsOutMcastOctets
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipSystemStatsDiscontinuityTime
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipSystemStatsRefreshRate
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipIfStatsInHdrErrors
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipIfStatsInNoRoutes
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipIfStatsInAddrErrors
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipIfStatsInUnknownProtos
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipIfStatsInTruncatedPkts
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipIfStatsInForwDatagrams
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipIfStatsReasmReqds
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipIfStatsReasmOKs
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipIfStatsReasmFails
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipIfStatsInDiscards
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipIfStatsInDelivers
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipIfStatsOutRequests
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipIfStatsOutForwDatagrams
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipIfStatsOutDiscards
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipIfStatsOutFragReqds
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipIfStatsOutFragOKs
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipIfStatsOutFragFails
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipIfStatsOutFragCreates
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipIfStatsRefreshRate
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipAddressPrefixAdvPreferredLifetime
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipAddressPrefixAdvValidLifetime
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipAddressSpinLock
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipAddressLastChanged
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipv6RouterAdvertSpinLock
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipv6RouterAdvertLinkMTU
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipv6RouterAdvertReachableTime
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipv6RouterAdvertRetransmitTime
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipv6RouterAdvertCurHopLimit
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipv6RouterAdvertDefaultLifetime
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       icmpStatsOutErrors
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported."

    VARIATION       ipForwarding
    SYNTAX          INTEGER  {
                        forwarding(1)
                    }
    DESCRIPTION
        "notForwarding(2)is not supported."

    VARIATION       ipAdEntBcastAddr
    ACCESS          not-implemented
    DESCRIPTION
        "Current MIB Implementation doesn't
        support configuration of broadcast
        address, So this is set to 1"

    VARIATION       ipNetToMediaIfIndex
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported
        in the current MIB Implentation."

    VARIATION       ipNetToMediaPhysAddress
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported
        in the current MIB Implentation."

    VARIATION       ipNetToMediaNetAddress
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported
        in the current MIB Implentation."

    VARIATION       ipNetToMediaType
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported
        in the current MIB Implentation."

    ::= { ciscoIpCapability 1 }

cIpCapACSWV03R000 AGENT-CAPABILITIES
    PRODUCT-RELEASE "ACSW (Application Control Software) 3.0"
    STATUS          current
    DESCRIPTION
        "IP-MIB capabilities."

    SUPPORTS        IP-MIB
    INCLUDES        {
                        ipv4GeneralGroup,
                        ipSystemStatsGroup,
                        ipv4SystemStatsGroup,
                        ipSystemStatsHCOctetGroup,
                        ipSystemStatsHCPacketGroup,
                        ipv4SystemStatsHCPacketGroup,
                        ipIfStatsGroup,
                        ipv4IfStatsGroup,
                        ipIfStatsHCOctetGroup,
                        ipIfStatsHCPacketGroup,
                        ipv4IfStatsHCPacketGroup,
                        icmpStatsGroup
                    }
    VARIATION       ipForwarding
    ACCESS          read-only
    DESCRIPTION
        "Write operation not allowed via SNMP."

    VARIATION       ipDefaultTTL
    ACCESS          read-only
    DESCRIPTION
        "Write operation not allowed via SNMP."

    ::= { ciscoIpCapability 2 }

cIpCapCTSV100 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco TelePresence System (CTS) 1.0.0"
    STATUS          current
    DESCRIPTION
        "IP-MIB capabilities."

    SUPPORTS        IP-MIB
    INCLUDES        {
                        ipGroup,
                        icmpGroup
                    }
    VARIATION       ipForwarding
    ACCESS          read-only
    DESCRIPTION
        "Write operation not allowed via SNMP."

    VARIATION       ipDefaultTTL
    ACCESS          read-only
    DESCRIPTION
        "Write operation not allowed via SNMP."

    VARIATION       ipNetToMediaNetAddress
    ACCESS          read-only
    DESCRIPTION
        "Write operation not allowed via SNMP."

    VARIATION       ipNetToMediaType
    ACCESS          read-only
    DESCRIPTION
        "Write operation not allowed via SNMP."

    ::= { ciscoIpCapability 3 }

cIpCapCTMV1000 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco TelePresence Manager (CTM) 1.0.0.0"
    STATUS          current
    DESCRIPTION
        "IP-MIB capabilities."

    SUPPORTS        IP-MIB
    INCLUDES        {
                        ipGroup,
                        icmpGroup
                    }
    VARIATION       ipForwarding
    ACCESS          read-only
    DESCRIPTION
        "Write operation not allowed via SNMP."

    VARIATION       ipDefaultTTL
    ACCESS          read-only
    DESCRIPTION
        "Write operation not allowed via SNMP."

    VARIATION       ipNetToMediaNetAddress
    ACCESS          read-only
    DESCRIPTION
        "Write operation not allowed via SNMP."

    VARIATION       ipNetToMediaType
    ACCESS          read-only
    DESCRIPTION
        "Write operation not allowed via SNMP."

    ::= { ciscoIpCapability 4 }

cIpCapc4710aceVA1R700 AGENT-CAPABILITIES
    PRODUCT-RELEASE "ACSW (Application Control Software) A1(7)
                    for ACE 4710 Application Control Engine 
                    Appliance"
    STATUS          current
    DESCRIPTION
        "IP-MIB capabilities."

    SUPPORTS        IP-MIB
    INCLUDES        {
                        ipv4GeneralGroup,
                        ipSystemStatsGroup,
                        ipv4SystemStatsGroup,
                        ipSystemStatsHCOctetGroup,
                        ipSystemStatsHCPacketGroup,
                        ipv4SystemStatsHCPacketGroup,
                        ipIfStatsGroup,
                        ipv4IfStatsGroup,
                        ipIfStatsHCOctetGroup,
                        ipIfStatsHCPacketGroup,
                        ipv4IfStatsHCPacketGroup,
                        icmpStatsGroup
                    }
    VARIATION       ipForwarding
    ACCESS          read-only
    DESCRIPTION
        "Write operation not allowed via SNMP."

    VARIATION       ipDefaultTTL
    ACCESS          read-only
    DESCRIPTION
        "Write operation not allowed via SNMP."

    ::= { ciscoIpCapability 5 }

END


