-- ----------------------------------------------------------------------------
-- File Main Owner: 
-- File Peer Owner:   
-- File Description:  Main entry point to build private MIBs.
--                    
--
-- { COPYRIGHT / HISTORY
--
--
--
-- PORTING HISTORY
--
-- } COPYRIGHT / HISTORY (end)
--


-- ----------------------------------------------------------------------------
-- { INSERT:  hpRoot
-- ----------------------------------------------------------------------------

BLADETYPE5-NETWORK-MIB                 DEFINITIONS ::= BEGIN

IMPORTS
    OBJECT-TYPE, Integer32, Unsigned32, Counter32, Gauge32,
    Counter64, TimeTicks, IpAddress
        FROM SNMPv2-SMI
    DisplayString, PhysAddress, MacAddress
        FROM SNMPv2-TC
    BridgeId
        FROM BRIDGE-MIB
    sysName, sysLocation, sysContact, ifIndex
        FROM RFC1213-MIB
    enterprises
        FROM RFC1155-SMI

    hpSwitchBladeType5-Products,
    hpSwitchBladeType5-Mgmt
        FROM HP-SWITCH-PL-MIB;



--   SysObjId for GbE2c-1-10G Interconnect Switch (1.3.6.1.4.1.11.2.3.7.11.33.5.1.1)
hpProLiant-GbE2c-1-10G-InterconnectSwitch  OBJECT IDENTIFIER 
     ::= { hpSwitchBladeType5-Products 1 }



-------------------------------------------------------------------------------
-- HP Platform Common Private MIBs
-------------------------------------------------------------------------------

agent                   OBJECT IDENTIFIER
    ::= { hpSwitchBladeType5-Mgmt 1 }

-- ----------------------------------------------------------------------------
-- { INSERT:  bt2Switch
-- ----------------------------------------------------------------------------

agentConfig       OBJECT IDENTIFIER ::= { agent 1 }
agentStats        OBJECT IDENTIFIER ::= { agent 2 }
agentInfo         OBJECT IDENTIFIER ::= { agent 3 }
agentOper         OBJECT IDENTIFIER ::= { agent 4 }

agSystem          OBJECT IDENTIFIER ::= { agentConfig 1 }
agPortConfig      OBJECT IDENTIFIER ::= { agentConfig 2 }
agRadiusConfig    OBJECT IDENTIFIER ::= { agentConfig 3 }
agNTP	          OBJECT IDENTIFIER ::= { agentConfig 4 }
agSyslog          OBJECT IDENTIFIER ::= { agentConfig 5 }
agTransfer            OBJECT IDENTIFIER ::= { agentConfig 7 }
agApply           OBJECT IDENTIFIER ::= { agentConfig 8 }
agTacacsConfig    OBJECT IDENTIFIER ::= { agentConfig 10 }
agMgmtNetConfig   OBJECT IDENTIFIER ::= { agentConfig 11 }
agAccess	  OBJECT IDENTIFIER ::= { agentConfig 12 }
agSSHConfig       OBJECT IDENTIFIER ::= { agentConfig 13 }


pktStats	  OBJECT IDENTIFIER ::= { agentStats 1 }
mpCpuStats	  OBJECT IDENTIFIER ::= { agentStats 2 }
portStats	  OBJECT IDENTIFIER ::= { agentStats 3 }
agClearStats	  OBJECT IDENTIFIER ::= { agentStats 7 }
ntpStats          OBJECT IDENTIFIER ::= { agentStats 9 }
aclStats          OBJECT IDENTIFIER ::= { agentStats 12 }
hardware          OBJECT IDENTIFIER ::= { agentInfo 1 }
portInfo          OBJECT IDENTIFIER ::= { agentInfo 2 }
agDiff            OBJECT IDENTIFIER ::= { agentInfo 4 }
agCfgDump         OBJECT IDENTIFIER ::= { agentInfo 5 }
geaportInfo       OBJECT IDENTIFIER ::= { agentInfo 7 }
ufdInfo           OBJECT IDENTIFIER ::= { agentInfo 8 }
sfpInfo                 OBJECT IDENTIFIER ::= { agentInfo 9 }




agNTPOper         OBJECT IDENTIFIER ::= { agentOper 2 }

-- There are two configuration blocks for Bladetype2 switches.
-- The "current_config" reflects the configuration parameters that the
-- switch is operating on and it is read-only.  The objects with "CurCfg"
-- in the name are reflect to this configuration block.
--
-- The "new_config" accepts user configurations on set.  The objects with
-- "NewCfg" in the name are reflect to this configuration block.
--
-- The newly set configurations will not take effect until a "apply"
-- command has been issued (See agApplyConfiguration object defined in
-- BLADETYPE2-SWITCH-MIB).
--
-- The newly set configurations will not be saved through next restarting
-- of the switch unless a "save" command has been issued (See
-- agSaveConfiguration object defined in BLADETYPE2-SWITCH-MIB).

-- Hardware Information

hwPartNumber OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..16))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The hardware part number of the Bladetype2 Switch." 
    ::= { hardware 1 }

hwRevision OBJECT-TYPE
    SYNTAX DisplayString (SIZE(0..16))
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The hardware revision.  If the revision is not
	 available, a zero length string should be returned."
    ::= { hardware 2 }


hwSerialNumber OBJECT-TYPE
    SYNTAX DisplayString (SIZE(0..16))
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The switch serial number."
    ::= { hardware 5 }

-- Port operation table
agPortOperTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF AgPortOperTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of port operations."
    ::= { agentOper 1 }

agPortOperTableEntry OBJECT-TYPE
    SYNTAX  AgPortOperTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the port operations table."
    INDEX   { portOperIdx }
    ::= { agPortOperTable 1 }

AgPortOperTableEntry ::=
    SEQUENCE {
	portOperIdx	 Integer32,
	portOperState	 INTEGER
	,portOperRmon	 INTEGER
	}

portOperIdx OBJECT-TYPE
    SYNTAX  Integer32  
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port index."
    ::= { agPortOperTableEntry 1 }

portOperState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable/Disable port."
    ::= { agPortOperTableEntry 2 }

portOperRmon OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable/Disable RMON for port."
    ::= { agPortOperTableEntry 3 }



--portOperDot1x	    OBJECT IDENTIFIER ::= { agPortOperTableEntry 4 }

portOperDot1xTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF PortOperDot1xTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of port operations."
    ::= { agentOper 3 }

portOperDot1xTableEntry OBJECT-TYPE
    SYNTAX  PortOperDot1xTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the port 802.1x operation table."
    INDEX   { portOperDot1xIndx }
    ::= { portOperDot1xTable 1 }

PortOperDot1xTableEntry ::= SEQUENCE {
    portOperDot1xIndx        	Integer32,
    portOperDot1xReset		INTEGER,
    portOperDot1xReauth		INTEGER
    }

portOperDot1xIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port index."
    ::= { portOperDot1xTableEntry 1 }

portOperDot1xReset OBJECT-TYPE
    SYNTAX  INTEGER {
        no(1),
        yes(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Reinitialize 802.1x access control on port."
    ::= { portOperDot1xTableEntry 2 }

portOperDot1xReauth OBJECT-TYPE
    SYNTAX  INTEGER {
        no(1),
        yes(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Initiate reauthentication on port."
    ::= { portOperDot1xTableEntry 3 }

-- NTP operation

ntpOperSendReq OBJECT-TYPE
    SYNTAX  INTEGER {
        no(1),
        yes(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Allows the user to send requests to the NTP server."
    ::= { agNTPOper 1 }

-- Port information table

portInfoTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF PortInfoTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of port information."
    ::= { portInfo 1 }

portInfoTableEntry OBJECT-TYPE
    SYNTAX  PortInfoTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the port information table."
    INDEX   { portInfoIndx }
    ::= { portInfoTable 1 }

PortInfoTableEntry ::= SEQUENCE {
    portInfoIndx        	Integer32,
    portInfoSpeed       	INTEGER,
    portInfoMode        	INTEGER,
    portInfoFlowCtrl    	INTEGER,
    portInfoLink        	INTEGER,
    portInfoPhyIfDescr  	DisplayString,
    portInfoPhyIfType   	INTEGER,
    portInfoPhyIfMtu    	Integer32,
    portInfoPhyIfPhysAddress  	PhysAddress,
    portInfoPhyIfOperStatus	INTEGER, 
    portInfoPhyIfLastChange	TimeTicks
    }

portInfoIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port index."
    ::= { portInfoTableEntry 1 }

portInfoSpeed OBJECT-TYPE
    SYNTAX  INTEGER {
        mbs10(2),
        mbs100(3),
        mbs1000(4),
        mbs10000(6),
        any(5)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The current operational speed of the port."
    ::= { portInfoTableEntry 2 }

portInfoMode OBJECT-TYPE
    SYNTAX  INTEGER {
        full-duplex(2),
        half-duplex(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The current operational mode of the port."
    ::= { portInfoTableEntry 3 }

portInfoFlowCtrl OBJECT-TYPE
    SYNTAX  INTEGER {
        transmit(2),
        receive(3),
        both(4),
        none(5)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The current operational flow control of the port."
    ::= { portInfoTableEntry 4 }

portInfoLink OBJECT-TYPE
    SYNTAX  INTEGER {
        up(1),
        down(2),
        disabled(3),
        inoperative(4) -- unrecognized PCI device
        }
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
         "The current operational link status of the port."
     ::= { portInfoTableEntry 5 }

portInfoPhyIfDescr OBJECT-TYPE
    SYNTAX  DisplayString (SIZE (0..255))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	    "A textual string containing information about the
	    interface.  This string should include the name of
	    the manufacturer, the product name and the version
	    of the hardware interface."
    ::= { portInfoTableEntry 6 }

portInfoPhyIfType OBJECT-TYPE
    SYNTAX  INTEGER {
		other(1),          -- none of the following
		regular1822(2),
		hdh1822(3),
		ddn-x25(4),
		rfc877-x25(5),
		ethernet-csmacd(6),
		iso88023-csmacd(7),
		iso88024-tokenBus(8),
		iso88025-tokenRing(9),
		iso88026-man(10),
		starLan(11),
		proteon-10Mbit(12),
		proteon-80Mbit(13),
		hyperchannel(14),
		fddi(15),
		lapb(16),
		sdlc(17),
		ds1(18),           -- T-1
		e1(19),            -- european equiv. of T-1
		basicISDN(20),
		primaryISDN(21),   -- proprietary serial
		propPointToPointSerial(22),
		ppp(23),
		softwareLoopback(24),
		eon(25),            -- CLNP over IP [11]
		ethernet-3Mbit(26),
		nsip(27),           -- XNS over IP
		slip(28),           -- generic SLIP
		ultra(29),          -- ULTRA technologies
		ds3(30),            -- T-3
		sip(31),            -- SMDS
		frame-relay(32)
	    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	    "The type of interface, distinguished according to
	    the physical/link protocol(s) immediately `below'
	    the network layer in the protocol stack."
    ::= { portInfoTableEntry 7 }

portInfoPhyIfMtu OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	    "The size of the largest datagram which can be
	    sent/received on the interface, specified in
	    octets.  For interfaces that are used for
	    transmitting network datagrams, this is the size
	    of the largest network datagram that can be sent
	    on the interface."
    ::= { portInfoTableEntry 8 }

portInfoPhyIfPhysAddress OBJECT-TYPE
    SYNTAX  PhysAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	    "The interface's address at the protocol layer
	    immediately `below' the network layer in the
	    protocol stack.  For interfaces which do not have
	    such an address (e.g., a serial line), this object
	    should contain an octet string of zero length."
    ::= { portInfoTableEntry 9 }

portInfoPhyIfOperStatus OBJECT-TYPE
    SYNTAX  INTEGER {
		up(1),       -- ready to pass packets
		down(2),
		testing(3)   -- in some test mode
	    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	    "The current operational state of the interface.
	    The testing(3) state indicates that no operational
	    packets can be passed."
    ::= { portInfoTableEntry 10 }

portInfoPhyIfLastChange OBJECT-TYPE
    SYNTAX  TimeTicks
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	    "The value of sysUpTime at the time the interface
	    entered its current operational state.  If the
	    current state was entered prior to the last re-
	    initialization of the local network management
	    subsystem, then this object contains a zero
	    value."
    ::= { portInfoTableEntry 11 }




-- Agent System Group
-- This group of objects take effect on the 'SET' request.
-- There is no need to 'apply' or 'save'.
 
agApplyConfiguration OBJECT-TYPE
    SYNTAX  INTEGER {
        other(1),
        apply(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "This is an action object to apply the changes made to configuration 
         of the switch. By setting the value to apply(2), all the changes 
         made since the last apply are written to the new_config block.

         other(1) is returned when this object ie read. "
    ::= { agSystem 2 }

agSavePending OBJECT-TYPE
    SYNTAX  INTEGER {
        saveNeeded(1),
        noSaveNeeded(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This object, when read, gives the user information
         whether an save action is needed and that the configuration
         has been applied but not saved to the flash."
    ::= { agSystem 3 }

agSaveConfiguration OBJECT-TYPE
    SYNTAX  INTEGER {
        ok(1),
        saveActive(2),
        notSaveActive(3)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "This is an action object to write current configuration to 
         nonvolatile storage.

         When issued with the saveActive, the active configuration
         in flash is saved to backup in flash and then the new
         configuration is saved to the active configuration in flash.

         When issued with notSaveActive, the active configuration
         is NOT saved to the flash and the active configuration is
         overwritten with the new configuration.

         ok(1) is returned always when read."
    ::= { agSystem 4 }

agRevert OBJECT-TYPE
    SYNTAX  INTEGER {
        other(1),
        revert(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "This is an action object to revert the unapplied changes 
         made to the switch. By setting the value to revert(2), 
         all the unapplied changes will be reverted. This action 
         will copy the current_config to the new_config block.

         other(1) is returned when this object is read. "
    ::= { agSystem 5 }

agRevertApply OBJECT-TYPE
    SYNTAX  INTEGER {
        other(1),
        revertApply(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "This is an action object to revert the unsaved changes 
         made to the switch. By setting the value to revertApply(2), 
         all the unsaved as well as unapplied changes will be 
         reverted.

         other(1) is returned when this object is read. "
    ::= { agSystem 6 }

agReset OBJECT-TYPE
    SYNTAX  INTEGER {
        other(1),
        coldReset(2),
        warmReset(3)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "This is an action object to reboot the switch.
         other(1) is returned always when read.

         The following values are writable:
             coldReset(2)...
             warmReset(3)..."
    ::= { agSystem 7 }

agConfigForNxtReset OBJECT-TYPE
    SYNTAX  INTEGER {
        active(2),
        backup(3),
        default(4)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The configuration information to be loaded from at next reset.

          The following values are writable:
              active(2)...active configuration block
              backup(3)...backup configuration block
              default(4)..default configuration block"
    ::= { agSystem 8 }

agImageForNxtReset OBJECT-TYPE
    SYNTAX  INTEGER {
        image1(2),
        image2(3)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The software image to be booted from at next reset.

         The following values are writable:
             image1(2)...image 1
             image2(3)...image 2"
    ::= { agSystem 9 }

agSoftwareVersion OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..16))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The version of the software image that is currently running on the 
         system in the form of 'major.minor.maintenance.bugfix'.  A zero 
         length string is returned if version is not available."
    ::= { agSystem 10 }

agBootVer OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..16))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The version of the boot code in the form of 'major.minor.bugfix'.
         A zero length string is returned if version is not available."
    ::= { agSystem 11 }

agImage1Ver OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The version of the software image stored in image 1 storage in the 
         form of 'major.minor.bugfix'.  A zero length string is returned if 
         version is not available or there is no valid software image."
    ::= { agSystem 12 }

agImage2Ver OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The version of the software image stored in image 2 storage in the 
         form of 'major.minor.bugfix'.  A zero length string is returned if 
         version is not available or there is no valid software image."
    ::= { agSystem 13 }

agRtcDate OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..16))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The date on the real time clock in the form of 'mm/dd/yy'.  
         A zero length string is returned if date is not available."
    ::= { agSystem 14 }

agRtcTime OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..16))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The time on the real time clock in the form of 'hh:mm:ss'.  
         A zero length string is returned if time is not available."
    ::= { agSystem 15 }

agLastSetErrorReason   OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..255))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The error reason of the last SET failure."
    ::= { agSystem 16 }

agCurCfgHttpServerPort OBJECT-TYPE
    SYNTAX  INTEGER (1..65535)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The TCP port number that the HTTP server is listening to 
         in the current_configuration block."
    ::= { agSystem 17 }

agNewCfgHttpServerPort OBJECT-TYPE
    SYNTAX  INTEGER (1..65535)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The TCP port number that the HTTP server is listening to 
         in the new_configuration block."
    ::= { agSystem 18 }

agCurCfgLoginBanner OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..79))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The user defined login banner."
    ::= { agSystem 19 }

agNewCfgLoginBanner OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..79))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The user defined login banner."
    ::= { agSystem 20 }


agCurCfgConsole OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable console output of syslog messages."
    ::= { agSystem 23 }

agNewCfgConsole OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable console output of syslog messages."
    ::= { agSystem 24 }


agCurCfgBootp OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(2),
        disabled(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable the use of BootP, as currently configured in the 
         current_configuration block."
    ::= { agSystem 29 }

agNewCfgBootp OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(2),
        disabled(3)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable the use of BootP, in the new_configuration block."
    ::= { agSystem 30 }

agSlotNumber OBJECT-TYPE
    SYNTAX INTEGER (1..10)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Identifies the slot in which this switch is installed. If the 
         agent implementing this MIB is not a blade in a chassis this 
         value has no meaning."
    ::= { agSystem 31 }

agCurCfgSnmpTimeout OBJECT-TYPE
    SYNTAX  INTEGER (1..30)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Once SNMP operations like agApplyConfig, agDiffState and  
         agDumpState, which use the state machine are done the resources
         used by these operations need to be freed by setting the state
         back to 'idle' so others can issue the commands via SNMP. 
         agSnmpTimeout indicates the number of minutes before the resources
         are freed and the state set back to 'idle' if this operation is not 
         performed by the user."
    ::= { agSystem 32 }

agNewCfgSnmpTimeout OBJECT-TYPE
    SYNTAX  INTEGER (1..30)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Once SNMP operations like agApplyConfig, agDiffState and  
         agDumpState, which use the state machine are done the resources
         used by these operations need to be freed by setting the state
         back to 'idle' so others can issue the commands via SNMP. 
         agSnmpTimeout indicates the number of minutes before the resources
         are freed and the state set back to 'idle' if this operation is not 
         performed by the user."
    ::= { agSystem 33 }

agCurCfgTelnetServerPort OBJECT-TYPE
    SYNTAX  INTEGER (1..65535)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The TCP port number that the telnet server listens for telnet 
         sessions."
    ::= { agSystem 34 }

agNewCfgTelnetServerPort OBJECT-TYPE
    SYNTAX  INTEGER (1..65535)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The TCP port number that the telnet server listens for telnet 
         sessions."
    ::= { agSystem 35 }

agClearFlashDump OBJECT-TYPE
    SYNTAX  INTEGER {
        ok(1),
        clear(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "This is an action object to clear the FLASH dump. 
         ok(1) is returned when this object is read. "
    ::= { agSystem 36 }

agRackId OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..127))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The rack unique identifier."
    ::= { agSystem 37 }

agChassis OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..127))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Chassis serial number."
    ::= { agSystem 38 }

agCurCfgTftpServerPort OBJECT-TYPE
    SYNTAX  INTEGER (1..65535)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The TCP port number that the TFTP server is listening to 
         in the current_configuration block."
    ::= { agSystem 39 }

agNewCfgTftpServerPort OBJECT-TYPE
    SYNTAX  INTEGER (1..65535)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The TCP port number that the TFTP server is listening to 
         in the new_configuration block."
    ::= { agSystem 40 }

agCurCfgHttpsServerPort OBJECT-TYPE
    SYNTAX  INTEGER (1..65535)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The TCP port number that the HTTPS server is listening to 
         in the current_configuration block."
    ::= { agSystem 49 }

agNewCfgHttpsServerPort OBJECT-TYPE
    SYNTAX  INTEGER (1..65535)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The TCP port number that the HTTPS server is listening to 
         in the new_configuration block."
    ::= { agSystem 50 }

agCurDaylightSavings   OBJECT-TYPE
    SYNTAX  INTEGER {
    none(0),
    africa-Algeria(1),
    africa-Angola(2),
    africa-Benin(3),
    africa-Botswana(4),
    africa-Burkina-Faso(5),
    africa-Burundi(6),
    africa-Cameroon(7),
    africa-Central-African-Rep(8),
    africa-Chad(9),
    africa-Congo-WestDemRepCongo(10),
    africa-Congo-EastDemRepCongo(11),
    africa-Congo-Rep(12),
    africa-Cote-dIvoire(13),
    africa-Djibouti(14),
    africa-Egypt(15),
    africa-Equatorial-Guinea(16),
    africa-Eritrea(17),
    africa-Ethiopia(18),
    africa-Gabon(19),
    africa-Gambia(20),
    africa-Ghana(21),
    africa-Guinea(22),
    africa-Guinea-Bissau(23),
    africa-Kenya(24),
    africa-Lesotho(25),
    africa-Liberia(26),
    africa-Libya(27),
    africa-Malawi(28),
    africa-Mali-SouthWestMali(29),
    africa-Mali-NorthEastMali(30),
    africa-Mauritania(31),
    africa-Morocco(32),
    africa-Mozambique(33),
    africa-Namibia(34),
    africa-Niger(35),
    africa-Nigeria(36),
    africa-Rwanda(37),
    africa-SaoTome-And-Principe(38),
    africa-Senegal(39),
    africa-SierraLeone(40),
    africa-Somalia(41),
    africa-SouthAfrica(42),
    africa-Spain-Mainland(43),
    africa-Spain-CeutaMelilla(44),
    africa-Spain-CanaryIslands(45),
    africa-Sudan(46), 
    africa-Swaziland(47),
    africa-Tanzania(48),
    africa-Togo(49),
    africa-Tunisia(50),
    africa-Uganda(51),
    africa-Western-Sahara(52),
    africa-Zambia(53),
    africa-Zimbabwe(54),
    americas-Anguilla(55),
    americas-Antigua-Barbuda(56),
    americas-Argentina-EArgentina(57),
    americas-Argentina-MostLocations(58),
    americas-Argentina-Jujuy(59),
    americas-Argentina-Catamarca(60),
    americas-Argentina-Mendoza(61),
    americas-Aruba(62),
    americas-Bahamas(63),
    americas-Barbados(64),
    americas-Belize(65),
    americas-Bolivia(66), 
    americas-Brazil-AtlanticIslands(67),
    americas-Brazil-AmapaEPara(68),
    americas-Brazil-NEBrazil(69),
    americas-Brazil-Pernambuco(70), 
    americas-Brazil-Tocantins(71),
    americas-Brazil-AlagoasSergipe(72),
    americas-Brazil-SSEBrazil(73),
    americas-Brazil-MatoGrossoDoSul(74),
    americas-Brazil-WParaRondonia(75),
    americas-Brazil-Roraima(76),
    americas-Brazil-EAmazonas(77),
    americas-Brazil-WAmazonas(78),
    americas-Brazil-Acre(79),
    americas-Canada-NewfoundlandIsland(80),
    americas-Canada-AtlanTime-NovaScotia(81),
    americas-Canada-AtlanTime-ELabrador(82),
    americas-Canada-EastTime-OntarioMostlocation(83),
    americas-Canada-EastTime-ThunderBay(84),
    americas-Canada-EastStdTime-PangnirtungNunavut(85),
    americas-Canada-EastStdTime-EastNunavut(86),
    americas-Canada-EastStdTime-CenNunavut(87),
    americas-Canada-CenTime-ManitobaWestOntario(88),
    americas-Canada-CenTime-RainyRiver(89),
    americas-Canada-CenTime-WestNunavut(90),
    americas-Canada-CenStdTime-SaskatchewanMostlocation(91),
    americas-Canada-CenStdTime-SaskatchewanMidwest(92),
    americas-Canada-MountTime-AlbertaEastBritishColumbia(93),
    americas-Canada-MountTime-CentralNorthwestTerritories(94),
    americas-Canada-MountTime-WestNorthwestTerritories(95),
    americas-Canada-MountStdTime-EastBritishColumbia(96),
    americas-Canada-PacificTime-WestBritishColumbia(97),
    americas-Canada-PacificTime-SouthYukon(98),
    americas-Canada-PacificTime-NorthYukon(99),
    americas-CaymanIslands(100),
    americas-Chile-MostLocation(101),
    americas-Chile-EasterIsland(102),
    americas-Colombia(103),
    americas-CostaRica(104),
    americas-Cuba(105),
    americas-Dominica(106), 
    americas-DominicanRepublic (107),
    americas-Ecuador(108),
    americas-ElSalvado(109),
    americas-FrenchGuiana(110),
    americas-Greenland-MostLocation(111),
    americas-Greenland-EastCoastNorthScoresbysund(112),
    americas-Greenland-ScoresbysundIttoqqortoormiit(113),
    americas-Greenland-ThulePituffik(114),
    americas-Grenada(115),
    americas-Guadeloupe(116),
    americas-Guatemala(117),
    americas-Guyana(118),
    americas-Haiti(119),
    americas-Honduras(120),
    americas-Jamaica(121),
    americas-Martinique(122),
    americas-Mexico-CentTime-Mostlocations(123),
    americas-Mexico-CentTime-QuintanaRoo(124),
    americas-Mexico-CentTime-CampecheYucatan(125),
    americas-Mexico-CentTime-CoahDurangoNLTamaulipas(126),
    americas-Mexico-MountTime-SBajaNayaritSinaloa(127),
    americas-Mexico-MountTime-Chihuahua(128),
    americas-Mexico-MountStdTime-Sonora(129),
    americas-Mexico-PacificTime(130),
    americas-Montserrat(131),
    americas-NetherlandsAntilles(132),
    americas-Nicaragua(133),
    americas-Panama(134),
    americas-Paraguay(135),
    americas-Peru(136),
    americas-PuertoRico(137),
    americas-StKittsAndNevis(138), 
    americas-StLucia(139),
    americas-StPierreAndMiquelon(140),
    americas-StVincent(141),
    americas-Suriname(142),
    americas-TrinidadAndTobago(143),
    americas-TurksAndCaicosIs(144),
    americas-USA-EastTime(145),
    americas-USA-EastTime-MichiganMostLocation(146),
    americas-USA-EastTime-KentuckyLouisvilleArea(147),
    americas-USA-EastTime-KentuckyWayneCounty(148),
    americas-USA-EastStdTime-IndianaMostLocations(149),
    americas-USA-EastStdTime-IndianaCrawfordCounty(150),
    americas-USA-EastStdTime-IndianaStarkeCounty(151),
    americas-USA-EastStdTime-IndianaSwitzerlandCounty(152),
    americas-USA-CentTime(153),
    americas-USA-CentTime-MichiganWisconsinborder(154),
    americas-USA-CentTime-NorthDakotaOliverCounty(155),
    americas-USA-MountTime(156),
    americas-USA-MountTime-SouthIdahoAndEastOregon(157),
    americas-USA-MountTime-Navajo(158),
    americas-USA-MountStdTime-Arizona(159),
    americas-USA-PacificTime(160),
    americas-USA-AlaskaTime(161),
    americas-USA-AlaskaTime-AlaskaPanhandle(162),
    americas-USA-AlaskaTime-AlaskaPanhandleNeck(163),
    americas-USA-AlaskaTime-WestAlaska(164),
    americas-USA-AleutianIslands(165),
    americas-USA-Hawaii(166),
    americas-Uruguay(167),
    americas-Venezuela(168),
    americas-VirginIslands-UK(169),
    americas-VirginIslands-US(170),
    antarctica-McMurdoStationRossIsland(171),
    antarctica-Amundsen-ScottStationSouthPole(172),
    antarctica-PalmerStationAnversIsland(173),
    antarctica-MawsonStationHolmeBay(174),
    antarctica-DavisStationVestfoldHills(175),
    antarctica-CaseyStationBaileyPeninsula(176),
    antarctica-VostokStationSMagneticPole(177),
    antarctica-Dumont-dUrvilleBaseTerreAdelie(178), 
    antarctica-SyowaStationEOngulI(179),
    arcticOcean-Svalbard(180),
    arcticOcean-JanMayen(181),
    asia-Afghanistan(182),
    asia-Armenia(183),
    asia-Azerbaijan(184),
    asia-Bahrain(185),
    asia-Bangladesh(186),
    asia-Bhutan(187),
    asia-Brunei(188),
    asia-Cambodia(189),
    asia-China-EastChinaBeijingGuangdongShanghai(190),
    asia-China-Heilongjiang(191),
    asia-China-CentralChinaGansuGuizhouSichuanYunnan(192),
    asia-China-TibetmostofXinjiangUyghur(193),
    asia-China-SouthwestXinjiangUyghur(194),
    asia-Cyprus(195),
    asia-EastTimor(196), 
    asia-Georgia(197),
    asia-HongKong(198),
    asia-India(199),
    asia-Indonesia-JavaAndSumatra(200),
    asia-Indonesia-WestCentralBorneo(201),
    asia-Indonesia-EastSouthBorneoBaliWestTimor(202),
    asia-Indonesia-IrianJayaAndMoluccas(203),
    asia-Iran(204),
    asia-Iraq(205),
    asia-Israel(206),
    asia-Japan(207),
    asia-Jordan(208),
    asia-Kazakhstan-MostLocations(209),
    asia-Kazakhstan-QyzylordaKyzylorda(210),
    asia-Kazakhstan-Aqtobe(211),
    asia-Kazakhstan-AtyrauMangghystau(212),
    asia-Kazakhstan-WestKazakhstan(213),
    asia-Korea-North(214),
    asia-Korea-South(215),
    asia-Kuwait(216),
    asia-Kyrgyzstan(217), 
    asia-Laos(218),
    asia-Lebanon(219),
    asia-Macau(220),
    asia-Malaysia-PeninsularMalaysia(221),
    asia-Malaysia-SabahSarawak(222),
    asia-Mongolia-MostLocations(223),
    asia-Mongolia-BayanOlgiyGoviAltaiHovdUvsZavkhan(224),
    asia-Mongolia-DornodSukhbaatar(225),
    asia-Myanmar(226),
    asia-Nepal(227),
    asia-Oman(228),
    asia-Pakistan(229), 
    asia-Palestine(230),
    asia-Philippines(231),
    asia-Qatar(232),
    asia-Russia-Moscow-01Kaliningrad(233),
    asia-Russia-Moscow00WestRussia(234),
    asia-Russia-Moscow01CaspianSea(235),
    asia-Russia-Moscow02Urals(236),
    asia-Russia-Moscow03WestSiberia(237),
    asia-Russia-Moscow03Novosibirsk(238),
    asia-Russia-Moscow04YeniseiRiver(239),
    asia-Russia-Moscow05LakeBaikal(240),
    asia-Russia-Moscow06LenaRiver(241),
    asia-Russia-Moscow07AmurRiver(242),
    asia-Russia-Moscow07SakhalinIsland(243),
    asia-Russia-Moscow08Magadan(244),
    asia-Russia-Moscow09Kamchatka(245),
    asia-Russia-Moscow10BeringSea(246),
    asia-SaudiArabia(247),
    asia-Singapore(248),
    asia-SriLanka(249),
    asia-Syria(250),
    asia-Taiwan(251),
    asia-Tajikistan(252), 
    asia-Thailand(253),
    asia-Turkmenistan(254), 
    asia-UnitedArabEmirates(255),
    asia-Uzbekistan-WestUzbekistan(256),
    asia-Uzbekistan-EastUzbekistan(257),
    asia-Vietnam(258),
    asia-Yemen(259),
    atlanticOcean-Bermuda(260),
    atlanticOcean-CapeVerde(261),
    atlanticOcean-FaeroeIslands(262),
    atlanticOcean-FalklandIslands(263),
    atlanticOcean-Iceland(264),
    atlanticOcean-Portugal-Mainland(265),
    atlanticOcean-Portugal-MadeiraIslands(266),
    atlanticOcean-Portugal-Azores(267),
    atlanticOcean-SouthGeorgia-SouthSandwichIslands(268),
    atlanticOcean-Spain-Mainland(269),
    atlanticOcean-Spain-CeutaMelilla(270),
    atlanticOcean-Spain-CanaryIslands(271),
    atlanticOcean-StHelena(272),
    atlanticOcean-Svalbard-JanMayen(273),
    australia-LordHoweIsland(274),
    australia-Tasmania(275),
    australia-Victoria(276),
    australia-NewSouthWales-MostLocations(277),
    australia-NewSouthWales-Yancowinna(278),
    australia-Queensland-MostLocations(279),
    australia-Queensland-HolidayIslands(280),
    australia-SouthAustralia(281),
    australia-NorthernTerritory(282),
    australia-WesternAustralia(283),
    europe-Albania(284),
    europe-Andorra(285),
    europe-Austria(286),
    europe-Belarus(287),
    europe-Belgium(288),
    europe-BosniaHerzegovina(289),
    europe-Britain-UKGreatBritain(290),
    europe-Britain-UKNorthernIreland(291),
    europe-Bulgaria(292),
    europe-Croatia(293),
    europe-CzechRepublic(294),
    europe-Denmark(295),
    europe-Estonia(296),
    europe-Finland(297),
    europe-France(298), 
    europe-Germany(299),
    europe-Gibraltar(300),
    europe-Greece(301),
    europe-Hungary(302),
    europe-Ireland(303),
    europe-Italy(304),
    europe-Latvia(305),
    europe-Liechtenstein(306),
    europe-Lithuania(307),
    europe-Luxembourg(308),
    europe-Macedonia(309),
    europe-Malta(310),
    europe-Moldova(311),
    europe-Monaco(312),
    europe-Netherlands(313),
    europe-Norway(314),
    europe-Poland(315),
    europe-Portugal-Mainland(316),
    europe-Portugal-MadeiraIslands(317),
    europe-Portugal-Azores(318),
    europe-Romania(319),
    europe-Russia-Moscow-01Kaliningrad(320),
    europe-Russia-Moscow00WestRussia(321),
    europe-Russia-Moscow01CaspianSea(322),
    europe-Russia-Moscow02Urals(323),
    europe-Russia-Moscow03WestSiberia(324),
    europe-Russia-Moscow03Novosibirsk(325),
    europe-Russia-Moscow04YeniseiRiver(326),
    europe-Russia-Moscow05LakeBaikal(327),
    europe-Russia-Moscow06LenaRiver(328),
    europe-Russia-Moscow07AmurRiver(329),
    europe-Russia-Moscow07SakhalinIsland(330),
    europe-Russia-Moscow08Magadan(331),
    europe-Russia-Moscow09Kamchatka(332),
    europe-Russia-Moscow10BeringSea(333),
    europe-SanMarino(334),
    europe-Slovakia(335),
    europe-Slovenia(336),
    europe-Spain-Mainland(337),
    europe-Spain-CeutaAndMelilla(338),
    europe-Spain-CanaryIslands(339),
    europe-Sweden(340),
    europe-Switzerland(341),
    europe-Turkey(342),
    europe-Ukraine-MostLocations(343),
    europe-Ukraine-Ruthenia(344),
    europe-Ukraine-Zaporozhye-ELugansk(345),
    europe-Ukraine-CentralCrimea(346),
    europe-VaticanCity(347),
    europe-Yugoslavia(348),
    indianOcean-BritishIndianOceanTerritory(349),
    indianOcean-ChristmasIsland(350),
    indianOcean-CocosOrKeelingIslands(351),
    indianOcean-Comoros(352),
    indianOcean-FrenchSouthernAndAntarcticLands(353),
    indianOcean-Madagascar(354),
    indianOcean-Maldives(355),
    indianOcean-Mauritius(356),
    indianOcean-Mayotte(357),
    indianOcean-Reunion(358),
    indianOcean-Seychelles(359),
    pacificOcean-Chile-MostLocations(360),
    pacificOcean-Chile-EasterIslandSalayGomez(361),
    pacificOcean-CookIslands(362),
    pacificOcean-Ecuador(363),
    pacificOcean-Fiji(364),
    pacificOcean-FrenchPolynesia-SocietyIslands(365),
    pacificOcean-FrenchPolynesia-MarquesasIslands(366),
    pacificOcean-FrenchPolynesia-GambierIslands(367),
    pacificOcean-Guam(368),
    pacificOcean-Kiribati-GilbertIslands(369),
    pacificOcean-Kiribati-PhoenixIslands(370),
    pacificOcean-Kiribati-LineIslands(371),
    pacificOcean-MarshallIslands-MostLocations(372),
    pacificOcean-MarshallIslands-Kwajalein(373),
    pacificOcean-Micronesia-Yap(374),
    pacificOcean-Micronesia-TrukOrChuuk(375),
    pacificOcean-Micronesia-PonapeOrPohnpei(376), 
    pacificOcean-Micronesia-Kosrae(377),
    pacificOcean-Nauru(378),
    pacificOcean-NewCaledonia(379),
    pacificOcean-NewZealand-MostLocations(380),
    pacificOcean-NewZealand-ChathamIslands(381),
    pacificOcean-Niue(382),
    pacificOcean-NorfolkIsland(383),
    pacificOcean-NorthernMarianaIslands(384),
    pacificOcean-Palau(385),
    pacificOcean-PapuaNewGuinea(386),
    pacificOcean-Pitcairn(387),
    pacificOcean-SamoaAmerican(388),
    pacificOcean-SamoaWestern(389),
    pacificOcean-SolomonIslands(390),
    pacificOcean-Tokelau(391),
    pacificOcean-Tonga(392),
    pacificOcean-Tuvalu(393),
    pacificOceanUSA-EastTime(394),
    pacificOceanUSA-EastTime-MichiganMostLocations(395),
    pacificOceanUSA-EastTime-KentuckyLouisvilleArea(396),
    pacificOceanUSA-EastTime-KentuckyWayneCounty(397),
    pacificOceanUSA-EastStdTime-IndianaMostLocations(398),
    pacificOceanUSA-EastStdTime-IndianaCrawfordCounty(399),
    pacificOceanUSA-EastStdTime-IndianaStarkeCounty(400),
    pacificOceanUSA-EastStdTime-IndianaSwitzerlandCounty(401),
    pacificOceanUSA-CentTime(402),
    pacificOceanUSA-CentTime-MichiganWisconsinborder(403),
    pacificOceanUSA-CentTime-NorthDakotaOliverCounty(404),
    pacificOceanUSA-MountTime(405),
    pacificOceanUSA-MountTime-SouthIdahoAndEastOregon(406),
    pacificOceanUSA-MountTime-Navajo(407),
    pacificOceanUSA-MountStdTime-Arizona(408),
    pacificOceanUSA-PacificTime(409),
    pacificOceanUSA-AlaskaTime(410),
    pacificOceanUSA-AlaskaTime-AlaskaPanhandle(411),
    pacificOceanUSA-AlaskaTime-AlaskaPanhandleNeck(412),
    pacificOceanUSA-AlaskaTime-WestAlaska(413),
    pacificOceanUSA-AleutianIslands(414),
    pacificOceanUSA-Hawaii(415),
    pacificOcean-USMinorOutlyingIslands-JohnstonAtoll(416),
    pacificOcean-USMinorOutlyingIslands-MidwayIslands(417),
    pacificOcean-USMinorOutlyingIslands-WakeIsland(418),
    pacificOcean-Vanuatu(419),
    pacificOcean-WallisAndFutuna(420)
	}
    MAX-ACCESS read-only 
    STATUS  current 
    DESCRIPTION
        "The daylight savings location."
    ::= { agSystem 51 }

agNewDaylightSavings   OBJECT-TYPE
    SYNTAX  INTEGER  {
    none(0),
    africa-Algeria(1),
    africa-Angola(2),
    africa-Benin(3),
    africa-Botswana(4),
    africa-Burkina-Faso(5),
    africa-Burundi(6),
    africa-Cameroon(7),
    africa-Central-African-Rep(8),
    africa-Chad(9),
    africa-Congo-WestDemRepCongo(10),
    africa-Congo-EastDemRepCongo(11),
    africa-Congo-Rep(12),
    africa-Cote-dIvoire(13),
    africa-Djibouti(14),
    africa-Egypt(15),
    africa-Equatorial-Guinea(16),
    africa-Eritrea(17),
    africa-Ethiopia(18),
    africa-Gabon(19),
    africa-Gambia(20),
    africa-Ghana(21),
    africa-Guinea(22),
    africa-Guinea-Bissau(23),
    africa-Kenya(24),
    africa-Lesotho(25),
    africa-Liberia(26),
    africa-Libya(27),
    africa-Malawi(28),
    africa-Mali-SouthWestMali(29),
    africa-Mali-NorthEastMali(30),
    africa-Mauritania(31),
    africa-Morocco(32),
    africa-Mozambique(33),
    africa-Namibia(34),
    africa-Niger(35),
    africa-Nigeria(36),
    africa-Rwanda(37),
    africa-SaoTome-And-Principe(38),
    africa-Senegal(39),
    africa-SierraLeone(40),
    africa-Somalia(41),
    africa-SouthAfrica(42),
    africa-Spain-Mainland(43),
    africa-Spain-CeutaMelilla(44),
    africa-Spain-CanaryIslands(45),
    africa-Sudan(46), 
    africa-Swaziland(47),
    africa-Tanzania(48),
    africa-Togo(49),
    africa-Tunisia(50),
    africa-Uganda(51),
    africa-Western-Sahara(52),
    africa-Zambia(53),
    africa-Zimbabwe(54),
    americas-Anguilla(55),
    americas-Antigua-Barbuda(56),
    americas-Argentina-EArgentina(57),
    americas-Argentina-MostLocations(58),
    americas-Argentina-Jujuy(59),
    americas-Argentina-Catamarca(60),
    americas-Argentina-Mendoza(61),
    americas-Aruba(62),
    americas-Bahamas(63),
    americas-Barbados(64),
    americas-Belize(65),
    americas-Bolivia(66), 
    americas-Brazil-AtlanticIslands(67),
    americas-Brazil-AmapaEPara(68),
    americas-Brazil-NEBrazil(69),
    americas-Brazil-Pernambuco(70), 
    americas-Brazil-Tocantins(71),
    americas-Brazil-AlagoasSergipe(72),
    americas-Brazil-SSEBrazil(73),
    americas-Brazil-MatoGrossoDoSul(74),
    americas-Brazil-WParaRondonia(75),
    americas-Brazil-Roraima(76),
    americas-Brazil-EAmazonas(77),
    americas-Brazil-WAmazonas(78),
    americas-Brazil-Acre(79),
    americas-Canada-NewfoundlandIsland(80),
    americas-Canada-AtlanTime-NovaScotia(81),
    americas-Canada-AtlanTime-ELabrador(82),
    americas-Canada-EastTime-OntarioMostlocation(83),
    americas-Canada-EastTime-ThunderBay(84),
    americas-Canada-EastStdTime-PangnirtungNunavut(85),
    americas-Canada-EastStdTime-EastNunavut(86),
    americas-Canada-EastStdTime-CenNunavut(87),
    americas-Canada-CenTime-ManitobaWestOntario(88),
    americas-Canada-CenTime-RainyRiver(89),
    americas-Canada-CenTime-WestNunavut(90),
    americas-Canada-CenStdTime-SaskatchewanMostlocation(91),
    americas-Canada-CenStdTime-SaskatchewanMidwest(92),
    americas-Canada-MountTime-AlbertaEastBritishColumbia(93),
    americas-Canada-MountTime-CentralNorthwestTerritories(94),
    americas-Canada-MountTime-WestNorthwestTerritories(95),
    americas-Canada-MountStdTime-EastBritishColumbia(96),
    americas-Canada-PacificTime-WestBritishColumbia(97),
    americas-Canada-PacificTime-SouthYukon(98),
    americas-Canada-PacificTime-NorthYukon(99),
    americas-CaymanIslands(100),
    americas-Chile-MostLocation(101),
    americas-Chile-EasterIsland(102),
    americas-Colombia(103),
    americas-CostaRica(104),
    americas-Cuba(105),
    americas-Dominica(106), 
    americas-DominicanRepublic (107),
    americas-Ecuador(108),
    americas-ElSalvado(109),
    americas-FrenchGuiana(110),
    americas-Greenland-MostLocation(111),
    americas-Greenland-EastCoastNorthScoresbysund(112),
    americas-Greenland-ScoresbysundIttoqqortoormiit(113),
    americas-Greenland-ThulePituffik(114),
    americas-Grenada(115),
    americas-Guadeloupe(116),
    americas-Guatemala(117),
    americas-Guyana(118),
    americas-Haiti(119),
    americas-Honduras(120),
    americas-Jamaica(121),
    americas-Martinique(122),
    americas-Mexico-CentTime-Mostlocations(123),
    americas-Mexico-CentTime-QuintanaRoo(124),
    americas-Mexico-CentTime-CampecheYucatan(125),
    americas-Mexico-CentTime-CoahDurangoNLTamaulipas(126),
    americas-Mexico-MountTime-SBajaNayaritSinaloa(127),
    americas-Mexico-MountTime-Chihuahua(128),
    americas-Mexico-MountStdTime-Sonora(129),
    americas-Mexico-PacificTime(130),
    americas-Montserrat(131),
    americas-NetherlandsAntilles(132),
    americas-Nicaragua(133),
    americas-Panama(134),
    americas-Paraguay(135),
    americas-Peru(136),
    americas-PuertoRico(137),
    americas-StKittsAndNevis(138), 
    americas-StLucia(139),
    americas-StPierreAndMiquelon(140),
    americas-StVincent(141),
    americas-Suriname(142),
    americas-TrinidadAndTobago(143),
    americas-TurksAndCaicosIs(144),
    americas-USA-EastTime(145),
    americas-USA-EastTime-MichiganMostLocation(146),
    americas-USA-EastTime-KentuckyLouisvilleArea(147),
    americas-USA-EastTime-KentuckyWayneCounty(148),
    americas-USA-EastStdTime-IndianaMostLocations(149),
    americas-USA-EastStdTime-IndianaCrawfordCounty(150),
    americas-USA-EastStdTime-IndianaStarkeCounty(151),
    americas-USA-EastStdTime-IndianaSwitzerlandCounty(152),
    americas-USA-CentTime(153),
    americas-USA-CentTime-MichiganWisconsinborder(154),
    americas-USA-CentTime-NorthDakotaOliverCounty(155),
    americas-USA-MountTime(156),
    americas-USA-MountTime-SouthIdahoAndEastOregon(157),
    americas-USA-MountTime-Navajo(158),
    americas-USA-MountStdTime-Arizona(159),
    americas-USA-PacificTime(160),
    americas-USA-AlaskaTime(161),
    americas-USA-AlaskaTime-AlaskaPanhandle(162),
    americas-USA-AlaskaTime-AlaskaPanhandleNeck(163),
    americas-USA-AlaskaTime-WestAlaska(164),
    americas-USA-AleutianIslands(165),
    americas-USA-Hawaii(166),
    americas-Uruguay(167),
    americas-Venezuela(168),
    americas-VirginIslands-UK(169),
    americas-VirginIslands-US(170),
    antarctica-McMurdoStationRossIsland(171),
    antarctica-Amundsen-ScottStationSouthPole(172),
    antarctica-PalmerStationAnversIsland(173),
    antarctica-MawsonStationHolmeBay(174),
    antarctica-DavisStationVestfoldHills(175),
    antarctica-CaseyStationBaileyPeninsula(176),
    antarctica-VostokStationSMagneticPole(177),
    antarctica-Dumont-dUrvilleBaseTerreAdelie(178), 
    antarctica-SyowaStationEOngulI(179),
    arcticOcean-Svalbard(180),
    arcticOcean-JanMayen(181),
    asia-Afghanistan(182),
    asia-Armenia(183),
    asia-Azerbaijan(184),
    asia-Bahrain(185),
    asia-Bangladesh(186),
    asia-Bhutan(187),
    asia-Brunei(188),
    asia-Cambodia(189),
    asia-China-EastChinaBeijingGuangdongShanghai(190),
    asia-China-Heilongjiang(191),
    asia-China-CentralChinaGansuGuizhouSichuanYunnan(192),
    asia-China-TibetmostofXinjiangUyghur(193),
    asia-China-SouthwestXinjiangUyghur(194),
    asia-Cyprus(195),
    asia-EastTimor(196), 
    asia-Georgia(197),
    asia-HongKong(198),
    asia-India(199),
    asia-Indonesia-JavaAndSumatra(200),
    asia-Indonesia-WestCentralBorneo(201),
    asia-Indonesia-EastSouthBorneoBaliWestTimor(202),
    asia-Indonesia-IrianJayaAndMoluccas(203),
    asia-Iran(204),
    asia-Iraq(205),
    asia-Israel(206),
    asia-Japan(207),
    asia-Jordan(208),
    asia-Kazakhstan-MostLocations(209),
    asia-Kazakhstan-QyzylordaKyzylorda(210),
    asia-Kazakhstan-Aqtobe(211),
    asia-Kazakhstan-AtyrauMangghystau(212),
    asia-Kazakhstan-WestKazakhstan(213),
    asia-Korea-North(214),
    asia-Korea-South(215),
    asia-Kuwait(216),
    asia-Kyrgyzstan(217), 
    asia-Laos(218),
    asia-Lebanon(219),
    asia-Macau(220),
    asia-Malaysia-PeninsularMalaysia(221),
    asia-Malaysia-SabahSarawak(222),
    asia-Mongolia-MostLocations(223),
    asia-Mongolia-BayanOlgiyGoviAltaiHovdUvsZavkhan(224),
    asia-Mongolia-DornodSukhbaatar(225),
    asia-Myanmar(226),
    asia-Nepal(227),
    asia-Oman(228),
    asia-Pakistan(229), 
    asia-Palestine(230),
    asia-Philippines(231),
    asia-Qatar(232),
    asia-Russia-Moscow-01Kaliningrad(233),
    asia-Russia-Moscow00WestRussia(234),
    asia-Russia-Moscow01CaspianSea(235),
    asia-Russia-Moscow02Urals(236),
    asia-Russia-Moscow03WestSiberia(237),
    asia-Russia-Moscow03Novosibirsk(238),
    asia-Russia-Moscow04YeniseiRiver(239),
    asia-Russia-Moscow05LakeBaikal(240),
    asia-Russia-Moscow06LenaRiver(241),
    asia-Russia-Moscow07AmurRiver(242),
    asia-Russia-Moscow07SakhalinIsland(243),
    asia-Russia-Moscow08Magadan(244),
    asia-Russia-Moscow09Kamchatka(245),
    asia-Russia-Moscow10BeringSea(246),
    asia-SaudiArabia(247),
    asia-Singapore(248),
    asia-SriLanka(249),
    asia-Syria(250),
    asia-Taiwan(251),
    asia-Tajikistan(252), 
    asia-Thailand(253),
    asia-Turkmenistan(254), 
    asia-UnitedArabEmirates(255),
    asia-Uzbekistan-WestUzbekistan(256),
    asia-Uzbekistan-EastUzbekistan(257),
    asia-Vietnam(258),
    asia-Yemen(259),
    atlanticOcean-Bermuda(260),
    atlanticOcean-CapeVerde(261),
    atlanticOcean-FaeroeIslands(262),
    atlanticOcean-FalklandIslands(263),
    atlanticOcean-Iceland(264),
    atlanticOcean-Portugal-Mainland(265),
    atlanticOcean-Portugal-MadeiraIslands(266),
    atlanticOcean-Portugal-Azores(267),
    atlanticOcean-SouthGeorgia-SouthSandwichIslands(268),
    atlanticOcean-Spain-Mainland(269),
    atlanticOcean-Spain-CeutaMelilla(270),
    atlanticOcean-Spain-CanaryIslands(271),
    atlanticOcean-StHelena(272),
    atlanticOcean-Svalbard-JanMayen(273),
    australia-LordHoweIsland(274),
    australia-Tasmania(275),
    australia-Victoria(276),
    australia-NewSouthWales-MostLocations(277),
    australia-NewSouthWales-Yancowinna(278),
    australia-Queensland-MostLocations(279),
    australia-Queensland-HolidayIslands(280),
    australia-SouthAustralia(281),
    australia-NorthernTerritory(282),
    australia-WesternAustralia(283),
    europe-Albania(284),
    europe-Andorra(285),
    europe-Austria(286),
    europe-Belarus(287),
    europe-Belgium(288),
    europe-BosniaHerzegovina(289),
    europe-Britain-UKGreatBritain(290),
    europe-Britain-UKNorthernIreland(291),
    europe-Bulgaria(292),
    europe-Croatia(293),
    europe-CzechRepublic(294),
    europe-Denmark(295),
    europe-Estonia(296),
    europe-Finland(297),
    europe-France(298), 
    europe-Germany(299),
    europe-Gibraltar(300),
    europe-Greece(301),
    europe-Hungary(302),
    europe-Ireland(303),
    europe-Italy(304),
    europe-Latvia(305),
    europe-Liechtenstein(306),
    europe-Lithuania(307),
    europe-Luxembourg(308),
    europe-Macedonia(309),
    europe-Malta(310),
    europe-Moldova(311),
    europe-Monaco(312),
    europe-Netherlands(313),
    europe-Norway(314),
    europe-Poland(315),
    europe-Portugal-Mainland(316),
    europe-Portugal-MadeiraIslands(317),
    europe-Portugal-Azores(318),
    europe-Romania(319),
    europe-Russia-Moscow-01Kaliningrad(320),
    europe-Russia-Moscow00WestRussia(321),
    europe-Russia-Moscow01CaspianSea(322),
    europe-Russia-Moscow02Urals(323),
    europe-Russia-Moscow03WestSiberia(324),
    europe-Russia-Moscow03Novosibirsk(325),
    europe-Russia-Moscow04YeniseiRiver(326),
    europe-Russia-Moscow05LakeBaikal(327),
    europe-Russia-Moscow06LenaRiver(328),
    europe-Russia-Moscow07AmurRiver(329),
    europe-Russia-Moscow07SakhalinIsland(330),
    europe-Russia-Moscow08Magadan(331),
    europe-Russia-Moscow09Kamchatka(332),
    europe-Russia-Moscow10BeringSea(333),
    europe-SanMarino(334),
    europe-Slovakia(335),
    europe-Slovenia(336),
    europe-Spain-Mainland(337),
    europe-Spain-CeutaAndMelilla(338),
    europe-Spain-CanaryIslands(339),
    europe-Sweden(340),
    europe-Switzerland(341),
    europe-Turkey(342),
    europe-Ukraine-MostLocations(343),
    europe-Ukraine-Ruthenia(344),
    europe-Ukraine-Zaporozhye-ELugansk(345),
    europe-Ukraine-CentralCrimea(346),
    europe-VaticanCity(347),
    europe-Yugoslavia(348),
    indianOcean-BritishIndianOceanTerritory(349),
    indianOcean-ChristmasIsland(350),
    indianOcean-CocosOrKeelingIslands(351),
    indianOcean-Comoros(352),
    indianOcean-FrenchSouthernAndAntarcticLands(353),
    indianOcean-Madagascar(354),
    indianOcean-Maldives(355),
    indianOcean-Mauritius(356),
    indianOcean-Mayotte(357),
    indianOcean-Reunion(358),
    indianOcean-Seychelles(359),
    pacificOcean-Chile-MostLocations(360),
    pacificOcean-Chile-EasterIslandSalayGomez(361),
    pacificOcean-CookIslands(362),
    pacificOcean-Ecuador(363),
    pacificOcean-Fiji(364),
    pacificOcean-FrenchPolynesia-SocietyIslands(365),
    pacificOcean-FrenchPolynesia-MarquesasIslands(366),
    pacificOcean-FrenchPolynesia-GambierIslands(367),
    pacificOcean-Guam(368),
    pacificOcean-Kiribati-GilbertIslands(369),
    pacificOcean-Kiribati-PhoenixIslands(370),
    pacificOcean-Kiribati-LineIslands(371),
    pacificOcean-MarshallIslands-MostLocations(372),
    pacificOcean-MarshallIslands-Kwajalein(373),
    pacificOcean-Micronesia-Yap(374),
    pacificOcean-Micronesia-TrukOrChuuk(375),
    pacificOcean-Micronesia-PonapeOrPohnpei(376), 
    pacificOcean-Micronesia-Kosrae(377),
    pacificOcean-Nauru(378),
    pacificOcean-NewCaledonia(379),
    pacificOcean-NewZealand-MostLocations(380),
    pacificOcean-NewZealand-ChathamIslands(381),
    pacificOcean-Niue(382),
    pacificOcean-NorfolkIsland(383),
    pacificOcean-NorthernMarianaIslands(384),
    pacificOcean-Palau(385),
    pacificOcean-PapuaNewGuinea(386),
    pacificOcean-Pitcairn(387),
    pacificOcean-SamoaAmerican(388),
    pacificOcean-SamoaWestern(389),
    pacificOcean-SolomonIslands(390),
    pacificOcean-Tokelau(391),
    pacificOcean-Tonga(392),
    pacificOcean-Tuvalu(393),
    pacificOceanUSA-EastTime(394),
    pacificOceanUSA-EastTime-MichiganMostLocations(395),
    pacificOceanUSA-EastTime-KentuckyLouisvilleArea(396),
    pacificOceanUSA-EastTime-KentuckyWayneCounty(397),
    pacificOceanUSA-EastStdTime-IndianaMostLocations(398),
    pacificOceanUSA-EastStdTime-IndianaCrawfordCounty(399),
    pacificOceanUSA-EastStdTime-IndianaStarkeCounty(400),
    pacificOceanUSA-EastStdTime-IndianaSwitzerlandCounty(401),
    pacificOceanUSA-CentTime(402),
    pacificOceanUSA-CentTime-MichiganWisconsinborder(403),
    pacificOceanUSA-CentTime-NorthDakotaOliverCounty(404),
    pacificOceanUSA-MountTime(405),
    pacificOceanUSA-MountTime-SouthIdahoAndEastOregon(406),
    pacificOceanUSA-MountTime-Navajo(407),
    pacificOceanUSA-MountStdTime-Arizona(408),
    pacificOceanUSA-PacificTime(409),
    pacificOceanUSA-AlaskaTime(410),
    pacificOceanUSA-AlaskaTime-AlaskaPanhandle(411),
    pacificOceanUSA-AlaskaTime-AlaskaPanhandleNeck(412),
    pacificOceanUSA-AlaskaTime-WestAlaska(413),
    pacificOceanUSA-AleutianIslands(414),
    pacificOceanUSA-Hawaii(415),
    pacificOcean-USMinorOutlyingIslands-JohnstonAtoll(416),
    pacificOcean-USMinorOutlyingIslands-MidwayIslands(417),
    pacificOcean-USMinorOutlyingIslands-WakeIsland(418),
    pacificOcean-Vanuatu(419),
    pacificOceanWallisAndFutuna(420)
	}
    MAX-ACCESS read-write 
    STATUS  current 
    DESCRIPTION
        "The daylight savings location."
    ::= { agSystem 52 }


agCfgSysDlight OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable/disable daylight savings time."
    ::= { agSystem 53 }


agCurCfgIdleCLITimeout OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Set idle CLI sessions timeout."
    ::= { agSystem 55 }

agNewCfgIdleCLITimeout OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Set idle CLI sessions timeout."
    ::= { agSystem 56 }

agCurCfgUfdTrap OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(2),
        disabled(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The current status of the UFDFO SNMP trap."
    ::= { agSystem 57 }

agNewCfgUfdTrap OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(2),
        disabled(3)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable sending UFDFO SNMP trap."
    ::= { agSystem 58 }

agCurCfgReminders OBJECT-TYPE
    SYNTAX  INTEGER {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Current status of reminders feature."
    ::= { agSystem 59 }

agNewCfgReminders OBJECT-TYPE
    SYNTAX  INTEGER {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable reminders feature."
    ::= { agSystem 60 }


agCurBootNxtCliMode OBJECT-TYPE
    SYNTAX  INTEGER {
        aoscli(1),
        iscli(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Current boot mode."
    ::= { agSystem 66 }

agNewBootNxtCliMode OBJECT-TYPE
    SYNTAX  INTEGER {
        aoscli(1),
        iscli(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Next cli boot mode."
    ::= { agSystem 67 }

agCurBootNxtCliModePrompt OBJECT-TYPE
    SYNTAX  INTEGER {
        disable(1),
        enable(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Current status of selectable CLI mode prompt."
    ::= { agSystem 78 }

agNewBootNxtCliModePrompt OBJECT-TYPE
    SYNTAX  INTEGER {
        disable(1),
        enable(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Next status of selectable CLI mode prompt."
    ::= { agSystem 79 }

agCurCfgDhcp OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable the use of DHCP, as currently configured in the 
         current_configuration block."
    ::= { agSystem 70 }

agNewCfgDhcp OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable the use of DHCP, in the new_configuration block."
    ::= { agSystem 71 }


agCurCfgHprompt OBJECT-TYPE
    SYNTAX  INTEGER {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Current status of hprompt."
    ::= { agSystem 73 }

agNewCfgHprompt OBJECT-TYPE
    SYNTAX  INTEGER {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "New status of hpprompt."
    ::= { agSystem 75 }

agCurCfgLoginNotice OBJECT-TYPE
    SYNTAX  DisplayString 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The user defined login notice."
    ::= { agSystem 76 }

agNewCfgLoginNotice OBJECT-TYPE
    SYNTAX  DisplayString
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The user defined login notice."
    ::= { agSystem 77 }

agCurCfgOldDst OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable system DST for US."
    ::= { agSystem 82 }

agNewCfgOldDst OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable system DST for US."
    ::= { agSystem 83 }

agHavePanicDump OBJECT-TYPE
    SYNTAX  INTEGER {
        havePanic(1),
        noHavePanic(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This object, when read, gives the user the information
         whether a panic dump exist in flash."
    ::= { agSystem 84 }

-- Syslog Configuration
agCurCfgSyslogHost OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The syslog host IP address, as currently configured in
         the current_configuration block."
    ::= { agSyslog 1 }

agNewCfgSyslogHost OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The syslog host IP address, in the new_configuration block."
    ::= { agSyslog 2 }

agCurCfgSyslog2Host OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The second syslog host IP address, as currently configured in
         the current_configuration block."
    ::= { agSyslog 3 }

agNewCfgSyslog2Host OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The second syslog host IP address, in the new_configuration block."
    ::= { agSyslog 4 }

agCurCfgSyslogFac   OBJECT-TYPE
    SYNTAX  INTEGER  {
	local0(1),
	local1(2),
	local2(3),
	local3(4),
	local4(5),
	local5(6),
	local6(7),
	local7(8)
	}
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The facility of syslog host in the current_configuration block."
    ::= { agSyslog 5 }

agNewCfgSyslogFac   OBJECT-TYPE
    SYNTAX  INTEGER  {
	local0(1), 
	local1(2),
	local2(3),
	local3(4),
	local4(5),
	local5(6),
        local6(7),
	local7(8)
	}
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The facility of syslog host in the new_configuration block."
    ::= { agSyslog 6 }

agCurCfgSyslog2Fac   OBJECT-TYPE
    SYNTAX  INTEGER  {
	local0(1),
	local1(2),
	local2(3),
	local3(4),
	local4(5),
	local5(6),
	local6(7),
	local7(8)
	}
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The facility of syslog2 host in the current_configuration block."
    ::= { agSyslog 7 }

agNewCfgSyslog2Fac   OBJECT-TYPE
    SYNTAX  INTEGER  {
	local0(1), 
	local1(2),
	local2(3),
	local3(4),
        local4(5),
	local5(6),
        local6(7),
	local7(8)
	}
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The facility of syslogs host in the new_configuration block."
    ::= { agSyslog 8 }

agCurCfgSyslogSev   OBJECT-TYPE
    SYNTAX  INTEGER  {
        emerg0(1),
	alert1(2),
	crit2(3),
	err3(4),
	warning4(5),
	notice5(6),
	info6(7),
	debug7(8)
	}
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The severity of syslog host in the current configuration block."
    ::= { agSyslog 13 }

agNewCfgSyslogSev   OBJECT-TYPE
    SYNTAX  INTEGER  {
        emerg0(1),
	alert1(2),
	crit2(3),
	err3(4),
	warning4(5),
	notice5(6),
	info6(7),
	debug7(8)
	}
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The severity of syslog host in the new configuration block."
    ::= { agSyslog 14 }

agCurCfgSyslog2Sev   OBJECT-TYPE
    SYNTAX  INTEGER  {
        emerg0(1),
	alert1(2),
	crit2(3),
	err3(4),
	warning4(5),
	notice5(6),
	info6(7),
	debug7(8)
	}
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The severity of syslog2 host in the current configuration block."
    ::= { agSyslog 15 }

agNewCfgSyslog2Sev   OBJECT-TYPE
    SYNTAX  INTEGER  {
        emerg0(1),
	alert1(2),
	crit2(3),
	err3(4),
	warning4(5),
	notice5(6),
	info6(7),
	debug7(8)
	}
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The severity of syslogs host in the new configuration block."
    ::= { agSyslog 16 }


agClrSyslogMsgs OBJECT-TYPE
    SYNTAX  INTEGER {
            other(1),
            reset(2)
            }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Clears all current Syslog messages."
    ::= { agSyslog 9 }

agSyslogMsgTableMaxSize OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum number of rows in the syslog message table."
    ::= { agSyslog 10 }

agSyslogMsgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF AgSyslogMsgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of syslog messages."
    ::= { agSyslog 11 }

agSyslogMsgTableEntry OBJECT-TYPE
    SYNTAX  AgSyslogMsgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A syslog message stored on the switch."
    INDEX   { agSyslogMsgIndex }
    ::= { agSyslogMsgTable 1 }

AgSyslogMsgTableEntry ::= SEQUENCE {
    agSyslogMsgIndex          Integer32,
    agSyslogMessage           DisplayString
    }

agSyslogMsgIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The syslog message table index."
    ::= { agSyslogMsgTableEntry 1 }

agSyslogMessage OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The syslog message."
    ::= { agSyslogMsgTableEntry 2 }

agLog OBJECT IDENTIFIER ::= { agSyslog 12 }

agNewCfgSyslogTrapConsole OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable console syslog and SNMP trap, in the 
         new_configuration block."
    ::= { agLog 1 }

agCurCfgSyslogTrapConsole OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable console syslog and SNMP trap, as currently 
         configured in the current_configuration block."
    ::= { agLog 2 }

agNewCfgSyslogTrapSystem OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable system level syslog and SNMP trap, in the 
         new_configuration block."
    ::= { agLog 3 }

agCurCfgSyslogTrapSystem OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable system level syslog and SNMP trap, as currently 
         configured in the current_configuration block."
    ::= { agLog 4 }

agNewCfgSyslogTrapMgmt OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable management(flash, config, login) syslog and SNMP 
         trap, in the new_configuration block."
    ::= { agLog 5 }

agCurCfgSyslogTrapMgmt OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable management(flash, config, login) syslog and SNMP 
         trap, as currently configured in the current_configuration block."
    ::= { agLog 6 }

agNewCfgSyslogTrapCli OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable CLI generated error syslog and SNMP trap, in the 
	 new_configuration block."
    ::= { agLog 7 }

agCurCfgSyslogTrapCli OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable CLI generated error syslog and SNMP trap, as 
         currently configured in the current_configuration block." 
    ::= { agLog 8 }

agNewCfgSyslogTrapStg OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable spanning tree syslog and SNMP trap, in the 
         new_configuration block."
    ::= { agLog 9 }

agCurCfgSyslogTrapStg OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable spanning tree syslog and SNMP trap, as currently 
         configured in the current_configuration block."
    ::= { agLog 10 }

agNewCfgSyslogTrapVlan OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable VLAN syslog and SNMP trap, in the new_configuration
         block."
    ::= { agLog 11 }

agCurCfgSyslogTrapVlan OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable VLAN syslog and SNMP trap, as currently configured 
         in the current_configuration block."
    ::= { agLog 12 }


agNewCfgSyslogTrapSsh OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable SSH, RADIUS syslog and SNMP trap, in the 
         new_configuration block."
    ::= { agLog 19 }

agCurCfgSyslogTrapSsh OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable SSH, RADIUS syslog and SNMP trap, as currently 
         configured in the current_configuration block."
    ::= { agLog 20 }

agNewCfgSyslogTrapVrrp OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable VRRP syslog and SNMP trap, in the new_configuration
         block."
    ::= { agLog 21 }

agCurCfgSyslogTrapVrrp OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable VRRP syslog and SNMP trap, as currently configured 
         in the current_configuration block."
    ::= { agLog 22 }


agNewCfgSyslogTrapNtp OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable NTP syslog and SNMP trap, in the new_configuration 
         block."
    ::= { agLog 25 }

agCurCfgSyslogTrapNtp OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable NTP syslog and SNMP trap, as currently configured 
         in the current_configuration block."
    ::= { agLog 26 }


agNewCfgSyslogTrapIp OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable IP related syslog and SNMP trap, in the 
         new_configuration block."
    ::= { agLog 31 }

agCurCfgSyslogTrapIp OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable IP related syslog and SNMP trap, as currently 
         configured in the current_configuration block."
    ::= { agLog 32 }

agNewCfgSyslogTrapWeb OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable WEBUI related syslog and SNMP trap, in the 
         new_configuration block."
    ::= { agLog 35 }

agCurCfgSyslogTrapWeb OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable WEBUI related syslog and SNMP trap, as currently 
         configured in the current_configuration block."
    ::= { agLog 36 }



agNewCfgSyslogTrapOspf OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable OSPF related syslog and SNMP trap, 
         in the new_configuration block."
    ::= { agLog 41 }

agCurCfgSyslogTrapOspf OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable OSPF related syslog and SNMP trap,
         as currently configured in the current_configuration block."
    ::= { agLog 42 }

agNewCfgSyslogTrapRmon OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable rmon related syslog and SNMP trap,
         in the new_configuration block."
    ::= { agLog 45 }

agCurCfgSyslogTrapRmon OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable rmon related syslog and SNMP trap,
         as currently configured in the current_configuration block."
    ::= { agLog 46 }

agNewCfgSyslogTrapUfd OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable UFD related syslog and SNMP trap, in the 
         new_configuration block."
    ::= { agLog 47 }

agCurCfgSyslogTrapUfd OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable UFD related syslog and SNMP trap,
         as currently configured in the current_configuration block."
    ::= { agLog 48 }

agNewCfgSyslogTrap8021x OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable 802.1 related syslog and SNMP trap, in the
         new_configuration block."
    ::= { agLog 51 } 

agCurCfgSyslogTrap8021x OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable 802.1 related syslog and SNMP trap, in the
         new_configuration block."
    ::= { agLog 52 }



agNewCfgSyslogTrapCfg OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable CFG related syslog and SNMP trap, in the
         new_configuration block."
    ::= { agLog 49 }

agCurCfgSyslogTrapCfg OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable CFG related syslog and SNMP trap,
         as currently configured in the current_configuration block."
    ::= { agLog 50 }

agNewCfgSyslogTrapAll OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable all syslog and SNMP traps, in the 
         new_configuration block."
    ::= { agLog 55 }

agCurCfgSyslogTrapAll OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable all syslog and SNMP traps, as currently 
         configured in the current_configuration block."
    ::= { agLog 56 }


-- TFTP Config
agTransferServer OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..64))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The FTP/TFTP server IP address or domain name."
    ::= { agTransfer 1 }

agTransferImage OBJECT-TYPE
    SYNTAX  INTEGER {
        image1(2),
        image2(3),
	boot(4)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Whether the image file should be loaded in image1 or image2 or
         boot in flash."
    ::= { agTransfer 2 }

agTransferImageFileName OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The image file name to be downloaded."
    ::= { agTransfer 3 }

agTransferCfgFileName OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The configuration file name."
    ::= { agTransfer 4 }

agTransferDumpFileName OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The core dump file name."
    ::= { agTransfer 5 }

agTransferAction OBJECT-TYPE
    SYNTAX  INTEGER {
        other(1),
        img-get(2),
        cfg-get(3),
        cfg-put(4),
        dump-put(5),
        img-put(7),
        tsdump-put(8)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "This is an action object to perform various FTP/TFTP Get or Put functions.
         The FTP/TFTP sever is specified in agTransferServer object.
         img-get(2) - Download switch image from a specified image
                      file(agTransferImageFileName) on the FTP/TFTP server to
                      the destinated storage(agTransferImage).
         cfg-get(3) - Download switch configuration from a specified
                      file(agTransferCfgFileName) on the FTP/TFTP server.
         cfg-put(4) - Upload switch configuration to a specified
                      file(agTransferCfgFileName) on the FTP/TFTP server.
         dump-put(5)- Download switch core dump to a specified
                      file(agTransferDumpFileName) on the FTP/TFTP server.
         img-put(7) - Upload specified switch image to a specified image
                      file(agTransferImageFileName) on the FTP/TFTP server.
         tsdump-put(5)- Download switch core dump to a specified
                      file (agTransferTSDumpFileName) on the FTP/TFTP server.
         other(1) is returned always when read."
    ::= { agTransfer 6 }

agTransferLastActionStatus OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The recorded status of the previous FTP/TFTP activity."
    ::= { agTransfer 7 }


agTransferUserName OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The username for FTP server or blank for TFTP server."
    ::= { agTransfer 9 }

agTransferPassword OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The password for FTP server."
    ::= { agTransfer 10 }

agTransferTSDumpFileName OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The TS dump file name."
    ::= { agTransfer 11 }

agTransferLastConfigurationActionStatus OBJECT-TYPE
    SYNTAX INTEGER {
        successfully(1),
        failed(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The status of the last configuration action using the file ftp/tftp'd
         from the server."
    ::= { agTransfer 14 }


-- Agent Port Table

agPortTableMaxEnt OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum number of rows in the port configuration host table."
    ::= { agPortConfig 1 }

agPortCurCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF AgPortCurCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of port configuration in the current_configuration block."
    ::= { agPortConfig 2 }

agPortCurCfgTableEntry OBJECT-TYPE
    SYNTAX  AgPortCurCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the port table in the current_configuration block."
    INDEX   { agPortCurCfgIndx }
    ::= { agPortCurCfgTable 1 }

AgPortCurCfgTableEntry ::= SEQUENCE {
    agPortCurCfgIndx           Integer32,
    agPortCurCfgState          INTEGER,
    agPortCurCfgVlanTag        INTEGER,
    agPortCurCfgRmon           INTEGER,
    agPortCurCfgPVID           INTEGER,
    agPortCurCfgGigEthAutoNeg  INTEGER,
    agPortCurCfgGigEthSpeed    INTEGER,
    agPortCurCfgGigEthMode     INTEGER,
    agPortCurCfgGigEthFctl     INTEGER,
    agPortCurCfgPortName       DisplayString
    ,agPortCurCfgLinkTrap       INTEGER
    ,agPortCurCfgTagPVID        INTEGER
    ,agPortCurCfgMulticastThreshold         INTEGER,
    agPortCurCfgMulticastThresholdRate     INTEGER,
    agPortCurCfgBroadcastThreshold         INTEGER,
    agPortCurCfgBroadcastThresholdRate     INTEGER,
    agPortCurCfgDLFThreshold               INTEGER,
    agPortCurCfgDLFThresholdRate           INTEGER
    ,agPortCurCfgType		DisplayString
    }

agPortCurCfgIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The index of the row in port configurations table."
    ::= { agPortCurCfgTableEntry 1 }

agPortCurCfgState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(2),
        disabled(3)
	}
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This is the state of the port."
    ::= { agPortCurCfgTableEntry 2 }

agPortCurCfgVlanTag OBJECT-TYPE
    SYNTAX  INTEGER {
        tagged(2),
        untagged(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This is VLAN tag state of the port"
    ::= { agPortCurCfgTableEntry 3 }

agPortCurCfgRmon OBJECT-TYPE
    SYNTAX  INTEGER {
        on(2),
        off(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This object is used to turn RMON on or off on the port."
   ::= { agPortCurCfgTableEntry 5 }

agPortCurCfgPVID OBJECT-TYPE
    SYNTAX  INTEGER (1..4095)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The default VLAN ID for the port."
    ::= { agPortCurCfgTableEntry 6 }

agPortCurCfgGigEthAutoNeg OBJECT-TYPE
    SYNTAX  INTEGER {
        on(2),
        off(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This object is used to turn the autonegotiation on or off
         for gigabit Ethernet connection."
    ::= { agPortCurCfgTableEntry 11 }

agPortCurCfgGigEthSpeed OBJECT-TYPE
    SYNTAX  INTEGER {
        mbs10(2),
        mbs100(3),
        any(4),
        mbs1000(5)
        ,mbs10000(6)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Selects the port speed for gigabit Ethernet connection."
    ::= { agPortCurCfgTableEntry 12 }

agPortCurCfgGigEthMode OBJECT-TYPE
    SYNTAX  INTEGER {
        full-duplex(2),
        half-duplex(3),
        full-or-half-duplex(4)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This object is used to select port mode for gigabit Ethernet connection."
    ::= { agPortCurCfgTableEntry 13 }

agPortCurCfgGigEthFctl OBJECT-TYPE
    SYNTAX  INTEGER {
        transmit(2),
        receive(3),
        both(4),
        none(5)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This object is used to select port flow control for
         gigabit Ethernet connection."
    ::= { agPortCurCfgTableEntry 14 }

agPortCurCfgPortName	OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..65))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The switch port name."
    ::= { agPortCurCfgTableEntry 15 }


agPortCurCfgLinkTrap OBJECT-TYPE
    SYNTAX  INTEGER {
	enabled(1),
	disabled(2)
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Indicates whether linkUp/linkDown traps should be
        generated for this interface.

        By default, this object should have the value
        enabled(1) for interfaces which do not operate on
        'top' of any other interface (as defined in the
        ifStackTable), and disabled(2) otherwise."
    ::= { agPortCurCfgTableEntry 18 }

agPortCurCfgTagPVID OBJECT-TYPE
    SYNTAX  INTEGER {
        tagged(2),
        untagged(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This is PVID tag state of the port"
    ::= { agPortCurCfgTableEntry 19 }

agPortCurCfgMulticastThreshold OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Current status of the port's Multicast Threshold."
    ::= { agPortCurCfgTableEntry 20 }

agPortCurCfgMulticastThresholdRate OBJECT-TYPE
    SYNTAX  INTEGER(0..262143)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Current port's Multicast Threshold Rate."
    ::= { agPortCurCfgTableEntry 21 }

agPortCurCfgBroadcastThreshold OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Current status of the port's Broadcast Threshold."
    ::= { agPortCurCfgTableEntry 22 }

agPortCurCfgBroadcastThresholdRate OBJECT-TYPE
    SYNTAX  INTEGER(0..262143)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Current port's Broadcast Threshold Rate."
    ::= { agPortCurCfgTableEntry 23 }

agPortCurCfgDLFThreshold OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Current status of the port's Destination Lookup Fail Threshold."
    ::= { agPortCurCfgTableEntry 24 }

agPortCurCfgDLFThresholdRate OBJECT-TYPE
    SYNTAX  INTEGER(0..262143)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Current port's Destination Lookup Fail Threshold Rate."
    ::= { agPortCurCfgTableEntry 25 }


agPortCurCfgType OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..65))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The switch port type."
    ::= { agPortCurCfgTableEntry 28 }


agPortNewCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF AgPortNewCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of port configuration in the new_configuration block."
    ::= { agPortConfig 3 }

agPortNewCfgTableEntry OBJECT-TYPE
    SYNTAX  AgPortNewCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the port configuration table in the new_configuration block."
    INDEX   { agPortNewCfgIndx }
    ::= { agPortNewCfgTable 1 }

AgPortNewCfgTableEntry ::= SEQUENCE {
    agPortNewCfgIndx           Integer32,
    agPortNewCfgState          INTEGER,
    agPortNewCfgVlanTag        INTEGER,
    agPortNewCfgRmon           INTEGER,
    agPortNewCfgPVID           INTEGER,
    agPortNewCfgGigEthAutoNeg  INTEGER,
    agPortNewCfgGigEthSpeed    INTEGER,
    agPortNewCfgGigEthMode     INTEGER,
    agPortNewCfgGigEthFctl     INTEGER,
    agPortNewCfgPortName       DisplayString
    ,agPortNewCfgLinkTrap       INTEGER
    ,agPortNewCfgTagPVID        INTEGER
    ,agPortNewCfgMulticastThreshold         INTEGER,
    agPortNewCfgMulticastThresholdRate     INTEGER,
    agPortNewCfgBroadcastThreshold         INTEGER,
    agPortNewCfgBroadcastThresholdRate     INTEGER,
    agPortNewCfgDLFThreshold               INTEGER,
    agPortNewCfgDLFThresholdRate           INTEGER
    ,agPortNewCfgType	                DisplayString	
    }

agPortNewCfgIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The index of the row in port configurations table."
    ::= { agPortNewCfgTableEntry 1 }

agPortNewCfgState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(2),
        disabled(3)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "This is the state of the port."
    ::= { agPortNewCfgTableEntry 2 }

agPortNewCfgVlanTag OBJECT-TYPE
    SYNTAX  INTEGER {
        tagged(2),
        untagged(3)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "This is VLAN tag state of the port"
    ::= { agPortNewCfgTableEntry 3 }

agPortNewCfgRmon OBJECT-TYPE
    SYNTAX  INTEGER {
        on(2),
        off(3)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "This object is used to turn RMON on or off on the port."
    ::= { agPortNewCfgTableEntry 5 }

agPortNewCfgPVID OBJECT-TYPE
    SYNTAX  INTEGER (1..4095)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The default VLAN ID for the port."
    ::= { agPortNewCfgTableEntry 6 }

agPortNewCfgGigEthAutoNeg OBJECT-TYPE
    SYNTAX  INTEGER {
        on(2),
        off(3)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "This object is used to turn the autonegotiation on or off
         for gigabit Ethernet connection."
    ::= { agPortNewCfgTableEntry 11 }

agPortNewCfgGigEthSpeed OBJECT-TYPE
    SYNTAX  INTEGER {
        mbs10(2),
        mbs100(3),
        any(4),
        mbs1000(5)
        ,mbs10000(6)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Selects the port speed for gigabit Ethernet connection."
    ::= { agPortNewCfgTableEntry 12 }
 
agPortNewCfgGigEthMode OBJECT-TYPE
    SYNTAX  INTEGER {
        full-duplex(2),
        half-duplex(3),
        full-or-half-duplex(4)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "This object is used to select port mode for gigabit Ethernet connection."
    ::= { agPortNewCfgTableEntry 13 }

agPortNewCfgGigEthFctl OBJECT-TYPE
    SYNTAX  INTEGER {
        transmit(2),
        receive(3),
        both(4),
        none(5)
       }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "This object is used to select port flow control for
         gigabit Ethernet connection."
    ::= { agPortNewCfgTableEntry 14 }

agPortNewCfgPortName	OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..65))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The switch port name."
    ::= { agPortNewCfgTableEntry 15 }


agPortNewCfgLinkTrap OBJECT-TYPE
    SYNTAX  INTEGER {
	enabled(1),
	disabled(2)
    }
    MAX-ACCESS  read-write
    STATUS  current 
    DESCRIPTION
        "Indicates whether linkUp/linkDown traps should be
        generated for this interface.

        By default, this object should have the value
        enabled(1) for interfaces which do not operate on
        'top' of any other interface (as defined in the
        ifStackTable), and disabled(2) otherwise."
    ::= { agPortNewCfgTableEntry 18 }

agPortNewCfgTagPVID OBJECT-TYPE
    SYNTAX  INTEGER {
        tagged(2),
        untagged(3)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "This is PVID tag state of the port"
    ::= { agPortNewCfgTableEntry 19 }

agPortNewCfgMulticastThreshold OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "New status of the port's Multicast Threshold."
    ::= { agPortNewCfgTableEntry 20 }

agPortNewCfgMulticastThresholdRate OBJECT-TYPE
    SYNTAX  INTEGER(0..262143)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "New port's Multicast Threshold Rate."
    ::= { agPortNewCfgTableEntry 21 }

agPortNewCfgBroadcastThreshold OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "New status of the port's Broadcast Threshold."
    ::= { agPortNewCfgTableEntry 22 }

agPortNewCfgBroadcastThresholdRate OBJECT-TYPE
    SYNTAX  INTEGER(0..262143)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "New port's Broadcast Threshold Rate."
    ::= { agPortNewCfgTableEntry 23 }

agPortNewCfgDLFThreshold OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "New status of the port's Destination Lookup Fail Threshold."
    ::= { agPortNewCfgTableEntry 24 }

agPortNewCfgDLFThresholdRate OBJECT-TYPE
    SYNTAX  INTEGER(0..262143)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "New port's Destination Lookup Fail Threshold Rate."
    ::= { agPortNewCfgTableEntry 25 }

 
agPortNewCfgType OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..65))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The switch port type."
    ::= { agPortNewCfgTableEntry 28 }




-- SSH Configuration 
sshCurCfgIntrval OBJECT-TYPE
    SYNTAX INTEGER(0..24)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Interval for generating the RSA server key."
    ::= { agSSHConfig 1 }

sshNewCfgIntrval OBJECT-TYPE
    SYNTAX INTEGER(0..24)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Set Interval for generating the RSA server key."
    ::= { agSSHConfig 2 }

sshCurCfgScpAdm OBJECT-TYPE
    SYNTAX DisplayString(SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "SCP-only admin password."
    ::= { agSSHConfig 3 }

sshNewCfgScpAdm OBJECT-TYPE
    SYNTAX DisplayString(SIZE(0..128))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Set SCP-only admin password."
    ::= { agSSHConfig 4 }

sshNewCfgHKeyGen OBJECT-TYPE
    SYNTAX INTEGER {
        generate(1),
        other(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "This is an action object to generate the RSA host key.
         other(2) is returned always when read.
         The following values are writable: generate(1).. Generate the RSA host key."
    ::= { agSSHConfig 5 }

sshNewCfgSKeyGen OBJECT-TYPE
    SYNTAX INTEGER {
        generate(1),
        other(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
         "This is an action object to generate the RSA server key.
         other(2) is returned always when read.
         The following values are writable: generate(1).. Generate the RSA server key."
    ::= { agSSHConfig 6 }

sshCurCfgSSHPort OBJECT-TYPE
    SYNTAX INTEGER (1..65535)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "SSH server port number."
    ::= { agSSHConfig 7 }

sshNewCfgSSHPort OBJECT-TYPE
    SYNTAX INTEGER (1..65535)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Set SSH server port number."
    ::= { agSSHConfig 8 }

sshCurCfgScpApplySave OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "SCP apply and save."
    ::= { agSSHConfig 9 }

sshNewCfgScpApplySave OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable/Disable the SCP apply and save."
    ::= { agSSHConfig 10 }

sshCurCfgStatus OBJECT-TYPE
    SYNTAX INTEGER {
        on(1),
        off(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "SSH server status."
    ::= { agSSHConfig 11 }

sshNewCfgStatus OBJECT-TYPE
    SYNTAX INTEGER {
        on(1),
        off(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Turn SSH server ON/OFF."
    ::= { agSSHConfig 12 }

-- RADIUS Configuration 
 
radCurCfgPrimaryIpAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IP address of the Primary RADIUS server."
    ::= { agRadiusConfig 1 }

radNewCfgPrimaryIpAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The IP address of the Primary RADIUS server."
    ::= { agRadiusConfig 2 }

radCurCfgSecondaryIpAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IP address of the Secondary RADIUS server."
    ::= { agRadiusConfig 3 }

radNewCfgSecondaryIpAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The IP address of the Secondary RADIUS server."
    ::= { agRadiusConfig 4 }

radCurCfgPort OBJECT-TYPE
    SYNTAX  INTEGER  (1500..3000)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specify the RADIUS port number."
    ::= { agRadiusConfig 5 }

radNewCfgPort OBJECT-TYPE
    SYNTAX  INTEGER  (1500..3000)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Speicfy the RADIUS port number."
    ::= { agRadiusConfig 6 }

radCurCfgTimeout OBJECT-TYPE
    SYNTAX  INTEGER  (1..10)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum number of seconds before resending authentication
         to RADIUS server."
    ::= { agRadiusConfig 7 }

radNewCfgTimeout OBJECT-TYPE
    SYNTAX  INTEGER  (1..10)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The maximum number of seconds before resending authentication
         to RADIUS server."
    ::= { agRadiusConfig 8 }

radCurCfgRetries OBJECT-TYPE
    SYNTAX  INTEGER  (1..3)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Number of retries to the RADIUS server."
    ::= { agRadiusConfig 9 }

radNewCfgRetries OBJECT-TYPE
    SYNTAX  INTEGER  (1..3)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Number of retries to the RADIUS server."
    ::= { agRadiusConfig 10 }

radCurCfgState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(2),
        disabled(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable RADIUS authentication."
    ::= { agRadiusConfig 11 }

radNewCfgState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(2),
        disabled(3)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable RADIUS authentication."
    ::= { agRadiusConfig 12 }

radCurCfgAuthenString OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..32))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The RADIUS authentication string."
    ::= { agRadiusConfig 13 }

radNewCfgAuthenString OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..32))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The RADIUS authentication string."
    ::= { agRadiusConfig 14 }

radCurCfgBackdoor OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable RADIUS backdoor for telnet/ssh/http/https."
    ::= { agRadiusConfig 15 }

radNewCfgBackdoor OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable RADIUS backdoor for telnet/ssh/http/https."
    ::= { agRadiusConfig 16 }

radCurCfgAuthenSecondString OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..32))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The second RADIUS authentication string."
    ::= { agRadiusConfig 17 }

radNewCfgAuthenSecondString OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..32))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The second RADIUS authentication string."
    ::= { agRadiusConfig 18 }

radCurCfgSecBd OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable RADIUS secure backdoor for telnet."
    ::= { agRadiusConfig 19 }

radNewCfgSecBd OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable RADIUS secure backdoor for telnet."
    ::= { agRadiusConfig 20 }

-- NTP Configuration 
agCurCfgNTPServer OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The NTP Server Address."
    ::= { agNTP 1 }

agNewCfgNTPServer OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The NTP Server Address."
    ::= { agNTP 2 }

agCurCfgNTPResyncInterval OBJECT-TYPE
    SYNTAX  INTEGER (1..44640)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The NTP Server resync interval in minutes."
    ::= { agNTP 3 }

agNewCfgNTPResyncInterval OBJECT-TYPE
    SYNTAX  INTEGER (1..44640)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The NTP Server resync interval in minutes."
    ::= { agNTP 4 }


agCurCfgNTPService OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable/disable NTP Service."
    ::= { agNTP 9 }

agNewCfgNTPService OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable/disable NTP Service."
    ::= { agNTP 10 }

agCurCfgNTPSecServer OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Secondary NTP Server Address."
    ::= { agNTP 11 }

agNewCfgNTPSecServer OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The Secondary NTP Server Address."
    ::= { agNTP 12 }


-- APPLY Configuration
agApplyPending OBJECT-TYPE
    SYNTAX  INTEGER {
        applyNeeded(2),
        noApplyNeeded(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This object, when read, gives the user information
         whether an apply action is needed and that the configuration
         has been chaged by the user actions. The user then can
         apply the changes by setting proper value to the object
         agApplyConfiguration described above."
    ::= { agApply 1 }

agApplyConfig OBJECT-TYPE
    SYNTAX  INTEGER {
        apply(1), 
        idle(2),
        inprogress(3),
        complete(4),
        failed(5)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
         "When this object is read the current state is returned.
          idle(3) indicates that there is no apply in progess.
          complete(5) indicates that the last apply operation is completed.
          Setting the value to apply(1), will write all the changes made
          since the last apply to the current configuration block.
	  If the apply is successful this variable will return the state
          'complete' else it will return 'failed'. In case of failure,
          to read the reason for failure use the agApplyTable."
    ::= { agApply 2 }

agApplyTableSize OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The number of strings in the apply table."
    ::= { agApply 4 }

agApplyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF AgApplyTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of URL path for URL load balancing in the current_config."
    ::= { agApply 5 }

agApplyTableEntry OBJECT-TYPE
    SYNTAX  AgApplyTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "Information about an URL path for URL load balancing."
    INDEX   { agApplyIndex }
    ::= { agApplyTable 1 }

AgApplyTableEntry ::= SEQUENCE {
    agApplyIndex      Integer32,
    agApplyString     OCTET STRING
    }

agApplyIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The table index."
    ::= { agApplyTableEntry 1 }

agApplyString OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "A string in the apply table."
    ::= { agApplyTableEntry 2 }

-- TACACS+ Configuration

tacCurCfgPrimaryIpAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IP address of the Primary TACACS+ server."
    ::= { agTacacsConfig 1 }

tacNewCfgPrimaryIpAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The IP address of the Primary TACACS+ server."
    ::= { agTacacsConfig 2 }

tacCurCfgSecondaryIpAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IP address of the Secondary TACSACS server."
    ::= { agTacacsConfig 3 }
tacNewCfgSecondaryIpAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The IP address of the Secondary TACACS+ server."
    ::= { agTacacsConfig 4 }


tacCurCfgPort OBJECT-TYPE
    SYNTAX  INTEGER  (1..65000)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Specify the TACACS+ port number."
    ::= { agTacacsConfig 5 }

tacNewCfgPort OBJECT-TYPE
    SYNTAX  INTEGER  (1..65000)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Specify the TACACS+ port number."
    ::= { agTacacsConfig 6 }

tacCurCfgTimeout OBJECT-TYPE
    SYNTAX  INTEGER  (4..15)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum number of seconds before resending authentication
         to TACACS+ server."
    ::= { agTacacsConfig 7 }

tacNewCfgTimeout OBJECT-TYPE
    SYNTAX  INTEGER  (4..15)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The maximum number of seconds before resending authentication
         to TACACS+ server."
    ::= { agTacacsConfig 8 }

tacCurCfgRetries OBJECT-TYPE
    SYNTAX  INTEGER  (1..3)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Number of retries to the TACACS+ server."
    ::= { agTacacsConfig 9 }

tacNewCfgRetries OBJECT-TYPE
    SYNTAX  INTEGER  (1..3)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Number of retries to the TACACS+ server."
    ::= { agTacacsConfig 10 }

tacCurCfgState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(2),
        disabled(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable TACACS+ authentication."
    ::= { agTacacsConfig 11 }

tacNewCfgState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(2),
        disabled(3)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable TACACS+ authentication."
    ::= { agTacacsConfig 12 }

tacCurCfgAuthenString OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..32))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The TACACS+ authentication string."
    ::= { agTacacsConfig 13 }

tacNewCfgAuthenString OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..32))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The TACACS+ authentication string."
    ::= { agTacacsConfig 14 }

tacCurCfgBackdoor OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable TACACS+ backdoor for telnet/ssh/http/https."
    ::= { agTacacsConfig 15 }

tacNewCfgBackdoor OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable TACACS+ backdoor for telnet/ssh/http/https."
    ::= { agTacacsConfig 16 }

tacCurCfgAuthenSecondString OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..32))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The second TACACS+ authentication string."
    ::= { agTacacsConfig 17 }

tacNewCfgAuthenSecondString OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..32))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The second TACACS+ authentication string."
    ::= { agTacacsConfig 18 }

tacCurCfgCmdAuthor OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable TACACS+ command authorization."
    ::= { agTacacsConfig 19 }

tacNewCfgCmdAuthor OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable TACACS+ command authorization."
    ::= { agTacacsConfig 20 }

tacCurCfgSecBd OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable TACACS+ secure backdoor for telnet."
    ::= { agTacacsConfig 23 }

tacNewCfgSecBd OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable TACACS+ secure backdoor for telnet."
    ::= { agTacacsConfig 24 }

tacCurCfgCmdLogging OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable TACACS+ command logging."
    ::= { agTacacsConfig 21 }

tacNewCfgCmdLogging OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable TACACS+ command logging."
    ::= { agTacacsConfig 22 }
tacCurCfgCmap OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable/Disable Tacacs+ new prividlege level maping."
    ::= { agTacacsConfig 25 }

tacNewCfgCmap OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable/Disable Tacacs+ new prividlege level maping."
    ::= { agTacacsConfig 26 }

agTacacsUserMapCurCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF AgTacacsUserMapCurCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of tacacs+ user map current configuration."
    ::= { agTacacsConfig 31 }

agTacacsUserMapCurCfgTableEntry OBJECT-TYPE
    SYNTAX  AgTacacsUserMapCurCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the tacacs+ user mapping table."
    INDEX  { agTacacsUserMapCurCfgUId }
    ::= { agTacacsUserMapCurCfgTable 1 }

AgTacacsUserMapCurCfgTableEntry ::= SEQUENCE {
    agTacacsUserMapCurCfgUId       Integer32,
    agTacacsUserMapCurCfgMapping   INTEGER
    }

agTacacsUserMapCurCfgUId OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The current config remote privilege identifier."
    ::= { agTacacsUserMapCurCfgTableEntry 1 }

agTacacsUserMapCurCfgMapping OBJECT-TYPE
    SYNTAX  INTEGER {
        none(0),
        user(1),
        oper(2),
        admin(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Current Tacacs+ user privilege mappings."
    ::= { agTacacsUserMapCurCfgTableEntry 2 }

agTacacsUserMapNewCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF AgTacacsUserMapNewCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of tacacs+ user map new configuration."
    ::= { agTacacsConfig 32 }

agTacacsUserMapNewCfgTableEntry OBJECT-TYPE
    SYNTAX  AgTacacsUserMapNewCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the tacacs+ user mapping table."
    INDEX  { agTacacsUserMapNewCfgUId }
    ::= { agTacacsUserMapNewCfgTable 1 }

AgTacacsUserMapNewCfgTableEntry ::= SEQUENCE {
    agTacacsUserMapNewCfgUId       Integer32,
    agTacacsUserMapNewCfgMapping   INTEGER
    }

agTacacsUserMapNewCfgUId OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The new config remote privilege identifier."
    ::= { agTacacsUserMapNewCfgTableEntry 1 }

agTacacsUserMapNewCfgMapping OBJECT-TYPE
    SYNTAX  INTEGER {
        none(0),
        user(1),
        oper(2),
        admin(3)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Set new Tacacs+ user privilege mappings."
    ::= { agTacacsUserMapNewCfgTableEntry 2 }

-- Multiple Management network MIB objects
agMgmtNetTableMaxSize OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "The maximum number of entries in the Management
         Network Table."
    ::= { agMgmtNetConfig 1 }

agCurCfgMgmtNetTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF AgCurCfgMgmtNetEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION
        "The table for Management Network definitions
         in the current configuration block."
    ::= { agMgmtNetConfig 2 }

agCurCfgMgmtNetEntry OBJECT-TYPE
    SYNTAX  AgCurCfgMgmtNetEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION
        "A row in the management network definition table."
    INDEX   {  agCurCfgMgmtNetIndex }
    ::= { agCurCfgMgmtNetTable 1 }

AgCurCfgMgmtNetEntry ::= SEQUENCE {
    agCurCfgMgmtNetIndex        Integer32,
    agCurCfgMgmtNetSubnet       IpAddress,
    agCurCfgMgmtNetMask         IpAddress
    }

agCurCfgMgmtNetIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "The index of the Management Network Definition table."
    ::= { agCurCfgMgmtNetEntry 1 }

agCurCfgMgmtNetSubnet OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "The Management Network Address in the current_configuration
         block."
    ::= { agCurCfgMgmtNetEntry 2 }

agCurCfgMgmtNetMask OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION
        "The Management Network Mask in the current_configuration
         block."
    ::= { agCurCfgMgmtNetEntry 3 }

agNewCfgMgmtNetTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF AgNewCfgMgmtNetEntry
    MAX-ACCESS  not-accessible
    STATUS current
    DESCRIPTION
        "The table for Management Network definitions
         in the new configuration block."
    ::= { agMgmtNetConfig 3 }

agNewCfgMgmtNetEntry OBJECT-TYPE
    SYNTAX  AgNewCfgMgmtNetEntry
    MAX-ACCESS  not-accessible 
    STATUS current
    DESCRIPTION
        "A row in the management network definition table."
    INDEX   {  agNewCfgMgmtNetIndex }
    ::= { agNewCfgMgmtNetTable 1 }
    
AgNewCfgMgmtNetEntry ::= SEQUENCE {
    agNewCfgMgmtNetIndex        Integer32,
    agNewCfgMgmtNetSubnet       IpAddress,
    agNewCfgMgmtNetMask         IpAddress,
    agNewCfgMgmtNetDelete       INTEGER
    }

agNewCfgMgmtNetIndex OBJECT-TYPE 
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS current
    DESCRIPTION 
        "The index of the Management Network Definition table."
    ::= { agNewCfgMgmtNetEntry 1 }

agNewCfgMgmtNetSubnet OBJECT-TYPE
    SYNTAX  IpAddress 
    MAX-ACCESS  read-create
    STATUS current 
    DESCRIPTION
        "The Management Network Address in the new_configuration
         block." 
    ::= { agNewCfgMgmtNetEntry 2 }

agNewCfgMgmtNetMask OBJECT-TYPE
    SYNTAX  IpAddress 
    MAX-ACCESS  read-create
    STATUS current
    DESCRIPTION
        "The Management Network Mask in the new_configuration
         block." 
    ::= { agNewCfgMgmtNetEntry 3 }

agNewCfgMgmtNetDelete OBJECT-TYPE 
    SYNTAX  INTEGER {
        other(1),
        delete(2)
        }
    MAX-ACCESS  read-create
    STATUS current
    DESCRIPTION
        "By setting the value to delete(2), the entire row is deleted."
    ::= { agNewCfgMgmtNetEntry 4 }

agMgmtNetClear OBJECT-TYPE
    SYNTAX  INTEGER {
        other(1),
        clear(2)
        }
    MAX-ACCESS  read-write
    STATUS current
    DESCRIPTION
        "By setting the value to delete(2), the entire table is cleared."
    ::= { agMgmtNetConfig 4 }

agAccessUserMaxUserID OBJECT-TYPE
    SYNTAX  Integer32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum number of Users ID."
    ::= { agAccess 1 }

agAccessUserCurCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF AgAccessUserCurCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of Access user configuration."
    ::= { agAccess 2 }

agAccessUserCurCfgTableEntry OBJECT-TYPE
    SYNTAX  AgAccessUserCurCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the Access user configuration table."
    INDEX  { agAccessUserCurCfgUId }
    ::= { agAccessUserCurCfgTable 1 }

AgAccessUserCurCfgTableEntry ::= SEQUENCE {
    agAccessUserCurCfgUId 	Integer32,
    agAccessUserCurCos 		INTEGER,
    agAccessUserCurCfgName 	DisplayString,
    agAccessUserCurCfgPswd 	DisplayString,
    agAccessUserCurCfgState	INTEGER
    }

agAccessUserCurCfgUId OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The User identifier."
    ::= { agAccessUserCurCfgTableEntry 1 }

agAccessUserCurCos OBJECT-TYPE
    SYNTAX  INTEGER {
        user(0),
        oper(3),
        admin(6)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The user class of service."
    ::= { agAccessUserCurCfgTableEntry 2 }

agAccessUserCurCfgName OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..8))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The user name."
    ::= { agAccessUserCurCfgTableEntry 3 }

agAccessUserCurCfgPswd OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..128))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The character string representing the user passworde."
    ::= { agAccessUserCurCfgTableEntry 4 }

agAccessUserCurCfgState OBJECT-TYPE
    SYNTAX  INTEGER  {
	enabled(2),
	disabled(3)
	}
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable a user."
    ::= { agAccessUserCurCfgTableEntry 5 }

agAccessUserNewCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF AgAccessUserNewCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of Access user configuration."
    ::= { agAccess 3 }

agAccessUserNewCfgTableEntry OBJECT-TYPE
    SYNTAX  AgAccessUserNewCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the Access user configuration table."
    INDEX  { agAccessUserNewCfgUId }
    ::= { agAccessUserNewCfgTable 1 }

AgAccessUserNewCfgTableEntry ::= SEQUENCE {
    agAccessUserNewCfgUId 	Integer32,
    agAccessUserNewCos 		INTEGER,
    agAccessUserNewCfgName 	DisplayString,
    agAccessUserNewCfgPswd 	DisplayString,
    agAccessUserNewCfgState	INTEGER,
    agAccessUserNewCfgDelete 	INTEGER
    }

agAccessUserNewCfgUId OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The User identifier."
    ::= { agAccessUserNewCfgTableEntry 1 }

agAccessUserNewCos OBJECT-TYPE
    SYNTAX  INTEGER {
        user(0),
        oper(3),
        admin(6)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The user class of service."
    ::= { agAccessUserNewCfgTableEntry 2 }

agAccessUserNewCfgName OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..8))
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The user name."
    ::= { agAccessUserNewCfgTableEntry 3 }

agAccessUserNewCfgPswd OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..128))
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The character string representing the user passworde."
    ::= { agAccessUserNewCfgTableEntry 4 }

agAccessUserNewCfgState OBJECT-TYPE
    SYNTAX  INTEGER  {
	enabled(2),
	disabled(3)
	}
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Enable or disable a user."
    ::= { agAccessUserNewCfgTableEntry 5 }

agAccessUserNewCfgDelete OBJECT-TYPE
    SYNTAX  INTEGER  {
        other(1),
        delete(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "This is an action object to create or delete a User.
         other(1) is returned always when read.
         The following values are writable: delete(2)...to delete a User"
    ::= { agAccessUserNewCfgTableEntry 6 }

-- Statistics Group

-- Packet Statistics Group
-- This group represents Packet Statistics information
 
pktStatsAllocs OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Total number of packet allocations from the packet buffer pool by 
         the TCP/IP protocol stack."
    ::= { pktStats 1 }
 
pktStatsFrees OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Total number of times the packet buffers are freed(released) to the
         packet buffer pool by the TCP/IP protocol stack."
    ::= { pktStats 2 }
 
pktStatsAllocFails OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Total number of packet allocation failures from the packet buffer 
         pool by the TCP/IP protocol stack."
    ::= { pktStats 3}
 
pktStatsMediums OBJECT-TYPE
    SYNTAX  Gauge32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Total number of packet allocations with size greater than 128 bytes
         and less than or equal to 1536 bytes from the packet buffer pool by 
         the TCP/IP protocol stack."
    ::= { pktStats 4}

pktStatsJumbos OBJECT-TYPE
    SYNTAX  Gauge32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Total number of packet allocations with size larger than 1536 bytes 
         from the packet buffer pool by the TCP/IP protocol stack."
    ::= { pktStats 5}
 
pktStatsSmalls OBJECT-TYPE
    SYNTAX  Gauge32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Total number of packet allocations with size less than or eqaul to 
         128 bytes from the packet buffer pool by the TCP/IP protocol stack."
    ::= { pktStats 6}

pktStatsMediumsHiWatermark OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The highest number of packet allocations with size greater than 
         128 bytes and less than or equal to 1536 bytes from the packet 
         buffer pool by the TCP/IP protocol stack."
    ::= { pktStats 7}

pktStatsJumbosHiWatermark OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The highest number of packet allocations with size larger than 
         1536 bytes from the packet buffer pool by the TCP/IP protocol stack."
    ::= { pktStats 8}

pktStatsSmallsHiWatermark OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The highest number of packet allocations with size less than or 
         eqaul to 128 bytes from the packet buffer pool by the TCP/IP 
         protocol stack."
    ::= { pktStats 9}

-- MP CPU Statisitics Group
 
mpCpuStatsUtil1Second OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The utilization of MP CPU over 1 second. It shows the percentage."
    ::= { mpCpuStats 1}
 
mpCpuStatsUtil4Seconds OBJECT-TYPE
    SYNTAX  Integer32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The utilization of MP CPU  over 4 seconds. 
	 It shows the percentage."
    ::= { mpCpuStats 2}
 
mpCpuStatsUtil64Seconds OBJECT-TYPE
    SYNTAX  Integer32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The utilization of MP CPU over 64 seconds. 
	 It shows the percentage."
    ::= { mpCpuStats 3}

--
-- Port statistics table
--
portStatsTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF PortStatsTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of port statistics."
    ::= { portStats 1 }

portStatsTableEntry OBJECT-TYPE
    SYNTAX  PortStatsTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the port stats table."
    INDEX   { portStatsIndx }
    ::= { portStatsTable 1 }

PortStatsTableEntry ::=
    SEQUENCE {
	portStatsIndx
	    Integer32,
	portStatsPhyIfInOctets
	    Counter32,
	portStatsPhyIfInUcastPkts
	    Counter32,
	portStatsPhyIfInNUcastPkts
	    Counter32,
	portStatsPhyIfInDiscards
	    Counter32,
	portStatsPhyIfInErrors
	    Counter32,
	portStatsPhyIfInUnknownProtos
	    Counter32,
	portStatsPhyIfOutOctets
	    Counter32,
	portStatsPhyIfOutUcastPkts
	    Counter32,
	portStatsPhyIfOutNUcastPkts
	    Counter32,
	portStatsPhyIfOutDiscards
	    Counter32,
	portStatsPhyIfOutErrors
	    Counter32,
	portStatsPhyIfOutQLen
	    Gauge32,
        portStatsPhyIfInBroadcastPkts
            Counter32,
        portStatsPhyIfOutBroadcastPkts
            Counter32,
	portStatsPhyIfInMulticastPkts
	    Counter32,
	portStatsPhyIfOutMulticastPkts
	    Counter32,
	portStatsClear
            INTEGER
    }

portStatsIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port index."
    ::= { portStatsTableEntry 1 }

portStatsPhyIfInOctets OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	    "The total number of octets received on the
	    interface, including framing characters."
    ::= { portStatsTableEntry 2 }

portStatsPhyIfInUcastPkts OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	    "The number of subnetwork-unicast packets
	    delivered to a higher-layer protocol."
    ::= { portStatsTableEntry 3 }

portStatsPhyIfInNUcastPkts OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	    "The number of non-unicast (i.e., subnetwork-
	    broadcast or subnetwork-multicast) packets
	    delivered to a higher-layer protocol."
    ::= { portStatsTableEntry 4 }

portStatsPhyIfInDiscards OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	    "The number of inbound packets which were chosen
	    to be discarded even though no errors had been
	    detected to prevent their being deliverable to a
	    higher-layer protocol.  One possible reason for
	    discarding such a packet could be to free up
	    buffer space."
    ::= { portStatsTableEntry 5 }

portStatsPhyIfInErrors OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	    "The number of inbound packets that contained
	    errors preventing them from being deliverable to a
	    higher-layer protocol."
    ::= { portStatsTableEntry 6 }

portStatsPhyIfInUnknownProtos OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	    "The number of packets received via the interface
	    which were discarded because of an unknown or
	    unsupported protocol."
    ::= { portStatsTableEntry 7 }

portStatsPhyIfOutOctets OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	    "The total number of octets transmitted out of the
	    interface, including framing characters."
    ::= { portStatsTableEntry 8 }

portStatsPhyIfOutUcastPkts OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	    "The total number of packets that higher-level
	    protocols requested be transmitted to a
	    subnetwork-unicast address, including those that
	    were discarded or not sent."
    ::= { portStatsTableEntry 9 }

portStatsPhyIfOutNUcastPkts OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	    "The total number of packets that higher-level
	    protocols requested be transmitted to a non-
	    unicast (i.e., a subnetwork-broadcast or
	    subnetwork-multicast) address, including those
	    that were discarded or not sent."
    ::= { portStatsTableEntry 10 }

portStatsPhyIfOutDiscards OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	    "The number of outbound packets which were chosen
	    to be discarded even though no errors had been
	    detected to prevent their being transmitted.  One
	    possible reason for discarding such a packet could
	    be to free up buffer space."
    ::= { portStatsTableEntry 11 }

portStatsPhyIfOutErrors OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	    "The number of outbound packets that could not be
	    transmitted because of errors."
    ::= { portStatsTableEntry 12 }

portStatsPhyIfOutQLen OBJECT-TYPE
    SYNTAX  Gauge32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	    "The length of the output packet queue (in
	    packets)."
    ::= { portStatsTableEntry 13 }

portStatsPhyIfInBroadcastPkts OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current 
    DESCRIPTION
            "The number of packets, delivered by this sub-layer to
            a higher (sub-)layer, which were addressed to a
            broadcast address at this sub-layer."
    ::= { portStatsTableEntry 14 }

portStatsPhyIfOutBroadcastPkts OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current 
    DESCRIPTION
	    "The total number of packets that higher-level
            protocols requested be transmitted, and which were
            addressed to a broadcast address at this sub-layer,
            including those that were discarded or not sent."
    ::= { portStatsTableEntry 15 }

portStatsPhyIfInMulticastPkts OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
            "The number of packets, delivered by this sub-layer to
            a higher (sub-)layer, which were addressed to a
            multicast address at this sub-layer."
    ::= { portStatsTableEntry 17 }

portStatsPhyIfOutMulticastPkts OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
            "The total number of packets that higher-level
            protocols requested be transmitted, and which were
            addressed to a multicast address at this sub-layer,
            including those that were discarded or not sent."
    ::= { portStatsTableEntry 18 }

portStatsClear OBJECT-TYPE
    SYNTAX  INTEGER {
        clear(1),
        ok(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
            "Setting this value to clear(1) clears the stats for this port."
    ::= { portStatsTableEntry 16 }


-- 802.1x port stats table

dot1xPortStatsTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF Dot1xPortStatsTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of 802.1x port statistics."
    ::= { portStats 2 }

dot1xPortStatsTableEntry OBJECT-TYPE
    SYNTAX  Dot1xPortStatsTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the 802.1x  port stats table."
    INDEX   { dot1xPortStatsIndx }
    ::= { dot1xPortStatsTable 1 }

Dot1xPortStatsTableEntry ::=
    SEQUENCE {
	dot1xPortStatsIndx Integer32,	
	eapolFramesRx Integer32, 
	eapolFramesTx Integer32,	
	eapolStartFramesRx Integer32,
	eapolLogoffFramesRx  Integer32,
	eapolRespIdFramesRx Integer32,
	eapolRespFramesRx  Integer32,
	eapolReqIdFramesTx Integer32,
	eapolReqFramesTx Integer32,	 
	invalidEapolFramesRx Integer32,	 
	eapLengthErrorFramesRx Integer32,
	authEntersConnecting Integer32,
	authEapLogoffsWhileConnecting Integer32,	
	authEntersAuthenticating  Integer32,
	authSuccessesWhileAuthenticating Integer32,
	authTimeoutsWhileAuthenticating Integer32,	 
	authFailWhileAuthenticating Integer32,	
	authReauthsWhileAuthenticating 	Integer32, 
	authEapStartsWhileAuthenticating Integer32,
	authEapLogoffWhileAuthenticating Integer32,
	authReauthsWhileAuthenticated 	Integer32, 
	authEapStartsWhileAuthenticated  Integer32,
	authEapLogoffWhileAuthenticated  Integer32,
	backendResponses Integer32,	
	backendAccessChallenges  Integer32,
	backendOtherRequestsToSupplicant Integer32,
	backendNonNakResponsesFromSupplicant Integer32,
	backendAuthSuccesses 	Integer32,
	backendAuthFails Integer32,
        lastEapolFrameVersion Integer32,
        lastEapolFrameSource MacAddress
    }

dot1xPortStatsIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The 802.1x port stats index."
    ::= { dot1xPortStatsTableEntry 1 }

eapolFramesRx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 2 }

eapolFramesTx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 3 }

eapolStartFramesRx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 4 }


eapolLogoffFramesRx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 5 }

eapolRespIdFramesRx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 6 }

eapolRespFramesRx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 7 }

eapolReqIdFramesTx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 8 }


eapolReqFramesTx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 9 }

invalidEapolFramesRx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= {dot1xPortStatsTableEntry 10  }

eapLengthErrorFramesRx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 11 }

authEntersConnecting  OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 12 }


authEapLogoffsWhileConnecting OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 13 }

authEntersAuthenticating  OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 14 }

authSuccessesWhileAuthenticating  OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 15 }

authTimeoutsWhileAuthenticating OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 16 }

authFailWhileAuthenticating OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 17 }

authReauthsWhileAuthenticating  OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 18 }

authEapStartsWhileAuthenticating  OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 19 }

authEapLogoffWhileAuthenticating  OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 20 }


authReauthsWhileAuthenticated  OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 21 }

authEapStartsWhileAuthenticated  OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 22 }

authEapLogoffWhileAuthenticated  OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 23 }

backendResponses  OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 24 }

backendAccessChallenges  OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 25 }

backendOtherRequestsToSupplicant  OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 26 }

backendNonNakResponsesFromSupplicant  OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 27 }

backendAuthSuccesses  OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 28 }

backendAuthFails   OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 29 }

lastEapolFrameVersion   OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 30 }

lastEapolFrameSource   OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { dot1xPortStatsTableEntry 31 }

allportsStatsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AllportsStatsTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table of all ports statistics."
    ::= { portStats 3 }

allportsStatsTableEntry OBJECT-TYPE
    SYNTAX      AllportsStatsTableEntry 
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A row in the table of all ports statistics."
    INDEX   { allportsStatsIndx }
    ::= { allportsStatsTable 1 }

AllportsStatsTableEntry ::=
    SEQUENCE {
        allportsStatsIndx                      Integer32,
        allportsStatsDescr                     DisplayString,
        allportsStatsSpeed		       INTEGER,
        allportsStatsPhysAddress	       PhysAddress,
        allportsStatsAdminStatus               INTEGER,
        allportsStatsOperStatus                INTEGER,
        allportsStatsInOctets                  Counter32,
        allportsStatsOutOctets                 Counter32,
        allportsStatsInPkts                    Counter32,
        allportsStatsOutPkts                   Counter32, 
        allportsStatsInUcast                   DisplayString,
        allportsStatsOutUcast                  DisplayString,
        allportsStatsInBcast                   DisplayString,
        allportsStatsOutBcast                  DisplayString,
        allportsStatsInMcast                   DisplayString,
        allportsStatsOutMcast                  DisplayString,
        allportsStatsInDiscards                Counter32,
        allportsStatsOutDiscards               Counter32,
        allportsStatsInErrors                  Counter32,
        allportsStatsOutErrors                 Counter32,
        allportsStatsInUnknownProtos           DisplayString,
        allportsStatsOutQLen                   DisplayString
        ,
        allportsStatsipInReceives              Counter32,
        allportsStatsipInHeaderErrors          Counter32,
        allportsStatsipInDiscards              Counter32        
        ,
        allportsStatsLinkStateChange           Counter32
}

allportsStatsIndx OBJECT-TYPE
    SYNTAX           Integer32
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "The port number."
    ::= { allportsStatsTableEntry 1 }

allportsStatsDescr OBJECT-TYPE
    SYNTAX           DisplayString(SIZE(0..5)) 
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "The port description."
    ::= { allportsStatsTableEntry 2 }

allportsStatsSpeed OBJECT-TYPE
    SYNTAX  INTEGER {
        mbs10(2),
        mbs100(3),
        mbs1000(4),
        any(5)
        ,
        mbs10000(6)
        }
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "The current operational speed of the port."
    ::= { allportsStatsTableEntry 3 }

allportsStatsPhysAddress OBJECT-TYPE
    SYNTAX           PhysAddress 
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "The port MAC Address."
    ::= { allportsStatsTableEntry 4 }

allportsStatsAdminStatus OBJECT-TYPE
    SYNTAX  INTEGER {
        up(1),
        down(2),
        testing(3)
        }
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "The port Admin state."
    ::= { allportsStatsTableEntry 5 }

allportsStatsOperStatus OBJECT-TYPE
    SYNTAX  INTEGER {
        up(1),
        down(2),
        testing(3)
        }
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "The port Operational Status."
    ::= { allportsStatsTableEntry 6 }
 
allportsStatsInOctets OBJECT-TYPE
    SYNTAX           Counter32 
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "Octets In for port."
    ::= { allportsStatsTableEntry 7 }

allportsStatsOutOctets OBJECT-TYPE
    SYNTAX           Counter32
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "Octets Out for port."
    ::= { allportsStatsTableEntry 8 }

allportsStatsInPkts OBJECT-TYPE
    SYNTAX           Counter32
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "Packets In for port."
    ::= { allportsStatsTableEntry 9 }

allportsStatsOutPkts OBJECT-TYPE
    SYNTAX           Counter32
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "Packets Out for port."
    ::= { allportsStatsTableEntry 10 }

allportsStatsInUcast OBJECT-TYPE
    SYNTAX           DisplayString(SIZE(0..20)) 
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "Unicast Packets In for port."
    ::= { allportsStatsTableEntry 11 }

allportsStatsOutUcast OBJECT-TYPE
    SYNTAX           DisplayString(SIZE(0..20))
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "Unicast Packets Out for port."
    ::= { allportsStatsTableEntry 12 }

allportsStatsInBcast OBJECT-TYPE
    SYNTAX           DisplayString(SIZE(0..20))
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "Broadcasts Packets In for port."
    ::= { allportsStatsTableEntry 13 }

allportsStatsOutBcast OBJECT-TYPE
    SYNTAX           DisplayString(SIZE(0..20))
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "Broadcasts Packets Out for port."
    ::= { allportsStatsTableEntry 14 }

allportsStatsInMcast OBJECT-TYPE
    SYNTAX           DisplayString(SIZE(0..20))
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "Multicast Packets In for port."
    ::= { allportsStatsTableEntry 15 }

allportsStatsOutMcast OBJECT-TYPE
    SYNTAX           DisplayString(SIZE(0..20))
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "Multicast Packets Out for port."
    ::= { allportsStatsTableEntry 16 }

allportsStatsInDiscards OBJECT-TYPE
    SYNTAX           Counter32
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "Discarded Packets for port."
    ::= { allportsStatsTableEntry 17 }

allportsStatsOutDiscards OBJECT-TYPE
    SYNTAX           Counter32
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "Outbound Packets for port."
    ::= { allportsStatsTableEntry 18 }

allportsStatsInErrors OBJECT-TYPE
    SYNTAX           Counter32
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "Error Packets for port."
    ::= { allportsStatsTableEntry 19 }

allportsStatsOutErrors OBJECT-TYPE
    SYNTAX           Counter32
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "Not sent packets due to error."
    ::= { allportsStatsTableEntry 20 }

allportsStatsInUnknownProtos OBJECT-TYPE
    SYNTAX           DisplayString(SIZE(0..20))
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "Unknown protocol packets."
    ::= { allportsStatsTableEntry 21 }

allportsStatsOutQLen OBJECT-TYPE
    SYNTAX           DisplayString(SIZE(0..20))
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "Outbound Packet Queue Length."
    ::= { allportsStatsTableEntry 22 }

allportsStatsipInReceives OBJECT-TYPE
    SYNTAX           Counter32
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "Ip In Receives."
    ::= { allportsStatsTableEntry 23 }

allportsStatsipInHeaderErrors OBJECT-TYPE
    SYNTAX           Counter32
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "Ip In Header Errors."
    ::= { allportsStatsTableEntry 24 }

allportsStatsipInDiscards OBJECT-TYPE
    SYNTAX           Counter32
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "Ip In Discards."
    ::= { allportsStatsTableEntry 25 }

allportsStatsLinkStateChange OBJECT-TYPE
    SYNTAX           Counter32
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
            "Number of link state changes."
    ::= { allportsStatsTableEntry 26 }

clearPortsStats OBJECT-TYPE
    SYNTAX  INTEGER { 
	ok(1),
	clear(2)
	}
    MAX-ACCESS  read-write
    STATUS  current  
    DESCRIPTION
        "Setting this to clear(2) results in clearing the statistics for all ports." 
    ::= { portStats 4 }

agDiffState OBJECT-TYPE
    SYNTAX  INTEGER {
        diff(1), 
        flashdiff(2),
        idle(3),
        inprogress(4),
        complete(5)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
         "When this object is read the current state is returned.
          idle(3) indicates that there is no diff in progess.
          complete(5) indicates that the last diff operation is completed.
          Setting the value to diff(1), will start a new diff operation
          Diff compares the new configuration with the current configuration
          and shows the pending configuration changes. 
          Setting the value to flashdiff(1), will start a new diff operation.
          flashdiff compares new configuration with the flash configuration.
          To read the configuration changes use the agDiffTable once the
          state of this variable returns complete."
    ::= { agDiff 2 }

agDiffTableSize OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The number of strings in the diff table."
    ::= { agDiff 3 }

agDiffTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF AgDiffTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of URL path for URL load balancing in the current_config."
    ::= { agDiff 4 }

agDiffTableEntry OBJECT-TYPE
    SYNTAX  AgDiffTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "Information about an URL path for URL load balancing."
    INDEX   { agDiffIndex }
    ::= { agDiffTable 1 }

AgDiffTableEntry ::= SEQUENCE {
    agDiffIndex      Integer32,
    agDiffString     OCTET STRING
    }

agDiffIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The table index."
    ::= { agDiffTableEntry 1 }

agDiffString OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "A string in the diff table."
    ::= { agDiffTableEntry 2 }

-- Config Dump 
agCfgDumpState OBJECT-TYPE
    SYNTAX  INTEGER {
        dump(1), 
        idle(2),
        inprogress(3),
        complete(4)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
         "When this object is read the current state is returned.
          idle(2) indicates that there is no dump in progess.
          complete(4) indicates that the last dump operation is completed.
          Setting the value to dump(1), will start a new dump operation
          Dump will show the current configuration.
          To read the configuration dump use the agCfgDumpTable once the
          state of this variable returns complete.
          Once the agCfgDumpTable is read the state should be set back to 
          'idle' which frees the dump buffer and others can issue a dump 
          command via SNMP."
    ::= { agCfgDump 2 }

agCfgDumpTableSize OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The number of strings in the dump table."
    ::= { agCfgDump 3 }

agCfgDumpTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF AgCfgDumpTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of dump strings."
    ::= { agCfgDump 4 }

agCfgDumpTableEntry OBJECT-TYPE
    SYNTAX  AgCfgDumpTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "An entry in the dump table."
    INDEX   { agCfgDumpIndex }
    ::= { agCfgDumpTable 1 }

AgCfgDumpTableEntry ::= SEQUENCE {
    agCfgDumpIndex      Integer32,
    agCfgDumpString     OCTET STRING
    }

agCfgDumpIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The table index."
    ::= { agCfgDumpTableEntry 1 }

agCfgDumpString OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "A string in the dump table."
    ::= { agCfgDumpTableEntry 2 }

-- GeaPort Information
geaportInfoTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF GeaportInfoTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of gea port mapping."
    ::= { geaportInfo 1 }

geaportInfoTableEntry OBJECT-TYPE
    SYNTAX  GeaportInfoTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "An entry in the geaport table mapping."
    INDEX   { geaportInfoLogicalIndex }
    ::= { geaportInfoTable 1 }

GeaportInfoTableEntry ::= SEQUENCE {
    geaportInfoLogicalIndex    Integer32,
    geaportInfoPort            INTEGER,
    geaportInfoUnit            INTEGER
    }

geaportInfoLogicalIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The logical port index."
    ::= { geaportInfoTableEntry 1 }

geaportInfoPort OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The GEA Port (0-based)."
    ::= { geaportInfoTableEntry 2 }

geaportInfoUnit OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The GEA Unit."
    ::= { geaportInfoTableEntry 3 }

-- UFDFO Information

ufdInfoState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Uplink Failure Detection State."
    ::= { ufdInfo 1 }

ufdInfoLtMStatus OBJECT-TYPE
    SYNTAX  INTEGER{
        up(1),
        down(2),
        forwarding(3),
        blocked(4)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "LtM Status."
    ::= { ufdInfo 2 }

ufdInfoLtMPorts OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The LtM port list. The ports are presented in bitmap format.
         in receiving order:

              OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             ||    || |_ port 8
             ||    ||
             ||    ||___ port 7
             ||    |____ port 6
             ||      .    .   .
             ||_________ port 1
             |__________ reserved

         where x : 1 - The represented port belongs to LtM
            0 - The represented port does not belong to LtM."
    ::= { ufdInfo 3 }

ufdInfoLtMTrunks OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The LtM trunk list. The trunks are presented in bitmap format.
         in receiving order:

              OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             ||    || |_ trunk 8
             ||    ||
             ||    ||___ trunk 7
             ||    |____ trunk 6
             ||      .    .   .
             ||_________ trunk 1
             |__________ reserved

         where x : 1 - The represented trunk belongs to LtM
            0 - The represented trunk does not belong to LtM."
    ::= { ufdInfo 4 }

ufdInfoLtMAdminkey OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The LtM admin key."
    ::= { ufdInfo 5 }

ufdInfoLtDStatus OBJECT-TYPE
    SYNTAX  INTEGER{
        up(1),
        autoDisabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "LtD status."
    ::= { ufdInfo 6 }

ufdInfoLtDPorts OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The LtD port list. The ports are presented in bitmap format.
         in receiving order:

              OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             ||    || |_ port 8
             ||    ||
             ||    ||___ port 7
             ||    |____ port 6
             ||      .    .   .
             ||_________ port 1
             |__________ reserved

         where x : 1 - The represented port belongs to LtD
            0 - The represented port does not belong to LtD."
    ::= { ufdInfo 7 }

ufdInfoLtDTrunks OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The LtD trunk list. The trunks are presented in bitmap format.
         in receiving order:

              OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             ||    || |_ trunk 8
             ||    ||
             ||    ||___ trunk 7
             ||    |____ trunk 6
             ||      .    .   .
             ||_________ trunk 1
             |__________ reserved

         where x : 1 - The represented trunk belongs to LtD
            0 - The represented trunk does not belong to LtD."
    ::= { ufdInfo 8 }


ufdInfoLtDAdminkeyMaxEnt OBJECT-TYPE
    SYNTAX  Integer32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum number of rows in the LtD admin key configuration table."
    ::= { ufdInfo 9 }

ufdInfoLtDAdminkeyTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF UfdInfoLtDAdminkeyTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of LtD admin key configuration."
    ::= { ufdInfo 10 }

ufdInfoLtDAdminkeyTableEntry OBJECT-TYPE
    SYNTAX  UfdInfoLtDAdminkeyTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the LtD admin key table."
    INDEX  { ufdInfoLtDAdminkey }
    ::= { ufdInfoLtDAdminkeyTable 1 }

UfdInfoLtDAdminkeyTableEntry ::= SEQUENCE {
    ufdInfoLtDAdminkey	INTEGER	    
    }

ufdInfoLtDAdminkey OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The LtD admin key."
    ::= { ufdInfoLtDAdminkeyTableEntry 1 }


-- SFP Information

sfpInfoTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF SfpInfoTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of external port SFP information."
    ::= { sfpInfo 1 }

sfpInfoTableEntry OBJECT-TYPE
    SYNTAX  SfpInfoTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the external port SFP information table."
    INDEX   { sfpInfoIndx }
    ::= { sfpInfoTable 1 }

SfpInfoTableEntry ::= SEQUENCE {
    sfpInfoIndx                 Integer32,
    sfpInfoPort                 DisplayString,
    sfpInfoDevice               DisplayString,
    sfpInfoTXEnable             INTEGER,
    sfpInfoRXSignal             INTEGER,
    sfpInfoTXFault              INTEGER,
    sfpInfoApproved             INTEGER
    }

sfpInfoIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The external port SFX index."
    ::= { sfpInfoTableEntry 1 }

sfpInfoPort OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..6))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
          "External Port SFP/XFP alias."
    ::= { sfpInfoTableEntry 2 }

sfpInfoDevice OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..6))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
          "External Port SFP/XFP Device."
    ::= { sfpInfoTableEntry 3 }

sfpInfoTXEnable OBJECT-TYPE
    SYNTAX  INTEGER {
          notInstalled (1),
          enabled (2),
          disabled (3)
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
          "External Port SFP/XFP TX-Enable."
    ::= { sfpInfoTableEntry 4  }

sfpInfoRXSignal  OBJECT-TYPE
    SYNTAX  INTEGER {
          notInstalled (1),
          lost (2),
          ok (3),
          notAvailable (4)
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
          "External Port SFP/XFP RX-Signal."
    ::= { sfpInfoTableEntry 5 }

sfpInfoTXFault  OBJECT-TYPE
    SYNTAX  INTEGER {
          notInstalled (1),
          fault (2),
          none (3),
          notAvailable (4)
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
          "External Port SFP/XFP TX-Fault."
    ::= { sfpInfoTableEntry 6 }

sfpInfoApproved  OBJECT-TYPE
    SYNTAX  INTEGER {
          notInstalled (1),
          notXFP (2),
          notSFP (3),
          yes (4)
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
          "External Port SFP/XFP Approval."
    ::= { sfpInfoTableEntry 7 }


-- NTP Statisitics

ntpPrimaryServerReqSent OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The total number of NTP requests sent to Primary NTP Server."
    ::= { ntpStats 1 }

ntpPrimaryServerRespRcvd OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The total number of NTP responces received from Primary NTP Server."
    ::= { ntpStats 2 }

ntpPrimaryServerUpdates OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The total number of NTP Updates by Primary NTP Server."
    ::= { ntpStats 3 }

ntpSecondaryServerReqSent OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The total number of NTP requests sent to Secondary NTP Server."
    ::= { ntpStats 4 }

ntpSecondaryServerRespRcvd OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The total number of NTP responces received from Secondary NTP Server."
    ::= { ntpStats 5 }

ntpSecondaryServerUpdates OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The total number of NTP Updates by Secondary NTP Server."
    ::= { ntpStats 6 }

ntpLastUpdateServer OBJECT-TYPE
    SYNTAX  INTEGER {
        none(0),
        primary(1),
        secondary(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The type of ntp server updated last time."
    ::= { ntpStats 7 }

ntpLastUpdateTime OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..127))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The last time updated by ntp server."
    ::= { ntpStats 8 }

ntpClearStats OBJECT-TYPE
    SYNTAX  INTEGER {
        ok(1),
        clear(2)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Setting this value to clear(2) clears the stats for ntp."
    ::= { ntpStats 9 }

ntpSystemCurrentTime OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..127))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The current system time."
    ::= { ntpStats 10 }


    aclStatsTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF AclStatsTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table of ACL statistics."
    ::= { aclStats 1 }

aclStatsTableEntry  OBJECT-TYPE
    SYNTAX      AclStatsTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Statistics about a particular ACL configuration entry."
    INDEX { aclStatsIndex }
    ::= { aclStatsTable 1 }

AclStatsTableEntry  ::= SEQUENCE {
    aclStatsIndex          Integer32,
    aclStatsHits           Counter32,
    aclClearStats          INTEGER
    }

aclStatsIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The acl index."
    ::= { aclStatsTableEntry 1 }

aclStatsHits OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Total number of hits for this ACL entry"
    ::= { aclStatsTableEntry 2 }

aclClearStats OBJECT-TYPE
    SYNTAX  INTEGER {
        ok(1),
        clear(2)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Setting this value to clear(2) clears the stats for the ACL."
    ::= { aclStatsTableEntry 3 }

-- Clear Statistics
snmpClearStats OBJECT-TYPE
    SYNTAX  INTEGER { 
	ok(1),
	clear(2)
	}
    MAX-ACCESS  read-write
    STATUS  current  
    DESCRIPTION
        "Setting this to clear(2) results in clearing the SNMP statistics." 
    ::= { agClearStats 1 }

-- ----------------------------------------------------------------------------
-- } INSERT:  bt2Switch
-- ----------------------------------------------------------------------------


layer2                  OBJECT IDENTIFIER
    ::= { hpSwitchBladeType5-Mgmt 2 }

-- ----------------------------------------------------------------------------
-- { INSERT:  bt2Physical
-- ----------------------------------------------------------------------------

layer2Configs     OBJECT IDENTIFIER ::= { layer2 1 }
layer2Stats       OBJECT IDENTIFIER ::= { layer2 2 }
layer2Info        OBJECT IDENTIFIER ::= { layer2 3 }
layer2Oper        OBJECT IDENTIFIER ::= { layer2 4 }

vlan              OBJECT IDENTIFIER ::= { layer2Configs 1 }
trunkgroup        OBJECT IDENTIFIER ::= { layer2Configs 2 }
stgCfg            OBJECT IDENTIFIER ::= { layer2Configs 3 }
mirroring         OBJECT IDENTIFIER ::= { layer2Configs 4 }
mstCfg            OBJECT IDENTIFIER ::= { layer2Configs 5 }
lacp		  OBJECT IDENTIFIER ::= { layer2Configs 6 }
thash             OBJECT IDENTIFIER ::= { layer2Configs 7 }
l2GeneralCfg      OBJECT IDENTIFIER ::= { layer2Configs 8 }
ufd               OBJECT IDENTIFIER ::= { layer2Configs 9 }

-- layer2Configs 10 is being used by failoverCfg in aosFailoverCfg.mib

dot1x             OBJECT IDENTIFIER ::= { layer2Configs 11 }
fdb               OBJECT IDENTIFIER ::= { layer2Configs 12 }

thashL2           OBJECT IDENTIFIER ::= { thash 1 }

mirrPortMirr      OBJECT IDENTIFIER ::= { mirroring 1 }

mstGeneralCfg     OBJECT IDENTIFIER ::= { mstCfg 1 }
mstCistCfg        OBJECT IDENTIFIER ::= { mstCfg 2 }

ufdGeneralCfg     OBJECT IDENTIFIER ::= { ufd 1 }
fdbGeneralCfg	  OBJECT IDENTIFIER ::= { fdb 1 }

dot1xCurCfgGlobalTable  OBJECT IDENTIFIER ::= { dot1x  5 }
dot1xNewCfgGlobalTable  OBJECT IDENTIFIER ::= { dot1x  6 }

fdbStats	  OBJECT IDENTIFIER ::= { layer2Stats 1 }
stpStats	  OBJECT IDENTIFIER ::= { layer2Stats 2 }
lacpStats	  OBJECT IDENTIFIER ::= { layer2Stats 3 }
ufdStats          OBJECT IDENTIFIER ::= { layer2Stats 4 }

cistInfo          OBJECT IDENTIFIER ::= { layer2Info 1 }
fdbInfo           OBJECT IDENTIFIER ::= { layer2Info 2 }
stpInfo           OBJECT IDENTIFIER ::= { layer2Info 3 }
lacpInfo          OBJECT IDENTIFIER ::= { layer2Info 4 }
dot1xInfo         OBJECT IDENTIFIER ::= { layer2Info 5 }
dot1pInfo         OBJECT IDENTIFIER ::= { layer2Info 6 }
genInfo           OBJECT IDENTIFIER ::= { layer2Info 7 }
vlanInfo          OBJECT IDENTIFIER ::= { layer2Info 8 }
trunkGroupInfo    OBJECT IDENTIFIER ::= { layer2Info 9 }

dot1xSystemInfo   OBJECT IDENTIFIER ::= { dot1xInfo 2 }


cistGeneralInfo   OBJECT IDENTIFIER ::= { cistInfo 1 }

-- VLAN group
vlanMaxEnt OBJECT-TYPE
    SYNTAX  Integer32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum number of rows in the VLAN configuration table."
    ::= { vlan 1 }

vlanCurCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF VlanCurCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of VLAN configuration."
    ::= { vlan 2 }

vlanCurCfgTableEntry OBJECT-TYPE
    SYNTAX  VlanCurCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the VLAN configuration table."
    INDEX  { vlanCurCfgVlanId }
    ::= { vlanCurCfgTable 1 }

VlanCurCfgTableEntry ::= SEQUENCE {
    vlanCurCfgVlanId 		Integer32,
    vlanCurCfgVlanName 		DisplayString,
    vlanCurCfgPorts 		OCTET STRING,
    vlanCurCfgState 		INTEGER, 
    vlanCurCfgStg  	        Integer32
    }

vlanCurCfgVlanId OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The VLAN identifier."
    ::= { vlanCurCfgTableEntry 1 }

vlanCurCfgVlanName OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..32))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The VLAN name."
    ::= { vlanCurCfgTableEntry 2 }

vlanCurCfgPorts	OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port list in the VLAN. The ports are presented in bitmap format.
	 in receiving order:

	     OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx ..... 
             ||    || |_ port 8
             ||    ||  
             ||    ||___ port 7
             ||    |____ port 6
             ||      .    .   .
             ||_________ port 1
             |__________ reserved

         where x : 1 - The represented port belongs to the VLAN
		   0 - The represented port does not belong to the VLAN"
    ::= { vlanCurCfgTableEntry 3 }

vlanCurCfgState	OBJECT-TYPE
    SYNTAX  INTEGER  {
	enabled(2),
	disabled(3)
	}
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable a VLAN"
    ::= { vlanCurCfgTableEntry 4 }


vlanCurCfgStg OBJECT-TYPE
    SYNTAX  Integer32  
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Spanning Tree Group for the VLAN."
    ::= { vlanCurCfgTableEntry 6 }



vlanNewCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF VlanNewCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of VLAN configuration."
    ::= { vlan 3 }

vlanNewCfgTableEntry OBJECT-TYPE
    SYNTAX  VlanNewCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the VLAN configuration table."
    INDEX  { vlanNewCfgVlanId }
    ::= { vlanNewCfgTable 1 }

VlanNewCfgTableEntry ::= SEQUENCE {
    vlanNewCfgVlanId 		Integer32,
    vlanNewCfgVlanName 		DisplayString,
    vlanNewCfgPorts 		OCTET STRING,
    vlanNewCfgState 		INTEGER,
    vlanNewCfgAddPort 		Integer32,
    vlanNewCfgRemovePort	Integer32,
    vlanNewCfgDelete 		INTEGER,
    vlanNewCfgStg  	        Integer32
    }

vlanNewCfgVlanId OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The VLAN identifier."
    ::= { vlanNewCfgTableEntry 1 }

vlanNewCfgVlanName OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..32))
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The VLAN name."
    ::= { vlanNewCfgTableEntry 2 }

vlanNewCfgPorts	OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port list in the VLAN.  The ports are presented in bitmap format.
         in receiving order:

	     OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx ..... 
             ||    || |_ port 8
             ||    ||  
             ||    ||___ port 7
             ||    |____ port 6
             ||      .    .   .
             ||_________ port 1
             |__________ reserved

         where x : 1 - The represented port belongs to the VLAN
	           0 - The represented port does not belong to the VLAN"
    ::= { vlanNewCfgTableEntry 3 }

vlanNewCfgState	OBJECT-TYPE
    SYNTAX  INTEGER  {
	enabled(2),
	disabled(3)
	}
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Enable or disable a VLAN"
    ::= { vlanNewCfgTableEntry 4 }

vlanNewCfgAddPort OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The port to be added to the specified VLAN.  A '0' value is 
         returned when read."
    ::= { vlanNewCfgTableEntry 5 }

vlanNewCfgRemovePort OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The port to be removed from the specified VLAN.  A '0'
         value is returned when read."
    ::= { vlanNewCfgTableEntry 6 }

vlanNewCfgDelete OBJECT-TYPE
    SYNTAX  INTEGER  {
        other(1),
        delete(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "This is an action object to create or delete a VLAN.
         other(1) is returned always when read.
         The following values are writable: delete(2)...to delete a VLAN"
    ::= { vlanNewCfgTableEntry 7 }


vlanNewCfgStg OBJECT-TYPE
    SYNTAX  Integer32  
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The Spanning Tree Group for the VLAN."
    ::= { vlanNewCfgTableEntry 9 }





-- Trunk Group Group
trunkGroupTableMaxSize OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum number of entries in trunk group table."
    ::= { trunkgroup 1 }

trunkGroupCurCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF TrunkGroupCurCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of trunk group configuration."
    ::= { trunkgroup 2 }

trunkGroupCurCfgTableEntry OBJECT-TYPE
    SYNTAX  TrunkGroupCurCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the trunk group configuration table."
    INDEX   { trunkGroupCurCfgIndex }
    ::= { trunkGroupCurCfgTable 1 }

TrunkGroupCurCfgTableEntry ::= SEQUENCE {
    trunkGroupCurCfgIndex         Integer32,
    trunkGroupCurCfgPorts         OCTET STRING,
    trunkGroupCurCfgState         INTEGER
    }
 
trunkGroupCurCfgIndex OBJECT-TYPE
    SYNTAX  Integer32  
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The identifier of the trunk group."
    ::= { trunkGroupCurCfgTableEntry 1 }
 
trunkGroupCurCfgPorts OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port list in the trunk group. The ports are presented in 
         bitmap format.
 
         in receiving order:
 
             OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx ..... 
             ||    || |_ port 8
             ||    ||  
             ||    ||___ port 7
             ||    |____ port 6
             ||      .    .   .
             ||_________ port 1
             |__________ reserved

         where x : 1 - The represented port belongs to the trunk group
                   0 - The represented port does not belong to the trunk group"
    ::= { trunkGroupCurCfgTableEntry 2 }
 
trunkGroupCurCfgState OBJECT-TYPE
    SYNTAX  INTEGER  {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable a trunk group."
    ::= { trunkGroupCurCfgTableEntry 3 }
 
 
trunkGroupNewCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF TrunkGroupNewCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of trunk group configuration."
    ::= { trunkgroup 3 }

trunkGroupNewCfgTableEntry OBJECT-TYPE
    SYNTAX  TrunkGroupNewCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the trunk group configuration table."
    INDEX   { trunkGroupNewCfgIndex }
    ::= { trunkGroupNewCfgTable 1 }

TrunkGroupNewCfgTableEntry ::= SEQUENCE {
    trunkGroupNewCfgIndex          Integer32,
    trunkGroupNewCfgPorts          OCTET STRING,
    trunkGroupNewCfgAddPort        Integer32,
    trunkGroupNewCfgRemovePort     Integer32,
    trunkGroupNewCfgState          INTEGER,
    trunkGroupNewCfgDelete         INTEGER
    }
 
trunkGroupNewCfgIndex OBJECT-TYPE
    SYNTAX  Integer32  
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The identifier of the trunk group."
    ::= { trunkGroupNewCfgTableEntry 1 }
 
trunkGroupNewCfgPorts OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port list in the trunk group.  The ports are presented
         in bitmap format.

         in receiving order:

             OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx ..... 
             ||    || |_ port 8
             ||    ||  
             ||    ||___ port 7
             ||    |____ port 6
             ||      .    .   .
             ||_________ port 1
             |__________ reserved
 
         where x : 1 - The represented port belongs to the trunk group
                   0 - The represented port does not belong to the trunk group"
    ::= { trunkGroupNewCfgTableEntry 2 }
 
trunkGroupNewCfgAddPort OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The port to be added in the trunk group. When read, 0 is returned."
    ::= { trunkGroupNewCfgTableEntry 3 }

trunkGroupNewCfgRemovePort OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The port to be deleted from the trunk group. when read, 0
	 is returned."
    ::= { trunkGroupNewCfgTableEntry 4 }

trunkGroupNewCfgState OBJECT-TYPE
    SYNTAX  INTEGER  {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Enable or disable a trunk group."
    ::= { trunkGroupNewCfgTableEntry 5 }
 
trunkGroupNewCfgDelete OBJECT-TYPE
    SYNTAX  INTEGER  {
        other(1),
        delete(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Setting the value to delete(2) will delete the entire
         row. When read, other(1) is returned."
    ::= { trunkGroupNewCfgTableEntry 6 }


-- Trunk hash
l2ThashCurCfgSmacState OBJECT-TYPE
    SYNTAX  INTEGER  {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable smac hash."
    ::= { thashL2 1 }

l2ThashNewCfgSmacState OBJECT-TYPE
    SYNTAX  INTEGER  {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable smac hash."
    ::= { thashL2 2 }

l2ThashCurCfgDmacState OBJECT-TYPE
    SYNTAX  INTEGER  {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable dmac hash."
    ::= { thashL2 3 }

l2ThashNewCfgDmacState OBJECT-TYPE
    SYNTAX  INTEGER  {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable dmac hash."
    ::= { thashL2 4 }

l2ThashCurCfgSipState OBJECT-TYPE
    SYNTAX  INTEGER  {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable sip hash."
    ::= { thashL2 5 }

l2ThashNewCfgSipState OBJECT-TYPE
    SYNTAX  INTEGER  {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable sip hash."
    ::= { thashL2 6 }

l2ThashCurCfgDipState OBJECT-TYPE
    SYNTAX  INTEGER  {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable dip hash."
    ::= { thashL2 7 }

l2ThashNewCfgDipState OBJECT-TYPE
    SYNTAX  INTEGER  {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable dip hash."
    ::= { thashL2 8 }


-- Spanning Tree Group Configuration
-- This group specifies the additional configurations that are not
-- covered by the Bridge MIB (RFC 1493).
-- The relative Spanning Tree information can be retrieved or configured
-- using Bridge MIB with an unique community string for each group specified
-- in entLogicalTable of Entity MIB (RFC 2037).
--
stgCurCfgTable OBJECT-TYPE
    SYNTAX SEQUENCE OF StgCurCfgTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of Spanning Tree Group configuration."
    ::= { stgCfg 1 }

stgCurCfgTableEntry OBJECT-TYPE
    SYNTAX StgCurCfgTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a particular Spanning Tree Group configuration."
    INDEX { stgCurCfgIndex }
    ::= { stgCurCfgTable 1 }

StgCurCfgTableEntry ::= SEQUENCE {
    stgCurCfgIndex           Integer32,
    stgCurCfgState           INTEGER,
    stgCurCfgPriority        INTEGER,
    stgCurCfgBrgHelloTime    INTEGER,
    stgCurCfgBrgForwardDelay INTEGER,
    stgCurCfgBrgMaxAge       INTEGER,
    stgCurCfgVlanBmap        OCTET STRING
    }

stgCurCfgIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The identifier of a particular Spanning Tree Group.  This is also
         index to the entLogicalTable of Entity MIB."
    ::= { stgCurCfgTableEntry 1 }

stgCurCfgState OBJECT-TYPE
    SYNTAX INTEGER {
        on(1),
        off(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Turn on of off Spanning Tree operation of a particular Spanning
         Tree Group."
    ::= { stgCurCfgTableEntry 2 }


stgCurCfgPriority OBJECT-TYPE
    SYNTAX  INTEGER (0..65535)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value of the write-able portion of the Bridge ID, i.e., the first
         two octets of the (8 octet long) Bridge ID."
    ::= { stgCurCfgTableEntry 5 }

stgCurCfgBrgHelloTime OBJECT-TYPE
    SYNTAX  INTEGER (1..10)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for HelloTime when this 
         bridge is acting as the root."
    ::= { stgCurCfgTableEntry 6 }

stgCurCfgBrgForwardDelay OBJECT-TYPE
    SYNTAX  INTEGER (4..30)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for ForwardDelay when this 
         bridge is acting as the root."
    ::= { stgCurCfgTableEntry 7 }

stgCurCfgBrgMaxAge OBJECT-TYPE
    SYNTAX  INTEGER (6..40)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for MaxAge when this bridge
         is acting as the root."
    ::= { stgCurCfgTableEntry 8 }


stgCurCfgVlanBmap OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(0..512)) 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	"The vlans applied to the spanning tree group.  The vlans are 
         presented in bitmap format. This string displays vlan number
	 from 1 to 4095.

	 in receiving order:

	     OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx ..... 
             ||    || |_ vlan 9
             ||    ||  
             ||    ||___ vlan 8
             ||    |____ vlan 7
             ||      .    .   .
             ||_________ vlan 2
             |__________ vlan 1 (as index to stgCurCfgTable)

         where x : 1 - The represented vlan applied to the spanning tree. 
		   0 - The represented vlan not applied to the spanning tree"
    ::= { stgCurCfgTableEntry 10 }


stgNewCfgTable OBJECT-TYPE
    SYNTAX SEQUENCE OF StgNewCfgTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of Spanning Tree Groups configuration in the new_config."
    ::= { stgCfg 2 }

stgNewCfgTableEntry OBJECT-TYPE
    SYNTAX StgNewCfgTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a particular Spanning Tree Group configuration."
    INDEX { stgNewCfgIndex }
    ::= { stgNewCfgTable 1 }

StgNewCfgTableEntry ::= SEQUENCE {
    stgNewCfgIndex           Integer32,
    stgNewCfgState           INTEGER,
    stgNewCfgDefaultCfg      INTEGER,
    stgNewCfgAddVlan         Integer32,
    stgNewCfgRemoveVlan      Integer32,
    stgNewCfgPriority        INTEGER,
    stgNewCfgBrgHelloTime    INTEGER,
    stgNewCfgBrgForwardDelay INTEGER,
    stgNewCfgBrgMaxAge       INTEGER,
    stgNewCfgVlanBmap        OCTET STRING
    }

stgNewCfgIndex  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The identifier of a particular Spanning Tree Group.  This is also
         index to the entLogicalTable of Entity MIB."
    ::= { stgNewCfgTableEntry 1 }

stgNewCfgState OBJECT-TYPE
    SYNTAX INTEGER {
        on(1),
        off(2)
        }
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Turn on of off Spanning Tree operation of a particular Spanning
         Tree Group."
    ::= { stgNewCfgTableEntry 2 }

stgNewCfgDefaultCfg OBJECT-TYPE
    SYNTAX INTEGER {
        default-config(1)
        }
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Setting the value to default-config(1) will set the default
         configuration as recommended by IEEE 802.1D for a particular
         Spanning Tree Group.  default-config (1) is always returned 
	 When read, but it does not mean anything."
    ::= { stgNewCfgTableEntry 3 }

stgNewCfgAddVlan OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The vlan to be added to the specified Spanning Tree Group.  A 
         '0' value is returned when read." 
    ::= {stgNewCfgTableEntry 4 }

stgNewCfgRemoveVlan OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The vlan to be removed from the specified Spanning Tree Group.
         A '0' value is returned when read."
    ::= { stgNewCfgTableEntry 5 }


stgNewCfgPriority OBJECT-TYPE
    SYNTAX  INTEGER (0..65535)
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The value of the write-able portion of the Bridge ID, i.e., the first
         two octets of the (8 octet long) Bridge ID."
    ::= { stgNewCfgTableEntry 8 }

stgNewCfgBrgHelloTime OBJECT-TYPE
    SYNTAX  INTEGER (1..10)
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for HelloTime when this 
         bridge is acting as the root."
    ::= { stgNewCfgTableEntry 9 }

stgNewCfgBrgForwardDelay OBJECT-TYPE
    SYNTAX  INTEGER (4..30)
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for ForwardDelay when this 
         bridge is acting as the root."
    ::= { stgNewCfgTableEntry 10 }

stgNewCfgBrgMaxAge OBJECT-TYPE
    SYNTAX  INTEGER (6..40)
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for MaxAge when this bridge
         is acting as the root."
    ::= { stgNewCfgTableEntry 11 }


stgNewCfgVlanBmap OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(0..512)) 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	"The vlans applied to the spanning tree group.  The vlans are 
         presented in bitmap format. This string displays vlan number
	 from 1 to 4095.

	 in receiving order:

	     OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx ..... 
             ||    || |_ vlan 9
             ||    ||  
             ||    ||___ vlan 8
             ||    |____ vlan 7
             ||      .    .   .
             ||_________ vlan 2
             |__________ vlan 1 (as index to stgCurCfgTable)

         where x : 1 - The represented vlan applied to the spanning tree. 
		   0 - The represented vlan not applied to the spanning tree"
    ::= { stgNewCfgTableEntry 13 }


stgCurCfgPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF StgCurCfgPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of Spanning Tree Group port configuration in the
         current_config."
    ::= { stgCfg 3 }

stgCurCfgPortTableEntry OBJECT-TYPE
    SYNTAX StgCurCfgPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about port configuration of a particular Spanning Tree
         Group."
    INDEX { stgCurCfgStgIndex, stgCurCfgPortIndex }
    ::= { stgCurCfgPortTable 1 }

StgCurCfgPortTableEntry ::= SEQUENCE {
    stgCurCfgStgIndex      Integer32,
    stgCurCfgPortIndex     Integer32,
    stgCurCfgPortState     INTEGER,
    stgCurCfgPortPriority  INTEGER,
    stgCurCfgPortPathCost  INTEGER,
    stgCurCfgPortLink      INTEGER,
    stgCurCfgPortEdge      INTEGER,
    stgCurCfgPortFastFwd   INTEGER
    }

stgCurCfgStgIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The identifier of a particular Spanning Tree Group.  This is also
         index to the entLogicalTable of Entity MIB."
    ::= { stgCurCfgPortTableEntry 1 }

stgCurCfgPortIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The port identifier of a particular Spanning Tree Group."
    ::= { stgCurCfgPortTableEntry 2 }

stgCurCfgPortState OBJECT-TYPE
    SYNTAX INTEGER {
        on(1),
        off(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Turn on of off Spanning Tree operation of a particular port of a
         Spanning Tree Group."
    ::= { stgCurCfgPortTableEntry 3 }

stgCurCfgPortPriority OBJECT-TYPE
    SYNTAX INTEGER (0..255)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The value of the priority field which is contained in the first 
         (in network byte order) octet of the (2 octet long) Port ID."
    ::= { stgCurCfgPortTableEntry 4 }

stgCurCfgPortPathCost OBJECT-TYPE
    SYNTAX INTEGER (0..65535)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
       "The contribution of this port to the path cost of paths towards the 
        spanning tree root which include this port."
    ::= { stgCurCfgPortTableEntry 5 }

stgCurCfgPortLink OBJECT-TYPE
    SYNTAX INTEGER {
        auto(1),
        p2p(2),
        shared(3)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The type of the port link."
    ::= { stgCurCfgPortTableEntry 6 }

stgCurCfgPortEdge OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The state of port edge."
    ::= { stgCurCfgPortTableEntry 7 }

stgCurCfgPortFastFwd OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The state of port fast forwarding."
    ::= { stgCurCfgPortTableEntry 8 }

stgNewCfgPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF StgNewCfgPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of Spanning Tree Group port configuration in the
         new_config."
    ::= { stgCfg 4 }

stgNewCfgPortTableEntry OBJECT-TYPE
    SYNTAX StgNewCfgPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about port configuration of a particular Spanning Tree
         Group."
    INDEX { stgNewCfgStgIndex, stgNewCfgPortIndex }
    ::= { stgNewCfgPortTable 1 }

StgNewCfgPortTableEntry ::= SEQUENCE {
    stgNewCfgStgIndex      Integer32,
    stgNewCfgPortIndex     Integer32,
    stgNewCfgPortState     INTEGER,
    stgNewCfgPortPriority  INTEGER,
    stgNewCfgPortPathCost  INTEGER,
    stgNewCfgPortLink      INTEGER,
    stgNewCfgPortEdge      INTEGER,
    stgNewCfgPortFastFwd   INTEGER
    }

stgNewCfgStgIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The identifier of a particular Spanning Tree Group.  This is also
         index to the entLogicalTable of Entity MIB."
    ::= { stgNewCfgPortTableEntry 1 }

stgNewCfgPortIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The port identifier of a particular Spanning Tree Group."
    ::= { stgNewCfgPortTableEntry 2 }

stgNewCfgPortState OBJECT-TYPE
    SYNTAX INTEGER {
        on(1),
        off(2)
        }
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Turn on of off Spanning Tree operation of a particular port of a
         Spanning Tree Group."
    ::= { stgNewCfgPortTableEntry 3 }

stgNewCfgPortPriority OBJECT-TYPE
    SYNTAX INTEGER (0..255)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The value of the priority field which is contained in the first 
         (in network byte order) octet of the (2 octet long) Port ID."
    ::= { stgNewCfgPortTableEntry 4 }

stgNewCfgPortPathCost OBJECT-TYPE
    SYNTAX INTEGER (0..65535)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
       "The contribution of this port to the path cost of paths towards the 
        spanning tree root which include this port."
    ::= { stgNewCfgPortTableEntry 5 }

stgNewCfgPortLink OBJECT-TYPE
    SYNTAX INTEGER {
        auto(1),
        p2p(2),
        shared(3)
        }
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The type of the port link."
    ::= { stgNewCfgPortTableEntry 6 }

stgNewCfgPortEdge OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The state of port edge."
    ::= { stgNewCfgPortTableEntry 7 }

stgNewCfgPortFastFwd OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The state of port fast forwarding."
    ::= { stgNewCfgPortTableEntry 8 }

-- MST Configuration 

mstCurCfgState	OBJECT-TYPE
    SYNTAX  INTEGER  {
	enabled(2),
	disabled(3)
	}
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable MSTP/RSTP"
    ::= { mstGeneralCfg 1 }

mstNewCfgState	OBJECT-TYPE
    SYNTAX  INTEGER  {
	enabled(2),
	disabled(3)
	}
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable MSTP/RSTP"
    ::= { mstGeneralCfg 2 }

mstCurCfgRegionName OBJECT-TYPE
   SYNTAX  DisplayString (SIZE (0..32))
   MAX-ACCESS  read-only
   STATUS  current
   DESCRIPTION
      "The Name for the Region's configuration."
   ::= { mstGeneralCfg 3 } 

mstNewCfgRegionName OBJECT-TYPE
   SYNTAX  DisplayString (SIZE (0..32))
   MAX-ACCESS  read-write
   STATUS  current
   DESCRIPTION
      "The Name for the Region's configuration."
   ::= { mstGeneralCfg 4 } 

mstCurCfgRegionVersion OBJECT-TYPE
    SYNTAX  INTEGER  (0..65535)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Version of the MST Region."
    ::= { mstGeneralCfg 5 }

mstNewCfgRegionVersion OBJECT-TYPE
    SYNTAX  INTEGER  (0..65535)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Version of the MST Region."
    ::= { mstGeneralCfg 6 }

mstCurCfgMaxHopCount OBJECT-TYPE
    SYNTAX  INTEGER  (4..60)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Indicates the maximum hop count value."
    ::= { mstGeneralCfg 7 }

mstNewCfgMaxHopCount OBJECT-TYPE
    SYNTAX  INTEGER  (4..60)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Indicates the maximum hop count value."
    ::= { mstGeneralCfg 8 }

mstCurCfgStpMode OBJECT-TYPE
    SYNTAX  INTEGER  {
        mstp(1),
        rstp(2)
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The version of Spanning Tree Protocal the bridge is currently 
         running."
    ::= { mstGeneralCfg 9 }

mstNewCfgStpMode OBJECT-TYPE
    SYNTAX  INTEGER  {
        mstp(1),
        rstp(2)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The version of Spanning Tree Protocal the bridge is currently 
         running."
    ::= { mstGeneralCfg 10 }

mstCistDefaultCfg OBJECT-TYPE
    SYNTAX INTEGER {
        default(1)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Setting the value to default(1) will set the Multiple
         Spanning Tree and member parameters to default.  default(1) is 
         always returned when read, but it does not mean anything."
    ::= { mstCistCfg 1 }

-- CIST Brige Configuration
mstCistBridgeCfg  OBJECT IDENTIFIER ::= { mstCistCfg 2 }

mstCistCurCfgBridgePriority OBJECT-TYPE
    SYNTAX  INTEGER  (0..65535)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value of the writable portion of the Brigde Identifier comprising
         of the first two octets."
    ::= { mstCistBridgeCfg 1 }

mstCistNewCfgBridgePriority OBJECT-TYPE
    SYNTAX  INTEGER  (0..65535)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The value of the writable portion of the Brigde Identifier comprising
         of the first two octets."
    ::= { mstCistBridgeCfg 2 }


mstCistCurCfgBridgeMaxAge OBJECT-TYPE
    SYNTAX  INTEGER  (6..40)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for MaxAge when this bridge
         is acting as the root."
    ::= { mstCistBridgeCfg 5 }

mstCistNewCfgBridgeMaxAge OBJECT-TYPE
    SYNTAX  INTEGER  (6..40)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for MaxAge when this bridge
         is acting as the root."
    ::= { mstCistBridgeCfg 6 }

mstCistCurCfgBridgeForwardDelay OBJECT-TYPE
    SYNTAX  INTEGER  (4..30)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for ForwardDelay when this 
         bridge is acting as the root."
    ::= { mstCistBridgeCfg 7 }

mstCistNewCfgBridgeForwardDelay OBJECT-TYPE
    SYNTAX  INTEGER  (4..30)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for ForwardDelay when this 
         bridge is acting as the root."
    ::= { mstCistBridgeCfg 8 }

mstCistCurCfgVlanBmap OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(0..512)) 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
    "The vlans applied to the CIST group.  The vlans are 
     presented in bitmap format. This string displays vlan number
     from 1 to 4094.

     in receiving order:

         OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx ..... 
             ||    || |_ vlan 9
             ||    ||  
             ||    ||___ vlan 8
             ||    |____ vlan 7
             ||      .    .   .
             ||_________ vlan 2
             |__________ vlan 1

         where x : 1 - The represented vlan applied to the CIST group. 
                   0 - The represented vlan not applied to the group"
    ::= { mstCistBridgeCfg 9 }

mstCistNewCfgVlanBmap OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(0..512)) 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
    "The vlans applied to the CIST group.  The vlans are 
     presented in bitmap format. This string displays vlan number
     from 1 to 4094.

     in receiving order:

         OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx ..... 
             ||    || |_ vlan 9
             ||    ||  
             ||    ||___ vlan 8
             ||    |____ vlan 7
             ||      .    .   .
             ||_________ vlan 2
             |__________ vlan 1

         where x : 1 - The represented vlan applied to the CIST group. 
                   0 - The represented vlan not applied to the group"
    ::= { mstCistBridgeCfg 10 }

mstCistNewCfgAddVlan OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The vlan to be added to the CIST Group.  A 
         '0' value is returned when read." 
    ::= { mstCistBridgeCfg 11 }

-- CIST Port Configuration

mstCistCurCfgPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MstCistCurCfgPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of CIST Port configuration."
    ::= { mstCistCfg 3 }

mstCistCurCfgPortTableEntry OBJECT-TYPE
    SYNTAX MstCistCurCfgPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a particular CIST Port configuration."
    INDEX { mstCistCurCfgPortIndex }
    ::= { mstCistCurCfgPortTable 1 }

MstCistCurCfgPortTableEntry ::= SEQUENCE {
    mstCistCurCfgPortIndex      Integer32,
    mstCistCurCfgPortPriority   INTEGER,
    mstCistCurCfgPortPathCost   INTEGER,
    mstCistCurCfgPortLinkType   INTEGER,
    mstCistCurCfgPortEdge       INTEGER,
    mstCistCurCfgPortStpState   INTEGER,
    mstCistCurCfgPortHelloTime  INTEGER
    }

mstCistCurCfgPortIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The port number of the port for which this entry contains spanning
         tree configuration."
    ::= { mstCistCurCfgPortTableEntry 1 }

mstCistCurCfgPortPriority OBJECT-TYPE
    SYNTAX INTEGER (0..240)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The four most significant bits of the Port Identifier of the 
         Spanning Tree instance can be modified by setting this value."
    ::= { mstCistCurCfgPortTableEntry 2 }

mstCistCurCfgPortPathCost OBJECT-TYPE
    SYNTAX INTEGER (0..200000000)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The contribution of this port to the path cost of paths towards 
         the CIST Root which include this port."
    ::= { mstCistCurCfgPortTableEntry 3 }

mstCistCurCfgPortLinkType OBJECT-TYPE
    SYNTAX INTEGER {
        auto(1),
        p2p(2),
        shared(3)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The administrative point-to-point status of the LAN segment attached 
         to this port.  A value of p2p (2) indicates that this port should 
         always be treated as if it is connected to a point-to-point link. 
         A value of shared(3) indicates that this port should be treated as 
         having a shared media connection.  A value of auto(1) indicates that 
         this port is considered to have a point-to-point link if it is an 
         Aggregator and all of its members are aggregatable, or if the MAC 
         entity is configured for full duplex operation, either through
         auto-negotiation or by management means."    
    ::= { mstCistCurCfgPortTableEntry 4 }

mstCistCurCfgPortEdge OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The value of the Edge Port parameter."
    ::= { mstCistCurCfgPortTableEntry 5 }

mstCistCurCfgPortStpState OBJECT-TYPE
    SYNTAX INTEGER {
        on(1),
        off(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Turn port's Spanning Tree on/off."
    ::= { mstCistCurCfgPortTableEntry 6 }

mstCistCurCfgPortHelloTime OBJECT-TYPE
    SYNTAX  INTEGER (1..10)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The amount of time between the transmission of Configuration Port 
         PDUs in seconds."
    ::= { mstCistCurCfgPortTableEntry 7 } 

mstCistNewCfgPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MstCistNewCfgPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of CIST Port configuration."
    ::= { mstCistCfg 4 }

mstCistNewCfgPortTableEntry OBJECT-TYPE
    SYNTAX MstCistNewCfgPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a particular CIST Port configuration."
    INDEX { mstCistNewCfgPortIndex }
    ::= { mstCistNewCfgPortTable 1 }

MstCistNewCfgPortTableEntry ::= SEQUENCE {
    mstCistNewCfgPortIndex      Integer32,
    mstCistNewCfgPortPriority   INTEGER,
    mstCistNewCfgPortPathCost   INTEGER,
    mstCistNewCfgPortLinkType   INTEGER,
    mstCistNewCfgPortEdge       INTEGER,
    mstCistNewCfgPortStpState   INTEGER,
    mstCistNewCfgPortHelloTime  INTEGER
    }

mstCistNewCfgPortIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The port number of the port for which this entry contains spanning
         tree configuration."
    ::= { mstCistNewCfgPortTableEntry 1 }

mstCistNewCfgPortPriority OBJECT-TYPE
    SYNTAX INTEGER (0..240)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The four most significant bits of the Port Identifier of the 
         Spanning Tree instance can be modified by setting this value."
    ::= { mstCistNewCfgPortTableEntry 2 }

mstCistNewCfgPortPathCost OBJECT-TYPE
    SYNTAX INTEGER (0..200000000)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The contribution of this port to the path cost of paths towards 
         the CIST Root which include this port."
    ::= { mstCistNewCfgPortTableEntry 3 }

mstCistNewCfgPortLinkType OBJECT-TYPE
    SYNTAX INTEGER {
        auto(1),
        p2p(2),
        shared(3)
        }
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The administrative point-to-point status of the LAN segment attached 
         to this port.  A value of p2p (2) indicates that this port should 
         always be treated as if it is connected to a point-to-point link. 
         A value of shared(3) indicates that this port should be treated as 
         having a shared media connection.  A value of auto(1) indicates that 
         this port is considered to have a point-to-point link if it is an 
         Aggregator and all of its members are aggregatable, or if the MAC 
         entity is configured for full duplex operation, either through
         auto-negotiation or by management means."    
    ::= { mstCistNewCfgPortTableEntry 4 }

mstCistNewCfgPortEdge OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The value of the Edge Port parameter."
    ::= { mstCistNewCfgPortTableEntry 5 }

mstCistNewCfgPortStpState OBJECT-TYPE
    SYNTAX INTEGER {
        on(1),
        off(2)
        }
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Turn port's Spanning Tree on/off."
    ::= { mstCistNewCfgPortTableEntry 6 }

mstCistNewCfgPortHelloTime OBJECT-TYPE
    SYNTAX  INTEGER (1..10)
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The amount of time between the transmission of Configuration Port 
         PDUs in seconds."
    ::= { mstCistNewCfgPortTableEntry 7 } 

-- Complete Port Mirroring 
pmCurCfgPortMirrState OBJECT-TYPE
    SYNTAX  INTEGER {
	enabled(1),
	disabled(2)
	}
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The state of port-based port mirroring."
    ::= { mirrPortMirr 1 }
 
pmNewCfgPortMirrState OBJECT-TYPE
    SYNTAX  INTEGER {
	enabled(1),
	disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The state of port-based port mirroring."
    ::= { mirrPortMirr 2 }

pmCurCfgPortMonitorTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF PmCurCfgPortMonitorEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of monitoring ports."
    ::= { mirrPortMirr 3 }

pmCurCfgPortMonitorEntry OBJECT-TYPE
    SYNTAX  PmCurCfgPortMonitorEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the monitoring port table."
    INDEX   { pmCurCfgPmirrMoniPortIndex, pmCurCfgPmirrMirrPortIndex }
    ::= { pmCurCfgPortMonitorTable 1 }

PmCurCfgPortMonitorEntry ::= SEQUENCE {
    pmCurCfgPmirrMoniPortIndex       Integer32,
    pmCurCfgPmirrMirrPortIndex       Integer32,
    pmCurCfgPmirrDirection           INTEGER
    }

pmCurCfgPmirrMoniPortIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The monitoring port number." 
    ::= { pmCurCfgPortMonitorEntry 1 }

pmCurCfgPmirrMirrPortIndex OBJECT-TYPE 
    SYNTAX  Integer32 
    MAX-ACCESS  read-only 
    STATUS  current 
    DESCRIPTION 
        "The mirrored port number" 
    ::= { pmCurCfgPortMonitorEntry 2 }

pmCurCfgPmirrDirection OBJECT-TYPE
    SYNTAX  INTEGER {
	in(1),
	out(2),
	both(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The type of traffic to be monitored with respect to the
         mirrored port."
    ::= { pmCurCfgPortMonitorEntry 3 }


pmNewCfgPortMonitorTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF PmNewCfgPortMonitorEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of monitoring ports."
    ::= { mirrPortMirr 4 }

pmNewCfgPortMonitorEntry OBJECT-TYPE
    SYNTAX  PmNewCfgPortMonitorEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the monitoring port table."
    INDEX   { pmNewCfgPmirrMoniPortIndex, pmNewCfgPmirrMirrPortIndex }
    ::= { pmNewCfgPortMonitorTable 1 }

PmNewCfgPortMonitorEntry ::= SEQUENCE {
    pmNewCfgPmirrMoniPortIndex          Integer32,
    pmNewCfgPmirrMirrPortIndex          Integer32,
    pmNewCfgPmirrDirection              INTEGER,
    pmNewCfgPmirrDelete                 INTEGER,
    pmNewCfgPmonDelete                 INTEGER
    }

pmNewCfgPmirrMoniPortIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The monitoring port number." 
    ::= { pmNewCfgPortMonitorEntry 1 }

pmNewCfgPmirrMirrPortIndex OBJECT-TYPE 
    SYNTAX  Integer32 
    MAX-ACCESS  read-only 
    STATUS  current 
    DESCRIPTION 
        "The mirrored port number" 
    ::= { pmNewCfgPortMonitorEntry 2 }

pmNewCfgPmirrDirection OBJECT-TYPE
    SYNTAX  INTEGER {
	in(1),
	out(2),
	both(3)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The type of traffic to be monitored with respect to the
         mirrored port."
    ::= { pmNewCfgPortMonitorEntry 3 }

pmNewCfgPmirrDelete OBJECT-TYPE
    SYNTAX  INTEGER  {
        other(1),
        delete(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Setting the value to delete(2) will delete the entire
         row. When read, other(1) is returned."
    ::= { pmNewCfgPortMonitorEntry 4 }


pmNewCfgPmonDelete OBJECT-TYPE
    SYNTAX  INTEGER  {
        other(1),
        delete(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Setting the value to delete(2) will delete the monitor
         port. When read, other(1) is returned."
    ::= { pmNewCfgPortMonitorEntry 10 }

-- Link Aggregation Control Protocol Group
lacpCurSystemPriority OBJECT-TYPE
    SYNTAX  INTEGER (1..65535)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
       "A 2-octet read-write value indicating the priority
        value associated with the Actor's System ID."
    ::= { lacp 1 }

lacpNewSystemPriority OBJECT-TYPE
    SYNTAX  INTEGER (1..65535)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "A 2-octet read-write value indicating the priority
        value associated with the Actor's System ID."
    ::= { lacp 2 }

lacpCurSystemTimeoutTime OBJECT-TYPE
    SYNTAX  INTEGER  {
        short(3),
        long(90)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "If a port does not receive LACPDUs for Timeout time LACP 
         information pertaining to the port is invalidated.
         Its every 3 sec (short) and every 90 sec (long 3)."
    ::= { lacp 5 }

lacpNewSystemTimeoutTime OBJECT-TYPE
    SYNTAX  INTEGER  {
        short(3),
        long(90)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "If a port does not receive LACPDUs for Timeout time LACP 
         information pertaining to the port is invalidated.
         Its every 3 sec (short) and every 90 sec (long 3)."
    ::= { lacp 6 }

lacpCurPortCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF LacpCurPortCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of LACP port configuration."
    ::= { lacp 7 }

lacpCurPortCfgTableEntry OBJECT-TYPE
    SYNTAX  LacpCurPortCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the LACP port configuration table."
    INDEX  { lacpCurPortCfgTableId }
    ::= { lacpCurPortCfgTable 1 }

LacpCurPortCfgTableEntry ::= SEQUENCE {
    lacpCurPortCfgTableId 	    Integer32,
    lacpCurPortState                INTEGER, 
    lacpCurPortActorPortPriority    INTEGER, 
    lacpCurPortActorAdminKey        INTEGER 
    }

lacpCurPortCfgTableId OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
          " LACP port number."
    ::= { lacpCurPortCfgTableEntry 1 }

lacpCurPortState OBJECT-TYPE
    SYNTAX  INTEGER  {
        off(1),
        active(2),
        passive(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "LACP port state can be one of three states 
         off (Not participating in LACP) 
         Active (Initiates LACPDU updates)
         Passive (Does not initiate LACPDU updates but responds to peer."
    ::= { lacpCurPortCfgTableEntry 2 }

lacpCurPortActorPortPriority OBJECT-TYPE
    SYNTAX       INTEGER (1..65535)
    MAX-ACCESS       read-only
    STATUS       current
    DESCRIPTION
        "The priority value assigned to this Aggregation Port.
        This 16-bit value is read-only."
    ::= { lacpCurPortCfgTableEntry 3 }

lacpCurPortActorAdminKey OBJECT-TYPE
    SYNTAX       INTEGER (1..65535)
    MAX-ACCESS       read-only
    STATUS       current
    DESCRIPTION
        "The current administrative value of the Key for the
        Aggregation Port. This is a 16-bit read-only value.
        The meaning of particular Key values is of local
        significance."
    ::= { lacpCurPortCfgTableEntry 4 }

lacpNewPortCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF LacpNewPortCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of LACP port configuration."
    ::= { lacp 8 }

lacpNewPortCfgTableEntry OBJECT-TYPE
    SYNTAX  LacpNewPortCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the LACP port configuration table."
    INDEX  { lacpNewPortCfgTableId }
    ::= { lacpNewPortCfgTable 1 }

LacpNewPortCfgTableEntry ::= SEQUENCE {
    lacpNewPortCfgTableId 	    Integer32,
    lacpNewPortState                INTEGER, 
    lacpNewPortActorPortPriority    INTEGER, 
    lacpNewPortActorAdminKey        INTEGER 
    }

lacpNewPortCfgTableId OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
          " LACP port number."
    ::= { lacpNewPortCfgTableEntry 1 }

lacpNewPortState OBJECT-TYPE
    SYNTAX  INTEGER  {
        off(1),
        active(2),
        passive(3)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "LACP port state can be one of three states 
         off (Not participating in LACP) 
         Active (Initiates LACPDU updates)
         Passive (Does not initiate LACPDU updates but responds to peer."
    ::= { lacpNewPortCfgTableEntry 2 }

lacpNewPortActorPortPriority OBJECT-TYPE
    SYNTAX       INTEGER (1..65535)
    MAX-ACCESS       read-write
    STATUS       current
    DESCRIPTION
        "The priority value assigned to this Aggregation Port.
        This 16-bit value is read-write."
    ::= { lacpNewPortCfgTableEntry 3 }

lacpNewPortActorAdminKey OBJECT-TYPE
    SYNTAX       INTEGER (1..65535)
    MAX-ACCESS       read-write
    STATUS       current
    DESCRIPTION
        "The current administrative value of the Key for the
        Aggregation Port. This is a 16-bit read-write value.
        The meaning of particular Key values is of local
        significance."
    ::= { lacpNewPortCfgTableEntry 4 }

-- L2 general
upfastCurCfgState OBJECT-TYPE
    SYNTAX  INTEGER  {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable uplink fast"
    ::= { l2GeneralCfg 1 }

upfastNewCfgState OBJECT-TYPE
    SYNTAX  INTEGER  {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable uplink fast"
    ::= { l2GeneralCfg 2 }

updateCurCfgState OBJECT-TYPE
    SYNTAX  INTEGER  (10..200)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "UplinkFast station update rate: packets per second"
    ::= { l2GeneralCfg 3 }

updateNewCfgState OBJECT-TYPE
    SYNTAX  INTEGER  (10..200)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "UplinkFast station update rate: packets per second"
    ::= { l2GeneralCfg 4 }

pvstCompatibilityCurCfgState OBJECT-TYPE
    SYNTAX INTEGER  {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable PVST+ compatibility"
    ::= { l2GeneralCfg 9 }

pvstCompatibilityNewCfgState OBJECT-TYPE
    SYNTAX INTEGER  {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable PVST+ compatibility"
    ::= { l2GeneralCfg 10 }

-- FDB Statistics


fdbStatsCurrent OBJECT-TYPE
    SYNTAX  Gauge32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Current number of entries in the Forwarding Database."
    ::= { fdbStats 3 }

fdbStatsHiwat OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Highest number of entries recorded at any given time in the 
         Forwarding Database."
    ::= { fdbStats 4 }


fdbStatsClear OBJECT-TYPE
    SYNTAX INTEGER {
      ok(1),
      clear(2) 
      } 
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Clear FDB statistics"
    ::= { fdbStats 11 }


-- STP Statistics

stgStatsPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF StgStatsPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of Spanning Tree Group port statistics."
    ::= { stpStats 1 }

stgStatsPortTableEntry OBJECT-TYPE
    SYNTAX StgStatsPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Statistics about port of a particular Spanning Tree Group."
    INDEX { stgStatsStpIndex, stgStatsPortIndex }
    ::= { stgStatsPortTable 1 }

StgStatsPortTableEntry ::= SEQUENCE {
    stgStatsStpIndex            Integer32,
    stgStatsPortIndex	        Integer32,
    stgStatsPortRcvCfgBpdus     Counter32,
    stgStatsPortRcvTcnBpdus     Counter32,
    stgStatsPortXmtCfgBpdus     Counter32,
    stgStatsPortXmtTcnBpdus     Counter32 
    }

stgStatsStpIndex OBJECT-TYPE
    SYNTAX Integer32  
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The identifier of a particular Spanning Tree Group."
    ::= { stgStatsPortTableEntry 1 }

stgStatsPortIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The port identifier of a particular Spanning Tree Group."
    ::= { stgStatsPortTableEntry 2 }

stgStatsPortRcvCfgBpdus OBJECT-TYPE
    SYNTAX Counter32 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Number of Configuration BPDU's received on this port."
    ::= { stgStatsPortTableEntry 3 }

stgStatsPortRcvTcnBpdus OBJECT-TYPE
    SYNTAX Counter32 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Number of TCN BPDU's received on this port."
    ::= { stgStatsPortTableEntry 4 }

stgStatsPortXmtCfgBpdus OBJECT-TYPE
    SYNTAX Counter32 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Number of Configuration BPDU's trasmitted from the port."
    ::= { stgStatsPortTableEntry 5 }

stgStatsPortXmtTcnBpdus OBJECT-TYPE
    SYNTAX Counter32 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Number of TCN BPDU's trasmitted from the port."
    ::= { stgStatsPortTableEntry 6 }


-- LACP Statistics

lacpStatsTable OBJECT-TYPE
    SYNTAX SEQUENCE OF LacpStatsTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of LACP Stats."
	::= {lacpStats 1}

lacpStatsTableEntry OBJECT-TYPE
    SYNTAX LacpStatsTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Lacp status info."
    INDEX { lacpStatsIndex }
    ::= { lacpStatsTable 1 }

LacpStatsTableEntry ::= SEQUENCE {
   lacpStatsIndex Integer32,
   lacpdusRx Integer32,
   markerpdusRx Integer32,
   markerresponsepdusRx Integer32,
   unknownRx Integer32,
   illegalRx Integer32,
   lacpdusTx Integer32,
   markerpdusTx Integer32,
   markerresponsepdusTx Integer32,
   lacpClearStats INTEGER
}

lacpStatsIndex OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
	"Index"
  ::= {lacpStatsTableEntry 1}

lacpdusRx OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
	"Valid LACPDUs received"
  ::= {lacpStatsTableEntry 2}

markerpdusRx OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
	"Valid Marker PDUs received"
  ::= {lacpStatsTableEntry 3}

markerresponsepdusRx OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
	"Valid Marker Rsp PDUs received"
  ::= {lacpStatsTableEntry 4}

unknownRx OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
	"Unknown version/TLV type"
  ::= {lacpStatsTableEntry 5}

illegalRx OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
	"Illegal subtype received"
  ::= {lacpStatsTableEntry 6}

lacpdusTx OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
	"LACPDUs transmitted"
  ::= {lacpStatsTableEntry 7}

markerpdusTx OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
	"Market PDUs transmitted"
  ::= {lacpStatsTableEntry 8}

markerresponsepdusTx OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
	"Marker Rsp PDUs transmitted "
  ::= {lacpStatsTableEntry 9}

lacpClearStats  OBJECT-TYPE
    SYNTAX  INTEGER {
        ok(1),
        clear(2)
        }
    MAX-ACCESS  read-write
    STATUS  current 
    DESCRIPTION 
        "Setting this to clear(2) results in clearing the LACP statistics."
    ::= { lacpStatsTableEntry 10 }


-- UFD stats

ufdNoLtMLinkFailure OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
	" "
  ::= {ufdStats 1}

ufdNoLtMLinkBlockingState OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
	" "
  ::= {ufdStats 2}

ufdNoLtDAutoDisabled OBJECT-TYPE
  SYNTAX Integer32
  MAX-ACCESS read-only
  STATUS current
  DESCRIPTION
	" "
  ::= {ufdStats 3}

ufdClearStats OBJECT-TYPE
  SYNTAX INTEGER {
      ok(1),
      clear(2)
  }
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION
	" Setting this value to clear(2) clears the UFD stats."
  ::= {ufdStats 4}






-- FDB stats

fdbClear OBJECT-TYPE
    SYNTAX  INTEGER {
        ok(1),
        clear(2)
        }
    MAX-ACCESS  read-write
    STATUS  current 
    DESCRIPTION
        "Setting this value to clear(2) clears the entire master FDB."
    ::= { fdbInfo 1 }

fdbTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF FdbEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of FDB entries."
    ::= { fdbInfo 2 }

fdbEntry OBJECT-TYPE
    SYNTAX  FdbEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the FDB table"
    INDEX   { fdbMacAddr }
    ::= { fdbTable 1 }

FdbEntry ::= SEQUENCE {
    fdbMacAddr            PhysAddress,
    fdbVlan       	  Integer32,
    fdbSrcPort            Integer32,
    fdbSrcTrunk           Integer32,
    fdbState              INTEGER,
    fdbRefSps             DisplayString,
    fdbLearnedPort        Integer32,
    fdbStatus             Integer32
    }

fdbMacAddr OBJECT-TYPE
    SYNTAX  PhysAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The MAC address for the FDB entry."
    ::= { fdbEntry 1 }

fdbVlan OBJECT-TYPE 
    SYNTAX  Integer32 
    MAX-ACCESS  read-only 
    STATUS  current 
    DESCRIPTION 
        "The VLAN ID for the FDB entry." 
    ::= { fdbEntry 2 }

fdbSrcPort OBJECT-TYPE  
    SYNTAX  Integer32 
    MAX-ACCESS  read-only  
    STATUS  current  
    DESCRIPTION  
       "Either the value '0', or the port number of the port on which a frame 
        having a source address equal to the value of the corresponding 
        instance has been seen.  A value of '0' indicates that the port 
        number has not been learned but that the bridge does have some
        forwarding/filtering information about this address."
    ::= { fdbEntry 3 }

fdbState OBJECT-TYPE  
    SYNTAX  INTEGER {
        unknown(1),
        forward(2),
        trunk(3)
        }
    MAX-ACCESS  read-only  
    STATUS  current  
    DESCRIPTION  
        "The state of the FDB entry. The meanings of the values are :
         unknown(1) : the MAC address has not yet been learned by the switch
                      but has only been seen as a destination address
         forward(2) : the MAC address has been learned by the switch
         trunk(3)   : frames with this MAC address are forwarded to trunk
                      group"
    ::= { fdbEntry 4 }

fdbRefSps OBJECT-TYPE   
    SYNTAX  DisplayString (SIZE(0..32))
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The referenced SPs associated with this FDB entry."   
    ::= { fdbEntry 5 }

fdbLearnedPort OBJECT-TYPE   
    SYNTAX  Integer32  
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The learned port associated with this FDB entry."   
    ::= { fdbEntry 6 }

fdbSrcTrunk OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
       "Either the value '0', or the trunk number of the trunk on which a frame
        having a source address equal to the value of the corresponding
        instance has been seen.  A value of '0' indicates that the source
        address is not associated with a trunk."
    ::= { fdbEntry 7 }

fdbStatus OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
       "'1'  if it is permanent 
        '0'  if it is not permanent"
    ::= { fdbEntry 8 }
    


-- STP information

stpInfoTable OBJECT-TYPE
    SYNTAX SEQUENCE OF StpInfoTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of Spanning Tree Group information."
    ::= { stpInfo 1 }

stpInfoTableEntry OBJECT-TYPE
    SYNTAX StpInfoTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a particular Spanning Tree Group."
    INDEX { stpInfoIndex }
    ::= { stpInfoTable 1 }

StpInfoTableEntry ::= SEQUENCE {
    stpInfoIndex              Integer32,
    stpInfoState              INTEGER,
    stgInfoVlanBmap           OCTET STRING,
    stpInfoTimeSinceTopChange TimeTicks,
    stpInfoTopChanges         Counter32,
    stpInfoDesignatedRoot     BridgeId,
    stpInfoRootCost           Integer32,
    stpInfoRootPort           Integer32,
    stpInfoHelloTime          Integer32,
    stpInfoMaxAge             Integer32,
    stpInfoForwardDelay       Integer32,
    stpInfoHoldTime           Integer32,
    stpInfoBrgPriority        INTEGER,
    stpInfoBrgHelloTime       INTEGER,
    stpInfoBrgForwardDelay    INTEGER,
    stpInfoBrgMaxAge          INTEGER,
    stpInfoAgingTime          INTEGER
    }

stpInfoIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The identifier of a particular Spanning Tree Group.  This is also
         index to the entLogicalTable of Entity MIB."
    ::= { stpInfoTableEntry 1 }

stpInfoState OBJECT-TYPE
    SYNTAX INTEGER {
        on(1),
        off(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Turn on of off Spanning Tree operation of a particular Spanning
         Tree Group."
    ::= { stpInfoTableEntry 2 }

stgInfoVlanBmap OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(0..512)) 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The vlans applied to the spanning tree group.  The vlans are 
         presented in bitmap format. This string displays vlan number
         from 1 to 4096.

         in receiving order:

             OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx ..... 
             ||    || |_ vlan 9
             ||    ||  
             ||    ||___ vlan 8
             ||    |____ vlan 7
             ||      .    .   .
             ||_________ vlan 2
             |__________ vlan 1 (as index to stgCurCfgTable)

         where x : 1 - The represented vlan applied to the spanning tree. 
                   0 - The represented vlan not applied to the spanning tree"
    ::= { stpInfoTableEntry 3 }

stpInfoTimeSinceTopChange OBJECT-TYPE
    SYNTAX  TimeTicks
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The time (in hundredths of a second) since the last time a topology 
         change was detected by the bridge entity."
    ::= { stpInfoTableEntry 4 }

stpInfoTopChanges OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of topology changes detected by this bridge since 
         the management entity was last reset or initialized."
    ::= { stpInfoTableEntry 5 }

stpInfoDesignatedRoot OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The bridge identifier of the root of the spanning tree as determined 
         by the Spanning Tree Protocol as executed by this node.  This value 
         is used as the Root Identifier parameter in all Configuration Bridge 
         PDUs originated by this node."
    ::= { stpInfoTableEntry 6 }

stpInfoRootCost OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The cost of the path to the root as seen from this bridge."
    ::= { stpInfoTableEntry 7 }

stpInfoRootPort OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port number of the port which offers the lowest cost path from 
         this bridge to the root bridge."
    ::= { stpInfoTableEntry 8 }

stpInfoMaxAge OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum age of Spanning Tree Protocol information learned from 
         the network on any port before it is discarded, in units of 
         hundredths of a second.  This is the actual value that this bridge is
         currently using."
    ::= { stpInfoTableEntry 9 }

stpInfoHelloTime OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The amount of time between the transmission of Configuration bridge 
         PDUs by this node on any port when it is the root of the spanning 
         tree or trying to become so, in units of hundredths of a second.
         This is the actual value that this bridge is currently using."
    ::= { stpInfoTableEntry 10 }

stpInfoForwardDelay OBJECT-TYPE
     SYNTAX  Integer32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
         "This time value, measured in units of hundredths of a second, 
          controls how fast a port changes its spanning state when moving 
          towards the Forwarding state.  The value determines how long the port
          stays in each of the Listening and Learning states, which precede 
          the Forwarding state.  This value is also used, when a topology 
          change has been detected and is underway, to age all dynamic entries
          in the Forwarding Database."
    ::= { stpInfoTableEntry 11 }

stpInfoHoldTime OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This time value determines the interval length during which no more 
         than two Configuration bridge PDUs shall be transmitted by this node,
         in units of hundredths of a second."
    ::= { stpInfoTableEntry 12 }

stpInfoBrgPriority OBJECT-TYPE
    SYNTAX  INTEGER (0..65535)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value of the write-able portion of the Bridge ID, i.e., the first
         two octets of the (8 octet long) Bridge ID."
    ::= { stpInfoTableEntry 13 }

stpInfoBrgHelloTime OBJECT-TYPE
    SYNTAX  INTEGER (1..10)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for HelloTime when this 
         bridge is acting as the root."
    ::= { stpInfoTableEntry 14 }

stpInfoBrgForwardDelay OBJECT-TYPE
    SYNTAX  INTEGER (4..30)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for ForwardDelay when this 
         bridge is acting as the root."
    ::= { stpInfoTableEntry 15 }

stpInfoBrgMaxAge OBJECT-TYPE
    SYNTAX  INTEGER (6..40)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for MaxAge when this bridge
         is acting as the root."
    ::= { stpInfoTableEntry 16 }

stpInfoAgingTime OBJECT-TYPE
    SYNTAX  INTEGER (0..65535)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The timeout period in seconds for aging out dynamically learned 
         forwarding information."
    ::= { stpInfoTableEntry 17 }

stpInfoPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF StpInfoPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of Spanning Tree Group port information."
    ::= { stpInfo 2 }

stpInfoPortTableEntry OBJECT-TYPE
    SYNTAX StpInfoPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about port configuration for a particular Spanning Tree
         Group."
    INDEX { stpInfoPortStpIndex, stpInfoPortIndex }
    ::= { stpInfoPortTable 1 }

StpInfoPortTableEntry ::= SEQUENCE {
    stpInfoPortStpIndex           Integer32,
    stpInfoPortIndex              Integer32,
    stpInfoPortState              INTEGER,
    stpInfoPortDesignatedRoot     BridgeId,
    stpInfoPortDesignatedCost     Integer32,
    stpInfoPortDesignatedBridge   BridgeId,
    stpInfoPortDesignatedPort     OCTET STRING,
    stpInfoPortForwardTransitions Counter32,
    stpInfoPortPathCost           Integer32
   }

stpInfoPortStpIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The identifier of a particular Spanning Tree Group."
    ::= { stpInfoPortTableEntry 1 }

stpInfoPortIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The port identifier of a particular Spanning Tree Group."
    ::= { stpInfoPortTableEntry 2 }

stpInfoPortState OBJECT-TYPE
    SYNTAX  INTEGER {
        disabled(1),
        blocking(2),
        listening(3),
        learning(4),
        forwarding(5),
        broken(6)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port's current state as defined by application of the Spanning 
         Tree Protocol.  This state controls what action a port takes on
         reception of a frame.  If the bridge has detected a port that is 
         malfunctioning it will place that port into the broken(6) state.  
         For ports which are disabled, this object will have a value of 
         disabled(1)."
    ::= { stpInfoPortTableEntry 3 }

stpInfoPortDesignatedRoot OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The unique Bridge Identifier of the Bridge recorded as the Root in 
         the Configuration BPDUs transmitted by the Designated Bridge for the
         segment to which the port is attached."
    ::= { stpInfoPortTableEntry 4 }

stpInfoPortDesignatedCost OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The path cost of the Designated Port of the segment connected to this
         port.  This value is compared to the Root Path Cost field in received
         bridge PDUs."
    ::= { stpInfoPortTableEntry 5 }

stpInfoPortDesignatedBridge OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Bridge Identifier of the bridge which this port considers to be 
         the Designated Bridge for this port's segment."
    ::= { stpInfoPortTableEntry 6 }

stpInfoPortDesignatedPort OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE (2))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Port Identifier of the port on the Designated Bridge for this 
         port's segment."
    ::= { stpInfoPortTableEntry 7 }

stpInfoPortForwardTransitions OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The number of times this port has transitioned from the Learning 
         state to the Forwarding state."
    ::= { stpInfoPortTableEntry 8 }

stpInfoPortPathCost OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The path cost of the port."
    ::= { stpInfoPortTableEntry 9 }

-- CIST Information

cistRoot OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The bridge identifier of the Root of the common spanning
         tree as determined by the Spanning Tree Protocol
         as executed by this node.  This value is used as
         the CIST Root Identifier parameter in all Configuration
         Bridge PDUs originated by this node."
    ::= { cistGeneralInfo 1 } 

cistRootPathCost OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The cost of the path to the CIST Root as seen from this bridge."
    ::= { cistGeneralInfo 2 } 

cistRootPort OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION 
        "The Port Number of the Port which offers the lowest path cost from 
        this bridge to the CIST Root Bridge."
    ::= { cistGeneralInfo 3 } 


cistRootMaxAge OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for MaxAge when this bridge
         is acting as the root."
    ::= { cistGeneralInfo 5 } 

cistRootForwardDelay OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for ForwardDelay when this 
         bridge is acting as the root."
    ::= { cistGeneralInfo 6 } 

cistRegionalRoot OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The bridge identifier of the Root of the Multiple
         spanning tree region as determined by the Spanning Tree
         Protocol as executed by this node.  This value is used as
         the CIST Regional Root Identifier parameter in all Configuration
         Bridge PDUs originated by this node."
   ::= { cistGeneralInfo 7 } 

cistRegionalPathCost OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Cost of the path to the CIST Regional Root as seen from this 
         bridge."
   ::= { cistGeneralInfo 8 } 

cistBridgePriority OBJECT-TYPE
    SYNTAX  INTEGER  (0..65535)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value of the writable portion of the Brigde Identifier comprising
         of the first two octets."
    ::= { cistGeneralInfo 9 }

cistBridgeMaxAge OBJECT-TYPE
    SYNTAX  INTEGER  (6..40)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for MaxAge when this bridge
         is acting as the root."
    ::= { cistGeneralInfo 10 }

cistBridgeForwardDelay OBJECT-TYPE
    SYNTAX  INTEGER  (4..30)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for ForwardDelay when this 
         bridge is acting as the root."
    ::= { cistGeneralInfo 11 }

cistMaxHopCount OBJECT-TYPE
    SYNTAX  INTEGER  (4..60)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Indicates the maximum hop count value."
    ::= { cistGeneralInfo 12 }

mstpDigest OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..63))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The digest of the mstp."
    ::= { cistGeneralInfo 13 }

-- CIST Port Information Table
cistInfoPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF CistInfoPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of CIST Port information."
    ::= { cistInfo 2 }

cistInfoPortTableEntry OBJECT-TYPE
    SYNTAX CistInfoPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a particular CIST Port."
    INDEX { cistInfoPortIndex }
    ::= { cistInfoPortTable 1 }

CistInfoPortTableEntry ::= SEQUENCE {
    cistInfoPortIndex            Integer32,
    cistInfoPortPriority         Integer32,
    cistInfoPortPathCost         Integer32,
    cistInfoPortState            INTEGER,
    cistInfoPortRole             INTEGER,
    cistInfoPortDesignatedBridge BridgeId,
    cistInfoPortDesignatedPort   OCTET STRING,
    cistInfoPortLinkType         INTEGER,
    cistInfoPortHelloTime        INTEGER
    }

cistInfoPortIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The port number of the port for which this entry contains spanning
         tree configuration."
    ::= { cistInfoPortTableEntry 1 }

cistInfoPortPriority OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The four most significant bits of the Port Identifier of the 
         Spanning Tree instance can be modified by setting this value."
    ::= { cistInfoPortTableEntry 2 }

cistInfoPortPathCost OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The contribution of this port to the path cost of paths towards 
         the CIST Root which include this port."
    ::= { cistInfoPortTableEntry 3 }

cistInfoPortState OBJECT-TYPE
    SYNTAX INTEGER {
        disabled (1),
        discarding (2),
        learning (4),
        forwarding (5)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Current state of the Port as defined by the Common    
         spanning tree protocol." 
    ::= { cistInfoPortTableEntry 4 }

cistInfoPortRole OBJECT-TYPE
    SYNTAX INTEGER {
        disabled(1),
        alternate(2),
        backup(3),
        root(4),
        designated(5),
        master(6),
        unknown(7)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
          "Selected Port Role of the port for this spanning tree instance."
    ::= { cistInfoPortTableEntry 5 }

cistInfoPortDesignatedBridge OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The unique Bridge Identifier of the bridge which this port  
         considers to be the Designated Bridge for the port's segment."   
    ::= { cistInfoPortTableEntry 6 }

cistInfoPortDesignatedPort OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE (2))
    MAX-ACCESS  read-only
    STATUS  current
      DESCRIPTION
          "The Port identifier of the port on the Designated Bridge    
           for this port's segment."                                           
    ::= { cistInfoPortTableEntry 7 }

cistInfoPortLinkType OBJECT-TYPE
    SYNTAX INTEGER {
        p2p(1),
        shared(2),
        unknown(3)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The point-to-point status of the LAN segment attached 
         to this port.  A value of p2p (2) indicates that this port is being
         treated as if it is connected to a point-to-point link. 
         A value of shared(3) indicates that this port is being treated as 
         having a shared media connection."
    ::= { cistInfoPortTableEntry 8 }

cistInfoPortHelloTime OBJECT-TYPE
    SYNTAX  INTEGER (1..10)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The amount of time between the transmission of Configuration Port 
         PDUs in seconds."
    ::= { cistInfoPortTableEntry 9 }


-- LACP information

lacpInfoAggrTable OBJECT-TYPE
    SYNTAX SEQUENCE OF LacpInfoAggrTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of LACP aggregator information."
    ::= { lacpInfo 1 }

lacpInfoAggrTableEntry OBJECT-TYPE
    SYNTAX LacpInfoAggrTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a LACP aggregator."
    INDEX { lacpInfoAggrIndex }
    ::= { lacpInfoAggrTable 1 }

LacpInfoAggrTableEntry ::= SEQUENCE {
    lacpInfoAggrIndex           Integer32,
    lacpInfoAggrId		Integer32,
    lacpInfoAggrMac		DisplayString,
    lacpInfoAggrActSysPrio	Integer32,
    lacpInfoAggrActSysId	DisplayString,
    lacpInfoAggrIndivState	INTEGER,
    lacpInfoAggrActAdminKey	Integer32,
    lacpInfoAggrActOperKey	Integer32,
    lacpInfoAggrPartSysPrio	Integer32,
    lacpInfoAggrPartSysId	DisplayString,
    lacpInfoAggrPartOperKey	Integer32,
    lacpInfoAggrReadyState	INTEGER,
    lacpInfoAggrNumPorts	Integer32,
    lacpInfoAggrPorts		DisplayString
    }

lacpInfoAggrIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The aggregator identifier."
    ::= { lacpInfoAggrTableEntry 1 }

lacpInfoAggrId OBJECT-TYPE 
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoAggrTableEntry 2 }

lacpInfoAggrMac OBJECT-TYPE 
    SYNTAX  DisplayString
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoAggrTableEntry 3 }

lacpInfoAggrActSysPrio OBJECT-TYPE 
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoAggrTableEntry 4 }

lacpInfoAggrActSysId OBJECT-TYPE 
    SYNTAX  DisplayString
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoAggrTableEntry 5 }

lacpInfoAggrIndivState OBJECT-TYPE 
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoAggrTableEntry 6 }

lacpInfoAggrActAdminKey OBJECT-TYPE 
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoAggrTableEntry 7 }

lacpInfoAggrActOperKey OBJECT-TYPE 
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoAggrTableEntry 8 }

lacpInfoAggrPartSysPrio OBJECT-TYPE 
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoAggrTableEntry 9 }

lacpInfoAggrPartSysId OBJECT-TYPE 
    SYNTAX  DisplayString
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoAggrTableEntry 10 }

lacpInfoAggrPartOperKey OBJECT-TYPE 
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoAggrTableEntry 11 }

lacpInfoAggrReadyState OBJECT-TYPE 
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoAggrTableEntry 12 }

lacpInfoAggrNumPorts OBJECT-TYPE 
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoAggrTableEntry 13 }

lacpInfoAggrPorts OBJECT-TYPE
    SYNTAX  DisplayString
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoAggrTableEntry 14 }


lacpInfoPort OBJECT IDENTIFIER ::= { lacpInfo 2 }

lacpInfoPortGeneralTable OBJECT-TYPE
    SYNTAX SEQUENCE OF LacpInfoPortGeneralTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of LACP port general information."
    ::= { lacpInfoPort 1 }

lacpInfoPortGeneralTableEntry OBJECT-TYPE
    SYNTAX LacpInfoPortGeneralTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "General information about a LACP port."
    INDEX { lacpInfoPortGeneralIndex }
    ::= { lacpInfoPortGeneralTable 1 }

LacpInfoPortGeneralTableEntry ::= SEQUENCE {
    lacpInfoPortGeneralIndex		Integer32,
    lacpInfoPortLacpEna 		INTEGER,
    lacpInfoPortAdminEna	 	INTEGER,
    lacpInfoPortActSysId		DisplayString,
    lacpInfoPortActSysPrio		Integer32,
    lacpInfoPortActAdminKey 		Integer32,
    lacpInfoPortActOperKey 		Integer32,
    lacpInfoPortActPortNum 		Integer32,
    lacpInfoPortActPortPrio 		Integer32,
    lacpInfoPortIndivState 		INTEGER,
    lacpInfoSelAggrId 			Integer32,
    lacpInfoAttAggrId 			Integer32,
    lacpInfoPortReadyN 			INTEGER,
    lacpInfoPortNtt 			INTEGER,
    lacpInfoPortSelected 		INTEGER,
    lacpInfoPortMoved 			INTEGER,
    lacpInfoCollDetState 		INTEGER,
    lacpInfoPortRxState 		DisplayString, 
    lacpInfoPortMuxState 		DisplayString,
    lacpInfoPortPerState 		DisplayString
    }

lacpInfoPortGeneralIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The port identifier."
    ::= { lacpInfoPortGeneralTableEntry 1 }

lacpInfoPortLacpEna OBJECT-TYPE 
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortGeneralTableEntry 2 }

lacpInfoPortAdminEna OBJECT-TYPE 
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortGeneralTableEntry 3 }

lacpInfoPortActSysId OBJECT-TYPE
    SYNTAX  DisplayString
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortGeneralTableEntry 4 }

lacpInfoPortActSysPrio OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortGeneralTableEntry 5 }

lacpInfoPortActAdminKey OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortGeneralTableEntry 6 }

lacpInfoPortActOperKey OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortGeneralTableEntry 7 }

lacpInfoPortActPortNum OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortGeneralTableEntry 8 }

lacpInfoPortActPortPrio OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortGeneralTableEntry 9 }

lacpInfoPortIndivState OBJECT-TYPE 
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortGeneralTableEntry 10 }

lacpInfoSelAggrId OBJECT-TYPE 
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortGeneralTableEntry 11 }

lacpInfoAttAggrId OBJECT-TYPE 
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortGeneralTableEntry 12 }

lacpInfoPortReadyN OBJECT-TYPE
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS read-only
    STATUS  current
    DESCRIPTION
        "True value for Ready_N flag indicates that the wait while timer 
         has expired and it is waiting to attach to an aggregator. 
         There is one Ready_N value for each port."
    ::= { lacpInfoPortGeneralTableEntry 13 }

lacpInfoPortNtt OBJECT-TYPE
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS read-only
    STATUS  current
    DESCRIPTION
        "Need to transmit flag. True indicates that there is new protocol 
         information that should be transmitted on the link."
    ::= { lacpInfoPortGeneralTableEntry 14 }

lacpInfoPortSelected OBJECT-TYPE
    SYNTAX  INTEGER {
        selected(1),
        unselected(2),
        standby(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Selected flag value indicates that the selection logic has selected
         an appropriate Aggregator. A value of unselected indicates that no 
         aggregator is currently selected. A value of standby indicates that
         although the selection logic has selected an appropriate Aggregator,
         aggregation restrictions currently precent the port from being 
         enabled as part of the aggregation, and so the port is being held
         in standby condition." 
    ::= { lacpInfoPortGeneralTableEntry 15 }

lacpInfoPortMoved OBJECT-TYPE
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS read-only
    STATUS  current
    DESCRIPTION
        "Port Moved flag is set to true if the receive machine for a port 
         is in the port_disabled state, and the combination of partner oper
         system and partner oper port number in use by the port has been 
         used by received in an incoming LACPDU on a different port."
    ::= { lacpInfoPortGeneralTableEntry 16 }

lacpInfoCollDetState OBJECT-TYPE 
    SYNTAX  INTEGER {
        on(1),
        off(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortGeneralTableEntry 17 }

lacpInfoPortRxState OBJECT-TYPE 
    SYNTAX  DisplayString 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortGeneralTableEntry 18 }

lacpInfoPortMuxState OBJECT-TYPE 
    SYNTAX  DisplayString
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortGeneralTableEntry 19 }

lacpInfoPortPerState OBJECT-TYPE 
    SYNTAX  DisplayString
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortGeneralTableEntry 20 }


lacpInfoPortAdminTable OBJECT-TYPE
    SYNTAX SEQUENCE OF LacpInfoPortAdminTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of LACP port admin information."
    ::= { lacpInfoPort 2 }

lacpInfoPortAdminTableEntry OBJECT-TYPE
    SYNTAX LacpInfoPortAdminTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Admin information about a LACP port."
    INDEX { lacpInfoPortAdminIndex }
    ::= { lacpInfoPortAdminTable 1 }

LacpInfoPortAdminTableEntry ::= SEQUENCE {
    lacpInfoPortAdminIndex		Integer32,
    lacpInfoPortActAdPortState 		DisplayString,
    lacpInfoPortActAdActiv 		INTEGER,
    lacpInfoPortActAdSync 		INTEGER,
    lacpInfoPortActAdDef 		INTEGER,
    lacpInfoPortActAdTimeout 		INTEGER,
    lacpInfoPortActAdColl 		INTEGER,
    lacpInfoPortActAdExp 		INTEGER,
    lacpInfoPortActAdAggr 		INTEGER,
    lacpInfoPortActAdDist 		INTEGER
    }

lacpInfoPortAdminIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The port identifier."
    ::= { lacpInfoPortAdminTableEntry 1 }


lacpInfoPortActAdPortState OBJECT-TYPE
    SYNTAX  DisplayString
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The state of Actor Administrator Port. This is a octet mask
         with the following bits: Activity, Synchronization, Defaulted, 
         Timeout, Collecting, Expired, Aggregation and Distributing.
         If all of them are 0 then the state is showed as 0x0, else it is
         displayed a blank state which mean is not a NULL state"
    ::= { lacpInfoPortAdminTableEntry 7 }

lacpInfoPortActAdActiv OBJECT-TYPE
    SYNTAX  INTEGER {
        active(1),
        passive(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortAdminTableEntry 8 }

lacpInfoPortActAdSync OBJECT-TYPE
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortAdminTableEntry 9 }

lacpInfoPortActAdDef OBJECT-TYPE
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortAdminTableEntry 10 }

lacpInfoPortActAdTimeout OBJECT-TYPE 
    SYNTAX  INTEGER {
        short(1),
        long(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortAdminTableEntry 11 }

lacpInfoPortActAdColl OBJECT-TYPE 
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortAdminTableEntry 12 }

lacpInfoPortActAdExp OBJECT-TYPE 
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortAdminTableEntry 13 }

lacpInfoPortActAdAggr OBJECT-TYPE 
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortAdminTableEntry 14 }

lacpInfoPortActAdDist OBJECT-TYPE 
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortAdminTableEntry 15 }



lacpInfoPortOperTable OBJECT-TYPE
    SYNTAX SEQUENCE OF LacpInfoPortOperTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of LACP port oper information."
    ::= { lacpInfoPort 3 }

lacpInfoPortOperTableEntry OBJECT-TYPE
    SYNTAX LacpInfoPortOperTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Oper information about a LACP port."
    INDEX { lacpInfoPortOperIndex }
    ::= { lacpInfoPortOperTable 1 }

LacpInfoPortOperTableEntry ::= SEQUENCE {
    lacpInfoPortOperIndex		Integer32,
    lacpInfoPortPartOpSysPrio 		Integer32,
    lacpInfoPortPartOpSysId 		DisplayString,
    lacpInfoPortPartOpKey 		Integer32,
    lacpInfoPortPartOpPortNum 		Integer32,
    lacpInfoPortPartOpPortPrio 		Integer32,
    lacpInfoPortActOpPortState 		DisplayString,
    lacpInfoPortActOpActiv 		INTEGER,
    lacpInfoPortActOpSync 		INTEGER,
    lacpInfoPortActOpDef 		INTEGER,
    lacpInfoPortActOpTimeout 		INTEGER,
    lacpInfoPortActOpColl 		INTEGER,
    lacpInfoPortActOpExp 		INTEGER,
    lacpInfoPortActOpAggr 		INTEGER,
    lacpInfoPortActOpDist 		INTEGER,
    lacpInfoPortPartOpPortState 	DisplayString,
    lacpInfoPortPartOpActiv 		INTEGER,
    lacpInfoPortPartOpSync 		INTEGER,
    lacpInfoPortPartOpDef 		INTEGER,
    lacpInfoPortPartOpTimeout 		INTEGER,
    lacpInfoPortPartOpColl 		INTEGER,
    lacpInfoPortPartOpExp 		INTEGER,
    lacpInfoPortPartOpAggr 		INTEGER,
    lacpInfoPortPartOpDist 		INTEGER 
    }

lacpInfoPortOperIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The port identifier."
    ::= { lacpInfoPortOperTableEntry 1 }

lacpInfoPortPartOpSysPrio OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortOperTableEntry 2 }

lacpInfoPortPartOpSysId OBJECT-TYPE
    SYNTAX  DisplayString
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortOperTableEntry 3 }

lacpInfoPortPartOpKey OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortOperTableEntry 4 }

lacpInfoPortPartOpPortNum OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortOperTableEntry 5 }

lacpInfoPortPartOpPortPrio OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortOperTableEntry 6 }

lacpInfoPortActOpPortState OBJECT-TYPE
    SYNTAX  DisplayString
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The state of Actor Operator Port. This is a octet mask
         with the following bits: Activity, Synchronization, Defaulted, 
         Timeout, Collecting, Expired, Aggregation and Distributing.
         If all of them are 0 then the state is showed as 0x0, else it is
         displayed a blank state which mean is not a NULL state"
    ::= { lacpInfoPortOperTableEntry 7 }

lacpInfoPortActOpActiv OBJECT-TYPE
    SYNTAX  INTEGER {
        active(1),
        passive(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortOperTableEntry 8 }

lacpInfoPortActOpSync OBJECT-TYPE
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortOperTableEntry 9 }

lacpInfoPortActOpDef OBJECT-TYPE
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortOperTableEntry 10 }

lacpInfoPortActOpTimeout OBJECT-TYPE 
    SYNTAX  INTEGER {
        short(1),
        long(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortOperTableEntry 11 }

lacpInfoPortActOpColl OBJECT-TYPE 
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortOperTableEntry 12 }

lacpInfoPortActOpExp OBJECT-TYPE 
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortOperTableEntry 13 }

lacpInfoPortActOpAggr OBJECT-TYPE 
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortOperTableEntry 14 }

lacpInfoPortActOpDist OBJECT-TYPE 
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortOperTableEntry 15 }

lacpInfoPortPartOpPortState OBJECT-TYPE
    SYNTAX  DisplayString
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The state of Partner Operator Port. This is a octet mask
         with the following bits: Activity, Synchronization, Defaulted, 
         Timeout, Collecting, Expired, Aggregation and Distributing.
         If all of them are 0 then the state is showed as 0x0, else it is
         displayed a blank state which mean is not a NULL state"
    ::= { lacpInfoPortOperTableEntry 16 }

lacpInfoPortPartOpActiv OBJECT-TYPE
    SYNTAX  INTEGER {
        active(1),
        passive(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortOperTableEntry 17 }

lacpInfoPortPartOpSync OBJECT-TYPE
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortOperTableEntry 18 }

lacpInfoPortPartOpDef OBJECT-TYPE
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortOperTableEntry 19 }

lacpInfoPortPartOpTimeout OBJECT-TYPE 
    SYNTAX  INTEGER {
        short(1),
        long(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortOperTableEntry 20 }

lacpInfoPortPartOpColl OBJECT-TYPE 
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortOperTableEntry 21 }

lacpInfoPortPartOpExp OBJECT-TYPE 
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortOperTableEntry 22 }

lacpInfoPortPartOpAggr OBJECT-TYPE 
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortOperTableEntry 23 }

lacpInfoPortPartOpDist OBJECT-TYPE 
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        ""
    ::= { lacpInfoPortOperTableEntry 24 }




-- UFD Configuration


ufdCurCfgState        OBJECT-TYPE
    SYNTAX  INTEGER  {
    enabled(1),
    disabled(2)
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable UFD state"
    ::= { ufdGeneralCfg 1 }

ufdNewCfgState OBJECT-TYPE
    SYNTAX  INTEGER  {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable UFD state"
    ::= { ufdGeneralCfg 2 }

ufdCurCfgLtMPorts      OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The LtM port list. The ports are presented in bitmap format.
         in receiving order:

              OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             ||    || |_ port 8
             ||    ||
             ||    ||___ port 7
             ||    |____ port 6
             ||      .    .   .
             ||_________ port 1
             |__________ reserved

         where x : 1 - The represented port belongs to LtM
            0 - The represented port does not belong to LtM"
    ::= { ufdGeneralCfg 3 }

ufdNewCfgLtMPorts      OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The LtM port list. The ports are presented in bitmap format.
         in receiving order:

              OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             ||    || |_ port 8
             ||    ||
             ||    ||___ port 7
             ||    |____ port 6
             ||      .    .   .
             ||_________ port 1
             |__________ reserved

         where x : 1 - The represented port belongs to LtM
            0 - The represented port does not belong to LtM"
    ::= { ufdGeneralCfg 4 }

ufdCurCfgLtMTrunks      OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The LtM trunk list. The trunks are presented in bitmap format.
         in receiving order:

              OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             ||    || |_ trunk 8
             ||    ||
             ||    ||___ trunk 7
             ||    |____ trunk 6
             ||      .    .   .
             ||_________ trunk 1
             |__________ reserved

         where x : 1 - The represented trunk belongs to LtM
            0 - The represented trunk does not belong to LtM"
    ::= { ufdGeneralCfg 5 }

ufdNewCfgLtMTrunks      OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The LtM trunk list. The trunks are presented in bitmap format.
         in receiving order:

              OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             ||    || |_ trunk 8
             ||    ||
             ||    ||___ trunk 7
             ||    |____ trunk 6
             ||      .    .   .
             ||_________ trunk 1
             |__________ reserved

         where x : 1 - The represented trunk belongs to LtM
            0 - The represented trunk does not belong to LtM"
    ::= { ufdGeneralCfg 6 }

ufdCurCfgLtMAdminkey      OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The LtM admin key."
    ::= { ufdGeneralCfg 7 }

ufdNewCfgLtMAdminkey      OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The LtM admin key."
    ::= { ufdGeneralCfg 8 }

ufdCurCfgLtDPorts      OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The LtD port list. The ports are presented in bitmap format.
         in receiving order:

              OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             ||    || |_ port 8
             ||    ||
             ||    ||___ port 7
             ||    |____ port 6
             ||      .    .   .
             ||_________ port 1
             |__________ reserved

         where x : 1 - The represented port belongs to LtD
            0 - The represented port does not belong to LtD"
    ::= { ufdGeneralCfg 9 }

ufdNewCfgLtDPorts      OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The LtD port list. The ports are presented in bitmap format.
         in receiving order:

              OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             ||    || |_ port 8
             ||    ||
             ||    ||___ port 7
             ||    |____ port 6
             ||      .    .   .
             ||_________ port 1
             |__________ reserved

         where x : 1 - The represented port belongs to LtD
            0 - The represented port does not belong to LtD"
    ::= { ufdGeneralCfg 10 }

ufdCurCfgLtDTrunks      OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The LtD trunk list. The trunks are presented in bitmap format.
         in receiving order:

              OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             ||    || |_ trunk 8
             ||    ||
             ||    ||___ trunk 7
             ||    |____ trunk 6
             ||      .    .   .
             ||_________ trunk 1
             |__________ reserved

         where x : 1 - The represented trunk belongs to LtD
            0 - The represented trunk does not belong to LtD"
    ::= { ufdGeneralCfg 11 }

ufdNewCfgLtDTrunks      OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The LtD trunk list. The trunks are presented in bitmap format.
         in receiving order:

              OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             ||    || |_ trunk 8
             ||    ||
             ||    ||___ trunk 7
             ||    |____ trunk 6
             ||      .    .   .
             ||_________ trunk 1
             |__________ reserved

         where x : 1 - The represented trunk belongs to LtD
            0 - The represented trunk does not belong to LtD"
    ::= { ufdGeneralCfg 12 }

ufdLtDAdminkeyMaxEnt OBJECT-TYPE
    SYNTAX  Integer32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum number of rows in the LtD admin key configuration table."
    ::= { ufdGeneralCfg 13 }

ufdLtDAdminkeyCurCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF UfdLtDAdminkeyCurCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of LtD admin key configuration."
    ::= { ufdGeneralCfg 14 }

ufdLtDAdminkeyCurCfgTableEntry OBJECT-TYPE
    SYNTAX  UfdLtDAdminkeyCurCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the LtD admin key table."
    INDEX  { ufdLtDAdminkeyCurCfg }
    ::= { ufdLtDAdminkeyCurCfgTable 1 }

UfdLtDAdminkeyCurCfgTableEntry ::= SEQUENCE {
    ufdLtDAdminkeyCurCfg	INTEGER	    
    }

ufdLtDAdminkeyCurCfg OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The LtD admin key."
    ::= { ufdLtDAdminkeyCurCfgTableEntry 1 }

ufdLtDAdminkeyNewCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF UfdLtDAdminkeyNewCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of LtD admin key configuration."
    ::= { ufdGeneralCfg 15 }

ufdLtDAdminkeyNewCfgTableEntry OBJECT-TYPE
    SYNTAX  UfdLtDAdminkeyNewCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the LtD admin key table."
    INDEX  { ufdLtDAdminkeyNewCfg }
    ::= { ufdLtDAdminkeyNewCfgTable 1 }

UfdLtDAdminkeyNewCfgTableEntry ::= SEQUENCE {
    ufdLtDAdminkeyNewCfg	INTEGER	    
    }

ufdLtDAdminkeyNewCfg OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The LtD admin key."
    ::= { ufdLtDAdminkeyNewCfgTableEntry 1 }

ufdNewCfgAddLtMPort OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The port to be added to LtM.  A '0' value is
         returned when read."
    ::= { ufdGeneralCfg 16 }

ufdNewCfgRemoveLtMPort OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The port to be removed from LtM.  A '0'
         value is returned when read."
    ::= { ufdGeneralCfg 17 }

ufdNewCfgAddLtMTrunk OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The trunk to be added to LtM.  A '0' value is
         returned when read."
    ::= { ufdGeneralCfg 18 }

ufdNewCfgRemoveLtMTrunk OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The trunk to be removed from LtM.  A '0'
         value is returned when read."
    ::= { ufdGeneralCfg 19 }

ufdNewCfgAddLtMAdminkey OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The admin key to be added to LtM.  A '0' value is
         returned when read."
    ::= { ufdGeneralCfg 20 }

ufdNewCfgRemoveLtMAdminkey OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The admin key to be removed from LtM.  A '0'
         value is returned when read."
    ::= { ufdGeneralCfg 21 }

ufdNewCfgAddLtDPort OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The port to be added to LtD.  A '0' value is
         returned when read."
    ::= { ufdGeneralCfg 22 }

ufdNewCfgRemoveLtDPort OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The port to be removed from LtM.  A '0'
         value is returned when read."
    ::= { ufdGeneralCfg 23 }

ufdNewCfgAddLtDTrunk OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The trunk to be added to LtM.  A '0' value is
         returned when read."
    ::= { ufdGeneralCfg 24 }

ufdNewCfgRemoveLtDTrunk OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The trunk to be removed from LtD.  A '0'
         value is returned when read."
    ::= { ufdGeneralCfg 25 }

ufdNewCfgAddLtDAdminkey OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The admin key to be added to LtD.  A '0' value is
         returned when read."
    ::= { ufdGeneralCfg 26 }

ufdNewCfgRemoveLtDAdminkey OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The admin key to be removed from LtD.  A '0'
         value is returned when read."
    ::= { ufdGeneralCfg 27 }

ufdCurCfgGlobalState        OBJECT-TYPE
    SYNTAX  INTEGER  {
    enabled(1),
    disabled(2)
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Current global Failover settings."
    ::= { ufdGeneralCfg 28 }

ufdNewCfgGlobalState OBJECT-TYPE
    SYNTAX  INTEGER  {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "New global Failover settings."
    ::= { ufdGeneralCfg 29 }





--dot1x


dot1xCurStatus OBJECT-TYPE
    SYNTAX INTEGER {
	enable(0),
        disable(1)
	}
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"  Dot1x  status    " 
    ::= { dot1x 1 }

dot1xNewStatus OBJECT-TYPE
    SYNTAX INTEGER {
	enable(0),
        disable(1)
	}
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"  Dot1x  status    " 
    ::= { dot1x 2 }



dot1xCurCfgPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF Dot1xCurCfgPortEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of 8021x configuration in the Current_config."
    ::= { dot1x 3 }

dot1xCurCfgPortEntry OBJECT-TYPE
    SYNTAX Dot1xCurCfgPortEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about 8021x Port Config"
    INDEX { dot1xCurCfgPortIndex }
    ::= { dot1xCurCfgPortTable 1 }
 
Dot1xCurCfgPortEntry ::= SEQUENCE {
    dot1xCurCfgPortIndex                Integer32,	
    dot1xCurCfgPortMode                 INTEGER,
    dot1xCurCfgPortQtPeriod             INTEGER,
    dot1xCurCfgPortTxPeriod             INTEGER,
    dot1xCurCfgPortSupTmout		INTEGER,
    dot1xCurCfgPortSrvTmout             INTEGER,
    dot1xCurCfgPortMaxRq 		INTEGER,
    dot1xCurCfgPortRaPeriod		INTEGER,
    dot1xCurCfgPortReAuth		INTEGER 
    }
 
dot1xCurCfgPortIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The 8021x Port number for which the table is related."
    ::= { dot1xCurCfgPortEntry 1}

dot1xCurCfgPortMode OBJECT-TYPE
    SYNTAX INTEGER {
      forceUnauth(0),
      auto(1),
      forceAuth(2)	
	}
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	" Port authenticaton mode
	  forceUnauth(0),
          auto(1),
          forceAuth(2)
	    " 
    ::= { dot1xCurCfgPortEntry 2 }

dot1xCurCfgPortQtPeriod OBJECT-TYPE
    SYNTAX INTEGER (0..65535)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Quiet period (0-65535) " 
    ::= { dot1xCurCfgPortEntry 3 }

dot1xCurCfgPortTxPeriod OBJECT-TYPE
    SYNTAX INTEGER (1..65535)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	" Tx Period     " 
    ::= { dot1xCurCfgPortEntry 4 }

dot1xCurCfgPortSupTmout OBJECT-TYPE
    SYNTAX INTEGER (1..65535)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"   Supplicant timeout (1..65535)  " 
    ::= { dot1xCurCfgPortEntry 5 }

dot1xCurCfgPortSrvTmout OBJECT-TYPE
    SYNTAX INTEGER (1..65535)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"  Server timeout (1..65535)   " 
    ::= { dot1xCurCfgPortEntry 6 }

dot1xCurCfgPortMaxRq OBJECT-TYPE
    SYNTAX INTEGER (1..10)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	" Maximum numer of requests   (1..10)   " 
    ::= { dot1xCurCfgPortEntry 7 }

dot1xCurCfgPortRaPeriod OBJECT-TYPE
    SYNTAX INTEGER (0..604800)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"  Reautentication period (0..604800)    " 
    ::= { dot1xCurCfgPortEntry 8 }


dot1xCurCfgPortReAuth OBJECT-TYPE
    SYNTAX INTEGER {
	off(0),
        on(1)
	}
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"  ReAuthentication state
	off(0),
        on(1)	
	    " 
    ::= { dot1xCurCfgPortEntry 9 }





dot1xNewCfgPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF Dot1xNewCfgPortEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of 8021x configuration in the new_config."
    ::= { dot1x 4 }

dot1xNewCfgPortEntry OBJECT-TYPE
    SYNTAX Dot1xNewCfgPortEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about 8021x Port Config"
    INDEX { dot1xNewCfgPortIndex }
    ::= { dot1xNewCfgPortTable 1 }
 
Dot1xNewCfgPortEntry ::= SEQUENCE {
    dot1xNewCfgPortIndex                Integer32,	
    dot1xNewCfgPortMode                 INTEGER,
    dot1xNewCfgPortQtPeriod             INTEGER,
    dot1xNewCfgPortTxPeriod             INTEGER,
    dot1xNewCfgPortSupTmout		INTEGER,
    dot1xNewCfgPortSrvTmout             INTEGER,
    dot1xNewCfgPortMaxRq 		INTEGER,
    dot1xNewCfgPortRaPeriod		INTEGER,
    dot1xNewCfgPortReAuth		INTEGER ,
    dot1xNewCfgPortDefault		INTEGER ,
    dot1xNewCfgPortApplyGlobal   	INTEGER 
    }
 
dot1xNewCfgPortIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The 8021x Port number for which the table is related."
    ::= { dot1xNewCfgPortEntry 1}

dot1xNewCfgPortMode OBJECT-TYPE
    SYNTAX INTEGER {
	forceUnauth(0),
	auto(1),
        forceAuth(2)
	}
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	" Port authentication mode 
	  forceUnauth(0),
	  auto(1),
          forceAuth(2)	     " 
    ::= { dot1xNewCfgPortEntry 2 }

dot1xNewCfgPortQtPeriod OBJECT-TYPE
    SYNTAX INTEGER (0..65535)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	" Quiet period (0..65535)     " 
    ::= { dot1xNewCfgPortEntry 3 }

dot1xNewCfgPortTxPeriod OBJECT-TYPE
    SYNTAX INTEGER (1..65535)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	" Tx Period  (1..65535)   " 
    ::= { dot1xNewCfgPortEntry 4 }

dot1xNewCfgPortSupTmout OBJECT-TYPE
    SYNTAX INTEGER (1..65535)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	" Supplicant Timeout (1..65535)    " 
    ::= { dot1xNewCfgPortEntry 5 }

dot1xNewCfgPortSrvTmout OBJECT-TYPE
    SYNTAX INTEGER (1..65535)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"  Server Timeout  (1..65535)   " 
    ::= { dot1xNewCfgPortEntry 6 }

dot1xNewCfgPortMaxRq OBJECT-TYPE
    SYNTAX INTEGER (1..10)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	" Maximum number of requests  (1..10)    " 
    ::= { dot1xNewCfgPortEntry 7 }

dot1xNewCfgPortRaPeriod OBJECT-TYPE
    SYNTAX INTEGER (1..604800)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	" Reauthentication period (1..604800)    " 
    ::= { dot1xNewCfgPortEntry 8 }


dot1xNewCfgPortReAuth OBJECT-TYPE
    SYNTAX INTEGER {
	off(0),
        on(1)
	}
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"  Reauthentication state
	   off(0),
           on(1)	    " 
    ::= { dot1xNewCfgPortEntry 9 }



dot1xNewCfgPortDefault OBJECT-TYPE
    SYNTAX INTEGER {
	other(0),
        apply(1)
	}
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"  Port default settings    " 
    ::= { dot1xNewCfgPortEntry 10 }


dot1xNewCfgPortApplyGlobal OBJECT-TYPE
    SYNTAX INTEGER {
	other(0),
        apply(1)
	}
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	" Apply Global config     " 
    ::= { dot1xNewCfgPortEntry 11 }




 


dot1xCurCfgGlobalMode OBJECT-TYPE
    SYNTAX INTEGER {
      forceUnauth(0),
      auto(1),
      forceAuth(2)	
	}
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"  Autehtication Mode
	   forceUnauth(0),
           auto(1),
           forceAuth(2)	    " 
    ::= { dot1xCurCfgGlobalTable 1 }

dot1xCurCfgGlobalQtPeriod OBJECT-TYPE
    SYNTAX INTEGER (0..65535)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	" Quiet period  (0..65535)    " 
    ::= { dot1xCurCfgGlobalTable 2 }

dot1xCurCfgGlobalTxPeriod OBJECT-TYPE
    SYNTAX INTEGER (1..65535)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	" Tx period  (1..65535)    " 
    ::= { dot1xCurCfgGlobalTable 3 }

dot1xCurCfgGlobalSupTmout OBJECT-TYPE
    SYNTAX INTEGER (1..65535)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"  Supplicant timeout (1..65535)    " 
    ::= { dot1xCurCfgGlobalTable 4 }

dot1xCurCfgGlobalSrvTmout OBJECT-TYPE
    SYNTAX INTEGER (1..65535)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"  Server timeout (1..65535)    " 
    ::= { dot1xCurCfgGlobalTable 5 }

dot1xCurCfgGlobalMaxRq OBJECT-TYPE
    SYNTAX INTEGER (1..10)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	" Maximum number of requests  (1..10)    " 
    ::= { dot1xCurCfgGlobalTable 6 }

dot1xCurCfgGlobalRaPeriod OBJECT-TYPE
    SYNTAX INTEGER (0..604800)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	" Reauthentication period  (0..604800)    " 
    ::= { dot1xCurCfgGlobalTable 7 }


dot1xCurCfgGlobalReAuth OBJECT-TYPE
    SYNTAX INTEGER {
	off(0),
        on(1)
	}
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"      " 
    ::= { dot1xCurCfgGlobalTable 8 }




 

dot1xNewCfgGlobalMode OBJECT-TYPE
    SYNTAX INTEGER {
	forceUnauth(0),
	auto(1),
        forceAuth(2)
	}
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"  Authentication Mode     " 
    ::= { dot1xNewCfgGlobalTable 1 }

dot1xNewCfgGlobalQtPeriod OBJECT-TYPE
    SYNTAX INTEGER (0..65535)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	" Quiet Period (0..65535)     " 
    ::= { dot1xNewCfgGlobalTable 2 }

dot1xNewCfgGlobalTxPeriod OBJECT-TYPE
    SYNTAX INTEGER (1..65535)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	" Tx Period (1..65535)    " 
    ::= { dot1xNewCfgGlobalTable 3 }

dot1xNewCfgGlobalSupTmout OBJECT-TYPE
    SYNTAX INTEGER (1..65535)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	" Supplicand timeout (1..65535)    " 
    ::= { dot1xNewCfgGlobalTable 4 }

dot1xNewCfgGlobalSrvTmout OBJECT-TYPE
    SYNTAX INTEGER (1..65535)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	" Server timeout (1..65535)     " 
    ::= { dot1xNewCfgGlobalTable 5 }

dot1xNewCfgGlobalMaxRq OBJECT-TYPE
    SYNTAX INTEGER (1..10)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	" Maximum number of requests (1..10)     " 
    ::= { dot1xNewCfgGlobalTable 6 }

dot1xNewCfgGlobalRaPeriod OBJECT-TYPE
    SYNTAX INTEGER (1..604800)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"  Reauthentication period (1..604800)   " 
    ::= { dot1xNewCfgGlobalTable 7 }


dot1xNewCfgGlobalReAuth OBJECT-TYPE
    SYNTAX INTEGER {
	off(0),
        on(1)
	}
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"  Reauthentication status    " 
    ::= { dot1xNewCfgGlobalTable 8 }










dot1xInfoPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF Dot1xInfoPortEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of 8021x configuration in the Current_config."
    ::= { dot1xInfo 1 }

dot1xInfoPortEntry OBJECT-TYPE
    SYNTAX Dot1xInfoPortEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about 8021x Port Config"
    INDEX { dot1xInfoPortIndex }
    ::= { dot1xInfoPortTable 1 }
 
Dot1xInfoPortEntry ::= SEQUENCE {
    dot1xInfoPortIndex                Integer32,	
    dot1xInfoPortAuthMode                 INTEGER,
    dot1xInfoPortAuthStatus             INTEGER,
    dot1xInfoPortCtrlDir             INTEGER,
    dot1xInfoPortAuthPAEState		INTEGER,
    dot1xInfoPortBackAuthState             INTEGER   
    }
 
dot1xInfoPortIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The 8021x Port number for which the table is related."
    ::= { dot1xInfoPortEntry 1}

dot1xInfoPortAuthMode OBJECT-TYPE
    SYNTAX INTEGER {
      forceUnauth(0),
      auto(1),
      forceAuth(2)	
	}
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	" Authentication mode     " 
    ::= { dot1xInfoPortEntry 2 }

dot1xInfoPortAuthStatus OBJECT-TYPE
    SYNTAX INTEGER {
	authorized(0),
	unauthorized(1)
	}
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	" Authentication status     " 
    ::= { dot1xInfoPortEntry 3 }

dot1xInfoPortCtrlDir OBJECT-TYPE
    SYNTAX INTEGER {
	both(0),
	in(1)	
	}
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	" Controlled Directions     " 
    ::= { dot1xInfoPortEntry 4 }

dot1xInfoPortAuthPAEState OBJECT-TYPE
    SYNTAX INTEGER {
	initialize(0),
	disconnected(1),
 	connecting(2),
   	authenticating(3),
    	authenticated(4),
   	aborting(5),
    	held(6),
   	forceauth(7),
    	forceunauth(8)

	}
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"  Authenticator PAE State    " 
    ::= { dot1xInfoPortEntry 5 }

dot1xInfoPortBackAuthState OBJECT-TYPE
    SYNTAX INTEGER {
	request(0),
	response(1),
	success(2),
   	fail(3),
    	timeout(4),
   	idle(5),
    	initialize(6)

	} 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	" Backend authenticator PAE state     " 
    ::= { dot1xInfoPortEntry 6 }






dot1xSystemCapability OBJECT-TYPE
    SYNTAX INTEGER {
	authenticator(0),
	supplicant(1),
        authenticatorAndSupplicant(2),
        unknown(3)
 	}
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"  System capability    " 
    ::= { dot1xSystemInfo 1 }



dot1xSystemStatus OBJECT-TYPE
    SYNTAX INTEGER {
	enabled(0),
	disabled(1)
	}
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"  System status    " 
    ::= { dot1xSystemInfo 2 }

dot1xSystemProtoVersion OBJECT-TYPE
    SYNTAX INTEGER 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"  Protocol version   " 
    ::= { dot1xSystemInfo 3 }

-- FDB
fdbCurCfgAgingTime  OBJECT-TYPE
    SYNTAX   Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Fdb current aging time"
    ::= { fdbGeneralCfg 1 }

fdbNewCfgAgingTime OBJECT-TYPE
    SYNTAX   Integer32
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Fdb new aging time."
    ::= { fdbGeneralCfg 2 }

fdbCurCfgStaticTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF FdbCurCfgStaticEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of FDB static entries."
    ::= { fdb 3 }

fdbCurCfgStaticEntry OBJECT-TYPE
    SYNTAX  FdbCurCfgStaticEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the fdb table."
    INDEX   { fdbCurCfgEntryIndex }
    ::= { fdbCurCfgStaticTable 1 }

FdbCurCfgStaticEntry ::= SEQUENCE {
    fdbCurCfgEntryIndex                 Integer32,
    fdbCurCfgVlan                    Integer32,
    fdbCurCfgPort                    Integer32,
    fdbCurCfgMac                     PhysAddress
    }

fdbCurCfgEntryIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The fdb entry index"
    ::= { fdbCurCfgStaticEntry 1 }

fdbCurCfgVlan OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Add vlan for fdb entry index"
    ::= { fdbCurCfgStaticEntry 2 }

fdbCurCfgPort OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS   read-only
    STATUS  current
    DESCRIPTION
        "The MAC address port number."
    ::= { fdbCurCfgStaticEntry 3 }

fdbCurCfgMac OBJECT-TYPE
    SYNTAX  PhysAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Add a fdb entry."
    ::= { fdbCurCfgStaticEntry 4 }

fdbNewCfgStaticTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF FdbNewCfgStaticEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of FDB static entries."
    ::= { fdb 2 }

fdbNewCfgStaticEntry OBJECT-TYPE
    SYNTAX  FdbNewCfgStaticEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the fdb table."
    INDEX   { fdbNewCfgEntryIndex }
    ::= { fdbNewCfgStaticTable 1 }

FdbNewCfgStaticEntry ::= SEQUENCE {
    fdbNewCfgEntryIndex			Integer32,
    fdbNewCfgAddVlan	                Integer32,
    fdbNewCfgAddPort	                Integer32,
    fdbNewCfgAddMac			PhysAddress,
    fdbNewCfgDelStaticEntry		INTEGER
    }

fdbNewCfgEntryIndex OBJECT-TYPE 
    SYNTAX  Integer32 
    MAX-ACCESS  read-only 
    STATUS  current 
    DESCRIPTION 
        "The fdb entry index" 
    ::= { fdbNewCfgStaticEntry 1 }

fdbNewCfgAddVlan OBJECT-TYPE 
    SYNTAX  Integer32 
    MAX-ACCESS  read-create
    STATUS  current 
    DESCRIPTION 
        "Add vlan for fdb entry index" 
    ::= { fdbNewCfgStaticEntry 2 }

fdbNewCfgAddPort OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS   read-create
    STATUS  current
    DESCRIPTION
        "The MAC address port number." 
    ::= { fdbNewCfgStaticEntry 3 }

fdbNewCfgAddMac OBJECT-TYPE
    SYNTAX  PhysAddress
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Add a fdb entry."
    ::= { fdbNewCfgStaticEntry 4 }

fdbNewCfgDelStaticEntry OBJECT-TYPE
    SYNTAX  INTEGER {
        other(1),
        delete(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "When set to the value of 2 (delete), the entire row is deleted.
         When read, other(1) is returned. Setting the value to anything
         other than 2(delete) has no effect on the state of the row."
    ::= { fdbNewCfgStaticEntry 5 }


-- 802.1p Information

dot1pInfoPriorityCOSTable OBJECT-TYPE
    SYNTAX SEQUENCE OF Dot1pInfoPriorityCOSEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of current priority to COS queue information."
    ::= { dot1pInfo 1 }

dot1pInfoPriorityCOSEntry OBJECT-TYPE
    SYNTAX Dot1pInfoPriorityCOSEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Current information about 8021p priority to COS queue."
    INDEX { dot1pInfoPriorityIndex }
    ::= { dot1pInfoPriorityCOSTable 1 }
 
Dot1pInfoPriorityCOSEntry ::= SEQUENCE {
    dot1pInfoPriorityIndex            INTEGER,
    dot1pInfoPriorityCOSQueue         INTEGER,
    dot1pInfoPriorityCOSWeight        INTEGER   
    }
 
dot1pInfoPriorityIndex OBJECT-TYPE
    SYNTAX INTEGER  (0..7)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The 8021p priority for which the table is related."
    ::= { dot1pInfoPriorityCOSEntry 1 }

dot1pInfoPriorityCOSQueue OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The 8021p priority COSq."
    ::= { dot1pInfoPriorityCOSEntry 2 }

dot1pInfoPriorityCOSWeight OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The 8021p priority weight."
    ::= { dot1pInfoPriorityCOSEntry 3 }


dot1pInfoPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF Dot1pInfoPortEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of 8021p port priority configuration 
       in the Current_config."
    ::= { dot1pInfo 2 }

dot1pInfoPortEntry OBJECT-TYPE
    SYNTAX Dot1pInfoPortEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about 8021p Port Priority"
    INDEX { dot1pInfoPortIndex }
    ::= { dot1pInfoPortTable 1 }
 
Dot1pInfoPortEntry ::= SEQUENCE {
    dot1pInfoPortIndex               Integer32, 
    dot1pInfoPortPriority            INTEGER,
    dot1pInfoPortCOSq                INTEGER,
    dot1pInfoPortWeight              INTEGER
    }
 
dot1pInfoPortIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The 8021p Port number for which the table is related."
    ::= { dot1pInfoPortEntry 1 }

dot1pInfoPortPriority OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The 8021p Port number for which the table is related."
    ::= { dot1pInfoPortEntry 2 }

dot1pInfoPortCOSq OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The 8021p port COSq."
    ::= { dot1pInfoPortEntry 3 }

dot1pInfoPortWeight OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The 8021p port weight."
    ::= { dot1pInfoPortEntry 4 }

-- General Information

generalInfoStpUplinkFast OBJECT-TYPE
    SYNTAX  INTEGER  {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "STP uplink fast mode"
    ::= { genInfo 1 }

generalInfoUplinkFastRate OBJECT-TYPE
    SYNTAX  INTEGER 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "STP fast uplink rate."
    ::= { genInfo 2 }

-- VLAN information

vlanInfoTable OBJECT-TYPE
    SYNTAX SEQUENCE OF VlanInfoTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of VLAN information."
    ::= { vlanInfo 1 }

vlanInfoTableEntry OBJECT-TYPE
    SYNTAX VlanInfoTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a particular VLAN."
    INDEX { vlanInfoId }
    ::= { vlanInfoTable 1 }

VlanInfoTableEntry ::= SEQUENCE {
    vlanInfoId                INTEGER,
    vlanInfoName              DisplayString,
    vlanInfoStatus            INTEGER,
    vlanInfoPorts             OCTET STRING
    }

vlanInfoId OBJECT-TYPE
    SYNTAX  INTEGER  (1..4095)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The VLAN identifier."
    ::= { vlanInfoTableEntry 1 }

vlanInfoName OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..32))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The VLAN name."
    ::= { vlanInfoTableEntry 2 }

vlanInfoStatus OBJECT-TYPE
    SYNTAX  INTEGER  {
        enabled(2),
        disabled(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable, VLAN state information"
    ::= { vlanInfoTableEntry 3 }

vlanInfoPorts OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port list information in the VLAN. The ports are presented 
         in bitmap format.
         in receiving order:

             OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx ..... 
             ||    || |_ port 8
             ||    ||  
             ||    ||___ port 7
             ||    |____ port 6
             ||      .    .   .
             ||_________ port 1
             |__________ reserved

         where x : 1 - The represented port belongs to the VLAN
                   0 - The represented port does not belong to the VLAN"
    ::= { vlanInfoTableEntry 4 }


-- Trunk Group Information

trunkGroupInfoTable OBJECT-TYPE
    SYNTAX SEQUENCE OF TrunkGroupInfoTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of trunk group information."
    ::= { trunkGroupInfo 1 }

trunkGroupInfoTableEntry OBJECT-TYPE
    SYNTAX TrunkGroupInfoTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "A row in trunk group information table."
    INDEX { trunkGroupInfoIndex }
    ::= { trunkGroupInfoTable 1 }

TrunkGroupInfoTableEntry ::= SEQUENCE {
    trunkGroupInfoIndex       Integer32,
    trunkGroupInfoState       INTEGER,
    trunkGroupInfoProtocol    INTEGER,
    trunkGroupInfoPorts       OCTET STRING,
    trunkGroupInfoStgs        OCTET STRING
    }

trunkGroupInfoIndex OBJECT-TYPE
    SYNTAX  Integer32  
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The identifier of the trunk group."
    ::= { trunkGroupInfoTableEntry 1 }

trunkGroupInfoState OBJECT-TYPE
    SYNTAX  INTEGER  {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Trunk group state."
    ::= { trunkGroupInfoTableEntry 2 }

trunkGroupInfoPorts OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port list in the trunk group. The ports are presented in 
         bitmap format.
 
         in receiving order:
 
             OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx ..... 
             ||    || |_ port 8
             ||    ||  
             ||    ||___ port 7
             ||    |____ port 6
             ||      .    .   .
             ||_________ port 1
             |__________ reserved

         where x : 1 - The represented port belongs to the trunk group
                   0 - The represented port does not belong to the trunk group"
    ::= { trunkGroupInfoTableEntry 3 }

trunkGroupInfoProtocol OBJECT-TYPE
    SYNTAX  INTEGER  {
        static(1),
        lacp(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Trunk group protocol
         Static - static trunk group
         Lacp - dynamic trunk group"
    ::= { trunkGroupInfoTableEntry 4 }

trunkGroupInfoStgs OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The stg list the trunk group is in. The stgs are presented in
         bitmap format."
    ::= { trunkGroupInfoTableEntry 5 }


trunkGroupInfoPortTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF TrunkGroupInfoPortTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of Trunk Group Info."
    ::= {trunkGroupInfo 2 }

trunkGroupInfoPortTableEntry OBJECT-TYPE
    SYNTAX  TrunkGroupInfoPortTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the Trunk Info table."
    INDEX  { trunkGroupInfoPortTrunkId, trunkGroupInfoPortPortId }
    ::= { trunkGroupInfoPortTable 1 }

TrunkGroupInfoPortTableEntry ::= SEQUENCE {
    trunkGroupInfoPortTrunkId   Integer32,
    trunkGroupInfoPortPortId    Integer32,
    trunkGroupInfoPortStatus    INTEGER
    }

trunkGroupInfoPortTrunkId OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Trunk identifier."
    ::= { trunkGroupInfoPortTableEntry 1 }

trunkGroupInfoPortPortId OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Port identifier."
    ::= { trunkGroupInfoPortTableEntry 2 }

trunkGroupInfoPortStatus OBJECT-TYPE
    SYNTAX  INTEGER{
        down(0),
        blocking(1),
        forwarding(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Port Status."
    ::= { trunkGroupInfoPortTableEntry 3 }

-- ----------------------------------------------------------------------------
-- } INSERT:  bt2Physical
-- ----------------------------------------------------------------------------


layer3                  OBJECT IDENTIFIER
    ::= { hpSwitchBladeType5-Mgmt 3 }

-- ----------------------------------------------------------------------------
-- { INSERT:  bt2Network
-- ----------------------------------------------------------------------------

layer3Configs     OBJECT IDENTIFIER ::= { layer3 1 }
layer3Stats       OBJECT IDENTIFIER ::= { layer3 2 }
layer3Info        OBJECT IDENTIFIER ::= { layer3 3 }
layer3Oper        OBJECT IDENTIFIER ::= { layer3 4 }

ipInterfaceCfg	  OBJECT IDENTIFIER ::= { layer3Configs 1 }
ipGatewayCfg	  OBJECT IDENTIFIER ::= { layer3Configs 2 }
ipStaticRouteCfg  OBJECT IDENTIFIER ::= { layer3Configs 3 }
ipForwardCfg	  OBJECT IDENTIFIER ::= { layer3Configs 4 }
vrrpCfg		  OBJECT IDENTIFIER ::= { layer3Configs 6 }
arpCfg		  OBJECT IDENTIFIER ::= { layer3Configs 7 }
ipBootpCfg	  OBJECT IDENTIFIER ::= { layer3Configs 8 }
dnsCfg  	  OBJECT IDENTIFIER ::= { layer3Configs 9 }
ipNwfCfg	  OBJECT IDENTIFIER ::= { layer3Configs 10 }
ipRmapCfg	  OBJECT IDENTIFIER ::= { layer3Configs 11 }
ospfCfg           OBJECT IDENTIFIER ::= { layer3Configs 13 }

ipGeneralCfg	  OBJECT IDENTIFIER ::= { layer3Configs 14 }
igmpCfg	          OBJECT IDENTIFIER ::= { layer3Configs 15 }
rip2Cfg		  OBJECT IDENTIFIER ::= { layer3Configs 18 }

arpStats  	  OBJECT IDENTIFIER ::= { layer3Stats 2 }
routeStats  	  OBJECT IDENTIFIER ::= { layer3Stats 3 }
vrrpStats         OBJECT IDENTIFIER ::= { layer3Stats 4 }
ospfStats	  OBJECT IDENTIFIER ::= { layer3Stats 5 }
clearStats	  OBJECT IDENTIFIER ::= { layer3Stats 6 }
igmpStats	  OBJECT IDENTIFIER ::= { layer3Stats 7 }
ipStats           OBJECT IDENTIFIER ::= { layer3Stats 8 }
rip2Stats  	  OBJECT IDENTIFIER ::= { layer3Stats 13 }
dnsStats  	  OBJECT IDENTIFIER ::= { layer3Stats 14 }
geal3Stats	  OBJECT IDENTIFIER ::= { layer3Stats 15 }
ipRoutingInfo	  OBJECT IDENTIFIER ::= { layer3Info 1 }
arpInfo		  OBJECT IDENTIFIER ::= { layer3Info 2 }
vrrpInfo	  OBJECT IDENTIFIER ::= { layer3Info 3 }
ospfInfo	  OBJECT IDENTIFIER ::= { layer3Info 4 }
igmpInfo	  OBJECT IDENTIFIER ::= { layer3Info 5 }
rip2Info          OBJECT IDENTIFIER ::= { layer3Info 7 }

ipInfo            OBJECT IDENTIFIER ::= { layer3Info 8 }

vrrpOper          OBJECT IDENTIFIER ::= { layer3Oper 1 }


-- IP Configuration

ipInterfaceTableMax OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum number of rows in the IP interface table."
    ::= { ipInterfaceCfg 1 }

ipCurCfgIntfTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF IpCurCfgIntfEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of IP interface configuration."
    ::= { ipInterfaceCfg 2 }

ipCurCfgIntfEntry OBJECT-TYPE
    SYNTAX  IpCurCfgIntfEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the Ip interface table"
    INDEX   { ipCurCfgIntfIndex }
    ::= { ipCurCfgIntfTable 1 }

IpCurCfgIntfEntry ::= SEQUENCE {
    ipCurCfgIntfIndex         Integer32,
    ipCurCfgIntfAddr          IpAddress,
    ipCurCfgIntfMask          IpAddress,
    ipCurCfgIntfBroadcast     IpAddress,
    ipCurCfgIntfVlan          INTEGER,
    ipCurCfgIntfState         INTEGER,
    ipCurCfgIntfBootpRelay    INTEGER
    }
 
ipCurCfgIntfIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The interface number for which the IP information is related."
    ::= { ipCurCfgIntfEntry 1}

ipCurCfgIntfAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IP address of the interface."
    ::= { ipCurCfgIntfEntry 2 }

ipCurCfgIntfMask OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current  
    DESCRIPTION
        "The subnet mask of the interface."
    ::= { ipCurCfgIntfEntry 3 }

ipCurCfgIntfBroadcast OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current  
    DESCRIPTION
        "The broadcast address of the interface."
    ::= { ipCurCfgIntfEntry 4 }

ipCurCfgIntfVlan OBJECT-TYPE
    SYNTAX  INTEGER (1..4094)
    MAX-ACCESS  read-only
    STATUS  current  
    DESCRIPTION
        "The VLAN associated with the interface."
    ::= { ipCurCfgIntfEntry 5 }

ipCurCfgIntfState OBJECT-TYPE
    SYNTAX  INTEGER { 
	enabled(2),
	disabled(3)
	}
    MAX-ACCESS  read-only
    STATUS  current  
    DESCRIPTION
        "The state of the interface."
    ::= { ipCurCfgIntfEntry 6 }

ipCurCfgIntfBootpRelay OBJECT-TYPE
    SYNTAX  INTEGER { 
	enabled(1),
	disabled(2)
	}
    MAX-ACCESS  read-only
    STATUS  current  
    DESCRIPTION
        "Enable/disable BOOTP relay."
    ::= { ipCurCfgIntfEntry 7 }

ipNewCfgIntfTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF IpNewCfgIntfEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of interface configuration in the New Configuration Block."
    ::= { ipInterfaceCfg 3 }

ipNewCfgIntfEntry OBJECT-TYPE
    SYNTAX  IpNewCfgIntfEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the Ip interface table"
    INDEX   { ipNewCfgIntfIndex }
    ::= { ipNewCfgIntfTable 1 }
 
IpNewCfgIntfEntry ::= SEQUENCE {
    ipNewCfgIntfIndex         Integer32,
    ipNewCfgIntfAddr          IpAddress,
    ipNewCfgIntfMask          IpAddress,
    ipNewCfgIntfVlan          INTEGER,
    ipNewCfgIntfState         INTEGER,
    ipNewCfgIntfDelete	      INTEGER,
    ipNewCfgIntfBootpRelay    INTEGER
    }
 
ipNewCfgIntfIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	"The interface number for which the IP information is related."
    ::= { ipNewCfgIntfEntry 1 }

ipNewCfgIntfAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The IP address of the interface."
    ::= { ipNewCfgIntfEntry 2 }

ipNewCfgIntfMask OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-create
    STATUS  current  
    DESCRIPTION
        "The subnet mask of the interface."
    ::= { ipNewCfgIntfEntry 3 }

ipNewCfgIntfVlan OBJECT-TYPE
    SYNTAX  INTEGER (1..4094)
    MAX-ACCESS  read-create
    STATUS  current  
    DESCRIPTION
        "The VLAN associated with the interface."
    ::= { ipNewCfgIntfEntry 5 }

ipNewCfgIntfState OBJECT-TYPE
    SYNTAX  INTEGER { 
	enabled(2),
	disabled(3)
	}
    MAX-ACCESS  read-create
    STATUS  current  
    DESCRIPTION
        "The state of the interface."
    ::= { ipNewCfgIntfEntry 6 }

ipNewCfgIntfDelete OBJECT-TYPE
    SYNTAX  INTEGER { 
	other(1),
        delete(2)
	}
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "When set to the value of 2 (delete), the entire row is deleted. 
         When read, other(1) is returned. Setting the value to anything 
         other than 2(delete) has no effect on the state of the row."
    ::= { ipNewCfgIntfEntry 7 }

ipNewCfgIntfBootpRelay OBJECT-TYPE
    SYNTAX  INTEGER { 
	enabled(1),
	disabled(2)
	}
    MAX-ACCESS  read-create
    STATUS  current  
    DESCRIPTION
        "Enable/disable BOOTP relay."
    ::= { ipNewCfgIntfEntry 8 }

-- IP Gateway Table Configuration


ipGatewayTableMax OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum number of rows in the IP gateway table."
    ::= { ipGatewayCfg 3 }

ipCurCfgGwTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF IpCurCfgGwEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of gateways  in the Current configuration Block."
    ::= { ipGatewayCfg 4 }

ipCurCfgGwEntry OBJECT-TYPE
    SYNTAX  IpCurCfgGwEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the Ip gateway table"
    INDEX   { ipCurCfgGwIndex }
    ::= { ipCurCfgGwTable 1 }

IpCurCfgGwEntry ::= SEQUENCE {
    ipCurCfgGwIndex         Integer32,
    ipCurCfgGwAddr          IpAddress,
    ipCurCfgGwInterval      INTEGER,
    ipCurCfgGwRetry         INTEGER,
    ipCurCfgGwArp           INTEGER,
    ipCurCfgGwState         INTEGER
    }

ipCurCfgGwIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The gateway number for which the information is related."
    ::= { ipCurCfgGwEntry 1}

ipCurCfgGwAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IP address of the default gateway."
    ::= { ipCurCfgGwEntry 2 }

ipCurCfgGwInterval OBJECT-TYPE 
    SYNTAX  INTEGER (0..60)
    MAX-ACCESS  read-only 
    STATUS  current 
    DESCRIPTION 
        "The interval between ping attempts." 
    ::= { ipCurCfgGwEntry 3 }

ipCurCfgGwRetry OBJECT-TYPE
    SYNTAX  INTEGER (1..120)   
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The number of failed attempts to declare the default gateway DOWN."
    ::= { ipCurCfgGwEntry 4 }

ipCurCfgGwState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(2),
        disabled(3)
	}  
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The state of the default gateway."
    ::= { ipCurCfgGwEntry 5 }

ipCurCfgGwArp OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(2),
        disabled(3)
        } 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The state of ARP only health checks."
    ::= { ipCurCfgGwEntry 6 }


ipNewCfgGwTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF IpNewCfgGwEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of gateway configuration in the new configuration block."
    ::= { ipGatewayCfg 5 }

ipNewCfgGwEntry OBJECT-TYPE
    SYNTAX  IpNewCfgGwEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the Ip default gateway table"
    INDEX   { ipNewCfgGwIndex }
    ::= { ipNewCfgGwTable 1 }

IpNewCfgGwEntry ::= SEQUENCE {
    ipNewCfgGwIndex         Integer32,
    ipNewCfgGwAddr          IpAddress,
    ipNewCfgGwInterval      INTEGER,
    ipNewCfgGwRetry         INTEGER,
    ipNewCfgGwState         INTEGER,
    ipNewCfgGwArp           INTEGER,
    ipNewCfgGwDelete        INTEGER
    }

ipNewCfgGwIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The gateway number for which the information is related."
    ::= { ipNewCfgGwEntry 1}

ipNewCfgGwAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The IP address of the default gateway."
    ::= { ipNewCfgGwEntry 2 }

ipNewCfgGwInterval OBJECT-TYPE 
    SYNTAX  INTEGER (0..60)
    MAX-ACCESS  read-create 
    STATUS  current 
    DESCRIPTION 
        "The interval in seconds between ping attempts." 
    ::= { ipNewCfgGwEntry 3 }

ipNewCfgGwRetry OBJECT-TYPE
    SYNTAX  INTEGER (1..120)   
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The number of failed attempts to declare the default gateway DOWN."
    ::= { ipNewCfgGwEntry 4 }

ipNewCfgGwState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(2),
        disabled(3)
	}
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The state of the default gateway."
    ::= { ipNewCfgGwEntry 5 }

ipNewCfgGwDelete OBJECT-TYPE
    SYNTAX  INTEGER {
	other(1),
        delete(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "When set to the value of 2 (delete), the entire row is deleted. 
         When read, other is returned. Setting the value to anything other 
         than 2(delete) has no effect on the state of the row."
    ::= { ipNewCfgGwEntry 6 }

ipNewCfgGwArp OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(2),
        disabled(3)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The state of the ARP only health checks."
    ::= { ipNewCfgGwEntry 7 }


--
-- IP Static Route Configuration
--
ipStaticRouteTableMaxSize OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum number of rows in the Static Route table."
    ::= { ipStaticRouteCfg 1 }

ipCurCfgStaticRouteTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF IpCurCfgStaticRouteEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of static routes in the current configuration block."
    ::= { ipStaticRouteCfg 2 }

ipCurCfgStaticRouteEntry OBJECT-TYPE
    SYNTAX  IpCurCfgStaticRouteEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the static IP route table"
    INDEX   { ipCurCfgStaticRouteIndx }
    ::= { ipCurCfgStaticRouteTable 1 }

IpCurCfgStaticRouteEntry ::= SEQUENCE {
    ipCurCfgStaticRouteIndx         Integer32,
    ipCurCfgStaticRouteDestIp       IpAddress,
    ipCurCfgStaticRouteMask         IpAddress,
    ipCurCfgStaticRouteGateway      IpAddress,
    ipCurCfgStaticRouteInterface    Integer32
    }

ipCurCfgStaticRouteIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The index of the static routing table."
    ::= { ipCurCfgStaticRouteEntry 1}

ipCurCfgStaticRouteDestIp OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The destination IP address of this route."
    ::= { ipCurCfgStaticRouteEntry 2}

ipCurCfgStaticRouteMask OBJECT-TYPE 
    SYNTAX  IpAddress
    MAX-ACCESS  read-only 
    STATUS  current 
    DESCRIPTION 
        "The destination IP address of this route."
    ::= { ipCurCfgStaticRouteEntry 3}

ipCurCfgStaticRouteGateway OBJECT-TYPE 
    SYNTAX  IpAddress
    MAX-ACCESS  read-only 
    STATUS  current 
    DESCRIPTION 
        "The destination IP address of this route."
    ::= { ipCurCfgStaticRouteEntry 4}

ipCurCfgStaticRouteInterface OBJECT-TYPE 
    SYNTAX  Integer32
    MAX-ACCESS  read-only 
    STATUS  current 
    DESCRIPTION 
        "The IP interface of this route.  The IP address of the specified 
         interface shall be use as source IP when performs routing."
    ::= { ipCurCfgStaticRouteEntry 5}

ipNewCfgStaticRouteTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF IpNewCfgStaticRouteEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of static routes in the new configuration block."
    ::= { ipStaticRouteCfg 3 }

ipStaticRouteClearAllByDestIp OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Clears all static routes with the specified destination IP address."
    ::= { ipStaticRouteCfg 4}

ipStaticRouteClearAllByGatewayIp OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Clears all static routes with the specified gateway IP address."
    ::= { ipStaticRouteCfg 5}

ipStaticRouteClearAllByInterface OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Clears all routes on the specified inteface number."
    ::= { ipStaticRouteCfg 6}

ipStaticRouteClearAll OBJECT-TYPE
    SYNTAX INTEGER { 
	ok(1),
	clear(2)
	}
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "When set to clear(2),clears all static routes. Otherwhise nothing is done."
    ::= { ipStaticRouteCfg 7}

ipNewCfgStaticRouteEntry OBJECT-TYPE
    SYNTAX  IpNewCfgStaticRouteEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the static IP route table"
    INDEX   { ipNewCfgStaticRouteIndx }
    ::= { ipNewCfgStaticRouteTable 1 }

IpNewCfgStaticRouteEntry ::= SEQUENCE {
    ipNewCfgStaticRouteIndx         Integer32,
    ipNewCfgStaticRouteDestIp       IpAddress,
    ipNewCfgStaticRouteMask         IpAddress,
    ipNewCfgStaticRouteGateway      IpAddress,
    ipNewCfgStaticRouteAction       INTEGER,
    ipNewCfgStaticRouteInterface    Integer32
    }

ipNewCfgStaticRouteIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The index of the static routing table."
    ::= { ipNewCfgStaticRouteEntry 1}

ipNewCfgStaticRouteDestIp OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The destination IP address of this route."
    ::= { ipNewCfgStaticRouteEntry 2}

ipNewCfgStaticRouteMask OBJECT-TYPE 
    SYNTAX  IpAddress
    MAX-ACCESS  read-create 
    STATUS  current 
    DESCRIPTION 
        "The subnet mask of this route."
    ::= { ipNewCfgStaticRouteEntry 3}

ipNewCfgStaticRouteGateway OBJECT-TYPE 
    SYNTAX  IpAddress
    MAX-ACCESS  read-create 
    STATUS  current 
    DESCRIPTION 
        "The IP address of the gateway for this route."
    ::= { ipNewCfgStaticRouteEntry 4}

ipNewCfgStaticRouteAction OBJECT-TYPE
    SYNTAX  INTEGER {
        other(1),
        delete(2)
       }  
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "When set to the value of 2 (delete), the entire row is deleted. 
         When read, other is returned. Setting the value to anything other 
         than 2(delete) has no effect on the state of the row."
    ::= { ipNewCfgStaticRouteEntry 5 }

ipNewCfgStaticRouteInterface OBJECT-TYPE 
    SYNTAX  Integer32
    MAX-ACCESS  read-create 
    STATUS  current 
    DESCRIPTION 
        "The IP interface of this route.  The IP address of the specified 
         interface shall be use as source IP when performs routing."
    ::= { ipNewCfgStaticRouteEntry 6 }



-- RIP version 2 Configuration 

ripCurCfgIntfTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RipCurCfgIntfEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of RIP on IP interface configuration in the current_config."
    ::= { rip2Cfg 1 }

ripCurCfgIntfEntry OBJECT-TYPE
    SYNTAX RipCurCfgIntfEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about  RIP on IP interface."
    INDEX { ripCurCfgIntfIndex }
    ::= { ripCurCfgIntfTable 1 }
 
RipCurCfgIntfEntry ::= SEQUENCE {
    ripCurCfgIntfIndex  	INTEGER,
    ripCurCfgIntfVersion	INTEGER,
    ripCurCfgIntfSupply		INTEGER,
    ripCurCfgIntfListen		INTEGER,
    ripCurCfgIntfDefault	INTEGER,
    ripCurCfgIntfTrigUpdate	INTEGER,
    ripCurCfgIntfMcastUpdate	INTEGER,
    ripCurCfgIntfPoisonReverse	INTEGER,
    ripCurCfgIntfState		INTEGER,
    ripCurCfgIntfMetric         INTEGER, 
    ripCurCfgIntfAuth           INTEGER, 
    ripCurCfgIntfKey            DisplayString, 
    ripCurCfgIntfSplitHorizon   INTEGER
    }
 
ripCurCfgIntfIndex OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The interface number for which the RIP information is related."
    ::= { ripCurCfgIntfEntry 1}

ripCurCfgIntfVersion OBJECT-TYPE
    SYNTAX INTEGER {
        ripVersion1(1),
        ripVersion2(2),
        ripVersionBoth(3)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "RIP version."
    ::= { ripCurCfgIntfEntry 2 }

ripCurCfgIntfSupply OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Enable or disable supplying route updates."
    ::= { ripCurCfgIntfEntry 3 }

ripCurCfgIntfListen OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Enable or disable listening to route updates."
    ::= { ripCurCfgIntfEntry 4 }

 ripCurCfgIntfDefault OBJECT-TYPE
    SYNTAX  INTEGER {
        both(1),
        listen(2),
        supply(3),
        none(4)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Specifies what RIP does with default routes."
    ::= { ripCurCfgIntfEntry 5 }

ripCurCfgIntfTrigUpdate OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Enable or disable tirggered updates."
    ::= { ripCurCfgIntfEntry 6 }

ripCurCfgIntfMcastUpdate OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Enable or disable multicast updates."
    ::= { ripCurCfgIntfEntry 7 }

ripCurCfgIntfPoisonReverse OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"RIP poison reverse."
    ::= { ripCurCfgIntfEntry 8 }

ripCurCfgIntfState OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Enable or disable RIP protocol."
    ::= { ripCurCfgIntfEntry 9 }

ripCurCfgIntfMetric OBJECT-TYPE
    SYNTAX  INTEGER (1..16)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "RIP route metric for this interface."
    ::= { ripCurCfgIntfEntry 10 }

ripCurCfgIntfAuth OBJECT-TYPE
    SYNTAX INTEGER {
        none(1),
        password(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Enable or disable RIP update authorization with a 
         simple plain text password."
    ::= { ripCurCfgIntfEntry 11 }

ripCurCfgIntfKey OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..16))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "RIP update authentication password."
    ::= { ripCurCfgIntfEntry 12 }

ripCurCfgIntfSplitHorizon OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(2),
        disabled(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
         "RIP split horizon."
    ::= {ripCurCfgIntfEntry 13 }

ripNewCfgIntfTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RipNewCfgIntfEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of RIP on IP interface configuration in the new_config."
    ::= { rip2Cfg 2 }

ripNewCfgIntfEntry OBJECT-TYPE
    SYNTAX RipNewCfgIntfEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about  RIP on IP interface."
    INDEX { ripNewCfgIntfIndex }
    ::= { ripNewCfgIntfTable 1 }
 
RipNewCfgIntfEntry ::= SEQUENCE {
    ripNewCfgIntfIndex  	INTEGER,
    ripNewCfgIntfVersion	INTEGER,
    ripNewCfgIntfSupply		INTEGER,
    ripNewCfgIntfListen		INTEGER,
    ripNewCfgIntfDefault	INTEGER,
    ripNewCfgIntfTrigUpdate	INTEGER,
    ripNewCfgIntfMcastUpdate	INTEGER,
    ripNewCfgIntfPoisonReverse	INTEGER,
    ripNewCfgIntfState		INTEGER,
    ripNewCfgIntfMetric         INTEGER, 
    ripNewCfgIntfAuth           INTEGER, 
    ripNewCfgIntfKey            DisplayString, 
    ripNewCfgIntfSplitHorizon   INTEGER
    }
 
ripNewCfgIntfIndex OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The interface number for which the RIP information is related."
    ::= { ripNewCfgIntfEntry 1}

ripNewCfgIntfVersion OBJECT-TYPE
    SYNTAX INTEGER {
        ripVersion1(1),
        ripVersion2(2),
        ripVersionBoth(3)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "RIP version."
    ::= { ripNewCfgIntfEntry 2 }

ripNewCfgIntfSupply OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Enable or disable supplying route updates."
    ::= { ripNewCfgIntfEntry 3 }

ripNewCfgIntfListen OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Enable or disable listening to route updates."
    ::= { ripNewCfgIntfEntry 4 }

 ripNewCfgIntfDefault OBJECT-TYPE
    SYNTAX INTEGER {
        both(1),
        listen(2),
        supply(3),
        none(4)
        }
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"Specifies what RIP does with default routes. The default routes 
         action could be set to listen/supply/both/none."
    ::= { ripNewCfgIntfEntry 5 }

ripNewCfgIntfTrigUpdate OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"Enable or disable tirggered updates."
    ::= { ripNewCfgIntfEntry 6 }

ripNewCfgIntfMcastUpdate OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"Enable or disable multicast updates."
    ::= { ripNewCfgIntfEntry 7 }

ripNewCfgIntfPoisonReverse OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"RIP poison reverse."
    ::= { ripNewCfgIntfEntry 8 }

ripNewCfgIntfState OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Enable or disable RIP protocol."
    ::= { ripNewCfgIntfEntry 9 }

ripNewCfgIntfMetric OBJECT-TYPE
    SYNTAX  INTEGER (1..15)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "RIP route metric for this interface."
    ::= { ripNewCfgIntfEntry 10 }

ripNewCfgIntfAuth OBJECT-TYPE
    SYNTAX INTEGER {
        none(1),
        password(2)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Enable or disable RIP update authorization with a 
         simple plain text password."
    ::= { ripNewCfgIntfEntry 11 }

ripNewCfgIntfKey OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..16))
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "RIP update authentication password."
    ::= { ripNewCfgIntfEntry 12 }

ripNewCfgIntfSplitHorizon OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(2),
        disabled(3)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "RIP split horizon."
    ::= { ripNewCfgIntfEntry 13 }

ripGeneral	OBJECT IDENTIFIER ::= { rip2Cfg 3 }

rip2CurCfgState OBJECT-TYPE
    SYNTAX INTEGER {
        on(1),
        off(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"RIP global state."
    ::= { ripGeneral 1 }

rip2NewCfgState OBJECT-TYPE
    SYNTAX INTEGER {
        on(1),
        off(2)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"Globally turn RIP on or off."
    ::= { ripGeneral 2 }

rip2CurCfgUpdatePeriod OBJECT-TYPE
      SYNTAX  INTEGER  (1..120)
      MAX-ACCESS  read-only
      STATUS  current
      DESCRIPTION
	      "Update Period in seconds."
      ::= { ripGeneral 3 }

rip2NewCfgUpdatePeriod OBJECT-TYPE
      SYNTAX  INTEGER  (1..120)
      MAX-ACCESS  read-write
      STATUS  current
      DESCRIPTION
	      "Update Period in seconds."
      ::= { ripGeneral 4 }

ripRouteRedistribution   OBJECT IDENTIFIER ::= { rip2Cfg 4 }

ripRedistributeStatic    OBJECT IDENTIFIER ::= { ripRouteRedistribution 1 }

ripCurCfgStaticMetric OBJECT-TYPE
    SYNTAX INTEGER (0..15)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The metric to be assigned to static routes. 
         A value of 0 indicates none."
    ::= { ripRedistributeStatic 1 }

ripNewCfgStaticMetric OBJECT-TYPE
    SYNTAX INTEGER (0..15)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"The metric to be assigned to static routes. 
         A value of 0 indicates none."
    ::= { ripRedistributeStatic 2 }

ripCurCfgStaticOutRmapList OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The route maps present in the out route map list. 
         The route maps are presented in a bitmap format.

         in receiving order:

         OCTET 1  OCTET 2  .....
         xxxxxxxx xxxxxxxx .....
         ||    || |_ Rmap 9
         ||    ||
         ||    ||___ Rmap 8
         ||    |____ Rmap 7
         ||      .    .   .
         ||_________ Rmap 2
         |__________ Rmap 1

         where x : 1 - The represented route map is selected
         0 - The represented route map is not selected"
    ::= { ripRedistributeStatic 5 }

ripNewCfgStaticOutRmapList OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The route maps present in the out route map list. 
         The route maps are presented in a bitmap format.

         in receiving order:

         OCTET 1  OCTET 2  .....
         xxxxxxxx xxxxxxxx .....
         ||    || |_ Rmap 9
         ||    ||
         ||    ||___ Rmap 8
         ||    |____ Rmap 7
         ||      .    .   .
         ||_________ Rmap 2
         |__________ Rmap 1

         where x : 1 - The represented route map is selected
         0 - The represented route map is not selected"
    ::= { ripRedistributeStatic 6 }

ripNewCfgStaticAddOutRmap OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS read-write
    STATUS current  
    DESCRIPTION
	"The route map to be add into out-rmap list. When read, 0 is returned."
    ::= { ripRedistributeStatic 7 }

ripNewCfgStaticRemoveOutRmap OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS read-write
    STATUS current  
    DESCRIPTION
	"The route map to be removed from out-rmap list. When read, 
         0 is returned."
    ::= { ripRedistributeStatic 8 }


ripRedistributeFixed    OBJECT IDENTIFIER ::= { ripRouteRedistribution 4 }

ripCurCfgFixedMetric OBJECT-TYPE
    SYNTAX INTEGER (0..15)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The export metric for fixed routes. A value of 0 indicates none"
    ::= { ripRedistributeFixed 1 }

ripNewCfgFixedMetric OBJECT-TYPE
    SYNTAX INTEGER (0..15)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"The export metric for fixed routes. A value of 0 indicates none"
    ::= { ripRedistributeFixed 2 }

ripCurCfgFixedOutRmapList OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The route maps present in the out route map list. 
         The route maps are presented in a bitmap format.

         in receiving order:

         OCTET 1  OCTET 2  .....
         xxxxxxxx xxxxxxxx .....
         ||    || |_ Rmap 9
         ||    ||
         ||    ||___ Rmap 8
         ||    |____ Rmap 7
         ||      .    .   .
         ||_________ Rmap 2
         |__________ Rmap 1

         where x : 1 - The represented route map is selected
         0 - The represented route map is not selected"
    ::= { ripRedistributeFixed 5 }

ripNewCfgFixedOutRmapList OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The route maps present in the out route map list. 
         The route maps are presented in a bitmap format.

         in receiving order:

         OCTET 1  OCTET 2  .....
         xxxxxxxx xxxxxxxx .....
         ||    || |_ Rmap 9
         ||    ||
         ||    ||___ Rmap 8
         ||    |____ Rmap 7
         ||      .    .   .
         ||_________ Rmap 2
         |__________ Rmap 1

         where x : 1 - The represented route map is selected
         0 - The represented route map is not selected"
    ::= { ripRedistributeFixed 6 }

ripNewCfgFixedAddOutRmap OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS read-write
    STATUS current  
    DESCRIPTION
	"The route map to be add into out-rmap list. When read, 0 is returned."
    ::= { ripRedistributeFixed 7 }

ripNewCfgFixedRemoveOutRmap OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS read-write
    STATUS current  
    DESCRIPTION
	"The route map to be removed from out-rmap list. When read, 
         0 is returned."
    ::= { ripRedistributeFixed 8 }

ripRedistributeOspf    OBJECT IDENTIFIER ::= { ripRouteRedistribution 5 }

ripCurCfgOspfMetric OBJECT-TYPE
    SYNTAX INTEGER (0..15)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The export metric for RIP routes. A value of 0 indicates none"
    ::= { ripRedistributeOspf 1 }

ripNewCfgOspfMetric OBJECT-TYPE
    SYNTAX INTEGER (0..15)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"The export metric for RIP routes. A value of 0 indicates none"
    ::= { ripRedistributeOspf 2 }

ripCurCfgOspfOutRmapList OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The route maps present in the out route map list. 
         The route maps are presented in a bitmap format.

         in receiving order:

         OCTET 1  OCTET 2  .....
         xxxxxxxx xxxxxxxx .....
         ||    || |_ Rmap 9
         ||    ||
         ||    ||___ Rmap 8
         ||    |____ Rmap 7
         ||      .    .   .
         ||_________ Rmap 2
         |__________ Rmap 1

         where x : 1 - The represented route map is selected
         0 - The represented route map is not selected"
    ::= { ripRedistributeOspf 5 }

ripNewCfgOspfOutRmapList OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The route maps present in the out route map list. 
         The route maps are presented in a bitmap format.

         in receiving order:

         OCTET 1  OCTET 2  .....
         xxxxxxxx xxxxxxxx .....
         ||    || |_ Rmap 9
         ||    ||
         ||    ||___ Rmap 8
         ||    |____ Rmap 7
         ||      .    .   .
         ||_________ Rmap 2
         |__________ Rmap 1

         where x : 1 - The represented route map is selected
         0 - The represented route map is not selected"
    ::= { ripRedistributeOspf 6 }

ripNewCfgOspfAddOutRmap OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS read-write
    STATUS current  
    DESCRIPTION
	"The route map to be add into out-rmap list. When read, 0 is returned."
    ::= { ripRedistributeOspf 7 }

ripNewCfgOspfRemoveOutRmap OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS read-write
    STATUS current  
    DESCRIPTION
	"The route map to be removed from out-rmap list. When read, 
         0 is returned."
    ::= { ripRedistributeOspf 8 }

ripRedistributeEospf    OBJECT IDENTIFIER ::= { ripRouteRedistribution 6 }

ripCurCfgEospfMetric OBJECT-TYPE
    SYNTAX INTEGER (0..15)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The export metric for RIP routes. A value of 0 indicates none"
    ::= { ripRedistributeEospf 1 }

ripNewCfgEospfMetric OBJECT-TYPE
    SYNTAX INTEGER (0..15)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"The export metric for RIP routes. A value of 0 indicates none"
    ::= { ripRedistributeEospf 2 }

ripCurCfgEospfOutRmapList OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The route maps present in the out route map list. 
         The route maps are presented in a bitmap format.

         in receiving order:

         OCTET 1  OCTET 2  .....
         xxxxxxxx xxxxxxxx .....
         ||    || |_ Rmap 9
         ||    ||
         ||    ||___ Rmap 8
         ||    |____ Rmap 7
         ||      .    .   .
         ||_________ Rmap 2
         |__________ Rmap 1

         where x : 1 - The represented route map is selected
         0 - The represented route map is not selected"
    ::= { ripRedistributeEospf 5 }

ripNewCfgEospfOutRmapList OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The route maps present in the out route map list. 
         The route maps are presented in a bitmap format.

         in receiving order:

         OCTET 1  OCTET 2  .....
         xxxxxxxx xxxxxxxx .....
         ||    || |_ Rmap 9
         ||    ||
         ||    ||___ Rmap 8
         ||    |____ Rmap 7
         ||      .    .   .
         ||_________ Rmap 2
         |__________ Rmap 1

         where x : 1 - The represented route map is selected
         0 - The represented route map is not selected"
    ::= { ripRedistributeEospf 6 }

ripNewCfgEospfAddOutRmap OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS read-write
    STATUS current  
    DESCRIPTION
	"The route map to be add into out-rmap list. When read, 0 is returned."
    ::= { ripRedistributeEospf 7 }

ripNewCfgEospfRemoveOutRmap OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS read-write
    STATUS current  
    DESCRIPTION
	"The route map to be removed from out-rmap list. When read, 
         0 is returned."
    ::= { ripRedistributeEospf 8 }

-- IP Forwarding Configuration 

ipFwdGeneralCfg   OBJECT IDENTIFIER ::=  {ipForwardCfg 1 }

ipFwdCurCfgState OBJECT-TYPE
    SYNTAX  INTEGER {
        on(2),
        off(3)
	}
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "IP forwarding global state."
    ::= { ipFwdGeneralCfg 1 }

ipFwdNewCfgState OBJECT-TYPE
    SYNTAX  INTEGER { 
        on(2),
        off(3) 
	}
    MAX-ACCESS  read-write
    STATUS  current  
    DESCRIPTION 
        "IP forwarding global state." 
    ::= { ipFwdGeneralCfg 2 }

ipFwdCurCfgDirectedBcast OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(2),
        disabled(3)
	}
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Enable or disable forwarding directed broadcasts."
    ::= { ipFwdGeneralCfg 3 }

ipFwdNewCfgDirectedBcast OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(2),
        disabled(3)
	}
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Enable or disable forwarding directed broadcasts."
    ::= { ipFwdGeneralCfg 4 }


--
-- ARP configuration
--
arpCurCfgReARPPeriod OBJECT-TYPE
    SYNTAX INTEGER (2..120)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Re-ARP Period in seconds."
    ::= { arpCfg 1 }

arpNewCfgReARPPeriod OBJECT-TYPE 
    SYNTAX  INTEGER (2..120)
    MAX-ACCESS  read-write
    STATUS  current 
    DESCRIPTION 
        "Re-ARP Period in seconds." 
    ::= { arpCfg 2 }

--
-- Static ARP Configuration
--
ipStaticArpTableMaxSize OBJECT-TYPE
    SYNTAX  INTEGER (1..128)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum number of rows in the Static ARP table."
    ::= { arpCfg 3 }

ipCurCfgStaticArpTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF IpCurCfgStaticArpEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of static ARPs in the current configuration block."
    ::= { arpCfg 4 }

ipCurCfgStaticArpEntry OBJECT-TYPE
    SYNTAX  IpCurCfgStaticArpEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the static ARP table"
    INDEX   { ipCurCfgStaticArpIndx }
    ::= { ipCurCfgStaticArpTable 1 }

IpCurCfgStaticArpEntry ::= SEQUENCE {
    ipCurCfgStaticArpIndx         Integer32,
    ipCurCfgStaticArpIp           IpAddress,
    ipCurCfgStaticArpMAC          DisplayString,
    ipCurCfgStaticArpVlan         INTEGER,
    ipCurCfgStaticArpPort         Integer32
    }

ipCurCfgStaticArpIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The index of the static ARP table."
    ::= { ipCurCfgStaticArpEntry 1}

ipCurCfgStaticArpIp OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IP address for the ARP entry."
    ::= { ipCurCfgStaticArpEntry 2}

ipCurCfgStaticArpMAC OBJECT-TYPE
    SYNTAX  DisplayString
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The MAC address for the ARP entry."
    ::= { ipCurCfgStaticArpEntry 3 }

ipCurCfgStaticArpVlan OBJECT-TYPE 
    SYNTAX  INTEGER(1..4095)
    MAX-ACCESS  read-only 
    STATUS  current
    DESCRIPTION 
        "The VLAN for the ARP entry."
    ::= { ipCurCfgStaticArpEntry 4}

ipCurCfgStaticArpPort OBJECT-TYPE 
    SYNTAX  Integer32
    MAX-ACCESS  read-only 
    STATUS  current 
    DESCRIPTION 
        "The port for the ARP entry."
    ::= { ipCurCfgStaticArpEntry 5}

ipNewCfgStaticArpTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF IpNewCfgStaticArpEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of static ARPs in the new configuration block."
    ::= { arpCfg 5 }

ipNewCfgStaticArpEntry OBJECT-TYPE
    SYNTAX  IpNewCfgStaticArpEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the static ARP table"
    INDEX   { ipNewCfgStaticArpIndx }
    ::= { ipNewCfgStaticArpTable 1 }

IpNewCfgStaticArpEntry ::= SEQUENCE {
    ipNewCfgStaticArpIndx         Integer32,
    ipNewCfgStaticArpIp           IpAddress,
    ipNewCfgStaticArpMAC          DisplayString,
    ipNewCfgStaticArpVlan         INTEGER,
    ipNewCfgStaticArpPort         Integer32,
    ipNewCfgStaticArpAction       INTEGER
    }

ipNewCfgStaticArpIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The index of the static ARP table."
    ::= { ipNewCfgStaticArpEntry 1}

ipNewCfgStaticArpIp OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The IP address for the ARP entry."
    ::= { ipNewCfgStaticArpEntry 2}

ipNewCfgStaticArpMAC OBJECT-TYPE
    SYNTAX  DisplayString
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The MAC address for the ARP entry."
    ::= { ipNewCfgStaticArpEntry 3 }

ipNewCfgStaticArpVlan OBJECT-TYPE 
    SYNTAX  INTEGER(1..4095)
    MAX-ACCESS  read-create 
    STATUS  current 
    DESCRIPTION 
        "The VLAN for the ARP entry."
    ::= { ipNewCfgStaticArpEntry 4}

ipNewCfgStaticArpPort OBJECT-TYPE 
    SYNTAX  Integer32
    MAX-ACCESS  read-create 
    STATUS  current 
    DESCRIPTION 
        "The port for the ARP entry."
    ::= { ipNewCfgStaticArpEntry 5}

ipNewCfgStaticArpAction OBJECT-TYPE
    SYNTAX  INTEGER {
        other(1),
        delete(2)
       }  
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "When set to the value of 2 (delete), the entire row is deleted. 
         When read, other is returned. Setting the value to anything other 
         than 2(delete) has no effect on the state of the row."
    ::= { ipNewCfgStaticArpEntry 6 }


--
-- IP Bootp Configration
--
ipCurCfgBootpAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IP address of BOOTP server."
    ::= { ipBootpCfg 1 }

ipNewCfgBootpAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The IP address of BOOTP server."
    ::= { ipBootpCfg 2 }

ipCurCfgBootpAddr2 OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IP address of second BOOTP server."
    ::= { ipBootpCfg 3 }

ipNewCfgBootpAddr2 OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The IP address of second BOOTP server."
    ::= { ipBootpCfg 4 }

ipCurCfgBootpState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(2),
        disabled(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The state of BOOTP relay."
    ::= { ipBootpCfg 5 }

ipNewCfgBootpState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(2),
        disabled(3)
        }
    MAX-ACCESS  read-write  
    STATUS  current
    DESCRIPTION
        "The state of BOOTP relay."
    ::= { ipBootpCfg 6 }



-- VRRP (Virtual Router Redundantcy Protocol) Group

vrrpGeneral       OBJECT IDENTIFIER ::= { vrrpCfg 1 }

vrrpCurCfgGenState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable VRRP operation globally."
    ::= { vrrpGeneral 1 }

vrrpNewCfgGenState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable VRRP operation globally."
    ::= { vrrpGeneral 2 }

vrrpCurCfgGenTckVirtRtrInc OBJECT-TYPE
    SYNTAX  INTEGER (0..254)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The increment of VRRP virtual router priority. The priority is 
         adjusted by tracking the state of other virtual routers."
    ::= { vrrpGeneral 3 }

vrrpNewCfgGenTckVirtRtrInc OBJECT-TYPE
    SYNTAX  INTEGER (0..254)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The increment of VRRP virtual router priority. The priority is 
         adjusted by tracking the state of other virtual routers."
    ::= { vrrpGeneral 4 }

vrrpCurCfgGenTckIpIntfInc OBJECT-TYPE
    SYNTAX  INTEGER (0..254)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The increment of VRRP virtual router priority. The priority is 
         adjusted by tracking the state of other router interfaces."
    ::= { vrrpGeneral 5 }

vrrpNewCfgGenTckIpIntfInc OBJECT-TYPE
    SYNTAX  INTEGER (0..254)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The increment of VRRP virtual router priority. The priority is 
         adjusted by tracking the state of other router interfaces."
    ::= { vrrpGeneral 6 }

vrrpCurCfgGenTckVlanPortInc OBJECT-TYPE
    SYNTAX  INTEGER (0..254)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The increment of VRRP virtual router priority. The priority is 
         adjusted by tracking the port state of ports that belongs to the 
         same virtual LAN as the virtual router."
    ::= { vrrpGeneral 7 }

vrrpNewCfgGenTckVlanPortInc OBJECT-TYPE
    SYNTAX  INTEGER (0..254)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The increment of VRRP virtual router priority. The priority is 
         adjusted by tracking the port state of ports that belongs to the 
         same virtual LAN as the virtual router."
    ::= { vrrpGeneral 8 }




vrrpVirtRtrTableMaxSize OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The maximum number of entries in VRRP virtual router table."
    ::= { vrrpCfg 2 }

vrrpCurCfgVirtRtrTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF VrrpCurCfgVirtRtrTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of VRRP virtual routers configuration in current_config."
    ::= { vrrpCfg 3 }
 
vrrpCurCfgVirtRtrTableEntry OBJECT-TYPE
    SYNTAX  VrrpCurCfgVirtRtrTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "Information about a VRRP virtual router."
    INDEX   { vrrpCurCfgVirtRtrIndx }
    ::= { vrrpCurCfgVirtRtrTable 1 }
 
VrrpCurCfgVirtRtrTableEntry ::= SEQUENCE {
    vrrpCurCfgVirtRtrIndx         Integer32,
    vrrpCurCfgVirtRtrID           INTEGER,
    vrrpCurCfgVirtRtrAddr         IpAddress,
    vrrpCurCfgVirtRtrIfIndex      Integer32,
    vrrpCurCfgVirtRtrInterval     INTEGER,
    vrrpCurCfgVirtRtrPriority     INTEGER,
    vrrpCurCfgVirtRtrPreempt      INTEGER,
    vrrpCurCfgVirtRtrState        INTEGER,
    vrrpCurCfgVirtRtrTckVirtRtr   INTEGER,
    vrrpCurCfgVirtRtrTckIpIntf    INTEGER,
    vrrpCurCfgVirtRtrTckVlanPort  INTEGER
    }

vrrpCurCfgVirtRtrIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The VRRP virtual router table index."
    ::= { vrrpCurCfgVirtRtrTableEntry 1 }

vrrpCurCfgVirtRtrID OBJECT-TYPE
    SYNTAX  INTEGER (1..255)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The VRRP virtual router identifier."
    ::= { vrrpCurCfgVirtRtrTableEntry 2 }

vrrpCurCfgVirtRtrAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The VRRP virtual router IP address."
    ::= { vrrpCurCfgVirtRtrTableEntry 3 }

vrrpCurCfgVirtRtrIfIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IfIndex that the VRRP virtual router is representing."
    ::= { vrrpCurCfgVirtRtrTableEntry 4 }

vrrpCurCfgVirtRtrInterval OBJECT-TYPE
    SYNTAX  INTEGER (1..255)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The time interval between VRRP advertisements in seconds."
    ::= { vrrpCurCfgVirtRtrTableEntry 5 }

vrrpCurCfgVirtRtrPriority OBJECT-TYPE
    SYNTAX  INTEGER (1..254)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The priority value to be used by the specified VRRP virtual routers."
    ::= { vrrpCurCfgVirtRtrTableEntry 6 }

vrrpCurCfgVirtRtrPreempt OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This is for controlling whether a higher priority Backup
          VRRP virtual router preempts a low priority Master.

          enabled(1)  - allow preemption
          disabled(2) - prohibit preemption"
    ::= { vrrpCurCfgVirtRtrTableEntry 7 }

vrrpCurCfgVirtRtrState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable the VRRP virtual router."
    ::= { vrrpCurCfgVirtRtrTableEntry 8 }


vrrpCurCfgVirtRtrTckVirtRtr OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable tracking other virtual routers for priority 
         adjustment. The priority increment is defined 
         in vrrpCurCfgGenTckVirtRtrInc."
    ::= { vrrpCurCfgVirtRtrTableEntry 10 }

vrrpCurCfgVirtRtrTckIpIntf OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable tracking other router interfaces for 
	 priority adjustment. The priority increment is defined 
	 in vrrpCurCfgGenTckIpIntfInc."
    ::= { vrrpCurCfgVirtRtrTableEntry 11 }

vrrpCurCfgVirtRtrTckVlanPort OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable tracking port state of VLAN ports 
	 for priority adjustment. The priority increment is 
	 defined in vrrpCurCfgGenTckVlanPortInc."
    ::= { vrrpCurCfgVirtRtrTableEntry 12 }


vrrpNewCfgVirtRtrTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF VrrpNewCfgVirtRtrTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of VRRP virtual routers configuration in current_config."
    ::= { vrrpCfg 4 }

vrrpNewCfgVirtRtrTableEntry OBJECT-TYPE
    SYNTAX  VrrpNewCfgVirtRtrTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "Information about a VRRP virtual router."
    INDEX   { vrrpNewCfgVirtRtrIndx }
    ::= { vrrpNewCfgVirtRtrTable 1 }

VrrpNewCfgVirtRtrTableEntry ::= SEQUENCE {
    vrrpNewCfgVirtRtrIndx         Integer32,
    vrrpNewCfgVirtRtrID           INTEGER,
    vrrpNewCfgVirtRtrAddr         IpAddress,
    vrrpNewCfgVirtRtrIfIndex      Integer32,
    vrrpNewCfgVirtRtrInterval     INTEGER,
    vrrpNewCfgVirtRtrPriority     INTEGER,
    vrrpNewCfgVirtRtrPreempt      INTEGER,
    vrrpNewCfgVirtRtrState        INTEGER,
    vrrpNewCfgVirtRtrDelete       INTEGER,
    vrrpNewCfgVirtRtrTckVirtRtr   INTEGER,
    vrrpNewCfgVirtRtrTckIpIntf    INTEGER,
    vrrpNewCfgVirtRtrTckVlanPort  INTEGER
    }

vrrpNewCfgVirtRtrIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The VRRP virtual router table index."
    ::= { vrrpNewCfgVirtRtrTableEntry 1 }

vrrpNewCfgVirtRtrID OBJECT-TYPE
    SYNTAX  INTEGER (1..255)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The VRRP virtual router identifier."
    ::= { vrrpNewCfgVirtRtrTableEntry 2 }

vrrpNewCfgVirtRtrAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The VRRP virtual router IP address."
    ::= { vrrpNewCfgVirtRtrTableEntry 3 }

vrrpNewCfgVirtRtrIfIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The IfIndex that the VRRP virtual router is representing."
   ::= { vrrpNewCfgVirtRtrTableEntry 4 }

vrrpNewCfgVirtRtrInterval OBJECT-TYPE
    SYNTAX  INTEGER (1..255)
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The time interval between VRRP advertisements in seconds."
    ::= { vrrpNewCfgVirtRtrTableEntry 5 }

vrrpNewCfgVirtRtrPriority OBJECT-TYPE
    SYNTAX  INTEGER (1..254)
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The priority value to be used by the specified VRRP virtual router."
    ::= { vrrpNewCfgVirtRtrTableEntry 6 }

vrrpNewCfgVirtRtrPreempt OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "This is for controlling whether a higher priority Backup
         VRRP virtual router preempts a low priority Master.

         enabled(1)  - allow preemption
         disabled(2) - prohibit preemption"
    ::= { vrrpNewCfgVirtRtrTableEntry 7 }

vrrpNewCfgVirtRtrState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Enable or disable the VRRP virtual router."
    ::= { vrrpNewCfgVirtRtrTableEntry 8 }

vrrpNewCfgVirtRtrDelete OBJECT-TYPE
    SYNTAX  INTEGER { 
	other(1),
        delete(2)
	}
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "When set to the value of 2 (delete), the entire row is deleted. 
         When read, other(1) is returned. Setting the value to anything 
         other than delete(2) has no effect on the state of the row."
    ::= { vrrpNewCfgVirtRtrTableEntry 9 }


vrrpNewCfgVirtRtrTckVirtRtr OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Enable or disable tracking other virtual routers for 
	 priority adjustment.  the priority increment is defined 
	 in vrrpNewCfgGenTckVirtRtrInc."
    ::= { vrrpNewCfgVirtRtrTableEntry 11 }

vrrpNewCfgVirtRtrTckIpIntf OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
     MAX-ACCESS  read-create
     STATUS  current
     DESCRIPTION
         "Enable or disable tracking other router interfaces for 
	  priority adjustment.  the priority increment is defined 
	  in vrrpNewCfgGenTckIpIntfInc."
    ::= { vrrpNewCfgVirtRtrTableEntry 12 }

vrrpNewCfgVirtRtrTckVlanPort OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Enable or disable tracking port state of VLAN ports 
	 for priority adjustment.  the priority increment is 
	 defined in vrrpNewCfgGenTckVlanPortInc."
    ::= { vrrpNewCfgVirtRtrTableEntry 13 }


-- VRRP Interface Table

vrrpIfTableMaxSize OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The maximum number of entries in VRRP interface table."
    ::= { vrrpCfg 5 }

vrrpCurCfgIfTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF VrrpCurCfgIfTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of VRRP interface configuration in current_config."
    ::= { vrrpCfg 6 }
 
vrrpCurCfgIfTableEntry OBJECT-TYPE
    SYNTAX  VrrpCurCfgIfTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "Information about a VRRP interface."
    INDEX   { vrrpCurCfgIfIndx }
    ::= { vrrpCurCfgIfTable 1 }
 
VrrpCurCfgIfTableEntry ::= SEQUENCE {
    vrrpCurCfgIfIndx         Integer32,
    vrrpCurCfgIfAuthType     INTEGER,
    vrrpCurCfgIfPasswd       DisplayString
    }

vrrpCurCfgIfIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The VRRP interface index.  This is eqivalent to IfIndex."
    ::= { vrrpCurCfgIfTableEntry 1 }

vrrpCurCfgIfAuthType OBJECT-TYPE
    SYNTAX  INTEGER {
        none(1),
        simple-text-password(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Type of authentication being used.
	 none(1) - no authentication
	 simple-text-password(2) - use password specified in 
         vrrpCurCfgIfPasswd for authentication."
    ::= { vrrpCurCfgIfTableEntry 2 }

vrrpCurCfgIfPasswd OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..8))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The password for authentication."
    ::= { vrrpCurCfgIfTableEntry 3 }

vrrpNewCfgIfTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF VrrpNewCfgIfTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of VRRP interface configuration in current_config."
    ::= { vrrpCfg 7 }
 
vrrpNewCfgIfTableEntry OBJECT-TYPE
    SYNTAX  VrrpNewCfgIfTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "Information about a VRRP interface."
    INDEX   { vrrpNewCfgIfIndx }
    ::= { vrrpNewCfgIfTable 1 }
 
VrrpNewCfgIfTableEntry ::= SEQUENCE {
    vrrpNewCfgIfIndx         Integer32,
    vrrpNewCfgIfAuthType     INTEGER,
    vrrpNewCfgIfPasswd       DisplayString,
    vrrpNewCfgIfDelete       INTEGER
    }

vrrpNewCfgIfIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The VRRP interface index.  This is eqivalent to IfIndex."
    ::= { vrrpNewCfgIfTableEntry 1 }

vrrpNewCfgIfAuthType OBJECT-TYPE
    SYNTAX  INTEGER {
        none(1),
        simple-text-password(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Type of authentication being used.
	 none(1) - no authentication
	 simple-text-password(2) - use password specified in 
         vrrpNewCfgIfPasswd for authentication."
    ::= { vrrpNewCfgIfTableEntry 2 }

vrrpNewCfgIfPasswd OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..8))
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The password for authentication."
    ::= { vrrpNewCfgIfTableEntry 3 }

vrrpNewCfgIfDelete OBJECT-TYPE
    SYNTAX  INTEGER {
        other(1),
        delete(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "When set to the value of 2 (delete), the entire row is deleted. 
         When read, other(1) is returned. Setting the value to anything 
         other than delete(2) has no effect on the state of the row."
    ::= { vrrpNewCfgIfTableEntry 4 }

-- Failover Virtual Router Groups
vrrpVirtRtrGrpTableMaxSize OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The maximum number of entries in VRRP Group table."
    ::= { vrrpCfg 8 }

vrrpCurCfgVirtRtrGrpTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF VrrpCurCfgVirtRtrGrpTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of VRRP virtual router group in current_config."
    ::= { vrrpCfg 9 }

vrrpCurCfgVirtRtrGrpTableEntry OBJECT-TYPE
    SYNTAX  VrrpCurCfgVirtRtrGrpTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "Information about a VRRP failover virtual router."
    INDEX   { vrrpCurCfgVirtRtrGrpIndx }
    ::= { vrrpCurCfgVirtRtrGrpTable 1 }

VrrpCurCfgVirtRtrGrpTableEntry ::= SEQUENCE {
    vrrpCurCfgVirtRtrGrpIndx         Integer32,
    vrrpCurCfgVirtRtrGrpID           INTEGER,
    vrrpCurCfgVirtRtrGrpIfIndex      Integer32,
    vrrpCurCfgVirtRtrGrpInterval     INTEGER,
    vrrpCurCfgVirtRtrGrpPriority     INTEGER,
    vrrpCurCfgVirtRtrGrpPreempt      INTEGER,
    vrrpCurCfgVirtRtrGrpState        INTEGER,
    vrrpCurCfgVirtRtrGrpTckIpIntf    INTEGER,
    vrrpCurCfgVirtRtrGrpTckVlanPort  INTEGER
    }
 
vrrpCurCfgVirtRtrGrpIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The VRRP virtual router table index."
    ::= { vrrpCurCfgVirtRtrGrpTableEntry 1 }
 
vrrpCurCfgVirtRtrGrpID OBJECT-TYPE
    SYNTAX  INTEGER (1..255)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The VRRP virtual router identifier."
    ::= { vrrpCurCfgVirtRtrGrpTableEntry 2 }
 
vrrpCurCfgVirtRtrGrpIfIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IfIndex that the VRRP virtual router is representing."
    ::= { vrrpCurCfgVirtRtrGrpTableEntry 3 }

vrrpCurCfgVirtRtrGrpInterval OBJECT-TYPE
    SYNTAX  INTEGER (1..255)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The time interval between VRRP advertisements in seconds."
    ::= { vrrpCurCfgVirtRtrGrpTableEntry 4 }

vrrpCurCfgVirtRtrGrpPriority OBJECT-TYPE
    SYNTAX  INTEGER (1..254)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The priority value to be used by the specified VRRP virtual routers."
    ::= { vrrpCurCfgVirtRtrGrpTableEntry 5 }

vrrpCurCfgVirtRtrGrpPreempt OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This is for controlling whether a higher priority Backup
         VRRP virtual router preempts a low priority Master.

         enabled(1)  - allow preemption
         disabled(2) - prohibit preemption"
   ::= { vrrpCurCfgVirtRtrGrpTableEntry 6 }

vrrpCurCfgVirtRtrGrpState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable the VRRP virtual router."
    ::= { vrrpCurCfgVirtRtrGrpTableEntry 7 }


vrrpCurCfgVirtRtrGrpTckIpIntf OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable tracking other router interfaces for
         priority adjustment.  the priority increment is defined
         in vrrpCurCfgGenTckIpIntfInc."
    ::= { vrrpCurCfgVirtRtrGrpTableEntry 10 }

vrrpCurCfgVirtRtrGrpTckVlanPort OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable tracking port state of VLAN ports
         for priority adjustment.  the priority increment is
         defined in vrrpCurCfgGenTckVlanPortInc."
    ::= { vrrpCurCfgVirtRtrGrpTableEntry 11 }


vrrpNewCfgVirtRtrGrpTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF VrrpNewCfgVirtRtrGrpTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of VRRP virtual router group configuration in new_config."
    ::= { vrrpCfg 10 }

vrrpNewCfgVirtRtrGrpTableEntry OBJECT-TYPE
    SYNTAX  VrrpNewCfgVirtRtrGrpTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "Information about a VRRP failover virtual router."
    INDEX   { vrrpNewCfgVirtRtrGrpIndx }
    ::= { vrrpNewCfgVirtRtrGrpTable 1 }
 
VrrpNewCfgVirtRtrGrpTableEntry ::= SEQUENCE {
    vrrpNewCfgVirtRtrGrpIndx         Integer32,
    vrrpNewCfgVirtRtrGrpID           INTEGER,
    vrrpNewCfgVirtRtrGrpIfIndex      Integer32,
    vrrpNewCfgVirtRtrGrpInterval     INTEGER,
    vrrpNewCfgVirtRtrGrpPriority     INTEGER,
    vrrpNewCfgVirtRtrGrpPreempt      INTEGER,
    vrrpNewCfgVirtRtrGrpState        INTEGER,
    vrrpNewCfgVirtRtrGrpDelete       INTEGER,
    vrrpNewCfgVirtRtrGrpTckIpIntf    INTEGER,
    vrrpNewCfgVirtRtrGrpTckVlanPort  INTEGER
    }
 
vrrpNewCfgVirtRtrGrpIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The VRRP virtual router table index."
    ::= { vrrpNewCfgVirtRtrGrpTableEntry 1 }
 
vrrpNewCfgVirtRtrGrpID OBJECT-TYPE
    SYNTAX  INTEGER (1..255)
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The VRRP virtual router identifier."
    ::= { vrrpNewCfgVirtRtrGrpTableEntry 2 }
 
vrrpNewCfgVirtRtrGrpIfIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The IfIndex that the VRRP virtual router is representing."
    ::= { vrrpNewCfgVirtRtrGrpTableEntry 3 }

vrrpNewCfgVirtRtrGrpInterval OBJECT-TYPE
    SYNTAX  INTEGER (1..255)
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The time interval between VRRP advertisements in seconds."
    ::= { vrrpNewCfgVirtRtrGrpTableEntry 4 }

vrrpNewCfgVirtRtrGrpPriority OBJECT-TYPE
    SYNTAX  INTEGER (1..254)
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The priority value to be used by the specified VRRP virtual router."
    ::= { vrrpNewCfgVirtRtrGrpTableEntry 5 }

vrrpNewCfgVirtRtrGrpPreempt OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "This is for controlling whether a higher priority Backup
         VRRP virtual router preempts a low priority Master.

         enabled(1)  - allow preemption
         disabled(2) - prohibit preemption"
    ::= { vrrpNewCfgVirtRtrGrpTableEntry 6 }

vrrpNewCfgVirtRtrGrpState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Enable or disable the VRRP virtual router."
    ::= { vrrpNewCfgVirtRtrGrpTableEntry 7 }

vrrpNewCfgVirtRtrGrpDelete OBJECT-TYPE
    SYNTAX  INTEGER {
        other(1),
        delete(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "When set to the value of 2 (delete), the entire row is deleted. 
         When read, other(1) is returned. Setting the value to anything 
         other than delete(2) has no effect on the state of the row."
    ::= { vrrpNewCfgVirtRtrGrpTableEntry 8 }


vrrpNewCfgVirtRtrGrpTckIpIntf OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Enable or disable tracking other router interfaces for
         priority adjustment.  the priority increment is defined
         in vrrpNewCfgGenTckIpIntfInc."
    ::= { vrrpNewCfgVirtRtrGrpTableEntry 11 }

vrrpNewCfgVirtRtrGrpTckVlanPort OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Enable or disable tracking port state of VLAN ports
         for priority adjustment.  the priority increment is
         defined in vrrpNewCfgGenTckVlanPortInc."
    ::= { vrrpNewCfgVirtRtrGrpTableEntry 12 }


-- Domain Name Server Configuration

dnsCurCfgPrimaryIpAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The DNS primary IP address in the current_configuration block."
    ::= { dnsCfg 1 }

dnsNewCfgPrimaryIpAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The DNS primary IP address in the new_configuration block."
    ::= { dnsCfg 2 }

dnsCurCfgSecondaryIpAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The DNS primary IP address in the current_configuration block."
    ::= { dnsCfg 3 }

dnsNewCfgSecondaryIpAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The DNS primary IP address in the new_configuration block."
    ::= { dnsCfg 4 }

dnsCurCfgDomainName OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..191))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The DNS doamin name in the current_configuration block."
    ::= { dnsCfg 5 }

dnsNewCfgDomainName OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..191))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The DNS doamin name in the new_configuration block."
    ::= { dnsCfg 6 }

--
-- IP network filter configuration
--
ipNwfTableMax OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The maximum number of rows in the IP network filter table."
    ::= { ipNwfCfg 1 }

ipCurCfgNwfTable OBJECT-TYPE
    SYNTAX SEQUENCE OF IpCurCfgNwfEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of IP network filter configuration in the current_config."
    ::= { ipNwfCfg 2 }

ipCurCfgNwfEntry OBJECT-TYPE
    SYNTAX IpCurCfgNwfEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about an IP network filter."
    INDEX { ipCurCfgNwfIndex }
    ::= { ipCurCfgNwfTable 1 }
 
IpCurCfgNwfEntry ::= SEQUENCE {
    ipCurCfgNwfIndex     Integer32,
    ipCurCfgNwfAddr      IpAddress,
    ipCurCfgNwfMask      IpAddress,
    ipCurCfgNwfState     INTEGER
    }
 
ipCurCfgNwfIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The netowrk filter number for which the NWF is related."
    ::= { ipCurCfgNwfEntry 1}

ipCurCfgNwfAddr OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The IP address of the network filter."
    ::= { ipCurCfgNwfEntry 2 }

ipCurCfgNwfMask OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current  
    DESCRIPTION
	"The subnet mask of the network filter."
    ::= { ipCurCfgNwfEntry 3 }

ipCurCfgNwfState OBJECT-TYPE
    SYNTAX INTEGER { 
        enabled(1),
        disabled(2)
	}
    MAX-ACCESS  read-only
    STATUS  current  
    DESCRIPTION
	"Enable or disable the network filter."
    ::= { ipCurCfgNwfEntry 4 }

ipNewCfgNwfTable OBJECT-TYPE
    SYNTAX SEQUENCE OF IpNewCfgNwfEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of IP network filter configuration in the current_config."
    ::= { ipNwfCfg 3 }

ipNewCfgNwfEntry OBJECT-TYPE
    SYNTAX IpNewCfgNwfEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about an IP network filter."
    INDEX { ipNewCfgNwfIndex }
    ::= { ipNewCfgNwfTable 1 }
 
IpNewCfgNwfEntry ::= SEQUENCE {
    ipNewCfgNwfIndex     Integer32,
    ipNewCfgNwfAddr      IpAddress,
    ipNewCfgNwfMask      IpAddress,
    ipNewCfgNwfState     INTEGER,
    ipNewCfgNwfDelete    INTEGER
    }
 
ipNewCfgNwfIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The netowrk filter number for which the NWF is related."
    ::= { ipNewCfgNwfEntry 1}

ipNewCfgNwfAddr OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"The IP address of the network filter."
    ::= { ipNewCfgNwfEntry 2 }

ipNewCfgNwfMask OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-create
    STATUS current  
    DESCRIPTION
	"The subnet mask of the network filter."
    ::= { ipNewCfgNwfEntry 3 }

ipNewCfgNwfState OBJECT-TYPE
    SYNTAX INTEGER { 
        enabled(1),
        disabled(2)
	}
    MAX-ACCESS  read-create
    STATUS  current  
    DESCRIPTION
	"Enable or disable the network filter."
    ::= { ipNewCfgNwfEntry 4 }

ipNewCfgNwfDelete OBJECT-TYPE
    SYNTAX INTEGER { 
        other(1),
        delete(2)
        }
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"When set to the value of 2 (delete), the entire row is deleted. 
	 When read, other(1) is returned. Setting the value to anything 
	 other than 2(delete) has no effect on the state of the row."
    ::= { ipNewCfgNwfEntry 5 }

--
-- IP route map configuration
--
ipRmapTableMax OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The maximum number of rows in the IP route map table."
    ::= { ipRmapCfg 1 }

ipCurCfgRmapTable OBJECT-TYPE
    SYNTAX SEQUENCE OF IpCurCfgRmapEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of IP route map configuration in the current_config."
    ::= { ipRmapCfg 2 }

ipCurCfgRmapEntry OBJECT-TYPE
    SYNTAX IpCurCfgRmapEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about an IP route map."
    INDEX { ipCurCfgRmapIndex }
    ::= { ipCurCfgRmapTable 1 }
 
IpCurCfgRmapEntry ::= SEQUENCE {
    ipCurCfgRmapIndex		Integer32,
    ipCurCfgRmapMetric	  	Unsigned32,
    ipCurCfgRmapPrec	  	INTEGER,
    ipCurCfgRmapState     	INTEGER,
    ipCurCfgRmapMetricType	INTEGER,
    ipCurCfgRmapState           INTEGER
    }
 
ipCurCfgRmapIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The route map number for which the RMAP is related."
    ::= { ipCurCfgRmapEntry 1}


ipCurCfgRmapMetric OBJECT-TYPE
    SYNTAX Unsigned32 (0..4294967295) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The metric of the route map. 4294967295 means none"
    ::= { ipCurCfgRmapEntry 3 }

ipCurCfgRmapPrec OBJECT-TYPE
    SYNTAX INTEGER (1..255) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The precedence of the route map."
    ::= { ipCurCfgRmapEntry 4 }


ipCurCfgRmapState OBJECT-TYPE
    SYNTAX INTEGER { 
        enabled(1),
        disabled(2)
	}
    MAX-ACCESS  read-only
    STATUS  current  
    DESCRIPTION
	"Enable or disable the route map."
    ::= { ipCurCfgRmapEntry 6 }


ipCurCfgRmapMetricType OBJECT-TYPE
    SYNTAX INTEGER {
        none(1),
        type1(2),
        type2(3)
        }
    MAX-ACCESS  read-only
    STATUS  current  
    DESCRIPTION
	"The OSPF metric-type of the matched route."
    ::= { ipCurCfgRmapEntry 8 }

ipNewCfgRmapTable OBJECT-TYPE
    SYNTAX SEQUENCE OF IpNewCfgRmapEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of IP route map configuration in the current_config."
    ::= { ipRmapCfg 3 }

ipNewCfgRmapEntry OBJECT-TYPE
    SYNTAX IpNewCfgRmapEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about an IP route map."
    INDEX { ipNewCfgRmapIndex }
    ::= { ipNewCfgRmapTable 1 }
 
IpNewCfgRmapEntry ::= SEQUENCE {
    ipNewCfgRmapIndex		Integer32,
    ipNewCfgRmapMetric	  	Unsigned32,
    ipNewCfgRmapPrec	  	INTEGER,
    ipNewCfgRmapState     	INTEGER,
    ipNewCfgRmapMetricType	INTEGER,
    ipNewCfgRmapDelete		INTEGER
    }
 
ipNewCfgRmapIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The route map number for which the RMAP is related."
    ::= { ipNewCfgRmapEntry 1}


ipNewCfgRmapMetric OBJECT-TYPE
    SYNTAX Unsigned32 (0..16777215) 
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"The metric of the route map. 16777215 means none"
    ::= { ipNewCfgRmapEntry 3 }

ipNewCfgRmapPrec OBJECT-TYPE
    SYNTAX INTEGER (1..255) 
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"The precedence of the route map."
    ::= { ipNewCfgRmapEntry 4 }


ipNewCfgRmapState OBJECT-TYPE
    SYNTAX INTEGER { 
        enabled(1),
        disabled(2)
	}
    MAX-ACCESS  read-create
    STATUS  current  
    DESCRIPTION
	"Enable or disable the route map."
    ::= { ipNewCfgRmapEntry 6 }


ipNewCfgRmapMetricType OBJECT-TYPE
    SYNTAX INTEGER {
        none(1),
        type1(2),
        type2(3)
        }
    MAX-ACCESS  read-create
    STATUS  current  
    DESCRIPTION
	"The OSPF metric-type of the matched route."
    ::= { ipNewCfgRmapEntry 8 }

ipNewCfgRmapDelete OBJECT-TYPE
    SYNTAX  INTEGER {
	other(1),
	delete(2)
	}
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
	"When set to the value of 2 (delete), the entire row is deleted. 
	 When read, other(1) is returned. Setting the value to anything 
	 other than 2(delete) has no effect on the state of the row."
    ::= { ipNewCfgRmapEntry 9 }

ipAlistTableMax OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The maximum number of rows in the IP route map table."
    ::= { ipRmapCfg 4 }

ipCurCfgAlistTable OBJECT-TYPE
    SYNTAX SEQUENCE OF IpCurCfgAlistEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of IP route map access list configuration in the 
       current_config."
    ::= { ipRmapCfg 5 }

ipCurCfgAlistEntry OBJECT-TYPE
    SYNTAX IpCurCfgAlistEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about an IP route map."
    INDEX { ipCurCfgAlistRmapIndex, ipCurCfgAlistIndex }
    ::= { ipCurCfgAlistTable 1 }
 
IpCurCfgAlistEntry ::= SEQUENCE {
    ipCurCfgAlistRmapIndex	Integer32,
    ipCurCfgAlistIndex		Integer32,
    ipCurCfgAlistNwf		INTEGER,
    ipCurCfgAlistMetric	  	Unsigned32,
    ipCurCfgAlistAction		INTEGER,
    ipCurCfgAlistState     	INTEGER
    }
 
ipCurCfgAlistRmapIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The route map number for which the RMAP is related."
    ::= { ipCurCfgAlistEntry 1 }

ipCurCfgAlistIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The access list number for which the access list is related."
    ::= { ipCurCfgAlistEntry 2 }

ipCurCfgAlistNwf OBJECT-TYPE
    SYNTAX INTEGER (0..256) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The network filter number of the route map access list. 
	 0 means none"
    ::= { ipCurCfgAlistEntry 3 }

ipCurCfgAlistMetric OBJECT-TYPE
    SYNTAX Unsigned32 (0..4294967295) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The metric of the route map access list. 4294967295 means none"
    ::= { ipCurCfgAlistEntry 4 }

ipCurCfgAlistAction OBJECT-TYPE
    SYNTAX INTEGER {
	permit(1),
	deny(2)
	}
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Action of the route map access list."
    ::= { ipCurCfgAlistEntry 5 }

ipCurCfgAlistState OBJECT-TYPE
    SYNTAX INTEGER { 
        enabled(1),
        disabled(2)
	}
    MAX-ACCESS  read-only
    STATUS  current  
    DESCRIPTION
	"Enable or disable the route map access list."
    ::= { ipCurCfgAlistEntry 6 }

ipNewCfgAlistTable OBJECT-TYPE
    SYNTAX SEQUENCE OF IpNewCfgAlistEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of IP route map access list configuration in the 
       current_config."
    ::= { ipRmapCfg 6 }

ipNewCfgAlistEntry OBJECT-TYPE
    SYNTAX IpNewCfgAlistEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about an IP route map."
    INDEX { ipNewCfgAlistRmapIndex, ipNewCfgAlistIndex }
    ::= { ipNewCfgAlistTable 1 }
 
IpNewCfgAlistEntry ::= SEQUENCE {
    ipNewCfgAlistRmapIndex	Integer32,
    ipNewCfgAlistIndex		Integer32,
    ipNewCfgAlistNwf		INTEGER,
    ipNewCfgAlistMetric	  	Unsigned32,
    ipNewCfgAlistAction		INTEGER,
    ipNewCfgAlistState     	INTEGER,
    ipNewCfgAlistDelete		INTEGER
    }
 
ipNewCfgAlistRmapIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The route map number for which the RMAP is related."
    ::= { ipNewCfgAlistEntry 1 }

ipNewCfgAlistIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The access list number for which the access list is related."
    ::= { ipNewCfgAlistEntry 2 }

ipNewCfgAlistNwf OBJECT-TYPE
    SYNTAX INTEGER (1..256) 
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"The network filter number of the route map access list. 
	 0 means none"
    ::= { ipNewCfgAlistEntry 3 }

ipNewCfgAlistMetric OBJECT-TYPE
    SYNTAX Unsigned32 (1..16777215) 
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"The metric of the route map access list. 16777215 means none"
    ::= { ipNewCfgAlistEntry 4 }

ipNewCfgAlistAction OBJECT-TYPE
    SYNTAX INTEGER {
	permit(1),
	deny(2)
	}
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"Action of the route map access list."
    ::= { ipNewCfgAlistEntry 5 }

ipNewCfgAlistState OBJECT-TYPE
    SYNTAX INTEGER { 
        enabled(1),
        disabled(2)
	}
    MAX-ACCESS  read-create
    STATUS  current  
    DESCRIPTION
	"Enable or disable the route map access list."
    ::= { ipNewCfgAlistEntry 6 }

ipNewCfgAlistDelete OBJECT-TYPE
    SYNTAX  INTEGER {
	other(1),
	delete(2)
	}
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
	"When set to the value of 2 (delete), the entire row is deleted. 
	 When read, other(1) is returned. Setting the value to anything 
	 other than 2(delete) has no effect on the state of the row."
    ::= { ipNewCfgAlistEntry 7 }



--
-- IP OSPF configuration
--
ospfGeneral	OBJECT IDENTIFIER ::= { ospfCfg 1 }

ospfCurCfgDefaultRouteMetric OBJECT-TYPE
    SYNTAX INTEGER (0..16777215)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Specify the metric to be assigned."
    ::= { ospfGeneral 1 }

ospfNewCfgDefaultRouteMetric OBJECT-TYPE
    SYNTAX INTEGER (0..16777214)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"Specify the metric to be assigned."
    ::= { ospfGeneral 2 }

ospfCurCfgDefaultRouteMetricType OBJECT-TYPE
    SYNTAX INTEGER {
        none(1),
        type1(2),
        type2(3)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Specify the AS External metric type to be assigned."
    ::= { ospfGeneral 3 }

ospfNewCfgDefaultRouteMetricType OBJECT-TYPE
    SYNTAX INTEGER {
        none(1),
        type1(2),
        type2(3)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"Specify the AS External metric type to be assigned."
    ::= { ospfGeneral 4 }

ospfIntfTableMaxSize OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The maximum number of rows in the OSPF Interface table."
    ::= { ospfGeneral 5 }

ospfAreaTableMaxSize OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The maximum number of rows in the OSPF Area table."
    ::= { ospfGeneral 6 }

ospfRangeTableMaxSize OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The maximum number of rows in the OSPF Range table."
    ::= { ospfGeneral 7 }

ospfVirtIntfTableMaxSize OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The maximum number of rows in the OSPF Virtual Interface
         table."
    ::= { ospfGeneral 8 }

ospfHostTableMaxSize OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The maximum number of rows in the OSPF Host table."
    ::= { ospfGeneral 9 }

ospfCurCfgState OBJECT-TYPE
    SYNTAX INTEGER {
        on(1),
        off(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"OSPF global state."
    ::= { ospfGeneral 10 }

ospfNewCfgState OBJECT-TYPE
    SYNTAX INTEGER {
        on(1),
        off(2)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"Globally turn OSPF on or off."
    ::= { ospfGeneral 11 }

ospfCurCfgLSDB OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The LSDB limit for external LSA."
    ::= { ospfGeneral 12 }

ospfNewCfgLSDB OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"Set the LSDB limit for external LSA."
    ::= { ospfGeneral 13 }

ospfCurCfgAreaTable OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfCurCfgAreaEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Area configuration in the current_config."
    ::= { ospfCfg 2 }

ospfCurCfgAreaEntry OBJECT-TYPE
    SYNTAX OspfCurCfgAreaEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about a OSPF area."
    INDEX { ospfCurCfgAreaIndex }
    ::= { ospfCurCfgAreaTable 1 }
 
OspfCurCfgAreaEntry ::= SEQUENCE {
    ospfCurCfgAreaIndex         Integer32,
    ospfCurCfgAreaId            IpAddress,
    ospfCurCfgAreaSpfInterval   INTEGER,
    ospfCurCfgAreaAuthType      INTEGER,
    ospfCurCfgAreaType 	        INTEGER,
    ospfCurCfgAreaMetric	INTEGER,
    ospfCurCfgAreaStatus        INTEGER
    }
 
ospfCurCfgAreaIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The OSPF area number for which the OSPF area table is related."
    ::= { ospfCurCfgAreaEntry 1}

ospfCurCfgAreaId OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The IP Address of the OSPF area." 
    ::= { ospfCurCfgAreaEntry 2 }

ospfCurCfgAreaSpfInterval OBJECT-TYPE
    SYNTAX INTEGER (1..255) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The SPF interval for the OSPF area." 
    ::= { ospfCurCfgAreaEntry 3 }

ospfCurCfgAreaAuthType OBJECT-TYPE
    SYNTAX  INTEGER {
        none(1),
        password(2),
	md5(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Type of authentication being used.
	 none(1) - no authentication
	 password(2) - use password
	 md5(3) - use MD5 authentication."
	
    ::= { ospfCurCfgAreaEntry 4 }

ospfCurCfgAreaType OBJECT-TYPE
	SYNTAX INTEGER {
	    transit(0),
	    stub(1),
	    nssa(2)
           }
	MAX-ACCESS   read-only
	STATUS  current
	DESCRIPTION
	    "Type of Area.
	    transit(0)
	    stub(1)
	    nssa(2)"
		   
	::= { ospfCurCfgAreaEntry 5 }
	
ospfCurCfgAreaMetric OBJECT-TYPE
    SYNTAX  INTEGER (1..65535)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Metric (1-65535)"
	
    ::= { ospfCurCfgAreaEntry 6 }

ospfCurCfgAreaStatus OBJECT-TYPE
    SYNTAX  INTEGER {
        disabled(0), 
	 enabled(1)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Status
	   disabled(0)
	   enabled(1)"
	
    ::= { ospfCurCfgAreaEntry 7 } 


ospfNewCfgAreaTable OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfNewCfgAreaEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Area configuration in the new_config."
    ::= { ospfCfg 3 }

ospfNewCfgAreaEntry OBJECT-TYPE
    SYNTAX OspfNewCfgAreaEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about a OSPF area."
    INDEX { ospfNewCfgAreaIndex }
    ::= { ospfNewCfgAreaTable 1 }
 
OspfNewCfgAreaEntry ::= SEQUENCE {
    ospfNewCfgAreaIndex         Integer32,
    ospfNewCfgAreaId            IpAddress, 
    ospfNewCfgAreaSpfInterval   INTEGER,
    ospfNewCfgAreaAuthType      INTEGER,	
    ospfNewCfgAreaType 	        INTEGER,
    ospfNewCfgAreaMetric	INTEGER,
    ospfNewCfgAreaStatus        INTEGER,
    ospfNewCfgAreaDelete        INTEGER	
    }
 
ospfNewCfgAreaIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The OSPF area number for which the OSPF area table is related."
    ::= { ospfNewCfgAreaEntry 1}

ospfNewCfgAreaId OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"The IP Address of the OSPF area." 
    ::= { ospfNewCfgAreaEntry 2 }

ospfNewCfgAreaSpfInterval OBJECT-TYPE
    SYNTAX INTEGER (1..255) 
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"The SPF interval for the OSPF area." 
    ::= { ospfNewCfgAreaEntry 3 }

ospfNewCfgAreaAuthType OBJECT-TYPE
    SYNTAX  INTEGER {
        none(1),
        password(2),
	md5(3)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Type of authentication being used.
	 none(1) - no authentication
	 password(2) - use password.
         md5(3) - use MD5 authentication."
    ::= { ospfNewCfgAreaEntry 4 }

ospfNewCfgAreaType OBJECT-TYPE
	SYNTAX INTEGER {
	    transit(0),
	    stub(1),
	    nssa(2)
           }
	MAX-ACCESS   read-write
	STATUS  current
	DESCRIPTION
	    "Type of Area.
	    transit(0)
	    stub(1)
           nssa(2)"
		   
	::= { ospfNewCfgAreaEntry 5 }
	
ospfNewCfgAreaMetric OBJECT-TYPE
    SYNTAX  INTEGER (1..65535)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Metric (1-65535)"
	
    ::= { ospfNewCfgAreaEntry 6 }

ospfNewCfgAreaStatus OBJECT-TYPE
    SYNTAX  INTEGER {
        disabled(0), 
	 enabled(1)
        }
    MAX-ACCESS  read-write
    STATUS current
    DESCRIPTION
        "Status
	   disabled(0)
	   enabled(1)"
	
    ::= { ospfNewCfgAreaEntry 7 }

ospfNewCfgAreaDelete OBJECT-TYPE
   SYNTAX INTEGER {
	no(0),
	yes(1)
	}
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
	"Delete the area
	    no(0),
            yes(1)"

    ::= { ospfNewCfgAreaEntry 8 }
		


-- OSPF Host Table

ospfCurCfgHostTable OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfCurCfgHostEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Host configuration."
    ::= { ospfCfg 12 }

ospfCurCfgHostEntry OBJECT-TYPE
    SYNTAX OspfCurCfgHostEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about a OSPF host."
    INDEX { ospfCurCfgHostIndex }
    ::= { ospfCurCfgHostTable 1 }
 
OspfCurCfgHostEntry ::= SEQUENCE {
    ospfCurCfgHostIndex         Integer32,
    ospfCurCfgHostIpAddr        IpAddress,
    ospfCurCfgHostAreaIndex     Integer32,
    ospfCurCfgHostCost          INTEGER,
    ospfCurCfgHostState		INTEGER
    }
 
ospfCurCfgHostIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The OSPF host number for which the OSPF host table is related."
    ::= { ospfCurCfgHostEntry 1}

ospfCurCfgHostIpAddr OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The IP Address of the OSPF host." 
    ::= { ospfCurCfgHostEntry 2 }

ospfCurCfgHostAreaIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The area index."
    ::= { ospfCurCfgHostEntry 3 }

ospfCurCfgHostCost OBJECT-TYPE
    SYNTAX  INTEGER (1..65535)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The cost of the OSPF host."
    ::= { ospfCurCfgHostEntry 4 }

ospfCurCfgHostState OBJECT-TYPE
    SYNTAX  INTEGER  {
	enabled(2),
	disabled(3)
	}
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable an OSPF Host"
    ::= { ospfCurCfgHostEntry 5 }

ospfNewCfgHostTable OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfNewCfgHostEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Host configuration."
    ::= { ospfCfg 13 }

ospfNewCfgHostEntry OBJECT-TYPE
    SYNTAX OspfNewCfgHostEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about a OSPF host."
    INDEX { ospfNewCfgHostIndex }
    ::= { ospfNewCfgHostTable 1 }
 
OspfNewCfgHostEntry ::= SEQUENCE {
    ospfNewCfgHostIndex         Integer32,
    ospfNewCfgHostIpAddr        IpAddress, 
    ospfNewCfgHostAreaIndex     Integer32,
    ospfNewCfgHostCost          INTEGER,
    ospfNewCfgHostState		INTEGER,
    ospfNewCfgHostDelete        INTEGER
    }
 
ospfNewCfgHostIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only 
    STATUS current
    DESCRIPTION
	"The OSPF host number for which the OSPF host table is related."
    ::= { ospfNewCfgHostEntry 1}

ospfNewCfgHostIpAddr OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"The IP Address of the OSPF host." 
    ::= { ospfNewCfgHostEntry 2 }

ospfNewCfgHostAreaIndex OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"The OSPF area index."
    ::= { ospfNewCfgHostEntry 3 }

ospfNewCfgHostCost OBJECT-TYPE
    SYNTAX  INTEGER (1..65535)
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The cost of the OSPF host."
    ::= { ospfNewCfgHostEntry 4 }

ospfNewCfgHostState OBJECT-TYPE
    SYNTAX  INTEGER  {
	enabled(2),
	disabled(3)
	}
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Enable or disable an OSPF Host"
    ::= { ospfNewCfgHostEntry 5 }

ospfNewCfgHostDelete  OBJECT-TYPE
    SYNTAX  INTEGER {
        no(0),
        yes(1)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"Delete the OSPF host:
         no(0),
         yes(1)" 
    ::= { ospfNewCfgHostEntry 6 }

ospfMdkeyTableMaxSize OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum number of rows in the OSPF Mdkey table."
    ::= { ospfCfg 11 }

ospfCurCfgMdkeyTable OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfCurCfgMdkeyEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF MD5 keys in the current_config."
    ::= { ospfCfg 5 }

ospfCurCfgMdkeyEntry OBJECT-TYPE
    SYNTAX OspfCurCfgMdkeyEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about an OSPF MD keys table."
    INDEX { ospfCurCfgMdkeyIndex }
    ::= { ospfCurCfgMdkeyTable 1 }
 
OspfCurCfgMdkeyEntry ::= SEQUENCE {
    ospfCurCfgMdkeyIndex        Integer32,
    ospfCurCfgMdkeyKey          DisplayString
    }
 
ospfCurCfgMdkeyIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only 
    STATUS current
    DESCRIPTION
	"The OSPF MD5 Key number for which the OSPF MdKey table is related."
    ::= { ospfCurCfgMdkeyEntry 1}

ospfCurCfgMdkeyKey OBJECT-TYPE
    SYNTAX DisplayString (SIZE(0..16)) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The character string representing the MD5 Key." 
    ::= { ospfCurCfgMdkeyEntry 2 }

ospfNewCfgMdkeyTable OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfNewCfgMdkeyEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF MD5 keys in the new_config."
    ::= { ospfCfg 6 }

ospfNewCfgMdkeyEntry OBJECT-TYPE
    SYNTAX OspfNewCfgMdkeyEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about an OSPF MD keys table."
    INDEX { ospfNewCfgMdkeyIndex }
    ::= { ospfNewCfgMdkeyTable 1 }
 
OspfNewCfgMdkeyEntry ::= SEQUENCE {
    ospfNewCfgMdkeyIndex        Integer32,
    ospfNewCfgMdkeyKey          DisplayString,
    ospfNewCfgMdkeyDelete       INTEGER 
    }
 
ospfNewCfgMdkeyIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only 
    STATUS current
    DESCRIPTION
	"The OSPF MD5 Key number for which the OSPF MdKey table is related."
    ::= { ospfNewCfgMdkeyEntry 1}

ospfNewCfgMdkeyKey OBJECT-TYPE
    SYNTAX DisplayString (SIZE(0..16)) 
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"The character string representing the MD5 Key." 
    ::= { ospfNewCfgMdkeyEntry 2 }

ospfNewCfgMdkeyDelete OBJECT-TYPE
    SYNTAX  INTEGER { 
	other(1),
        delete(2)
	}
    MAX-ACCESS read-create 
    STATUS current
    DESCRIPTION
	"When set to the value of 2 (delete), the entire row is deleted. 
	 When read, other(1) is returned. Setting the value to anything 
	 other than 2(delete) has no effect on the state of the row."
    ::= { ospfNewCfgMdkeyEntry 3}

ospfCurCfgIntfTable OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfCurCfgIntfEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Interface configuration in the current_config."
    ::= { ospfCfg 7 }

ospfCurCfgIntfEntry OBJECT-TYPE
    SYNTAX OspfCurCfgIntfEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about an OSPF Interface."
    INDEX { ospfCurCfgIntfIndex }
    ::= { ospfCurCfgIntfTable 1 }
 
OspfCurCfgIntfEntry ::= SEQUENCE {
    ospfCurCfgIntfIndex         Integer32,
    ospfCurCfgIntfId            IpAddress,
    ospfCurCfgIntfArea          INTEGER,
    ospfCurCfgIntfMdkey         INTEGER, 
    ospfCurCfgIntfCost          INTEGER,
    ospfCurCfgIntfPrio          INTEGER,
    ospfCurCfgIntfHello         INTEGER,
    ospfCurCfgIntfDead          INTEGER,
    ospfCurCfgIntfTrans         INTEGER,
    ospfCurCfgIntfRetra         INTEGER,
    ospfCurCfgIntfAuthKey       DisplayString,
    ospfCurCfgIntfStatus        INTEGER

}
 
ospfCurCfgIntfIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The OSPF Interface number for which the OSPF Interface table is related."
    ::= { ospfCurCfgIntfEntry 1}

ospfCurCfgIntfId OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The IP Address of the OSPF interface." 
    ::= { ospfCurCfgIntfEntry 2 }


ospfCurCfgIntfArea OBJECT-TYPE
    SYNTAX INTEGER (0..2) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The index of the area that the interface belongs" 
    ::= { ospfCurCfgIntfEntry 3 }


ospfCurCfgIntfMdkey OBJECT-TYPE
    SYNTAX INTEGER (0..255) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The MD5 key for the OSPF interface
         0 (none) no MD5 authentication." 
    ::= { ospfCurCfgIntfEntry 4 }


ospfCurCfgIntfCost  OBJECT-TYPE 
    SYNTAX INTEGER (1..65535) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Interface cost" 
    ::= { ospfCurCfgIntfEntry 5 }

ospfCurCfgIntfPrio   OBJECT-TYPE
   SYNTAX INTEGER (1..255) 
    MAX-ACCESS read-only
    STATUS current 
    DESCRIPTION
	"Interface router priority" 
    ::= { ospfCurCfgIntfEntry 6 }

ospfCurCfgIntfHello  OBJECT-TYPE 
    SYNTAX INTEGER (1..65535) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Hello interval" 
    ::= { ospfCurCfgIntfEntry 7 }

ospfCurCfgIntfDead   OBJECT-TYPE
   SYNTAX INTEGER (1..65535) 
    MAX-ACCESS read-only
    STATUS current 
    DESCRIPTION
	"Dead interval" 
    ::= { ospfCurCfgIntfEntry 8 }

ospfCurCfgIntfTrans  OBJECT-TYPE
   SYNTAX INTEGER (1..3600) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Transit delay" 
    ::= { ospfCurCfgIntfEntry 9 }
	

ospfCurCfgIntfRetra OBJECT-TYPE
    SYNTAX INTEGER (1..3600) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Retransmit interval" 
    ::= { ospfCurCfgIntfEntry 10 }

ospfCurCfgIntfAuthKey OBJECT-TYPE  
   SYNTAX DisplayString (SIZE(0..8))
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Authentication Key" 
    ::= { ospfCurCfgIntfEntry 11 }
 
    
ospfCurCfgIntfStatus  OBJECT-TYPE
    SYNTAX  INTEGER {
        disabled(0),
        enabled(1)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Status of the interface
	disabled(0),
        enabled(1)" 
    ::= { ospfCurCfgIntfEntry 12 }

ospfNewCfgIntfTable OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfNewCfgIntfEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Interface configuration in the new_config."
    ::= { ospfCfg 8 }

ospfNewCfgIntfEntry OBJECT-TYPE
    SYNTAX OspfNewCfgIntfEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about an OSPF Interface."
    INDEX { ospfNewCfgIntfIndex }
    ::= { ospfNewCfgIntfTable 1 }
 
OspfNewCfgIntfEntry ::= SEQUENCE {
    ospfNewCfgIntfIndex         Integer32,
    ospfNewCfgIntfId            IpAddress,
    ospfNewCfgIntfArea          INTEGER,
    ospfNewCfgIntfMdkey         INTEGER,
    ospfNewCfgIntfCost		INTEGER,
    ospfNewCfgIntfPrio		INTEGER,
    ospfNewCfgIntfHello         INTEGER,
    ospfNewCfgIntfDead          INTEGER,
    ospfNewCfgIntfTrans         INTEGER,
    ospfNewCfgIntfRetra         INTEGER,
    ospfNewCfgIntfAuthKey       DisplayString,
    ospfNewCfgIntfStatus        INTEGER, 
    ospfNewCfgIntfDelete        INTEGER
    
}
 
ospfNewCfgIntfIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The OSPF Interface number for which the OSPF Interface table is related."
    ::= { ospfNewCfgIntfEntry 1}

ospfNewCfgIntfId OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The IP Address of the OSPF interface." 
    ::= { ospfNewCfgIntfEntry 2 }


ospfNewCfgIntfArea OBJECT-TYPE
    SYNTAX INTEGER (0..2) 
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"The index of the area that the interface belongs (0..2)" 
    ::= { ospfNewCfgIntfEntry 3 }



ospfNewCfgIntfMdkey OBJECT-TYPE
    SYNTAX INTEGER (0..255) 
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"The MD5 key for the OSPF interface
         0 (none) no MD5 authentication." 
    ::= { ospfNewCfgIntfEntry 4 }

ospfNewCfgIntfCost  OBJECT-TYPE 
    SYNTAX INTEGER (1..65535) 
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"Interface cost(1..65535)" 
    ::= { ospfNewCfgIntfEntry 5 }

ospfNewCfgIntfPrio   OBJECT-TYPE
   SYNTAX INTEGER (0..255) 
    MAX-ACCESS read-create
    STATUS current 
    DESCRIPTION
	"Interface router priority(0..255)" 
    ::= { ospfNewCfgIntfEntry 6 }


ospfNewCfgIntfHello  OBJECT-TYPE 
    SYNTAX INTEGER (1..65535) 
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"Hello interval(1..65535)" 
    ::= { ospfNewCfgIntfEntry 7 }

ospfNewCfgIntfDead   OBJECT-TYPE
   SYNTAX INTEGER (1..65535) 
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"Dead interval(1..65535)" 
    ::= { ospfNewCfgIntfEntry 8 }

ospfNewCfgIntfTrans  OBJECT-TYPE
   SYNTAX INTEGER (1..3600) 
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"Transit delay(1..3600)" 
    ::= { ospfNewCfgIntfEntry 9 }
	

ospfNewCfgIntfRetra OBJECT-TYPE
  SYNTAX INTEGER (1..3600) 
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"Retransmit interval(1..3600)" 
    ::= { ospfNewCfgIntfEntry 10 }


ospfNewCfgIntfAuthKey OBJECT-TYPE  
   SYNTAX DisplayString (SIZE(0..8))
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"Authentication Key" 
    ::= { ospfNewCfgIntfEntry 11 }
 
    
ospfNewCfgIntfStatus  OBJECT-TYPE
    SYNTAX  INTEGER {
        disabled(0),
        enabled(1)
        }
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"Status of the interface
	disabled(0),
        enabled(1)" 
    ::= { ospfNewCfgIntfEntry 12 }

      
ospfNewCfgIntfDelete  OBJECT-TYPE
    SYNTAX  INTEGER {
        other(0),
        delete(1)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"Delete the interface
         other(0),
         delete(1)" 
    ::= { ospfNewCfgIntfEntry 13 }

ospfCurCfgVirtIntfTable OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfCurCfgVirtIntfEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Virtual Interface configuration in the current_config."
    ::= { ospfCfg 9 }

ospfCurCfgVirtIntfEntry OBJECT-TYPE
    SYNTAX OspfCurCfgVirtIntfEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about an OSPF virtual Interface."
    INDEX { ospfCurCfgVirtIntfIndex }
    ::= { ospfCurCfgVirtIntfTable 1 }
 
OspfCurCfgVirtIntfEntry ::= SEQUENCE {
    ospfCurCfgVirtIntfIndex         Integer32,
    ospfCurCfgVirtIntfAreaId        INTEGER,
    ospfCurCfgVirtIntfNbr           IpAddress,
    ospfCurCfgVirtIntfMdkey         INTEGER,
    ospfCurCfgVirtIntfHello         INTEGER,
    ospfCurCfgVirtIntfDead          INTEGER,
    ospfCurCfgVirtIntfTrans         INTEGER,
    ospfCurCfgVirtIntfRetra         INTEGER,
    ospfCurCfgVirtIntfAuthKey       DisplayString,
    ospfCurCfgVirtIntfStatus        INTEGER 
    }
 
ospfCurCfgVirtIntfIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The OSPF Virtual Interface number for which the OSPF 
         Virtual Interface table is related."
    ::= { ospfCurCfgVirtIntfEntry 1}

ospfCurCfgVirtIntfAreaId OBJECT-TYPE
    SYNTAX INTEGER (0..2) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The index of the OSPF area to which this virtual interface
         belongs." 
    ::= { ospfCurCfgVirtIntfEntry 2 }

ospfCurCfgVirtIntfNbr OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The IP Address of the OSPF neighbor for this virtual interface."
    ::= { ospfCurCfgVirtIntfEntry 3 }

ospfCurCfgVirtIntfMdkey OBJECT-TYPE
    SYNTAX INTEGER (0..255) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The MD5 key for the OSPF virtual interface
         0 (none) no MD5 authentication." 
    ::= { ospfCurCfgVirtIntfEntry 4 }



ospfCurCfgVirtIntfHello  OBJECT-TYPE 
    SYNTAX INTEGER (1..65535) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Hello interval" 
    ::= { ospfCurCfgVirtIntfEntry 5 }

ospfCurCfgVirtIntfDead   OBJECT-TYPE
   SYNTAX INTEGER (1..65535) 
    MAX-ACCESS read-only
    STATUS current 
    DESCRIPTION
	"Dead interval" 
    ::= { ospfCurCfgVirtIntfEntry 6 }

 

ospfCurCfgVirtIntfTrans  OBJECT-TYPE
   SYNTAX INTEGER (1..3600) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Transit delay" 
    ::= { ospfCurCfgVirtIntfEntry 7 }
	

ospfCurCfgVirtIntfRetra OBJECT-TYPE
    SYNTAX INTEGER (1..3600) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Retransmit interval" 
    ::= { ospfCurCfgVirtIntfEntry 8 }

ospfCurCfgVirtIntfAuthKey OBJECT-TYPE  
   SYNTAX DisplayString (SIZE(0..8))
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Authentication Key" 
    ::= { ospfCurCfgVirtIntfEntry 9 }
 
    
ospfCurCfgVirtIntfStatus  OBJECT-TYPE
    SYNTAX  INTEGER {
        disabled(0),
        enabled(1)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Status
	 disabled(0),
        enabled(1)" 
    ::= { ospfCurCfgVirtIntfEntry 10 }

      




ospfNewCfgVirtIntfTable OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfNewCfgVirtIntfEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Virtual Interface configuration in the new_config."
    ::= { ospfCfg 10 }

ospfNewCfgVirtIntfEntry OBJECT-TYPE
    SYNTAX OspfNewCfgVirtIntfEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about an OSPF virtual Interface."
    INDEX { ospfNewCfgVirtIntfIndex }
    ::= { ospfNewCfgVirtIntfTable 1 }
 
OspfNewCfgVirtIntfEntry ::= SEQUENCE {
    ospfNewCfgVirtIntfIndex         Integer32,
    ospfNewCfgVirtIntfAreaId        INTEGER,
    ospfNewCfgVirtIntfNbr           IpAddress,
    ospfNewCfgVirtIntfMdkey         INTEGER,
    ospfNewCfgVirtIntfHello         INTEGER,
    ospfNewCfgVirtIntfDead          INTEGER,
    ospfNewCfgVirtIntfTrans         INTEGER,
    ospfNewCfgVirtIntfRetra         INTEGER,
    ospfNewCfgVirtIntfAuthKey       DisplayString,
    ospfNewCfgVirtIntfStatus        INTEGER, 
    ospfNewCfgVirtIntfDelete        INTEGER	 
   }
 
ospfNewCfgVirtIntfIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The OSPF Virtual Interface number for which the OSPF 
         Virtual Interface table is related."
    ::= { ospfNewCfgVirtIntfEntry 1}

ospfNewCfgVirtIntfAreaId OBJECT-TYPE
    SYNTAX INTEGER (0..2)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"The index of the OSPF area to which this virtual interface
         belongs." 
    ::= { ospfNewCfgVirtIntfEntry 2 }

ospfNewCfgVirtIntfNbr OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"The IP Address of the OSPF neighbor for this virtual interface."
    ::= { ospfNewCfgVirtIntfEntry 3 }

ospfNewCfgVirtIntfMdkey OBJECT-TYPE
    SYNTAX INTEGER (0..255) 
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"The MD5 key for the OSPF virtual interface
         0 (none) no MD5 authentication." 
    ::= { ospfNewCfgVirtIntfEntry 4 }


ospfNewCfgVirtIntfHello  OBJECT-TYPE 
    SYNTAX INTEGER (1..65535) 
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"Hello interval(1..65535)" 
    ::= { ospfNewCfgVirtIntfEntry 5 }

ospfNewCfgVirtIntfDead   OBJECT-TYPE
   SYNTAX INTEGER (1..65535) 
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"Dead interval(1..65535)" 
    ::= { ospfNewCfgVirtIntfEntry 6 }

 

ospfNewCfgVirtIntfTrans  OBJECT-TYPE
   SYNTAX INTEGER (1..3600) 
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"Transit dela(1..3600)y" 
    ::= { ospfNewCfgVirtIntfEntry 7 }
	

ospfNewCfgVirtIntfRetra OBJECT-TYPE
  SYNTAX INTEGER (1..3600) 
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"Retransmit interval(1..3600)" 
    ::= { ospfNewCfgVirtIntfEntry 8 }


ospfNewCfgVirtIntfAuthKey OBJECT-TYPE  
   SYNTAX DisplayString (SIZE(0..8))
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"Authentication Key SIZE(0..8)" 
    ::= { ospfNewCfgVirtIntfEntry 9 }
 
    
ospfNewCfgVirtIntfStatus  OBJECT-TYPE
    SYNTAX  INTEGER {
        disabled(0),
        enabled(1)
        }
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
	"Status 
         disabled(0),
         enabled(1) " 
    ::= { ospfNewCfgVirtIntfEntry 10 }

      
ospfNewCfgVirtIntfDelete  OBJECT-TYPE
    SYNTAX  INTEGER {
        other(0),
        delete(1)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"Delete
	 other(0),
         delete(1)" 
    ::= { ospfNewCfgVirtIntfEntry 11 }





-- ospf range

ospfCurCfgRangeTable OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfCurCfgRangeEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF summary range in the current configuration."
    ::= { ospfCfg 14 }

ospfCurCfgRangeEntry OBJECT-TYPE
    SYNTAX OspfCurCfgRangeEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about an OSPF summary range."
    INDEX { ospfCurCfgRangeIndex }
    ::= { ospfCurCfgRangeTable 1 }

OspfCurCfgRangeEntry ::= SEQUENCE {
    ospfCurCfgRangeIndex            Integer32,
    ospfCurCfgRangeAddr             IpAddress,
    ospfCurCfgRangeMask             IpAddress,
    ospfCurCfgRangeAreaIndex        Integer32,
    ospfCurCfgRangeHideState        INTEGER,
    ospfCurCfgRangeState            INTEGER
    }

ospfCurCfgRangeIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The range number for which the OSPF summary range table is related."
    ::= { ospfCurCfgRangeEntry 1}

ospfCurCfgRangeAddr OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The IP Address of the range."
    ::= { ospfCurCfgRangeEntry 2 }

ospfCurCfgRangeMask OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The mask of the range."
    ::= { ospfCurCfgRangeEntry 3 }

ospfCurCfgRangeAreaIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The area index."
    ::= { ospfCurCfgRangeEntry 4 }

ospfCurCfgRangeHideState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The state of the hide range."
    ::= { ospfCurCfgRangeEntry 5 }

ospfCurCfgRangeState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The state of the range."
    ::= { ospfCurCfgRangeEntry 6 }

ospfNewCfgRangeTable OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfNewCfgRangeEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF summary range in the new configuration."
    ::= { ospfCfg 15 }

ospfNewCfgRangeEntry OBJECT-TYPE
    SYNTAX OspfNewCfgRangeEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about an OSPF summary range."
    INDEX { ospfNewCfgRangeIndex }
    ::= { ospfNewCfgRangeTable 1 }

OspfNewCfgRangeEntry ::= SEQUENCE {
    ospfNewCfgRangeIndex            Integer32,
    ospfNewCfgRangeAddr             IpAddress,
    ospfNewCfgRangeMask             IpAddress,
    ospfNewCfgRangeAreaIndex        Integer32,
    ospfNewCfgRangeHideState        INTEGER,
    ospfNewCfgRangeState            INTEGER,
    ospfNewCfgRangeDelete           INTEGER
    }

ospfNewCfgRangeIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The range number for which the OSPF summary range table is related."
    ::= { ospfNewCfgRangeEntry 1}

ospfNewCfgRangeAddr OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The IP Address of the range."
    ::= { ospfNewCfgRangeEntry 2 }

ospfNewCfgRangeMask OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The mask of the range."
    ::= { ospfNewCfgRangeEntry 3 }

ospfNewCfgRangeAreaIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The area index."
    ::= { ospfNewCfgRangeEntry 4 }

ospfNewCfgRangeHideState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-create
    STATUS  current
    DESCRIPTION
        "The state of the hide range."
    ::= { ospfNewCfgRangeEntry 5 }

ospfNewCfgRangeState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-create
    STATUS  current
    DESCRIPTION
        "The state of the range."
    ::= { ospfNewCfgRangeEntry 6 }

ospfNewCfgRangeDelete OBJECT-TYPE
    SYNTAX  INTEGER {
        other(1),
        delete(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "When set to the value of 2 (delete), the entire row is deleted.
         When read, other(1) is returned. Setting the value to anything
         other than 2(delete) has no effect on the state of the row."
    ::= { ospfNewCfgRangeEntry 7 }

ospfRouteRedistribution   OBJECT IDENTIFIER ::= { ospfCfg 4 }

ospfRedistributeStatic    OBJECT IDENTIFIER ::= { ospfRouteRedistribution 1 }

ospfCurCfgStaticMetric OBJECT-TYPE
    SYNTAX INTEGER (0..16777214)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The metric to be assigned to static routes. 
         A value of 0 indicates none."
    ::= { ospfRedistributeStatic 1 }

ospfNewCfgStaticMetric OBJECT-TYPE
    SYNTAX INTEGER (0..16777214)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"The metric to be assigned to static routes. 
         A value of 0 indicates none."
    ::= { ospfRedistributeStatic 2 }

ospfCurCfgStaticMetricType OBJECT-TYPE
    SYNTAX INTEGER {
        none(1),
        type1(2),
        type2(3)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The AS External metric type for static routes."
    ::= { ospfRedistributeStatic 3 }

ospfNewCfgStaticMetricType OBJECT-TYPE
    SYNTAX INTEGER {
        none(1),
        type1(2),
        type2(3)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"The AS External metric type for static routes."
    ::= { ospfRedistributeStatic 4 }

ospfCurCfgStaticOutRmapList OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The route maps present in the out route map list. 
         The route maps are presented in a bitmap format.

         in receiving order:

         OCTET 1  OCTET 2  .....
         xxxxxxxx xxxxxxxx .....
         ||    || |_ Rmap 9
         ||    ||
         ||    ||___ Rmap 8
         ||    |____ Rmap 7
         ||      .    .   .
         ||_________ Rmap 2
         |__________ Rmap 1

         where x : 1 - The represented route map is selected
         0 - The represented route map is not selected"
    ::= { ospfRedistributeStatic 5 }

ospfNewCfgStaticOutRmapList OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The route maps present in the out route map list. 
         The route maps are presented in a bitmap format.

         in receiving order:

         OCTET 1  OCTET 2  .....
         xxxxxxxx xxxxxxxx .....
         ||    || |_ Rmap 9
         ||    ||
         ||    ||___ Rmap 8
         ||    |____ Rmap 7
         ||      .    .   .
         ||_________ Rmap 2
         |__________ Rmap 1

         where x : 1 - The represented route map is selected
         0 - The represented route map is not selected"
    ::= { ospfRedistributeStatic 6 }

ospfNewCfgStaticAddOutRmap OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS read-write
    STATUS current  
    DESCRIPTION
	"The route map to be add into out-rmap list. When read, 0 is returned."
    ::= { ospfRedistributeStatic 7 }

ospfNewCfgStaticRemoveOutRmap OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS read-write
    STATUS current  
    DESCRIPTION
	"The route map to be removed from out-rmap list. When read, 
         0 is returned."
    ::= { ospfRedistributeStatic 8 }


ospfRedistributeFixed    OBJECT IDENTIFIER ::= { ospfRouteRedistribution 4 }

ospfCurCfgFixedMetric OBJECT-TYPE
    SYNTAX INTEGER (0..16777214)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The export metric for fixed routes. A value of 0 indicates none"
    ::= { ospfRedistributeFixed 1 }

ospfNewCfgFixedMetric OBJECT-TYPE
    SYNTAX INTEGER (0..16777214)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"The export metric for fixed routes. A value of 0 indicates none"
    ::= { ospfRedistributeFixed 2 }

ospfCurCfgFixedMetricType OBJECT-TYPE
    SYNTAX INTEGER {
        none(1),
        type1(2),
        type2(3)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The AS External metric type for fixed routes."
    ::= { ospfRedistributeFixed 3 }

ospfNewCfgFixedMetricType OBJECT-TYPE
    SYNTAX INTEGER {
        none(1),
        type1(2),
        type2(3)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"The AS External metric type for fixed routes."
    ::= { ospfRedistributeFixed 4 }

ospfCurCfgFixedOutRmapList OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The route maps present in the out route map list. 
         The route maps are presented in a bitmap format.

         in receiving order:

         OCTET 1  OCTET 2  .....
         xxxxxxxx xxxxxxxx .....
         ||    || |_ Rmap 9
         ||    ||
         ||    ||___ Rmap 8
         ||    |____ Rmap 7
         ||      .    .   .
         ||_________ Rmap 2
         |__________ Rmap 1

         where x : 1 - The represented route map is selected
         0 - The represented route map is not selected"
    ::= { ospfRedistributeFixed 5 }

ospfNewCfgFixedOutRmapList OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The route maps present in the out route map list. 
         The route maps are presented in a bitmap format.

         in receiving order:

         OCTET 1  OCTET 2  .....
         xxxxxxxx xxxxxxxx .....
         ||    || |_ Rmap 9
         ||    ||
         ||    ||___ Rmap 8
         ||    |____ Rmap 7
         ||      .    .   .
         ||_________ Rmap 2
         |__________ Rmap 1

         where x : 1 - The represented route map is selected
         0 - The represented route map is not selected"
    ::= { ospfRedistributeFixed 6 }

ospfNewCfgFixedAddOutRmap OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS read-write
    STATUS current  
    DESCRIPTION
	"The route map to be add into out-rmap list. When read, 0 is returned."
    ::= { ospfRedistributeFixed 7 }

ospfNewCfgFixedRemoveOutRmap OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS read-write
    STATUS current  
    DESCRIPTION
	"The route map to be removed from out-rmap list. When read, 
         0 is returned."
    ::= { ospfRedistributeFixed 8 }

ospfRedistributeRip    OBJECT IDENTIFIER ::= { ospfRouteRedistribution 5 }

ospfCurCfgRipMetric OBJECT-TYPE
    SYNTAX INTEGER (0..16777214)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The export metric for RIP routes. A value of 0 indicates none"
    ::= { ospfRedistributeRip 1 }

ospfNewCfgRipMetric OBJECT-TYPE
    SYNTAX INTEGER (0..16777214)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"The export metric for RIP routes. A value of 0 indicates none"
    ::= { ospfRedistributeRip 2 }

ospfCurCfgRipMetricType OBJECT-TYPE
    SYNTAX INTEGER {
        none(1),
        type1(2),
        type2(3)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The AS External metric type for RIP routes."
    ::= { ospfRedistributeRip 3 }

ospfNewCfgRipMetricType OBJECT-TYPE
    SYNTAX INTEGER {
        none(1),
        type1(2),
        type2(3)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"The AS External metric type for RIP routes."
    ::= { ospfRedistributeRip 4 }

ospfCurCfgRipOutRmapList OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The route maps present in the out route map list. 
         The route maps are presented in a bitmap format.

         in receiving order:

         OCTET 1  OCTET 2  .....
         xxxxxxxx xxxxxxxx .....
         ||    || |_ Rmap 9
         ||    ||
         ||    ||___ Rmap 8
         ||    |____ Rmap 7
         ||      .    .   .
         ||_________ Rmap 2
         |__________ Rmap 1

         where x : 1 - The represented route map is selected
         0 - The represented route map is not selected"
    ::= { ospfRedistributeRip 5 }

ospfNewCfgRipOutRmapList OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The route maps present in the out route map list. 
         The route maps are presented in a bitmap format.

         in receiving order:

         OCTET 1  OCTET 2  .....
         xxxxxxxx xxxxxxxx .....
         ||    || |_ Rmap 9
         ||    ||
         ||    ||___ Rmap 8
         ||    |____ Rmap 7
         ||      .    .   .
         ||_________ Rmap 2
         |__________ Rmap 1

         where x : 1 - The represented route map is selected
         0 - The represented route map is not selected"
    ::= { ospfRedistributeRip 6 }

ospfNewCfgRipAddOutRmap OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS read-write
    STATUS current  
    DESCRIPTION
	"The route map to be add into out-rmap list. When read, 0 is returned."
    ::= { ospfRedistributeRip 7 }

ospfNewCfgRipRemoveOutRmap OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS read-write
    STATUS current  
    DESCRIPTION
	"The route map to be removed from out-rmap list. When read, 
         0 is returned."
    ::= { ospfRedistributeRip 8 }

ipCurCfgRouterID OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The router ID of the switch." 
    ::= { ipGeneralCfg 1 }

ipNewCfgRouterID OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"The router ID of the switch." 
    ::= { ipGeneralCfg 2 }


-- IGMP Snooping config
igmpCurCfgOnOff OBJECT-TYPE
    SYNTAX INTEGER { 
        on(1),
        off(2)
	}
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Globally turn IGMP On/Off."
    ::= { igmpCfg 1}

igmpNewCfgOnOff OBJECT-TYPE
    SYNTAX INTEGER { 
        on(1),
        off(2)
	}
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Globally turn IGMP On/Off."
    ::= { igmpCfg 2}

igmpSnoopCfgGen	  OBJECT IDENTIFIER ::= { igmpCfg 3 }
igmpStaticMrtrCfg OBJECT IDENTIFIER ::= { igmpCfg 4 }
igmpFilterCfg     OBJECT IDENTIFIER ::= { igmpCfg 5 }

igmpSnoopCfg	  OBJECT IDENTIFIER ::= { igmpSnoopCfgGen 1 }

igmpSnoopCurCfgTimeout OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Set IGMP Report timeout."
    ::= { igmpSnoopCfg 1 }

igmpSnoopNewCfgTimeout OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Set IGMP Report timeout."
    ::= { igmpSnoopCfg 2 }

igmpSnoopCurCfgMrto OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current  
    DESCRIPTION
        "The value of multicast router timeout in the current config."
    ::= { igmpSnoopCfg 3 }

igmpSnoopNewCfgMrto OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-write
    STATUS  current  
    DESCRIPTION
        "The value of multicast router timeout in the new config."
    ::= { igmpSnoopCfg 4 }


igmpSnoopNewCfgVlanFastlvAdd OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-write
    STATUS  current  
    DESCRIPTION
	"The VLAN to be added to fastleave vlan list. When read,
	 0 is returned."
    ::= { igmpSnoopCfg 12 }

igmpSnoopNewCfgVlanFastlvRem OBJECT-TYPE
    SYNTAX  Integer32 
    MAX-ACCESS  read-write
    STATUS  current  
    DESCRIPTION
	"The VLAN to be removed from fastleave vlan list. When read,
	 0 is returned."
    ::= { igmpSnoopCfg 13 }

igmpSnoopCurCfgVlanFastlvBmap OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The fastlv enabled vlans present in the in vlan map list. 
         The fastlv enabled vlans are presented in a bitmap format.

         in receiving order:

         OCTET 1  OCTET 2  .....
         xxxxxxxx xxxxxxxx .....
         ||    || |_ Vlan 9
         ||    ||
         ||    ||___ Vlan 8
         ||    |____ Vlan 7
         ||      .    .   .
         ||_________ Vlan 2
         |__________ Vlan 1

         where x : 1 - The represented vlan has fastlv enabled
         0 - The represented vlan does not have fastlv enabled." 
    ::= { igmpSnoopCfg 14 }

igmpSnoopNewCfgVlanFastlvBmap OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The fastlv enabled vlans present in the in vlan map list. 
         The fastlv enabled vlans are presented in a bitmap format.

         in receiving order:

         OCTET 1  OCTET 2  .....
         xxxxxxxx xxxxxxxx .....
         ||    || |_ Vlan 9
         ||    ||
         ||    ||___ Vlan 8
         ||    |____ Vlan 7
         ||      .    .   .
         ||_________ Vlan 2
         |__________ Vlan 1

         where x : 1 - The represented vlan has fastlv enabled
         0 - The represented vlan does not have fastlv enabled." 
    ::= { igmpSnoopCfg 15 }

igmpSnoopCurCfgRobust OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current  
    DESCRIPTION
        "The value of expected packet loss on subnet in the current config."
    ::= { igmpSnoopCfg 16 }

igmpSnoopNewCfgRobust OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-write
    STATUS  current  
    DESCRIPTION
        "The value of expected packet loss on subnet in the new config."
    ::= { igmpSnoopCfg 17 }

igmpSnoopNewCfgVlanAdd OBJECT-TYPE
    SYNTAX  Integer32 
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The VLAN to be added to snooping vlan list. When read,
         0 is returned."
    ::= { igmpSnoopCfg 18 }

igmpSnoopNewCfgVlanRem OBJECT-TYPE
    SYNTAX  Integer32 
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The VLAN to be removed from snooping vlan list. When read,
         0 is returned."
    ::= { igmpSnoopCfg 19 }

igmpSnoopNewCfgVlanClear OBJECT-TYPE
    SYNTAX  INTEGER {
        clear(1),
        ok(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Removing ALL Snooping Vlans."
    ::= { igmpSnoopCfg 20 }

igmpSnoopCurCfgVlanBmap OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The snooping vlans present in the in vlan map list.
         The snooping vlans are presented in a bitmap format.

         in receiving order:

         OCTET 1  OCTET 2  .....
         xxxxxxxx xxxxxxxx .....
         ||    || |_ Vlan 9
         ||    ||
         ||    ||___ Vlan 8
         ||    |____ Vlan 7
         ||      .    .   .
         ||_________ Vlan 2
         |__________ Vlan 1

         where x : 1 - The represented vlan has snoop enabled
         0 - The represented vlan does not have snooping enabled."
    ::= { igmpSnoopCfg 21 }

igmpSnoopNewCfgVlanBmap OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The snooping vlans present in the in vlan map list.
         The snooping vlans are presented in a bitmap format.

         in receiving order:

         OCTET 1  OCTET 2  .....
         xxxxxxxx xxxxxxxx .....
         ||    || |_ Vlan 9
         ||    ||
         ||    ||___ Vlan 8
         ||    |____ Vlan 7
         ||      .    .   .
         ||_________ Vlan 2
         |__________ Vlan 1

         where x : 1 - The represented vlan has snoop enabled
         0 - The represented vlan does not have snooping enabled."
    ::= { igmpSnoopCfg 22 }

igmpSnoopCurCfgQInterval OBJECT-TYPE
    SYNTAX  Integer32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "IGMP Query Interval of current config."
    ::= { igmpSnoopCfg 23 }

igmpSnoopNewCfgQInterval OBJECT-TYPE
    SYNTAX  Integer32 
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "IGMP Query Interval of new config."
    ::= { igmpSnoopCfg 24 }

igmpSnoopCurCfgSrcIp OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The source ip for GSQ proxy in current config." 
    ::= { igmpSnoopCfg 25 }

igmpSnoopNewCfgSrcIp OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
	"The source ip for GSQ proxy in new config." 
    ::= { igmpSnoopCfg 26 }

igmpSnoopCurCfgAggrEnaDis OBJECT-TYPE
    SYNTAX INTEGER {
       enable(1),
       disable(2)
      }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable/Disable of IGMP Report aggregation."
    ::= { igmpSnoopCfg 27}

igmpSnoopNewCfgAggrEnaDis OBJECT-TYPE
    SYNTAX INTEGER {
        enable(1),
        disable(2)
      }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable/Disable of IGMP Report aggregation."
    ::= { igmpSnoopCfg 28}

igmpSnoopCurCfgFlood OBJECT-TYPE
    SYNTAX INTEGER {
        enable(1),
        disable(2)
      }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable/Disable of flood unregistered IPMC"
    ::= { igmpSnoopCfg 29}

igmpSnoopNewCfgFlood OBJECT-TYPE
    SYNTAX INTEGER {
        enable(1),
        disable(2)
      }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable/Disable of flood unregistered IPMC"
    ::= { igmpSnoopCfg 30}

igmpV3SnoopCfg      OBJECT IDENTIFIER ::= { igmpSnoopCfgGen 2 }

igmpV3SnoopCurCfgSources OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Number of sources to snoop in a group record in current config."
    ::= { igmpV3SnoopCfg 1 }

igmpV3SnoopNewCfgSources OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Number of sources to snoop in a group record in new config."
    ::= { igmpV3SnoopCfg 2 }

igmpV3SnoopCurCfgEnaDis OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The current status of IGMP V3 Snooping."
    ::= { igmpV3SnoopCfg 3 }

igmpV3SnoopNewCfgEnaDis OBJECT-TYPE
    SYNTAX INTEGER {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Set Enable/Disable of IGMP V3 Snooping."
    ::= { igmpV3SnoopCfg 4 }

igmpV3SnoopCurCfgExcludeEnaDis OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The current status of IGMP V3 EXCLUDE filter-mode Snooping."
    ::= { igmpV3SnoopCfg 5 }

igmpV3SnoopNewCfgExcludeEnaDis OBJECT-TYPE
    SYNTAX INTEGER {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Set Enable/Disable of IGMP V3 EXCLUDE filter-mode Snooping."
    ::= { igmpV3SnoopCfg 6 }

igmpV3SnoopCurCfgV1V2EnaDis OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The current status of IGMP V1/V2 Report Snooping."
    ::= { igmpV3SnoopCfg 7 }

igmpV3SnoopNewCfgV1V2EnaDis OBJECT-TYPE
    SYNTAX INTEGER {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Set Enable/Disable of IGMP V1/V2 Report Snooping."
    ::= { igmpV3SnoopCfg 8 }


-- IGMP Static Mrtr Support
igmpStaticMrtrCurCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF IgmpStaticMrtrCurCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The IGMP Static Multicast Router table in the current configuration block."
    ::= { igmpStaticMrtrCfg 1 }

igmpStaticMrtrCurCfgTableEntry OBJECT-TYPE
    SYNTAX  IgmpStaticMrtrCurCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the Static Multicast Router table."
    INDEX   { igmpStaticMrtrCurCfgIndx }
    ::= { igmpStaticMrtrCurCfgTable 1 }

IgmpStaticMrtrCurCfgTableEntry ::= SEQUENCE {
    igmpStaticMrtrCurCfgIndx         Integer32,
    igmpStaticMrtrCurCfgPortId       Integer32,
    igmpStaticMrtrCurCfgVlanId       Integer32,
    igmpStaticMrtrCurCfgVersion      INTEGER
    }

igmpStaticMrtrCurCfgIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IGMP Multicast Router table port index."
    ::= { igmpStaticMrtrCurCfgTableEntry 1 }

igmpStaticMrtrCurCfgPortId OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IGMP Multicast Router port in the current configuration block."
    ::= { igmpStaticMrtrCurCfgTableEntry 2 }

igmpStaticMrtrCurCfgVlanId OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IGMP Multicast Router port in the current configuration block."
    ::= { igmpStaticMrtrCurCfgTableEntry 3 }

igmpStaticMrtrCurCfgVersion OBJECT-TYPE
    SYNTAX  INTEGER {
        version1(1),
        version2(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IGMP version of the IGMP Static Multicast Router."
    ::= { igmpStaticMrtrCurCfgTableEntry 4 }

igmpStaticMrtrNewCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF IgmpStaticMrtrNewCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The IGMP Static Multicast Router table in the new configuration block."
    ::= { igmpStaticMrtrCfg 2 }

igmpStaticMrtrNewCfgTableEntry OBJECT-TYPE
    SYNTAX  IgmpStaticMrtrNewCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the Static Multicast Router table."
    INDEX   { igmpStaticMrtrNewCfgIndx }
    ::= { igmpStaticMrtrNewCfgTable 1 }

IgmpStaticMrtrNewCfgTableEntry ::= SEQUENCE {
    igmpStaticMrtrNewCfgIndx         Integer32,
    igmpStaticMrtrNewCfgPortId       Integer32,
    igmpStaticMrtrNewCfgVlanId       Integer32,
    igmpStaticMrtrNewCfgVersion      INTEGER,
    igmpStaticMrtrNewCfgDelete       INTEGER
    }

igmpStaticMrtrNewCfgIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IGMP Multicast Router table port index."
    ::= { igmpStaticMrtrNewCfgTableEntry 1 }

igmpStaticMrtrNewCfgPortId OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The IGMP Multicast Router port in the new configuration block."
    ::= { igmpStaticMrtrNewCfgTableEntry 2 }

igmpStaticMrtrNewCfgVlanId OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The IGMP Multicast Router port in the new configuration block."
    ::= { igmpStaticMrtrNewCfgTableEntry 3 }

igmpStaticMrtrNewCfgVersion OBJECT-TYPE
    SYNTAX  INTEGER {
        version1(1),
        version2(2),
        version3(3)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The IGMP version of the IGMP Static Multicast Router."
    ::= { igmpStaticMrtrNewCfgTableEntry 4 }

igmpStaticMrtrNewCfgDelete OBJECT-TYPE
    SYNTAX  INTEGER {
        other(1),
        delete(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "When set to the value of 2 (delete), the entire row is deleted.
         When read, other(1) is returned. Setting the value to anything
         other than 2(delete) has no effect on the state of the row."
    ::= { igmpStaticMrtrNewCfgTableEntry 5 }

-- IGMP Filtering
igmpFltCurCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF IgmpFltCurCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The IGMP filtering table in the current configuration block."
    ::= { igmpFilterCfg 1 }

igmpFltCurCfgTableEntry OBJECT-TYPE
    SYNTAX  IgmpFltCurCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the filtering table."
    INDEX   { igmpFltCurCfgIndx }
    ::= { igmpFltCurCfgTable 1 }

IgmpFltCurCfgTableEntry ::= SEQUENCE {
    igmpFltCurCfgIndx         Integer32,
    igmpFltCurCfgMcastIp1     IpAddress,
    igmpFltCurCfgMcastIp2     IpAddress,
    igmpFltCurCfgAction       INTEGER,
    igmpFltCurCfgState        INTEGER
    }

igmpFltCurCfgIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IGMP filter table index."
    ::= { igmpFltCurCfgTableEntry 1 }

igmpFltCurCfgMcastIp1 OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Range1 Multicast IP address to be filtered."
    ::= { igmpFltCurCfgTableEntry 2 }

igmpFltCurCfgMcastIp2 OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Range2 Multicast IP address to be filtered."
    ::= { igmpFltCurCfgTableEntry 3 }

igmpFltCurCfgAction OBJECT-TYPE
    SYNTAX  INTEGER {
        allow(1),
        deny(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The action for the IGMP filtering rule."
    ::= { igmpFltCurCfgTableEntry 4 }

igmpFltCurCfgState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The state of this IGMP filtering rule."
    ::= { igmpFltCurCfgTableEntry 5 }

igmpFltNewCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF IgmpFltNewCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The IGMP filtering table in the current configuration block."
    ::= { igmpFilterCfg 2 }

igmpFltNewCfgTableEntry OBJECT-TYPE
    SYNTAX  IgmpFltNewCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the filtering table."
    INDEX   { igmpFltNewCfgIndx }
    ::= { igmpFltNewCfgTable 1 }

IgmpFltNewCfgTableEntry ::= SEQUENCE {
    igmpFltNewCfgIndx         Integer32,
    igmpFltNewCfgMcastIp1     IpAddress,
    igmpFltNewCfgMcastIp2     IpAddress,
    igmpFltNewCfgAction       INTEGER,
    igmpFltNewCfgState        INTEGER,
    igmpFltNewCfgDelete       INTEGER
    }

igmpFltNewCfgIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IGMP filter table index."
    ::= { igmpFltNewCfgTableEntry 1 }

igmpFltNewCfgMcastIp1 OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Range1 Multicast source IP address to be filtered."
    ::= { igmpFltNewCfgTableEntry 2 }

igmpFltNewCfgMcastIp2 OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Range2 Multicast source IP address to be filtered."
    ::= { igmpFltNewCfgTableEntry 3 }

igmpFltNewCfgAction OBJECT-TYPE
    SYNTAX  INTEGER {
        allow(1),
        deny(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The action for the IGMP filtering rule."
    ::= { igmpFltNewCfgTableEntry 4 }

igmpFltNewCfgState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The state of this IGMP filtering rule."
    ::= { igmpFltNewCfgTableEntry 5 }

igmpFltNewCfgDelete OBJECT-TYPE
    SYNTAX  INTEGER {
        other(1),
        delete(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "When set to the value of 2 (delete), the entire row is deleted. 
         When read, other(1) is returned. Setting the value to anything 
         other than 2(delete) has no effect on the state of the row."
    ::= { igmpFltNewCfgTableEntry 6 }


-- IGMP Filtering Port Table

igmpFltCurCfgPortTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF IgmpFltCurCfgPortTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The IGMP filtering port table in the current configuration block."
    ::= { igmpFilterCfg 3 }

igmpFltCurCfgPortTableEntry OBJECT-TYPE
    SYNTAX  IgmpFltCurCfgPortTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the IGMP filtering port table."
    INDEX   { igmpFltCurCfgPortIndx }
    ::= { igmpFltCurCfgPortTable 1 }

IgmpFltCurCfgPortTableEntry ::= SEQUENCE {
    igmpFltCurCfgPortIndx         Integer32,
    igmpFltCurCfgPortState        INTEGER,
    igmpFltCurCfgPortFiltBmap     OCTET STRING
    }

igmpFltCurCfgPortIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port index."
    ::= { igmpFltCurCfgPortTableEntry 1 }

igmpFltCurCfgPortState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable IGMP filtering."
    ::= { igmpFltCurCfgPortTableEntry 2 }

igmpFltCurCfgPortFiltBmap OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(0..256))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	"The IGMP filtering rules applied to the port.  The filtering rules are 
         presented in bitmap format.

	 in receiving order:

	     OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx ..... 
             ||    || |_ filter 9
             ||    ||  
             ||    ||___ filter 8
             ||    |____ filter 7
             ||      .    .   .
             ||_________ filter 2
             |__________ filter 1 (as index to igmpFltCurCfgTable)

         where x : 1 - The represented IGMP filter rule applied to the port
		   0 - The represented IGMP filter rule not applied to the port "
    ::= { igmpFltCurCfgPortTableEntry 3 }

igmpFltNewCfgPortTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF IgmpFltNewCfgPortTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The IGMP filtering port table in the new configuration block."
    ::= { igmpFilterCfg 4 }

igmpFltNewCfgPortTableEntry OBJECT-TYPE
    SYNTAX  IgmpFltNewCfgPortTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the IGMP filtering port table."
    INDEX   { igmpFltNewCfgPortIndx }
    ::= { igmpFltNewCfgPortTable 1 }

IgmpFltNewCfgPortTableEntry ::= SEQUENCE {
    igmpFltNewCfgPortIndx         Integer32,
    igmpFltNewCfgPortState        INTEGER,
    igmpFltNewCfgPortFiltBmap     OCTET STRING,
    igmpFltNewCfgPortAddFiltRule  Integer32,
    igmpFltNewCfgPortRemFiltRule  Integer32
    }

igmpFltNewCfgPortIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port index."
    ::= { igmpFltNewCfgPortTableEntry 1 }

igmpFltNewCfgPortState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Enable or disable IGMP filtering."
    ::= { igmpFltNewCfgPortTableEntry 2 }

igmpFltNewCfgPortFiltBmap OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(0..256))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IGMP filtering rules applied to the port.  The filtering rules
         are presented in bitmap format.

         in receiving order:

	     OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx ..... 
             ||    || |_ filter 9
             ||    ||  
             ||    ||___ filter 8
             ||    |____ filter 7
             ||      .    .   .
             ||_________ filter 2
             |__________ filter 1 (as index to fltNewCfgTable)

         where x : 1 - The represented filter rule applied to the port
		   0 - The represented filter rule not applied to the port "
    ::= { igmpFltNewCfgPortTableEntry 3 }

igmpFltNewCfgPortAddFiltRule OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "This is an action object to add filtering rule to a port. The value 
         specified with this object is the index to the fltNewCfgTable for 
         which filtering rule to be added to the port. The range of the 
         valid index is between 1 and igmpFltCurCfgTableMaxSize. When read, the 
         value '0' is returned always."
    ::= { igmpFltNewCfgPortTableEntry 4 }

igmpFltNewCfgPortRemFiltRule OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "This is an action object to remove filtering rule from a port.	The 
         value specified with this object is the index to the fltNewCfgTable 
         for which filtering rule to be removed from the port. The range of 
         the valid index is between 1 and igmpFltCurCfgTableMaxSize.  When read, 
         the value '0' is returned always."
    ::= { igmpFltNewCfgPortTableEntry 5 }

igmpFltCurCfgEnaDis OBJECT-TYPE
    SYNTAX INTEGER { 
        enable(1),
        disable(2)
	}
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable/Disable of IGMP Filtering."
    ::= { igmpFilterCfg 5 }

igmpFltNewCfgEnaDis OBJECT-TYPE
    SYNTAX INTEGER { 
        enable(1),
        disable(2)
	}
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable/Disable of IGMP Filtering."
    ::= { igmpFilterCfg 6 }

-- Statistics


-- RIPv2 Statistics

ripStatInPackets OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of RIP packets recieved."
    ::= { rip2Stats 1 }

ripStatOutPackets OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of RIP packets transmitted."
    ::= { rip2Stats 2 }

ripStatInRequestPkts OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of RIP requests recieved."
    ::= { rip2Stats 3 }

ripStatInResponsePkts OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of RIP response recieved."
    ::= { rip2Stats 4 }

ripStatOutRequestPkts OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of RIP requests transmitted."
    ::= { rip2Stats 5 }

ripStatOutResponsePkts OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of RIP responses transmitted."
    ::= { rip2Stats 6 }

ripStatRouteTimeout OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of RIP route timeouts."
    ::= { rip2Stats 7 }

ripStatInBadSizePkts OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of bad size RIP packets recieved."
    ::= { rip2Stats 8 }

ripStatInBadVersion OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of RIP bad versions recieved."
    ::= { rip2Stats 9 }

ripStatInBadZeros OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of RIP bad zeros recieved."
    ::= { rip2Stats 10 }

ripStatInBadSourcePort OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of RIP bad source port recieved."
    ::= { rip2Stats 11 }

ripStatInBadSourceIP OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of RIP bad source IP recieved."
    ::= { rip2Stats 12 }

ripStatInSelfRcvPkts OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of RIP packets from self received."
    ::= { rip2Stats 13 }

--DNS Statistics


dnsStatInGoodDnsRequests OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of good DNS request packets received."
    ::= { dnsStats 1 }

dnsStatOutDnsRequests  OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of  DNS request packets"
    ::= { dnsStats 2 }

dnsStatInBadDnsRequests OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of  bad DNS request packets received"
    ::= { dnsStats 3 }


-- GEAL3 Stats

maxL3TableSize OBJECT-TYPE
   SYNTAX Integer32
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
	"Max L3 table size"
   ::= {geal3Stats 1}

noL3EntriesUsed OBJECT-TYPE
   SYNTAX Integer32
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
	"Number of L3 entries used"
   ::= {geal3Stats 2}

maxLpmTableSize OBJECT-TYPE
   SYNTAX Integer32
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
	"Max LPM table size"
   ::= {geal3Stats 3}

noLpmEntriesUsed OBJECT-TYPE
   SYNTAX Integer32
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
	"Number of LPM entries used"
   ::= {geal3Stats 4}

maxBlockInLpmTable OBJECT-TYPE
   SYNTAX Integer32
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
	"Max number of blocks in LPM table"
   ::= {geal3Stats 5}

noBlocksUsedInLpmTable OBJECT-TYPE
   SYNTAX Integer32
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
	"Number of blocks used in LPM table"
   ::= {geal3Stats 6}


-- ARP Statistics Group

arpStatEntries OBJECT-TYPE
    SYNTAX  Gauge32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The current number of ARP entries."
    ::= { arpStats 1 }

arpStatHighWater OBJECT-TYPE
    SYNTAX  Gauge32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The highest number of ARP entries."
    ::= { arpStats 2 }

arpStatMaxEntries OBJECT-TYPE
    SYNTAX  Gauge32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum number of ARP entries."
    ::= { arpStats 3 }

-- ROUTE Statistics Group

routeStatEntries OBJECT-TYPE
    SYNTAX  Gauge32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The current number of IP routes."
    ::= { routeStats 1 }

routeStatHighWater OBJECT-TYPE
    SYNTAX  Gauge32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The highest number of IP routes."
    ::= { routeStats 2 }

routeStatMaxEntries OBJECT-TYPE
    SYNTAX  Gauge32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum number of IP routes."
    ::= { routeStats 3 }

-- The VRRP Statistics

vrrpStatInAdvers OBJECT-TYPE 
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current 
    DESCRIPTION 
        "The number of good VRRP advertisements which are received."
    ::= { vrrpStats 1 }

vrrpStatOutAdvers OBJECT-TYPE 
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current 
    DESCRIPTION 
        "The number of good VRRP advertisements which are transmitted."
    ::= { vrrpStats 2 }

vrrpStatOutBadAdvers OBJECT-TYPE 
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current 
    DESCRIPTION 
        "The number of bad VRRP advertisements which are received."
    ::= { vrrpStats 3 }

vrrpStatBadVersion OBJECT-TYPE 
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current 
    DESCRIPTION 
        "The number of bad VRRP version adv which are received."
    ::= { vrrpStats 4 }

vrrpStatBadAddress OBJECT-TYPE 
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current 
    DESCRIPTION 
        "The number of bad VRRP addres adv which are received."
    ::= { vrrpStats 5 }

vrrpStatBadPassword OBJECT-TYPE 
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current 
    DESCRIPTION 
        "The number of bad VRRP advertisements which are received."
    ::= { vrrpStats 6 }

vrrpStatBadVrid OBJECT-TYPE 
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current 
    DESCRIPTION 
        "The number of bad VRRP version ID adv which are received."
    ::= { vrrpStats 7 }

vrrpStatBadData OBJECT-TYPE 
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current 
    DESCRIPTION 
        "The number of bad VRRP advertisements which are received."
    ::= { vrrpStats 8 }

vrrpStatBadInterval OBJECT-TYPE 
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current 
    DESCRIPTION 
        "The number of bad VRRP iutervals which are received."
    ::= { vrrpStats 9 }


-- Clear Statistics  for ip and ip interface
ipClearStats OBJECT-TYPE
    SYNTAX  INTEGER { 
	clear(1),
	ok(2)
	}
    MAX-ACCESS  read-write
    STATUS  current  
    DESCRIPTION
        "Setting this to clear(1) results in clearing the IP statistics." 
    ::= { clearStats 1 }

vrrpClearStats OBJECT-TYPE 
    SYNTAX  INTEGER {
        ok(1),
        clear(2)
        }
    MAX-ACCESS  read-write
    STATUS  current 
    DESCRIPTION 
        "Setting this to clear(2) results in clearing the VRRP statistics."
    ::= { clearStats 2 }


ripClearStats OBJECT-TYPE
    SYNTAX  INTEGER {
        clear(1),
        ok(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Setting this to clear(1) results in clearing the RIP statistics."
    ::= { clearStats 4 }

ospfClearStats OBJECT-TYPE
    SYNTAX  INTEGER {
        clear(1),
        ok(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Setting this to clear(1) results in clearing the OSPF statistics."
    ::= { clearStats 5 }

tcpClearStats OBJECT-TYPE
    SYNTAX  INTEGER {
        clear(1),
        ok(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Setting this to clear(1) results in clearing the TCP statistics."
    ::= { clearStats 6 }

udpClearStats OBJECT-TYPE
    SYNTAX  INTEGER {
        clear(1),
        ok(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Setting this to clear(1) results in clearing the UDP statistics."
    ::= { clearStats 7 }

dnsClearStats OBJECT-TYPE
    SYNTAX  INTEGER {
        clear(1),
        ok(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Setting this to clear(1) results in clearing the DNS statistics."
    ::= { clearStats 8 }

arpClearStats OBJECT-TYPE
    SYNTAX  INTEGER {
        clear(1),
        ok(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Setting this to clear(1) results in clearing the ARP statistics."
    ::= { clearStats 9 }

icmpClearStats OBJECT-TYPE
    SYNTAX  INTEGER {
        clear(1),
        ok(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Setting this to clear(1) results in clearing the ICMP statistics."
    ::= { clearStats 10 }

routeClearStats OBJECT-TYPE
    SYNTAX  INTEGER {
        clear(1),
        ok(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Setting this to clear(1) results in clearing the Route statistics."
    ::= { clearStats 11 }

-- igmp stats
igmpClearAllStats OBJECT-TYPE
    SYNTAX  INTEGER { 
	clear(1),
	ok(2)
	}
    MAX-ACCESS  read-write
    STATUS  current  
    DESCRIPTION
        "Setting this to clear(1) results in clearing the IGMP statistics." 
    ::= { igmpStats 2 }

igmpStatsTotalIgmpGroups OBJECT-TYPE 
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current 
    DESCRIPTION 
        "The total number of IGMP groups."
    ::= { igmpStats 3 }

igmpStatsTotalIpmcGroups OBJECT-TYPE 
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current 
    DESCRIPTION 
        "The total number of IPMC groups."
    ::= { igmpStats 4 }

-- Ospf Statistics 

-- Ospf Statistics for all interfaces and OSPF areas 
ospfGeneralStats       OBJECT IDENTIFIER ::= { ospfStats  1 }
ospfCumRxTxStats       OBJECT IDENTIFIER ::= { ospfGeneralStats  1 }
ospfCumNbrChangeStats  OBJECT IDENTIFIER ::= { ospfGeneralStats  2 }
ospfCumIntfChangeStats OBJECT IDENTIFIER ::= { ospfGeneralStats  3 }
ospfTimersKickOffStats OBJECT IDENTIFIER ::= { ospfGeneralStats  4 }

-- Ospf Statistics / Area
ospfArea	       OBJECT IDENTIFIER ::= { ospfStats  2 }

ospfAreaRxTxStats OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfAreaRxTxStatsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Area Rx/Tx Statistics."
    ::= { ospfArea 1 }

ospfAreaRxTxStatsEntry OBJECT-TYPE
    SYNTAX OspfAreaRxTxStatsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Rx Tx packet Statistics about a OSPF area."
    INDEX { ospfAreaRxTxIndex }
    ::= { ospfAreaRxTxStats 1 }
 
OspfAreaRxTxStatsEntry ::= SEQUENCE {
    ospfAreaRxTxIndex          Integer32,
    ospfAreaRxPkts             Counter32,
    ospfAreaTxPkts             Counter32,
    ospfAreaRxHello            Counter32,
    ospfAreaTxHello            Counter32,
    ospfAreaRxDatabase         Counter32,
    ospfAreaTxDatabase         Counter32,
    ospfAreaRxlsReqs           Counter32,
    ospfAreaTxlsReqs           Counter32,
    ospfAreaRxlsAcks           Counter32,
    ospfAreaTxlsAcks           Counter32,
    ospfAreaRxlsUpdates        Counter32,
    ospfAreaTxlsUpdates        Counter32
    }

ospfAreaRxTxIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The index of the ospf Area for which these statistics apply."
    ::= { ospfAreaRxTxStatsEntry 1 }

ospfAreaRxPkts OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of OSPF packets received in this OSPF area."
    ::= { ospfAreaRxTxStatsEntry 2 }
 
ospfAreaTxPkts OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of OSPF packets transmitted in this OSPF area."
    ::= { ospfAreaRxTxStatsEntry 3 }
 
ospfAreaRxHello OBJECT-TYPE
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Hello packets received in this OSPF area."
    ::= { ospfAreaRxTxStatsEntry 4 }

ospfAreaTxHello OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Hello packets transmitted in this OSPF
         area."
    ::= { ospfAreaRxTxStatsEntry 5 }
 
ospfAreaRxDatabase OBJECT-TYPE
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Database Description packets transmitted 
         for this OSPF area."
    ::= { ospfAreaRxTxStatsEntry 6 }

ospfAreaTxDatabase OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Database Description packets transmitted 
         for this OSPF area."
    ::= { ospfAreaRxTxStatsEntry 7 }
 
ospfAreaRxlsReqs OBJECT-TYPE
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Link State Request packets received for 
         this OSPF area."
    ::= { ospfAreaRxTxStatsEntry 8 }

ospfAreaTxlsReqs OBJECT-TYPE
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Link State Request packets transmitted for 
         this OSPF area."
    ::= { ospfAreaRxTxStatsEntry 9 }

ospfAreaRxlsAcks OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Link State Acknowledgement packets received for 
         this OSPF area."
    ::= { ospfAreaRxTxStatsEntry 10 }
 
ospfAreaTxlsAcks OBJECT-TYPE
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Link State Acknowledgement packets transmitted
         for this OSPF area."
    ::= { ospfAreaRxTxStatsEntry 11 }

ospfAreaRxlsUpdates OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Link State Update packets received for 
         this OSPF area."
    ::= { ospfAreaRxTxStatsEntry 12 }
 
ospfAreaTxlsUpdates OBJECT-TYPE
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Link State Update packets transmitted for 
         this OSPF area."
    ::= { ospfAreaRxTxStatsEntry 13 }


ospfAreaNbrChangeStats OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfAreaNbrChangeStatsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Area Neighbour Statistics."
    ::= { ospfArea 2 }

ospfAreaNbrChangeStatsEntry OBJECT-TYPE
    SYNTAX OspfAreaNbrChangeStatsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Area Neighbour Change Statistics about a OSPF area."
    INDEX { ospfAreaNbrIndex }
    ::= { ospfAreaNbrChangeStats 1 }
 
OspfAreaNbrChangeStatsEntry ::= SEQUENCE {
    ospfAreaNbrIndex  	       	Integer32,
    ospfAreaNbrhello           	Counter32,
    ospfAreaNbrStart           	Counter32,
    ospfAreaNbrAdjointOk       	Counter32,
    ospfAreaNbrNegotiationDone 	Counter32,
    ospfAreaNbrExchangeDone     Counter32,
    ospfAreaNbrBadRequests      Counter32,
    ospfAreaNbrBadSequence      Counter32,
    ospfAreaNbrLoadingDone      Counter32,
    ospfAreaNbrN1way        	Counter32,
    ospfAreaNbrRstAd        	Counter32,
    ospfAreaNbrDown        	Counter32,
    ospfAreaNbrN2way           	Counter32
    }

ospfAreaNbrIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The index of the ospf Area for which these statistics apply."
    ::= { ospfAreaNbrChangeStatsEntry 1 }

ospfAreaNbrhello OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Hello packets received from neighbours
         in this OSPF area."
    ::= { ospfAreaNbrChangeStatsEntry 2 }

ospfAreaNbrStart OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of neighbours in this state (i.e. an indication
         that  Hello packets should now be sent to the neighbour at intervals
         of HelloInterval seconds.) in this OSPF area."
    ::= { ospfAreaNbrChangeStatsEntry 3 }

ospfAreaNbrAdjointOk OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of decisions to be made (again) as to whether
         an adjacency should be established/maintained with the neighbour.
         for this OSPF area."
    ::= { ospfAreaNbrChangeStatsEntry 4 }

ospfAreaNbrNegotiationDone OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of neighbours in this state wherein the 
         Master/slave relationship has been negotiated, and sequence
         numbers have been exchanged, for this OSPF area."
    ::= { ospfAreaNbrChangeStatsEntry 5 }

ospfAreaNbrExchangeDone OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of neighbours in this state (i.e. in an
         adjacency's final state) having transimitted a full sequence 
         of Database Description packets, for this OSPF area."
    ::= { ospfAreaNbrChangeStatsEntry 6 }

ospfAreaNbrBadRequests OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total number of Link State Requests which have been received
         for a link state advertisement not contained in the database across
         this OSPF area."
    ::= { ospfAreaNbrChangeStatsEntry 7 }

ospfAreaNbrBadSequence OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Database Description packets which have been
         received that either 
         a) has an unexpected DD sequence number
         b) Unexpectedly has the init bit set
         c) Has an options field differing from the last Options field
            received in a Database Description packet.
         Any of these conditions indicate that some error has occured during
         adjacency establishment for this OSPF area."
    ::= { ospfAreaNbrChangeStatsEntry 8 }

ospfAreaNbrLoadingDone OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of link state updates received for all 
         out-of-date portions of the database in this OSPF area."
    ::= { ospfAreaNbrChangeStatsEntry 9 }

ospfAreaNbrN1way OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Hello packets received from neighbours, in
         which this router is not mentioned in this OSPF area."
    ::= { ospfAreaNbrChangeStatsEntry 10 }

ospfAreaNbrRstAd OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of times the Neighbour adjacency has been reset
         across this OPSF area."
    ::= { ospfAreaNbrChangeStatsEntry 11 }

ospfAreaNbrDown OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Neighbouring routers down (i.e. in the initial
         state of a neighbour conversation.) in this OSPF area."
    ::= { ospfAreaNbrChangeStatsEntry 12 }

ospfAreaNbrN2way OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Hello packets received from neighbours, in
         which this router is mentioned in this OSPF area."
    ::= { ospfAreaNbrChangeStatsEntry 13 }

ospfAreaChangeStats OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfAreaChangeStatsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Area Change Statistics."
    ::= { ospfArea 3 }

ospfAreaChangeStatsEntry OBJECT-TYPE
    SYNTAX OspfAreaChangeStatsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Area  Change Statistics about a OSPF area."
    INDEX { ospfAreaIntfIndex }
    ::= { ospfAreaChangeStats 1 }
 
OspfAreaChangeStatsEntry ::= SEQUENCE {
    ospfAreaIntfIndex     	Integer32,
    ospfAreaIntfHello           Counter32,
    ospfAreaIntfDown           	Counter32,
    ospfAreaIntfLoop       	Counter32,
    ospfAreaIntfUnloop 		Counter32,
    ospfAreaIntfWaitTimer     	Counter32,
    ospfAreaIntfBackup	        Counter32,
    ospfAreaIntfNbrChange       Counter32
    }

ospfAreaIntfIndex OBJECT-TYPE
    SYNTAX    Integer32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The index of the OSPF Area for which these statistics apply."
    ::= { ospfAreaChangeStatsEntry 1 }

ospfAreaIntfHello OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of Hello packets sent on this OSPF area."
    ::= { ospfAreaChangeStatsEntry 2 }

ospfAreaIntfDown OBJECT-TYPE
    SYNTAX   Counter32
    MAX-ACCESS   read-only
    STATUS   current
    DESCRIPTION
        "The total number of interfaces down in this OSPF area."
    ::= { ospfAreaChangeStatsEntry 3 }

ospfAreaIntfLoop OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of interfaces no longer connected to 
         the attatched network in this OSPF area."
    ::= { ospfAreaChangeStatsEntry 4 }

ospfAreaIntfUnloop OBJECT-TYPE
    SYNTAX   Counter32
    MAX-ACCESS   read-only
    STATUS   current
    DESCRIPTION
        "The total number of interfaces connected to the attatched
	 network in this OSPF area.."
    ::= { ospfAreaChangeStatsEntry 5 }


ospfAreaIntfWaitTimer OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS        read-only
    STATUS        current
    DESCRIPTION
        "The total number of times the Wait Timer has been fired,
         (indicating the end of the waiting period that is required
          before electing a (Backup) Designated Router) for this 
          OSPF area."
    ::= { ospfAreaChangeStatsEntry 6 }

ospfAreaIntfBackup OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS     read-only
    STATUS     current
    DESCRIPTION
        "The total number of Backup Designated Routers on the attatched
         network for this OSPF area."
    ::= { ospfAreaChangeStatsEntry 7 }


ospfAreaIntfNbrChange OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS     read-only
    STATUS     current
    DESCRIPTION
        "The total number of changes in the set of bidirectional neighbours
         associated with the interface in this OSPF area."
    ::= { ospfAreaChangeStatsEntry 8 }

ospfAreaErrorStats OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfAreaErrorStatsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Area Error Statistics."
    ::= { ospfArea 4 }

ospfAreaErrorStatsEntry OBJECT-TYPE
    SYNTAX OspfAreaErrorStatsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Error Statistics for an OSPF area."
    INDEX { ospfAreaErrIndex }
    ::= { ospfAreaErrorStats 1 }
 
OspfAreaErrorStatsEntry ::= SEQUENCE {
    ospfAreaErrIndex     	Integer32,
    ospfAreaErrAuthFailure      Counter32,
    ospfAreaErrNetmaskMismatch  Counter32,
    ospfAreaErrHelloMismatch    Counter32,
    ospfAreaErrDeadMismatch     Counter32,
    ospfAreaErrOptionsMismatch  Counter32,
    ospfAreaErrUnknownNbr       Counter32,
    ospfAreaErrAreaMismatch     Counter32
    }

ospfAreaErrIndex OBJECT-TYPE
    SYNTAX    Integer32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The index of the OSPF Area for which these statistics apply."
    ::= { ospfAreaErrorStatsEntry 1 }

ospfAreaErrAuthFailure OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of packets received with a wrong password in 
         this area."
    ::= { ospfAreaErrorStatsEntry 2 }

ospfAreaErrNetmaskMismatch OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of packets received with a wrong netmask in 
         this area."
    ::= { ospfAreaErrorStatsEntry 3 }

ospfAreaErrHelloMismatch OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of packets received with a different hello interval
         in this area."
    ::= { ospfAreaErrorStatsEntry 4 }

ospfAreaErrDeadMismatch OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of packets received with a different dead interval
         in this area."
    ::= { ospfAreaErrorStatsEntry 5 }

ospfAreaErrOptionsMismatch OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of packets received with a different options
         in this area."
    ::= { ospfAreaErrorStatsEntry 6 }

ospfAreaErrUnknownNbr OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of packets received from an unknown neighbor
         in this area."
    ::= { ospfAreaErrorStatsEntry 7 }

ospfAreaErrAreaMismatch OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of packets received with a wrong  area."
    ::= { ospfAreaErrorStatsEntry 8 }

-- Ospf Statistics / Interface
ospfInterface	       OBJECT IDENTIFIER ::= { ospfStats  3 }

ospfIntfRxTxStats OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfIntfRxTxStatsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Interface Rx/Tx packet Statistics."
    ::= { ospfInterface 1 }

ospfIntfRxTxStatsEntry OBJECT-TYPE
    SYNTAX OspfIntfRxTxStatsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "OSPF interface Rx/Tx packet statistics."
    INDEX { ospfIntfRxTxIndex }
    ::= { ospfIntfRxTxStats 1 }

OspfIntfRxTxStatsEntry ::= SEQUENCE {
    ospfIntfRxTxIndex          Integer32,
    ospfIntfRxPkts             Counter32,
    ospfIntfTxPkts             Counter32,
    ospfIntfRxHello            Counter32,
    ospfIntfTxHello            Counter32,
    ospfIntfRxDatabase         Counter32,
    ospfIntfTxDatabase         Counter32,
    ospfIntfRxlsReqs           Counter32,
    ospfIntfTxlsReqs           Counter32,
    ospfIntfRxlsAcks           Counter32,
    ospfIntfTxlsAcks           Counter32,
    ospfIntfRxlsUpdates        Counter32,
    ospfIntfTxlsUpdates        Counter32
    }

ospfIntfRxTxIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The OSPF interface for which these statistics apply."
    ::= { ospfIntfRxTxStatsEntry 1 }

ospfIntfRxPkts OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of OSPF packets received for this OSPF interface."
    ::= { ospfIntfRxTxStatsEntry 2 }
 
ospfIntfTxPkts OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of OSPF packets transmitted for this OSPF interface."
    ::= { ospfIntfRxTxStatsEntry 3 }
 
ospfIntfRxHello OBJECT-TYPE
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Hello packets received 
         for this OSPF interface."
    ::= { ospfIntfRxTxStatsEntry 4 }

ospfIntfTxHello OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Hello packets transmitted 
         for this OSPF interface."
    ::= { ospfIntfRxTxStatsEntry 5 }
 
ospfIntfRxDatabase OBJECT-TYPE
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Database Description packets received 
         for this OSPF interface."
    ::= { ospfIntfRxTxStatsEntry 6 }

ospfIntfTxDatabase OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Database Description packets transmitted 
         for this OSPF interface."
    ::= { ospfIntfRxTxStatsEntry 7 }
 
ospfIntfRxlsReqs OBJECT-TYPE
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Link State Request packets received
         for this OSPF interface."
    ::= { ospfIntfRxTxStatsEntry 8 }

ospfIntfTxlsReqs OBJECT-TYPE
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Link State Request packets transmitted
         for this OSPF interface."
    ::= { ospfIntfRxTxStatsEntry 9 }

ospfIntfRxlsAcks OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Link State Acknowledgement packets received
         for this OSPF interface."
    ::= { ospfIntfRxTxStatsEntry 10 }
 
ospfIntfTxlsAcks OBJECT-TYPE
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Link State Acknowledgement packets transmitted
         for this OSPF interface."
    ::= { ospfIntfRxTxStatsEntry 11 }

ospfIntfRxlsUpdates OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Link State Update packets received for 
         this OSPF interface."
    ::= { ospfIntfRxTxStatsEntry 12 }
 
ospfIntfTxlsUpdates OBJECT-TYPE
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Link State Update packets transmitted for 
         this OSPF interface."
    ::= { ospfIntfRxTxStatsEntry 13 }


ospfIntfNbrChangeStats OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfIntfNbrChangeStatsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Interface Neighbour change Statistics."
    ::= { ospfInterface 2 }

ospfIntfNbrChangeStatsEntry OBJECT-TYPE
    SYNTAX OspfIntfNbrChangeStatsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "OSPF interface Neighbour Change statistics."
    INDEX { ospfIntfNbrIndex }
    ::= { ospfIntfNbrChangeStats 1 }

OspfIntfNbrChangeStatsEntry ::= SEQUENCE {
    ospfIntfNbrIndex     	Integer32,
    ospfIntfNbrhello           	Counter32,
    ospfIntfNbrStart           	Counter32,
    ospfIntfNbrAdjointOk       	Counter32,
    ospfIntfNbrNegotiationDone 	Counter32,
    ospfIntfNbrExchangeDone     Counter32,
    ospfIntfNbrBadRequests      Counter32,
    ospfIntfNbrBadSequence      Counter32,
    ospfIntfNbrLoadingDone      Counter32,
    ospfIntfNbrN1way        	Counter32,
    ospfIntfNbrRstAd        	Counter32,
    ospfIntfNbrDown        	Counter32,
    ospfIntfNbrN2way        	Counter32
    }

ospfIntfNbrIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The index of the OSPF Interface for which these statistics apply."
    ::= { ospfIntfNbrChangeStatsEntry 1 }

ospfIntfNbrhello OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Hello packets received from neighbours
         in this OSPF interface."
    ::= { ospfIntfNbrChangeStatsEntry 2 }

ospfIntfNbrStart OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of neighbours in this state (i.e. an indication
         that  Hello packets should now be sent to the neighbour at intervals
         of HelloInterval seconds.) in this OSPF interface."
    ::= { ospfIntfNbrChangeStatsEntry  3 }

ospfIntfNbrAdjointOk OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of decisions to be made (again) as to whether
         an adjacency should be established/maintained with the neighbour.
         for this OSPF interface."
    ::= { ospfIntfNbrChangeStatsEntry 4 }

ospfIntfNbrNegotiationDone OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of neighbours in this state wherein the 
         Master/slave relationship has been negotiated, and sequence
         numbers have been exchanged, for this OSPF interface."
    ::= { ospfIntfNbrChangeStatsEntry 5 }

ospfIntfNbrExchangeDone OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of neighbours in this state (i.e. in an
         adjacency's final state) having transimitted a full sequence 
         of Database Description packets, for this OSPF interface."
    ::= { ospfIntfNbrChangeStatsEntry 6 }

ospfIntfNbrBadRequests OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Link State Requests which have been received
         for a link state advertisement not contained in the database for
         this interface."
    ::= { ospfIntfNbrChangeStatsEntry 7 }

ospfIntfNbrBadSequence OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Database Description packets which have been
         received that either 
         a) has an unexpected DD sequence number
         b) Unexpectedly has the init bit set
         c) Has an options field differing from the last Options field
            received in a Database Description packet.
         Any of these conditions indicate that some error has occured during
         adjacency establishment for this interface."
    ::= { ospfIntfNbrChangeStatsEntry 8 }

ospfIntfNbrLoadingDone OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of link state updates received for all 
         out-of-date portions of the database for this OSPF interface."
    ::= { ospfIntfNbrChangeStatsEntry 9 }

ospfIntfNbrN1way OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Hello packets received from neighbours, in
         which this router is not mentioned for this OSPF interface."
    ::= { ospfIntfNbrChangeStatsEntry 10 }

ospfIntfNbrRstAd OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total number of times the Neighbour adjacency has been reset
         on this interface."
    ::= { ospfIntfNbrChangeStatsEntry 11 }

ospfIntfNbrDown OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Neighbouring routers down (i.e. in the initial
         state of a neighbour conversation.) for this interface."
    ::= { ospfIntfNbrChangeStatsEntry 12 }

ospfIntfNbrN2way OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Hello packets received from neighbours, in
         which this router is mentioned for this OSPF interface."
    ::= { ospfIntfNbrChangeStatsEntry 13 }

ospfIntfChangeStats OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfIntfChangeStatsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Interface change Statistics."
    ::= { ospfInterface 3 }

ospfIntfChangeStatsEntry OBJECT-TYPE
    SYNTAX OspfIntfChangeStatsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "OSPF interface Change statistics."
    INDEX { ospfIntfIndex }
    ::= { ospfIntfChangeStats 1 }

OspfIntfChangeStatsEntry ::= SEQUENCE {
    ospfIntfIndex     	       	Integer32,
    ospfIntfHello           	Counter32,
    ospfIntfDown           	Counter32,
    ospfIntfLoop       		Counter32,
    ospfIntfUnloop 		Counter32,
    ospfIntfWaitTimer     	Counter32,
    ospfIntfBackup	        Counter32,
    ospfIntfNbrChange       	Counter32
    }

ospfIntfIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The index of the OSPF Interface for which these statistics apply."
    ::= { ospfIntfChangeStatsEntry 1 }

ospfIntfHello OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of Hello packets sent by this interface."
    ::= { ospfIntfChangeStatsEntry 2 }

ospfIntfDown OBJECT-TYPE
    SYNTAX   Counter32
    MAX-ACCESS   read-only
    STATUS   current
    DESCRIPTION
        "The total number of times the interface was down."
    ::= { ospfIntfChangeStatsEntry 3 }

ospfIntfLoop OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of times the interface was no longer connected to 
         the attatched network."
    ::= { ospfIntfChangeStatsEntry 4 }

ospfIntfUnloop OBJECT-TYPE
    SYNTAX   Counter32
    MAX-ACCESS   read-only
    STATUS   current
    DESCRIPTION
        "The total number of times the interface, connected back to
         the attatched network."
    ::= { ospfIntfChangeStatsEntry 5 }

ospfIntfWaitTimer OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS        read-only
    STATUS        current
    DESCRIPTION
        "The total number of times the Wait Timer has been fired,
         (indicating the end of the waiting period that is required
          before electing a (Backup) Designated Router) for this 
          OSPF interface."
    ::= { ospfIntfChangeStatsEntry 6 }

ospfIntfBackup OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS     read-only
    STATUS     current
    DESCRIPTION
        "The total number of Backup Designated Routers on the attatched
         network for this OSPF interface."
    ::= { ospfIntfChangeStatsEntry 7 }

ospfIntfNbrChange OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS     read-only
    STATUS     current
    DESCRIPTION
        "The total number of changes in the set of bidirectional neighbours
         associated with the interface for this OSPF interface."
    ::= { ospfIntfChangeStatsEntry 8 }

ospfIntfErrorStats OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfIntfErrorStatsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Interface Error Statistics."
    ::= { ospfInterface 4 }

ospfIntfErrorStatsEntry OBJECT-TYPE
    SYNTAX OspfIntfErrorStatsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Error Statistics for an OSPF area."
    INDEX { ospfIntfErrIndex }
    ::= { ospfIntfErrorStats 1 }
 
OspfIntfErrorStatsEntry ::= SEQUENCE {
    ospfIntfErrIndex     	Integer32,
    ospfIntfErrAuthFailure      Counter32,
    ospfIntfErrNetmaskMismatch  Counter32,
    ospfIntfErrHelloMismatch    Counter32,
    ospfIntfErrDeadMismatch     Counter32,
    ospfIntfErrOptionsMismatch  Counter32,
    ospfIntfErrUnknownNbr       Counter32,
    ospfIntfErrAreaMismatch     Counter32
    }

ospfIntfErrIndex OBJECT-TYPE
    SYNTAX    Integer32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The index of the OSPF Intf for which these statistics apply."
    ::= { ospfIntfErrorStatsEntry 1 }

ospfIntfErrAuthFailure OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of packets received with a wrong password in 
         this area."
    ::= { ospfIntfErrorStatsEntry 2 }

ospfIntfErrNetmaskMismatch OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of packets received with a wrong netmask in 
         this area."
    ::= { ospfIntfErrorStatsEntry 3 }

ospfIntfErrHelloMismatch OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of packets received with a different hello interval
         in this area."
    ::= { ospfIntfErrorStatsEntry 4 }

ospfIntfErrDeadMismatch OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of packets received with a different dead interval
         in this area."
    ::= { ospfIntfErrorStatsEntry 5 }

ospfIntfErrOptionsMismatch OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of packets received with a different options
         in this area."
    ::= { ospfIntfErrorStatsEntry 6 }

ospfIntfErrUnknownNbr OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of packets received from an unknown neighbor
         in this area."
    ::= { ospfIntfErrorStatsEntry 7 }

ospfIntfErrAreaMismatch OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of packets received with a wrong  area."
    ::= { ospfIntfErrorStatsEntry 8 }

-- Ospf General Statistics contains the cumulative stats for all
-- areas / interfaces
ospfCumRxPkts OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total of all OSPF packets received on all OSPF areas
         and interfaces."
    ::= { ospfCumRxTxStats 1 }
 
ospfCumTxPkts OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total of all OSPF packets transmitted on all OSPF areas
         and interfaces."
    ::= { ospfCumRxTxStats 2 }
 
ospfCumRxHello OBJECT-TYPE
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total of all Hello packets received on all OSPF areas
         and interfaces."
    ::= { ospfCumRxTxStats 3 }

ospfCumTxHello OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total of all Hello packets transmitted on all OSPF areas
         and interfaces."
    ::= { ospfCumRxTxStats 4 }
 
ospfCumRxDatabase OBJECT-TYPE
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total of all Database Description packets received on
         all OSPF areas and interfaces."
    ::= { ospfCumRxTxStats 5 }

ospfCumTxDatabase OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total of all Database Description packets transmitted on
         all OSPF areas and interfaces."
    ::= { ospfCumRxTxStats 6 }
 
ospfCumRxlsReqs OBJECT-TYPE
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total of all Link State Request packets received on
         all OSPF areas and interfaces."
    ::= { ospfCumRxTxStats 7 }

ospfCumTxlsReqs OBJECT-TYPE
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total of all Link State Request packets transmitted on
         all OSPF areas and interfaces."
    ::= { ospfCumRxTxStats 8 }

ospfCumRxlsAcks OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total of all Link State Acknowledgement packets received
         on all OSPF areas and interfaces."
    ::= { ospfCumRxTxStats 9 }
 
ospfCumTxlsAcks OBJECT-TYPE
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total of all Link State Acknowledgement packets transmitted
         on all OSPF areas and interfaces."
    ::= { ospfCumRxTxStats 10 }

ospfCumRxlsUpdates OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total of all Link State Update packets received
         on all OSPF areas and interfaces."
    ::= { ospfCumRxTxStats 11 }
 
ospfCumTxlsUpdates OBJECT-TYPE
    SYNTAX  Counter32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total of all Link State Update packets transmitted
         on all OSPF areas and interfaces."
    ::= { ospfCumRxTxStats 12 }

ospfCumNbrhello OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total of all Hello packets received from neighbours
         on all OSPF areas and interfaces."
    ::= { ospfCumNbrChangeStats 1 }

ospfCumNbrStart OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total number of neighbours in this state (i.e. an indication
         that  Hello packets should now be sent to the neighbour at intervals
         of HelloInterval seconds.) across all OSPF areas and interfaces."
    ::= { ospfCumNbrChangeStats 2 }

ospfCumNbrAdjointOk OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total number of decisions to be made (again) as to whether
         an adjacency should be established/maintained with the neighbour
         across all OSPF areas and interfaces."
    ::= { ospfCumNbrChangeStats 3 }

ospfCumNbrNegotiationDone OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total number of neighbours in this state wherein the 
         Master/slave relationship has been negotiated, and sequence
         numbers have been exchanged, across all OSPF areas and 
         interfaces."
    ::= { ospfCumNbrChangeStats 4 }

ospfCumNbrExchangeDone OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total number of neighbours in this state (i.e. in an
         adjacency's final state) having transimitted a full sequence 
         of Database Description packets, across all OSPF areas
         and interfaces."
    ::= { ospfCumNbrChangeStats 5 }

ospfCumNbrBadRequests OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total number of Link State Requests which have been received
         for a link state advertisement not contained in the database across
         all interfaces and OSPF areas."
    ::= { ospfCumNbrChangeStats 6 }

ospfCumNbrBadSequence OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total number of Database Description packets which have been
         received that either 
         a) has an unexpected DD sequence number
         b) Unexpectedly has the init bit set
         c) Has an options field differing from the last Options field
            received in a Database Description packet.
         Any of these conditions indicate that some error has occured during
         adjacency establishment for all OSPF areas and interfaces."
    ::= { ospfCumNbrChangeStats 7 }

ospfCumNbrLoadingDone OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total number of link state updates received for all 
         out-of-date portions of the database across all OSPF areas
         and interfaces."
    ::= { ospfCumNbrChangeStats 8 }

ospfCumNbrN1way OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total number of Hello packets received from neighbours, in
         which this router is not mentioned across all OSPF interfaces
         and areas."
    ::= { ospfCumNbrChangeStats 9 }

ospfCumNbrRstAd OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total number of times the Neighbour adjacency has been reset
         across all OPSF areas and interfaces."
    ::= { ospfCumNbrChangeStats 10 }

ospfCumNbrDown OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of Neighbouring routers down (i.e. in the initial
         state of a neighbour conversation.) across all OSPF areas and 
         interfaces."
    ::= { ospfCumNbrChangeStats 11 }

ospfCumNbrN2way OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The sum total number of Hello packets received from neighbours, in
         which this router is mentioned across all OSPF interfaces
         and areas."
    ::= { ospfCumNbrChangeStats 12 }

ospfCumIntfHello OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The sum total number of Hello packets sent on all interfaces 
         and areas"
    ::= { ospfCumIntfChangeStats 1 }

ospfCumIntfDown OBJECT-TYPE
    SYNTAX   Counter32
    MAX-ACCESS   read-only
    STATUS   current
    DESCRIPTION
        "The sum total number of interfaces down in all OSPF areas."
    ::= { ospfCumIntfChangeStats 2 }

ospfCumIntfLoop OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The sum total of interfaces no longer connected to 
         the attatched network across all OSPF areas and interfaces."
    ::= { ospfCumIntfChangeStats 3 }

ospfCumIntfUnloop OBJECT-TYPE
    SYNTAX   Counter32
    MAX-ACCESS   read-only
    STATUS   current
    DESCRIPTION
        "The sum total number of interfaces, connected to
         the attatched network in all OSPF areas."
    ::= { ospfCumIntfChangeStats 4 }

ospfCumIntfWaitTimer OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS        read-only
    STATUS        current
    DESCRIPTION
        "The sum total number of times the Wait Timer has been fired,
         (indicating the end of the waiting period that is required
          before electing a (Backup) Designated Router) across all 
          OSPF areas and interfaces."
    ::= { ospfCumIntfChangeStats 5 }

ospfCumIntfBackup OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS     read-only
    STATUS     current
    DESCRIPTION
        "The sum total number of Backup Designated Routers on the attatched
         network for all OSPF areas and interfaces."
    ::= { ospfCumIntfChangeStats 6 }

ospfCumIntfNbrChange OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS     read-only
    STATUS     current
    DESCRIPTION
        "The sum total number of changes in the set of bidirectional
         neighbours associated with any interface across all OSPF areas."
    ::= { ospfCumIntfChangeStats 7 }

ospfTmrsKckOffHello OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The sum total number of times the Hello timer has been fired
         (which triggers the send of a Hello packet) across all OPSF 
         areas and interfaces."
    ::= { ospfTimersKickOffStats 1 }

ospfTmrsKckOffRetransmit OBJECT-TYPE
    SYNTAX   Counter32
    MAX-ACCESS   read-only
    STATUS   current
    DESCRIPTION
        "The sum total number of times the Retransmit timer has been
         fired across all OPSF areas and interfaces."
    ::= { ospfTimersKickOffStats 2 }

ospfTmrsKckOffLsaLock OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The sum total number of times the Lsa Lock timer has been 
         fired across all OSPF areas and interfaces."
    ::= { ospfTimersKickOffStats 3 }

ospfTmrsKckOffLsaAck OBJECT-TYPE
    SYNTAX   Counter32
    MAX-ACCESS   read-only
    STATUS   current
    DESCRIPTION
        "The sum total number of times the Lsa Ack timer has been 
         fired across all ospf areas and interfaces."
    ::= { ospfTimersKickOffStats 4 }

ospfTmrsKckOffDbage OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS        read-only
    STATUS        current
    DESCRIPTION
        "The total number of times the Dbage has been fired."
    ::= { ospfTimersKickOffStats 5 }

ospfTmrsKckOffSummary OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS     read-only
    STATUS     current
    DESCRIPTION
        "The total number of times the Summary timer has been fired."
    ::= { ospfTimersKickOffStats 6 }

ospfTmrsKckOffAseExport OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS     read-only
    STATUS     current
    DESCRIPTION
        "The total number of times the ASE Export timer has been fired."
    ::= { ospfTimersKickOffStats 7 }

-- IP statistics

ipStatsInReceives OBJECT-TYPE
    SYNTAX         Counter32
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
        "ip InReceive"
    ::= { ipStats 1 }

ipStatsInHdrErrors OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "ip InHdrError"
    ::= { ipStats 2 }

ipStatsInAddrErrors OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "ip InAddrErrors"
    ::= { ipStats 3 }

ipStatsInUnknownProtos OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "ip InUnknownProtos"
    ::= { ipStats 4 }

ipStatsInDiscards OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "ip InDiscards"
    ::= { ipStats 5 }

ipStatsInDelivers OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "ip InDelivers"
    ::= { ipStats 6 }

ipStatsOutRequests OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "ip OutRequests"
    ::= { ipStats 7 }

ipStatsOutDiscards OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "ip OutDiscards"
    ::= { ipStats 8 }

ipStatsDefaultTTL OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "ip DefaultTTL"
    ::= { ipStats 9 }

-- IGMP Snooping statistics
igmpSnoopStats OBJECT-TYPE
    SYNTAX SEQUENCE OF IgmpSnoopStatsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Interface Error Statistics."
    ::= { igmpStats 1 }

igmpSnoopStatsEntry OBJECT-TYPE
    SYNTAX IgmpSnoopStatsEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Statistics for IGMP Snooping."
    INDEX { igmpSnoopVlanIndex }
    ::= { igmpSnoopStats 1 }
 
IgmpSnoopStatsEntry ::= SEQUENCE {
    igmpSnoopVlanIndex     	Integer32,
    rxIgmpValidPkts             Counter32,
    rxIgmpInvalidPkts           Counter32,
    rxIgmpGenQueries            Counter32,
    rxIgmpGrpSpecificQueries    Counter32,
    rxIgmpLeaves                Counter32,
    rxIgmpReports               Counter32,
    txIgmpGrpSpecificQueries    Counter32,
    txIgmpReports               Counter32,
    txIgmpLeaves                         Counter32,
    rxIgmpGroupSourceSpecificQueries     Counter32,
    rxIgmpV3CurrentStateRecords          Counter32,
    rxIgmpV3SourceListChangeRecords      Counter32,
    rxIgmpV3FilterChangeRecords          Counter32
    }

igmpSnoopVlanIndex OBJECT-TYPE
    SYNTAX    Integer32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The index of the VLAN for which these statistics apply."
    ::= { igmpSnoopStatsEntry 1 }

rxIgmpValidPkts OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of valid IGMP packets received 
         on this VLAN." 
    ::= { igmpSnoopStatsEntry 2 }

rxIgmpInvalidPkts OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of invalid IGMP packets received 
         on this VLAN." 
    ::= { igmpSnoopStatsEntry 3 }

rxIgmpGenQueries OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of IGMP General Query packets received
         on this VLAN." 
    ::= { igmpSnoopStatsEntry 4 }

rxIgmpGrpSpecificQueries OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of IGMP Group Specific Query packets received
         on this VLAN." 
    ::= { igmpSnoopStatsEntry 5 }

rxIgmpLeaves OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of IGMP Leave packets received
         on this VLAN." 
    ::= { igmpSnoopStatsEntry 6 }

rxIgmpReports OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of IGMP Report packets received
         on this VLAN." 
    ::= { igmpSnoopStatsEntry 7 }

txIgmpGrpSpecificQueries OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of IGMP Group Specific Query packets
         transmitted on this VLAN." 
    ::= { igmpSnoopStatsEntry 8 }

txIgmpReports OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of IGMP Report packets transmitted
         on this VLAN." 
    ::= { igmpSnoopStatsEntry 9 }

txIgmpLeaves OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of IGMP Leave packets transmitted
         on this VLAN." 
    ::= { igmpSnoopStatsEntry 10 }

rxIgmpGroupSourceSpecificQueries OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of IGMP Group Source Specific (GSSQ) Queries received
         on this VLAN."
    ::= { igmpSnoopStatsEntry 11 }

rxIgmpV3CurrentStateRecords OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of IGMP Current State Records (CSRs) received
         on this VLAN."
    ::= { igmpSnoopStatsEntry 12 }

rxIgmpV3SourceListChangeRecords OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of IGMP Source List Change Records (SLCRs) received
         on this VLAN."
    ::= { igmpSnoopStatsEntry 13 }

rxIgmpV3FilterChangeRecords OBJECT-TYPE
    SYNTAX    Counter32
    MAX-ACCESS    read-only
    STATUS    current
    DESCRIPTION
        "The total number of IGMP Filter Mode Change Records (FMCRs) received
         on this VLAN."
    ::= { igmpSnoopStatsEntry 14 }

-- Information - Run-time IP Route Table 

ipRouteInfoTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF IpRouteInfoEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of run-time IP routes."
    ::= { ipRoutingInfo 1 }

ipRouteInfoEntry OBJECT-TYPE
    SYNTAX  IpRouteInfoEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the run-time IP route table"
    INDEX   { ipRouteInfoIndx }
    ::= { ipRouteInfoTable 1 }

IpRouteInfoEntry ::= SEQUENCE {
    ipRouteInfoIndx	        Integer32,
    ipRouteInfoDestIp           IpAddress,
    ipRouteInfoMask             IpAddress,
    ipRouteInfoGateway          IpAddress,
    ipRouteInfoTag       	INTEGER,
    ipRouteInfoType       	INTEGER,
    ipRouteInfoInterface        Integer32,
    ipRouteInfoMetric           Integer32
    }

ipRouteInfoIndx OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The index of this route table."
    ::= { ipRouteInfoEntry 1 }

ipRouteInfoDestIp OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The destination IP address of this route."
    ::= { ipRouteInfoEntry 2 }

ipRouteInfoMask OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The destination IP mask of this route."
    ::= { ipRouteInfoEntry 3 }
 
ipRouteInfoGateway OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The next-hop router address for this route."
    ::= { ipRouteInfoEntry 4 }

ipRouteInfoTag OBJECT-TYPE
    SYNTAX  INTEGER {
	fixed(1),
  	static(2),
	addr(3),
	rip(4),
	broadcast(5),
	martian(6),
	multicast(7),
        ospf(10),
        none(11)
	}
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The tag-type for this route."
    ::= { ipRouteInfoEntry 5 }

ipRouteInfoType OBJECT-TYPE 
    SYNTAX  INTEGER {
	indirect(1),
	direct(2),
	local(3),
	broadcast(4),
	martian(5),
	multicast(6),
	other(7)
	}
    MAX-ACCESS  read-only 
    STATUS  current 
    DESCRIPTION 
        "The type of the route." 
    ::= { ipRouteInfoEntry 6 }

ipRouteInfoInterface OBJECT-TYPE 
    SYNTAX  Integer32
    MAX-ACCESS  read-only 
    STATUS  current 
    DESCRIPTION 
        "The interface number for which the destination	address is applicable."
    ::= { ipRouteInfoEntry 7 }

ipRouteInfoMetric  OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The metric of this route."
    ::= { ipRouteInfoEntry 8 }

routeTableClear OBJECT-TYPE
    SYNTAX  INTEGER {
        ok(1),
        clear(2)
        }
    MAX-ACCESS  read-write
    STATUS  current 
    DESCRIPTION
        "Setting this value to clear(2) clears the route table."
    ::= { ipRoutingInfo 2 }

-- Run Time ARP Table

arpInfoTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF AgArpInfoEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of ARP entries."
    ::= { arpInfo 1 }

arpInfoEntry OBJECT-TYPE
    SYNTAX  AgArpInfoEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the ARP table"
    INDEX   { arpInfoDestIp }
    ::= { arpInfoTable 1 }

AgArpInfoEntry ::= SEQUENCE {
    arpInfoDestIp         IpAddress,
    arpInfoMacAddr        PhysAddress,
    arpInfoVLAN        	  Integer32,
    arpInfoSrcPort        Integer32,
    arpInfoFlag           INTEGER
    }

arpInfoDestIp OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The destination IP address of the ARP entry."
    ::= { arpInfoEntry 1 }

arpInfoMacAddr OBJECT-TYPE
    SYNTAX  PhysAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The MAC address for the ARP entry."
    ::= { arpInfoEntry 2 }

arpInfoVLAN OBJECT-TYPE 
    SYNTAX  Integer32 
    MAX-ACCESS  read-only 
    STATUS  current 
    DESCRIPTION 
        "The VLAN identifier for the ARP entry." 
    ::= { arpInfoEntry 3 }

arpInfoSrcPort OBJECT-TYPE  
    SYNTAX  Integer32 
    MAX-ACCESS  read-only  
    STATUS  current  
    DESCRIPTION  
        "The  port number on which this entry's equivalence is effective."  
    ::= { arpInfoEntry 4 }


arpInfoFlag OBJECT-TYPE   
    SYNTAX  INTEGER {
	clear(1),
	unresolved(2),
	permanent(3),
	indirect(4)
	}
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The flag associated with this ARP entry."   
    ::= { arpInfoEntry 6 }

arpCacheClear OBJECT-TYPE
    SYNTAX  INTEGER {
        ok(1),
        clear(2)
        }
    MAX-ACCESS  read-write
    STATUS  current 
    DESCRIPTION
        "Setting this value to clear(2) clears the ARP cache."
    ::= { arpInfo 2 }

-- igmp snooping info table
igmpInfoTable OBJECT-TYPE
    SYNTAX SEQUENCE OF IgmpInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of IGMP group membership information."
    ::= { igmpInfo 1 }

igmpInfoEntry OBJECT-TYPE
    SYNTAX IgmpInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about an IGMP group member ."
    INDEX { igmpInfoIndex }
    ::= { igmpInfoTable 1 }
 
IgmpInfoEntry ::= SEQUENCE {
    igmpInfoIndex             Integer32,
    igmpInfoGroupId   	      IpAddress,
    igmpInfoVlanId   	      Integer32,
    igmpInfoVersion   	      INTEGER,
    igmpInfoPortNum           Integer32,
    igmpInfoExpires           DisplayString,
    igmpInfoMode              INTEGER,
    igmpInfoSourceIp          IpAddress,
    igmpInfoFwd               INTEGER
    }
 
igmpInfoIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The igmp group number for which the IGMP info table is related."
    ::= { igmpInfoEntry 1}

igmpInfoGroupId OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The IP address of the IGMP group." 
    ::= { igmpInfoEntry 2}

igmpInfoVlanId OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The VLAN ID for this IGMP group." 
    ::= { igmpInfoEntry 3}



igmpInfoVersion OBJECT-TYPE
    SYNTAX INTEGER { 
        v3(1),
        v2(2),
        v1(3)
	}
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The Version of IGMP host." 
    ::= { igmpInfoEntry 5}

igmpInfoPortNum OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The Version of IGMP host." 
    ::= { igmpInfoEntry 6 }

igmpInfoExpires OBJECT-TYPE
    SYNTAX DisplayString 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The expiration time for this host." 
    ::= { igmpInfoEntry 7 }

igmpInfoMode OBJECT-TYPE
    SYNTAX INTEGER {
        exclude(1),
        include(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The IGMPv3 filter-mode for this host."
    ::= { igmpInfoEntry 8 }

igmpInfoSourceIp OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The source IP address of the IGMP group."
    ::= { igmpInfoEntry 9 }

igmpInfoFwd OBJECT-TYPE
    SYNTAX INTEGER {
        yes(1),
        no(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The IGMPv3 forwarding for this source/group IP for this host."
    ::= { igmpInfoEntry 10 }


igmpMrtrInfoTable OBJECT-TYPE
    SYNTAX SEQUENCE OF IgmpMrtrInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of IGMP mrouters."
    ::= { igmpInfo 2 }

igmpMrtrInfoEntry OBJECT-TYPE
    SYNTAX IgmpMrtrInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about an IGMP mrouter."
    INDEX { igmpMrtrInfoIndex }
    ::= { igmpMrtrInfoTable 1 }
 
IgmpMrtrInfoEntry ::= SEQUENCE {
    igmpMrtrInfoIndex         Integer32,
    igmpMrtrInfoVlanId        Integer32,
    igmpMrtrInfoPortId        Integer32,
    igmpMrtrInfoVersion       Integer32,
    igmpMrtrInfoExpires       DisplayString,
    igmpMrtrInfoMrt           Integer32,
    igmpMrtrInfoQrv           INTEGER,
    igmpMrtrInfoQqic          INTEGER
    }
 
igmpMrtrInfoIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The mrouter number for which the IGMP mrouter info table is related."
    ::= { igmpMrtrInfoEntry 1}

igmpMrtrInfoVlanId OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The VLAN ID on which this IGMP mrouter is attached." 
    ::= { igmpMrtrInfoEntry 2}

igmpMrtrInfoPortId OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The port on which this IGMP mrouter is attached." 
    ::= { igmpMrtrInfoEntry 3}

igmpMrtrInfoVersion OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The version of this IGMP mrouter." 
    ::= { igmpMrtrInfoEntry 4}

igmpMrtrInfoExpires OBJECT-TYPE
    SYNTAX DisplayString 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The expiration time for this mrouter." 
    ::= { igmpMrtrInfoEntry 5 }

igmpMrtrInfoMrt OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The Maximum Query Response time of this IGMP mrouter." 
    ::= { igmpMrtrInfoEntry 6 }

igmpMrtrInfoQrv OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The Querier Robustness value of this IGMP mrouter."
    ::= { igmpMrtrInfoEntry 7 }

igmpMrtrInfoQqic OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The Querier query interval code of this IGMP mrouter."
    ::= { igmpMrtrInfoEntry 8 }

-- RIP Information

rip2GeneralInfo	OBJECT IDENTIFIER ::= { rip2Info 1 }

ripInfoState OBJECT-TYPE
    SYNTAX INTEGER {
        on(1),
        off(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"RIP global state."
    ::= { rip2GeneralInfo 1 }

ripInfoUpdatePeriod OBJECT-TYPE
    SYNTAX  INTEGER  (1..120)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Update Period in seconds."
    ::= { rip2GeneralInfo 2 }

rip2InfoIntfTable OBJECT-TYPE
    SYNTAX SEQUENCE OF RipInfoIntfEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The information table of RIP."
    ::= { rip2Info 2 }

ripInfoIntfEntry OBJECT-TYPE
    SYNTAX RipInfoIntfEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about  RIP on IP interface."
    INDEX { ripInfoIntfIndex }
    ::= { rip2InfoIntfTable 1 }
 
RipInfoIntfEntry ::= SEQUENCE {
    ripInfoIntfIndex  	      Integer32,
    ripInfoIntfVersion	      INTEGER,
    ripInfoIntfAddress        IpAddress,
    ripInfoIntfState	      INTEGER,
    ripInfoIntfListen	      INTEGER,
    ripInfoIntfTrigUpdate     INTEGER,
    ripInfoIntfMcastUpdate    INTEGER,
    ripInfoIntfPoisonReverse  INTEGER,
    ripInfoIntfSupply         INTEGER,
    ripInfoIntfMetric         INTEGER, 
    ripInfoIntfAuth           INTEGER, 
    ripInfoIntfKey            DisplayString,
    ripInfoIntfDefault	      INTEGER
    }
 
ripInfoIntfIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The interface number for which the RIP information is related."
    ::= { ripInfoIntfEntry 1 }

ripInfoIntfVersion OBJECT-TYPE
    SYNTAX INTEGER {
        ripVersion1(1),
        ripVersion2(2),
        ripVersionBoth(3)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "RIP version."
    ::= { ripInfoIntfEntry 2 }

ripInfoIntfAddress OBJECT-TYPE
    SYNTAX  IpAddress 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The interface address."
    ::= { ripInfoIntfEntry 3 } 

ripInfoIntfState OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The status of RIP protocol."
    ::= { ripInfoIntfEntry 4 }

ripInfoIntfListen OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The status of listening to route updates."
    ::= { ripInfoIntfEntry 5 }
 
ripInfoIntfTrigUpdate OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The status of triggered updates."
    ::= { ripInfoIntfEntry 6 }

ripInfoIntfMcastUpdate OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The status of multicast updates."
    ::= { ripInfoIntfEntry 7 }

ripInfoIntfPoisonReverse OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The status of RIP poison reverse."
    ::= { ripInfoIntfEntry 8 }

ripInfoIntfSupply OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The status of supplying route updates."
    ::= { ripInfoIntfEntry 9 }

ripInfoIntfMetric OBJECT-TYPE
    SYNTAX  INTEGER (1..15)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "RIP route metric for this interface."
    ::= { ripInfoIntfEntry 10 }

ripInfoIntfAuth OBJECT-TYPE
    SYNTAX INTEGER {
        none(1),
        password(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The type of Authentication used on this interface."
    ::= { ripInfoIntfEntry 11 }

ripInfoIntfKey OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..16))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "RIP update authentication password."
    ::= { ripInfoIntfEntry 12 }

ripInfoIntfDefault OBJECT-TYPE
    SYNTAX  INTEGER {
        both(1),
        listen(2),
        supply(3),
        none(4)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Specifies what RIP does with default routes."
    ::= { ripInfoIntfEntry 13 }


-- IP Interface Information

ipInfoRouterID OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Router ID information."
    ::= { ipInfo 1 }

ipIntfInfoTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF IntfInfoEntry
    MAX-ACCESS not-accessible
    STATUS current 
    DESCRIPTION
        "The table of IP interface information."
    ::= { ipInfo 2 }

intfInfoEntry OBJECT-TYPE
    SYNTAX  IntfInfoEntry 
    MAX-ACCESS not-accessible
    STATUS  current 
    DESCRIPTION
        "A row in IP interface information table."
    INDEX   { intfInfoIndex }
    ::= { ipIntfInfoTable 1 }

IntfInfoEntry ::= SEQUENCE {
    intfInfoIndex         Integer32,
    intfInfoAddr          DisplayString,
    intfInfoNetMask       DisplayString,
    intfInfoBcastAddr     DisplayString,
    intfInfoVlan          Integer32,
    intfInfoStatus        INTEGER
    }

intfInfoIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	"The interface number for which the information is related."
    ::= { intfInfoEntry 1 }

intfInfoAddr  OBJECT-TYPE
    SYNTAX    DisplayString
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	"The IP address of the interface."
    ::= { intfInfoEntry 2 }

intfInfoNetMask OBJECT-TYPE
    SYNTAX   DisplayString
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The subnet mask of the interface."
    ::= { intfInfoEntry 3 }

intfInfoBcastAddr OBJECT-TYPE
    SYNTAX   DisplayString
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The broadcast address of the interface."
    ::= { intfInfoEntry 4 }

intfInfoVlan OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The VLAN number for this interface."
    ::= { intfInfoEntry 5 }

intfInfoStatus OBJECT-TYPE
    SYNTAX  INTEGER {
	up(1),
	down(2),
        disabled(3)
    }  
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	"The status of the interface."
    ::= { intfInfoEntry 6 }

-- IP Gateway Information

gatewayInfoTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF GatewayInfoEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table containing information for the default gateways."
    ::= { ipInfo 3 }

gatewayInfoEntry OBJECT-TYPE
    SYNTAX  GatewayInfoEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the gateway information table"
    INDEX   { gatewayInfoIndex }
    ::= { gatewayInfoTable 1 }

GatewayInfoEntry ::= SEQUENCE {
    gatewayInfoIndex         Integer32,
    gatewayInfoAddr          IpAddress,
    gatewayInfoVlan          Integer32,
    gatewayInfoStatus        INTEGER
    }

gatewayInfoIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The gateway number for which the information is related."
    ::= { gatewayInfoEntry 1}

gatewayInfoAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IP address of the default gateway."
    ::= { gatewayInfoEntry 2 }

gatewayInfoVlan OBJECT-TYPE
    SYNTAX  Integer32 (0..4090)   
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The VLAN number for this gateway (0 for any)."
    ::= { gatewayInfoEntry 3 }

gatewayInfoStatus OBJECT-TYPE
    SYNTAX  INTEGER {
        up(1),
        failed(2)
	}  
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The status of the default gateway."
    ::= { gatewayInfoEntry 4 }

ipInfoBootpRelayState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(2),
        disabled(3)
    }	
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The state of BOOTP relay."
    ::= { ipInfo 4 }

ipInfoBootpRelayAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IP address of BOOTP server."
    ::= { ipInfo 5 }

ipInfoBootpRelayAddr2 OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IP address of second BOOTP server."
    ::= { ipInfo 6 }

ipInfoFwdState OBJECT-TYPE
    SYNTAX  INTEGER { 
	on(1),
	off(2)
    }	
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "IP forwarding global state." 
    ::= { ipInfo 7 }

ipInfoFwdDirectedBcast OBJECT-TYPE
    SYNTAX  INTEGER { 
        enabled(2),
        disabled(3)
    }	
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The state of forwarding directed broadcasts."
    ::= { ipInfo 8 }

ipInfoNwfTable OBJECT-TYPE
    SYNTAX SEQUENCE OF IpInfoNwfEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of IP network filter information."
    ::= { ipInfo 9 }

ipInfoNwfEntry OBJECT-TYPE
    SYNTAX IpInfoNwfEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "A row in the IP network filter information table."
    INDEX { ipInfoNwfIndex }
    ::= { ipInfoNwfTable 1 }
 
IpInfoNwfEntry ::= SEQUENCE {
    ipInfoNwfIndex     Integer32,
    ipInfoNwfAddr      IpAddress,
    ipInfoNwfMask      IpAddress,
    ipInfoNwfState     INTEGER
    }
 
ipInfoNwfIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The netowrk filter number for which the NWF is related."
    ::= { ipInfoNwfEntry 1}

ipInfoNwfAddr OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The IP address of the network filter."
    ::= { ipInfoNwfEntry 2 }

ipInfoNwfMask OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current  
    DESCRIPTION
	"The subnet mask of the network filter."
    ::= { ipInfoNwfEntry 3 }

ipInfoNwfState OBJECT-TYPE
    SYNTAX INTEGER { 
        enabled(1),
        disabled(2)
	}
    MAX-ACCESS  read-only
    STATUS  current  
    DESCRIPTION
	"The state of the network filter."
    ::= { ipInfoNwfEntry 4 }


-- IP Route Map Information

ipInfoRmapTable OBJECT-TYPE
    SYNTAX SEQUENCE OF IpInfoRmapEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of IP route map information."
    ::= { ipInfo 10 }

ipInfoRmapEntry OBJECT-TYPE
    SYNTAX IpInfoRmapEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about an IP route map."
    INDEX { ipInfoRmapIndex }
    ::= { ipInfoRmapTable 1 }
 
IpInfoRmapEntry ::= SEQUENCE {
    ipInfoRmapIndex		Integer32,
    ipInfoRmapLp	  	Unsigned32,
    ipInfoRmapMetric	  	Unsigned32,
    ipInfoRmapPrec	  	INTEGER,
    ipInfoRmapWeight	 	INTEGER, 
    ipInfoRmapState     	INTEGER,
    ipInfoRmapAp		DisplayString,
    ipInfoRmapMetricType	INTEGER
    }
 
ipInfoRmapIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The route map number for which the RMAP is related."
    ::= { ipInfoRmapEntry 1}

ipInfoRmapLp OBJECT-TYPE
    SYNTAX Unsigned32 (0..4294967295) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The local-preference of the route map. 4294967295 means none"
    ::= { ipInfoRmapEntry 2 }

ipInfoRmapMetric OBJECT-TYPE
    SYNTAX Unsigned32 (0..4294967295) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The metric of the route map. 4294967295 means none"
    ::= { ipInfoRmapEntry 3 }

ipInfoRmapPrec OBJECT-TYPE
    SYNTAX INTEGER (1..255) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The precedence of the route map."
    ::= { ipInfoRmapEntry 4 }

ipInfoRmapWeight OBJECT-TYPE
    SYNTAX INTEGER (0..65535) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The weight of the route map. 65535 means none"
    ::= { ipInfoRmapEntry 5 }

ipInfoRmapState OBJECT-TYPE
    SYNTAX INTEGER { 
        enabled(1),
        disabled(2)
	}
    MAX-ACCESS  read-only
    STATUS  current  
    DESCRIPTION
	"Enable or disable the route map."
    ::= { ipInfoRmapEntry 6 }

ipInfoRmapAp OBJECT-TYPE
    SYNTAX DisplayString (SIZE(0..17)) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The as-path prepend of the matched route. Up to 3 AS number can be 
	 displayed for the string. 
	 The usuage is:<AS number> [<AS number>][ <AS number>]"
    ::= { ipInfoRmapEntry 7 }

ipInfoRmapMetricType OBJECT-TYPE
    SYNTAX INTEGER {
        none(1),
        type1(2),
        type2(3)
        }
    MAX-ACCESS  read-only
    STATUS  current  
    DESCRIPTION
	"The OSPF metric-type of the matched route."
    ::= { ipInfoRmapEntry 8 }

-- IP OSPF Information

ipOspfInfo OBJECT IDENTIFIER
    ::= { ipInfo 11 }

ipOspfInfoState OBJECT-TYPE
    SYNTAX INTEGER {
        on(1),
        off(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"OSPF global state."
    ::= { ipOspfInfo 1 }

ipOspfInfoDefaultRouteMetric OBJECT-TYPE
    SYNTAX INTEGER (0..16777215)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The metric to be assigned."
    ::= { ipOspfInfo 2 }

ipOspfInfoDefaultRouteMetricType OBJECT-TYPE
    SYNTAX INTEGER {
        none(1),
        type1(2),
        type2(3)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The AS External metric type to be assigned."
    ::= { ipOspfInfo 3 }

ipOspfInfoRouterID OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The router ID of the switch." 
    ::= { ipOspfInfo 4 }

ipOspfInfoLsdbLimit OBJECT-TYPE
    SYNTAX  INTEGER (0..2000)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The LSDB limit for external LSA." 
    ::= { ipOspfInfo 5 }

-- IP OSPF Area Information
ipOspfAreaInfoTable OBJECT-TYPE
    SYNTAX SEQUENCE OF IpOspfAreaInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Area Information."
    ::= { ipOspfInfo 6 }

ipOspfAreaInfoEntry OBJECT-TYPE
    SYNTAX IpOspfAreaInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about a OSPF area."
    INDEX { ipOspfAreaInfoIndex, ipOspfAreaInfoId }
    ::= { ipOspfAreaInfoTable 1 }
 
IpOspfAreaInfoEntry ::= SEQUENCE {
    ipOspfAreaInfoIndex         Integer32,
    ipOspfAreaInfoId            IpAddress,
    ipOspfAreaInfoSpfInterval   INTEGER,
    ipOspfAreaInfoAuthType      INTEGER,
    ipOspfAreaInfoType 	        INTEGER,
    ipOspfAreaInfoMetric	INTEGER,
    ipOspfAreaInfoStatus        INTEGER
    }

ipOspfAreaInfoIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The OSPF area number for which the OSPF area table is related."
    ::= { ipOspfAreaInfoEntry 1 }

ipOspfAreaInfoId OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The IP Address of the OSPF area." 
    ::= { ipOspfAreaInfoEntry 2 }

ipOspfAreaInfoSpfInterval OBJECT-TYPE
    SYNTAX INTEGER (1..255) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The SPF interval for the OSPF area." 
    ::= { ipOspfAreaInfoEntry 3 }

ipOspfAreaInfoAuthType OBJECT-TYPE
    SYNTAX  INTEGER {
        none(1),
        password(2),
	md5(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Type of authentication being used.
	 none(1) - no authentication
	 password(2) - use password
	 md5(3) - use MD5 authentication."
    ::= { ipOspfAreaInfoEntry 4 }

ipOspfAreaInfoType OBJECT-TYPE
	SYNTAX INTEGER {
	    transit(0),
	    stub(1),
	    nssa(2)
           }
	MAX-ACCESS   read-only
	STATUS  current
	DESCRIPTION
	    "Type of Area.
	    transit(0)
	    stub(1)
	    nssa(2)"
	::= { ipOspfAreaInfoEntry 5 }
	
ipOspfAreaInfoMetric OBJECT-TYPE
    SYNTAX  INTEGER (1..65535)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Metric (1-65535)"
    ::= { ipOspfAreaInfoEntry 6 }

ipOspfAreaInfoStatus OBJECT-TYPE
    SYNTAX  INTEGER {
        disabled(0), 
	 enabled(1)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Status
	   disabled(0)
	   enabled(1)"
    ::= { ipOspfAreaInfoEntry 7 }


-- IP OSPF Range Information
ipOspfRangeInfoTable OBJECT-TYPE
    SYNTAX SEQUENCE OF IpOspfRangeInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF summary range information."
    ::= { ipOspfInfo 7 }

ipOspfRangeInfoEntry OBJECT-TYPE
    SYNTAX IpOspfRangeInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about an OSPF summary range."
    INDEX { ipOspfRangeInfoIndex }
    ::= { ipOspfRangeInfoTable 1 }

IpOspfRangeInfoEntry ::= SEQUENCE {
    ipOspfRangeInfoIndex            Integer32,
    ipOspfRangeInfoAddr             IpAddress,
    ipOspfRangeInfoMask             IpAddress,
    ipOspfRangeInfoAreaIndex        Integer32,
    ipOspfRangeInfoHideState        INTEGER,
    ipOspfRangeInfoState            INTEGER
    }

ipOspfRangeInfoIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The range number for which the OSPF summary range table is related."
    ::= { ipOspfRangeInfoEntry 1}

ipOspfRangeInfoAddr OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The IP Address of the range."
    ::= { ipOspfRangeInfoEntry 2 }

ipOspfRangeInfoMask OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The mask of the range."
    ::= { ipOspfRangeInfoEntry 3 }

ipOspfRangeInfoAreaIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The area index."
    ::= { ipOspfRangeInfoEntry 4 }

ipOspfRangeInfoHideState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The state of the hide range."
    ::= { ipOspfRangeInfoEntry 5 }

ipOspfRangeInfoState OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The state of the range."
    ::= { ipOspfRangeInfoEntry 6 }


-- IP OSPF Interface Information
ipOspfIntfInfoTable OBJECT-TYPE
    SYNTAX SEQUENCE OF IpOspfIntfInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Interface Information."
    ::= { ipOspfInfo 8 }

ipOspfIntfInfoEntry OBJECT-TYPE
    SYNTAX IpOspfIntfInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about an OSPF Interface."
    INDEX { ipOspfIntfInfoIndex }
    ::= { ipOspfIntfInfoTable 1 }
 
IpOspfIntfInfoEntry ::= SEQUENCE {
    ipOspfIntfInfoIndex         Integer32,
    ipOspfIntfInfoId            IpAddress,
    ipOspfIntfInfoArea          INTEGER,
    ipOspfIntfInfoMdkey         INTEGER, 
    ipOspfIntfInfoCost          INTEGER,
    ipOspfIntfInfoPrio          INTEGER,
    ipOspfIntfInfoHello         INTEGER,
    ipOspfIntfInfoDead          INTEGER,
    ipOspfIntfInfoTrans         INTEGER,
    ipOspfIntfInfoRetra         INTEGER,
    ipOspfIntfInfoAuthKey       DisplayString,
    ipOspfIntfInfoStatus        INTEGER

}

ipOspfIntfInfoIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The OSPF Interface number for which the OSPF Interface table is related."
    ::= { ipOspfIntfInfoEntry 1}

ipOspfIntfInfoId OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The IP Address of the OSPF interface." 
    ::= { ipOspfIntfInfoEntry 2 }

ipOspfIntfInfoArea OBJECT-TYPE
    SYNTAX INTEGER (0..2) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The index of the area that the interface belongs" 
    ::= { ipOspfIntfInfoEntry 3 }

ipOspfIntfInfoMdkey OBJECT-TYPE
    SYNTAX INTEGER (0..255) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The MD5 key for the OSPF interface
         0 (none) no MD5 authentication." 
    ::= { ipOspfIntfInfoEntry 4 }

ipOspfIntfInfoCost  OBJECT-TYPE 
    SYNTAX INTEGER (1..65535) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Interface cost" 
    ::= { ipOspfIntfInfoEntry 5 }

ipOspfIntfInfoPrio   OBJECT-TYPE
   SYNTAX INTEGER (1..255) 
    MAX-ACCESS read-only
    STATUS current 
    DESCRIPTION
	"Interface router priority" 
    ::= { ipOspfIntfInfoEntry 6 }

ipOspfIntfInfoHello  OBJECT-TYPE 
    SYNTAX INTEGER (1..65535) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Hello interval" 
    ::= { ipOspfIntfInfoEntry 7 }

ipOspfIntfInfoDead   OBJECT-TYPE
   SYNTAX INTEGER (1..65535) 
    MAX-ACCESS read-only
    STATUS current 
    DESCRIPTION
	"Dead interval" 
    ::= { ipOspfIntfInfoEntry 8 }

ipOspfIntfInfoTrans  OBJECT-TYPE
   SYNTAX INTEGER (1..3600) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Transit delay" 
    ::= { ipOspfIntfInfoEntry 9 }
	
ipOspfIntfInfoRetra OBJECT-TYPE
    SYNTAX INTEGER (1..3600) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Retransmit interval" 
    ::= { ipOspfIntfInfoEntry 10 }

ipOspfIntfInfoAuthKey OBJECT-TYPE  
   SYNTAX DisplayString (SIZE(0..8))
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Authentication Key" 
    ::= { ipOspfIntfInfoEntry 11 }
     
ipOspfIntfInfoStatus  OBJECT-TYPE
    SYNTAX  INTEGER {
        disabled(0),
        enabled(1)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Status of the interface
	disabled(0),
        enabled(1)" 
    ::= { ipOspfIntfInfoEntry 12 }


-- IP OSPF Virtual Link Information
ipOspfVirtIntfInfoTable OBJECT-TYPE
    SYNTAX SEQUENCE OF IpOspfVirtIntfInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Virtual Interface Information."
    ::= { ipOspfInfo 9 }

ipOspfVirtIntfInfoEntry OBJECT-TYPE
    SYNTAX IpOspfVirtIntfInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about an OSPF virtual Interface."
    INDEX { ipOspfVirtIntfInfoIndex }
    ::= { ipOspfVirtIntfInfoTable 1 }
 
IpOspfVirtIntfInfoEntry ::= SEQUENCE {
    ipOspfVirtIntfInfoIndex         Integer32,
    ipOspfVirtIntfInfoAreaId        INTEGER,
    ipOspfVirtIntfInfoNbr           IpAddress,
    ipOspfVirtIntfInfoMdkey         INTEGER,
    ipOspfVirtIntfInfoHello         INTEGER,
    ipOspfVirtIntfInfoDead          INTEGER,
    ipOspfVirtIntfInfoTrans         INTEGER,
    ipOspfVirtIntfInfoRetra         INTEGER,
    ipOspfVirtIntfInfoAuthKey       DisplayString,
    ipOspfVirtIntfInfoStatus        INTEGER 
    }

ipOspfVirtIntfInfoIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The OSPF Virtual Interface number for which the OSPF 
         Virtual Interface table is related."
    ::= { ipOspfVirtIntfInfoEntry 1}

ipOspfVirtIntfInfoAreaId OBJECT-TYPE
    SYNTAX INTEGER (0..2) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The index of the OSPF area to which this virtual interface
         belongs." 
    ::= { ipOspfVirtIntfInfoEntry 2 }

ipOspfVirtIntfInfoNbr OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The IP Address of the OSPF neighbor for this virtual interface."
    ::= { ipOspfVirtIntfInfoEntry 3 }

ipOspfVirtIntfInfoMdkey OBJECT-TYPE
    SYNTAX INTEGER (0..255) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The MD5 key for the OSPF virtual interface
         0 (none) no MD5 authentication." 
    ::= { ipOspfVirtIntfInfoEntry 4 }

ipOspfVirtIntfInfoHello  OBJECT-TYPE 
    SYNTAX INTEGER (1..65535) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Hello interval" 
    ::= { ipOspfVirtIntfInfoEntry 5 }

ipOspfVirtIntfInfoDead   OBJECT-TYPE
   SYNTAX INTEGER (1..65535) 
    MAX-ACCESS read-only
    STATUS current 
    DESCRIPTION
	"Dead interval" 
    ::= { ipOspfVirtIntfInfoEntry 6 }

ipOspfVirtIntfInfoTrans  OBJECT-TYPE
   SYNTAX INTEGER (1..3600) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Transit delay" 
    ::= { ipOspfVirtIntfInfoEntry 7 }

ipOspfVirtIntfInfoRetra OBJECT-TYPE
    SYNTAX INTEGER (1..3600) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Retransmit interval" 
    ::= { ipOspfVirtIntfInfoEntry 8 }

ipOspfVirtIntfInfoAuthKey OBJECT-TYPE  
   SYNTAX DisplayString (SIZE(0..8))
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Authentication Key" 
    ::= { ipOspfVirtIntfInfoEntry 9 }
    
ipOspfVirtIntfInfoStatus  OBJECT-TYPE
    SYNTAX  INTEGER {
        disabled(0),
        enabled(1)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Status
	 disabled(0),
        enabled(1)" 
    ::= { ipOspfVirtIntfInfoEntry 10 }


--IP OSPF Host Information
ipOspfHostInfoTable OBJECT-TYPE
    SYNTAX SEQUENCE OF IpOspfHostInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Host Information."
    ::= { ipOspfInfo 10 }

ipOspfHostInfoEntry OBJECT-TYPE
    SYNTAX IpOspfHostInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about a OSPF host."
    INDEX { ipOspfHostInfoIndex, ipOspfHostInfoIpAddr }
    ::= { ipOspfHostInfoTable 1 }
 
IpOspfHostInfoEntry ::= SEQUENCE {
    ipOspfHostInfoIndex         Integer32,
    ipOspfHostInfoIpAddr        IpAddress,
    ipOspfHostInfoAreaIndex     Integer32,
    ipOspfHostInfoCost          Integer32,
    ipOspfHostInfoState		INTEGER
    }
 
ipOspfHostInfoIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The OSPF host number for which the OSPF host table is related."
    ::= { ipOspfHostInfoEntry 1}

ipOspfHostInfoIpAddr OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The IP Address of the OSPF host." 
    ::= { ipOspfHostInfoEntry 2 }

ipOspfHostInfoAreaIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The area index."
    ::= { ipOspfHostInfoEntry 3 }

ipOspfHostInfoCost OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The cost of the corresponding host."
    ::= { ipOspfHostInfoEntry 4 }

ipOspfHostInfoState OBJECT-TYPE
    SYNTAX  INTEGER  {
	enabled(2),
	disabled(3)
	}
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable an OSPF Host"
    ::= { ipOspfHostInfoEntry 5 }

ipOspfRedistributeInfo  OBJECT IDENTIFIER ::= { ipOspfInfo 11 }

ipOspfRedistributeStaticInfo  OBJECT IDENTIFIER 
    ::= { ipOspfRedistributeInfo 1 }

ipOspfRedistributeStaticInfoMetric OBJECT-TYPE
    SYNTAX INTEGER (0..16777214)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The metric to be assigned to static routes. 
         A value of 0 indicates none."
    ::= { ipOspfRedistributeStaticInfo 1 }

ipOspfRedistributeStaticInfoMetricType OBJECT-TYPE
    SYNTAX INTEGER {
        none(1),
        type1(2),
        type2(3)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The AS External metric type for static routes."
    ::= { ipOspfRedistributeStaticInfo 2 }

ipOspfRedistributeStaticInfoOutRmapList OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The route maps present in the out route map list. 
         The route maps are presented in a bitmap format.

         in receiving order:

         OCTET 1  OCTET 2  .....
         xxxxxxxx xxxxxxxx .....
         ||    || |_ Rmap 9
         ||    ||
         ||    ||___ Rmap 8
         ||    |____ Rmap 7
         ||      .    .   .
         ||_________ Rmap 2
         |__________ Rmap 1

         where x : 1 - The represented route map is selected
         0 - The represented route map is not selected"
    ::= { ipOspfRedistributeStaticInfo 3 }


ipOspfRedistributeFixedInfo  OBJECT IDENTIFIER 
    ::= { ipOspfRedistributeInfo 2 }

ipOspfRedistributeFixedInfoMetric OBJECT-TYPE
    SYNTAX INTEGER (0..16777214)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The export metric for fixed routes. A value of 0 indicates none"
    ::= { ipOspfRedistributeFixedInfo 1 }

ipOspfRedistributeFixedInfoMetricType OBJECT-TYPE
    SYNTAX INTEGER {
        none(1),
        type1(2),
        type2(3)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The AS External metric type for fixed routes."
    ::= { ipOspfRedistributeFixedInfo 2 }

ipOspfRedistributeFixedInfoOutRmapList OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The route maps present in the out route map list. 
         The route maps are presented in a bitmap format.

         in receiving order:

         OCTET 1  OCTET 2  .....
         xxxxxxxx xxxxxxxx .....
         ||    || |_ Rmap 9
         ||    ||
         ||    ||___ Rmap 8
         ||    |____ Rmap 7
         ||      .    .   .
         ||_________ Rmap 2
         |__________ Rmap 1

         where x : 1 - The represented route map is selected
         0 - The represented route map is not selected"
    ::= { ipOspfRedistributeFixedInfo 3 }


ipOspfRedistributeRipInfo  OBJECT IDENTIFIER 
    ::= { ipOspfRedistributeInfo 3 }

ipOspfRedistributeRipInfoMetric OBJECT-TYPE
    SYNTAX INTEGER (0..16777214)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The export metric for RIP routes. A value of 0 indicates none"
    ::= { ipOspfRedistributeRipInfo 1 }

ipOspfRedistributeRipInfoMetricType OBJECT-TYPE
    SYNTAX INTEGER {
        none(1),
        type1(2),
        type2(3)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The AS External metric type for RIP routes."
    ::= { ipOspfRedistributeRipInfo 2 }

ipOspfRedistributeRipInfoOutRmapList OBJECT-TYPE
    SYNTAX OCTET STRING
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The route maps present in the out route map list. 
         The route maps are presented in a bitmap format.

         in receiving order:

         OCTET 1  OCTET 2  .....
         xxxxxxxx xxxxxxxx .....
         ||    || |_ Rmap 9
         ||    ||
         ||    ||___ Rmap 8
         ||    |____ Rmap 7
         ||      .    .   .
         ||_________ Rmap 2
         |__________ Rmap 1

         where x : 1 - The represented route map is selected
         0 - The represented route map is not selected"
    ::= { ipOspfRedistributeRipInfo 3 }

ipOspfMd5keyInfoTable OBJECT-TYPE
    SYNTAX SEQUENCE OF IpOspfMd5keyInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF MD5 keys Information."
    ::= { ipOspfInfo 12 }

ipOspfMd5keyInfoEntry OBJECT-TYPE
    SYNTAX IpOspfMd5keyInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about an OSPF MD keys table."
    INDEX { ipOspfMd5keyInfoIndex }
    ::= { ipOspfMd5keyInfoTable 1 }
 
IpOspfMd5keyInfoEntry ::= SEQUENCE {
    ipOspfMd5keyInfoIndex        Integer32,
    ipOspfMd5keyInfoKey          DisplayString
    }
 
ipOspfMd5keyInfoIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only 
    STATUS current
    DESCRIPTION
	"The OSPF MD5 Key number for which the OSPF MdKey table is related."
    ::= { ipOspfMd5keyInfoEntry 1}

ipOspfMd5keyInfoKey OBJECT-TYPE
    SYNTAX DisplayString (SIZE(0..16)) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The character string representing the MD5 Key." 
    ::= { ipOspfMd5keyInfoEntry 2 }


-- VRRP Information

vrrpInfoVirtRtrTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF VrrpInfoVirtRtrTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of VRRP virtual router run-time information."
    ::= { vrrpInfo 1 }

vrrpInfoVirtRtrTableEntry OBJECT-TYPE
    SYNTAX  VrrpInfoVirtRtrTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The run-time information about a VRRP virtual router."
    INDEX   { vrrpInfoVirtRtrIndex }
    ::= { vrrpInfoVirtRtrTable 1 }
 
VrrpInfoVirtRtrTableEntry ::= SEQUENCE {
    vrrpInfoVirtRtrIndex      Integer32,
    vrrpInfoVirtRtrConfig     INTEGER,
    vrrpInfoVirtRtrID         INTEGER,
    vrrpInfoVirtRtrAddr       IpAddress,
    vrrpInfoVirtRtrIfIndex    Integer32,
    vrrpInfoVirtRtrOwnership  INTEGER,
    vrrpInfoVirtRtrPriority   INTEGER,
    vrrpInfoVirtRtrState      INTEGER
    }

vrrpInfoVirtRtrIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The VRRP virtual router index." 
    ::= { vrrpInfoVirtRtrTableEntry 1 }

vrrpInfoVirtRtrConfig OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The status of the VRRP virtual router."
    ::= { vrrpInfoVirtRtrTableEntry 2 }

vrrpInfoVirtRtrID OBJECT-TYPE
    SYNTAX  INTEGER (1..255)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The VRRP virtual router identifier."
    ::= { vrrpInfoVirtRtrTableEntry 3 }

vrrpInfoVirtRtrAddr OBJECT-TYPE
    SYNTAX  IpAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The VRRP virtual router IP address."
    ::= { vrrpInfoVirtRtrTableEntry 4 }

vrrpInfoVirtRtrIfIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The IfIndex that the VRRP virtual router is representing."
    ::= { vrrpInfoVirtRtrTableEntry 5 }

vrrpInfoVirtRtrPriority OBJECT-TYPE
    SYNTAX  INTEGER (1..254)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The priority value to be used by the specified VRRP virtual routers."
    ::= { vrrpInfoVirtRtrTableEntry 6 }

vrrpInfoVirtRtrState OBJECT-TYPE   
    SYNTAX  INTEGER {
	init(1),
	master(2),
	backup(3)
	}
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The VRRP virtual router state."   
    ::= { vrrpInfoVirtRtrTableEntry 7 }

vrrpInfoVirtRtrOwnership OBJECT-TYPE   
    SYNTAX  INTEGER {
	owner(1),
	renter(2)
	}
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The VRRP virtual router ownership status."   
    ::= { vrrpInfoVirtRtrTableEntry 8 }


-- Ospf Information 

ospfGeneralInfo  OBJECT IDENTIFIER ::= { ospfInfo 1 }

ospfVersion OBJECT-TYPE
    SYNTAX INTEGER {
        ospfVersion1(1),
        ospfVersion2(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "OSPF version."
    ::= { ospfGeneralInfo 1 }

ospfRouterID OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The router ID of the switch." 
    ::= { ospfGeneralInfo 2 }

ospfStartTime OBJECT-TYPE   
    SYNTAX  Integer32 
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The time when ospf has been started."   
    ::= { ospfGeneralInfo 3 }

ospfProcessUptime OBJECT-TYPE   
    SYNTAX  Counter32 
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The time since ospf has been started."   
    ::= { ospfGeneralInfo 4 }

ospfLsTypesSupported OBJECT-TYPE   
    SYNTAX  Integer32 
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The Link State Types that are supported."   
    ::= { ospfGeneralInfo 5 }

ospfAreaBorderRouter OBJECT-TYPE   
    SYNTAX  INTEGER {
	yes(1),
	no(2)
	}
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "Area Border Router Role."
    ::= { ospfGeneralInfo 6 }

ospfAreaBoundaryRouter OBJECT-TYPE   
    SYNTAX  INTEGER {
	yes(1),
	no(2)
	}
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "Area Boundary Router Role." 
    ::= { ospfGeneralInfo 7 }

ospfExternalLsa OBJECT-TYPE   
    SYNTAX  Integer32 
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The number of external LSAs." 
    ::= { ospfGeneralInfo 8 }

ospfIntfCountForRouter OBJECT-TYPE   
    SYNTAX  Integer32 
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The number of interfaces for this router." 
    ::= { ospfGeneralInfo 9 }

ospfVlinkCountForRouter OBJECT-TYPE   
    SYNTAX  Integer32 
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The number of virtual links for this router." 
    ::= { ospfGeneralInfo 10 }

ospfNewLsaReceived OBJECT-TYPE   
    SYNTAX  Integer32 
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The number of new LSAs reveived." 
    ::= { ospfGeneralInfo 11 }

ospfTotalLsaOriginated OBJECT-TYPE   
    SYNTAX  Integer32 
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The number of LSAs originated." 
    ::= { ospfGeneralInfo 12 }

ospfTotalNumberOfLsdbEntries OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"Total number of entries in the  Link State Database." 
    ::= { ospfGeneralInfo 13 }

ospfTotalNeighbours OBJECT-TYPE   
    SYNTAX  Integer32 
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The total number of OSPF neighbours." 
    ::= { ospfGeneralInfo 14 }

ospfNbrInInitState OBJECT-TYPE   
    SYNTAX  Integer32 
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The number of neighbours in the initial state of exchange." 
    ::= { ospfGeneralInfo 15 }

ospfNbrInExchState OBJECT-TYPE   
    SYNTAX  Integer32 
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The number of neighbours in the exchange state." 
    ::= { ospfGeneralInfo 16 }

ospfNbrInFullState OBJECT-TYPE   
    SYNTAX  Integer32 
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The number of neighbours in the Full state of exchange." 
    ::= { ospfGeneralInfo 17 }

ospfTotalAreas OBJECT-TYPE   
    SYNTAX  Integer32 
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The Total number of areas." 
    ::= { ospfGeneralInfo 18 }

ospfTotalTransitAreas OBJECT-TYPE   
    SYNTAX  Integer32 
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The Total number of Transit areas." 
    ::= { ospfGeneralInfo 19 }

ospfTotalNssaAreas OBJECT-TYPE   
    SYNTAX  Integer32 
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The Total number of NSSA areas." 
    ::= { ospfGeneralInfo 20 }

ospfTotalStubAreas OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Total number of STUB areas."
    ::= { ospfGeneralInfo 21 }

ospfAreaInfoTable OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfAreaInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Area information."
    ::= { ospfInfo 2 }

ospfAreaInfoEntry OBJECT-TYPE
    SYNTAX OspfAreaInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about a OSPF area."
    INDEX { ospfAreaInfoIndex }
    ::= { ospfAreaInfoTable 1 }
 
OspfAreaInfoEntry ::= SEQUENCE {
    ospfAreaInfoIndex                 Integer32,
    ospfAreaInfoId                    IpAddress,
    ospfAreaInfoStatus                INTEGER,
    ospfTotalNumberOfInterfaces       Integer32,
    ospfNumberOfInterfacesUp          Integer32,
    ospfAreaInfoAuthType              INTEGER,
    ospfAreaInfoSPF                   Integer32,
    ospfNumberOfLsdbEntries           Integer32,
    ospfAreaInfoAreaBorderRouter      Integer32,
    ospfAreaInfoASBoundaryRouter      Integer32,
    ospfAreaInfoTotalNeighbours	      Integer32,
    ospfAreaInfoNeighborsINITstate    Integer32,
    ospfAreaInfoNeighborsEXCHstate    Integer32,
    ospfAreaInfoNeighborsFULLstate    Integer32,
    ospfAreaInfoLsTypesAccepted       DisplayString
    }
 
ospfAreaInfoIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The OSPF area number for which the OSPF info table is related."
    ::= { ospfAreaInfoEntry 1 } 

ospfAreaInfoId OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The IP address of the OSPF area." 
    ::= { ospfAreaInfoEntry 2 }

ospfAreaInfoStatus OBJECT-TYPE
    SYNTAX  INTEGER {
        disabled(0), 
        enabled(1)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Area Status:
           disabled(0), enabled(1)."
    ::= { ospfAreaInfoEntry 3 }

ospfTotalNumberOfInterfaces OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The total number of interfaces for this OSPF area." 
    ::= { ospfAreaInfoEntry 4 }

ospfNumberOfInterfacesUp OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The number of interfaces UP in area." 
    ::= { ospfAreaInfoEntry 5 }

ospfAreaInfoAuthType OBJECT-TYPE
    SYNTAX  INTEGER {
        none(1),
        password(2),
        md5(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Type of authentication being used:
         none(1) - no authentication
         password(2) - use password
         md5(3) - use MD5 authentication."
    ::= { ospfAreaInfoEntry 6 }

ospfAreaInfoSPF OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The number of times SPF ran."
    ::= { ospfAreaInfoEntry 7 }

ospfNumberOfLsdbEntries OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The number of Link State Database entries for this OSPF area." 
    ::= { ospfAreaInfoEntry 8 }

ospfAreaInfoAreaBorderRouter OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The Area Border Router count."
    ::= { ospfAreaInfoEntry 9 }

ospfAreaInfoASBoundaryRouter OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The AS Boundary Router count."
    ::= { ospfAreaInfoEntry 10 }

ospfAreaInfoTotalNeighbours OBJECT-TYPE   
    SYNTAX  Integer32 
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The total number of OSPF neighbors." 
    ::= { ospfAreaInfoEntry 11 }

 ospfAreaInfoNeighborsINITstate OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Total neighbors in INIT state."
    ::= { ospfAreaInfoEntry 12 }

ospfAreaInfoNeighborsEXCHstate OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Total neighbors in EXCH state."
    ::= { ospfAreaInfoEntry 13 }

ospfAreaInfoNeighborsFULLstate OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Total neighbors in FULL state."
    ::= { ospfAreaInfoEntry 14 }

ospfAreaInfoLsTypesAccepted OBJECT-TYPE
    SYNTAX DisplayString  (SIZE(0..40))
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "LS types accepted by this area."
    ::= { ospfAreaInfoEntry 15 }


ospfIntfInfoTable OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfIntfInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Interface information."
    ::= { ospfInfo 3 }

ospfIntfInfoEntry OBJECT-TYPE
    SYNTAX OspfIntfInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about a OSPF interface."
    INDEX { ospfIfInfoIndex }
    ::= { ospfIntfInfoTable 1 }
 
OspfIntfInfoEntry ::= SEQUENCE {
    ospfIfInfoIndex                                     Integer32,
    ospfIfInfoIpAddress                                 IpAddress,
    ospfIfInfoArea                                      INTEGER,
    ospfIfInfoAdminStatus                               INTEGER,
    ospfIfInfoRouterID                                  IpAddress,
    ospfIfInfoState                                     INTEGER,
    ospfIfInfoPriority                                  INTEGER,
    ospfIfInfoDesignatedRouterID                        IpAddress,
    ospfIfInfoDesignatedRouterIpAddress                 IpAddress,
    ospfIfInfoBackupDesignatedRouterID                  IpAddress,
    ospfIfInfoBackupDesignatedRouterIpAddress           IpAddress,
    ospfIfInfoHello                                     INTEGER,
    ospfIfInfoDead                                      INTEGER,
    ospfIfInfoWait                                      Integer32,
    ospfIfInfoRetransmit                                INTEGER,
    ospfIfInfoTransitDelay                              INTEGER,
    ospfIfInfoTotalNeighbours                           Integer32,
    ospfIfInfoEvents                                    Integer32,
    ospfIfInfoAuthType                                  INTEGER
    }
 
ospfIfInfoIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The OSPF interface number for which the OSPF info table is related."
    ::= { ospfIntfInfoEntry 1 }

ospfIfInfoIpAddress OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The IP address of the OSPF interface." 
    ::= { ospfIntfInfoEntry 2 }

ospfIfInfoArea OBJECT-TYPE
    SYNTAX INTEGER (0..2) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The index of the area that the interface belongs." 
    ::= { ospfIntfInfoEntry 3 }

ospfIfInfoAdminStatus  OBJECT-TYPE
    SYNTAX  INTEGER {
        down(0),
        up(1)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Admin Status of the interface:
        down(0), up(1)." 
    ::= { ospfIntfInfoEntry 4 }

ospfIfInfoRouterID OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The router ID of the switch." 
    ::= { ospfIntfInfoEntry 5 }

ospfIfInfoState  OBJECT-TYPE
    SYNTAX  INTEGER {
        down(0),
        loopback(1),
        waiting(2),
        ptop(3),
        dr(4),
        backupdr(5),
        drother(6)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The state of the interface:
        Down(0), Loopback(1),
        Waiting(2), P to P(3),
        DR(4), BackuDR(5),
        DR Other(6)." 
    ::= { ospfIntfInfoEntry 6 }

ospfIfInfoPriority   OBJECT-TYPE
   SYNTAX INTEGER (1..255) 
    MAX-ACCESS read-only
    STATUS current 
    DESCRIPTION
        "Interface router priority" 
    ::= { ospfIntfInfoEntry 7 }

ospfIfInfoDesignatedRouterID OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The OSPF Designated Router ID for this OSPF interface." 
    ::= { ospfIntfInfoEntry 8 }

ospfIfInfoDesignatedRouterIpAddress OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The OSPF Designated Router IP Address for this OSPF interface." 
    ::= { ospfIntfInfoEntry 9 }

ospfIfInfoBackupDesignatedRouterID OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The OSPF Backup Designated Router ID for this OSPF
         interface." 
    ::= { ospfIntfInfoEntry 10 }

ospfIfInfoBackupDesignatedRouterIpAddress OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The OSPF Backup Designated Router Ip Address for this OSPF
         interface." 
    ::= { ospfIntfInfoEntry 11 }

ospfIfInfoHello  OBJECT-TYPE 
    SYNTAX INTEGER (1..65535) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The hello timer for this OSPF interface." 
    ::= { ospfIntfInfoEntry 12 }

ospfIfInfoDead   OBJECT-TYPE
   SYNTAX INTEGER (1..65535) 
    MAX-ACCESS read-only
    STATUS current 
    DESCRIPTION
        "The dead timer for this OSPF interface." 
    ::= { ospfIntfInfoEntry 13 }

ospfIfInfoWait OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The OSPF Wait interval for this OSPF interface." 
    ::= { ospfIntfInfoEntry 14 }

ospfIfInfoRetransmit OBJECT-TYPE
    SYNTAX INTEGER (1..3600) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The retransmit interval for this OSPF interface." 
    ::= { ospfIntfInfoEntry 15 }

ospfIfInfoTransitDelay  OBJECT-TYPE
   SYNTAX INTEGER (1..3600) 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The transit delay for this OSPF interface." 
    ::= { ospfIntfInfoEntry 16 }
        
ospfIfInfoTotalNeighbours OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The total number of neighbours for this OSPF interface." 
    ::= { ospfIntfInfoEntry 17 }

ospfIfInfoEvents OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The total number of events for this OSPF interface." 
    ::= { ospfIntfInfoEntry 18 }

ospfIfInfoAuthType OBJECT-TYPE
    SYNTAX  INTEGER {
        none(1),
        password(2),
        md5(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Type of authentication being used:
         none(1) - no authentication,
         password(2) - use password,
         md5(3) - use MD5 authentication."
    ::= { ospfIntfInfoEntry 19 }

-- OSPF Interface/Virtual Interface Table

ospfVirtIntfInfoTable OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfVirtIntfInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF virtual interfaces information."
    ::= { ospfInfo 4 }

ospfVirtIntfInfoEntry OBJECT-TYPE
    SYNTAX OspfVirtIntfInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about an OSPF virtual interface."
    INDEX { ospfVirtIntfInfoIndex }
    ::= { ospfVirtIntfInfoTable 1 }

OspfVirtIntfInfoEntry ::= SEQUENCE {
    ospfVirtIntfInfoIndex         Integer32,
    ospfVirtIntfInfoIpAddr        IpAddress,
    ospfVirtIntfInfoArea          INTEGER,
    ospfVirtIntfInfoRouterId      IpAddress,
    ospfVirtIntfInfoState         INTEGER,
    ospfVirtIntfInfoCost          INTEGER,
    ospfVirtIntfInfoTrans         INTEGER,
    ospfVirtIntfInfoHello         INTEGER,
    ospfVirtIntfInfoDead          INTEGER,
    ospfVirtIntfInfoWait          INTEGER,
    ospfVirtIntfInfoRetra         INTEGER,
    ospfVirtIntfInfoAuth          DisplayString,
    ospfVirtIntfInfoEvents        INTEGER,
    ospfVirtIntfInfoNbr           IpAddress,
    ospfVirtIntfInfoNbrState      INTEGER,
    ospfVirtIntfInfoAreaId        IpAddress
    }

ospfVirtIntfInfoIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The OSPF Virtual Interface number for which this table is
         related."
    ::= { ospfVirtIntfInfoEntry 1 }

ospfVirtIntfInfoIpAddr OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The IP Address of this virtual interface."
    ::= { ospfVirtIntfInfoEntry 2 }

ospfVirtIntfInfoArea OBJECT-TYPE
    SYNTAX INTEGER (0..2)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The index of the OSPF area to which this virtual interface
         belongs."
    ::= { ospfVirtIntfInfoEntry 3 }

ospfVirtIntfInfoRouterId OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The Router ID."
    ::= { ospfVirtIntfInfoEntry 4 }

ospfVirtIntfInfoState   OBJECT-TYPE
    SYNTAX  INTEGER {
        disabled(0),
        enabled(1)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "State
         disabled(0),
         enabled(1)"
    ::= { ospfVirtIntfInfoEntry 5 }

ospfVirtIntfInfoCost OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The cost of the virtual interface."
    ::= { ospfVirtIntfInfoEntry 6 }

ospfVirtIntfInfoTrans OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The transit delay for the virtual interface."
    ::= { ospfVirtIntfInfoEntry 7 }

ospfVirtIntfInfoHello  OBJECT-TYPE
    SYNTAX INTEGER (1..65535)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Hello interval."
    ::= { ospfVirtIntfInfoEntry 8 }

ospfVirtIntfInfoDead   OBJECT-TYPE
   SYNTAX INTEGER (1..65535)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Dead interval."
    ::= { ospfVirtIntfInfoEntry 9 }

ospfVirtIntfInfoWait   OBJECT-TYPE
    SYNTAX INTEGER (1..65535)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Wait interval."
    ::= { ospfVirtIntfInfoEntry 10 }

ospfVirtIntfInfoRetra  OBJECT-TYPE
    SYNTAX INTEGER (1..3600)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Retransmit interval."
    ::= { ospfVirtIntfInfoEntry 11 }

ospfVirtIntfInfoAuth OBJECT-TYPE
   SYNTAX DisplayString (SIZE(0..8))
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Authentication."
    ::= { ospfVirtIntfInfoEntry 12 }

ospfVirtIntfInfoEvents OBJECT-TYPE
    SYNTAX INTEGER
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
         "Events."
    ::= { ospfVirtIntfInfoEntry 13 }

ospfVirtIntfInfoNbr OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The IP Address of the OSPF neighbor for this virtual interface."
    ::= { ospfVirtIntfInfoEntry 14 }

ospfVirtIntfInfoNbrState  OBJECT-TYPE
    SYNTAX  INTEGER {
        down(0),attempt(1),init(2),twoway(3),
        exstart(4),exchange(5),loading(6),full(7)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "State
         down(0),attempt(1),init(2),2 way(3),
         exstart(4),exchange(5),loading(6),full(7)"
    ::= { ospfVirtIntfInfoEntry 15 }

ospfVirtIntfInfoAreaId OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Thea AreaId of the virtual interface."
    ::= { ospfVirtIntfInfoEntry 16 }


-- OSPF Interface/Nbr Info Table

ospfIfNbrTable OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfIfNbrEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF Interface Neighbor information."
    ::= { ospfInfo 5 }

ospfIfNbrEntry OBJECT-TYPE
    SYNTAX OspfIfNbrEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Information about a OSPF interface, neighbor pair."
    INDEX { ospfIfNbrIntfIndex, ospfIfNbrIpAddr }
    ::= { ospfIfNbrTable 1 }
 
OspfIfNbrEntry ::= SEQUENCE {
    ospfIfNbrIntfIndex               Integer32,
    ospfIfNbrIpAddr                  IpAddress,
    ospfIfNbrPriority                Integer32,
    ospfIfNbrState                   INTEGER,
    ospfIfNbrDesignatedRtr     	     IpAddress,
    ospfIfNbrBackupDesignatedRtr     IpAddress,
    ospfIfNbrIpAddress               IpAddress 
    }
 
ospfIfNbrIntfIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The OSPF Interface number for which this Interface/Nbr table is 
         related."
    ::= { ospfIfNbrEntry 1}

ospfIfNbrIpAddr OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The OSPF Neighbor ID ." 
    ::= { ospfIfNbrEntry 2 }

ospfIfNbrPriority OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The priority of the OSPF neighbor."
    ::= { ospfIfNbrEntry 3 }

ospfIfNbrState OBJECT-TYPE
    SYNTAX  INTEGER { 
	down(1),
	attempt(2),
	init(3),
	twoway(4),
	exStart(5),
	exchange(6),
	loading(7),
	full(8)
	}
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The state of the OSPF neighbor."
    ::= { ospfIfNbrEntry 4 }

ospfIfNbrDesignatedRtr OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The IP Address of the Designated Router for this OSPF Neighbor." 
    ::= { ospfIfNbrEntry 5 }

ospfIfNbrBackupDesignatedRtr OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The IP Address of the backup designated Router for this OSPF Neighbor." 
    ::= { ospfIfNbrEntry 6 }

ospfIfNbrIpAddress OBJECT-TYPE
    SYNTAX IpAddress 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
	"The IP Address of the OSPF Neighbor." 
    ::= { ospfIfNbrEntry 7 }


-- OSPF Interface/Summary Ranges Table

ospfSumRangesInfoTable OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfSumRangesInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF summary ranges information."
    ::= { ospfInfo 6 }

ospfSumRangesInfoEntry OBJECT-TYPE
    SYNTAX OspfSumRangesInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "Summary ranges information."
    INDEX { ospfSumRangesInfoIndex }
    ::= { ospfSumRangesInfoTable 1 }

OspfSumRangesInfoEntry ::= SEQUENCE {
    ospfSumRangesInfoIndex         Integer32,
    ospfSumRangesInfoArea          INTEGER,
    ospfSumRangesInfoNetwork       IpAddress,
    ospfSumRangesInfoMask          IpAddress,
    ospfSumRangesInfoAction        INTEGER,
    ospfSumRangesInfoListType      INTEGER
    }

ospfSumRangesInfoIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The OSPF range index for which this table is
         related."
    ::= { ospfSumRangesInfoEntry 1 }

ospfSumRangesInfoArea OBJECT-TYPE
    SYNTAX INTEGER (0..2)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Area."
    ::= { ospfSumRangesInfoEntry 2 }

ospfSumRangesInfoNetwork OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Network."
    ::= { ospfSumRangesInfoEntry 3 }

ospfSumRangesInfoMask OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Mask."
    ::= { ospfSumRangesInfoEntry 4 }

ospfSumRangesInfoAction  OBJECT-TYPE
    SYNTAX  INTEGER {
        propagate(0),
        hide(1)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Action
         propagate(0),
         hide(1)"
    ::= { ospfSumRangesInfoEntry 5 }

ospfSumRangesInfoListType  OBJECT-TYPE
    SYNTAX  INTEGER {
        non-nssa(0),
        nssa(1)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
       "Summary address list 
         Non-NSSA(0),
         NSSA(1)"
    ::= { ospfSumRangesInfoEntry 6 }


-- OSPF Interface/Routes Table

ospfRoutesInfoTable OBJECT-TYPE
    SYNTAX SEQUENCE OF OspfRoutesInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "The table of OSPF routes information."
    ::= { ospfInfo 7 }

ospfRoutesInfoEntry OBJECT-TYPE
    SYNTAX OspfRoutesInfoEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
      "OSPF routes information."
    INDEX { ospfRoutesInfoIndex }
    ::= { ospfRoutesInfoTable 1 }

OspfRoutesInfoEntry ::= SEQUENCE {
    ospfRoutesInfoIndex            Integer32,
    ospfRoutesInfoDestination      IpAddress,
    ospfRoutesInfoMask             IpAddress,
    ospfRoutesInfoVia              IpAddress,
    ospfRoutesInfoType             DisplayString
    }

ospfRoutesInfoIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The OSPF route table entry index for which 
          this table is related."
    ::= { ospfRoutesInfoEntry 1 }

ospfRoutesInfoDestination OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Destination."
    ::= { ospfRoutesInfoEntry 2 }

ospfRoutesInfoMask OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Mask."
    ::= { ospfRoutesInfoEntry 3 }

ospfRoutesInfoVia OBJECT-TYPE
    SYNTAX IpAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Next hop."
    ::= { ospfRoutesInfoEntry 4 }

ospfRoutesInfoType OBJECT-TYPE
    SYNTAX DisplayString (SIZE(0..8))
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Route type. Codes: IA - OSPF inter area,
         N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
         E1 - OSPF external type 1, E2 - OSPF external type 2
         *  - best"
    ::= { ospfRoutesInfoEntry 5 }


--  OSPF Link State Database

--      The Link State Database contains the Link State
--      Advertisements from throughout the areas that the
--      device is attached to.

--  The Area ID, in OSPF, has the same format as an IP Address,
--  but has the function of defining a summarization point for
--  Link State Advertisements.

--  The Router ID, in OSPF, has the same format as an IP Address,
--  but identifies the router independent of its IP Address.

    ospfLsdbInfoTable OBJECT-TYPE
        SYNTAX   SEQUENCE OF OspfLsdbInfoEntry
        MAX-ACCESS   not-accessible
        STATUS   current
        DESCRIPTION
           "The OSPF Process's Link State Database."
       REFERENCE
          "OSPF Version 2, Section 12  Link  State  Adver-
          tisements"
      ::= { ospfInfo 8 }


    ospfLsdbInfoEntry OBJECT-TYPE
        SYNTAX   OspfLsdbInfoEntry
        MAX-ACCESS   not-accessible
        STATUS   current
        DESCRIPTION
           "A single Link State Advertisement."
       INDEX { ospfLsdbInfoIndex }
       ::= { ospfLsdbInfoTable 1 }


OspfLsdbInfoEntry ::=
    SEQUENCE {
        ospfLsdbInfoIndex
            Integer32,
        ospfLsdbInfoAreaId
            IpAddress,
        ospfLsdbInfoType
            INTEGER,
        ospfLsdbInfoLsid
            IpAddress,
        ospfLsdbInfoRouterId
            IpAddress,
        ospfLsdbInfoSequence
            OCTET STRING,
        ospfLsdbInfoAge
            Integer32,
        ospfLsdbInfoChecksum
            Integer32,
        ospfLsdbInfoAdvertisement
            OCTET STRING
              }


    ospfLsdbInfoIndex OBJECT-TYPE
        SYNTAX   Integer32
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The 32 bit index in the table."
       REFERENCE
          "Private MIBS"
      ::= { ospfLsdbInfoEntry 1 }


    ospfLsdbInfoAreaId OBJECT-TYPE
        SYNTAX   IpAddress
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The 32 bit identifier of the Area  from  which
           the LSA was received."
       REFERENCE
          "OSPF Version 2, Appendix C.2 Area parameters"
      ::= { ospfLsdbInfoEntry 2 }

-- External Link State Advertisements are permitted
-- for backward compatibility, but should be displayed in
-- the ospfExtLsdbTable rather than here.

    ospfLsdbInfoType OBJECT-TYPE
        SYNTAX   INTEGER    {
                    routerLink (1),
                    networkLink (2),
                    summaryLink (3),
                    asSummaryLink (4),
                    asExternalLink (5), -- but see ospfExtLsdbTable
                    multicastLink (6),
                    nssaExternalLink (7)
                  }
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The type  of  the  link  state  advertisement.
           Each  link state type has a separate advertise-
           ment format."
       REFERENCE
          "OSPF Version 2, Appendix A.4.1 The  Link  State
          Advertisement header"
      ::= { ospfLsdbInfoEntry 3 }


    ospfLsdbInfoLsid OBJECT-TYPE
        SYNTAX   IpAddress
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The Link State ID is an LS Type Specific field
           containing either a Router ID or an IP Address;
           it identifies the piece of the  routing  domain
           that is being described by the advertisement."
       REFERENCE
          "OSPF Version 2, Section 12.1.4 Link State ID"
      ::= { ospfLsdbInfoEntry 4 }


    ospfLsdbInfoRouterId OBJECT-TYPE
        SYNTAX   IpAddress
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The 32 bit number that uniquely identifies the
           originating router in the Autonomous System."
       REFERENCE
          "OSPF Version 2, Appendix C.1 Global parameters"
      ::= { ospfLsdbInfoEntry 5 }

--  Note that the OSPF Sequence Number is a 32 bit signed
--  integer.  It starts with the value '80000001'h,
--  or -'7FFFFFFF'h, and increments until '7FFFFFFF'h
--  Thus, a typical sequence number will be very negative.
--  Modified to OCTET STRING - for BLADE HARMONY

    ospfLsdbInfoSequence OBJECT-TYPE
        SYNTAX   OCTET STRING (SIZE(10))
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The sequence number field is a  signed  32-bit
           integer.   It  is used to detect old and dupli-
           cate link state advertisements.  The  space  of
           sequence  numbers  is  linearly  ordered.   The
           larger the sequence number the more recent  the
           advertisement - displayed here in hexazecimal."
       REFERENCE
          "OSPF Version  2,  Section  12.1.6  LS  sequence
          number"
      ::= { ospfLsdbInfoEntry 6 }


    ospfLsdbInfoAge OBJECT-TYPE
        SYNTAX   Integer32    -- Should be 0..MaxAge
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "This field is the age of the link state adver-
           tisement in seconds."
       REFERENCE
          "OSPF Version 2, Section 12.1.1 LS age"
      ::= { ospfLsdbInfoEntry 7 }


    ospfLsdbInfoChecksum OBJECT-TYPE
        SYNTAX   Integer32
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "This field is the  checksum  of  the  complete
           contents  of  the  advertisement, excepting the
           age field.  The age field is excepted  so  that
           an   advertisement's  age  can  be  incremented
           without updating the  checksum.   The  checksum
           used  is  the same that is used for ISO connec-
           tionless datagrams; it is commonly referred  to
           as the Fletcher checksum."
       REFERENCE
          "OSPF Version 2, Section 12.1.7 LS checksum"
      ::= { ospfLsdbInfoEntry 8 }


    ospfLsdbInfoAdvertisement OBJECT-TYPE
        SYNTAX   OCTET STRING (SIZE(36))
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The entire Link State Advertisement, including
           its header."
       REFERENCE
          "OSPF Version 2, Section 12  Link  State  Adver-
          tisements"
      ::= { ospfLsdbInfoEntry 9 }


--  SPF Link State Database, External

--      The Link State Database contains the Link State
--      Advertisements from throughout the areas that the
--      device is attached to.

--             This table is identical to the OSPF LSDB Table in
--      format, but contains only External Link State
--             Advertisements.  The purpose is to allow external
--      LSAs to be displayed once for the router rather
--      than once in each non-stub area.

    ospfExtLsdbInfoTable OBJECT-TYPE
        SYNTAX   SEQUENCE OF OspfExtLsdbInfoEntry
        MAX-ACCESS   not-accessible
        STATUS   current
        DESCRIPTION
           "The OSPF Process's Links State Database."
       REFERENCE
          "OSPF Version 2, Section 12  Link  State  Adver-
          tisements"
      ::= { ospfInfo 9 }


    ospfExtLsdbInfoEntry OBJECT-TYPE
        SYNTAX   OspfExtLsdbInfoEntry
        MAX-ACCESS   not-accessible
        STATUS   current
        DESCRIPTION
           "A single Link State Advertisement."
       INDEX { ospfExtLsdbInfoIndex }
       ::= { ospfExtLsdbInfoTable 1 }


OspfExtLsdbInfoEntry ::=
    SEQUENCE {
        ospfExtLsdbInfoIndex
            Integer32,
        ospfExtLsdbInfoType
            INTEGER,
        ospfExtLsdbInfoLsid
            IpAddress,
        ospfExtLsdbInfoRouterId
            IpAddress,
        ospfExtLsdbInfoSequence
            OCTET STRING,
        ospfExtLsdbInfoAge
            Integer32,
        ospfExtLsdbInfoChecksum
            Integer32,
        ospfExtLsdbInfoAdvertisement
            OCTET STRING
              }


   ospfExtLsdbInfoIndex OBJECT-TYPE
        SYNTAX   Integer32
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The 32 bit index in the table."
       REFERENCE
          "Private MIBS"
      ::= { ospfExtLsdbInfoEntry 1 }


    ospfExtLsdbInfoType OBJECT-TYPE
        SYNTAX   INTEGER    {
                    asExternalLink (5)
                  }
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The type  of  the  link  state  advertisement.
           Each  link state type has a separate advertise-
           ment format."
       REFERENCE
          "OSPF Version 2, Appendix A.4.1 The  Link  State
          Advertisement header"
      ::= { ospfExtLsdbInfoEntry 2 }


    ospfExtLsdbInfoLsid OBJECT-TYPE
        SYNTAX   IpAddress
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The Link State ID is an LS Type Specific field
           containing either a Router ID or an IP Address;
           it identifies the piece of the  routing  domain
           that is being described by the advertisement."
       REFERENCE
          "OSPF Version 2, Section 12.1.4 Link State ID"
      ::= { ospfExtLsdbInfoEntry 3 }


    ospfExtLsdbInfoRouterId OBJECT-TYPE
        SYNTAX   IpAddress
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The 32 bit number that uniquely identifies the
           originating router in the Autonomous System."
       REFERENCE
          "OSPF Version 2, Appendix C.1 Global parameters"
      ::= { ospfExtLsdbInfoEntry 4 }

--  Note that the OSPF Sequence Number is a 32 bit signed
--  integer.  It starts with the value '80000001'h,
--  or -'7FFFFFFF'h, and increments until '7FFFFFFF'h
--  Thus, a typical sequence number will be very negative.
--  Modified to OCTET STRING - for BLADE HARMONY

    ospfExtLsdbInfoSequence OBJECT-TYPE
        SYNTAX   OCTET STRING (SIZE(10))
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The sequence number field is a  signed  32-bit
           integer.   It  is used to detect old and dupli-
           cate link state advertisements.  The  space  of
           sequence  numbers  is  linearly  ordered.   The
           larger the sequence number the more recent  the
           advertisement - displayed here in hexazecimal."
       REFERENCE
          "OSPF Version  2,  Section  12.1.6  LS  sequence
          number"
      ::= { ospfExtLsdbInfoEntry 5 }


    ospfExtLsdbInfoAge OBJECT-TYPE
        SYNTAX   Integer32    -- Should be 0..MaxAge
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "This field is the age of the link state adver-
           tisement in seconds."
       REFERENCE
          "OSPF Version 2, Section 12.1.1 LS age"
      ::= { ospfExtLsdbInfoEntry 6 }


    ospfExtLsdbInfoChecksum OBJECT-TYPE
        SYNTAX   Integer32
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "This field is the  checksum  of  the  complete
           contents  of  the  advertisement, excepting the
           age field.  The age field is excepted  so  that
           an   advertisement's  age  can  be  incremented
           without updating the  checksum.   The  checksum
           used  is  the same that is used for ISO connec-
           tionless datagrams; it is commonly referred  to
           as the Fletcher checksum."
       REFERENCE
          "OSPF Version 2, Section 12.1.7 LS checksum"
      ::= { ospfExtLsdbInfoEntry 7 }


    ospfExtLsdbInfoAdvertisement OBJECT-TYPE
        SYNTAX   OCTET STRING (SIZE(36))
        MAX-ACCESS   read-only
        STATUS   current
        DESCRIPTION
           "The entire Link State Advertisement, including
           its header."
       REFERENCE
          "OSPF Version 2, Section 12  Link  State  Adver-
          tisements"
      ::= { ospfExtLsdbInfoEntry 8 }

vrrpOperVirtRtrTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF VrrpOperVirtRtrEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "An entry in the table of virtual routers."
    ::= { vrrpOper 1 }

vrrpOperVirtRtrEntry OBJECT-TYPE
    SYNTAX  VrrpOperVirtRtrEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the vrrpOperVirtRtrTable "
    INDEX   { vrrpOperVirtRtrIndex }
    ::= { vrrpOperVirtRtrTable 1 }

VrrpOperVirtRtrEntry ::= SEQUENCE {
    vrrpOperVirtRtrIndex              Integer32,
    vrrpOperVirtRtrBackup             INTEGER
    }

vrrpOperVirtRtrIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The index for the  VRRP virtual router." 
    ::= { vrrpOperVirtRtrEntry 1 }

vrrpOperVirtRtrBackup OBJECT-TYPE
    SYNTAX  INTEGER {
	ok(1),
	backup(2)
	}
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "When set to a value of 'backup(2)' it forces the specified 
         master virtual router into backup mode.
         'ok(1)' is returned when the object os read."
    ::= { vrrpOperVirtRtrEntry 2 }

vrrpOperVirtRtrGroupBackup OBJECT-TYPE
    SYNTAX  INTEGER {
	ok(1),
	backup(2)
	}
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "When set to a value of 'backup(2)' it forces the specified 
         master virtual router group into backup mode.
         'ok(1)' is returned when the object os read."
    ::= { vrrpOper 2 }

-- ----------------------------------------------------------------------------
-- } INSERT:  bt2Network
-- ----------------------------------------------------------------------------


bntTraps	OBJECT IDENTIFIER
    ::= { hpSwitchBladeType5-Mgmt 7 }

-- ----------------------------------------------------------------------------
-- { INSERT:  bt2trap
-- ----------------------------------------------------------------------------

-- SECTION 2:  Temporary Object Definitions Used In Traps

bntSwTrapDisplayString OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(0..255))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Temporary string object used to store information being sent
                 in an BNT Switch trap."
        ::= { bntTraps 1000 }


-- SECTION 3:  Trap Definitions


bntSwDefGwUp TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { ipCurCfgGwIndex,
                          ipCurCfgGwAddr,
                          sysName, sysLocation, sysContact }
        DESCRIPTION
                "A bntSwDefGwUp trap signifies that the default
                 gateway is alive."
	--#SEVERITY INFORMATIONAL
        ::= 2   -- 0x02

bntSwDefGwDown TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { ipCurCfgGwIndex,
                          ipCurCfgGwAddr,
                          sysName, sysLocation, sysContact }
        DESCRIPTION
                "A bntSwDefGwDown trap signifies that the default
                 gateway is down."
	--#SEVERITY INFORMATIONAL
        ::= 3   -- 0x03

bntSwDefGwInService TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { ipCurCfgGwIndex,
                          ipCurCfgGwAddr,
                          sysName, sysLocation, sysContact }
        DESCRIPTION
                "A bntSwDefGwEnabled trap signifies that the default
                 gateway is up and in service."
	--#SEVERITY INFORMATIONAL
        ::= 4   -- 0x04

bntSwDefGwNotInService TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { ipCurCfgGwIndex,
                          ipCurCfgGwAddr,
                          sysName, sysLocation, sysContact }
        DESCRIPTION
                "A bntSwDefGwDisabled trap signifies that the default
                 gateway is alive but not in service."
	--#SEVERITY INFORMATIONAL
        ::= 5   -- 0x05


bntSwLoginFailure TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { bntSwTrapDisplayString,
                          sysName, sysLocation, sysContact }
        DESCRIPTION
                "A bntSwLoginFailure trap signifies that someone failed to
                 enter a valid username/password combination."
	--#SEVERITY MAJOR
        ::= 19 -- 0x13

bntSwTempExceedThreshold TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { bntSwTrapDisplayString,
                          sysName, sysLocation, sysContact }
        DESCRIPTION
              "A bntSwTempExceedThreshold trap signifies that the
               switch temperature has exceeded maximum safety limits."
        --#SEVERITY CRITICAL
        ::= 22   -- 0x16


bntSwApplyComplete TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { bntSwTrapDisplayString,
                          sysName, sysLocation, sysContact }
        DESCRIPTION
                "A bntSwApplyComplete signifies that new configuration
		 has been applied." 
	--#SEVERITY INFORMATIONAL
        ::= 27 -- 0x1B

bntSwSaveComplete TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { bntSwTrapDisplayString,
                          sysName, sysLocation, sysContact }
        DESCRIPTION
                "A bntSwApplyComplete signifies that new configuration
		 has been saved." 
	--#SEVERITY INFORMATIONAL
        ::= 28 -- 0x1C

bntSwFwDownloadSucess TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { bntSwTrapDisplayString,
                          sysName, sysLocation, sysContact }
        DESCRIPTION
                "A bntSwFwDownloadSuccess signifies that firmware
		 has been downloaded to [image1|image2|boot image]." 
	--#SEVERITY INFORMATIONAL
        ::= 29 -- 0x1D

bntSwFwDownloadFailure TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { bntSwTrapDisplayString,
                          sysName, sysLocation, sysContact }
        DESCRIPTION
                "A bntSwFwDownloadFailure signifies that firmware 
		 downloaded failed to [image1|image2|boot image]." 
	--#SEVERITY MINOR
        ::= 30 -- 0x1E

bntSwTempReturnThreshold TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { bntSwTrapDisplayString,
                          sysName, sysLocation, sysContact }
        DESCRIPTION
              "A bntSwTempReturnThreshold trap signifies that the
               switch temperature has returned below maximum safety limits."
        --#SEVERITY INFORMATIONAL
        ::= 31   -- 0x1F


bntSwUfdfoLtMFailure TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { bntSwTrapDisplayString,
                          sysName, sysLocation, sysContact }
        DESCRIPTION
               "A bntSwUfdfoLtMFailure trap signifies that a LtM link is down."
        --#SEVERITY MAJOR
        ::= 34 -- 0x22

bntSwUfdfoLtMUP TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { bntSwTrapDisplayString,
                          sysName, sysLocation, sysContact }
        DESCRIPTION
                "A bntSwUfdfoLtMUP trap signifies that a LtM link is up."
        --#SEVERITY INFORMATIONAL
        ::= 35 -- 0x23

bntSwUfdfoGlobalEna TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { bntSwTrapDisplayString,
                          sysName, sysLocation, sysContact }
        DESCRIPTION
                "A bntSwUfdfoGlobalEna trap signifies that Global UFD is enabled."
        --#SEVERITY INFORMATIONAL
        ::= 36 -- 0x24

bntSwUfdfoGlobalDis TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { bntSwTrapDisplayString,
                          sysName, sysLocation, sysContact }
        DESCRIPTION
                "A bntSwUfdfoGlobalDis trap signifies that Global UFD is disabled."
        --#SEVERITY INFORMATIONAL
        ::= 37 -- 0x25

bntSwUfdfoLtDAutoEna TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { bntSwTrapDisplayString,
                          sysName, sysLocation, sysContact }
        DESCRIPTION
                "A bntSwUfdfoLtDAutoEna trap signifies that a LtD link is Auto Enabled."
        --#SEVERITY INFORMATIONAL
        ::= 38 -- 0x26

bntSwUfdfoLtDAutoDis TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { bntSwTrapDisplayString,
                          sysName, sysLocation, sysContact }
        DESCRIPTION
                "A bntSwUfdfoLtDAutoDis trap signifies that a LtD link is Auto Disabled."
        --#SEVERITY INFORMATIONAL
        ::= 39 -- 0x27


bntSwStgNewRoot TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { bntSwTrapDisplayString, stgCurCfgIndex,
                          sysName, sysLocation, sysContact }
        DESCRIPTION
                "A bntSwStgNewRoot trap signifies that the bridge has become the new root of the STG."
        --#SEVERITY INFORMATIONAL
        ::= 42 -- 0x2A

bntSwCistNewRoot TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { bntSwTrapDisplayString,
                          sysName, sysLocation, sysContact }
        DESCRIPTION
                "A bntSwCistNewRoot trap signifies that the bridge has become the new root of the CIST."
        --#SEVERITY INFORMATIONAL
        ::= 43 -- 0x2B

bntSwStgTopologyChanged TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { bntSwTrapDisplayString, stgCurCfgIndex,
                          sysName, sysLocation, sysContact }
        DESCRIPTION
                "A bntSwStgTopologyChanged trap signifies that there was a STG topology change."
        --#SEVERITY INFORMATIONAL
        ::= 44 -- 0x2C

bntSwCistTopologyChanged TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { bntSwTrapDisplayString,
                          sysName, sysLocation, sysContact }
        DESCRIPTION
                "A bntSwCistTopologyChanged trap signifies that there was a CIST topology change."
        --#SEVERITY INFORMATIONAL
        ::= 45 -- 0x2D


bntSFPInserted       TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { bntSwTrapDisplayString, ifIndex,
                          sysName, sysLocation, sysContact }
        DESCRIPTION     "A bntSFPInserted trap signifies that a SFP is inserted."
        --#SEVERITY INFORMATIONAL
        ::= 51 -- 0x33

bntSFPRemoved       TRAP-TYPE
        ENTERPRISE      bntTraps
        VARIABLES       { bntSwTrapDisplayString, ifIndex,
                          sysName, sysLocation, sysContact }
        DESCRIPTION     "A bntSFPRemoved trap signifies that a SFP is removed."
        --#SEVERITY INFORMATIONAL
        ::= 52 -- 0x34

-- ----------------------------------------------------------------------------
-- } INSERT:  bt2trap
-- ----------------------------------------------------------------------------

-------------------------------------------------------------------------------
-- HP Platform Common Private MIBs
-------------------------------------------------------------------------------

-------------------------------------------------------------------------------
-- Feature Dependent Private MIBs
-------------------------------------------------------------------------------
acl                     OBJECT IDENTIFIER 
    ::= { hpSwitchBladeType5-Mgmt 9 }

-- ----------------------------------------------------------------------------
-- { INSERT:  bt2acl
-- ----------------------------------------------------------------------------

acConfig   OBJECT IDENTIFIER ::= { acl 1 }

acList      OBJECT IDENTIFIER ::= { acConfig 1 }
aclGroup    OBJECT IDENTIFIER ::= { acConfig 3 }
aclCfg      OBJECT IDENTIFIER ::= { acConfig 4 }

-- ---------------------------------------------------------- --
-- Access Control List (ACL) Configuration
-- ---------------------------------------------------------- --

aclCurCfgTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF AclCurCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table of current ACL configuration."
    ::= { acList 1 }

aclCurCfgEntry  OBJECT-TYPE
    SYNTAX      AclCurCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Current information about a particular ACL configuration entry."
    INDEX { aclCurCfgIndex }
    ::= { aclCurCfgTable 1 }

AclCurCfgEntry  ::= SEQUENCE {
    aclCurCfgIndex              Unsigned32,
    aclCurCfgGroup              Unsigned32,
    aclCurCfgFilterAction       INTEGER,
    aclCurCfgFilterActionSetPrio INTEGER,
    aclCurCfgEthFmt             INTEGER,
    aclCurCfgTagFmt             INTEGER,
    aclCurCfgIPFmt              INTEGER,
    aclCurCfgSrcMACAddress      MacAddress,
    aclCurCfgSrcMACMask         MacAddress,
    aclCurCfgDstMACAddress      MacAddress,
    aclCurCfgDstMACMask         MacAddress,
    aclCurCfgEthernetTypeName   INTEGER,
    aclCurCfgEthernetTypeValue  INTEGER,
    aclCurCfgVLanId             INTEGER,
    aclCurCfgVLanMask           DisplayString,
    aclCurCfg8021pPriority      INTEGER,
    aclCurCfgTypeOfService      DisplayString,
    aclCurCfgProtocol           DisplayString,
    aclCurCfgSrcIPAddress       IpAddress,
    aclCurCfgSrcIPMask          IpAddress,
    aclCurCfgDstIPAddress       IpAddress,
    aclCurCfgDstIPMask          IpAddress,
    aclCurCfgSrcPort            INTEGER,
    aclCurCfgSrcPortMask        DisplayString,
    aclCurCfgDstPort            INTEGER,
    aclCurCfgDstPortMask        DisplayString,
    aclCurCfgTCPFlags           BITS,
    aclCurCfgTCPFlagsMask       BITS,
    aclCurCfgEgressPorts        OCTET STRING,
    aclCurCfgStatistics         INTEGER,
    aclCurCfgMeterAction        INTEGER,
    aclCurCfgMeterEnable        INTEGER,
    aclCurCfgKbitsSec          	Unsigned32,
    aclCurCfgKbitsBurst        	INTEGER,
    aclCurCfgInprofUser      	INTEGER,
    aclCurCfgInprofDscp        	INTEGER,
    aclCurCfgInprofTos        	INTEGER,
    aclCurCfgOutprofDscp        INTEGER,
    aclCurCfgInprofUserEnable  	INTEGER,
    aclCurCfgInprofDscpEnable  	INTEGER,
    aclCurCfgOutprofDscpEnable  INTEGER
    }

aclCurCfgIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible 
    STATUS      current
    DESCRIPTION
        "The index associated with this ACL entry."
    ::= { aclCurCfgEntry 1 }


aclCurCfgGroup  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The index of the ACL group to which this ACL entry is a member of.
        A value of zero means the ACL is not a member of any group."
    ::= { aclCurCfgEntry 3 }

aclCurCfgFilterAction  OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    permit(1),
                    deny(2),
                    setprio(3)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The action to be performed on a packet that matches the filter
        settings of this ACL entry."
    ::= { aclCurCfgEntry 4 }

aclCurCfgFilterActionSetPrio  OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    prio0(1),
                    prio1(2),
                    prio2(3),
                    prio3(4),
                    prio4(5),
                    prio5(6),
                    prio6(7),
                    prio7(8)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value to be used when the action to be performed is setprio
        for this ACL entry."
    ::= { aclCurCfgEntry 5 }

aclCurCfgEthFmt  OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    ethernet2(1),
                    snap(2),
                    llc(3)
                    ,ieee802dot3(4)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The packet ethernet format to be filtered."
    ::= { aclCurCfgEntry 6 }

aclCurCfgTagFmt  OBJECT-TYPE
    SYNTAX      INTEGER {
                    disabled(1),
                    any(2),
                    untagged(3),
                    tagged(4)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The packet tag format to be filtered."
    ::= { aclCurCfgEntry 7 }

aclCurCfgIPFmt  OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(1),
                    ipv4(2),
                    ipv6(3)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The packet IP format to be filtered."
    ::= { aclCurCfgEntry 8 }

aclCurCfgSrcMACAddress  OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The source MAC address to be filtered."
    ::= { aclCurCfgEntry 9 }

aclCurCfgSrcMACMask  OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The address mask applied to aclCurCfgSrcMACAddress for filtering."
    ::= { aclCurCfgEntry 10 }

aclCurCfgDstMACAddress  OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The destination MAC address to be filtered."
    ::= { aclCurCfgEntry 11 }

aclCurCfgDstMACMask  OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The address mask applied to aclCurCfgDstMACAddress for filtering."
    ::= { aclCurCfgEntry 12 }

aclCurCfgEthernetTypeName  OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    arp(1),
                    ipv4(2),
                    ipv6(3),
                    mpls(4),
                    rarp(5),
                    any(6),
                    other(7)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The Ethernet type to be filtered. If the value of this
        object is other(7), the value of aclNewCfgEthernetTypeValue
        indicates the ethernet type that will be filtered."
    ::= { aclCurCfgEntry 13 }

aclCurCfgEthernetTypeValue  OBJECT-TYPE
    SYNTAX      INTEGER (1536..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The Ethernet type value to be filtered. The value of this
        object is equivalent to the value of aclNewCfgEthernetTypeName
        except when the value of aclNewCfgEthernetTypeName is other(7),
        which can be any user-defined value for this object."
    ::= { aclCurCfgEntry 14 }

aclCurCfgVLanId  OBJECT-TYPE
    SYNTAX      INTEGER (0..4095)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The virtual LAN identifier to be filtered."
    ::= { aclCurCfgEntry 15 }

aclCurCfgVLanMask  OBJECT-TYPE
    SYNTAX      DisplayString 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The mask applied to aclCurCfgVLanId for filtering."
    ::= { aclCurCfgEntry 16 }

aclCurCfg8021pPriority  OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    priority0(1),
                    priority1(2),
                    priority2(3),
                    priority3(4),
                    priority4(5),
                    priority5(6),
                    priority6(7),
                    priority7(8)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The 802.1p priority to be filtered."
    ::= { aclCurCfgEntry 17 }

aclCurCfgTypeOfService  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The type of service to be filtered."
    ::= { aclCurCfgEntry 18 }

aclCurCfgProtocol  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The protocol to be filtered."
    ::= { aclCurCfgEntry 19 }

aclCurCfgSrcIPAddress  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The source IP address to be filtered."
    ::= { aclCurCfgEntry 20 }

aclCurCfgSrcIPMask  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The address mask applied to aclCurCfgSrcIPAddress for filtering."
    ::= { aclCurCfgEntry 21 }

aclCurCfgDstIPAddress  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The destination IP address to be filtered."
    ::= { aclCurCfgEntry 22 }

aclCurCfgDstIPMask  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The address mask applied to aclCurCfgDstIPAddress for filtering."
    ::= { aclCurCfgEntry 23 }

aclCurCfgSrcPort  OBJECT-TYPE
    SYNTAX      INTEGER (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The source TCP/UDP port number to be filtered."
    ::= { aclCurCfgEntry 24 }

aclCurCfgSrcPortMask  OBJECT-TYPE
    SYNTAX      DisplayString 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The mask applied to aclCurCfgSrcPort for filtering."
    ::= { aclCurCfgEntry 25 }

aclCurCfgDstPort  OBJECT-TYPE
    SYNTAX      INTEGER (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The destination TCP/UDP port number to be filtered."
    ::= { aclCurCfgEntry 26 }

aclCurCfgDstPortMask  OBJECT-TYPE
    SYNTAX      DisplayString 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The mask applied to aclCurCfgDstPort for filtering."
    ::= { aclCurCfgEntry 27 }

aclCurCfgTCPFlags  OBJECT-TYPE
    SYNTAX      BITS {
                    reserved1(0),
                    reserved2(1),
                    tcpURG(2),
                    tcpACK(3),
                    tcpPSH(4),
                    tcpRST(5),
                    tcpSYN(6),
                    tcpFIN(7)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The TCP flags to be filtered.
         OCTET
         xxxxxxxx
         ||||..||
         ||||..||_tcpFIN(7)
         ||||..|__tcpSYN(6)
         ||||
         ||||_____tcpACK(3)
         |||______tcpURG(2)
         ||_______reserved2(1)
         |________reserved1(0)

         where:
         - reserved1 - 0;
         - reserved2 - 0;
         - x - 0 or 1;
        "
    ::= { aclCurCfgEntry 28 }

aclCurCfgTCPFlagsMask  OBJECT-TYPE
    SYNTAX      BITS {
                    reserved1(0),
                    reserved2(1),
                    tcpURG(2),
                    tcpACK(3),
                    tcpPSH(4),
                    tcpRST(5),
                    tcpSYN(6),
                    tcpFIN(7)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The TCP flags mask.
         OCTET
         xxxxxxxx
         ||||..||
         ||||..||_tcpFIN(7)
         ||||..|__tcpSYN(6)
         ||||
         ||||_____tcpACK(3)
         |||______tcpURG(2)
         ||_______reserved2(1)
         |________reserved1(0)

         where:
         - reserved1 - 0;
         - reserved2 - 0;
         - x - 0 or 1;
        "
    ::= { aclCurCfgEntry 39 }

aclCurCfgEgressPorts  OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The port list in the ACL configured for egress filtering.
         The ports are presented in bitmap format, as follows:

            OCTET 1  OCTET 2  .....
            xxxxxxxx xxxxxxxx .....
            ||    || |
            ||    || |_ port 9
            ||    ||
            ||    ||___ port 8
            ||    |____ port 7
            ||      .    .   .
            ||_________ port 2
            |__________ port 1

         where x:
            1 - the represented port is configured for filtering.
            0 - the represented port is not configured for filtering."
    ::= { aclCurCfgEntry 29 }

aclCurCfgStatistics  OBJECT-TYPE
    SYNTAX      INTEGER {
                    disable(0),
                    enable(1)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Whether statistics collection for this ACL is enabled or not."
    ::= { aclCurCfgEntry 30 }

aclCurCfgMeterAction  OBJECT-TYPE
    SYNTAX      INTEGER {
					unconfigured(0),
					outdrop(1),
					outpass(2)
				}
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Meter Action for this ACL."
    ::= { aclCurCfgEntry 41 }

aclCurCfgMeterEnable  OBJECT-TYPE
    SYNTAX      INTEGER {
	enabled(0),
	disabled(1)
				}
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Meter state for this ACL."
    ::= { aclCurCfgEntry 42 }

aclCurCfgKbitsSec  OBJECT-TYPE
    SYNTAX      Unsigned32 (64..10000000)
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
        "The commited rate of meter associated with this ACL entry."
    ::= { aclCurCfgEntry 43 }

aclCurCfgKbitsBurst  OBJECT-TYPE
    SYNTAX      INTEGER {
					kbits32(32),
					kbits64(64),
					kbits128(128),
					kbits256(256),
					kbits512(512),
					kbits1024(1024),
					kbits2048(2048),
					kbits4096(4096)
   				} 
	MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
        "The maxmium burst sizeof meter associated with this ACL entry."
    ::= { aclCurCfgEntry 44 }

aclCurCfgInprofUser  OBJECT-TYPE
    SYNTAX      INTEGER (0..7)
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
        "Set in profile user defined priority for this ACL."
    ::= { aclCurCfgEntry 45 }

aclCurCfgInprofDscp  OBJECT-TYPE
    SYNTAX      INTEGER (0..63)
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
        "Set in profile pkts DSCP value."
    ::= { aclCurCfgEntry 46 }

aclCurCfgInprofTos  OBJECT-TYPE
    SYNTAX      INTEGER {
                    disable(0),
                    enable(1)
                }
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
        "To enable/disable setting in profile pkts based on TOS bits."
    ::= { aclCurCfgEntry 47 }

aclCurCfgOutprofDscp  OBJECT-TYPE
    SYNTAX      INTEGER (0..63)
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
        "Set out profile pkts DSCP value."
    ::= { aclCurCfgEntry 48 }

aclCurCfgInprofUserEnable  OBJECT-TYPE
    SYNTAX      INTEGER {
				    disabled(0),	
					userdefined(1)
				}
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
        "Set in profile update method for this ACL."
    ::= { aclCurCfgEntry 49 }

aclCurCfgInprofDscpEnable  OBJECT-TYPE
    SYNTAX      INTEGER {
                    disable(0),
                    enable(1)
                }
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
        "Whether in profile update DSCP for this ACL is enabled or not."
    ::= { aclCurCfgEntry 50 }

aclCurCfgOutprofDscpEnable  OBJECT-TYPE
    SYNTAX      INTEGER {
                    disable(0),
                    enable(1)
                }
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
        "Whether out profile update DSCP for this ACL is enabled or not."
    ::= { aclCurCfgEntry 51 }


--
-- New ACL Configuration Table
--

aclNewCfgTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AclNewCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table of new ACL configuration."
    ::= { acList 2 }

aclNewCfgEntry OBJECT-TYPE
    SYNTAX      AclNewCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "New information about a particular ACL configuration."
    INDEX { aclNewCfgIndex }
    ::= { aclNewCfgTable 1 }

AclNewCfgEntry ::= SEQUENCE {
    aclNewCfgIndex              Unsigned32,
    aclNewCfgGroup              Unsigned32,
    aclNewCfgFilterAction       INTEGER,
    aclNewCfgFilterActionSetPrio INTEGER,
    aclNewCfgEthFmt       INTEGER,
    aclNewCfgTagFmt       INTEGER,
    aclNewCfgIPFmt        INTEGER,
    aclNewCfgSrcMACAddress      MacAddress,
    aclNewCfgSrcMACMask         MacAddress,
    aclNewCfgDstMACAddress      MacAddress,
    aclNewCfgDstMACMask         MacAddress,
    aclNewCfgEthernetTypeName   INTEGER,
    aclNewCfgEthernetTypeValue  INTEGER,
    aclNewCfgVLanId             INTEGER,
    aclNewCfgVLanMask           DisplayString,
    aclNewCfg8021pPriority      INTEGER,
    aclNewCfgTypeOfService      DisplayString,
    aclNewCfgProtocol           DisplayString,
    aclNewCfgSrcIPAddress       IpAddress,
    aclNewCfgSrcIPMask          IpAddress,
    aclNewCfgDstIPAddress       IpAddress,
    aclNewCfgDstIPMask          IpAddress,
    aclNewCfgSrcPort            INTEGER,
    aclNewCfgSrcPortMask        DisplayString,
    aclNewCfgDstPort            INTEGER,
    aclNewCfgDstPortMask        DisplayString,
    aclNewCfgTCPFlags           BITS,
    aclNewCfgTCPFlagsMask       BITS,
    aclNewCfgEgressPorts        OCTET STRING,
    aclNewCfgStatistics         INTEGER,
    aclNewCfgAddEgressPort      INTEGER,
    aclNewCfgRemoveEgressPort   Unsigned32,
    aclNewCfgDelete             INTEGER,
    aclNewCfgMeterAction        INTEGER,
    aclNewCfgMeterEnable        INTEGER,
    aclNewCfgKbitsSec          	Unsigned32,
    aclNewCfgKbitsBurst        	INTEGER,
    aclNewCfgInprofUser      	INTEGER,
    aclNewCfgInprofDscp        	INTEGER,
    aclNewCfgInprofTos        	INTEGER,
    aclNewCfgOutprofDscp        INTEGER,
    aclNewCfgInprofUserEnable  	INTEGER,
    aclNewCfgInprofDscpEnable  	INTEGER,
    aclNewCfgOutprofDscpEnable  INTEGER,
    aclNewCfgReset		INTEGER,
    aclNewCfgEthernetReset      INTEGER,
    aclNewCfgIpv4Reset          INTEGER,
    aclNewCfgTcpudpReset        INTEGER,
    aclNewCfgMeterReset         INTEGER,
    aclNewCfgRemarkReset        INTEGER,
    aclNewCfgRemarkInprofReset  INTEGER,
    aclNewCfgRemarkOutprofReset INTEGER,
    aclNewCfgPktfmtReset        INTEGER
    }

aclNewCfgIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The index associated with this ACL entry."
    ::= { aclNewCfgEntry 1 }


aclNewCfgGroup  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The index of the ACL group to which this ACL entry is a member of.
        A value of zero means the ACL is not a member of any group."
    ::= { aclNewCfgEntry 3 }

aclNewCfgFilterAction  OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    permit(1),
                    deny(2),
                    setprio(3)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The action to be performed on a packet that matches the filter
        settings of this ACL entry."
    ::= { aclNewCfgEntry 4 }

aclNewCfgFilterActionSetPrio  OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    prio0(1),
                    prio1(2),
                    prio2(3),
                    prio3(4),
                    prio4(5),
                    prio5(6),
                    prio6(7),
                    prio7(8)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The COS queue to be used when the action for this ACL entry is
        set to setprio."
    ::= { aclNewCfgEntry 5 }

aclNewCfgEthFmt  OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    ethernet2(1),
                    snap(2),
                    llc(3)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The packet ethernet format to be filtered."
    ::= { aclNewCfgEntry 6 }

aclNewCfgTagFmt  OBJECT-TYPE
    SYNTAX      INTEGER {
                    disabled(1),
                    any(2),
                    none(3),
                    tagged(4)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The packet tagging format to be filtered."
    ::= { aclNewCfgEntry 7 }
    
aclNewCfgIPFmt  OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(1),
                    ipv4(2),
                    ipv6(3)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The packet IP format to be filtered."
    ::= { aclNewCfgEntry 8 }

aclNewCfgSrcMACAddress  OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The source MAC address to be filtered. Whenever this object is
        set to a nonzero value, the aclNewCfgSrcMACMask object, if not
        yet set, will be automatically set to ff:ff:ff:ff:ff."
    ::= { aclNewCfgEntry 9 }

aclNewCfgSrcMACMask  OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The address mask to be applied to aclNewCfgSrcMACAddress
         for filtering."
    ::= { aclNewCfgEntry 10 }

aclNewCfgDstMACAddress  OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The destination MAC address to be filtered. Whenever this object
        is set to a nonzero value, the aclNewCfgDstMACMask object, if not
        yet set, will be automatically set to ff:ff:ff:ff:ff."
    ::= { aclNewCfgEntry 11 }

aclNewCfgDstMACMask  OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The address mask to be applied to aclNewCfgDstMACAddress
         for filtering."
    ::= { aclNewCfgEntry 12 }

aclNewCfgEthernetTypeName  OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    arp(1),
                    ipv4(2),
                    ipv6(3),
                    mpls(4),
                    rarp(5),
                    any(6),
                    other(7)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The Ethernet type to be filtered. If the value of this
        object is other(7), the value of aclNewCfgEthernetTypeValue
        indicates the ethernet type that will be filtered. If this
        object is set to a value other than other(7), the value of
        the aclNewCfgEthernetTypeValue object is automatically set,
        as follows:

        aclNewCfgEthernetTypeName   aclNewCfgEthernetTypeValue
            none(0)                         0
            arp(1)                       2054  (0x0806)
            ipv4(2)                      2048  (0x0800)
            ipv6(3)                     34525  (0x86dd)
            mpls(4)                     34887  (0x8847)
            rarp(5)                     32821  (0x8035)
            any(6)                      65535  (0xffff)
        "
    ::= { aclNewCfgEntry 13 }

aclNewCfgEthernetTypeValue  OBJECT-TYPE
    SYNTAX      INTEGER (1536..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The Ethernet type value to be filtered. The value of this
        object is equivalent to the value of aclNewCfgEthernetTypeName
        except when the value of aclNewCfgEthernetTypeName is other(7),
        which can be any user-defined value for this object."
    ::= { aclNewCfgEntry 14 }

aclNewCfgVLanId  OBJECT-TYPE
    SYNTAX      INTEGER (1..4095)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The virtual LAN identifier to be filtered. Whenever this object
        is set to a nonzero value, the aclNewCfgVLanMask object, if not
        yet set, will be automatically set to 4095 (0xfff)."
    ::= { aclNewCfgEntry 15 }

aclNewCfgVLanMask  OBJECT-TYPE
    SYNTAX      DisplayString 
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The mask to be applied to aclNewCfgVLanId for filtering."
    ::= { aclNewCfgEntry 16 }

aclNewCfg8021pPriority  OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    priority0(1),
                    priority1(2),
                    priority2(3),
                    priority3(4),
                    priority4(5),
                    priority5(6),
                    priority6(7),
                    priority7(8)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The 802.1p priority to be filtered."
    ::= { aclNewCfgEntry 17 }

aclNewCfgTypeOfService  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The type of service to be filtered."
    ::= { aclNewCfgEntry 18 }

aclNewCfgProtocol  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The protocol to be filtered."
    ::= { aclNewCfgEntry 19 }

aclNewCfgSrcIPAddress  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The source IP address to be filtered. Whenever this object is set
        to a nonzero value, the aclNewCfgSrcIPMask object, if not yet set,
        will be automatically set to 255.255.255.255."
    ::= { aclNewCfgEntry 20 }

aclNewCfgSrcIPMask  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The address mask to be applied to aclNewCfgSrcIPAddress
         for filtering."
    ::= { aclNewCfgEntry 21 }

aclNewCfgDstIPAddress  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The destination IP address to be filtered. Whenever this object is set
        to a nonzero value, the aclNewCfgDstIPMask object, if not yet set,
        will be automatically set to 255.255.255.255."
    ::= { aclNewCfgEntry 22 }

aclNewCfgDstIPMask  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The address mask to be applied to aclNewCfgDstIPAddress for filtering."
    ::= { aclNewCfgEntry 23 }

aclNewCfgSrcPort  OBJECT-TYPE
    SYNTAX      INTEGER (1..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The source TCP/UDP port number to be filtered. Whenever this
        object is set if the aclNewCfgSrcPortMask object is not set
        will be automatically set to 65535 (0xffff)."
    ::= { aclNewCfgEntry 24 }

aclNewCfgSrcPortMask  OBJECT-TYPE
    SYNTAX      DisplayString 
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The mask to be applied to aclNewCfgSrcPort for filtering."
    ::= { aclNewCfgEntry 25 }

aclNewCfgDstPort  OBJECT-TYPE
    SYNTAX      INTEGER (1..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The destination TCP/UDP port number to be filtered.  Whenever this
        object is set the aclNewCfgSrcPortMask object, if not yet set, will 
        be automatically set to 65535 (0xffff)."
    ::= { aclNewCfgEntry 26 }

aclNewCfgDstPortMask  OBJECT-TYPE
    SYNTAX      DisplayString 
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The mask to be applied to aclNewCfgDstPort for filtering."
    ::= { aclNewCfgEntry 27 }

aclNewCfgTCPFlags  OBJECT-TYPE
    SYNTAX      BITS {
                    reserved1(0),
                    reserved2(1),
                    tcpURG(2),
                    tcpACK(3),
                    tcpPSH(4),
                    tcpRST(5),
                    tcpSYN(6),
                    tcpFIN(7)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The TCP flags to be filtered.
         The TCP flags are presented in bitmap format, as follows:
         OCTET
         xxxxxxxx
         ||||..||
         ||||..||_tcpFIN(7)
         ||||..|__tcpSYN(6)
         ||||
         ||||_____tcpACK(3)
         |||______tcpURG(2)
         ||_______reserved2(1)
         |________reserved1(0)

         where:
         - reserved1 - 0;
         - reserved2 - 0;
         - x - 0 or 1;
        "
    ::= { aclNewCfgEntry 28 }

aclNewCfgTCPFlagsMask  OBJECT-TYPE
    SYNTAX      BITS {
                    reserved1(0),
                    reserved2(1),
                    tcpURG(2),
                    tcpACK(3),
                    tcpPSH(4),
                    tcpRST(5),
                    tcpSYN(6),
                    tcpFIN(7)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The TCP flags mask.
         The TCP flags are presented in bitmap format, as follows:
         OCTET
         xxxxxxxx
         ||||..||
         ||||..||_tcpFIN(7)
         ||||..|__tcpSYN(6)
         ||||
         ||||_____tcpACK(3)
         |||______tcpURG(2)
         ||_______reserved2(1)
         |________reserved1(0)

         where:
         - reserved1 - 0;
         - reserved2 - 0;
         - x - 0 or 1;
         Default value is 0x3f."
    ::= { aclNewCfgEntry 39 }

aclNewCfgEgressPorts  OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The port list in the ACL configured for egress filtering.
         The ports are presented in bitmap format, as follows:

            OCTET 1  OCTET 2  .....
            xxxxxxxx xxxxxxxx .....
            ||    || |
            ||    || |_ port 9
            ||    ||
            ||    ||___ port 8
            ||    |____ port 7
            ||      .    .   .
            ||_________ port 2
            |__________ port 1

         where x:
            1 - the represented port is configured for filtering.
            0 - the represented port is not configured for filtering."
    ::= { aclNewCfgEntry 29 }

aclNewCfgStatistics  OBJECT-TYPE
    SYNTAX      INTEGER {
                    disable(0),
                    enable(1)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Whether statistics collection for this ACL is enabled or not."
    ::= { aclNewCfgEntry 30 }

aclNewCfgAddEgressPort OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The port to be added to the specified ACL for egress filtering.
        A value of zero is always returned when this object is read."
    ::= { aclNewCfgEntry 31 }

aclNewCfgRemoveEgressPort OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The port to be removed from the specified ACL.  A value of zero
        is always returned when this object is read."
    ::= { aclNewCfgEntry 32 }

aclNewCfgDelete OBJECT-TYPE
    SYNTAX      INTEGER {
                    other(1),
                    delete(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This is an action object to delete an ACL entry.  A value of
        other(1) is always returned when this object is read."
    ::= { aclNewCfgEntry 33 }

aclNewCfgMeterAction  OBJECT-TYPE
    SYNTAX      INTEGER {
					unconfigured(0),
					outdrop(1),
					outpass(2)
				}
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Meter Action for this ACL."
    ::= { aclNewCfgEntry 41 }

aclNewCfgMeterEnable  OBJECT-TYPE
    SYNTAX      INTEGER {
	enabled(0),
	disabled(1)
				}		
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Meter state for this ACL."
    ::= { aclNewCfgEntry 42 }

aclNewCfgKbitsSec  OBJECT-TYPE
    SYNTAX      Unsigned32 (1000..10000000)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The commited rate of meter associated with this ACL entry."
    ::= { aclNewCfgEntry 43 }

aclNewCfgKbitsBurst  OBJECT-TYPE
    SYNTAX      INTEGER {
					kbits32(32),
					kbits64(64),
					kbits128(128),
					kbits256(256),
					kbits512(512),
					kbits1024(1024),
					kbits2048(2048),
					kbits4096(4096)
   				} 
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The maxmium burst sizeof meter associated with this ACL entry."
    ::= { aclNewCfgEntry 44 }

aclNewCfgInprofUser  OBJECT-TYPE
    SYNTAX      INTEGER (0..7)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Set in profile user defined priority for this ACL."
    ::= { aclNewCfgEntry 45 }

aclNewCfgInprofDscp  OBJECT-TYPE
    SYNTAX      INTEGER (0..63)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Set in profile pkts DSCP value."
    ::= { aclNewCfgEntry 46 }

aclNewCfgInprofTos  OBJECT-TYPE
    SYNTAX      INTEGER {
                    disable(0),
                    enable(1)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "To enable/disable setting in profile pkts based on TOS bits."
    ::= { aclNewCfgEntry 47 }

aclNewCfgOutprofDscp  OBJECT-TYPE
    SYNTAX      INTEGER (0..63)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Set out profile pkts DSCP value."
    ::= { aclNewCfgEntry 48 }

aclNewCfgInprofUserEnable  OBJECT-TYPE
    SYNTAX      INTEGER {
				    disabled(0),	
					userdefined(1)
				}
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Set in profile update method for this ACL."
    ::= { aclNewCfgEntry 49 }

aclNewCfgInprofDscpEnable  OBJECT-TYPE
    SYNTAX      INTEGER {
                    disable(0),
                    enable(1)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Whether in profile update DSCP for this ACL is enabled or not."
    ::= { aclNewCfgEntry 50 }

aclNewCfgOutprofDscpEnable  OBJECT-TYPE
    SYNTAX      INTEGER {
                    disable(0),
                    enable(1)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Whether out profile update DSCP for this ACL is enabled or not."
    ::= { aclNewCfgEntry 51 }

aclNewCfgReset OBJECT-TYPE
    SYNTAX      INTEGER {
                    other(1),
                    reset(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This is an action object to reset an ACL entry.  A value of
        other(1) is always returned when this object is read."
    ::= { aclNewCfgEntry 52 } 

aclNewCfgEthernetReset OBJECT-TYPE
    SYNTAX      INTEGER {
                    other(1),
                    reset(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This is an action object to reset an ACL Ethernet entry. A value of
        other(1) is always returned when this object is read."
    ::= { aclNewCfgEntry 53 }

aclNewCfgIpv4Reset OBJECT-TYPE
    SYNTAX      INTEGER {
                    other(1),
                    reset(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This is an action object to reset an ACL IPV4 entry. A value of
        other(1) is always returned when this object is read."
    ::= { aclNewCfgEntry 54 }

aclNewCfgTcpudpReset OBJECT-TYPE
    SYNTAX      INTEGER {
                    other(1),
                    reset(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This is an action object to reset an ACL Tcpudp entry. A value of
        other(1) is always returned when this object is read."
    ::= { aclNewCfgEntry 55 } 

aclNewCfgMeterReset OBJECT-TYPE
    SYNTAX      INTEGER {
                    other(1),
                    reset(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This is an action object to reset an ACL Meter entry. A value of
        other(1) is always returned when this object is read."
    ::= { aclNewCfgEntry 56 }

aclNewCfgRemarkReset OBJECT-TYPE
    SYNTAX      INTEGER {
                    other(1),
                    reset(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This is an action object to reset an ACL Remark entry. A value of
        other(1) is always returned when this object is read."
    ::= { aclNewCfgEntry 57 }    

aclNewCfgRemarkInprofReset OBJECT-TYPE
    SYNTAX      INTEGER {
                    other(1),
                    reset(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This is an action object to reset an ACL Remark Inprof entry. A value of
        other(1) is always returned when this object is read."
    ::= { aclNewCfgEntry 58 }

aclNewCfgRemarkOutprofReset OBJECT-TYPE
    SYNTAX      INTEGER {
                    other(1),
                    reset(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This is an action object to reset an ACL Remark Outprof entry. A value of
        other(1) is always returned when this object is read."
    ::= { aclNewCfgEntry 59 }

aclNewCfgPktfmtReset OBJECT-TYPE
    SYNTAX      INTEGER {
                    other(1),
                    reset(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This is an action object to reset an ACL Pktfmt entry. A value of
        other(1) is always returned when this object is read."
    ::= { aclNewCfgEntry 60 }


-- ---------------------------------------------------------- --
-- ACL Group Configuration
-- ---------------------------------------------------------- --

aclGroupCurCfgTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AclGroupCurCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table of current ACL Group configuration."
    ::= { aclGroup 1 }

aclGroupCurCfgEntry OBJECT-TYPE
    SYNTAX      AclGroupCurCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information about a particular ACL configuration."
    INDEX { aclGroupCurCfgIndex }
    ::= { aclGroupCurCfgTable 1 }

AclGroupCurCfgEntry ::= SEQUENCE {
    aclGroupCurCfgIndex        Unsigned32,
    aclGroupCurCfgMemberAcls   OCTET STRING
    }

aclGroupCurCfgIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The index associated with this ACL Group entry."
    ::= { aclGroupCurCfgEntry 1 }

aclGroupCurCfgMemberAcls  OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The ACL members of this ACL group, presented in bitmap
         format, as follows:

            OCTET 1  OCTET 2  .....
            xxxxxxxx xxxxxxxx .....
            ||    || |
            ||    || |_ ACL 9
            ||    ||
            ||    ||___ ACL 8
            ||    |____ ACL 7
            ||      .    .   .
            ||_________ ACL 2
            |__________ ACL 1

         where x:
            1 - the represented ACL is a member of the group.
            0 - the represented ACL is not a member of the group."
    ::= { aclGroupCurCfgEntry 2 }


aclGroupNewCfgTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF AclGroupNewCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table of new ACL Group configuration."
    ::= { aclGroup 2 }

aclGroupNewCfgEntry OBJECT-TYPE
    SYNTAX      AclGroupNewCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "New information about a particular ACL configuration."
    INDEX { aclGroupNewCfgIndex }
    ::= { aclGroupNewCfgTable 1 }

AclGroupNewCfgEntry ::= SEQUENCE {
    aclGroupNewCfgIndex        Unsigned32,
    aclGroupNewCfgMemberAcls   OCTET STRING,
    aclGroupNewCfgAddAcl       Unsigned32,
    aclGroupNewCfgRemoveAcl    Unsigned32,
    aclGroupNewCfgDelete       INTEGER
    }

aclGroupNewCfgIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The index associated with this ACL Group entry."
    ::= { aclGroupNewCfgEntry 1 }

aclGroupNewCfgMemberAcls  OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The ACL members of this ACL group, presented in bitmap
         format, as follows:

            OCTET 1  OCTET 2  .....
            xxxxxxxx xxxxxxxx .....
            ||    || |
            ||    || |_ ACL 9
            ||    ||
            ||    ||___ ACL 8
            ||    |____ ACL 7
            ||      .    .   .
            ||_________ ACL 2
            |__________ ACL 1

         where x:
            1 - the represented ACL is a member of the group.
            0 - the represented ACL is not a member of the group."
    ::= { aclGroupNewCfgEntry 2 }


aclGroupNewCfgAddAcl  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The index of the ACL entry to be added into this ACL group.
        A successful set operation on this object will also set the bit
        corresponding to the ACL entry in the aclGroupNewCfgMemberAcls
        bitmap. A value of zero is always returned when this object
        is read."
    ::= { aclGroupNewCfgEntry 4 }

aclGroupNewCfgRemoveAcl  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The index of the ACL entry to be removed from this ACL group.
        A successful set operation on this object will unset the bit
        corresponding to the ACL entry in the aclGroupNewCfgMemberAcls
        bitmap. A value of zero is always returned when this object
        is read."
    ::= { aclGroupNewCfgEntry 5 }


aclGroupNewCfgDelete  OBJECT-TYPE
    SYNTAX      INTEGER {
                    other(1),
                    delete(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This is an action object to delete an ACL group.  A value of other(1)
        is always returned when this object is read."
    ::= { aclGroupNewCfgEntry 8 }

aclCurCfgPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AclCurCfgPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of port acl groups configuration."
    ::= { aclCfg 1 }

aclCurCfgPortTableEntry OBJECT-TYPE
    SYNTAX AclCurCfgPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a particular port acl configuration."
    INDEX { aclCurCfgPortIndex }
    ::= { aclCurCfgPortTable 1 }

AclCurCfgPortTableEntry ::= SEQUENCE {
    aclCurCfgPortIndex    Integer32,
    aclCurCfgPortAclBmap  OCTET STRING,
    aclCurCfgPortAclGrpBmap  OCTET STRING
    }

aclCurCfgPortIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The identifier of a particular port.  This is also
         index to the entLogicalTable of Entity MIB."
    ::= { aclCurCfgPortTableEntry 1 }

aclCurCfgPortAclBmap OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(0..512))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The acls applied to the port.  The acls are
         presented in bitmap format. This string displays acl number
         from 1 to 896.

         in receiving order:

             OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             ||    || |_ acl 9
             ||    ||
             ||    ||___ acl 8
             ||    |____ acl 7
             ||      .    .   .
             ||_________ acl 2
             |__________ acl 1

         where x : 1 - The represented acl applied to the port.
                   0 - The represented acl not applied to the port."
    ::= { aclCurCfgPortTableEntry 2 }



aclCurCfgPortAclGrpBmap OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(0..512))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The acl groups applied to the port.  The acls are
         presented in bitmap format. This string displays acl number
         from 1 to 896.
         in receiving order:

             OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             ||    || |_ aclgrp 9
             ||    ||
             ||    ||___ aclgrp 8
             ||    |____ aclgrp 7
             ||      .    .   .
             ||_________ aclgrp 2
             |__________ aclgrp 1

         where x : 1 - The represented acl applied to the port.
                   0 - The represented acl not applied to the port."
    ::= { aclCurCfgPortTableEntry 4 }

aclNewCfgPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF AclNewCfgPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of port acl configuration."
    ::= { aclCfg 2 }

aclNewCfgPortTableEntry OBJECT-TYPE
    SYNTAX AclNewCfgPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a particular port acl groups configuration."
    INDEX { aclNewCfgPortIndex }
    ::= { aclNewCfgPortTable 1 }

AclNewCfgPortTableEntry ::= SEQUENCE {
    aclNewCfgPortIndex         Integer32,
    aclNewCfgPortAddAcl        Unsigned32,
    aclNewCfgPortAddAclGrp     Unsigned32,
    aclNewCfgPortRemoveAcl     Unsigned32,
    aclNewCfgPortRemoveAclGrp  Unsigned32,
    aclNewCfgPortAclBmap       OCTET STRING,
    aclNewCfgPortAclGrpBmap    OCTET STRING
    }

aclNewCfgPortIndex  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The identifier of a particular port. This is also
         index to the entLogicalTable of Entity MIB."
    ::= { aclNewCfgPortTableEntry 1 }

aclNewCfgPortAddAcl OBJECT-TYPE
    SYNTAX  Unsigned32
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The acl to be added to the specified port.  A
         '0' value is returned when read."
    ::= {aclNewCfgPortTableEntry 2 }


aclNewCfgPortAddAclGrp OBJECT-TYPE
    SYNTAX  Unsigned32
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The acl group to be added to the specified port.  A
         '0' value is returned when read."
    ::= {aclNewCfgPortTableEntry 4 }

aclNewCfgPortRemoveAcl OBJECT-TYPE
    SYNTAX  Unsigned32
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The acl to be removed from the specified port.
         A '0' value is returned when read."
    ::= { aclNewCfgPortTableEntry 5 }


aclNewCfgPortRemoveAclGrp OBJECT-TYPE
    SYNTAX  Unsigned32
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The acl group to be removed from the specified port.
         A '0' value is returned when read."
    ::= { aclNewCfgPortTableEntry 7 }

aclNewCfgPortAclBmap OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(0..512))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The acls applied to the port.  The acls are
         presented in bitmap format. This string displays acl number
         from 1 to 896.
         in receiving order:

             OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             ||    || |_ acl 9
             ||    ||
             ||    ||___ acl 8
             ||    |____ acl 7
             ||      .    .   .
             ||_________ acl 2
             |__________ acl 1

         where x : 1 - The represented acl applied to the port.
                   0 - The represented acl not applied to the port."
    ::= { aclNewCfgPortTableEntry 8 }


aclNewCfgPortAclGrpBmap OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(0..512))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The acl groups applied to the port.  The acl groups are
         presented in bitmap format. This string displays group number
         from 1 to 4096.

         in receiving order:

             OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             ||    || |_ aclgrp 9
             ||    ||
             ||    ||___ aclgrp 8
             ||    |____ aclgrp 7
             ||      .    .   .
             ||_________ aclgrp 2
             |__________ aclgrp 1

         where x : 1 - The represented acl group applied to the port.
                   0 - The represented acl group not applied to the port."
    ::= { aclNewCfgPortTableEntry 10 }

-- ----------------------------------------------------------------------------
-- } INSERT:  bt2acl
-- ----------------------------------------------------------------------------


qos                     OBJECT IDENTIFIER
    ::= { hpSwitchBladeType5-Mgmt 8 }

-- ----------------------------------------------------------------------------
-- { INSERT:  bt2qos
-- ----------------------------------------------------------------------------

qosConfigs     OBJECT IDENTIFIER ::= { qos 1 }
qosStats       OBJECT IDENTIFIER ::= { qos 2 }
qosInfo        OBJECT IDENTIFIER ::= { qos 3 }
qosOper        OBJECT IDENTIFIER ::= { qos 4 }

qos8021p   OBJECT IDENTIFIER ::= { qosConfigs 1 }
-- QOS Configuration 

qosCurCfgPortPriorityTable OBJECT-TYPE
    SYNTAX SEQUENCE OF QoSCurCfgPortPriorityEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of QOS Port Priority configuration."
    ::= { qos8021p  1 }

qosCurCfgPortPriorityEntry OBJECT-TYPE
    SYNTAX QoSCurCfgPortPriorityEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a particular QOS Port Priority configuration."
    INDEX { qosCurCfgPortIndex }
    ::= { qosCurCfgPortPriorityTable 1 }

QoSCurCfgPortPriorityEntry ::= SEQUENCE {
    qosCurCfgPortIndex      Integer32,
    qosCurCfgPortPriority   INTEGER
    }

qosCurCfgPortIndex  OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Switch Port Number"
    ::= { qosCurCfgPortPriorityEntry 1 }

qosCurCfgPortPriority  OBJECT-TYPE
    SYNTAX  INTEGER  (0..7)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Switch Port Priority Should be between 0 and 7"
    ::= { qosCurCfgPortPriorityEntry 2 }

qosNewCfgPortPriorityTable OBJECT-TYPE
    SYNTAX SEQUENCE OF QoSNewCfgPortPriorityEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of QOS Port Priority configuration."
    ::= { qos8021p  2 }

qosNewCfgPortPriorityEntry OBJECT-TYPE
    SYNTAX QoSNewCfgPortPriorityEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a particular QOS Port Priority configuration."
    INDEX { qosNewCfgPortIndex }
    ::= { qosNewCfgPortPriorityTable 1 }

QoSNewCfgPortPriorityEntry ::= SEQUENCE {
    qosNewCfgPortIndex      Integer32,
    qosNewCfgPortPriority   INTEGER
    }

qosNewCfgPortIndex  OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Switch Port Number"
    ::= { qosNewCfgPortPriorityEntry 1 }

qosNewCfgPortPriority  OBJECT-TYPE
    SYNTAX  INTEGER  (0..7)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Switch Port Priority Should be between 0 and 7"
    ::= { qosNewCfgPortPriorityEntry 2 }

qosCurCfgPriorityCoSTable OBJECT-TYPE
    SYNTAX SEQUENCE OF QoSCurCfgPriorityCoSEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of Frame Priority and COSq configuration."
    ::= { qos8021p  3 }

qosCurCfgPriorityCoSEntry OBJECT-TYPE
    SYNTAX QoSCurCfgPriorityCoSEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a particular Frame Priority and COSq configuration."
    INDEX { qosCurCfgPriorityIndex }
    ::= { qosCurCfgPriorityCoSTable 1 }

QoSCurCfgPriorityCoSEntry ::= SEQUENCE {
    qosCurCfgPriorityIndex INTEGER,
    qosCurCfgPriorityCoSq  INTEGER
    }

qosCurCfgPriorityIndex  OBJECT-TYPE
    SYNTAX  INTEGER  (0..7)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Frame priority Number"
    ::= { qosCurCfgPriorityCoSEntry 1 }

qosCurCfgPriorityCoSq  OBJECT-TYPE
    SYNTAX  INTEGER  (0..7)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "CoSq for a Frame Priority Should be between 0 and 7"
    ::= { qosCurCfgPriorityCoSEntry 2 }

qosNewCfgPriorityCoSTable OBJECT-TYPE
    SYNTAX SEQUENCE OF QoSNewCfgPriorityCoSEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of Frame Priority and COSq configuration."
    ::= { qos8021p  4 }

qosNewCfgPriorityCoSEntry OBJECT-TYPE
    SYNTAX QoSNewCfgPriorityCoSEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a particular Frame Priority and COSq configuration."
    INDEX { qosNewCfgPriorityIndex }
    ::= { qosNewCfgPriorityCoSTable 1 }

QoSNewCfgPriorityCoSEntry ::= SEQUENCE {
    qosNewCfgPriorityIndex INTEGER,
    qosNewCfgPriorityCoSq  INTEGER
    }

qosNewCfgPriorityIndex  OBJECT-TYPE
    SYNTAX  INTEGER  (0..7)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Frame priority Number"
    ::= { qosNewCfgPriorityCoSEntry 1 }

qosNewCfgPriorityCoSq  OBJECT-TYPE
    SYNTAX  INTEGER  (0..7)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "CoSq for a Frame Priority Should be between 0 and 7"
    ::= { qosNewCfgPriorityCoSEntry 2 }

qosCurCfgCosWeightTable OBJECT-TYPE
    SYNTAX SEQUENCE OF QoSCurCfgCosWeightEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of CoSq and Weight configuration."
    ::= { qos8021p  5 }

qosCurCfgCosWeightEntry OBJECT-TYPE
    SYNTAX QoSCurCfgCosWeightEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a particular CoSq and Weight configuration."
    INDEX { qosCurCfgCosIndex }
    ::= { qosCurCfgCosWeightTable 1 }

QoSCurCfgCosWeightEntry ::= SEQUENCE {
    qosCurCfgCosIndex    INTEGER,
    qosCurCfgCosWeight   INTEGER
    }

qosCurCfgCosIndex  OBJECT-TYPE
    SYNTAX  INTEGER  (0..7)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "CoSq Number"
    ::= { qosCurCfgCosWeightEntry 1 }

qosCurCfgCosWeight  OBJECT-TYPE
    SYNTAX  INTEGER  (0..15)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Weight of CoSq"
    ::= { qosCurCfgCosWeightEntry 2 }

qosNewCfgCosWeightTable OBJECT-TYPE
    SYNTAX SEQUENCE OF QoSNewCfgCosWeightEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of CoSq and Weight configuration."
    ::= { qos8021p  6 }

qosNewCfgCosWeightEntry OBJECT-TYPE
    SYNTAX QoSNewCfgCosWeightEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a particular CoSq and Weight configuration."
    INDEX { qosNewCfgCosIndex }
    ::= { qosNewCfgCosWeightTable 1 }

QoSNewCfgCosWeightEntry ::= SEQUENCE {
    qosNewCfgCosIndex    INTEGER,
    qosNewCfgCosWeight   INTEGER
    }

qosNewCfgCosIndex  OBJECT-TYPE
    SYNTAX INTEGER  (0..7)
    MAX-ACCESS read-only
    STATUS  current
    DESCRIPTION
        "CoSq Number"
    ::= { qosNewCfgCosWeightEntry 1 }

qosNewCfgCosWeight  OBJECT-TYPE
    SYNTAX INTEGER  (0..15)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Weight of CoSq"
    ::= { qosNewCfgCosWeightEntry 2 }

qosCurCfgCosNum OBJECT-TYPE
    SYNTAX  INTEGER { 
	num2(2),
	num8(8)
	}
    MAX-ACCESS  read-only
    STATUS  current  
    DESCRIPTION
        "Number of CoSq." 
    ::= { qos8021p 7 }

qosNewCfgCosNum OBJECT-TYPE
    SYNTAX  INTEGER { 
	num2(2),
	num8(8)
	}
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Number of CoSq."
    ::= { qos8021p 8 }

qosDefaultCfg OBJECT-TYPE
    SYNTAX  INTEGER {
        none(0),
        defaultCosNum(1),
        defaultWeight(2),
        defaultPriority(3)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Load default configuration."
    ::= { qos8021p 9 }

-- ----------------------------------------------------------------------------
-- } INSERT:  bt2qos
-- ----------------------------------------------------------------------------
-- ----------------------------------------------------------------------------
-- } INSERT:  hpRoot
-- ----------------------------------------------------------------------------

END


