EXTREME-WIRELESS-MIB DEFINITIONS ::= BEGIN

        IMPORTS 
                ifIndex                 FROM IF-MIB
                InterfaceIndex          FROM IF-MIB
        MODULE-IDENTITY         FROM SNMPv2-SMI
                OBJECT-TYPE             FROM SNMPv2-SMI
                NOTIFICATION-TYPE       FROM SNMPv2-SMI
                RowStatus               FROM SNMPv2-TC
        Unsigned32              FROM SNMPv2-SMI
                IpAddress               FROM SNMPv2-SMI
                TimeTicks               FROM SNMPv2-SMI
                Counter32               FROM SNMPv2-SMI
        Counter64               FROM SNMPv2-SMI
        Integer32               FROM SNMPv2-SMI
        TruthValue      FROM SNMPv2-TC
                MacAddress              FROM SNMPv2-TC
                DisplayString   FROM RFC1213-MIB
        extremeAgent    FROM EXTREME-BASE-MIB
        ExtremeDeviceId     FROM EXTREME-BASE-MIB
                extremeV2Traps          FROM EXTREME-BASE-MIB
        ClientAuthType          FROM EXTREME-BASE-MIB
                WPACipherSet            FROM EXTREME-BASE-MIB
                WPAKeyMgmtSet           FROM EXTREME-BASE-MIB
        WirelessRemoteConnectBindingType FROM EXTREME-BASE-MIB
                InetAddressType         FROM INET-ADDRESS-MIB
                InetAddress             FROM INET-ADDRESS-MIB
                extremeAP               FROM EXTREME-BASE-MIB
                extremeLAC              FROM EXTREME-BASE-MIB
                TEXTUAL-CONVENTION      FROM SNMPv2-TC;

        extremeWireless MODULE-IDENTITY
                LAST-UPDATED "0211230000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme Wireless Access Tables"
        ::= { extremeAgent 25 }

        extremeAPTraps          OBJECT IDENTIFIER ::= { extremeV2Traps 5 }
        extremeAPTrapsPrefix    OBJECT IDENTIFIER ::= { extremeAPTraps 0 }
        extremeLACGeneral       OBJECT IDENTIFIER ::= { extremeLAC 1 }
        extremeProfile          OBJECT IDENTIFIER ::= { extremeLAC 2 }


-- *************************************************************** --
-- *************************************************************** --
Dot11Type ::= TEXTUAL-CONVENTION
          STATUS        current
          DESCRIPTION
                "The current standard supports A, B, G interfaces."
          SYNTAX INTEGER { a(1), b(2), g(3), bg(4) }

Dot11Speed ::= TEXTUAL-CONVENTION
          STATUS        current
          DESCRIPTION   "Specifies the speed in Mbps to use for the interface. A value of 0 indicates auto."
        SYNTAX BITS {   speed1(0),
                        speed2(1),
                        speed5(2),
                        speed11(3),
                        speed6(4),
                        speed9(5),
                        speed12(6),
                        speed18(7),
                        speed24(8),
                        speed36(9),
                        speed48(10),
                        speed54(11)}

-- Added for DFS support. To be used for listing channels on 
-- which Radar interference was detected.
Dot11AChannel ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION "Specifies the channel number for 802.11A interface."
    SYNTAX BITS { 
            channel36(0),
            channel40(1),
            channel44(2),
            channel52(3),
            channel56(4),
            channel60(5),
            channel64(6),
            channel100(7),
            channel104(8),
            channel108(9),
            channel112(10),
            channel116(11),
            channel120(12),
            channel124(13),
            channel128(14),
            channel132(15),
            channel140(16)
            }

Dot11AuthMode ::= TEXTUAL-CONVENTION
        STATUS     current
        DESCRIPTION "Specifies the allowed authentication type."
        SYNTAX          INTEGER { open(0), shared(1)}

NetworkAuthMode ::= TEXTUAL-CONVENTION
        STATUS     current
        DESCRIPTION "Specifies the allowed authentication type."
        SYNTAX          INTEGER { none(0), webNetlogin(1), macRadius(2), wpaPlusLegacy(3), wpaOnly(4), wpa2PlusWPA(5), wpa2Only(6)}

ExtremeWirelessCountryCode ::= TEXTUAL-CONVENTION
    STATUS     current
    DESCRIPTION "Specifies the country code the AP operates in."
    SYNTAX INTEGER { 
                        unitedStates(840),
                        japan(392),
                        taiwan(158),
                        newZealand(554),
                        albania              ( 8),       
                        algeria              ( 12),      
                        argentina            ( 32),      
                        armenia              ( 51),      
                        australia            ( 36),      
                        austria              ( 40),      
                        azerbaijan           ( 31),      
                        bahrain              ( 48),      
                        belarus              ( 112),     
                        belgium              ( 56),      
                        belize               ( 84),      
                        bolivia              ( 68),      
                        brazil               ( 76),      
                        bruneiDarussalam    ( 96),      
                        bulgaria             ( 100),     
                        canada               ( 124),     
                        chile                ( 152),     
                        china                ( 156),     
                        colombia             ( 170),     
                        costaRica           ( 188),     
                        croatia              ( 191),     
                        cyprus               ( 196),
                        czech                ( 203),     
                        denmark              ( 208),     
                        dominicanRepublic   ( 214),     
                        ecuador              ( 218),     
                        egypt                ( 818),     
                        elSalvador          ( 222),     
                        estonia              ( 233),     
                        faeroeIslands       ( 234),     
                        finland              ( 246),     
                        france               ( 250),     
                        georgia              ( 268),     
                        germany              ( 276),     
                        greece               ( 300),     
                        guatemala            ( 320),     
                        honduras             ( 340),     
                        hongKong            ( 344),     
                        hungary              ( 348),     
                        iceland              ( 352),     
                        india                ( 356),     
                        indonesia            ( 360),     
                        iran                 ( 364),     
                        iraq                 ( 368),     
                        ireland              ( 372),     
                        israel               ( 376),     
                        italy                ( 380),     
                        jamaica              ( 388),     
                        japan1               ( 393),     
                        japan2               ( 394),     
                        japan3               ( 395),     
                        jordan               ( 400),     
                        kazakhstan           ( 398),     
                        kenya                ( 404),     
                        koreaNorth          ( 408),     
                        koreaRoc            ( 410),     
                        koreaRoc2           ( 411),     
                        kuwait               ( 414),     
                        latvia               ( 428),     
                        lebanon              ( 422),     
                        libya                ( 434),     
                        liechtenstein        ( 438),     
                        lithuania            ( 440),     
                        luxembourg           ( 442),     
                        macau                ( 446),     
                        macedonia            ( 807),     
                        malaysia             ( 458),     
                        mexico               ( 484),     
                        monaco               ( 492),     
                        morocco              ( 504),     
                        netherlands          ( 528),     
                        nicaragua            ( 558),     
                        norway               ( 578),     
                        oman                 ( 512),     
                        pakistan             ( 586),     
                        panama               ( 591),     
                        paraguay             ( 600),     
                        peru                 ( 604),     
                        philippines          ( 608),     
                        poland               ( 616),     
                        portugal             ( 620),     
                        puertoRico          ( 630),     
                        qatar                ( 634),     
                        romania              ( 642),     
                        russia               ( 643),     
                        saudiArabia         ( 682),     
                        singapore            ( 702),     
                        slovakia             ( 703),     
                        slovenia             ( 705),     
                        southAfrica         ( 710),     
                        spain                ( 724),     
                        sweden               ( 752),     
                        switzerland          ( 756),     
                        syria                ( 760),     
                        thailand             ( 764),     
                        trinidadTYobago    ( 780),     
                        tunisia              ( 788),     
                        turkey               ( 792),     
                        uae                  ( 784),     
                        ukraine              ( 804),     
                        unitedKingdom       ( 826),     
                        uruguay              ( 858),     
                        uzbekistan           ( 860),     
                        venezuela            ( 862),     
                        vietNam             ( 704),     
                        yemen                ( 887),     
                        zimbabwe             ( 716),     
                        restOfTheWorld       ( 0),
                        extremeDefault       ( 998),
                        unknown              ( 999)
                        }

ExtremeWirelessAntennaType ::= TEXTUAL-CONVENTION
    STATUS     current
    DESCRIPTION "Specifies Antenna type attached to the access-point. 
    The integrated antenna is specified by CTL table on PCI eeprom.
    The detachable model 15901 is an omni-directional antenna.
    The detachable model 15902 is a  directional antenna."
    SYNTAX    INTEGER { integrated(0), detachable15901(1), detachable15902(2) }


ExtremeWirelessAntennaLocation ::= TEXTUAL-CONVENTION
    STATUS     current
    DESCRIPTION "Specifies whether the antenna is an indoor or outdoor antenna"
    SYNTAX       INTEGER { indoor(0), outdoor(1) }

ExtremeWirelessPhysInterfaceIndex ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION  "The value of a physical interface number. Each radio on an AP
                        corresponds to a physical interface. There can be multiple
                        virtual interface on each physical interface. The format
                        for the physical interface is xxxxyy where xxxx is the
                        port IF index to which the AP is connected. YY is the 
                        interface index within that AP."
    SYNTAX      Integer32(1..2147483647)

ExtremeWirelessVirtInterfaceIndex ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION  "The value of a virtual interface number. Each radio on an AP
                        corresponds to a physical interface. There can be multiple
                        virtual interface on each physical interface. The format
                        for the virtual interface is xxxxyyzz where xxxx is the
                        port IF index to which the AP is connected. YY is the 
                        physical interface index within that AP and ZZ is the index
                        of the virtual interface within that physical interface."
    SYNTAX      Integer32(1..2147483647)

ExtremeWirelessChannelAutoSelectStatus ::= TEXTUAL-CONVENTION
    STATUS        current
    DESCRIPTION   "Specifies the status of the channel auto-selection process."
    SYNTAX BITS {       notApplicable(0),
                        inProgress(1),
                        success(2),
                        radarInterferenceDuringScan(3),
                        radarInterferenceDuringOperation(4),
                        restartedDueToInterference(5)}


-- *************************************************************** --
--                      Device wide Properties                     --
-- *************************************************************** --   
extremeAPTotalAuthFailures OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "This variable gives the total number of
                 Authentication failures that have been seen by all
                 the wireless ports."
        ::= { extremeLACGeneral 1 }

extremeAPTotalDetectedStations OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "This variable gives the total number of detected
                 stations on all the wireless ports."
        ::= { extremeLACGeneral 2 }

extremeAPTotalAssociatedStations OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "This variable gives the total number of associated
                 stations on all the wireless ports."
        ::= { extremeLACGeneral 3 }

extremeAPTotalAuthenticatedStations OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
           "This variable gives the total number of authenticated
       stations on all the wireless ports."
        ::= { extremeLACGeneral 4 }

extremeWirelessCfgMgmtVLAN OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This value indicates the VLAN tag that should be
                 applied to all control traffic between the AP and
                 the platform."
        ::= { extremeLACGeneral 5 }

extremeWirelessCfgNetmask OBJECT-TYPE
        SYNTAX          IpAddress
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This value is the subnet of the Mgmt Vlan"
        ::= { extremeLACGeneral 6 }

extremeWirelessCfgGateway OBJECT-TYPE
        SYNTAX          IpAddress
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This value is assigned to the APs as the gateway
                for the management vlan."
        ::= { extremeLACGeneral 7 }

extremeWirelessCfgEnableWirelessTraps OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "If set to TRUE the wireless port will send traps for
                 Authentication and association events.  
                 If set to FALSE no traps will be generated.
                 Note: We always generate the wireless port status
                 traps."
        ::= { extremeLACGeneral 8 }

extremeWirelessCfgCountryCode OBJECT-TYPE
        SYNTAX           ExtremeWirelessCountryCode
        MAX-ACCESS       read-write
        STATUS           current
        DESCRIPTION
                "This variable allows configuration of the 
                 country code in which the AP will operate.

                 Setting this value will enable the AP to range
                 check frequency and other regulatory settings."
        ::= { extremeLACGeneral 10 }


-- *************************************************************** --
--             Wireless Port Configuration Table                   --
--                                                                 --
-- The configuration table contains one entry for each port on the --
-- device which can host wireless function.  Configuration of the  --
-- port is done without regard to the presence or absence of an AP --
-- on that port.                                                   --
--                                                                 --
-- *************************************************************** --
extremeWirelessPortCfgTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF ExtremeWirelessPortCfgEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This table contains one entry per wireless port that
                 the user has configured.  The AP does not have to be
                 plugged in for the user to configure it via this 
                 table."
        ::= { extremeLAC 3 }

extremeWirelessPortCfgEntry OBJECT-TYPE
        SYNTAX          ExtremeWirelessPortCfgEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                ""
        INDEX { extremeWirelessPortIfIndex }
        ::= { extremeWirelessPortCfgTable 1 }

ExtremeWirelessPortCfgEntry ::= SEQUENCE {
        extremeWirelessPortIfIndex                      InterfaceIndex,
        extremeWirelessPortCfgIpAddress             IpAddress,
        extremeWirelessPortCfgLocation              DisplayString,
        extremeWirelessPortCfgDetectedTimeout   TimeTicks,
        extremeWirelessPortCfgClientWatchdog    TruthValue,
        extremeWirelessPortLastChange               TimeTicks,
        extremeWirelessPortState                        INTEGER,
    extremeWirelessPortAntennaType          ExtremeWirelessAntennaType,
    extremeWirelessPortAntennaLocation      ExtremeWirelessAntennaLocation
}


extremeWirelessPortIfIndex OBJECT-TYPE
        SYNTAX          InterfaceIndex
        MAX-ACCESS      read-only 
        STATUS          current
        DESCRIPTION
                "This is the MIB-II ifIndex of the port this entry
                 describes."
        ::= { extremeWirelessPortCfgEntry 1 }

extremeWirelessPortCfgIpAddress OBJECT-TYPE
        SYNTAX          IpAddress
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This value is assigned to the port for external
                 management."
        ::= { extremeWirelessPortCfgEntry 2 }

extremeWirelessPortCfgLocation OBJECT-TYPE
        SYNTAX          DisplayString
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This describes the physical location of the wireless 
                 port."
        ::= { extremeWirelessPortCfgEntry 3 }

extremeWirelessPortCfgDetectedTimeout OBJECT-TYPE
        SYNTAX          TimeTicks
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This is the number of seconds a station can stay
                 in the detected station table without authenticating."
        ::= { extremeWirelessPortCfgEntry 4 }

extremeWirelessPortCfgClientWatchdog OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "Setting this value to true will force the AP to 
                 run a watch-dog process for system health."
        ::= { extremeWirelessPortCfgEntry 5 }

extremeWirelessPortLastChange OBJECT-TYPE
        SYNTAX          TimeTicks
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "The value of sysUpTime when the port entered its last state"
        ::= { extremeWirelessPortCfgEntry 6 }

extremeWirelessPortState OBJECT-TYPE
        SYNTAX          INTEGER {
                                disabled(1),
                                enabled(2),
                                reset(3),
                                addressing(4),
                                register(5),
                                syncing(6),
                                online(7),
                                error(8)
                        }
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "The current state of the wireless part of this port.

                 enabled  : Port is actively looking for wireless
                            interfaces.

                 disabled : Port is administratively unable to detect
                            new interfaces.

                 reset    : Interfaces have been detected and are 
                            being brought up (access point is booting).

                 addressing : IP Address is being assigned.

                 register : Interfaces are registering for service

                 syncing  : Interfaces are retrieving their 
                            configuration and updating their state.

                 online   : Interfaces are operational.

                 If an error occurs the wireless port will 
                 transistion to the error state."
        ::= { extremeWirelessPortCfgEntry 7 }

-- TODO: What is the meaning of this variable?
extremeWirelessPortAntennaType OBJECT-TYPE
        SYNTAX          ExtremeWirelessAntennaType      
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This is the type of the Antenna for Detachable product.
                 For Altitude-2d series, further selection is available
                 through this variable."
        ::= { extremeWirelessPortCfgEntry 8 }

extremeWirelessPortAntennaLocation OBJECT-TYPE
        SYNTAX          ExtremeWirelessAntennaLocation
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This specifies the location the detachable antenna."
        ::= { extremeWirelessPortCfgEntry 9 }

-- *************************************************************** --
--                    Wireless Port Status Table                   --
--                                                                 --
-- Status table has one entry for every attached AP.  Each entry   --
-- contains a duplicate of the values which are configured in the  --
-- configuration table, as well as status and other information    --
-- learned from the device.                                        --
-- *************************************************************** --
extremeWirelessPortStatusTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF ExtremeWirelessPortStatusEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This table contains one entry per detected AP."
        ::= { extremeAP 1 }

extremeWirelessPortStatusEntry OBJECT-TYPE
        SYNTAX          ExtremeWirelessPortStatusEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                ""
        INDEX { extremeWirelessPortIfIndex }
        ::= { extremeWirelessPortStatusTable 1 }

ExtremeWirelessPortStatusEntry ::= SEQUENCE {
        extremeWirelessPortIpAddress                 IpAddress,
        extremeWirelessPortNetmask                       IpAddress,
        extremeWirelessPortGateway                       IpAddress,
        extremeWirelessPortManagementIP              IpAddress,
        extremeWirelessPortEnableWirelessTraps   TruthValue,
        extremeWirelessPortLocation                      DisplayString,
        extremeWirelessPortDetectedMaxAge            TimeTicks,
        extremeWirelessPortMgmtVLAN                      INTEGER,
        extremeWirelessPortBootromVersion            DisplayString,
        extremeWirelessPortSWVersion                 DisplayString,
        extremeWirelessPortSysDescr                      DisplayString,
        extremeWirelessPortManufacturerName          DisplayString,
        extremeWirelessPortProductName               DisplayString,
        extremeWirelessPortSerialNumber              DisplayString,
        extremeWirelessPortEdpNeighborId             ExtremeDeviceId,
        extremeWirelessPortClearCounters             TruthValue,
        extremeWirelessPortClearLog                      TruthValue,
        extremeWirelessPortWatchdogReset             TruthValue,
        extremeWirelessPortNumPhysInterfaces     INTEGER,
        extremeWirelessPortHWVersion             DisplayString,
        extremeWirelessPortMacAddress            MacAddress,
        extremeWirelessPortRadiusPortID              DisplayString,
    extremeWirelessPortBootUpTime            TimeTicks,
    extremeWirelessPortCountryCode                   ExtremeWirelessCountryCode,
        extremeWirelessPortWallclockTime         INTEGER,
        extremeWirelessPortPartNumber                DisplayString,
        extremeWirelessPortPartRevision          DisplayString,
        extremeWirelessPortUpTime                TimeTicks,
    extremeWirelessPortStatusAntennaType     ExtremeWirelessAntennaType,
    extremeWirelessPortStatusAntennaLocation ExtremeWirelessAntennaLocation,
    extremeWirelessPortStatusAntenna2point4GHZGain INTEGER,
    extremeWirelessPortStatusAntenna5GHZGain INTEGER,
    extremeWirelessPortPrimaryBootloaderVersion     DisplayString,
    extremeWirelessPortSecondaryBootloaderVersion   DisplayString,
    extremeWirelessPortCurrentBootloaderInUse       INTEGER
}


extremeWirelessPortIpAddress OBJECT-TYPE
        SYNTAX          IpAddress
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This value is assigned to the port for external
                 management."
        ::= { extremeWirelessPortStatusEntry 1 }

extremeWirelessPortNetmask OBJECT-TYPE
        SYNTAX          IpAddress
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This value is assigned to the AP for external
                 management."
        ::= { extremeWirelessPortStatusEntry 2 }

extremeWirelessPortGateway OBJECT-TYPE
        SYNTAX          IpAddress
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This value is assigned to the AP for external
                 management."
        ::= { extremeWirelessPortStatusEntry 3 }

extremeWirelessPortManagementIP OBJECT-TYPE
        SYNTAX          IpAddress
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This value is used by the AP when sending out Management 
                packets to the external world. This IP is used as src-ip 
                address in Syslog messages, as NAS-Identifier in Radius requests, 
                and as Agent-Addr in SNMP trap pdu's."
        ::= { extremeWirelessPortStatusEntry 4 }

extremeWirelessPortEnableWirelessTraps OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "If set to TRUE the wireless port will send traps for
                 Authentication and association successful events.  
                 If set to FALSE no traps will be generated.

                 Note: We always generate the wireless port status
                 traps."
        ::= { extremeWirelessPortStatusEntry 5 }

extremeWirelessPortLocation OBJECT-TYPE
        SYNTAX          DisplayString
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This describes the physical location of the wireless 
                 port."
        ::= { extremeWirelessPortStatusEntry 6 }

extremeWirelessPortDetectedMaxAge OBJECT-TYPE
        SYNTAX          TimeTicks
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This is the number of seconds a station can stay
                 in the detected station table without authenticating."
        ::= { extremeWirelessPortStatusEntry 7 }

extremeWirelessPortMgmtVLAN OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "This value indicates the VLAN tag that should be
                 applied to all control traffic between the AP and
                 the platform."
        ::= { extremeWirelessPortStatusEntry 8 }

extremeWirelessPortBootromVersion OBJECT-TYPE
        SYNTAX          DisplayString
        MAX-ACCESS              read-only
        STATUS          current
        DESCRIPTION
                "This is the current version of the bootrom on this AP."
        ::= { extremeWirelessPortStatusEntry 9 }

extremeWirelessPortSWVersion OBJECT-TYPE
        SYNTAX          DisplayString
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "This is the current software version of this AP."
        ::= { extremeWirelessPortStatusEntry 10 }

extremeWirelessPortSysDescr OBJECT-TYPE
        SYNTAX          DisplayString
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "This is the equivalent value of sysDescr from the AP."
        ::= { extremeWirelessPortStatusEntry 11 }

extremeWirelessPortManufacturerName OBJECT-TYPE
        SYNTAX          DisplayString
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                " "
        REFERENCE "dot11ManufacturerName"
        ::= { extremeWirelessPortStatusEntry 12 }

extremeWirelessPortProductName OBJECT-TYPE
        SYNTAX          DisplayString
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                " "
        REFERENCE "dot11ProductName"
        ::= { extremeWirelessPortStatusEntry 13 }

extremeWirelessPortSerialNumber OBJECT-TYPE
        SYNTAX          DisplayString
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "This is the unique serial number for this device."
        ::= { extremeWirelessPortStatusEntry 14 }

extremeWirelessPortEdpNeighborId  OBJECT-TYPE
        SYNTAX          ExtremeDeviceId
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "EDP assigns a unique ID to each neighbor to 
                 disambiguate references.  This can be used to index 
                 into the extremeEdpTable."
        ::= { extremeWirelessPortStatusEntry 15 }

extremeWirelessPortClearCounters OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This value can be set to true to force the device
                 to reset it's counters.  A read will return false."
        ::= { extremeWirelessPortStatusEntry 16 }

extremeWirelessPortClearLog OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This value can be set to true to force the device
                 to clear its local log store.  A read will return
                 false."
        ::= { extremeWirelessPortStatusEntry 17 }

extremeWirelessPortWatchdogReset OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This is to enable/disable watchdog timer reset on timeout. 
                Default is enable. If it is enabled, system should reset
                when the watchdog kicks in. On next bootup, it should 
                send out an syslog message to syslog server.  If it is 
                disabled, it should record the error and not reset the system."
        ::= { extremeWirelessPortStatusEntry 18 }

extremeWirelessPortNumPhysInterfaces OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-only
        STATUS          current         
        DESCRIPTION
                "Each wireless port has a set of physical interface which are
                 numbered 1-N.  This variable gives the number of 
                 physical interfaces on this AP."
        ::= { extremeWirelessPortStatusEntry 19 }

extremeWirelessPortHWVersion OBJECT-TYPE
        SYNTAX          DisplayString
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "This is the current hardware version of this AP."
        ::= { extremeWirelessPortStatusEntry 20 }


extremeWirelessPortMacAddress OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Unique MAC Address assigned to the ethernet interface on the AP."
        ::= { extremeWirelessPortStatusEntry 21 }

extremeWirelessPortRadiusPortID OBJECT-TYPE
        SYNTAX  DisplayString
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "A string value that should be sent by the AP to the radius
                server as the Port-ID radius attribute in authentication requests"
        ::= { extremeWirelessPortStatusEntry 22 }

extremeWirelessPortBootUpTime OBJECT-TYPE
                SYNTAX  TimeTicks
                MAX-ACCESS      read-write
                STATUS  current
                DESCRIPTION     
                "The sysUpTime of the LAC when the port was booted up.
                Should be set only during the AP boot up."
        ::= { extremeWirelessPortStatusEntry 23 }

extremeWirelessPortCountryCode OBJECT-TYPE
                SYNTAX ExtremeWirelessCountryCode
                MAX-ACCESS      read-write
                STATUS  current
                DESCRIPTION     
                "The country code that the AP is programmed to operate in."
        ::= { extremeWirelessPortStatusEntry 24 }

extremeWirelessPortWallclockTime OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS      read-write
                STATUS  current
                DESCRIPTION     
                "The wall clock time as known to the LAC. 
                        Expressed in number of seconds since Jan 1, 1970"
        ::= { extremeWirelessPortStatusEntry 25 }

extremeWirelessPortPartNumber OBJECT-TYPE
        SYNTAX          DisplayString
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This describes the part number of the AP."
        ::= { extremeWirelessPortStatusEntry 26 }

extremeWirelessPortPartRevision OBJECT-TYPE
        SYNTAX          DisplayString
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This describes the revision of the AP."
        ::= { extremeWirelessPortStatusEntry 27 }

extremeWirelessPortUpTime OBJECT-TYPE
                SYNTAX  TimeTicks
                MAX-ACCESS      read-write
                STATUS  current
                DESCRIPTION     
                "The number of seconds the port has been in the online state."
        ::= { extremeWirelessPortStatusEntry 28 }

extremeWirelessPortStatusAntennaType OBJECT-TYPE
        SYNTAX          ExtremeWirelessAntennaType
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This is the type of the Antenna for Detachable product.
                 For Altitude-2d series, further selection is available
                 through this variable."
        ::= { extremeWirelessPortStatusEntry 29 }

extremeWirelessPortStatusAntennaLocation OBJECT-TYPE
        SYNTAX          ExtremeWirelessAntennaLocation
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This specifies the location the detachable antenna."
        ::= { extremeWirelessPortStatusEntry 30 }

extremeWirelessPortStatusAntenna2point4GHZGain OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
               "This specifies 2.4GHz gain value for detachable antenna in dbi"
        ::= { extremeWirelessPortStatusEntry 31 }

extremeWirelessPortStatusAntenna5GHZGain OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
               "This specifies 5GHz gain value for detachable antenna in dbi"
        ::= { extremeWirelessPortStatusEntry 32 }

extremeWirelessPortPrimaryBootloaderVersion OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
        "This is the version of the primary bootloader on this AP."
        ::= { extremeWirelessPortStatusEntry 33 }

extremeWirelessPortSecondaryBootloaderVersion OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
        "This is the version of the Secondary bootloader on this AP."
        ::= { extremeWirelessPortStatusEntry 34 }

extremeWirelessPortCurrentBootloaderInUse OBJECT-TYPE
        SYNTAX INTEGER { primary(1),
                                 secondary(2) }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
        "This specifies if the bootloader booted is primary or secondary one."
        ::= { extremeWirelessPortStatusEntry 35 }
-- *************************************************************** --
--                 Wireless Port Syslog Status Table               --
-- *************************************************************** --
extremeWirelessPortLogStatusTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF ExtremeWirelessPortLogStatusEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This table contains one entry for each wireless port
                 which is configured via the configuration table."
        ::= { extremeAP 2 }

extremeWirelessPortLogStatusEntry OBJECT-TYPE
        SYNTAX          ExtremeWirelessPortLogStatusEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                ""
        INDEX { extremeWirelessPortIfIndex, 
                extremeWirelessPortLogStatusIndex }
        ::= { extremeWirelessPortLogStatusTable 1 }

ExtremeWirelessPortLogStatusEntry ::= SEQUENCE {
        extremeWirelessPortLogStatusIndex       INTEGER,
        extremeWirelessPortLogStatusDestIp      InetAddress,
        extremeWirelessPortLogStatusDestIpType  InetAddressType,
        extremeWirelessPortLogStatusPort        INTEGER,
        extremeWirelessPortLogStatusFacility    INTEGER,
        extremeWirelessPortLogStatusSeverity    INTEGER,
        extremeWirelessPortLogStatusStatus      TruthValue }

extremeWirelessPortLogStatusIndex OBJECT-TYPE
        SYNTAX          INTEGER(1..9)
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "There are 9 entries in this table to correspond to
                 the 8 entries configured in the cfg table plus one
                 for the LAC."
        ::= { extremeWirelessPortLogStatusEntry 1 }

extremeWirelessPortLogStatusDestIp OBJECT-TYPE
        SYNTAX          InetAddress
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This is the IP address to which syslog messsages
                 will be sent.  A value of 0.0.0.0 indicates that
                 this entry is disabled. The source IP for every syslog
                message comes from the ManagementIP field in 
                extremeWirelessPortStatusTable"
        ::= { extremeWirelessPortLogStatusEntry 2 }

extremeWirelessPortLogStatusDestIpType          OBJECT-TYPE
        SYNTAX                                  InetAddressType
        MAX-ACCESS                              read-write
        STATUS                                  current
        DESCRIPTION
            "The type of address specified in the object
                'extremeWirelessPortLogStatusDestIp.
             Currently, only 'ipv4' and 'dns' are supported."
        DEFVAL { ipv4 }
      ::= { extremeWirelessPortLogStatusEntry 3 }

extremeWirelessPortLogStatusPort OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This is the port to which syslog messages will be
                 sent."
        ::= { extremeWirelessPortLogStatusEntry 4 }

extremeWirelessPortLogStatusFacility OBJECT-TYPE
        SYNTAX          INTEGER(0..7)
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "Optional value for syslog facility local0-7."
        ::= { extremeWirelessPortLogStatusEntry 5 }

extremeWirelessPortLogStatusSeverity               OBJECT-TYPE
            SYNTAX  INTEGER { 
                                critical (0),
                                error (1),
                                warning (2),
                                notice (3),
                                info (4),
                                debugSummary (5),
                                debugVerbose (6),
                                debugData (7)                                   
                                }
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                    "The syslog message severity. All syslog
                        messages that have a severity >= specified severity, 
                        will be sent to this syslog server."
            DEFVAL { debugData }
            ::= { extremeWirelessPortLogStatusEntry 6 }

extremeWirelessPortLogStatusStatus OBJECT-TYPE
                SYNTAX TruthValue
                MAX-ACCESS  read-write
                STATUS current
                DESCRIPTION
                        "Specifies whether the log server is enabled or not."
        ::= { extremeWirelessPortLogStatusEntry 7 }


-- *************************************************************** --
--                   Wireless Port Log Table                       --
-- *************************************************************** --
extremeWirelessPortLogTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF ExtremeWirelessPortLogEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This table allows access to the syslog entries on
                 particular wireless ports."
        ::= { extremeAP 3 }

extremeWirelessPortLogEntry OBJECT-TYPE
        SYNTAX          ExtremeWirelessPortLogEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                ""
        INDEX { extremeWirelessPortIfIndex, 
                extremeWirelessPortLogIndex }
        ::= { extremeWirelessPortLogTable 1 }

ExtremeWirelessPortLogEntry ::= SEQUENCE {
        extremeWirelessPortLogIndex     INTEGER,
        extremeWirelessPortLogMessage   DisplayString }

extremeWirelessPortLogIndex OBJECT-TYPE
        SYNTAX          INTEGER(0..65535)
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This is an arbitrary integer which is assinged to
                 entries in order of their insertion."
        ::= { extremeWirelessPortLogEntry 1 }

extremeWirelessPortLogMessage OBJECT-TYPE
        SYNTAX          DisplayString
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "This is the formatted syslog message which was sent."
        ::= { extremeWirelessPortLogEntry 2 }
        
-- *************************************************************** --
--           Wireless Physical Interface Ctl Table                 --
-- This table allows for the configuration of parameters that deal --
-- with physical interfaces. Each radio on the AP is represented by--
-- a physical interface. Each physical interface can have multiple --
-- (upto 8) virtual interfaces. RF properties are configured on the--
-- physical interface using the extremeWirelessInterfaceRFCtlTable --
-- Security parameters are configured on the virtual interface     --
-- using the extremeWirelessInterfaceSecurityCtlTable          --
-- *************************************************************** --

extremeWirelessPhysInterfaceCtlTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF ExtremeWirelessPhysInterfaceCtlEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This table provides configuration of per-physical interface
                 values."
        ::= { extremeAP 4 }

ExtremeWirelessPhysInterfaceCtlEntry ::= SEQUENCE {
        extremeWirelessPhysInterfaceIndex               ExtremeWirelessPhysInterfaceIndex,
        extremeWirelessPhysInterfacePHYChannel       INTEGER,
        extremeWirelessPhysInterfaceSpeed                       Dot11Speed,
        extremeWirelessPhysInterfaceNumVirtInterfaces INTEGER,
    extremeWirelessPhysInterfaceChannelAutoSelectStatus ExtremeWirelessChannelAutoSelectStatus,
    extremeWirelessPhysInterfaceRadarInterfaceChannelList Dot11AChannel
}


extremeWirelessPhysInterfaceCtlEntry OBJECT-TYPE
        SYNTAX          ExtremeWirelessPhysInterfaceCtlEntry
        MAX-ACCESS      not-accessible
        STATUS          current 
        DESCRIPTION
                "Each entry is indexed by the wirelessInterfaceIndex, and
                represents a wireless interface."
        INDEX { extremeWirelessPhysInterfaceIndex }
        ::= { extremeWirelessPhysInterfaceCtlTable 1 }

extremeWirelessPhysInterfaceIndex OBJECT-TYPE
        SYNTAX  ExtremeWirelessPhysInterfaceIndex
        MAX-ACCESS      accessible-for-notify
        STATUS          current
        DESCRIPTION
                "This is the ifIndex of an individual physical interface on an AP.
                Each radio will have a unique value."
        ::= { extremeWirelessPhysInterfaceCtlEntry 1 }


extremeWirelessPhysInterfacePHYChannel OBJECT-TYPE
        SYNTAX          INTEGER (0..99)
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This is the RF channel which will be used by 
                 this transmitter.  Range should be established
                 by configuration of RegDomain and PHYType."
        ::= { extremeWirelessPhysInterfaceCtlEntry 2 }

extremeWirelessPhysInterfaceSpeed OBJECT-TYPE
        SYNTAX          Dot11Speed 
        MAX-ACCESS       read-write
        STATUS           current
        DESCRIPTION
                "This value indicates the current setting for 
                 Tx speed for the interface. Only one of thebits of this bit set can be set.
                 If all bits are unset (ie a 0 is passed as a value) then 
                 it means that the interface should choose a speed
                 based on some algorithm."
        ::= { extremeWirelessPhysInterfaceCtlEntry 3 }

extremeWirelessPhysInterfaceNumVirtInterfaces OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS       read-write
        STATUS           current
        DESCRIPTION
                "Each physical interface has a number of virtual interfaces
                 This specifies the number of virt interfaces."
        ::= { extremeWirelessPhysInterfaceCtlEntry 4 }

-- Added for DFS
extremeWirelessPhysInterfaceChannelAutoSelectStatus OBJECT-TYPE
    SYNTAX          ExtremeWirelessChannelAutoSelectStatus 
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "This OID reflects the status of the channel auto selection process."
        ::= { extremeWirelessPhysInterfaceCtlEntry 5 }

-- Added for DFS
extremeWirelessPhysInterfaceRadarInterfaceChannelList OBJECT-TYPE
        SYNTAX          Dot11AChannel 
        MAX-ACCESS       read-only
        STATUS           current
        DESCRIPTION
                "This OID reflects the list oc 802.11(a) channels on which
radar interference was detected."
        ::= { extremeWirelessPhysInterfaceCtlEntry 6 }

        
        
-- *************************************************************** --
--           Wireless Virtual  Interface Ctl Table                 --
-- This table allows for the configuration of parameters that deal --
-- with virtual interfaces. Each radio on the AP is represented by--
-- a physical interface. Each physical interface can have multiple --
-- (upto 8) virtual interfaces. RF properties are configured on the--
-- physical interface using the extremeWirelessInterfaceRFCtlTable --
-- Security parameters are configured on the virtual interface     --
-- using the extremeWirelessInterfaceSecurityCtlTable          --
-- *************************************************************** --
extremeWirelessVirtInterfaceCtlTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF ExtremeWirelessVirtInterfaceCtlEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This table provides configuration of per-physical-interface
                 values."
        ::= { extremeAP 6 }

ExtremeWirelessVirtInterfaceCtlEntry ::= SEQUENCE {
        extremeWirelessVirtInterfaceIndex                       ExtremeWirelessVirtInterfaceIndex,
        extremeWirelessVirtInterfaceMacAddress              MacAddress,
        extremeWirelessVirtInterfaceMaxClients              INTEGER,
        extremeWirelessVirtInterfaceWirelessBridging    TruthValue,
        extremeWirelessVirtInterfaceLastStateChange         TimeTicks,
        extremeWirelessVirtInterfaceState                       INTEGER,
    extremeWirelessVirtInterfaceIappEnabled         TruthValue,
    extremeWirelessVirtInterfaceSvpEnabled          TruthValue
}

extremeWirelessVirtInterfaceCtlEntry OBJECT-TYPE
        SYNTAX          ExtremeWirelessVirtInterfaceCtlEntry
        MAX-ACCESS      not-accessible
        STATUS          current 
        DESCRIPTION
                "Each entry is indexed by the wirelessInterfaceIndex, and
                represents a virtual wireless interface."
        INDEX { extremeWirelessVirtInterfaceIndex }
        ::= { extremeWirelessVirtInterfaceCtlTable 1 }

extremeWirelessVirtInterfaceIndex OBJECT-TYPE
        SYNTAX  ExtremeWirelessVirtInterfaceIndex
        MAX-ACCESS      accessible-for-notify
        STATUS          current
        DESCRIPTION
                "This is the ifIndex of an individual interface on an AP.
                Each virtual interface will have a unique value."
        ::= { extremeWirelessVirtInterfaceCtlEntry 1 }
        
extremeWirelessVirtInterfaceMacAddress OBJECT-TYPE
        SYNTAX          MacAddress
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "The maximum number of clients that can associate with this virtual interface."
        ::= { extremeWirelessVirtInterfaceCtlEntry 2 }

extremeWirelessVirtInterfaceMaxClients OBJECT-TYPE
        SYNTAX          INTEGER (1..128)
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "The maximum number of clients that can associate with this virtual interface."
        ::= { extremeWirelessVirtInterfaceCtlEntry 3 }

extremeWirelessVirtInterfaceWirelessBridging OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This specifies whether wireless bridging is enabled on this interface.
                 If wireless bridging is enabled then traffic originating from a client on this
                 interface will be bridged to clients on the same VLAN on this or other 
                 virtual interfaces that have wireless bridging enabled. So basically
                 wireless bridging should be enabled on both the source and the destination
                 virtual interface for traffic to be bridged."
        ::= { extremeWirelessVirtInterfaceCtlEntry 4 }

extremeWirelessVirtInterfaceLastStateChange OBJECT-TYPE
        SYNTAX          TimeTicks
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "The value of sysUpTime when the virtual interface entered its current state"
        ::= { extremeWirelessVirtInterfaceCtlEntry 5 }

extremeWirelessVirtInterfaceState OBJECT-TYPE
        SYNTAX          INTEGER { enabled(1), disabled(2) } 
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This value specifies whether the virtual interface is active or not"
        ::= { extremeWirelessVirtInterfaceCtlEntry 6 }

extremeWirelessVirtInterfaceIappEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
    "IAPP status. A value of TRUE indicates IAPP is enabled on the
    interface."
    ::= { extremeWirelessVirtInterfaceCtlEntry 7 }

extremeWirelessVirtInterfaceSvpEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
    "SVP status. A value of TRUE indicates SVP is enabled on the
    interface."
    ::= { extremeWirelessVirtInterfaceCtlEntry 8 }

-- *************************************************************** --
--              Wireless Interface Security Ctl Table              --
-- This table allows for the configuration of per-wireless-intf    --
-- security parameters. Each Wireless interface is represented in  --
-- ifTable, and is represented by extremeWirelessInterfaceIfIndex. --
-- *************************************************************** --
extremeWirelessVirtInterfaceSecurityCtlTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF ExtremeWirelessVirtInterfaceSecurityCtlEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This table provides configuration of per-interface
                 values."
        ::= { extremeAP 7 }

extremeWirelessVirtInterfaceSecurityCtlEntry OBJECT-TYPE
        SYNTAX          ExtremeWirelessVirtInterfaceSecurityCtlEntry
        MAX-ACCESS      not-accessible
        STATUS          current 
        DESCRIPTION
                "Each entry is indexed by the wirelessInterfaceIndex, and
                represents a wireless interface."
        INDEX { extremeWirelessVirtInterfaceIndex }
        ::= { extremeWirelessVirtInterfaceSecurityCtlTable 1 }

ExtremeWirelessVirtInterfaceSecurityCtlEntry ::= SEQUENCE {
        extremeWirelessVirtInterfaceESSName             OCTET STRING,
        extremeWirelessVirtInterfaceSSIDInBeacon        TruthValue,
        extremeWirelessVirtInterfaceDot11AuthMode       Dot11AuthMode, 
        extremeWirelessVirtInterfaceNetworkAuthMode     NetworkAuthMode, 
        extremeWirelessVirtInterfaceDataVlan    INTEGER,
        extremeWirelessVirtInterfaceIgnoreVSAVlan       TruthValue,
        extremeWirelessVirtInterfaceWEPDefaultKey       INTEGER,
        extremeWirelessVirtInterfaceEncryptionLength            INTEGER
}

extremeWirelessVirtInterfaceESSName OBJECT-TYPE
        SYNTAX          OCTET STRING
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "The ESS ID of this interface."
        ::= { extremeWirelessVirtInterfaceSecurityCtlEntry 1 }

extremeWirelessVirtInterfaceSSIDInBeacon OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "Does this interface generate a beacon with the
                 SSID in it?"
        ::= { extremeWirelessVirtInterfaceSecurityCtlEntry 2 }

extremeWirelessVirtInterfaceDot11AuthMode OBJECT-TYPE
        SYNTAX          Dot11AuthMode
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "Setting this to true indicates whether to use open or shared authentication"
        ::= { extremeWirelessVirtInterfaceSecurityCtlEntry 3 }

extremeWirelessVirtInterfaceNetworkAuthMode OBJECT-TYPE
        SYNTAX          NetworkAuthMode
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This specifies the authentication mode to use on top of dot11 MAC authentication"
        ::= { extremeWirelessVirtInterfaceSecurityCtlEntry 4 }

extremeWirelessVirtInterfaceDataVlan OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This is the VLAN to use for client data in case of the VLAN is not received as a VSA. 
                This VLAN is also used for authentication types like PSK, WEP, etc"
        ::= { extremeWirelessVirtInterfaceSecurityCtlEntry 5 }

extremeWirelessVirtInterfaceIgnoreVSAVlan OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "If this is set then the VLAN returned as a VSA will be ignored and the Data Vlan specified above
                will be used instead"
        ::= { extremeWirelessVirtInterfaceSecurityCtlEntry 6 }

extremeWirelessVirtInterfaceWEPDefaultKey OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This value indicates the index in dot11WEPDefaultKeyTable that 
                identifies the key this interface will use to decrypt packets."
        ::= { extremeWirelessVirtInterfaceSecurityCtlEntry 7 }

extremeWirelessVirtInterfaceEncryptionLength OBJECT-TYPE
        SYNTAX      INTEGER { none(0),
                              sixtyfour(64),
                              onetwentyeight(128)  }
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This is the length of the encryption key to use in case
                 of dot1x legacy mode and WEP. If this length is 0 then no WEP encryption."
        ::= { extremeWirelessVirtInterfaceSecurityCtlEntry 8 }

-- *************************************************************** --
--              Wireless Interface Dot1x Ctl Table              --
-- This table allows for the configuration of per-wireless-intf    --
-- dot1x parameters. Each Wireless interface is represented in  --
-- ifTable, and is represented by extremeWirelessVirtInterfaceIfIndex. --
-- *************************************************************** --
extremeWirelessVirtInterfaceDot1xCtlTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF ExtremeWirelessVirtInterfaceDot1xCtlEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "There is one entry in this table for each virtual interface 
                It reflects the dot1x security config"
        ::= { extremeAP 8 }

extremeWirelessVirtInterfaceDot1xCtlEntry OBJECT-TYPE
        SYNTAX  ExtremeWirelessVirtInterfaceDot1xCtlEntry
        MAX-ACCESS      not-accessible
        STATUS  current
        DESCRIPTION
                ""
        INDEX { extremeWirelessVirtInterfaceIndex }
        ::= { extremeWirelessVirtInterfaceDot1xCtlTable 1 }

ExtremeWirelessVirtInterfaceDot1xCtlEntry ::= SEQUENCE {
        extremeWirelessVirtInterfaceKeyMgmtSuite                WPAKeyMgmtSet,
        extremeWirelessVirtInterfaceMcastCipherSuite    WPACipherSet,
        extremeWirelessVirtInterfaceDot1xPSKValue               OCTET STRING,
        extremeWirelessVirtInterfaceDot1xPSKPassPhrase  DisplayString,
        extremeWirelessVirtInterfaceDot1xReAuthPeriod   INTEGER,
        extremeWirelessVirtInterfaceGroupUpdateTimeOut  Unsigned32,
        extremeWirelessVirtInterfacePairwiseUpdateTimeOut Unsigned32
}

extremeWirelessVirtInterfaceKeyMgmtSuite OBJECT-TYPE
        SYNTAX  WPAKeyMgmtSet
        MAX-ACCESS      read-write
        STATUS  current
        DESCRIPTION
                "This bitmask configures the authentication suites to be used."
        ::= { extremeWirelessVirtInterfaceDot1xCtlEntry 1 }

extremeWirelessVirtInterfaceMcastCipherSuite OBJECT-TYPE
        SYNTAX  WPACipherSet
        MAX-ACCESS      read-write
        STATUS  current
        DESCRIPTION
                "This configures the cipher suite to use for mcast traffic. The cipher suite to use for unicast traffic
                 is derived from this using the following algorithm:
                        Mcast cipher = WEP (64/128), Unicast cipher = TKIP
                        Mcast cipher = TKIP, Unicast cipher = TKIP
                        Mcast cipher = AES, Unicast cipher = AES.
                 This therefore determines the max unicast cipher suite the client can use to associate with 
                 this interface."
        ::= { extremeWirelessVirtInterfaceDot1xCtlEntry 2 }


extremeWirelessVirtInterfaceDot1xPSKValue OBJECT-TYPE
        SYNTAX          OCTET STRING (SIZE(32))
        MAX-ACCESS      read-write
        STATUS          current 
        DESCRIPTION
                "The Pre-Shared Key (PSK) for when WPA in PSK mode is
                 the selected authentication suite."
        REFERENCE "dot11RSNConfigPSKValue"
        ::= { extremeWirelessVirtInterfaceDot1xCtlEntry 3 }

extremeWirelessVirtInterfaceDot1xPSKPassPhrase OBJECT-TYPE
        SYNTAX          DisplayString
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
        "The PSK, for when WPA in PSK mode is the selected authentication
         suite, is configured by extremeWirelessVirtInterfaceKeyMgmtSuite.
         An alternative manner of setting the PSK uses the password-to-key
         algorithm defined in section XXX. This variable provides a means
         to enter a pass phrase. When this object is written, the RSN
         entity shall use the password-to-key algorithm specified in
         section XXX to derive a pre-shared and populate
         extremeWirelessVirtInerfaceDot1xPSKValue with this key.
         This object is logically write-only. Reading this variable shall
         return unsuccessful status or null or zero."
        ::= { extremeWirelessVirtInterfaceDot1xCtlEntry 4 }

extremeWirelessVirtInterfaceDot1xReAuthPeriod OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "Number of seconds a clients authentication will last before
                 the AP automatically issues a reauthentication request."
        ::= { extremeWirelessVirtInterfaceDot1xCtlEntry 5 }

extremeWirelessVirtInterfaceGroupUpdateTimeOut OBJECT-TYPE
        SYNTAX          Unsigned32 (1..1440)
        UNITS           "minutes"
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "The time in minutes after which the RSN group
                 update handshake will be retried. The timer shall
                 start at the moment the group update message is
                 sent."
        REFERENCE "dot11RSNConfigGroupUpdateTimeOut"
        DEFVAL          { 100 } -- 
        ::= { extremeWirelessVirtInterfaceDot1xCtlEntry 6 }

extremeWirelessVirtInterfacePairwiseUpdateTimeOut OBJECT-TYPE
        SYNTAX          Unsigned32 (1..1440)
        UNITS           "minutes"
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "The time in minutes after which the RSN 4-way
                 handshake will be retried. The timer shall start at
                 the moment a 4-way message is sent."
        REFERENCE "dot11RSNConfigPairwiseUpdateTimeOut"
        DEFVAL          { 100 } -- 
        ::= { extremeWirelessVirtInterfaceDot1xCtlEntry 7 }


-- *************************************************************** --
--                     Default WEP Key Table                       --
-- *************************************************************** --
extremeWirelessVirtInterfaceWEPKeyTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF ExtremeWirelessVirtInterfaceWEPKeyEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This table contains per-profile WEP keys.

                 Reference ieee802dot11.1.2.3."
        ::= { extremeAP 9 }

extremeWirelessVirtInterfaceWEPKeyEntry OBJECT-TYPE
        SYNTAX  ExtremeWirelessVirtInterfaceWEPKeyEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                " "
        INDEX { extremeWirelessVirtInterfaceIndex, extremeWirelessVirtInterfaceWEPKeyIndex }
        ::= { extremeWirelessVirtInterfaceWEPKeyTable 1 }
        
ExtremeWirelessVirtInterfaceWEPKeyEntry ::= SEQUENCE {
        extremeWirelessVirtInterfaceWEPKeyIndex INTEGER,
        extremeWirelessVirtInterfaceWEPKey              OCTET STRING,
        extremeWirelessVirtInterfaceWEPKeyStatus        TruthValue }
        
extremeWirelessVirtInterfaceWEPKeyIndex OBJECT-TYPE
        SYNTAX          INTEGER(1..4)
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "There can be upto 4 wep keys for any wireless
                 interface. Four of the keys are to be used with
                 WEP Authentication, and the other four with MAC Auth."
        ::= { extremeWirelessVirtInterfaceWEPKeyEntry 1 }

extremeWirelessVirtInterfaceWEPKey OBJECT-TYPE
        SYNTAX          OCTET STRING (SIZE(1..19))
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "This is a write-only wep key."
        ::= { extremeWirelessVirtInterfaceWEPKeyEntry 2 }

extremeWirelessVirtInterfaceWEPKeyStatus OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "Specifies whether the key is present or not."
        ::= { extremeWirelessVirtInterfaceWEPKeyEntry 3 }

-- *************************************************************** --
--              Wireless Interface RF Ctl Table                    --
-- This table allows for the configuration of per-wireless-intf    --
-- RF parameters. Each Wireless interface is represented in        --
-- ifTable, and is represented by extremeWirelessPhysInterfaceIfIndex. --
-- *************************************************************** --
extremeWirelessPhysInterfaceRFCtlTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF ExtremeWirelessPhysInterfaceRFCtlEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This table provides configuration of per-interface
                 values."
        ::= { extremeAP 10 }

extremeWirelessPhysInterfaceRFCtlEntry OBJECT-TYPE
        SYNTAX          ExtremeWirelessPhysInterfaceRFCtlEntry
        MAX-ACCESS      not-accessible
        STATUS          current 
        DESCRIPTION
                "Each entry is indexed by the wirelessInterfaceIndex, and
                represents a wireless interface."
        INDEX { extremeWirelessPhysInterfaceIndex }
        ::= { extremeWirelessPhysInterfaceRFCtlTable 1 }

ExtremeWirelessPhysInterfaceRFCtlEntry ::= SEQUENCE {
        extremeWirelessPhysInterfaceBeaconPeriod        INTEGER,
        extremeWirelessPhysInterfaceTxPowerLevel        INTEGER,
        extremeWirelessPhysInterfaceDTIMPeriod  INTEGER,
        extremeWirelessPhysInterfaceFragLength  INTEGER,
        extremeWirelessPhysInterfaceLongRetry   INTEGER,        
        extremeWirelessPhysInterfaceShortRetry  INTEGER,
        extremeWirelessPhysInterfaceRTSThreshold        INTEGER,
        extremeWirelessPhysInterfaceSupportedDataRatesRxValue Dot11Speed,
        extremeWirelessPhysInterfaceSupportedDataRatesTxValue Dot11Speed,
        extremeWirelessPhysInterfacePHYType                  Dot11Type,
        extremeWirelessPhysInterfacePHYSupportedTypes     BITS,
        extremeWirelessPhysInterfacePreamble            INTEGER,
    extremeWirelessPhysInterfaceAbsTxPowerLevel INTEGER
}

extremeWirelessPhysInterfaceBeaconPeriod OBJECT-TYPE
        SYNTAX          INTEGER 
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This is the beacon interval to use"
        ::= { extremeWirelessPhysInterfaceRFCtlEntry 1 }

extremeWirelessPhysInterfaceTxPowerLevel OBJECT-TYPE
        SYNTAX          INTEGER (1..100)
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This is the % of max power to transmit at."
        ::= { extremeWirelessPhysInterfaceRFCtlEntry 2 }

extremeWirelessPhysInterfaceDTIMPeriod OBJECT-TYPE
        SYNTAX          INTEGER 
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This is the DTIM period."
        ::= { extremeWirelessPhysInterfaceRFCtlEntry 3 }

extremeWirelessPhysInterfaceFragLength OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                " "
        REFERENCE "ieee802dot11.2.1.1.5."
        ::= { extremeWirelessPhysInterfaceRFCtlEntry 4 }

extremeWirelessPhysInterfaceLongRetry OBJECT-TYPE
        SYNTAX          INTEGER (1..255)
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION             
                "Attribute indicates the maximum number of transmission
                 attempts of a frame whose size is > RTS."
        REFERENCE "dot11LongRetryLimit"
        ::= { extremeWirelessPhysInterfaceRFCtlEntry 5 }

extremeWirelessPhysInterfaceShortRetry OBJECT-TYPE
        SYNTAX          INTEGER (1..255)
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION             
                "Attribute indicates the maximum number of transmission
                 attempts of a frame whose size is <= RTS."
        REFERENCE "dot11ShortRetryLimit"
        ::= { extremeWirelessPhysInterfaceRFCtlEntry 6 }

extremeWirelessPhysInterfaceRTSThreshold OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-write
        STATUS          current 
        DESCRIPTION 
                " "
        REFERENCE "ieee802dot11.2.1.1.2."
        ::= { extremeWirelessPhysInterfaceRFCtlEntry 7 }

extremeWirelessPhysInterfaceSupportedDataRatesRxValue OBJECT-TYPE
        SYNTAX          Dot11Speed
        MAX-ACCESS      read-only
        STATUS          current 
        DESCRIPTION 
                "A bitmask of all supported datarates for Rx."
        ::= { extremeWirelessPhysInterfaceRFCtlEntry 8 }
        
extremeWirelessPhysInterfaceSupportedDataRatesTxValue OBJECT-TYPE
        SYNTAX          Dot11Speed
        MAX-ACCESS      read-only
        STATUS          current 
        DESCRIPTION 
                "A bitmask of all supported datarates for Tx."
        ::= { extremeWirelessPhysInterfaceRFCtlEntry 9 }

extremeWirelessPhysInterfacePHYType OBJECT-TYPE
        SYNTAX         Dot11Type
        MAX-ACCESS     read-write
        STATUS         current
        DESCRIPTION
                "This variable selects between 802.11 a/b/g 
                 for this transmitter.  It should be used by
                 ap to range check frequency, etc."
        ::= { extremeWirelessPhysInterfaceRFCtlEntry 10 }

extremeWirelessPhysInterfacePHYSupportedTypes OBJECT-TYPE
        SYNTAX          BITS { bsupported(0),
                               asupported(1),
                               gsupported(2) }
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "This is the 802.11 standard supported by this
                 interface as a bitmask"
        ::= { extremeWirelessPhysInterfaceRFCtlEntry 11 }

extremeWirelessPhysInterfacePreamble OBJECT-TYPE
        SYNTAX          INTEGER { short(0),
                                  long(1) }
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This changes the 802 preamble expected by the
                 interface."
        ::= { extremeWirelessPhysInterfaceRFCtlEntry 12 }

extremeWirelessPhysInterfaceAbsTxPowerLevel OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This is the absolute value of max power to transmit level in dBm."
    ::= { extremeWirelessPhysInterfaceRFCtlEntry 13 }

-- *************************************************************** --
-- Wireless Interface Status Table
-- *************************************************************** --
extremeWirelessInterfaceStatusTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF ExtremeWirelessInterfaceStatusEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
        "This table provides statistics and information on the
        current condition of each wireless interace.
        There is one entry per virtual and physical wireless 
        interface in this table.  The values for the physical 
        interfaces represent the sum of the values for all sub
        interfaces."
        ::= { extremeAP 5 }

extremeWirelessInterfaceStatusEntry OBJECT-TYPE
        SYNTAX          ExtremeWirelessInterfaceStatusEntry
        MAX-ACCESS      not-accessible
        STATUS          current 
        DESCRIPTION
        "Each entry in this table is indexed by either a virtual or
        a physical ifIndex."
        INDEX { ifIndex }
        ::= { extremeWirelessInterfaceStatusTable 1 }
        
ExtremeWirelessInterfaceStatusEntry ::= SEQUENCE {
        extremeWirelessIntfTotalDetected    Unsigned32,
        extremeWirelessIntfTotalAuthed      Unsigned32,
        extremeWirelessIntfTotalAuthFailed  Unsigned32,
        extremeWirelessIntfTotalAssoc       Unsigned32,
    extremeWirelessIntfTotalAssocFailed Unsigned32,
        extremeWirelessIntfRateDetected     Unsigned32,
        extremeWirelessIntfRateAuthed       Unsigned32,
        extremeWirelessIntfRateAuthFailed   Unsigned32,
    extremeWirelessIntfRateAssoc        Unsigned32,
    extremeWirelessIntfRateAssocFailed  Unsigned32,
    extremeWirelessIntfBlockTime        Unsigned32,
        extremeWirelessIntfCurrentDetected    Unsigned32,
        extremeWirelessIntfCurrentAuthed      Unsigned32,
        extremeWirelessIntfCurrentAssoc       Unsigned32,
        extremeWirelessIntfCurrentForwarding  Unsigned32}

        
extremeWirelessIntfTotalDetected OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of stations which have entered
        the detected state on this wireless interface since the last
        time the counters were cleared."
        ::= { extremeWirelessInterfaceStatusEntry 1 }
        
extremeWirelessIntfTotalAuthed OBJECT-TYPE      
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of stations which have entered
        the authenticated state on this wireless interface since the 
        last time the counters were cleared.  Note that this is equal 
        to the number of stations which have entered the forwarding 
        state.  This is not necessaryly equivalent to the number of
        stations which have succeeded in MAC-level authentication."
        ::= { extremeWirelessInterfaceStatusEntry 2 }
        
extremeWirelessIntfTotalAuthFailed OBJECT-TYPE  
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of stations which have failed
        to authenticate on this wireless interface.  Note that no
        distinction is made between a MAC-layer or higher-layer
        authentication failure."
        ::= { extremeWirelessInterfaceStatusEntry 3 }
        
extremeWirelessIntfTotalAssoc OBJECT-TYPE       
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of stations which have entered
        the associated state on this wireless interface since the 
        last time the counters were cleared."
        ::= { extremeWirelessInterfaceStatusEntry 4 }

extremeWirelessIntfTotalAssocFailed OBJECT-TYPE   
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the total number of stations which have failed
    the association on this wireless interface since the 
    last time the counters were cleared."
    ::= { extremeWirelessInterfaceStatusEntry 5 }

extremeWirelessIntfRateDetected OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the rate of clients being detected on this 
         interface over a 5 second period using EMWA averaging."
        ::= { extremeWirelessInterfaceStatusEntry 6 }

extremeWirelessIntfRateAuthed OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives teh rate of clients being authenticated on this 
    interface over a 5 second period using EMWA averaging."
        ::= { extremeWirelessInterfaceStatusEntry 7 }

extremeWirelessIntfRateAuthFailed OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the rate of clients failed authentication on this
         interface over a 5 second period using EMWA averaging."
        ::= { extremeWirelessInterfaceStatusEntry 8 }

extremeWirelessIntfRateAssoc OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the rate of clients being associated on this 
    interface over a 5 second period using EMWA averaging."
    ::= { extremeWirelessInterfaceStatusEntry 9 }

extremeWirelessIntfRateAssocFailed OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the rate of clients failing association on this 
    interface over a 5 second period using EMWA averaging."
    ::= { extremeWirelessInterfaceStatusEntry 10 }

extremeWirelessIntfBlockTime OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "This value specifies the number of ticks until traffic will be 
    allowed back on this interface.  A non-zero value indicates that
    traffic has been blocked, most likely due to countermeasures."
    ::= { extremeWirelessInterfaceStatusEntry 11 }

extremeWirelessIntfCurrentDetected OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the current number of stations which are in
        the detected state on this wireless interface."
        ::= { extremeWirelessInterfaceStatusEntry 12 }
        
extremeWirelessIntfCurrentAuthed OBJECT-TYPE    
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the current number of stations which are in
        the authenticated state on this wireless interface."
        ::= { extremeWirelessInterfaceStatusEntry 13 }
        
extremeWirelessIntfCurrentAssoc OBJECT-TYPE     
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the current number of stations which are in
        the associated state on this wireless interface."
        ::= { extremeWirelessInterfaceStatusEntry 14 }

extremeWirelessIntfCurrentForwarding OBJECT-TYPE        
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the current number of stations which are in
        the forwarding state on this wireless interface."
        ::= { extremeWirelessInterfaceStatusEntry 15 }

--TODO: Do we need to fix this table
-- *************************************************************** --
--                     AP Wireless Client Table                    --
-- *************************************************************** --
extremeWirelessClientTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF ExtremeWirelessClientEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This table augments the Dot11AccessPointAddressTableEntry
                 to add a per-client VLAN entry."
        ::= { extremeAP 11 }
        
extremeWirelessClientEntry OBJECT-TYPE
        SYNTAX          ExtremeWirelessClientEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
        "An entry in the extremeWirelessClientTable. It is possible
         for there to be multiple IEEE 802.11 interfaces on one agent,
         each with its unique MAC address. The relationship between an
         IEEE 802.11 interface and an interface in the context of the
         Internet-standard MIB is one-to-one. As such, the value of an
         ifIndex object instance can be directly used to identify
         corresponding instances of the objects defined herein. by
         ifIndex."
    INDEX {ifIndex, extremeWirelessClientID} 
        ::= { extremeWirelessClientTable 1 }

ExtremeWirelessClientEntry ::= SEQUENCE {
        extremeWirelessClientID                 MacAddress, 
        extremeWirelessClientState              INTEGER, 
        extremeWirelessClientEncryption         WPACipherSet, 
        extremeWirelessClientSignalStrength INTEGER, 
        extremeWirelessClientLinkQuality        INTEGER, 
        extremeWirelessClientVLAN               INTEGER,
        extremeWirelessClientPriority           INTEGER,
        extremeWirelessClientAuthType           ClientAuthType,
        extremeWirelessClientLastStateChangeTime        TimeTicks, 
        extremeWirelessClientTxFrames           Counter32,
        extremeWirelessClientRxFrames           Counter32,
        extremeWirelessClientTxBytes            Counter64,
        extremeWirelessClientRxBytes            Counter64,
        extremeWirelessClientLastPacketType     INTEGER,
        extremeWirelessClientSSID               OCTET STRING,
        extremeWirelessClientStatus             RowStatus,
    extremeWirelessClientIP                     IpAddress,
    extremeWirelessClientUsername           DisplayString,
    extremeWirelessClientDecryptionFailures Counter32,
    extremeWirelessClientMICFailures        Counter32}

extremeWirelessClientID OBJECT-TYPE 
    SYNTAX MacAddress 
    MAX-ACCESS read-only 
    STATUS current 
    DESCRIPTION 
        "The Unique MAC Address of the station for which this address 
         table entry pertains." 
    ::= { extremeWirelessClientEntry 1 } 

extremeWirelessClientState OBJECT-TYPE 
    SYNTAX INTEGER { detected (1),
                        authenticated (2), 
                        associated (3) ,
                        data-forwarding (4)} 
    MAX-ACCESS read-only 
    STATUS current 
    DESCRIPTION 
        "This attribute shall indicate the current state of the connection
         between a wireless station and the AP. The attribute is
         enumerated as follows: 

        1 - Detected - station has been detected, but not is communicating with AP
        2 - Authenticated - station is authenticated but not currently 
                        associated. 
        3 - Associated - station is authenticated and associated 
        4 - Data-forwarding - station is on the network
        It is assumed that if an station is deauthenticated, or disassociated 
        then it no longer has an entry the AP's Address Table." 
    ::= { extremeWirelessClientEntry 2 } 

extremeWirelessClientEncryption OBJECT-TYPE 
    SYNTAX WPACipherSet
    MAX-ACCESS read-only 
    STATUS current 
    DESCRIPTION 
        "This attribute is contains the encryption mechanism being used 
         by the station in an AP that allows mixed encryption modes." 
    ::= { extremeWirelessClientEntry 3 } 

extremeWirelessClientSignalStrength OBJECT-TYPE 
    SYNTAX INTEGER (1..100) 
    MAX-ACCESS read-only 
    STATUS current 
    DESCRIPTION 
        "This attribute shall specify the signal strength of the last
         frame received from the station in - dBm. e.g. a value of 50
         implies -50 dBm." 
    ::= { extremeWirelessClientEntry 4 } 

extremeWirelessClientLinkQuality OBJECT-TYPE 
    SYNTAX INTEGER (1..100) 
    MAX-ACCESS read-only 
    STATUS current 
    DESCRIPTION 
        "This attribute shall contain an indication of the quality 
         of the signal as measured in the last frame received from the 
         station. TBD format of this attribute" 
    ::= { extremeWirelessClientEntry 5 } 

extremeWirelessClientVLAN OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "This is the per-client VLAN which was pushed over
                 by a RADIUS server or other mechanism."
        ::= { extremeWirelessClientEntry 6 }

extremeWirelessClientPriority OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "This is a per-client 802.1p value which was either
                 configured by the RADIUS server or statically through
                 the port configuration table."
        ::= { extremeWirelessClientEntry 7 }

extremeWirelessClientAuthType OBJECT-TYPE
        SYNTAX          ClientAuthType
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "This is an indication of what access method was 
                 used to authenticated the client.  The strongest
                 mechanism used should be listed here, in case more
                 than one was used.  For example, if a combination of
                 mac-based shared-key and dot1x were used, this value
                 should indicated dot1x."
        ::= { extremeWirelessClientEntry 8 }

extremeWirelessClientLastStateChangeTime OBJECT-TYPE
        SYNTAX          TimeTicks
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "This is the sysUpTime of the switch when the clients state changed last"
        ::= { extremeWirelessClientEntry 9 }

extremeWirelessClientTxFrames OBJECT-TYPE
        SYNTAX  Counter32
        MAX-ACCESS      read-only
        STATUS  current
        DESCRIPTION
                "This is the number of packets transmitted to the client"
        ::= { extremeWirelessClientEntry 10 }

extremeWirelessClientRxFrames OBJECT-TYPE
        SYNTAX  Counter32
        MAX-ACCESS      read-only
        STATUS  current
        DESCRIPTION
                "This is the number of packets transmitted by the client"
        ::= { extremeWirelessClientEntry 11 }

extremeWirelessClientTxBytes OBJECT-TYPE
        SYNTAX  Counter64
        MAX-ACCESS      read-only
        STATUS  current
        DESCRIPTION
                "This is the number of bytes transmitted to the client"
        ::= { extremeWirelessClientEntry 12 }

extremeWirelessClientRxBytes OBJECT-TYPE
        SYNTAX  Counter64
        MAX-ACCESS      read-only
        STATUS  current
        DESCRIPTION
                "This is the number of bytes transmitted by the client"
        ::= { extremeWirelessClientEntry 13 }

extremeWirelessClientLastPacketType OBJECT-TYPE
        SYNTAX  INTEGER { data (0),
                                psPoll (1),
                                probeRequest (2),
                                disassociation (3),
                                deauthentication (4),
                                association (5),
                                reassociation (6),
                                authentication (7) }
--                              inf-beacon (8),
--                              adhoc-beacon (9) }                              
        MAX-ACCESS      read-only
        STATUS  current
        DESCRIPTION
                "This the the last packet type seen from the specific client"
        ::= { extremeWirelessClientEntry 14 }

extremeWirelessClientSSID OBJECT-TYPE
        SYNTAX  OCTET STRING
        MAX-ACCESS      read-only
        STATUS  current
        DESCRIPTION
                "The SSID that this client was using"
        ::= { extremeWirelessClientEntry 15 }

extremeWirelessClientStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS      read-write
        STATUS  current
        DESCRIPTION
                "This variable is used to delete an entry from the table.
                The only value this can be set to, is delete (6).
                
                If an entry is deleted, that is already in Associated or 
                data-forwarding state, then the AP should dis-associate the 
                particular client by sending a disassociate message.
                
                If an entry is in Authenticated state, and is deleted, then 
                the AP should 'deAuthenticate' that client.
                
                If an entry is in 'detected' state and is deleted, then the
                entry should just be removed from the table."
        ::= { extremeWirelessClientEntry 16 }

extremeWirelessClientIP OBJECT-TYPE
        SYNTAX          IpAddress
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "IP Address of the wireless client."
        ::= { extremeWirelessClientEntry 17 }

    extremeWirelessClientUsername OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Username (if any) of the wireless client."
    ::= { extremeWirelessClientEntry 18 }

extremeWirelessClientDecryptionFailures OBJECT-TYPE
        SYNTAX  Counter32
        MAX-ACCESS      read-only
        STATUS  current
        DESCRIPTION
                "This is the number of failures during decrypting packets from this client."
        ::= { extremeWirelessClientEntry 19 }

extremeWirelessClientMICFailures OBJECT-TYPE
        SYNTAX  Counter32
        MAX-ACCESS      read-only
        STATUS  current
        DESCRIPTION
                "This is the number of MIC failures for this client."
        ::= { extremeWirelessClientEntry 20 }

-- *************************************************************** --
--                  RF Profile Table                               --
-- *************************************************************** --
extremeRFProfile OBJECT IDENTIFIER ::= { extremeProfile 1 }

extremeRFProfileTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF ExtremeRFProfileEntry
        MAX-ACCESS      not-accessible
        STATUS          current 
        DESCRIPTION
                "There is one entry in this table for each RF profile
                 defined on the LAC.  Configuration for wireless intf.
                 should only be done by manipulating these variables.

                 Changes here will be reflected in the corresponding
                 802dot11 MIB variables (see references below).

                 On bootup this table should be populated with one
                 default entry for each supported type (A, G, etc)."
        ::= { extremeRFProfile 1 } 

extremeRFProfileEntry OBJECT-TYPE
        SYNTAX          ExtremeRFProfileEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                ""
        INDEX { extremeRFProfileIndex }
        ::= { extremeRFProfileTable 1 }

ExtremeRFProfileEntry ::= SEQUENCE {
        extremeRFProfileIndex           INTEGER,
        extremeRFProfileName            DisplayString,
        extremeRFProfileType            Dot11Type,
        extremeRFProfileBeaconInterval  INTEGER,
        extremeRFProfileDTIM            INTEGER,
        extremeRFProfileFragLength      INTEGER,
        extremeRFProfileRTSThresh       INTEGER,
        extremeRFProfilePreamble        INTEGER,
        extremeRFProfileShortRetry      INTEGER,
        extremeRFProfileLongRetry       INTEGER,
        extremeRFProfileStatus          RowStatus }

extremeRFProfileIndex OBJECT-TYPE
        SYNTAX          INTEGER(1..34)
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "Integer index for this table.  This is here to avoid
                 having to index into the table via the string name."
        ::= { extremeRFProfileEntry 1 }

extremeRFProfileName OBJECT-TYPE
        SYNTAX          DisplayString (SIZE(1..32))
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "String name of this profile.  The value |default| is
                 a special token and should not be allowed."
        ::= { extremeRFProfileEntry 2 }

extremeRFProfileType OBJECT-TYPE
        SYNTAX          Dot11Type
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "This is the type of this RF profile.  This
                 will decide the ranges of some of the values
                 (i.e. channel)."
        ::= { extremeRFProfileEntry 3 }

extremeRFProfileBeaconInterval OBJECT-TYPE
        SYNTAX          INTEGER(1..65535)
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "This is the number of TU between beacon frames."
        REFERENCE "ieee802dot11.1.1.1.12."
        ::= { extremeRFProfileEntry 5 }

extremeRFProfileDTIM OBJECT-TYPE
        SYNTAX          INTEGER(1..255)
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                " "
        REFERENCE "ieee802dot11.1.1.1.13."
        ::= { extremeRFProfileEntry 6 }

extremeRFProfileFragLength OBJECT-TYPE
        SYNTAX          INTEGER(256..2345)
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                " "
        REFERENCE "ieee802dot11.2.1.1.5."
        ::= { extremeRFProfileEntry 7 }

extremeRFProfileRTSThresh OBJECT-TYPE
        SYNTAX          INTEGER(0..2347)
        MAX-ACCESS      read-create
        STATUS          current 
        DESCRIPTION 
                " "
        REFERENCE "ieee802dot11.2.1.1.2."
        ::= { extremeRFProfileEntry 8 }

extremeRFProfilePreamble OBJECT-TYPE
        SYNTAX          INTEGER { short(0),
                                  long(1) }
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "This changes the 802 preamble expected by the
                 interface."
        ::= { extremeRFProfileEntry 9 }

extremeRFProfileShortRetry OBJECT-TYPE
        SYNTAX          INTEGER (1..255)
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "Attribute indicates the maximum number of transmission
                 attempts of a frame whose size is <= RTS."
        REFERENCE "dot11ShortRetryLimit"
        ::= { extremeRFProfileEntry 11 }

extremeRFProfileLongRetry OBJECT-TYPE
        SYNTAX          INTEGER (1..255)
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION             
                "Attribute indicates the maximum number of transmission
                 attempts of a frame whose size is > RTS."
        REFERENCE "dot11LongRetryLimit"
        ::= { extremeRFProfileEntry 12 }

extremeRFProfileStatus OBJECT-TYPE
        SYNTAX          RowStatus
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "Standard row-status semantics."
        ::= { extremeRFProfileEntry 13 }


-- *************************************************************** --
--                      Security Profile Table                     --
-- *************************************************************** --


extremeSecurityProfile OBJECT IDENTIFIER ::= { extremeProfile 2 }

extremeSecurityProfileTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF ExtremeSecurityProfileEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "There is one entry in this table per security 
                 profile on the LAC.  Each profile is identified by a
                 string name."
        ::= { extremeSecurityProfile 1 }

extremeSecurityProfileEntry OBJECT-TYPE
        SYNTAX          ExtremeSecurityProfileEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                ""
        INDEX { extremeSecurityProfileIndex }
        ::= { extremeSecurityProfileTable 1 }

ExtremeSecurityProfileEntry ::= SEQUENCE {
        extremeSecurityProfileIndex             INTEGER,
        extremeSecurityProfileName              DisplayString,
        extremeSecurityProfileESSName           OCTET STRING,
        extremeSecurityProfileSSIDInBeacon              TruthValue,
        extremeSecurityProfileDot11AuthMode     Dot11AuthMode,
        extremeSecurityProfileNetworkAuthMode   NetworkAuthMode,
        extremeSecurityProfileDataVlan                  INTEGER,
        extremeSecurityProfileIgnoreVSAVlan             TruthValue,
    extremeSecurityWEPDefaultKey  INTEGER,
        extremeSecurityProfileEncryptionLength  INTEGER, 
        extremeSecurityProfileStatus            RowStatus }

extremeSecurityProfileIndex OBJECT-TYPE
        SYNTAX          INTEGER(1..32)
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This is an integer index used instead of string
                 name."
        ::= { extremeSecurityProfileEntry 1 }

extremeSecurityProfileName OBJECT-TYPE
        SYNTAX          DisplayString (SIZE(1..32))
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "This is a unique string name which identifies this
                 profile.  The token |default| is special and should
                 not be allowed."
        ::= { extremeSecurityProfileEntry 2 }

extremeSecurityProfileESSName OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE(0..32))
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "This is the desired ESS name."
        REFERENCE "ieee802dot11.1.1.1.9"
        ::= { extremeSecurityProfileEntry 3 }

extremeSecurityProfileSSIDInBeacon OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "Setting this value to true will have the channel
                 place the ssid in the beacon frame."
        ::= { extremeSecurityProfileEntry 4 }

extremeSecurityProfileDot11AuthMode OBJECT-TYPE
        SYNTAX          Dot11AuthMode
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "Specified whether to use open or shared authentication"
        ::= { extremeSecurityProfileEntry 5 }

extremeSecurityProfileNetworkAuthMode OBJECT-TYPE
        SYNTAX          NetworkAuthMode
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This specifies the authentication to use on top of dot11 mac authentication"
        ::= { extremeSecurityProfileEntry 6 }

extremeSecurityProfileDataVlan OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This specifies the VLAN to use in case it does not come back as a VSA or in case the IgnoreVSAVlan is set
                 to true"
        ::= { extremeSecurityProfileEntry 7 }

extremeSecurityProfileIgnoreVSAVlan OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION     "This specifies if Vlan associations in VSAs from the radius server has to be ignored or not"
        ::= { extremeSecurityProfileEntry 8 }

extremeSecurityWEPDefaultKey OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "This value indicates the index in extremeWEPKeyTable that 
                identifies the key this interface will use to decrypt packets."
        ::= { extremeSecurityProfileEntry 9 }

extremeSecurityProfileEncryptionLength OBJECT-TYPE
    SYNTAX      INTEGER { none(0),
                          sixtyfour(64),
                          onetwentyeight(128)  }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This gives the size in bits of the key.
         This variable defines the length of all WEP keys and also
         the encryption to use in case of legacy dot1x.
         If the encryption is set to none then no WEP encryption is set."
    ::= { extremeSecurityProfileEntry 10 }

-- extremeSecurityEnableWebNetlogin OBJECT-TYPE
--        SYNTAX          TruthValue
--        MAX-ACCESS      read-create
--        STATUS          current
--        DESCRIPTION
--                "Enable disable netlogin on the wireless interface where
--                security profile is applied."
--        ::= { extremeSecurityProfileEntry 11 }

extremeSecurityProfileStatus OBJECT-TYPE
        SYNTAX          RowStatus
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "Standard row-creation semantics."
        ::= { extremeSecurityProfileEntry 11 }

extremeSecurityDot1xConfigTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF ExtremeSecurityDot1xConfigEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "There is one entry in this table per security 
                 profile on the LAC. It reflects the dot1x security config"
        ::= { extremeSecurityProfile 2 }

extremeSecurityDot1xConfigEntry OBJECT-TYPE
        SYNTAX  ExtremeSecurityDot1xConfigEntry
        MAX-ACCESS      not-accessible
        STATUS  current
        DESCRIPTION
                ""
        INDEX { extremeSecurityProfileIndex }
        ::= { extremeSecurityDot1xConfigTable 1 }

ExtremeSecurityDot1xConfigEntry ::= SEQUENCE {
        extremeSecurityKeyMgmtSuite             WPAKeyMgmtSet,
        extremeSecurityMcastCipherSuite WPACipherSet,
        extremeSecurityDot1xPSKValue            OCTET STRING,
        extremeSecurityDot1xPSKPassPhrase       DisplayString,
        extremeSecurityDot1xReAuthPeriod        INTEGER,
        extremeSecurityGroupUpdateTimeOut       Unsigned32,
        extremeSecurityPairwiseUpdateTimeOut Unsigned32
}

extremeSecurityKeyMgmtSuite OBJECT-TYPE
        SYNTAX  WPAKeyMgmtSet
        MAX-ACCESS      read-write
        STATUS  current
        DESCRIPTION
                "This bitmask configures the authentication suites to be used."
        ::= { extremeSecurityDot1xConfigEntry 1 }

extremeSecurityMcastCipherSuite OBJECT-TYPE
        SYNTAX  WPACipherSet
        MAX-ACCESS      read-write
        STATUS  current
        DESCRIPTION
                "This configures the cipher suite to use for mcast traffic. The cipher suite to use for unicast traffic
                 is derived from this using the following algorithm:
                        Mcast cipher = WEP (64/128), Unicast cipher = TKIP
                        Mcast cipher = TKIP, Unicast cipher = TKIP
                        Mcast cipher = AES, Unicast cipher = AES.
                 This therefore determines the max unicast cipher suite the client can use to associate with 
                 this interface."
        ::= { extremeSecurityDot1xConfigEntry 2 }


extremeSecurityDot1xPSKValue OBJECT-TYPE
        SYNTAX          OCTET STRING (SIZE(32))
        MAX-ACCESS      read-write
        STATUS          current 
        DESCRIPTION
                "The Pre-Shared Key (PSK) for when RSN in PSK mode is
                 the selected authentication suite."
        REFERENCE "dot11RSNConfigPSKValue"
        ::= { extremeSecurityDot1xConfigEntry 3 }

extremeSecurityDot1xPSKPassPhrase OBJECT-TYPE
        SYNTAX          DisplayString
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
        "The PSK, for when WPA in PSK mode is the selected authentication
         suite, is configured by extremeSecurityKeyMgmtSuite.
         An alternative manner of setting the PSK uses the password-to-key
         algorithm defined in section XXX. This variable provides a means
         to enter a pass phrase. When this object is written, the RSN entity
         shall use the password-to-key algorithm specified in section XXX to
         derive a pre-shared and populate extremeSecurityDot1xPSKValue with this key.
         This object is logically write-only. Reading this variable shall
         return unsuccessful status or null or zero."
        ::= { extremeSecurityDot1xConfigEntry 4 }

extremeSecurityDot1xReAuthPeriod OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "Number of seconds a clients authentication will last before
                 the AP automatically issues a reauthentication request."
        ::= { extremeSecurityDot1xConfigEntry 5 }

extremeSecurityGroupUpdateTimeOut OBJECT-TYPE
        SYNTAX          Unsigned32 (1..1440)
        UNITS           "minutes"
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "The time in minutes after which the RSN group
                 update handshake will be retried. The timer shall
                 start at the moment the group update message is
                 sent."
        REFERENCE "dot11RSNConfigGroupUpdateTimeOut"
        DEFVAL          { 100 } -- 
        ::= { extremeSecurityDot1xConfigEntry 6 }

extremeSecurityPairwiseUpdateTimeOut OBJECT-TYPE
        SYNTAX          Unsigned32 (1..1440)
        UNITS           "minutes"
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "The time in minutes after which the RSN 4-way
                 handshake will be retried. The timer shall start at
                 the moment a 4-way message is sent."
        REFERENCE "dot11RSNConfigPairwiseUpdateTimeOut"
        DEFVAL          { 100 } -- 
        ::= { extremeSecurityDot1xConfigEntry 7 }

-- *************************************************************** --
--                     Default WEP Key Table                       --
-- *************************************************************** --
extremeWEPKeyTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF ExtremeWEPKeyEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This table contains per-profile WEP keys.

                 Reference ieee802dot11.1.2.3."
        ::= { extremeSecurityProfile 4 }

extremeWEPKeyEntry OBJECT-TYPE
        SYNTAX  ExtremeWEPKeyEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                " "
        INDEX { extremeSecurityProfileIndex, extremeWEPKeyIndex }
        ::= { extremeWEPKeyTable 1 }
        
ExtremeWEPKeyEntry ::= SEQUENCE {
        extremeWEPKeyIndex      INTEGER,
        extremeWEPKey           OCTET STRING,
        extremeWEPKeyStatus     RowStatus }
        
extremeWEPKeyIndex OBJECT-TYPE
        SYNTAX          INTEGER(0..8)
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "There can be upto 8 wep keys for any wireless
                 interface. Four of the keys are to be used with
                 WEP Authentication, and the other four with MAC Auth."
        ::= { extremeWEPKeyEntry 1 }

extremeWEPKey OBJECT-TYPE
        SYNTAX          OCTET STRING (SIZE(1..19))
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "This is a write-only wep key."
        ::= { extremeWEPKeyEntry 2 }

extremeWEPKeyStatus OBJECT-TYPE
        SYNTAX          RowStatus
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "Standard row-creation semantics."
        ::= { extremeWEPKeyEntry 3 }

-- *************************************************************** --
--              Wireless Physical Interface Config Table           --
-- *************************************************************** --
extremeWirelessPhysInterfaceConfigTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF ExtremeWirelessPhysInterfaceConfigEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This table contains the configured bindings between    
                 physical wireless interfaces and RF profiles and other
                 RF properties. There is one instance of a physical wireless
                 interface per radio on the AP.

                 Entries in this table have a duration that exceeds
                 the lifetime of entries in the wirelessPhysInterfaceCtlTable.
                 A configured binding spans the reset or removal of 
                 a wireless interface.

                 Entries can be removed from this table by the user.

                 If there is a mismatch between a new wireless port
                 and a previously configured profile, the default
                 profile will be applied and this table will be
                 updated."
        ::= { extremeProfile 3 }

extremeWirelessPhysInterfaceConfigEntry OBJECT-TYPE
        SYNTAX  ExtremeWirelessPhysInterfaceConfigEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                " "
        INDEX { extremeWirelessPhysInterfaceIndex }
        ::= { extremeWirelessPhysInterfaceConfigTable 1 }

ExtremeWirelessPhysInterfaceConfigEntry ::= SEQUENCE {
        extremeWirelessPhysInterfaceConfigRFProfile             INTEGER,
        extremeWirelessPhysInterfaceConfigRFChannel             INTEGER,
        extremeWirelessPhysInterfaceConfigSpeed         Dot11Speed,
        extremeWirelessPhysInterfaceConfigPowerLevel    INTEGER 
}
        
extremeWirelessPhysInterfaceConfigRFProfile OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "This is the index into the extremeRFProfileTable for
                 the RF profile that this wireless interface is bound 
                 to.  

                 The default value is equivalent to the profile index for
                 the interface-appropriate default in the table."
        ::= { extremeWirelessPhysInterfaceConfigEntry 1 }
                 
extremeWirelessPhysInterfaceConfigRFChannel     OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "This is the RF channel which has been selected for this
                 wireless interface.  It should be one of the supported 
                 channels as given by the phy tables in the dot11 mib."
        ::= { extremeWirelessPhysInterfaceConfigEntry 2 }

extremeWirelessPhysInterfaceConfigSpeed OBJECT-TYPE
        SYNTAX          Dot11Speed
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "This is the speed to configure the interface at. A value of 0 indicates
                 automatic speed detection."
        ::= { extremeWirelessPhysInterfaceConfigEntry 3 }

extremeWirelessPhysInterfaceConfigPowerLevel OBJECT-TYPE
        SYNTAX          INTEGER 
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "This value specifies the tx power (in % of max power) to use."
        ::= { extremeWirelessPhysInterfaceConfigEntry 4 }

-- *************************************************************** --
--              Wireless Virtual  Interface Config Table           --
-- *************************************************************** --
extremeWirelessVirtInterfaceConfigTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF ExtremeWirelessVirtInterfaceConfigEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This table contains the configured bindings between    
                 virtual wireless interfaces and security profiles and other
                 security properties. There are upto 8 virtual interface for
                 each physical interface.

                 Entries in this table have a duration that exceeds
                 the lifetime of entries in the wirelessVirtInterfaceCtlTable.
                 A configured binding spans the reset or removal of 
                 a wireless interface.

                 Entries can be removed from this table by the user."

        ::= { extremeProfile 4 }

extremeWirelessVirtInterfaceConfigEntry OBJECT-TYPE
        SYNTAX  ExtremeWirelessVirtInterfaceConfigEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                " "
        INDEX { extremeWirelessVirtInterfaceIndex }
        ::= { extremeWirelessVirtInterfaceConfigTable 1 }

ExtremeWirelessVirtInterfaceConfigEntry ::= SEQUENCE {
        extremeWirelessVirtInterfaceConfigSecurityProfile       INTEGER,
        extremeWirelessVirtInterfaceConfigMaxClients                    INTEGER,
        extremeWirelessVirtInterfaceConfigWirelessBridging              TruthValue,
        extremeWirelessVirtInterfaceConfigState                 INTEGER
}
        
extremeWirelessVirtInterfaceConfigSecurityProfile OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This is the index into the extremeSecurityProfileTable for
                 the security profile that this wireless interface is bound 
                 to.  

                 The default value is equivalent to the profile index for
                 the interface-appropriate default in the table."
        ::= { extremeWirelessVirtInterfaceConfigEntry 1 }

extremeWirelessVirtInterfaceConfigMaxClients OBJECT-TYPE
        SYNTAX          INTEGER (1..128)
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "The maximum number of clients that can associate with this virtual interface."
        ::= { extremeWirelessVirtInterfaceConfigEntry 2 }

extremeWirelessVirtInterfaceConfigWirelessBridging OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This specifies whether wireless bridging is enabled on this interface.
                 If wireless bridging is enabled then traffic originating from a client on this
                 interface will be bridged to clients on the same VLAN on this or other 
                 virtual interfaces that have wireless bridging enabled. So basically
                 wireless bridging should be enabled on both the source and the destination
                 virtual interface for traffic to be bridged."
        ::= { extremeWirelessVirtInterfaceConfigEntry 3 }

extremeWirelessVirtInterfaceConfigState OBJECT-TYPE
        SYNTAX          INTEGER { enabled(0), disabled(1) } 
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This value specifies whether the virtual interface is active or not"
        ::= { extremeWirelessVirtInterfaceConfigEntry 4 }

-- *************************************************************** --
--                      Antenna Profile Table                     --
-- *************************************************************** --

extremeAntennaProfile OBJECT IDENTIFIER ::= { extremeProfile 5 }

extremeAntennaProfileTable OBJECT-TYPE
SYNTAX  SEQUENCE OF ExtremeAntennaProfileEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "There is one entry in this table per  antenna
                profile on the LAC.  Each profile is identified by a
                string name."
        ::= { extremeAntennaProfile 1 }

extremeAntennaProfileEntry OBJECT-TYPE
SYNTAX      ExtremeAntennaProfileEntry
MAX-ACCESS  not-accessible
STATUS      current
DESCRIPTION
""
        INDEX { extremeAntennaProfileIndex }
        ::= { extremeAntennaProfileTable 1 }

ExtremeAntennaProfileEntry ::= SEQUENCE
{
    extremeAntennaProfileIndex          INTEGER,
    extremeAntennaProfileName           DisplayString,
    extremeAntennaProfile2point4GHZGain INTEGER,
    extremeAntennaProfile5GHZGain               INTEGER,
    extremeAntennaProfileStatus         RowStatus 
}

extremeAntennaProfileIndex OBJECT-TYPE
    SYNTAX      INTEGER(1..32)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
    "This is an integer index used instead of string name."
    ::= { extremeAntennaProfileEntry 1 }

extremeAntennaProfileName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..32))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
    "This is a unique string name which identifies this
      profile.  The token |default| is special and should
      not be allowed."
    ::= { extremeAntennaProfileEntry 2 }

extremeAntennaProfile2point4GHZGain OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This specifies 2.4GHz gain value for detachable antenna in dbi"
    ::= { extremeAntennaProfileEntry 3 }

extremeAntennaProfile5GHZGain OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This specifies 5GHz gain value for detachable antenna in dbi"
    ::= { extremeAntennaProfileEntry 4 }

extremeAntennaProfileStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Standard row-creation semantics."
    ::= { extremeAntennaProfileEntry 5 }

-- *************************************************************** --
--                   RemoteConnect configuration                         --
-- *************************************************************** --


extremeWirelessRemoteConnectGlobalCfgGroup OBJECT IDENTIFIER ::=   { extremeProfile 6 }

extremeWirelessRemoteConnectGlobalBindingType OBJECT-TYPE
  SYNTAX                WirelessRemoteConnectBindingType
  MAX-ACCESS  read-write
  STATUS current
  DESCRIPTION
  "Global Binding Tye"
 ::= { extremeWirelessRemoteConnectGlobalCfgGroup 1 }

extremeWirelessRemoteConnectBindingTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessRemoteConnectBindingEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This table specifies the RemoteConnect binding configuration for various ports."
        ::= { extremeProfile 7 }

extremeWirelessRemoteConnectBindingEntry OBJECT-TYPE
        SYNTAX          ExtremeWirelessRemoteConnectBindingEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                " "
        INDEX { extremeWirelessRemoteConnectBindingPortIndex }
        ::= { extremeWirelessRemoteConnectBindingTable 1 }

ExtremeWirelessRemoteConnectBindingEntry ::= SEQUENCE {
        extremeWirelessRemoteConnectBindingPortIndex    INTEGER,
        extremeWirelessRemoteConnectBindingIfIndex      Integer32,
        extremeWirelessRemoteConnectBindingType WirelessRemoteConnectBindingType,
        extremeWirelessRemoteConnectBindingMAC  MacAddress,
        extremeWirelessRemoteConnectBindingSerial       OCTET STRING,
        extremeWirelessRemoteConnectBindingIPAddressType        InetAddressType,
        extremeWirelessRemoteConnectBindingIPAddress    InetAddress,
        extremeWirelessRemoteConnectBindingEnabled      TruthValue,
        extremeWirelessRemoteConnectBindingBound        TruthValue,
        extremeWirelessRemoteConnectBindingRowStatus    RowStatus}

extremeWirelessRemoteConnectBindingPortIndex    OBJECT-TYPE
        SYNTAX  INTEGER(1..48)
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION     "The index of this binding. This maps one-to-one with the value
                        specified in the CLI. For example, if you say v:1 in the CLI, then
                        this value should be 1."
        ::= { extremeWirelessRemoteConnectBindingEntry 1}

extremeWirelessRemoteConnectBindingIfIndex      OBJECT-TYPE
        SYNTAX  Integer32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION     "This is the IF index that is used in the extremeWirelessPortConfigTable
                        etc to refer to this RemoteConnect port."
        ::= { extremeWirelessRemoteConnectBindingEntry 2}

extremeWirelessRemoteConnectBindingType OBJECT-TYPE
        SYNTAX          WirelessRemoteConnectBindingType
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "This is the type of binding. Based on this, one of the following columns will be valid."
        ::= { extremeWirelessRemoteConnectBindingEntry 3 }

extremeWirelessRemoteConnectBindingMAC OBJECT-TYPE
        SYNTAX          MacAddress
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION     "The MAC address of the AP that is bound to this virtual port. 
                        This is valid only if the extremeWirelessRemoteConnectBindingType is set to
                        mac-address"
        ::= { extremeWirelessRemoteConnectBindingEntry 4}

extremeWirelessRemoteConnectBindingSerial OBJECT-TYPE
        SYNTAX          OCTET STRING
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION     "The serial number of the AP that is bound to this virtual port. 
                        This is valid only if the extremeWirelessRemoteConnectBindingType is set to
                        serial-number"
        ::= { extremeWirelessRemoteConnectBindingEntry 5}

extremeWirelessRemoteConnectBindingIPAddressType OBJECT-TYPE
        SYNTAX          InetAddressType
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION     "The IP address type of the AP that is bound to this virtual port. 
                        This is valid only if the extremeWirelessRemoteConnectBindingType is set to
                        ip-address"
        ::= { extremeWirelessRemoteConnectBindingEntry 6}

extremeWirelessRemoteConnectBindingIPAddress OBJECT-TYPE
        SYNTAX          InetAddress
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION     "The IP address of the AP that is bound to this virtual port. 
                        This is valid only if the extremeWirelessRemoteConnectBindingType is set to
                        ip-address"
        ::= { extremeWirelessRemoteConnectBindingEntry 7}

extremeWirelessRemoteConnectBindingEnabled      OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION     "An entry in this table can be created but left as disabled. If you 
                        set this variable to True then the RemoteConnect controller will consider
                        this binding when trying to map APs to RemoteConnect ports. Else, it will
                        ignore it."
        ::= {extremeWirelessRemoteConnectBindingEntry 8}

extremeWirelessRemoteConnectBindingBound        OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION     "Specifies if an AP has come up and has been matched to this binding.
                        If this is true, then the extremeWirelessPortStatus table will have
                        an entry for this RemoteConnect port."
        ::= {extremeWirelessRemoteConnectBindingEntry 9}

extremeWirelessRemoteConnectBindingRowStatus    OBJECT-TYPE
        SYNTAX          RowStatus
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION     "RowStatus attribute. When this row is deleted, the binding goes away"
        ::= {extremeWirelessRemoteConnectBindingEntry 10}

-- ***************************************************************************************
-- This table specifies how the controller should choose to redirect certain APs to other
-- controllers
-- ***************************************************************************************
extremeWirelessRemoteConnectRedirectBindingTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessRemoteConnectRedirectBindingEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This table specifies the RemoteConnect redirection configuration for various ports."
        ::= { extremeProfile 8 }

extremeWirelessRemoteConnectRedirectBindingEntry OBJECT-TYPE
        SYNTAX          ExtremeWirelessRemoteConnectRedirectBindingEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                " "
        INDEX { extremeWirelessRemoteConnectRedirectBindingIndex }
        ::= { extremeWirelessRemoteConnectRedirectBindingTable 1 }

ExtremeWirelessRemoteConnectRedirectBindingEntry ::= SEQUENCE {
        extremeWirelessRemoteConnectRedirectBindingIndex        INTEGER,
        extremeWirelessRemoteConnectRedirectBindingType WirelessRemoteConnectBindingType,
        extremeWirelessRemoteConnectRedirectBindingMAC  MacAddress,
        extremeWirelessRemoteConnectRedirectBindingSerial       OCTET STRING,
        extremeWirelessRemoteConnectRedirectBindingIPAddressType        InetAddressType,
        extremeWirelessRemoteConnectRedirectBindingIPAddress    InetAddress,
        extremeWirelessRemoteConnectRedirectBindAttachSwitchIPAddrType  InetAddressType,
        extremeWirelessRemoteConnectRedirectBindAttachSwitchIPAddr      InetAddress,
        extremeWirelessRemoteConnectRedirectBindingEnabled              TruthValue,
        extremeWirelessRemoteConnectRedirectBindingNumRedirects Counter32,
        extremeWirelessRemoteConnectRedirectBindingRowStatus            RowStatus}

extremeWirelessRemoteConnectRedirectBindingIndex        OBJECT-TYPE
        SYNTAX  INTEGER(1..255)
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION     "The index of this RedirectBinding."
        ::= { extremeWirelessRemoteConnectRedirectBindingEntry 1}

extremeWirelessRemoteConnectRedirectBindingType OBJECT-TYPE
        SYNTAX          WirelessRemoteConnectBindingType
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "This is the type of RedirectBinding. Based on this, one of the following columns will be valid."
        ::= { extremeWirelessRemoteConnectRedirectBindingEntry 2 }

extremeWirelessRemoteConnectRedirectBindingMAC OBJECT-TYPE
        SYNTAX          MacAddress
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION     "The MAC address of the AP that will be redirected. 
                        This is valid only if the extremeWirelessRemoteConnectRedirectBindingType is set to
                        mac-address"
        ::= { extremeWirelessRemoteConnectRedirectBindingEntry 3}

extremeWirelessRemoteConnectRedirectBindingSerial OBJECT-TYPE
        SYNTAX          OCTET STRING
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION     "The serial number of the AP that is bound to this virtual port. 
                        This is valid only if the extremeWirelessRemoteConnectRedirectBindingType 
                        is set to serial-number"
        ::= { extremeWirelessRemoteConnectRedirectBindingEntry 4}

extremeWirelessRemoteConnectRedirectBindingIPAddressType OBJECT-TYPE
        SYNTAX          InetAddressType
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION     "The IP address type of the AP that will be redirected. 
                        This is valid only if the extremeWirelessRemoteConnectRedirectBindingType 
                        is set to ip-address"
        ::= { extremeWirelessRemoteConnectRedirectBindingEntry 5}

extremeWirelessRemoteConnectRedirectBindingIPAddress OBJECT-TYPE
        SYNTAX          InetAddress
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION     "The IP address of the AP that will be redirected. 
                        This is valid only if the extremeWirelessRemoteConnectRedirectBindingType 
                        is set to ip-address"
        ::= { extremeWirelessRemoteConnectRedirectBindingEntry 6}

extremeWirelessRemoteConnectRedirectBindAttachSwitchIPAddrType OBJECT-TYPE
        SYNTAX          InetAddressType
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION     "The IP address type of the slave "
        ::= { extremeWirelessRemoteConnectRedirectBindingEntry 7}

extremeWirelessRemoteConnectRedirectBindAttachSwitchIPAddr OBJECT-TYPE
        SYNTAX          InetAddress
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION     "The IP address of the slave"
        ::= { extremeWirelessRemoteConnectRedirectBindingEntry 8}

extremeWirelessRemoteConnectRedirectBindingEnabled      OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION     "An entry in this table can be created but left as disabled. If you 
                        set this variable to True then the RemoteConnect controller will consider
                        this RedirectBinding when trying to redirect APs. Else, it will
                        ignore it."
        ::= {extremeWirelessRemoteConnectRedirectBindingEntry 9}

extremeWirelessRemoteConnectRedirectBindingNumRedirects OBJECT-TYPE
        SYNTAX          Counter32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION     "The number of times this redirect has been invoked."
        ::= {extremeWirelessRemoteConnectRedirectBindingEntry 10}

extremeWirelessRemoteConnectRedirectBindingRowStatus    OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION     "Standard row status semantics."
        ::= {extremeWirelessRemoteConnectRedirectBindingEntry 11}

-- ***************************************************************************************
-- This table specifies the list of APs that could not be bound or redirected due to 
-- a lack of mapping on this controller
-- ***************************************************************************************

extremeWirelessRemoteConnectDeviceDBGroup OBJECT IDENTIFIER ::=   { extremeProfile 9 }

extremeWirelessRemoteConnectDeviceDBTimeOut OBJECT-TYPE
  SYNTAX  INTEGER (0 | 30..3600)
  MAX-ACCESS  read-write
  STATUS current
  DESCRIPTION
  "Timeout value for unbound APs entry in seconds. 0 for disable"
 ::= { extremeWirelessRemoteConnectDeviceDBGroup 1 }


extremeWirelessRemoteConnectUnboundAPsTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessRemoteConnectUnboundAPsEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This table contains the list of APs that could not be bound or redirected."
        ::= { extremeProfile 10 }

extremeWirelessRemoteConnectUnboundAPsEntry OBJECT-TYPE
        SYNTAX          ExtremeWirelessRemoteConnectUnboundAPsEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                " "
        INDEX { extremeWirelessRemoteConnectUnboundAPsIndex }
        ::= { extremeWirelessRemoteConnectUnboundAPsTable 1 }

ExtremeWirelessRemoteConnectUnboundAPsEntry ::= SEQUENCE {
        extremeWirelessRemoteConnectUnboundAPsIndex     INTEGER,
        extremeWirelessRemoteConnectUnboundAPsMAC       MacAddress,
        extremeWirelessRemoteConnectUnboundAPsSerial    OCTET STRING,
        extremeWirelessRemoteConnectUnboundAPsIPAddressType     InetAddressType,
        extremeWirelessRemoteConnectUnboundAPsIPAddress InetAddress,
        extremeWirelessRemoteConnectUnboundAPsNumAttempts       Counter32,
        extremeWirelessRemoteConnectUnboundAPsRowStatus RowStatus}

extremeWirelessRemoteConnectUnboundAPsIndex     OBJECT-TYPE
        SYNTAX  INTEGER(0..65535)
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION     "The index of this table."
        ::= { extremeWirelessRemoteConnectUnboundAPsEntry 1}

extremeWirelessRemoteConnectUnboundAPsMAC OBJECT-TYPE
        SYNTAX          MacAddress
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION     "The MAC address of the unbound AP."
        ::= { extremeWirelessRemoteConnectUnboundAPsEntry 2}

extremeWirelessRemoteConnectUnboundAPsSerial OBJECT-TYPE
        SYNTAX          OCTET STRING
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION     "The serial number of the unbound AP"
        ::= { extremeWirelessRemoteConnectUnboundAPsEntry 3}

extremeWirelessRemoteConnectUnboundAPsIPAddressType OBJECT-TYPE
        SYNTAX          InetAddressType
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION     "The IP address type of the unbound AP"
        ::= { extremeWirelessRemoteConnectUnboundAPsEntry 4}

extremeWirelessRemoteConnectUnboundAPsIPAddress OBJECT-TYPE
        SYNTAX          InetAddress
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION     "The IP address of the unbound AP"
        ::= { extremeWirelessRemoteConnectUnboundAPsEntry 5}

extremeWirelessRemoteConnectUnboundAPsNumAttempts       OBJECT-TYPE
        SYNTAX          Counter32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION     "The number of times this AP contacted this controller."
        ::= {extremeWirelessRemoteConnectUnboundAPsEntry 6}

extremeWirelessRemoteConnectUnboundAPsRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION     "Standard row status semantics. Only valid value to set is destroy (6)."
        ::= {extremeWirelessRemoteConnectUnboundAPsEntry 7}

-- *************************************************************** --
--                   RADIUS Server Configuration                   --
-- The Radius Server Table on the Ethernet switch is implemented   --
-- using the extremeAuthServerTable, defines under extremeServices --
--                                                                 --
-- The extremeAPAuthServerTable is implemented per wireless port.  --
-- Each AP will have to implement this table to allow the LAC to   --
-- propogate configuration information.                            --
-- *************************************************************** --
extremeAPAuthServerTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF ExtremeAPAuthServerEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This table is proxied by the wireless APs.  It 
                 allows the wireless concentrator to configure the 
                 APs security settings."
        ::= { extremeAP 12 }

extremeAPAuthServerEntry OBJECT-TYPE
        SYNTAX          ExtremeAPAuthServerEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                " "
        INDEX { extremeWirelessPortIfIndex, extremeAPAuthServerIndex }
        ::= { extremeAPAuthServerTable 1 }

ExtremeAPAuthServerEntry ::= SEQUENCE {
        extremeAPAuthServerIndex                INTEGER,
        extremeAPAuthServerAddressType          InetAddressType,
        extremeAPAuthServerAddress              InetAddress,
        extremeAPAuthServerPort                 INTEGER,
        extremeAPAuthServerSecret               OCTET STRING,
        extremeAPAuthServerReTransmit           INTEGER,
        extremeAPAuthServerStatus               TruthValue}

extremeAPAuthServerIndex OBJECT-TYPE
        SYNTAX          INTEGER (1..2)
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "Integer representing either primary (1) or backup
                 (2) server."
        ::= { extremeAPAuthServerEntry 1 }

extremeAPAuthServerAddressType          OBJECT-TYPE
        SYNTAX                          InetAddressType
        MAX-ACCESS                      read-only
        STATUS                          current
        DESCRIPTION
            "The type of address specified in the object
                'extremeAuthServerAddress'.
             Currently, only 'ipv4' and 'dns' are supported."
        DEFVAL { ipv4 }
      ::= { extremeAPAuthServerEntry 2 }

extremeAPAuthServerAddress OBJECT-TYPE
        SYNTAX          InetAddress
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "IP address of the radius server.  The act of
                 assigning an IP address enables the client to use
                 the server.  Setting this value to 0.0.0.0 disables
                 this entry."
        ::= { extremeAPAuthServerEntry 3 }

extremeAPAuthServerPort                    OBJECT-TYPE
       SYNTAX                          INTEGER (0..65535)
       MAX-ACCESS                      read-only
       STATUS                          current
       DESCRIPTION
           "The UDP port number of the remote syslog server
                to which syslog messages will be sent."
     ::= { extremeAPAuthServerEntry 4 }

extremeAPAuthServerSecret OBJECT-TYPE
        SYNTAX          OCTET STRING
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This is the shared secret between the Authenticator
                 and radius server.  This is logically write-only."
        ::= { extremeAPAuthServerEntry 5 }

extremeAPAuthServerReTransmit OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This is the timeout in seconds after which the 
                 Authenticator will re transmit requests to the
                 radius server."
        ::= { extremeAPAuthServerEntry 6 }

extremeAPAuthServerStatus OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS  read-write
        STATUS current
        DESCRIPTION
                "Specifies whether the DNS entry is in use or not"
        ::= { extremeAPAuthServerEntry 7 }

-- *************************************************************** --
-- Scan Configuration Table : This table provides the ability to   --
-- configure the parameters associated with ON-Channel scanning    --
-- for other access points.                                        --
-- *************************************************************** --
extremeWirelessScanCfgTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessScanCfgEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "This table contains one entry per wireless interface.  It
         allows for configuration of active and passive scan
         parameters."
         ::= { extremeAP 24 }

extremeWirelessScanCfgEntry OBJECT-TYPE
        SYNTAX ExtremeWirelessScanCfgEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        ""
        INDEX { ifIndex }
         ::= { extremeWirelessScanCfgTable 1 }

ExtremeWirelessScanCfgEntry ::= SEQUENCE {
        extremeWirelessScanEnable                       TruthValue,
        extremeWirelessScanSendProbe                    TruthValue,
        extremeWirelessScanProbeInterval                Unsigned32,
        extremeWirelessScanResultTableSize              Unsigned32,
        extremeWirelessScanResultTimeout                Unsigned32,
        extremeWirelessScanResetStats                   TruthValue,
        extremeWirelessScanClearTable                   TruthValue,
        extremeWirelessScanSendAPAddedTrap              TruthValue,
        extremeWirelessScanSendAPRemovedTrap            TruthValue,
        extremeWirelessScanSendAPUpdatedTrap            TruthValue
}

extremeWirelessScanEnable OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "By setting this to true the wireless interface will collect
         information from beacons and (possible) probe responses.  If
         this value is set to false this information will not be 
         collected."
        DEFVAL { true }
         ::= { extremeWirelessScanCfgEntry 1 }

extremeWirelessScanSendProbe OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "If this value is set to TRUE the wireless interface will send
         probe requests to the broadcast SSID every ProbeInterval.  The
         results of these probes will be recorded in the scan results
         table.  If this is false, the AP will only collect information
         from beacon frames."
        DEFVAL { false }
         ::= { extremeWirelessScanCfgEntry 2 }

extremeWirelessScanProbeInterval OBJECT-TYPE
        SYNTAX Unsigned32
        UNITS "milliseconds"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "This allows for the configuration of the interval over which
         probe requests will be sent."
        DEFVAL { 100 }
         ::= { extremeWirelessScanCfgEntry 3 }

extremeWirelessScanResultTableSize OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "This parameter permits the configuration of the result table
         size.  If there are more entries discovered than there are 
         room for the new entry will replace the oldest entry in the
         table.  In this case a new entry trap will be sent with the
         OverFlow value set to TRUE."
        DEFVAL { 1024 }
         ::= { extremeWirelessScanCfgEntry 4 }

extremeWirelessScanResultTimeout OBJECT-TYPE
        SYNTAX Unsigned32
        UNITS "seconds"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "By default the scan result table will age out entries which
         haven't been updated for some time.  When an entry is aged
         out of the table a scanResultAgeOut trap is generated.  
         Setting this value to 0 will disable the aging out of entries."
        DEFVAL { 3600 }
         ::= { extremeWirelessScanCfgEntry 5 }

extremeWirelessScanResetStats OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Setting this to TRUE will cause the scan module to reset its
         internal statistics, as well as the packet counts for each 
         entry in the scan results table.  It will *not* remove any
         entries in the scan table."
         ::= { extremeWirelessScanCfgEntry 6 }

extremeWirelessScanClearTable OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Setting this to TRUE will cause the scan module to reset its
         internal table.  All currently detected stations will be 
         removed.  Scan statistics (i.e. watermark) will not be reset."
         ::= { extremeWirelessScanCfgEntry 7 }

extremeWirelessScanSendAPAddedTrap OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Setting this to TRUE will cause the scan module to send a trap
         whenever a new entry is added to the scan results table.  If
         this value is false the scan module will suppress the trap."
        DEFVAL { true }
         ::= { extremeWirelessScanCfgEntry 8 }

extremeWirelessScanSendAPRemovedTrap OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Setting this to TRUE will cause the scan module to send a trap
         whenever an entry is removed from the scan results table."
        DEFVAL { true }
         ::= { extremeWirelessScanCfgEntry 9 }

extremeWirelessScanSendAPUpdatedTrap OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Setting this to TRUE will cause the scan module to send a trap
         whenever an entry is updated in the scan results table.  This 
         will happen if the list of IEs sent from a particular MAC address
         changes."
        DEFVAL { true }
         ::= { extremeWirelessScanCfgEntry 10 }

-- *************************************************************** --
-- Off-Channel AP Scan : This table provides the ability to confi  --
-- ure and start an off-channel scan for other APs.                --
-- *************************************************************** --
extremeWirelessOffChannelScanCfgTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessOffChannelScanCfgEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "This table contains one entry per wireless interface.  It
         allows for configuration of off-channel scan.  To start an
         off-channel scan the management station should write values
         for channel list, min and max wait.  Toggling the start
         value at this point will start an off-channel scan, unless
         one is already running.
         Results of the off-channel scan are reported to the scan
         results table together with the results of passive scan."
         ::= { extremeAP 25 }

extremeWirelessOffChannelScanCfgEntry OBJECT-TYPE
        SYNTAX ExtremeWirelessOffChannelScanCfgEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        ""
        INDEX { ifIndex }
         ::= { extremeWirelessOffChannelScanCfgTable 1 }

ExtremeWirelessOffChannelScanCfgEntry ::= SEQUENCE {
        extremeWirelessOffChannelScanStart              TruthValue,
        extremeWirelessOffChannelScanList               BITS,
        extremeWirelessOffChannelScanMinWait            Unsigned32,
        extremeWirelessOffChannelScanMaxWait            Unsigned32,
        extremeWirelessOffChannelContinuous             TruthValue
}

extremeWirelessOffChannelScanStart OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Setting this to TRUE will cause the scan module to start an
         off-channel scan.  The radio will be disabled for the 
         duration of the scan.  The scan module will change to each 
         of the specified channels in order.  It will then conduct 
         passive (and perhaps active) scans on that channel for the 
         configured intervals.  When the scan is finished the radio 
         will be re-enabled.
         The scan will wait on each channel for at least MinWait 
         milliseconds even if it sees no traffic on the channel. It
         will wait for at most MaxWait msecs even if it sees traffic.
         As a result the best case time for the scan is given by:
                # Of Channels * extremeWirelessOffChannelScanMinWait
         The worst case completion time is given by:
                # Of Channels * extremeWirelessOffChannelScanMaxWait
         Results of the off-channnel scan a reported to the scan 
         results table."
         ::= { extremeWirelessOffChannelScanCfgEntry 1 }

extremeWirelessOffChannelScanList OBJECT-TYPE
        SYNTAX BITS {
                scanAll(0),
                scanEvery(1),
                scanChannel1(2),
                scanChannel2(3),
                scanChannel3(4),
                scanChannel4(5),
                scanChannel5(6),
                scanChannel6(7),
                scanChannel7(8),
                scanChannel8(9),
                scanChannel9(10),
                scanChannel10(11),
                scanChannel11(12),
                scanChannel12(13),
                scanChannel13(14),
                scanChannel14(15),
                scanChannel34(16),
                scanChannel36(17),
                scanChannel40(18),
                scanChannel44(19),
                scanChannel48(20),
                scanChannel52(21),
                scanChannel56(22),
                scanChannel60(23),
                scanChannel64(24),
                scanChannel100(25),
                scanChannel104(26),
                scanChannel108(27),
                scanChannel113(28),
                scanChannel116(29),
                scanChannel120(30),
                scanChannel124(31),
                scanChannel128(32),
                scanChannel132(33),
                scanChannel140(34),
                scanChannel149(35),
                scanChannel153(36),
                scanChannel157(37),
                scanChannel161(38),
                scanChannel165(39)
        }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "This value controls the channels which will be scanned during
         the off-channel scan.  Two special values should be noted:
         
         all -   causes the radio to scan all channels supported by
                 the configured country code.  While on each channel
                     the radio will send out probe requests if the value
                     of extremeWirelessScanSendProbeRequest is true.
         every - causes the radio to scan all channels, even those
                     which are restricted by the country code.  The
                         radio will only send probe request on channels that
                         are legal for that country code."
         ::= { extremeWirelessOffChannelScanCfgEntry 2 }

extremeWirelessOffChannelScanMinWait OBJECT-TYPE
        SYNTAX Unsigned32
        UNITS "milliseconds"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "This value controls the minimum time the off-channel scan
         will wait on a particular channel if it doesn't see any
         traffic."
         DEFVAL { 1 }
         ::= { extremeWirelessOffChannelScanCfgEntry 3 }

extremeWirelessOffChannelScanMaxWait OBJECT-TYPE
        SYNTAX Unsigned32
        UNITS "milliseconds"
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "This value controls the maximum time the off-channel scan will
         wait on a particular channel even if it is receiving beacons
         etc."
         DEFVAL { 10 }
         ::= { extremeWirelessOffChannelScanCfgEntry 4 }

extremeWirelessOffChannelContinuous OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
 
        DESCRIPTION
        "Setting this value to true results in the off-channel scan
        looping on the configured values until the channel scan is
        disabled."
        DEFVAL { false }
         ::= { extremeWirelessOffChannelScanCfgEntry 5 }
 


-- *************************************************************** --
-- Scan Status Table : This table contains information about the   --
-- current status of the scan feature.                             --
-- *************************************************************** --
extremeWirelessScanStatusTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessScanStatusEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "This table contains one entry per wireless interface.  It
         provides status and statistics information for the scan 
         feature operating on that wireless interface."
         ::= { extremeAP 26 }

extremeWirelessScanStatusEntry OBJECT-TYPE
        SYNTAX ExtremeWirelessScanStatusEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        ""
        INDEX { ifIndex }
         ::= { extremeWirelessScanStatusTable 1 }

ExtremeWirelessScanStatusEntry ::= SEQUENCE {
        extremeWirelessScanCurrentTableSize     Unsigned32,
        extremeWirelessScanTableWatermark       Unsigned32,
        extremeWirelessScanTotalOverflows       Unsigned32,
        extremeWirelessScanTotalTimeouts        Unsigned32,
        extremeWirelessScanOffChannelRunning    TruthValue,
        extremeWirelessScanCurrentChannel       Unsigned32,
        extremeWirelessScanLastElement          TimeTicks,
        extremeWirelessScanNumProbes            Unsigned32
}

extremeWirelessScanCurrentTableSize OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This indicates the current number of entries in the scan results
         table."
         ::= { extremeWirelessScanStatusEntry 1 }

extremeWirelessScanTableWatermark OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This indicates the largest size the results table has reached
         since the status values have been reset, or the system has
         booted."
         ::= { extremeWirelessScanStatusEntry 2 }

extremeWirelessScanTotalOverflows OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of entries which have been removed
         to make room for a newer entry.   This should be equal to the
         number of AP added traps the system has generated with the 
         overflow value set to true."
         ::= { extremeWirelessScanStatusEntry 3 }

extremeWirelessScanTotalTimeouts OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of entries which have been removed
         because they have become stale.  This should be equal to the 
         number of AP removed traps sent by the system."
         ::= { extremeWirelessScanStatusEntry 4 }

extremeWirelessScanOffChannelRunning OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "If this value is true it indicates that an off-channel scan is
         currently running.  This implies that the radio is current
         disabled."
         ::= { extremeWirelessScanStatusEntry 5 }

extremeWirelessScanCurrentChannel OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "If the value of extremeWirelessScanOffChannelRunning is true
         this variable give the value of the current channel the AP is
         scanning on.  If a scan is not running, the value of this variable
         is undefined."
         ::= { extremeWirelessScanStatusEntry 6 }

extremeWirelessScanLastElement OBJECT-TYPE
        SYNTAX TimeTicks
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the sysUpTime when the last new station was inserted
         in the results table."
         ::= { extremeWirelessScanStatusEntry 7 }

extremeWirelessScanNumProbes OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of probe requests sent by this wireless 
         interface."
         ::= { extremeWirelessScanStatusEntry 8 }

-- *************************************************************** --
-- Scan Results Table : This table provides information collected  --
-- during on and off-channel scans about the APs discovered.       --
-- *************************************************************** --
extremeWirelessScanResultsTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessScanResultsEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "This table contains one entry per wireless interface.  It
         provides status and statistics information for the scan 
         feature operating on that wireless interface."
         ::= { extremeAP 27 }

extremeWirelessScanResultsEntry OBJECT-TYPE
        SYNTAX ExtremeWirelessScanResultsEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        ""
        INDEX { ifIndex, extremeWirelessScanResultsStationId }
         ::= { extremeWirelessScanResultsTable 1 }

ExtremeWirelessScanResultsEntry ::= SEQUENCE {
        extremeWirelessScanResultsStationId              MacAddress,
        extremeWirelessScanResultsFirstSeen              TimeTicks,
        extremeWirelessScanResultsLastChange             TimeTicks,
        extremeWirelessScanResultsPacketTime             INTEGER,
        extremeWirelessScanResultsPacketRate             INTEGER,
        extremeWirelessScanResultsChannel                INTEGER,
        extremeWirelessScanResultsMinRSS                 INTEGER,
        extremeWirelessScanResultsMaxRSS                 INTEGER,
        extremeWirelessScanResultsAvgRSS                 INTEGER,
        extremeWirelessScanResultsTotalBeacons           Unsigned32,
        extremeWirelessScanResultsTotalProbes            Unsigned32,
        extremeWirelessScanResultsDiscoveredBy           INTEGER,
        extremeWirelessScanResultsDSSOFDM                TruthValue,
        extremeWirelessScanResultsRSNEnabled             TruthValue,
        extremeWirelessScanResultsGShortSlot             TruthValue,
        extremeWirelessScanResultsChannelAgility         TruthValue,
        extremeWirelessScanResultsPBCC                   TruthValue,
        extremeWirelessScanResultsPreamble               TruthValue,
        extremeWirelessScanResultsPrivacy                TruthValue,
        extremeWirelessScanResultsCFPollReq              TruthValue,
        extremeWirelessScanResultsCFPollable             TruthValue,
        extremeWirelessScanResultsNetworkType            INTEGER,
        extremeWirelessScanResultsSSID                   OCTET STRING,
        extremeWirelessScanResultsRateSet                OCTET STRING,
        extremeWirelessScanResultsExtRateSet             OCTET STRING,
        extremeWirelessScanResultsDSSParameter           INTEGER,
        extremeWirelessScanResultsTIMCount               INTEGER,
        extremeWirelessScanResultsTIMPeriod              INTEGER,
        extremeWirelessScanResultsTIMTrafficInd          TruthValue,
        extremeWirelessScanResultsCountryCode            OCTET STRING,
        extremeWirelessScanWPAIEPresent                  TruthValue,
        extremeWirelessScanWPAVersion                    Unsigned32,
        extremeWirelessScanWPAIEMcastCipher              WPACipherSet,
        extremeWirelessScanWPAUcastCipherCount           Unsigned32,
        extremeWirelessScanWPAUcastCipher                WPACipherSet,
        extremeWirelessScanWPAKeyMgmtCount               Unsigned32,
        extremeWirelessScanWPAKeyMgmtSuite               WPAKeyMgmtSet,
        extremeWirelessScanResultsIEBlob                 OCTET STRING
}
        
extremeWirelessScanResultsStationId OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the MAC address of the detected station."
         ::= { extremeWirelessScanResultsEntry 1 }

extremeWirelessScanResultsFirstSeen OBJECT-TYPE
        SYNTAX TimeTicks
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the sysUpTime when this station entry was created."
         ::= { extremeWirelessScanResultsEntry 2 }

extremeWirelessScanResultsLastChange OBJECT-TYPE
        SYNTAX TimeTicks
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the sysUpTime of the station entry the last time it was
         updated (i.e. a beacon etc was received)."
         ::= { extremeWirelessScanResultsEntry 3 }

extremeWirelessScanResultsPacketTime OBJECT-TYPE
        SYNTAX INTEGER
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the timestamp field from the last beacon/probe response
         received from this station."
         ::= { extremeWirelessScanResultsEntry 4 }

extremeWirelessScanResultsPacketRate OBJECT-TYPE
        SYNTAX INTEGER
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the rate at which the last packet was sent by the
         station.

         TODO: What are the units here on rate?"
         ::= { extremeWirelessScanResultsEntry 5 }

extremeWirelessScanResultsChannel OBJECT-TYPE
        SYNTAX INTEGER
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the channel the last packet received by this station
         was recieved on."
         ::= { extremeWirelessScanResultsEntry 6 }

extremeWirelessScanResultsMinRSS OBJECT-TYPE
        SYNTAX INTEGER
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the smallest RSS value of any packet recieved from this
         station."
         ::= { extremeWirelessScanResultsEntry 7 }

extremeWirelessScanResultsMaxRSS OBJECT-TYPE
        SYNTAX INTEGER
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the largest RSS value of any packet recieved from this
         station."
         ::= { extremeWirelessScanResultsEntry 8 }

extremeWirelessScanResultsAvgRSS OBJECT-TYPE
        SYNTAX INTEGER
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is a running average of RSS values of all the packets
         received from this station."
         ::= { extremeWirelessScanResultsEntry 9 }

extremeWirelessScanResultsTotalBeacons OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This counter gives the total number of beacons received from this
         station."
         ::= { extremeWirelessScanResultsEntry 10 }

extremeWirelessScanResultsTotalProbes OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This counter gives the total number of probe responses
         received from this station."
         ::= { extremeWirelessScanResultsEntry 11 }

extremeWirelessScanResultsDiscoveredBy OBJECT-TYPE
        SYNTAX INTEGER { probe (1),
                         beacon (2) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the type of packet which cause this results entry to be
         created."
         ::= { extremeWirelessScanResultsEntry 12 }

extremeWirelessScanResultsDSSOFDM OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "TODO : What is this?"
         ::= { extremeWirelessScanResultsEntry 13 }

extremeWirelessScanResultsRSNEnabled OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Indicates if RSN capabilities are enabled on the sending station."
         ::= { extremeWirelessScanResultsEntry 14 }

extremeWirelessScanResultsGShortSlot OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "TODO : What is this?"
         ::= { extremeWirelessScanResultsEntry 15 }

extremeWirelessScanResultsChannelAgility OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "TODO : What is this?"
         ::= { extremeWirelessScanResultsEntry 16 }

extremeWirelessScanResultsPBCC OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "TODO : What is this?"
         ::= { extremeWirelessScanResultsEntry 17 }

extremeWirelessScanResultsPreamble OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "TODO : What is this?"
         ::= { extremeWirelessScanResultsEntry 18 }

extremeWirelessScanResultsPrivacy OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is true if MAC-based privacy is invoked on the sending
         station."
         ::= { extremeWirelessScanResultsEntry 19 }

extremeWirelessScanResultsCFPollReq OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "TODO: What is this?"
         ::= { extremeWirelessScanResultsEntry 20 }

extremeWirelessScanResultsCFPollable OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "TODO: What is this?"
         ::= { extremeWirelessScanResultsEntry 21 }

extremeWirelessScanResultsNetworkType OBJECT-TYPE
        SYNTAX INTEGER { ibss (1),
                         bss  (2) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This indicates what type of network it is.  If this value is IBSS
         the last beacon/probe response was sent by a host operating in
         ad-hoc mode."
         ::= { extremeWirelessScanResultsEntry 22 }

extremeWirelessScanResultsSSID OBJECT-TYPE
        SYNTAX OCTET STRING
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This provides the value of the SSID value as is was recieved in
         the beacon or probe response.  If no SSID was sent in the probe
         this value is NULL."
         ::= { extremeWirelessScanResultsEntry 23 }

extremeWirelessScanResultsRateSet OBJECT-TYPE
        SYNTAX OCTET STRING
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This provides the value of the rate set IE as it was received in
         the beacon or probe response.  If no rate set was recieved then
         this value is NULL."
         ::= { extremeWirelessScanResultsEntry 24 }

extremeWirelessScanResultsExtRateSet OBJECT-TYPE
        SYNTAX OCTET STRING
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This provides the value of the extended rate set IE as it was 
         received in the beacon or probe response.  If no rate set was 
         recieved then this value is NULL."
         ::= { extremeWirelessScanResultsEntry 25 }

extremeWirelessScanResultsDSSParameter OBJECT-TYPE
        SYNTAX INTEGER
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Provides the value of the DSS parameter IE, which is the channel."
         ::= { extremeWirelessScanResultsEntry 26 }

extremeWirelessScanResultsTIMCount OBJECT-TYPE
        SYNTAX INTEGER
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "TODO: What is this?"
         ::= { extremeWirelessScanResultsEntry 27 }

extremeWirelessScanResultsTIMPeriod OBJECT-TYPE
        SYNTAX INTEGER
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "TODO: What is this?"
         ::= { extremeWirelessScanResultsEntry 28 }

extremeWirelessScanResultsTIMTrafficInd OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "TODO: What is this?"
         ::= { extremeWirelessScanResultsEntry 29 }

extremeWirelessScanResultsCountryCode OBJECT-TYPE
        SYNTAX OCTET STRING
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Value of country code supplied by the IE"
         ::= { extremeWirelessScanResultsEntry 30 }

extremeWirelessScanWPAIEPresent OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "If this value is true it indicates that WPA information was
         gathered from this AP in the last beacon.  It implies that
         the WPA variables below are valid.
         If this value is false it indicates that this AP did not 
         send a WPA IE in its last beacon, and the values below are
         meaningless."
        ::= { extremeWirelessScanResultsEntry 31 }

extremeWirelessScanWPAVersion OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This value gives the version of WPA supported by this AP.
         See IEEE 802.11i Draft 3.0 section 7 for meaning of various
         values."
        ::= { extremeWirelessScanResultsEntry 32 }

extremeWirelessScanWPAIEMcastCipher OBJECT-TYPE
        SYNTAX WPACipherSet
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This value gives the single multicast cipher supported by this
         AP."
        ::= { extremeWirelessScanResultsEntry 33 }

extremeWirelessScanWPAUcastCipherCount OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This value gives the total number of unicast ciphers supported
         by this AP.  It corresponds to the number of bits set in the 
         extremeWirelessScanWPAUcastCipher variable."
        ::= { extremeWirelessScanResultsEntry 34 }

extremeWirelessScanWPAUcastCipher OBJECT-TYPE
        SYNTAX WPACipherSet
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the list of cipher suites which are supported by 
         this AP."
        ::= { extremeWirelessScanResultsEntry 35 }

extremeWirelessScanWPAKeyMgmtCount OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of key-management schemes supported by
         this AP.  It corresponds to the number of bits set in the
         extremeWirelessScanWPAKeyMgmtSuite variable."
        ::= { extremeWirelessScanResultsEntry 36 }

extremeWirelessScanWPAKeyMgmtSuite OBJECT-TYPE
        SYNTAX WPAKeyMgmtSet
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This indicates the supported key-management suites supported
         by this AP."
        ::= { extremeWirelessScanResultsEntry 37 }

extremeWirelessScanResultsIEBlob OBJECT-TYPE
        SYNTAX OCTET STRING
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "All the IEs received in the last packet encoded as a blob of
         Type, Length, Value tuples."
         ::= { extremeWirelessScanResultsEntry 38 }

-- *************************************************************** --
-- Probe Info Configuration Table : This table allows for config   --
-- for the collection of probe request packets.  The AP uses this  --
-- to populate the client information tables.                      --
-- *************************************************************** --
extremeWirelessProbeInfoCfgTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessProbeInfoCfgEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "This table contains one entry per physical and virtual interface.
         It controls the collection of client information via PROBE REQ
         packets."
         ::= { extremeAP 28 } 

extremeWirelessProbeInfoCfgEntry OBJECT-TYPE
        SYNTAX ExtremeWirelessProbeInfoCfgEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Note that the ifIndex here can be either a physical or virtual
         wireless interface index."
        INDEX { ifIndex }
         ::= { extremeWirelessProbeInfoCfgTable 1 }

ExtremeWirelessProbeInfoCfgEntry ::= SEQUENCE {
        extremeWirelessProbeInfoEnable           TruthValue,
        extremeWirelessProbeInfoKeepIEs          TruthValue,
        extremeWirelessProbeInfoTableSize        Unsigned32,
        extremeWirelessProbeInfoTimeout          Unsigned32,
        extremeWirelessProbeInfoTableClear       TruthValue,
        extremeWirelessProbeInfoSourceClear      MacAddress,
        extremeWirelessProbeInfoTableStatsClear  TruthValue,
        extremeWirelessProbeInfoSourceStatsClear MacAddress,
        extremeWirelessProbeInfoSendAddedTrap    TruthValue,
        extremeWirelessProbeInfoSendRemovedTrap  TruthValue }

extremeWirelessProbeInfoEnable OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "If this is set to TRUE then this virtual or physical
        interface will register with the MAC layer to receive
        notification of PROBE REQ packets.  In the case of 
        a virtual interface this implies the receipt of directed
        PROBE REQ packets.  If set to FALSE no PROBE REQ packets
        will be received, and current entries will eventually
        timeout."
        DEFVAL { true }
         ::= { extremeWirelessProbeInfoCfgEntry 1 }

extremeWirelessProbeInfoKeepIEs OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "If this value is set to TRUE then the rate IE which
         is carried in the PROBE REQ packet will be recorded.
         If FALSE, no rate information will be kept."
         DEFVAL { false }
         ::= { extremeWirelessProbeInfoCfgEntry 2 }

extremeWirelessProbeInfoTableSize OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "This value sets the maximum size of the probe info 
         results table, which limits the number of clients this
         AP can record PROBE REQ information from."
         DEFVAL { 128 }
         ::= { extremeWirelessProbeInfoCfgEntry 3 }

extremeWirelessProbeInfoTimeout OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "This is the timeout, in seconds, for an entry in the 
         probe info table.  Once a PROBE REQ has not been heard
         from a client in this time period, it's entry is removed.
         The value 0 is a sentinel, indicating no timeout."
         DEFVAL { 3600 }
         ::= { extremeWirelessProbeInfoCfgEntry 4 }

extremeWirelessProbeInfoTableClear OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Setting this value to TRUE causes all entries in the 
         probe info table to be removed.  Reading this value
         has no meaning."
         ::= { extremeWirelessProbeInfoCfgEntry 5 }

extremeWirelessProbeInfoSourceClear OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Setting this to the value of some MAC address results in
         any matching MAC address in the probe info table being
         removed.  Reading this value has no meaning."
         ::= { extremeWirelessProbeInfoCfgEntry 6 }

extremeWirelessProbeInfoTableStatsClear OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Setting this to TRUE results in all historical statistics
         in the probe info table being set to 0.  No entries will
         be removed.  Reading this has no meaning."
         ::= { extremeWirelessProbeInfoCfgEntry 7 }

extremeWirelessProbeInfoSourceStatsClear OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Setting this to a MAC address will clear the historical
         stats associated with the matching MAC address in the
         probe info table.  Reading this has no meaning."
         ::= { extremeWirelessProbeInfoCfgEntry 8 }

extremeWirelessProbeInfoSendAddedTrap OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Setting this to TRUE will cause the management module to
         send a trap whenever a new PROBE REQ source is added to 
         the probe info table.  Setting this to FALSE will 
         suppress the trap."
         DEFVAL { false }
         ::= { extremeWirelessProbeInfoCfgEntry 9 }

extremeWirelessProbeInfoSendRemovedTrap OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Setting this to TRUE will cause the management module to
         send a trap whenever a PROBE REQ source is removed from
         the probe info table.  Setting this to false will 
         suppress the trap."
         DEFVAL { false }
         ::= { extremeWirelessProbeInfoCfgEntry 10 }

-- *************************************************************** --
-- Probe Info Status Table : This table gives current status of    --
-- the probe request storage feature.                              --
-- *************************************************************** --
extremeWirelessProbeInfoStatusTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessProbeInfoStatusEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "This table contains one entry per physical and virtual interface.
         It gives debugging and status information for the operation of the
         probe info feature on that interface."
         ::= { extremeAP 29 }

extremeWirelessProbeInfoStatusEntry OBJECT-TYPE
        SYNTAX ExtremeWirelessProbeInfoStatusEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Note that the ifIndex here can be either a physical or virtual
         wireless interface index."
        INDEX { ifIndex }
         ::= { extremeWirelessProbeInfoStatusTable 1 }

ExtremeWirelessProbeInfoStatusEntry ::= SEQUENCE {
        extremeWirelessProbeInfoStatusCurrentTableSize Unsigned32,
        extremeWirelessProbeInfoStatusWatermark        Unsigned32,
        extremeWirelessProbeInfoStatusTotalOverflows   Unsigned32,
        extremeWirelessProbeInfoStatusTotalTimeouts    Unsigned32,
        extremeWirelessProbeInfoStatusLastElement      TimeTicks,
        extremeWirelessProbeInfoStatusTotalProbes      Unsigned32
}

extremeWirelessProbeInfoStatusCurrentTableSize OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the current number of entries in the probe 
         info table for this interface."
         ::= { extremeWirelessProbeInfoStatusEntry 1 }

extremeWirelessProbeInfoStatusWatermark OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the maximum size the probe info table has been
         since the statistics have been reset."
         ::= { extremeWirelessProbeInfoStatusEntry 2 }

extremeWirelessProbeInfoStatusTotalOverflows OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of times an entry in the probe info
         table was overwritten because the table was full."
         ::= { extremeWirelessProbeInfoStatusEntry 3 }

extremeWirelessProbeInfoStatusTotalTimeouts OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of times an entry in the probe info
         table was timed out."
         ::= { extremeWirelessProbeInfoStatusEntry 4 }

extremeWirelessProbeInfoStatusLastElement OBJECT-TYPE
        SYNTAX TimeTicks
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the sysUpTime the last time an entry was added
         to the probe info table (or modified)."
         ::= { extremeWirelessProbeInfoStatusEntry 5 }

extremeWirelessProbeInfoStatusTotalProbes OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of PROBE REQ packets that
         this interface has gotten."
         ::= { extremeWirelessProbeInfoStatusEntry 6 }

-- *************************************************************** --
-- Probe Info Table : This table contains information on the probe --
-- request packets recieved from particular hosts.                 --
-- *************************************************************** --
extremeWirelessProbeInfoTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessProbeInfoEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "This table contains one entry for each source MAC from which
         a PROBE REQ packet has been received.  Entries are added when
         a packet is recieved from a new source mac.  Entries are 
         removed via management action, or by timeout or overflow."
         ::= { extremeAP 30 }

extremeWirelessProbeInfoEntry OBJECT-TYPE
        SYNTAX ExtremeWirelessProbeInfoEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Note that the ifIndex here can be either a physical or virtual
         wireless interface index.  In addition, this table is indexed
         by the MAC address of the PROBE REQ source."
        INDEX { ifIndex, extremeWirelessProbeInfoSource }
         ::= { extremeWirelessProbeInfoTable 1 }

ExtremeWirelessProbeInfoEntry ::= SEQUENCE {
        extremeWirelessProbeInfoSource          MacAddress,
        extremeWirelessProbeInfoTotalProbes     Unsigned32,
        extremeWirelessProbeInfoTotalProbeResp  Unsigned32,
        extremeWirelessProbeInfoRateIESize      Unsigned32,
        extremeWirelessProbeInfoRateIE          OCTET STRING,
        extremeWirelessProbeInfoFirstSeen       TimeTicks,
        extremeWirelessProbeInfoLastChange      TimeTicks,
        extremeWirelessProbeInfoLastRSS         INTEGER,
        extremeWirelessProbeInfoLastRate        INTEGER,
        extremeWirelessProbeInfoLastChannel     INTEGER }

extremeWirelessProbeInfoSource OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the MAC address of the source which sent us the 
         PROBE REQ packets described by this entry."
         ::= { extremeWirelessProbeInfoEntry 1 }

extremeWirelessProbeInfoTotalProbes OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of PROBE REQ packets we have
         received from this source since the last time the stats
         were cleared."
         ::= { extremeWirelessProbeInfoEntry 2 }

extremeWirelessProbeInfoTotalProbeResp OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of PROBE RESP packets we have
         sent to this source.  This may not be equal to PROBE REQ
         based on rxmit, misses, etc."
         ::= { extremeWirelessProbeInfoEntry 3 }

extremeWirelessProbeInfoRateIESize OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the size of the rate-ie field in bytes.  This
         may be 0, at which point there is no rate-ie."
         ::= { extremeWirelessProbeInfoEntry 4 }

extremeWirelessProbeInfoRateIE OBJECT-TYPE
        SYNTAX OCTET STRING
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the rate IE as recieved in the last PROBE REQ
         packet.  It is encoded as a TLV exactly as it was in the
         frame.  This field may return NULL if storing of rate IE
         fields is disabled."
         ::= { extremeWirelessProbeInfoEntry 5 }

extremeWirelessProbeInfoFirstSeen OBJECT-TYPE
        SYNTAX TimeTicks
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the sysUpTime the first time a PROBE REQ was
         seen from this source."
         ::= { extremeWirelessProbeInfoEntry 6 }

extremeWirelessProbeInfoLastChange OBJECT-TYPE
        SYNTAX TimeTicks
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the sysUpTime the last time a PROBE REQ was
         seen from this source."
         ::= { extremeWirelessProbeInfoEntry 7 }

extremeWirelessProbeInfoLastRSS OBJECT-TYPE
        SYNTAX INTEGER
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the RSSI from the last PROBE REQ packet received
         from this station."
         ::= { extremeWirelessProbeInfoEntry 8 }

extremeWirelessProbeInfoLastRate OBJECT-TYPE
        SYNTAX INTEGER
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the rate at which the last packet was received
         from this station."
         ::= { extremeWirelessProbeInfoEntry 9 }

extremeWirelessProbeInfoLastChannel OBJECT-TYPE
        SYNTAX INTEGER
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the channel on which the last PROBE REQ from
         this station was heard.  PROBE REQs may be heard during
         an off-channel scan, at which point this may not be
         equal to the current channel."
         ::= { extremeWirelessProbeInfoEntry 10 }

-- *************************************************************** --
-- Per Client Historical Diagnostic Table : This table allows for  --
-- configuration of diagnostic information collection.             --
-- *************************************************************** -- 
extremeWirelessClientDiagCfgTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessClientDiagCfgEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "This table contains one row per wireless interface.  Each row
         contains configuration values for collection of per-client
         diagnostic information."
         ::= { extremeAP 31 }

extremeWirelessClientDiagCfgEntry OBJECT-TYPE
        SYNTAX ExtremeWirelessClientDiagCfgEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "There is one entry in this table per virtual interface
         (SSID)."
        INDEX { ifIndex }
         ::= { extremeWirelessClientDiagCfgTable 1 }

ExtremeWirelessClientDiagCfgEntry ::= SEQUENCE {
        extremeWirelessClientDiagCfgEnable              TruthValue,
        extremeWirelessClientDiagCfgClearClient         MacAddress,
        extremeWirelessClientDiagCfgTableSize           Unsigned32,
        extremeWirelessClientDiagCfgTimeout             Unsigned32
}

extremeWirelessClientDiagCfgEnable OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Setting this to TRUE enables the collection of historical 
         information on this virtual interface.  This implies that 
         stations which send ASSOC or AUTH packets will have new 
         entries created in the table for this interface."
         DEFVAL { true }
         ::= { extremeWirelessClientDiagCfgEntry 1 }

extremeWirelessClientDiagCfgClearClient OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Setting this to the MAC address of a client in the diag
         tables will clear the counters for that client.  The entry
         will not be removed from the table, but all summation 
         counters will be cleared."
         ::= { extremeWirelessClientDiagCfgEntry 2 }

extremeWirelessClientDiagCfgTableSize OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "This value will configure the maximum size of the diag table.
         The value is specified in number of entries.  A value of 0
         implies no upper limit."
         DEFVAL { 128 }
         ::= { extremeWirelessClientDiagCfgEntry 3 }

extremeWirelessClientDiagCfgTimeout OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "This value will configure the timeout of an entry from the
         diagnostics tables.  The value is given in seconds.  A value
         of 0 implies no timeout."
         DEFVAL { 3600 }
         ::= { extremeWirelessClientDiagCfgEntry 4 }

-- *************************************************************** --
-- Per client historical feature status                            --
-- *************************************************************** --
extremeWirelessClientDiagStatusTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessClientDiagStatusEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "This table contains one entry per virtual interface.  Values
         stored here give current status of the historical client diag
         feature."
         ::= { extremeAP 32 }

extremeWirelessClientDiagStatusEntry OBJECT-TYPE
        SYNTAX ExtremeWirelessClientDiagStatusEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Note that ifIndex here is virtual ifIndex (SSID)."
        INDEX { ifIndex }
         ::= { extremeWirelessClientDiagStatusTable 1 }

ExtremeWirelessClientDiagStatusEntry ::= SEQUENCE {
        extremeWirelessClientDiagCurrentTableSize       Unsigned32,
        extremeWirelessClientDiagTableWatermark         Unsigned32,
        extremeWirelessClientDiagTotalOverflows         Unsigned32,
        extremeWirelessClientDiagTotalTimeouts          Unsigned32,
        extremeWirelessClientDiagLastElement            TimeTicks,
        extremeWirelessClientDiagSupportsSizeCounters   TruthValue,
        extremeWirelessClientDiagSupportsSpeedCounters  TruthValue,
        extremeWirelessClientDiagSupportsPacketCounters TruthValue
}

extremeWirelessClientDiagCurrentTableSize OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the current size, in entries of the client diag
         tables."
         ::= { extremeWirelessClientDiagStatusEntry 1 }

extremeWirelessClientDiagTableWatermark OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the maximum size the client diag table has been
         since the last time the statistics were cleared."
         ::= { extremeWirelessClientDiagStatusEntry 2 }

extremeWirelessClientDiagTotalOverflows OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of times an entry has been
         replaced by a newer entry because there was no room
         left in the table."
         ::= { extremeWirelessClientDiagStatusEntry 3 }

extremeWirelessClientDiagTotalTimeouts OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of times an entry has been
         aged-out of the table."
         ::= { extremeWirelessClientDiagStatusEntry 4 }

extremeWirelessClientDiagLastElement OBJECT-TYPE
        SYNTAX TimeTicks
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is sysUpTime when the last entry was added to
         the table."
         ::= { extremeWirelessClientDiagStatusEntry 5 }

extremeWirelessClientDiagSupportsSpeedCounters OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This value indicates if this AP supports the speed-based
         counters from the extremeWirelessClientSpeedCountersTable."
         ::= { extremeWirelessClientDiagStatusEntry 6 }

extremeWirelessClientDiagSupportsSizeCounters OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This value indicates if this AP supports the size-based
         counters from the extremeWirelessClientMACSizeCounterTable."
         ::= { extremeWirelessClientDiagStatusEntry 7 }

extremeWirelessClientDiagSupportsPacketCounters OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This value indicates if this AP supports the packet-based
         counters from the extremeWirelessClientPacketCountersTable."
         ::= { extremeWirelessClientDiagStatusEntry 8 }

-- *************************************************************** --
-- Per Client Historical Diagnostics : This table contains info    --
-- about state transitions for each client.
-- *************************************************************** --
extremeWirelessClientDiagTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessClientDiagEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "This table contains information on a per-client basis.  Rows are
         indexed first by virtual interface, then by client MAC."
         ::= { extremeAP 33 }

extremeWirelessClientDiagEntry OBJECT-TYPE
        SYNTAX ExtremeWirelessClientDiagEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Note that ifIndex here is virtual ifIndex (SSID)."
        INDEX { ifIndex, extremeWirelessClientDiagMac }
         ::= { extremeWirelessClientDiagTable 1 }

ExtremeWirelessClientDiagEntry ::= SEQUENCE {
        extremeWirelessClientDiagMac                    MacAddress,
        extremeWirelessClientDiagStateWatermark         INTEGER,
        extremeWirelessClientDiagEntersInDetected       Unsigned32,
        extremeWirelessClientDiagErrorsInDetected       Unsigned32,
        extremeWirelessClientDiagAuthReqInDetected      Unsigned32,
        extremeWirelessClientDiagOtherReqInDetected     Unsigned32,
        extremeWirelessClientDiagMgmtActionInDetected   Unsigned32,
        extremeWirelessClientDiagTimeOutInDetected      Unsigned32,
        extremeWirelessClientDiagEntersInAuth           Unsigned32,
        extremeWirelessClientDiagErrorsInAuth           Unsigned32,
        extremeWirelessClientDiagAssocReqInAuth         Unsigned32,
        extremeWirelessClientDiagOtherReqInAuth         Unsigned32,
        extremeWirelessClientDiagMgmtActionInAuth       Unsigned32,
        extremeWirelessClientDiagTimeOutInAuth          Unsigned32,
        extremeWirelessClientDiagEntersInAssoc          Unsigned32,
        extremeWirelessClientDiagErrorsInAssoc          Unsigned32,
        extremeWirelessClientDiagMgmtActionInAssoc      Unsigned32,
        extremeWirelessClientDiagTimeOutInAssoc         Unsigned32,
        extremeWirelessClientDiagEntersInForward        Unsigned32,
        extremeWirelessClientDiagMgmtActionInForward    Unsigned32,
        extremeWirelessClientDiagTimeOutInForward       Unsigned32,
        extremeWirelessClientDiagTotal802Auths          Unsigned32,
        extremeWirelessClientDiagTotalNetLoginAuths     Unsigned32
}

extremeWirelessClientDiagMac OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the MAC address of the station this entry 
         describes."
         ::= { extremeWirelessClientDiagEntry 1 }

extremeWirelessClientDiagStateWatermark OBJECT-TYPE
        SYNTAX INTEGER
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the highest state this client has been in."
        ::= { extremeWirelessClientDiagEntry 2 }

extremeWirelessClientDiagEntersInDetected OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the total number of times the client has entered
         the detected state."
        ::= { extremeWirelessClientDiagEntry 3 }

extremeWirelessClientDiagErrorsInDetected OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the total number of errors this client has 
         experienced since the counters were cleared."
        ::= { extremeWirelessClientDiagEntry 4 }

extremeWirelessClientDiagAuthReqInDetected OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the total number of AUTH REQ packets received
         from this client while it was in the detected state."
        ::= { extremeWirelessClientDiagEntry 5 }

extremeWirelessClientDiagOtherReqInDetected OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the total number of REQ packets received from
         this client while it was in detected state that were
         not AUTH REQ packets."
        ::= { extremeWirelessClientDiagEntry 6 }

extremeWirelessClientDiagMgmtActionInDetected OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the total number of times management initiated
         action (i.e. force-disassociate) was received for this
         client in the detected state."
        ::= { extremeWirelessClientDiagEntry 7 }

extremeWirelessClientDiagTimeOutInDetected OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the total number of timeouts which happened to
         this client in the detected state."
        ::= { extremeWirelessClientDiagEntry 8 }

extremeWirelessClientDiagEntersInAuth OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the total number of times the client has entered
         the AUTHED state."
        ::= { extremeWirelessClientDiagEntry 9 }

extremeWirelessClientDiagErrorsInAuth OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the total number of times the client has had
         errors in the AUTHED state."
        ::= { extremeWirelessClientDiagEntry 10 }

extremeWirelessClientDiagAssocReqInAuth OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the total number of ASSOC REQ or REASSOC REQ
         packets received from this client while in the AUTHED 
         state."
        ::= { extremeWirelessClientDiagEntry 11 }

extremeWirelessClientDiagOtherReqInAuth OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the total number of non-ASSOC/REASSOC packets
         received from this client while in the AUTHED state."
        ::= { extremeWirelessClientDiagEntry 12 }

extremeWirelessClientDiagMgmtActionInAuth OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the total number of management initiated action
         which this client experienced while in the AUTHED state."
        ::= { extremeWirelessClientDiagEntry 13 }

extremeWirelessClientDiagTimeOutInAuth OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the total number of times this client timed out
         while in the authed state."
        ::= { extremeWirelessClientDiagEntry 14 }

extremeWirelessClientDiagEntersInAssoc OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the total number of times this client has entered
         the associated state."
        ::= { extremeWirelessClientDiagEntry 15 }

extremeWirelessClientDiagErrorsInAssoc OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the total number of errors this client has had
         in the associated state."
        ::= { extremeWirelessClientDiagEntry 16 }

extremeWirelessClientDiagMgmtActionInAssoc OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the total number of management actions which have
         happened to this client in the associated state."
        ::= { extremeWirelessClientDiagEntry 17 }

extremeWirelessClientDiagTimeOutInAssoc OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the total number of times this station has been
         timed-out in the associated state."
        ::= { extremeWirelessClientDiagEntry 18 }

extremeWirelessClientDiagEntersInForward OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the total number of times this client has entered
         the forwarding state."
        ::= { extremeWirelessClientDiagEntry 19 }

extremeWirelessClientDiagMgmtActionInForward OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the total number of times this client has
         experience a management action while in forwarding."
        ::= { extremeWirelessClientDiagEntry 20 }

extremeWirelessClientDiagTimeOutInForward OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the total number of timeouts this client has
         experienced while in forwarding."
        ::= { extremeWirelessClientDiagEntry 21 }

extremeWirelessClientDiagTotal802Auths OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the total number of times this client has tried
         to authenticate using 802.1x."
        ::= { extremeWirelessClientDiagEntry 22 }

extremeWirelessClientDiagTotalNetLoginAuths OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "This is the total number of times this client has tried
         to authenticate using NetLogin."
        ::= { extremeWirelessClientDiagEntry 23 }

-- *************************************************************** --
-- Per Client Association Information : This table gives history   --
-- on the association packets sent by each client on the AP.       --
-- *************************************************************** --
extremeWirelessClientAssocInfoTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessClientAssocInfoEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "This table contains one row per client on a wireless interface.
         It gives information about the association history and parameters
         of that client."
         ::= { extremeAP 34 }

extremeWirelessClientAssocInfoEntry OBJECT-TYPE
        SYNTAX ExtremeWirelessClientAssocInfoEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Note that ifIndex here is virtual ifIndex (SSID)."
        INDEX { ifIndex, extremeWirelessClientDiagMac }
         ::= { extremeWirelessClientAssocInfoTable 1 }

ExtremeWirelessClientAssocInfoEntry ::= SEQUENCE {
        extremeWirelessClientAssocInfoAssociated                TruthValue,
        extremeWirelessClientAssocInfoTotalAssocReq             Unsigned32,
        extremeWirelessClientAssocInfoTotalReAssocReq           Unsigned32,
        extremeWirelessClientAssocInfoTotalAssocResp            Unsigned32,
        extremeWirelessClientAssocInfoTotalAssocOK              Unsigned32,
        extremeWirelessClientAssocInfoTotalAssocFail            Unsigned32,
        extremeWirelessClientAssocInfoTotalDisassocReq          Unsigned32,
        extremeWirelessClientAssocInfoTotalDisassocResp         Unsigned32,
        extremeWirelessClientAssocInfoRateIE                    OCTET STRING,
        extremeWirelessClientAssocInfoLastAssoc                 TimeTicks,
        extremeWirelessClientAssocInfoLastError                 TimeTicks,
        extremeWirelessClientAssocInfoLastErrorType             INTEGER,
        extremeWirelessClientAssocInfoErrorRateMismatch         Unsigned32,
        extremeWirelessClientAssocInfoErrorBadState             Unsigned32,
        extremeWirelessClientAssocInfoErrorBadCapability        Unsigned32,
        extremeWirelessClientAssocInfoErrorCounterMeasure       Unsigned32,
        extremeWirelessClientAssocInfoErrorMcastCipher          Unsigned32,
        extremeWirelessClientAssocInfoErrorMaxAssoc             Unsigned32,
        extremeWirelessClientAssocInfoErrorRSNRequired          Unsigned32,
        extremeWirelessClientAssocInfoErrorRSNMismatch          Unsigned32,
        extremeWirelessClientAssocInfoErrorOther                Unsigned32,
        extremeWirelessClientAssocInfoWPAIEPresent              TruthValue,
        extremeWirelessClientAssocInfoWPAVersion                Unsigned32,
        extremeWirelessClientAssocInfoWPAIEMcastCipher          WPACipherSet,
        extremeWirelessClientAssocInfoWPAUcastCipherCount       Unsigned32,
        extremeWirelessClientAssocInfoWPAUcastCipher            WPACipherSet,
        extremeWirelessClientAssocInfoWPAKeyMgmtCount           Unsigned32,
        extremeWirelessClientAssocInfoWPAKeyMgmtSuite           WPAKeyMgmtSet,
        extremeWirelessClientAssocIEBlob                        OCTET STRING
}

extremeWirelessClientAssocInfoAssociated OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the current MAC-layer association status of 
         this client."
         ::= { extremeWirelessClientAssocInfoEntry 1 }

extremeWirelessClientAssocInfoTotalAssocReq OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of ASSOC REQ pdus recieved
         from this client since the last time the counters were
         cleared."
         ::= { extremeWirelessClientAssocInfoEntry 2 }

extremeWirelessClientAssocInfoTotalReAssocReq OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of REASSOC REQ PDUs received
         from this client since the last time the counters were
         cleared."
         ::= { extremeWirelessClientAssocInfoEntry 3 }

extremeWirelessClientAssocInfoTotalAssocResp OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of ASSOC RESP pdus sent to
         this client since the last time the counters were cleared."
         ::= { extremeWirelessClientAssocInfoEntry 4 }

extremeWirelessClientAssocInfoTotalAssocOK OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of ASSOC RESP PDUs which
         carried a status = ok response."
         ::= { extremeWirelessClientAssocInfoEntry 5 }

extremeWirelessClientAssocInfoTotalAssocFail OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of ASSOC RESP PDUs which
         carried a status = failed response."
         ::= { extremeWirelessClientAssocInfoEntry 6 }

extremeWirelessClientAssocInfoTotalDisassocReq OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of ASSOC RESP PDUs which
         carried a status = failed response."
         ::= { extremeWirelessClientAssocInfoEntry 7 }

extremeWirelessClientAssocInfoTotalDisassocResp OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of ASSOC RESP PDUs which
         carried a status = failed response."
         ::= { extremeWirelessClientAssocInfoEntry 8 }

extremeWirelessClientAssocInfoRateIE OBJECT-TYPE
        SYNTAX OCTET STRING
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the value of the rate IE carried in the last
         ASSOC REQ packet if this wireless interface is configured
         to keep IEs.  If it's not, this will be NULL.  The IE
         is encoded as a series of bytes exactly as the value 
         portion of the IE in the PDU."
         ::= { extremeWirelessClientAssocInfoEntry 9 }

extremeWirelessClientAssocInfoLastAssoc OBJECT-TYPE
        SYNTAX TimeTicks
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is sysUpTime when the last ASSOC REQ was received
         from this client."
         ::= { extremeWirelessClientAssocInfoEntry 10 }

extremeWirelessClientAssocInfoLastError OBJECT-TYPE
        SYNTAX TimeTicks
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is sysUpTime when the last ASSOC RESP was sent to
         this client with a failure status."
         ::= { extremeWirelessClientAssocInfoEntry 11 }

extremeWirelessClientAssocInfoLastErrorType OBJECT-TYPE
        SYNTAX INTEGER { noError(0),
                         rateMismatch(1),
                         badState(2),
                         badCapability(3),
                         couterMeasure(4),
                         mcastCipher(5),
                         maxAssoc(6),
                         rsnRequired(7),
                         rsnMismatch(8),
                         otherError(9) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is an enumerated type which indicates which was the
         last error this client experienced during association."
         ::= { extremeWirelessClientAssocInfoEntry 12 }

extremeWirelessClientAssocInfoErrorRateMismatch OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of failed associations due to 
         a mismatch of the rate IEs."
         ::= { extremeWirelessClientAssocInfoEntry 13 }

extremeWirelessClientAssocInfoErrorBadState OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of failed associations due to 
         the client being in the wrong state."
         ::= { extremeWirelessClientAssocInfoEntry 14 }

extremeWirelessClientAssocInfoErrorBadCapability OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of failed associations due to 
         the client having a capability mismatch with the AP."
         ::= { extremeWirelessClientAssocInfoEntry 15 }

extremeWirelessClientAssocInfoErrorCounterMeasure OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of failed associations due to 
         the client being subject to a counter measure."
         ::= { extremeWirelessClientAssocInfoEntry 16 }

extremeWirelessClientAssocInfoErrorMcastCipher OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of failed associations due to 
         the client not supporting the current multicast cipher."
         ::= { extremeWirelessClientAssocInfoEntry 17 }

extremeWirelessClientAssocInfoErrorMaxAssoc OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of failed associations due to 
         the AP having too many associations already."
         ::= { extremeWirelessClientAssocInfoEntry 18 }

extremeWirelessClientAssocInfoErrorRSNRequired OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of failed associations due to 
         the client not supplying the (required) RSN IE."
         ::= { extremeWirelessClientAssocInfoEntry 19 }

extremeWirelessClientAssocInfoErrorRSNMismatch OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of failed associations due to 
         the client's RSN IE not matching supported features on 
         the AP."
         ::= { extremeWirelessClientAssocInfoEntry 20 }

extremeWirelessClientAssocInfoErrorOther OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of failed associations due to 
         the client's RSN IE not matching supported features on 
         the AP."
         ::= { extremeWirelessClientAssocInfoEntry 21 }

extremeWirelessClientAssocInfoWPAIEPresent OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "If this value is true it indicates that WPA information was
         gathered from this station in the last association request.
         If true, it implies the values of the WPA variables below 
         are valid.  If false, it indicates that this station did not
         send a WPA IE in its last association."
        ::= { extremeWirelessClientAssocInfoEntry 22 }

extremeWirelessClientAssocInfoWPAVersion OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This value gives the version of WPA supported by this station.
         See IEEE 802.11i Draft 3.0 section 7 for meaning of various
         values."
        ::= { extremeWirelessClientAssocInfoEntry 23 }

extremeWirelessClientAssocInfoWPAIEMcastCipher OBJECT-TYPE
        SYNTAX WPACipherSet
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This value gives the single multicast cipher supported by this
         client."
        ::= { extremeWirelessClientAssocInfoEntry 24 }

extremeWirelessClientAssocInfoWPAUcastCipherCount OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of set bits in the ucast cipher
         variable below.  In this case this number should always
         be 1."
        ::= { extremeWirelessClientAssocInfoEntry 25 }

extremeWirelessClientAssocInfoWPAUcastCipher OBJECT-TYPE
        SYNTAX WPACipherSet
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the cipher suites which was requested by 
         this client during its last assoc req."
        ::= { extremeWirelessClientAssocInfoEntry 26 }

extremeWirelessClientAssocInfoWPAKeyMgmtCount OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This value gives the number of key management suites 
         requested by this client in the last assoc. req message.
         It indicates the number of set bits in the mgmt suite 
         variable below."
        ::= { extremeWirelessClientAssocInfoEntry 27 }

extremeWirelessClientAssocInfoWPAKeyMgmtSuite OBJECT-TYPE
        SYNTAX WPAKeyMgmtSet
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Gives the key management suite requested by this client 
         during its last association request."
        ::= { extremeWirelessClientAssocInfoEntry 28 }

extremeWirelessClientAssocIEBlob OBJECT-TYPE
        SYNTAX OCTET STRING
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the IE list sent in the association frame encoded as
         a series of TLVs."
        ::= { extremeWirelessClientAssocInfoEntry 29 }


-- *************************************************************** --
-- Authentication Information Table : This table contains infor on --
-- the MAC-layer authentication of each client which has tried to  --
-- authenticate with this AP.
-- *************************************************************** --
extremeWirelessClientAuthInfoTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessClientAuthInfoEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "This table contains one row per client on a wireless interface.
         It gives information about the authentication history and params
         of that client."
         ::= { extremeAP 35 }

extremeWirelessClientAuthInfoEntry OBJECT-TYPE
        SYNTAX ExtremeWirelessClientAuthInfoEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Note that ifIndex here is virtual ifIndex (SSID)."
        INDEX { ifIndex, extremeWirelessClientDiagMac }
         ::= { extremeWirelessClientAuthInfoTable 1 }

ExtremeWirelessClientAuthInfoEntry ::= SEQUENCE {
        extremeWirelessClientAuthInfoCurrentAuth        TruthValue,
        extremeWirelessClientAuthInfoTotalAuths         Unsigned32,
        extremeWirelessClientAuthInfoTotalAuthResp      Unsigned32,
        extremeWirelessClientAuthInfoTotalAuthsOK       Unsigned32,
        extremeWirelessClientAuthInfoTotalAuthsFailed   Unsigned32,
        extremeWirelessClientAuthInfoTotalDeauthReq     Unsigned32,
        extremeWirelessClientAuthInfoTotalDeauthResp    Unsigned32,
        extremeWirelessClientAuthInfoTotalOpen          Unsigned32,
        extremeWirelessClientAuthInfoTotalShared        Unsigned32,
        extremeWirelessClientAuthInfoLastAuth           TimeTicks,
        extremeWirelessClientAuthInfoLastAuthType       INTEGER,
        extremeWirelessClientAuthInfoLastError          TimeTicks,
        extremeWirelessClientAuthInfoLastErrorType      INTEGER,
        extremeWirelessClientAuthInfoErrorResourceFailure  Unsigned32,
        extremeWirelessClientAuthInfoErrorSequenceNum   Unsigned32,
        extremeWirelessClientAuthInfoErrorChallengeText Unsigned32,
        extremeWirelessClientAuthInfoErrorTypeMismatch  Unsigned32,
        extremeWirelessClientAuthInfoErrorKeyIndex      Unsigned32,
        extremeWirelessClientAuthInfoErrorOther         Unsigned32
}

extremeWirelessClientAuthInfoCurrentAuth OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the current MAC-layer authentication status of the
         client."
         ::= { extremeWirelessClientAuthInfoEntry 1 }

extremeWirelessClientAuthInfoTotalAuths OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of AUTH REQ packets received from 
         this client since the last time the counters were cleared."
         ::= { extremeWirelessClientAuthInfoEntry 2 }

extremeWirelessClientAuthInfoTotalAuthResp OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of AUTH RESP packets sent to
         this client since the last time the counters were cleared."
         ::= { extremeWirelessClientAuthInfoEntry 3 }

extremeWirelessClientAuthInfoTotalAuthsOK OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of AUTH RESP packets sent to
         this client which carried a STATUS = OK message."
         ::= { extremeWirelessClientAuthInfoEntry 4 }

extremeWirelessClientAuthInfoTotalAuthsFailed OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of AUTH RESP packets sent to
         this client which carried a STATUS = Failed message."
         ::= { extremeWirelessClientAuthInfoEntry 5 }

extremeWirelessClientAuthInfoTotalDeauthReq OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of DEAUTH REQ packets sent from
         this client."
         ::= { extremeWirelessClientAuthInfoEntry 6 }

extremeWirelessClientAuthInfoTotalDeauthResp OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of DEAUTH RESP packets sent to
         this client."
         ::= { extremeWirelessClientAuthInfoEntry 7 }

extremeWirelessClientAuthInfoTotalOpen OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of AUTH REQ packets which 
         requested open authentication from the AP."
         ::= { extremeWirelessClientAuthInfoEntry 8 }

extremeWirelessClientAuthInfoTotalShared OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of AUTH REQ packets which 
         requested shared authentication from the AP."
         ::= { extremeWirelessClientAuthInfoEntry 9 }

extremeWirelessClientAuthInfoLastAuth OBJECT-TYPE
        SYNTAX TimeTicks
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the sysUpTime the last time this client sent
         a request for authentication."
         ::= { extremeWirelessClientAuthInfoEntry 10 }

extremeWirelessClientAuthInfoLastAuthType OBJECT-TYPE
        SYNTAX INTEGER { open(1), shared(2) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the last type of authentication requested by 
         this client."
         ::= { extremeWirelessClientAuthInfoEntry 11 }

extremeWirelessClientAuthInfoLastError OBJECT-TYPE
        SYNTAX TimeTicks
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the sysUpTime of the last authentication failure
         for this client."
         ::= { extremeWirelessClientAuthInfoEntry 12 }

extremeWirelessClientAuthInfoLastErrorType OBJECT-TYPE
    SYNTAX INTEGER { noError(0),
        resourceFailure(1),
        sequenceNumber(2),
        challengeText(3),
        algorithmMismatch(4),
        keyIndex(5),
        otherError(6) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the OID of the last error counter that was 
         incremented for this client."
         ::= { extremeWirelessClientAuthInfoEntry 13 }

extremeWirelessClientAuthInfoErrorResourceFailure OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of authentication failures 
         which have resulted from resource failures."
         ::= { extremeWirelessClientAuthInfoEntry 14 }

extremeWirelessClientAuthInfoErrorSequenceNum OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of authentication failures 
         which have resulted from bad packet sequence numbers."
         ::= { extremeWirelessClientAuthInfoEntry 15 }

extremeWirelessClientAuthInfoErrorChallengeText OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of authentication failures 
         which have resutled from challenge text mismatch."
         ::= { extremeWirelessClientAuthInfoEntry 16 }

extremeWirelessClientAuthInfoErrorTypeMismatch OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of authentication failures 
         which have resutled from the requested authentication
         type (i.e. open/shared) not matching what this virutal
         interface is configured for."
         ::= { extremeWirelessClientAuthInfoEntry 17 }

extremeWirelessClientAuthInfoErrorKeyIndex OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of authentication failures 
         which have resulted from key index mismatches."
         ::= { extremeWirelessClientAuthInfoEntry 18 }

extremeWirelessClientAuthInfoErrorOther OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This is the total number of authentication failures 
         which have resulted from unspecified errors."
         ::= { extremeWirelessClientAuthInfoEntry 19 }


-- *************************************************************** --
-- Client MAC information : This table contains statistics and     --
-- information on each client which has tried to authenticate with --
-- this virtual interface.
-- *************************************************************** --
extremeWirelessClientMACInfoTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessClientMACInfoEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "This table contains one entry per source MAC which has tried to
         authenticate with this virtual interface (SSID).  Entries
         are created when AUTH or REATH REQ packets are received from
         new clients.  Entries can be aged out, removed by management
         action, or overwritten by an overflow."
         ::= { extremeAP 36 }

extremeWirelessClientMACInfoEntry OBJECT-TYPE
        SYNTAX ExtremeWirelessClientMACInfoEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        ""
        INDEX { ifIndex, extremeWirelessClientDiagMac }
         ::= { extremeWirelessClientMACInfoTable 1 }

ExtremeWirelessClientMACInfoEntry ::= SEQUENCE {
        extremeWirelessClientMACInfoMinRSS              INTEGER,
        extremeWirelessClientMACInfoMaxRSS              INTEGER,
        extremeWirelessClientMACInfoAvgRSS              INTEGER,
        extremeWirelessClientMACInfoTotalProbeReq       Unsigned32,
        extremeWirelessClientMACInfoTotalAuthReq        Unsigned32,
        extremeWirelessClientMACInfoTotalAssocReq       Unsigned32,
        extremeWirelessClientMACInfoTotalReAssocReq     Unsigned32,
        extremeWirelessClientMACInfoTotalDeAssocReq     Unsigned32,
        extremeWirelessClientMACInfoTotalDeAuthReq      Unsigned32,
        extremeWirelessClientMACInfoTotalPsPoll         Unsigned32,
        extremeWirelessClientMACInfoTotalData           Unsigned32,
        extremeWirelessClientMACInfoNavValue            Unsigned32
}

extremeWirelessClientMACInfoMinRSS OBJECT-TYPE
        SYNTAX INTEGER
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the minimum RSS indication of any packet we have
         seen from this client.  A value of 0 indicates that RSSI has
         been unavailable."
         ::= { extremeWirelessClientMACInfoEntry 1 }

extremeWirelessClientMACInfoMaxRSS OBJECT-TYPE
        SYNTAX INTEGER
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the maximum RSS indication of any packet we have
         seen from this client.  A value of 0 indicates that RSSI has
         been unavailable."
         ::= { extremeWirelessClientMACInfoEntry 2 }

extremeWirelessClientMACInfoAvgRSS OBJECT-TYPE
        SYNTAX INTEGER
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the average RSS indication of any packet we have
         seen from this client.  A value of 0 indicates that RSSI has
         been unavailable."
         ::= { extremeWirelessClientMACInfoEntry 3 }

extremeWirelessClientMACInfoTotalProbeReq OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of PROBE REQ packets recieved from
         this client since the counters have been cleared."
         ::= { extremeWirelessClientMACInfoEntry 4 }

extremeWirelessClientMACInfoTotalAuthReq OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of AUTH REQ packets recieved from
         this client since the counters have been cleared."
         ::= { extremeWirelessClientMACInfoEntry 5 }

extremeWirelessClientMACInfoTotalAssocReq OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of ASSOC REQ packets recieved from
         this client since the counters have been cleared."
         ::= { extremeWirelessClientMACInfoEntry 6 }

extremeWirelessClientMACInfoTotalReAssocReq OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of REASSOC REQ packets recieved from
         this client since the counters have been cleared."
         ::= { extremeWirelessClientMACInfoEntry 7 }

extremeWirelessClientMACInfoTotalDeAssocReq OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of DEASSOC REQ packets recieved from
         this client since the counters have been cleared."
         ::= { extremeWirelessClientMACInfoEntry 8 }

extremeWirelessClientMACInfoTotalDeAuthReq OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of DEAUTH REQ packets recieved from
         this client since the counters have been cleared."
         ::= { extremeWirelessClientMACInfoEntry 9 }

extremeWirelessClientMACInfoTotalPsPoll OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of PS POLL packets recieved from
         this client since the counters have been cleared."
         ::= { extremeWirelessClientMACInfoEntry 10 }

extremeWirelessClientMACInfoTotalData OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of data frames received from this
         client since the counters have been cleared."
         ::= { extremeWirelessClientMACInfoEntry 11 }

extremeWirelessClientMACInfoNavValue OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "TODO: Is this an average, total, what?"
         ::= { extremeWirelessClientMACInfoEntry 12 }


-- *************************************************************** --
-- Size Based Counters : This table gives per-client histogram     --
-- counters based on the size of received packets/fragments.       --
-- *************************************************************** --
extremeWirelessClientSizeCounterTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessClientSizeCounterEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "There is one entry in this table for each client which has
         tried to authenticate with this virtual interface.  A new 
         entry is created when an AUTH or REATH REQ packet is received
         from a new station.  Entries are removed by management action,
         timeout or overwritten due to overflow.
         
         Entries in this table are also indexed by virtual interface.
         A client which has tried to authenticate to multiple virtual   
         interfaces may have more than one entry in this table."
         ::= { extremeAP 37 }

extremeWirelessClientSizeCounterEntry OBJECT-TYPE
        SYNTAX ExtremeWirelessClientSizeCounterEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        ""
        INDEX { ifIndex, extremeWirelessClientDiagMac }
         ::= { extremeWirelessClientSizeCounterTable 1 }

ExtremeWirelessClientSizeCounterEntry ::= SEQUENCE {
        extremeWirelessClientFrameSizeReXmit64          Unsigned32,
        extremeWirelessClientFrameSizeReXmit128         Unsigned32,
        extremeWirelessClientFrameSizeReXmit256         Unsigned32,
        extremeWirelessClientFrameSizeReXmit512         Unsigned32,
        extremeWirelessClientFrameSizeReXmit1024        Unsigned32,
        extremeWirelessClientFrameSizeReXmit2048        Unsigned32,
        extremeWirelessClientFrameSizeTX64              Unsigned32,
        extremeWirelessClientFrameSizeTX128             Unsigned32,
        extremeWirelessClientFrameSizeTX256             Unsigned32,
        extremeWirelessClientFrameSizeTX512             Unsigned32,
        extremeWirelessClientFrameSizeTX1024            Unsigned32,
        extremeWirelessClientFrameSizeTX2048            Unsigned32,
        extremeWirelessClientFrameSizeRX64              Unsigned32,
        extremeWirelessClientFrameSizeRX128             Unsigned32,
        extremeWirelessClientFrameSizeRX256             Unsigned32,
        extremeWirelessClientFrameSizeRX512             Unsigned32,
        extremeWirelessClientFrameSizeRX1024            Unsigned32,
        extremeWirelessClientFrameSizeRX2048            Unsigned32,
        extremeWirelessClientFrameSizeErrorTX64         Unsigned32,
        extremeWirelessClientFrameSizeErrorTX128        Unsigned32,
        extremeWirelessClientFrameSizeErrorTX256        Unsigned32,
        extremeWirelessClientFrameSizeErrorTX512        Unsigned32,
        extremeWirelessClientFrameSizeErrorTX1024       Unsigned32,
        extremeWirelessClientFrameSizeErrorTX2048       Unsigned32,
        extremeWirelessClientFrameSizeErrorRX64         Unsigned32,
        extremeWirelessClientFrameSizeErrorRX128        Unsigned32,
        extremeWirelessClientFrameSizeErrorRX256        Unsigned32,
        extremeWirelessClientFrameSizeErrorRX512        Unsigned32,
        extremeWirelessClientFrameSizeErrorRX1024       Unsigned32,
        extremeWirelessClientFrameSizeErrorRX2048       Unsigned32,
        extremeWirelessClientPacketSizeTX64             Unsigned32,
        extremeWirelessClientPacketSizeTX128            Unsigned32,
        extremeWirelessClientPacketSizeTX256            Unsigned32,
        extremeWirelessClientPacketSizeTX512            Unsigned32,
        extremeWirelessClientPacketSizeTX1024           Unsigned32,
        extremeWirelessClientPacketSizeTX2048           Unsigned32,
        extremeWirelessClientPacketSizeRX64             Unsigned32,
        extremeWirelessClientPacketSizeRX128            Unsigned32,
        extremeWirelessClientPacketSizeRX256            Unsigned32,
        extremeWirelessClientPacketSizeRX512            Unsigned32,
        extremeWirelessClientPacketSizeRX1024           Unsigned32,
        extremeWirelessClientPacketSizeRX2048           Unsigned32
}

extremeWirelessClientFrameSizeReXmit64 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags retransmitted to this
         client which were less than or equal to 64 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 1 }

extremeWirelessClientFrameSizeReXmit128 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags retransmitted to this
         client which were between 64 and 128 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 2 }

extremeWirelessClientFrameSizeReXmit256 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags retransmitted to this
         client which were between 128 and 256 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 3 }

extremeWirelessClientFrameSizeReXmit512 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags retransmitted to this
         client which were between 256 and 512 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 4 }

extremeWirelessClientFrameSizeReXmit1024 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags retransmitted to this
         client which were between 512 and 1024 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 5 }

extremeWirelessClientFrameSizeReXmit2048 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags retransmitted to this
         client which were between 1024 and 2048 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 6 }

extremeWirelessClientFrameSizeTX64 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags transmitted to this
         client which were less than or equal to 64 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 7 }

extremeWirelessClientFrameSizeTX128 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags transmitted to this
         client which were between 64 and 128 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 8 }

extremeWirelessClientFrameSizeTX256 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags transmitted to this
         client which were between 128 and 256 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 9 }

extremeWirelessClientFrameSizeTX512 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags transmitted to this
         client which were between 256 and 512 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 10 }

extremeWirelessClientFrameSizeTX1024 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags transmitted to this
         client which were between 512 and 1024 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 11 }

extremeWirelessClientFrameSizeTX2048 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags transmitted to this
         client which were between 1024 and 2048 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 12 }

extremeWirelessClientFrameSizeRX64 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags received from this
         client which were less than or equal to 64 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 13 }

extremeWirelessClientFrameSizeRX128 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags received from this
         client which were between 64 and 128 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 14 }

extremeWirelessClientFrameSizeRX256 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags received from this
         client which were between 128 and 256 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 15 }

extremeWirelessClientFrameSizeRX512 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags received from this
         client which were between 256 and 512 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 16 }

extremeWirelessClientFrameSizeRX1024 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags received from this
         client which were between 512 and 1024 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 17 }

extremeWirelessClientFrameSizeRX2048 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags received from this
         client which were between 1024 and 2048 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 18 }

extremeWirelessClientFrameSizeErrorTX64 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which failed to be sent from
         this client with a length between 0 and 64 bytes."
         ::= { extremeWirelessClientSizeCounterEntry 19 }

extremeWirelessClientFrameSizeErrorTX128 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which failed to be sent from
         this client with a length between 65 and 128 bytes."
         ::= { extremeWirelessClientSizeCounterEntry 20 }

extremeWirelessClientFrameSizeErrorTX256 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which failed to be sent from
         this client with a length between 129 and 256 bytes."
         ::= { extremeWirelessClientSizeCounterEntry 21 }

extremeWirelessClientFrameSizeErrorTX512 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which failed to be sent from
         this client with a length between 257 and 512 bytes."
         ::= { extremeWirelessClientSizeCounterEntry 22 }

extremeWirelessClientFrameSizeErrorTX1024 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which failed to be sent from
         this client with a length between 513 and 1024 bytes."
         ::= { extremeWirelessClientSizeCounterEntry 23 }

extremeWirelessClientFrameSizeErrorTX2048 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which failed to be sent from
         this client with a length between 1025 and 2048 bytes."
         ::= { extremeWirelessClientSizeCounterEntry 24 }

extremeWirelessClientFrameSizeErrorRX64 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were received with
         an FCS or other error and a length between 0 and 64 bytes."
         ::= { extremeWirelessClientSizeCounterEntry 25 }

extremeWirelessClientFrameSizeErrorRX128 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were received with
         an FCS or other error and a length between 65 and 128 bytes."
         ::= { extremeWirelessClientSizeCounterEntry 26 }

extremeWirelessClientFrameSizeErrorRX256 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were received with
         an FCS or other error and a length between 129 and 256 bytes."
         ::= { extremeWirelessClientSizeCounterEntry 27 }

extremeWirelessClientFrameSizeErrorRX512 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were received with
         an FCS or other error and a length between 257 and 512 bytes."
         ::= { extremeWirelessClientSizeCounterEntry 28 }

extremeWirelessClientFrameSizeErrorRX1024 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were received with
         an FCS or other error and a length between 513 and 1024 bytes."
         ::= { extremeWirelessClientSizeCounterEntry 29 }

extremeWirelessClientFrameSizeErrorRX2048 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were received with
         an FCS or other error and a length between 1025 and 2048 bytes."
         ::= { extremeWirelessClientSizeCounterEntry 30 }

extremeWirelessClientPacketSizeTX64 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of packets transmitted to this
         client which were less than or equal to 64 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 31 }

extremeWirelessClientPacketSizeTX128 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of packets transmitted to this
         client which were between 64 and 128 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 32 }

extremeWirelessClientPacketSizeTX256 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of packets transmitted to this
         client which were between 128 and 256 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 33 }

extremeWirelessClientPacketSizeTX512 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of packets transmitted to this
         client which were between 256 and 512 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 34 }

extremeWirelessClientPacketSizeTX1024 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of packets transmitted to this
         client which were between 512 and 1024 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 35 }

extremeWirelessClientPacketSizeTX2048 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of packets transmitted to this
         client which were between 1024 and 2048 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 36 }

extremeWirelessClientPacketSizeRX64 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of packets received from this
         client which were less than or equal to 64 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 37 }

extremeWirelessClientPacketSizeRX128 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of packets received from this
         client which were between 64 and 128 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 38 }

extremeWirelessClientPacketSizeRX256 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of packets received from this
         client which were between 128 and 256 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 39 }

extremeWirelessClientPacketSizeRX512 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of packets received from this
         client which were between 256 and 512 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 40 }

extremeWirelessClientPacketSizeRX1024 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of packets received from this
         client which were between 512 and 1024 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 41 }

extremeWirelessClientPacketSizeRX2048 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of packets received from this
         client which were between 1024 and 2048 bytes in length."
         ::= { extremeWirelessClientSizeCounterEntry 42 }

-- *************************************************************** --
-- Per Client Speed : This table gives a histogram of statistics   --
-- based on the speed of transmission/reception of packets on a    --
-- virtual interface.                                              --
-- *************************************************************** --
extremeWirelessClientSpeedCounterTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessClientSpeedCounterEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "This table is indexed by wireless interface index.  These
         are the virtual interfaces corresponding to the SSID.  Support
         for this table is optional, indicated by the value of the variable
         extremeWirelessClientDiagSupportsSpeedCounters in the status table."
         ::= { extremeAP 38 }

extremeWirelessClientSpeedCounterEntry OBJECT-TYPE
        SYNTAX ExtremeWirelessClientSpeedCounterEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The ifIndex here is the wireless interface (SSID).  It is expected
         that an entry will be created in this table only after a client
         sends a AUTH or REATH packet to the SSID."
        INDEX { ifIndex, extremeWirelessClientDiagMac }
         ::= { extremeWirelessClientSpeedCounterTable 1 }

ExtremeWirelessClientSpeedCounterEntry ::= SEQUENCE {
        extremeWirelessClientSpeedReXmit1       Unsigned32,
        extremeWirelessClientSpeedReXmit2       Unsigned32,
        extremeWirelessClientSpeedReXmit5p5     Unsigned32,
        extremeWirelessClientSpeedReXmit6       Unsigned32,
        extremeWirelessClientSpeedReXmit9       Unsigned32,
        extremeWirelessClientSpeedReXmit12      Unsigned32,
        extremeWirelessClientSpeedReXmit18      Unsigned32,
        extremeWirelessClientSpeedReXmit24      Unsigned32,
        extremeWirelessClientSpeedReXmit36      Unsigned32,
        extremeWirelessClientSpeedReXmit48      Unsigned32,
        extremeWirelessClientSpeedReXmit54      Unsigned32,
        extremeWirelessClientSpeedTX1           Unsigned32,
        extremeWirelessClientSpeedTX2           Unsigned32,
        extremeWirelessClientSpeedTX5p5         Unsigned32,
        extremeWirelessClientSpeedTX6           Unsigned32,
        extremeWirelessClientSpeedTX9           Unsigned32,
        extremeWirelessClientSpeedTX12          Unsigned32,
        extremeWirelessClientSpeedTX18          Unsigned32,
        extremeWirelessClientSpeedTX24          Unsigned32,
        extremeWirelessClientSpeedTX36          Unsigned32,
        extremeWirelessClientSpeedTX48          Unsigned32,
        extremeWirelessClientSpeedTX54          Unsigned32,
        extremeWirelessClientSpeedRX1           Unsigned32,
        extremeWirelessClientSpeedRX2           Unsigned32,
        extremeWirelessClientSpeedRX5p5         Unsigned32,
        extremeWirelessClientSpeedRX6           Unsigned32,
        extremeWirelessClientSpeedRX9           Unsigned32,
        extremeWirelessClientSpeedRX12          Unsigned32,
        extremeWirelessClientSpeedRX18          Unsigned32,
        extremeWirelessClientSpeedRX24          Unsigned32,
        extremeWirelessClientSpeedRX36          Unsigned32,
        extremeWirelessClientSpeedRX48          Unsigned32,
        extremeWirelessClientSpeedRX54          Unsigned32
}

extremeWirelessClientSpeedReXmit1       OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were retransmitted to
         the given client at 1 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 1 }

extremeWirelessClientSpeedReXmit2       OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were retransmitted to
         the given client at 2 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 2 }

extremeWirelessClientSpeedReXmit5p5 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were retransmitted to
         the given client at 5 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 3 }

extremeWirelessClientSpeedReXmit6 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were retransmitted to
         the given client at 6 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 4 }

extremeWirelessClientSpeedReXmit9 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were retransmitted to
         the given client at 9 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 5 }

extremeWirelessClientSpeedReXmit12 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were retransmitted to
         the given client at 12 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 6 }

extremeWirelessClientSpeedReXmit18 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were retransmitted to
         the given client at 18 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 7 }

extremeWirelessClientSpeedReXmit24 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were retransmitted to
         the given client at 24 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 8 }
        
extremeWirelessClientSpeedReXmit36 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were retransmitted to
         the given client at 36 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 9 }

extremeWirelessClientSpeedReXmit48 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were retransmitted to
         the given client at 48 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 10 }

extremeWirelessClientSpeedReXmit54 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were retransmitted to
         the given client at 54 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 11 }

extremeWirelessClientSpeedTX1   OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were transmitted to
         the given client at 1 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 12 }

extremeWirelessClientSpeedTX2   OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were transmitted to
         the given client at 2 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 13 }

extremeWirelessClientSpeedTX5p5 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were transmitted to
         the given client at 5 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 14 }

extremeWirelessClientSpeedTX6 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were transmitted to
         the given client at 6 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 15 }

extremeWirelessClientSpeedTX9 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were transmitted to
         the given client at 9 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 16 }

extremeWirelessClientSpeedTX12 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were transmitted to
         the given client at 12 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 17 }

extremeWirelessClientSpeedTX18 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were transmitted to
         the given client at 18 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 18 }

extremeWirelessClientSpeedTX24 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were transmitted to
         the given client at 24 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 19 }
        
extremeWirelessClientSpeedTX36 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were transmitted to
         the given client at 36 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 20 }

extremeWirelessClientSpeedTX48 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were transmitted to
         the given client at 48 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 21 }

extremeWirelessClientSpeedTX54 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were transmitted to
         the given client at 54 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 22 }

extremeWirelessClientSpeedRX1   OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were received from
         the given client at 1 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 23 }

extremeWirelessClientSpeedRX2   OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were received from
         the given client at 2 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 24 }

extremeWirelessClientSpeedRX5p5 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were received from
         the given client at 5 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 25 }

extremeWirelessClientSpeedRX6 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were received from
         the given client at 6 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 26 }

extremeWirelessClientSpeedRX9 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were received from
         the given client at 9 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 27 }

extremeWirelessClientSpeedRX12 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were received from
         the given client at 12 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 28 }

extremeWirelessClientSpeedRX18 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were received from
         the given client at 18 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 29 }

extremeWirelessClientSpeedRX24 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were received from
         the given client at 24 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 30 }
        
extremeWirelessClientSpeedRX36 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were received from
         the given client at 36 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 31 }

extremeWirelessClientSpeedRX48 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were received from
         the given client at 48 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 32 }

extremeWirelessClientSpeedRX54 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frags which were received from
         the given client at 54 Mbps."
        ::= { extremeWirelessClientSpeedCounterEntry 33 }

-- *************************************************************** --
-- Frame Size Table : This table presents a historgram of frames   --
--                    based on type and size.                      --
-- *************************************************************** --
extremeWirelessIntfFrameSizeTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessIntfFrameSizeEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "There is one entry in this table for each virtual and
         physical interface.  Values for physical interfaces are
         summations of the values for the constituent virtual 
         interfaces."
         ::= { extremeAP 39 }

extremeWirelessIntfFrameSizeEntry OBJECT-TYPE
        SYNTAX ExtremeWirelessIntfFrameSizeEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        ""
        INDEX { ifIndex }
         ::= { extremeWirelessIntfFrameSizeTable 1 }
ExtremeWirelessIntfFrameSizeEntry ::= SEQUENCE {
        extremeWirelessIntfFrameSizeMgmtTX64    Unsigned32,
        extremeWirelessIntfFrameSizeMgmtTX128   Unsigned32,
        extremeWirelessIntfFrameSizeMgmtTX256   Unsigned32,
        extremeWirelessIntfFrameSizeMgmtTX512   Unsigned32,
        extremeWirelessIntfFrameSizeMgmtTX1024  Unsigned32,
        extremeWirelessIntfFrameSizeMgmtTX2048  Unsigned32,
        extremeWirelessIntfFrameSizeMgmtRX64    Unsigned32,
        extremeWirelessIntfFrameSizeMgmtRX128   Unsigned32,
        extremeWirelessIntfFrameSizeMgmtRX256   Unsigned32,
        extremeWirelessIntfFrameSizeMgmtRX512   Unsigned32,
        extremeWirelessIntfFrameSizeMgmtRX1024  Unsigned32,
        extremeWirelessIntfFrameSizeMgmtRX2048  Unsigned32,
        extremeWirelessIntfFrameSizeCtlTX64     Unsigned32,
        extremeWirelessIntfFrameSizeCtlTX128    Unsigned32,
        extremeWirelessIntfFrameSizeCtlTX256    Unsigned32,
        extremeWirelessIntfFrameSizeCtlTX512    Unsigned32,
        extremeWirelessIntfFrameSizeCtlTX1024   Unsigned32,
        extremeWirelessIntfFrameSizeCtlTX2048   Unsigned32,
        extremeWirelessIntfFrameSizeCtlRX64     Unsigned32,
        extremeWirelessIntfFrameSizeCtlRX128    Unsigned32,
        extremeWirelessIntfFrameSizeCtlRX256    Unsigned32,
        extremeWirelessIntfFrameSizeCtlRX512    Unsigned32,
        extremeWirelessIntfFrameSizeCtlRX1024   Unsigned32,
        extremeWirelessIntfFrameSizeCtlRX2048   Unsigned32,
        extremeWirelessIntfFrameSizeDataTX64    Unsigned32,
        extremeWirelessIntfFrameSizeDataTX128   Unsigned32,
        extremeWirelessIntfFrameSizeDataTX256   Unsigned32,
        extremeWirelessIntfFrameSizeDataTX512   Unsigned32,
        extremeWirelessIntfFrameSizeDataTX1024  Unsigned32,
        extremeWirelessIntfFrameSizeDataTX2048  Unsigned32,
        extremeWirelessIntfFrameSizeDataRX64    Unsigned32,
        extremeWirelessIntfFrameSizeDataRX128   Unsigned32,
        extremeWirelessIntfFrameSizeDataRX256   Unsigned32,
        extremeWirelessIntfFrameSizeDataRX512   Unsigned32,
        extremeWirelessIntfFrameSizeDataRX1024  Unsigned32,
        extremeWirelessIntfFrameSizeDataRX2048  Unsigned32 }

extremeWirelessIntfFrameSizeMgmtTX64 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of management-type frames transmitted 
         on this interface which were less than or equal to 64 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 1 }

extremeWirelessIntfFrameSizeMgmtTX128 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of management-type frames transmitted 
         on this interface which were between 65 and 128 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 2 }

extremeWirelessIntfFrameSizeMgmtTX256 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of management-type frames transmitted 
         on this interface which were between 129 and 256 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 3 }

extremeWirelessIntfFrameSizeMgmtTX512 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of management-type frames transmitted 
         on this interface which were between 257 and 512 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 4 }

extremeWirelessIntfFrameSizeMgmtTX1024 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of management-type frames transmitted 
         on this interface which were between 513 and 1024 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 5 }

extremeWirelessIntfFrameSizeMgmtTX2048 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of management-type frames transmitted 
         on this interface which were between 1025 and 2048 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 6 }

extremeWirelessIntfFrameSizeMgmtRX64 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of management-type frames received 
         on this interface which were less than or equal to 64 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 7 }

extremeWirelessIntfFrameSizeMgmtRX128 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of management-type frames received 
         on this interface which were between 65 and 128 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 8 }

extremeWirelessIntfFrameSizeMgmtRX256 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of management-type frames received 
         on this interface which were between 129 and 256 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 9 }

extremeWirelessIntfFrameSizeMgmtRX512 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of management-type frames received 
         on this interface which were between 257 and 512 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 10 }

extremeWirelessIntfFrameSizeMgmtRX1024 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of management-type frames received 
         on this interface which were between 513 and 1024 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 11 }

extremeWirelessIntfFrameSizeMgmtRX2048 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of management-type frames received 
         on this interface which were between 1025 and 2048 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 12 }

extremeWirelessIntfFrameSizeCtlTX64 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of control-type frames transmitted 
         on this interface which were less than or equal to 64 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 13 }

extremeWirelessIntfFrameSizeCtlTX128 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of control-type frames transmitted 
         on this interface which were between 65 and 128 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 14 }

extremeWirelessIntfFrameSizeCtlTX256 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of control-type frames transmitted 
         on this interface which were between 129 and 256 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 15 }

extremeWirelessIntfFrameSizeCtlTX512 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of control-type frames transmitted 
         on this interface which were between 257 and 512 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 16 }

extremeWirelessIntfFrameSizeCtlTX1024 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of control-type frames transmitted 
         on this interface which were between 513 and 1024 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 17 }

extremeWirelessIntfFrameSizeCtlTX2048 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of control-type frames transmitted 
         on this interface which were between 1025 and 2048 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 18 }

extremeWirelessIntfFrameSizeCtlRX64 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of control-type frames received 
         on this interface which were less than or equal to 64 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 19 }

extremeWirelessIntfFrameSizeCtlRX128 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of control-type frames received 
         on this interface which were between 65 and 128 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 20 }

extremeWirelessIntfFrameSizeCtlRX256 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of control-type frames received 
         on this interface which were between 129 and 256 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 21 }

extremeWirelessIntfFrameSizeCtlRX512 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of control-type frames received 
         on this interface which were between 257 and 512 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 22 }

extremeWirelessIntfFrameSizeCtlRX1024 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of control-type frames received 
         on this interface which were between 513 and 1024 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 23 }

extremeWirelessIntfFrameSizeCtlRX2048 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of control-type frames received 
         on this interface which were between 1025 and 2048 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 24 }

extremeWirelessIntfFrameSizeDataTX64 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of data-type frames transmitted 
         on this interface which were less than or equal to 64 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 25 }

extremeWirelessIntfFrameSizeDataTX128 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of data-type frames transmitted 
         on this interface which were between 65 and 128 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 26 }

extremeWirelessIntfFrameSizeDataTX256 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of data-type frames transmitted 
         on this interface which were between 129 and 256 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 27 }

extremeWirelessIntfFrameSizeDataTX512 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of data-type frames transmitted 
         on this interface which were between 257 and 512 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 28 }

extremeWirelessIntfFrameSizeDataTX1024 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of data-type frames transmitted 
         on this interface which were between 513 and 1024 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 29 }

extremeWirelessIntfFrameSizeDataTX2048 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of data-type frames transmitted 
         on this interface which were between 1025 and 2048 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 30 }

extremeWirelessIntfFrameSizeDataRX64 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of data-type frames received 
         on this interface which were less than or equal to 64 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 31 }

extremeWirelessIntfFrameSizeDataRX128 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of data-type frames received 
         on this interface which were between 65 and 128 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 32 }

extremeWirelessIntfFrameSizeDataRX256 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of data-type frames received 
         on this interface which were between 129 and 256 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 33 }

extremeWirelessIntfFrameSizeDataRX512 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of data-type frames received 
         on this interface which were between 257 and 512 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 34 }

extremeWirelessIntfFrameSizeDataRX1024 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of data-type frames received 
         on this interface which were between 513 and 1024 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 35 }

extremeWirelessIntfFrameSizeDataRX2048 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of data-type frames received 
         on this interface which were between 1025 and 2048 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeEntry 36 }

-- *************************************************************** --
-- Frame errors by size.                                           --
-- *************************************************************** --
extremeWirelessIntfFrameSizeErrorTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessIntfFrameSizeErrorEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "There is one entry in this table for each virtual and
         physical interface.  Values for physical interfaces are
         summations of the values for the constituent virtual 
         interfaces."
         ::= { extremeAP 40 }

extremeWirelessIntfFrameSizeErrorEntry OBJECT-TYPE
        SYNTAX ExtremeWirelessIntfFrameSizeErrorEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        ""
        INDEX { ifIndex }
         ::= { extremeWirelessIntfFrameSizeErrorTable 1 }


ExtremeWirelessIntfFrameSizeErrorEntry ::= SEQUENCE {
        extremeWirelessIntfFrameSizeReXmit64    Unsigned32,
        extremeWirelessIntfFrameSizeReXmit128   Unsigned32,
        extremeWirelessIntfFrameSizeReXmit256   Unsigned32,
        extremeWirelessIntfFrameSizeReXmit512   Unsigned32,
        extremeWirelessIntfFrameSizeReXmit1024  Unsigned32,
        extremeWirelessIntfFrameSizeReXmit2048  Unsigned32,
        extremeWirelessIntfFrameSizeErrorTX64   Unsigned32,
        extremeWirelessIntfFrameSizeErrorTX128  Unsigned32,
        extremeWirelessIntfFrameSizeErrorTX256  Unsigned32,
        extremeWirelessIntfFrameSizeErrorTX512  Unsigned32,
        extremeWirelessIntfFrameSizeErrorTX1024 Unsigned32,
        extremeWirelessIntfFrameSizeErrorTX2048 Unsigned32,
        extremeWirelessIntfFrameSizeErrorRX64   Unsigned32,
        extremeWirelessIntfFrameSizeErrorRX128  Unsigned32,
        extremeWirelessIntfFrameSizeErrorRX256  Unsigned32,
        extremeWirelessIntfFrameSizeErrorRX512  Unsigned32,
        extremeWirelessIntfFrameSizeErrorRX1024 Unsigned32,
        extremeWirelessIntfFrameSizeErrorRX2048 Unsigned32 }

extremeWirelessIntfFrameSizeReXmit64 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames retransmitted on this 
         interface which were less than or equal to 64 bytes
         in length."
         ::= { extremeWirelessIntfFrameSizeErrorEntry 1 }

extremeWirelessIntfFrameSizeReXmit128 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames retransmitted on this 
         interface which were between 65 and 128 bytes in length."
         ::= { extremeWirelessIntfFrameSizeErrorEntry 2 }

extremeWirelessIntfFrameSizeReXmit256 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames retransmitted on this 
         interface which were between 129 and 256 bytes in length."
         ::= { extremeWirelessIntfFrameSizeErrorEntry 3 }

extremeWirelessIntfFrameSizeReXmit512 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames retransmitted on this 
         interface which were between 257 and 512 bytes in length."
         ::= { extremeWirelessIntfFrameSizeErrorEntry 4 }

extremeWirelessIntfFrameSizeReXmit1024 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames retransmitted on this 
         interface which were between 513 and 1024 bytes in length."
         ::= { extremeWirelessIntfFrameSizeErrorEntry 5 }

extremeWirelessIntfFrameSizeReXmit2048 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames retransmitted on this 
         interface which were between 1025 and 2048 bytes in length."
         ::= { extremeWirelessIntfFrameSizeErrorEntry 6 }

extremeWirelessIntfFrameSizeErrorTX64 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which failed to be 
         transmitted interface which were less than or equal 
         to 64 bytes in length."
         ::= { extremeWirelessIntfFrameSizeErrorEntry 7 }

extremeWirelessIntfFrameSizeErrorTX128 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which failed to be 
         transmitted interface which were between 65 and 128
         bytes in length."
         ::= { extremeWirelessIntfFrameSizeErrorEntry 8 }

extremeWirelessIntfFrameSizeErrorTX256 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which failed to be 
         transmitted interface which were between 129 and 256
         bytes in length."
         ::= { extremeWirelessIntfFrameSizeErrorEntry 9 }

extremeWirelessIntfFrameSizeErrorTX512 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which failed to be 
         transmitted interface which were between 257 and 512
         bytes in length."
         ::= { extremeWirelessIntfFrameSizeErrorEntry 10 }

extremeWirelessIntfFrameSizeErrorTX1024 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which failed to be 
         transmitted interface which were between 513 and 1024
         bytes in length."
         ::= { extremeWirelessIntfFrameSizeErrorEntry 11 }

extremeWirelessIntfFrameSizeErrorTX2048 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which failed to be 
         transmitted interface which were between 1025 and 2048
         bytes in length."
         ::= { extremeWirelessIntfFrameSizeErrorEntry 12 }

extremeWirelessIntfFrameSizeErrorRX64 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which had errors on
         receive on this interface which were less than or equal 
         to 64 bytes in length."
         ::= { extremeWirelessIntfFrameSizeErrorEntry 13 }

extremeWirelessIntfFrameSizeErrorRX128 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which had errors on
         receive on this interface which were between 65 and
         128 bytes in length."
         ::= { extremeWirelessIntfFrameSizeErrorEntry 14 }

extremeWirelessIntfFrameSizeErrorRX256 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which had errors on
         receive on this interface which were between 129 and
         256 bytes in length."
         ::= { extremeWirelessIntfFrameSizeErrorEntry 15 }

extremeWirelessIntfFrameSizeErrorRX512 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which had errors on
         receive on this interface which were between 257 and
         512 bytes in length."
         ::= { extremeWirelessIntfFrameSizeErrorEntry 16 }

extremeWirelessIntfFrameSizeErrorRX1024 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which had errors on
         receive on this interface which were between 513 and
         1024 bytes in length."
         ::= { extremeWirelessIntfFrameSizeErrorEntry 17 }

extremeWirelessIntfFrameSizeErrorRX2048 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which had errors on
         receive on this interface which were between 1025 and
         2048 bytes in length."
         ::= { extremeWirelessIntfFrameSizeErrorEntry 18 }

-- *************************************************************** --
-- TX/RX Histogram based on speed.
-- *************************************************************** --
extremeWirelessIntfFrameSpeedTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessIntfFrameSpeedEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "There is one entry in this table for each virtual and
         physical interface.  Values for physical interfaces are
         summations of the values for the constituent virtual 
         interfaces."
         ::= { extremeAP 41 }

extremeWirelessIntfFrameSpeedEntry OBJECT-TYPE
        SYNTAX ExtremeWirelessIntfFrameSpeedEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        ""
        INDEX { ifIndex }
         ::= { extremeWirelessIntfFrameSpeedTable 1 }

ExtremeWirelessIntfFrameSpeedEntry ::= SEQUENCE {
        extremeWirelessIntfSpeedMgmtTX1         Unsigned32,
        extremeWirelessIntfSpeedMgmtTX2         Unsigned32,
        extremeWirelessIntfSpeedMgmtTX5p5       Unsigned32,
        extremeWirelessIntfSpeedMgmtTX6         Unsigned32,
        extremeWirelessIntfSpeedMgmtTX9         Unsigned32,
    extremeWirelessIntfSpeedMgmtTX11    Unsigned32,
        extremeWirelessIntfSpeedMgmtTX12        Unsigned32,
        extremeWirelessIntfSpeedMgmtTX18        Unsigned32,
        extremeWirelessIntfSpeedMgmtTX24        Unsigned32,
        extremeWirelessIntfSpeedMgmtTX36        Unsigned32,
        extremeWirelessIntfSpeedMgmtTX48        Unsigned32,
        extremeWirelessIntfSpeedMgmtTX54        Unsigned32,
        extremeWirelessIntfSpeedMgmtRX1         Unsigned32,
        extremeWirelessIntfSpeedMgmtRX2         Unsigned32,
        extremeWirelessIntfSpeedMgmtRX5p5       Unsigned32,
        extremeWirelessIntfSpeedMgmtRX6         Unsigned32,
        extremeWirelessIntfSpeedMgmtRX9         Unsigned32,
        extremeWirelessIntfSpeedMgmtRX11        Unsigned32,
        extremeWirelessIntfSpeedMgmtRX12        Unsigned32,
        extremeWirelessIntfSpeedMgmtRX18        Unsigned32,
        extremeWirelessIntfSpeedMgmtRX24        Unsigned32,
        extremeWirelessIntfSpeedMgmtRX36        Unsigned32,
        extremeWirelessIntfSpeedMgmtRX48        Unsigned32,
        extremeWirelessIntfSpeedMgmtRX54        Unsigned32,
        extremeWirelessIntfSpeedCtlTX1          Unsigned32,
        extremeWirelessIntfSpeedCtlTX2          Unsigned32,
        extremeWirelessIntfSpeedCtlTX5p5        Unsigned32,
        extremeWirelessIntfSpeedCtlTX6          Unsigned32,
        extremeWirelessIntfSpeedCtlTX9          Unsigned32,
    extremeWirelessIntfSpeedCtlTX11     Unsigned32,
        extremeWirelessIntfSpeedCtlTX12         Unsigned32,
        extremeWirelessIntfSpeedCtlTX18         Unsigned32,
        extremeWirelessIntfSpeedCtlTX24         Unsigned32,
        extremeWirelessIntfSpeedCtlTX36         Unsigned32,
        extremeWirelessIntfSpeedCtlTX48         Unsigned32,
        extremeWirelessIntfSpeedCtlTX54         Unsigned32,
        extremeWirelessIntfSpeedCtlRX1          Unsigned32,
        extremeWirelessIntfSpeedCtlRX2          Unsigned32,
        extremeWirelessIntfSpeedCtlRX5p5        Unsigned32,
        extremeWirelessIntfSpeedCtlRX6          Unsigned32,
        extremeWirelessIntfSpeedCtlRX9          Unsigned32,
    extremeWirelessIntfSpeedCtlRX11     Unsigned32,
        extremeWirelessIntfSpeedCtlRX12         Unsigned32,
        extremeWirelessIntfSpeedCtlRX18         Unsigned32,
        extremeWirelessIntfSpeedCtlRX24         Unsigned32,
        extremeWirelessIntfSpeedCtlRX36         Unsigned32,
        extremeWirelessIntfSpeedCtlRX48         Unsigned32,
        extremeWirelessIntfSpeedCtlRX54         Unsigned32,
        extremeWirelessIntfSpeedDataTX1         Unsigned32,
        extremeWirelessIntfSpeedDataTX2         Unsigned32,
        extremeWirelessIntfSpeedDataTX5p5       Unsigned32,
        extremeWirelessIntfSpeedDataTX6         Unsigned32,
        extremeWirelessIntfSpeedDataTX9         Unsigned32,
    extremeWirelessIntfSpeedDataTX11    Unsigned32,
        extremeWirelessIntfSpeedDataTX12        Unsigned32,
        extremeWirelessIntfSpeedDataTX18        Unsigned32,
        extremeWirelessIntfSpeedDataTX24        Unsigned32,
        extremeWirelessIntfSpeedDataTX36        Unsigned32,
        extremeWirelessIntfSpeedDataTX48        Unsigned32,
        extremeWirelessIntfSpeedDataTX54        Unsigned32,
        extremeWirelessIntfSpeedDataRX1         Unsigned32,
        extremeWirelessIntfSpeedDataRX2         Unsigned32,
        extremeWirelessIntfSpeedDataRX5p5       Unsigned32,
        extremeWirelessIntfSpeedDataRX6         Unsigned32,
        extremeWirelessIntfSpeedDataRX9         Unsigned32,
    extremeWirelessIntfSpeedDataRX11    Unsigned32,
        extremeWirelessIntfSpeedDataRX12        Unsigned32,
        extremeWirelessIntfSpeedDataRX18        Unsigned32,
        extremeWirelessIntfSpeedDataRX24        Unsigned32,
        extremeWirelessIntfSpeedDataRX36        Unsigned32,
        extremeWirelessIntfSpeedDataRX48        Unsigned32,
        extremeWirelessIntfSpeedDataRX54        Unsigned32 }

extremeWirelessIntfSpeedMgmtTX1 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of management-type frames transmitted
         on this interface at 1Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 1 }

extremeWirelessIntfSpeedMgmtTX2 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of management-type frames transmitted
         on this interface at 2Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 2 }

extremeWirelessIntfSpeedMgmtTX5p5 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of management-type frames transmitted
         on this interface at 5.5Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 3 }

extremeWirelessIntfSpeedMgmtTX6 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of management-type frames transmitted
         on this interface at 6Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 4 }

extremeWirelessIntfSpeedMgmtTX9 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of management-type frames transmitted
         on this interface at 9Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 5 }

extremeWirelessIntfSpeedMgmtTX11 OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "This gives the number of management-type frames transmitted
     on this interface at 11Mbps."
     ::= { extremeWirelessIntfFrameSpeedEntry 6 }

extremeWirelessIntfSpeedMgmtTX12 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of management-type frames transmitted
         on this interface at 12Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 7 }

extremeWirelessIntfSpeedMgmtTX18 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of management-type frames transmitted
         on this interface at 18Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 8 }

extremeWirelessIntfSpeedMgmtTX24 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of management-type frames transmitted
         on this interface at 24Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 9 }

extremeWirelessIntfSpeedMgmtTX36 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of management-type frames transmitted
         on this interface at 36Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 10 }

extremeWirelessIntfSpeedMgmtTX48 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of management-type frames transmitted
         on this interface at 48Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 11 }

extremeWirelessIntfSpeedMgmtTX54 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of management-type frames transmitted
         on this interface at 54Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 12 }

extremeWirelessIntfSpeedMgmtRX1 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of management-type frames recieved
         on this interface at 1Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 13 }

extremeWirelessIntfSpeedMgmtRX2 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of management-type frames recieved
         on this interface at 2Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 14 }

extremeWirelessIntfSpeedMgmtRX5p5 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of management-type frames recieved
         on this interface at 5.5Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 15 }

extremeWirelessIntfSpeedMgmtRX6 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of management-type frames recieved
         on this interface at 6Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 16 }

extremeWirelessIntfSpeedMgmtRX9 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of management-type frames recieved
         on this interface at 9Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 17 }

extremeWirelessIntfSpeedMgmtRX11 OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "This gives the number of management-type frames recieved
     on this interface at 11Mbps."
     ::= { extremeWirelessIntfFrameSpeedEntry 18 }

extremeWirelessIntfSpeedMgmtRX12 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of management-type frames recieved
         on this interface at 12Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 19 }

extremeWirelessIntfSpeedMgmtRX18 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of management-type frames recieved
         on this interface at 18Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 20 }

extremeWirelessIntfSpeedMgmtRX24 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of management-type frames recieved
         on this interface at 24Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 21 }

extremeWirelessIntfSpeedMgmtRX36 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of management-type frames recieved
         on this interface at 36Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 22 }

extremeWirelessIntfSpeedMgmtRX48 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of management-type frames recieved
         on this interface at 48Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 23 }

extremeWirelessIntfSpeedMgmtRX54 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of management-type frames recieved
         on this interface at 54Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 24 }

extremeWirelessIntfSpeedCtlTX1 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of control-type frames transmitted
         on this interface at 1Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 25 }

extremeWirelessIntfSpeedCtlTX2 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of control-type frames transmitted
         on this interface at 2Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 26 }

extremeWirelessIntfSpeedCtlTX5p5 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of control-type frames transmitted
         on this interface at 5.5Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 27 }

extremeWirelessIntfSpeedCtlTX6 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of control-type frames transmitted
         on this interface at 6Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 28 }

extremeWirelessIntfSpeedCtlTX9 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of control-type frames transmitted
         on this interface at 9Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 29 }

extremeWirelessIntfSpeedCtlTX11 OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "This gives the number of control-type frames transmitted
     on this interface at 11Mbps."
     ::= { extremeWirelessIntfFrameSpeedEntry 30 }

extremeWirelessIntfSpeedCtlTX12 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of control-type frames transmitted
         on this interface at 12Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 31 }

extremeWirelessIntfSpeedCtlTX18 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of control-type frames transmitted
         on this interface at 18Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 32 }

extremeWirelessIntfSpeedCtlTX24 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of control-type frames transmitted
         on this interface at 24Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 33 }

extremeWirelessIntfSpeedCtlTX36 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of control-type frames transmitted
         on this interface at 36Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 34 }

extremeWirelessIntfSpeedCtlTX48 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of control-type frames transmitted
         on this interface at 48Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 35 }

extremeWirelessIntfSpeedCtlTX54 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of control-type frames transmitted
         on this interface at 54Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 36 }

extremeWirelessIntfSpeedCtlRX1 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of control-type frames recieved
         on this interface at 1Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 37 }

extremeWirelessIntfSpeedCtlRX2 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of control-type frames recieved
         on this interface at 2Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 38 }

extremeWirelessIntfSpeedCtlRX5p5 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of control-type frames recieved
         on this interface at 5.5Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 39 }

extremeWirelessIntfSpeedCtlRX6 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of control-type frames recieved
         on this interface at 6Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 40 }

extremeWirelessIntfSpeedCtlRX9 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of control-type frames recieved
         on this interface at 9Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 41 }

extremeWirelessIntfSpeedCtlRX11 OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "This gives the number of control-type frames recieved
     on this interface at 11Mbps."
     ::= { extremeWirelessIntfFrameSpeedEntry 42 }


extremeWirelessIntfSpeedCtlRX12 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of control-type frames recieved
         on this interface at 12Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 43 }

extremeWirelessIntfSpeedCtlRX18 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of control-type frames recieved
         on this interface at 18Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 44 }

extremeWirelessIntfSpeedCtlRX24 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of control-type frames recieved
         on this interface at 24Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 45 }

extremeWirelessIntfSpeedCtlRX36 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of control-type frames recieved
         on this interface at 36Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 46 }

extremeWirelessIntfSpeedCtlRX48 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of control-type frames recieved
         on this interface at 48Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 47 }

extremeWirelessIntfSpeedCtlRX54 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of control-type frames recieved
         on this interface at 54Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 48 }

extremeWirelessIntfSpeedDataTX1 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of data-type frames transmitted
         on this interface at 1Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 49 }

extremeWirelessIntfSpeedDataTX2 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of data-type frames transmitted
         on this interface at 2Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 50 }

extremeWirelessIntfSpeedDataTX5p5 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of data-type frames transmitted
         on this interface at 5.5Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 51 }

extremeWirelessIntfSpeedDataTX6 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of data-type frames transmitted
         on this interface at 6Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 52 }

extremeWirelessIntfSpeedDataTX9 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of data-type frames transmitted
         on this interface at 9Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 53 }

extremeWirelessIntfSpeedDataTX11 OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "This gives the number of data-type frames transmitted
     on this interface at 11Mbps."
     ::= { extremeWirelessIntfFrameSpeedEntry 54 }

extremeWirelessIntfSpeedDataTX12 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of data-type frames transmitted
         on this interface at 12Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 55 }

extremeWirelessIntfSpeedDataTX18 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of data-type frames transmitted
         on this interface at 18Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 56 }

extremeWirelessIntfSpeedDataTX24 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of data-type frames transmitted
         on this interface at 24Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 57 }

extremeWirelessIntfSpeedDataTX36 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of data-type frames transmitted
         on this interface at 36Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 58 }

extremeWirelessIntfSpeedDataTX48 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of data-type frames transmitted
         on this interface at 48Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 59 }

extremeWirelessIntfSpeedDataTX54 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of data-type frames transmitted
         on this interface at 54Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 60 }

extremeWirelessIntfSpeedDataRX1 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of data-type frames recieved
         on this interface at 1Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 61 }

extremeWirelessIntfSpeedDataRX2 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of data-type frames recieved
         on this interface at 2Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 62 }

extremeWirelessIntfSpeedDataRX5p5 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of data-type frames recieved
         on this interface at 5.5Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 63 }

extremeWirelessIntfSpeedDataRX6 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of data-type frames recieved
         on this interface at 6Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 64 }

extremeWirelessIntfSpeedDataRX9 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of data-type frames recieved
         on this interface at 9Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 65 }

extremeWirelessIntfSpeedDataRX11 OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "This gives the number of data-type frames recieved
     on this interface at 11Mbps."
     ::= { extremeWirelessIntfFrameSpeedEntry 66 }

extremeWirelessIntfSpeedDataRX12 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of data-type frames recieved
         on this interface at 12Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 67 }

extremeWirelessIntfSpeedDataRX18 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of data-type frames recieved
         on this interface at 18Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 68 }

extremeWirelessIntfSpeedDataRX24 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of data-type frames recieved
         on this interface at 24Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 69 }

extremeWirelessIntfSpeedDataRX36 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of data-type frames recieved
         on this interface at 36Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 70 }

extremeWirelessIntfSpeedDataRX48 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of data-type frames recieved
         on this interface at 48Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 71 }

extremeWirelessIntfSpeedDataRX54 OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of data-type frames recieved
         on this interface at 54Mbps."
         ::= { extremeWirelessIntfFrameSpeedEntry 72 }

-- *************************************************************** --
-- Error Histograms of retransmission by frame speed.              --
-- *************************************************************** --
extremeWirelessIntfFrameSpeedErrorTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessIntfFrameSpeedErrorEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "There is one entry in this table for each virtual and
         physical interface.  Values for physical interfaces are
         summations of the values for the constituent virtual 
         interfaces."
         ::= { extremeAP 42 }

extremeWirelessIntfFrameSpeedErrorEntry OBJECT-TYPE
        SYNTAX ExtremeWirelessIntfFrameSpeedErrorEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        ""
        INDEX { ifIndex }
         ::= { extremeWirelessIntfFrameSpeedErrorTable 1 }

ExtremeWirelessIntfFrameSpeedErrorEntry ::= SEQUENCE {
        extremeWirelessIntfSpeedReXmit1         Unsigned32,
        extremeWirelessIntfSpeedReXmit2         Unsigned32,
        extremeWirelessIntfSpeedReXmit5p5       Unsigned32,
        extremeWirelessIntfSpeedReXmit6         Unsigned32,
        extremeWirelessIntfSpeedReXmit9         Unsigned32,
    extremeWirelessIntfSpeedReXmit11    Unsigned32,
        extremeWirelessIntfSpeedReXmit12        Unsigned32,
        extremeWirelessIntfSpeedReXmit18        Unsigned32,
        extremeWirelessIntfSpeedReXmit24        Unsigned32,
        extremeWirelessIntfSpeedReXmit36        Unsigned32,
        extremeWirelessIntfSpeedReXmit48        Unsigned32,
        extremeWirelessIntfSpeedReXmit54        Unsigned32,
    extremeWirelessIntfSpeedErrorTX1    Unsigned32,
    extremeWirelessIntfSpeedErrorTX2    Unsigned32,
    extremeWirelessIntfSpeedErrorTX5p5  Unsigned32,
    extremeWirelessIntfSpeedErrorTX6    Unsigned32,
    extremeWirelessIntfSpeedErrorTX9    Unsigned32,
    extremeWirelessIntfSpeedErrorTX11   Unsigned32,
    extremeWirelessIntfSpeedErrorTX12   Unsigned32,
    extremeWirelessIntfSpeedErrorTX18   Unsigned32,
    extremeWirelessIntfSpeedErrorTX24   Unsigned32,
    extremeWirelessIntfSpeedErrorTX36   Unsigned32,
    extremeWirelessIntfSpeedErrorTX48   Unsigned32,
    extremeWirelessIntfSpeedErrorTX54   Unsigned32,
        extremeWirelessIntfSpeedErrorRX1        Unsigned32,
        extremeWirelessIntfSpeedErrorRX2        Unsigned32,
        extremeWirelessIntfSpeedErrorRX5p5      Unsigned32,
        extremeWirelessIntfSpeedErrorRX6        Unsigned32,
        extremeWirelessIntfSpeedErrorRX9        Unsigned32,
    extremeWirelessIntfSpeedErrorRX11   Unsigned32,
        extremeWirelessIntfSpeedErrorRX12       Unsigned32,
        extremeWirelessIntfSpeedErrorRX18       Unsigned32,
        extremeWirelessIntfSpeedErrorRX24       Unsigned32,
        extremeWirelessIntfSpeedErrorRX36       Unsigned32,
        extremeWirelessIntfSpeedErrorRX48       Unsigned32,
        extremeWirelessIntfSpeedErrorRX54       Unsigned32 }

extremeWirelessIntfSpeedReXmit1 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which were retransmitted on
         this interface at 1 Mbps."
        ::= { extremeWirelessIntfFrameSpeedErrorEntry 1 }

extremeWirelessIntfSpeedReXmit2 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which were retransmitted on
         this interface at 2 Mbps."
        ::= { extremeWirelessIntfFrameSpeedErrorEntry 2 }

extremeWirelessIntfSpeedReXmit5p5 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which were retransmitted on
         this interface at 5 Mbps."
        ::= { extremeWirelessIntfFrameSpeedErrorEntry 3 }

extremeWirelessIntfSpeedReXmit6 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which were retransmitted on
         this interface at 6 Mbps."
        ::= { extremeWirelessIntfFrameSpeedErrorEntry 4 }

extremeWirelessIntfSpeedReXmit9 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which were retransmitted on
         this interface at 9 Mbps."
        ::= { extremeWirelessIntfFrameSpeedErrorEntry 5 }

extremeWirelessIntfSpeedReXmit11 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were retransmitted on
    this interface at 11 Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 6 }

extremeWirelessIntfSpeedReXmit12 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which were retransmitted on
         this interface at 12 Mbps."
        ::= { extremeWirelessIntfFrameSpeedErrorEntry 7 }

extremeWirelessIntfSpeedReXmit18 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which were retransmitted on
         this interface at 18 Mbps."
        ::= { extremeWirelessIntfFrameSpeedErrorEntry 8 }

extremeWirelessIntfSpeedReXmit24 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which were retransmitted on
         this interface at 24 Mbps."
        ::= { extremeWirelessIntfFrameSpeedErrorEntry 9 }
        
extremeWirelessIntfSpeedReXmit36 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which were retransmitted on
         this interface at 36 Mbps."
        ::= { extremeWirelessIntfFrameSpeedErrorEntry 10 }

extremeWirelessIntfSpeedReXmit48 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which were retransmitted on
         this interface at 48 Mbps."
        ::= { extremeWirelessIntfFrameSpeedErrorEntry 11 }

extremeWirelessIntfSpeedReXmit54 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which were retransmitted on
         this interface at 54 Mbps."
        ::= { extremeWirelessIntfFrameSpeedErrorEntry 12 }

extremeWirelessIntfSpeedErrorTX1 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 1Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 13 }

extremeWirelessIntfSpeedErrorTX2 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 2Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 14 }

extremeWirelessIntfSpeedErrorTX5p5 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 5.5Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 15 }

extremeWirelessIntfSpeedErrorTX6 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 6Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 16 }

extremeWirelessIntfSpeedErrorTX9 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 9Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 17 }

extremeWirelessIntfSpeedErrorTX11 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 11Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 18 }

extremeWirelessIntfSpeedErrorTX12 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 12Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 19 }

extremeWirelessIntfSpeedErrorTX18 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 18Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 20 }

extremeWirelessIntfSpeedErrorTX24 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 24Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 21 }

extremeWirelessIntfSpeedErrorTX36 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 36Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 22 }

extremeWirelessIntfSpeedErrorTX48 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 48Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 23 }

extremeWirelessIntfSpeedErrorTX54 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 54Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 24 }

extremeWirelessIntfSpeedErrorRX1 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which were received with errors
         on this interface at 1Mbps."
        ::= { extremeWirelessIntfFrameSpeedErrorEntry 25 }

extremeWirelessIntfSpeedErrorRX2 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which were received with errors
         on this interface at 2Mbps."
        ::= { extremeWirelessIntfFrameSpeedErrorEntry 26 }

extremeWirelessIntfSpeedErrorRX5p5 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which were received with errors
         on this interface at 5.5Mbps."
        ::= { extremeWirelessIntfFrameSpeedErrorEntry 27 }

extremeWirelessIntfSpeedErrorRX6 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which were received with errors
         on this interface at 6Mbps."
        ::= { extremeWirelessIntfFrameSpeedErrorEntry 28 }

extremeWirelessIntfSpeedErrorRX9 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which were received with errors
         on this interface at 9Mbps."
        ::= { extremeWirelessIntfFrameSpeedErrorEntry 29 }

extremeWirelessIntfSpeedErrorRX11 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were received with errors
    on this interface at 11Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 30 }

extremeWirelessIntfSpeedErrorRX12 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which were received with errors
         on this interface at 12Mbps."
        ::= { extremeWirelessIntfFrameSpeedErrorEntry 31 }

extremeWirelessIntfSpeedErrorRX18 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which were received with errors
         on this interface at 18Mbps."
        ::= { extremeWirelessIntfFrameSpeedErrorEntry 32 }

extremeWirelessIntfSpeedErrorRX24 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which were received with errors
         on this interface at 24Mbps."
        ::= { extremeWirelessIntfFrameSpeedErrorEntry 33 }

extremeWirelessIntfSpeedErrorRX36 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which were received with errors
         on this interface at 36Mbps."
        ::= { extremeWirelessIntfFrameSpeedErrorEntry 34 }

extremeWirelessIntfSpeedErrorRX48 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which were received with errors
         on this interface at 48Mbps."
        ::= { extremeWirelessIntfFrameSpeedErrorEntry 35 }

extremeWirelessIntfSpeedErrorRX54 OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the number of frames which were received with errors
         on this interface at 54Mbps."
        ::= { extremeWirelessIntfFrameSpeedErrorEntry 36 }

-- *************************************************************** --
-- Interface utilization/noise.                                    --
-- *************************************************************** --
extremeWirelessIntfUtilizationTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessIntfUtilizationEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "There is one entry in this table for each virtual and
         physical interface.  Values for physical interfaces are
         summations of the values for the constituent virtual 
         interfaces."
         ::= { extremeAP 43 }

extremeWirelessIntfUtilizationEntry OBJECT-TYPE
        SYNTAX ExtremeWirelessIntfUtilizationEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        ""
        INDEX { ifIndex }
         ::= { extremeWirelessIntfUtilizationTable 1 }

ExtremeWirelessIntfUtilizationEntry ::= SEQUENCE {
        extremeWirelessIntfUtilizationNav                Unsigned32,
        extremeWirelessIntfUtilizationNoiseFloor         Unsigned32 }

extremeWirelessIntfUtilizationNav OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the instantaneous NAV value on this interface, or
         some increasing-metric of utilization."
        ::= { extremeWirelessIntfUtilizationEntry 1 }

extremeWirelessIntfUtilizationNoiseFloor OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the noise floor in dBm for this interface."
        ::= { extremeWirelessIntfUtilizationEntry 2 }

-- *************************************************************** --
-- Opaque client MIBs. These mibs are provided as a performance    --
-- gain for the LAC management of the switch.                      --
--                                                                 --
-- Some of the items in this table are encoded as a series of TLVs.--
-- In this case, they are encoded as:                              --
--                                                                 --
--   | Type (8 bits) | length (8 bits) | value (variable) |        --
--                                                                 --
-- type - equal to the index field of the element                  --
--        in the table this value corresponds to.                  --
--                                                                 --
-- length - equal to the length in bytes of the value              --
--                                                                 --
-- value -  this is the value.  Integer value are NBO,             --
--          strings are non-null terminated ASCII.                 --
--                                                                 --
-- *************************************************************** --
extremeWirelessOpaqueTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF ExtremeWirelessOpaqueEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                " "
        ::= { extremeAP 99 }

extremeWirelessOpaqueEntry OBJECT-TYPE
        SYNTAX          ExtremeWirelessOpaqueEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                " "
        INDEX { ifIndex }
        ::= { extremeWirelessOpaqueTable 1 }

ExtremeWirelessOpaqueEntry ::= SEQUENCE {
        extremeWirelessClientData               OCTET STRING,
        extremeWirelessPAEStatsData             OCTET STRING,
        extremeWirelessPAEDiagData              OCTET STRING,
        extremeWirelessScanResultsData          OCTET STRING,
        extremeWirelessProbeInfoData            OCTET STRING,
        extremeWirelessClientDiagData           OCTET STRING,
        extremeWirelessClientAssocData          OCTET STRING,
        extremeWirelessClientAuthData           OCTET STRING,
        extremeWirelessClientMACInfoData        OCTET STRING,
        extremeWirelessSizeCounterData          OCTET STRING,
        extremeWirelessSpeedCounterData         OCTET STRING }

extremeWirelessClientData OBJECT-TYPE
        SYNTAX          OCTET STRING
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        ""
        ::= { extremeWirelessOpaqueEntry 1 }    

extremeWirelessPAEStatsData OBJECT-TYPE
        SYNTAX          OCTET STRING
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        ""
        ::= { extremeWirelessOpaqueEntry 2 }    

extremeWirelessPAEDiagData OBJECT-TYPE
        SYNTAX          OCTET STRING
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        ""
        ::= { extremeWirelessOpaqueEntry 3 }

extremeWirelessScanResultsData OBJECT-TYPE
        SYNTAX          OCTET STRING
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This is the contents of the scan results table encoded
         as a series of TLVs."
        ::= { extremeWirelessOpaqueEntry 4 }

extremeWirelessProbeInfoData OBJECT-TYPE
        SYNTAX          OCTET STRING
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This is the contents of the probe info table encoded 
         as a series of TLVs.    Each item is encoded as the
         entry above."
        ::= { extremeWirelessOpaqueEntry 5 }

extremeWirelessClientDiagData OBJECT-TYPE
        SYNTAX          OCTET STRING
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This is the contents of the client diag table encoded 
         as a series of TLVs.    Each item is encoded as the
         entry above."
        ::= { extremeWirelessOpaqueEntry 6 }

extremeWirelessClientAssocData OBJECT-TYPE
        SYNTAX          OCTET STRING
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This is the contents of the client assoc table encoded 
         as a series of TLVs.    Each item is encoded as the
         entry above.  Note that since the MAC address is not a
         member of the table (it is an index) it will be encoded
         as type = 0."
        ::= { extremeWirelessOpaqueEntry 7 }

extremeWirelessClientAuthData OBJECT-TYPE
        SYNTAX          OCTET STRING
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This is the contents of the client auth table encoded 
         as a series of TLVs.    Each item is encoded as the
         entry above.  Note that since the MAC address is not a
         member of the table (it is an index) it will be encoded
         as type = 0."
        ::= { extremeWirelessOpaqueEntry 8 }

extremeWirelessClientMACInfoData OBJECT-TYPE
        SYNTAX          OCTET STRING
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This is the contents of the client MAC info table 
         encoded as a series of TLVs.    Each item is encoded 
         as the entry above.  Note that since the MAC address 
         is not a member of the table (it is an index) it will 
         be encoded as type = 0."
        ::= { extremeWirelessOpaqueEntry 9 }

extremeWirelessSizeCounterData OBJECT-TYPE
        SYNTAX          OCTET STRING
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This is the contents of the client size counter table
         encoded as a series of TLVs.    Each item is encoded 
         as the entry above.  Note that since the MAC address 
         is not a member of the table (it is an index) it will 
         be encoded as type = 0."
        ::= { extremeWirelessOpaqueEntry 10 }

extremeWirelessSpeedCounterData OBJECT-TYPE
        SYNTAX          OCTET STRING
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This is the contents of the client speed counter table
         encoded as a series of TLVs.    Each item is encoded 
         as the entry above.  Note that since the MAC address 
         is not a member of the table (it is an index) it will 
         be encoded as type = 0."
        ::= { extremeWirelessOpaqueEntry 11 }

-- *************************************************************** --
-- TRACE MIBS                                                      --
--                                                                 --
-- These mibs are provided on a per-wireless port basis to support --
-- configurable tracing.  Each subsystem associated with a         --
-- wireless port has an entry in the trace module table.  These    --
-- entries allow for configuration of the current trace level.     --
-- statistics on each modules tracing output are also kept.  At    --
-- a global level several statistics are available from the trace  --
-- table.                                                          --
-- *************************************************************** --
extremeWirelessTraceTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessTraceTableEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
         "This table contains one entry per wireless port.  This
          allows access to various stastics about the tracing mod  --
          ule on that wireless port."
        ::= { extremeAP 100 }

extremeWirelessTraceEntry OBJECT-TYPE
        SYNTAX          ExtremeWirelessTraceTableEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        ""
        INDEX { ifIndex }
        ::= { extremeWirelessTraceTable 1 }

ExtremeWirelessTraceTableEntry ::= SEQUENCE {
        extremeWirelessTraceMsgsOut     INTEGER,
        extremeWirelessTraceBytesOut    INTEGER,
        extremeWirelessTraceSuppressed  INTEGER,
        extremeWirelessTraceOtherErr    INTEGER,
        extremeWirelessTraceOpaque      OCTET STRING }

extremeWirelessTraceMsgsOut OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This gives the number of trace messages the system has
         sent out to the syslog server.  Suppressed messages are
         not counted toward this total."
        ::= { extremeWirelessTraceEntry 1 }

extremeWirelessTraceBytesOut OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This give the number of bytes total sent out by the
         trace system.  This is a simple sum of the string
         lengths of all messages sent out."
        ::= { extremeWirelessTraceEntry 2 }

extremeWirelessTraceSuppressed OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This variable is incremented whenever a message is
         not sent out because the trace level of that system
         is lower than the message level."
        ::= { extremeWirelessTraceEntry 3 }

extremeWirelessTraceOtherErr OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This variable is incremented when a message is not 
         sent out due to internal errors (i.e. out of memory)."
        ::= { extremeWirelessTraceEntry 4 }

extremeWirelessTraceOpaque OBJECT-TYPE
        SYNTAX          OCTET STRING
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
        "This is the opaque representation of the module table
         to optimize retreival."
        ::= { extremeWirelessTraceEntry 5 }

extremeWirelessTraceModuleTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessTraceModuleEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
         "This table contains one entry per trace module.  Each entry
          is indexed by an arbitrary integer value."
        ::= { extremeAP 101 }

extremeWirelessTraceModuleEntry OBJECT-TYPE
        SYNTAX ExtremeWirelessTraceModuleEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        ""
        INDEX { ifIndex, extremeWirelessTraceModuleId }
        ::= { extremeWirelessTraceModuleTable 1 }

ExtremeWirelessTraceModuleEntry ::= SEQUENCE {
        extremeWirelessTraceModuleId         INTEGER,
        extremeWirelessTraceModuleDesc       DisplayString,
        extremeWirelessTraceModuleHeader     DisplayString,
        extremeWirelessTraceModuleLevel      INTEGER,
        extremeWirelessTraceModuleSuppressed INTEGER,
        extremeWirelessTraceModuleMsgsOut    INTEGER,
        extremeWirelessTraceModuleBytesOut   INTEGER }

extremeWirelessTraceModuleId         OBJECT-TYPE
        SYNTAX  INTEGER(0..65535)
        MAX-ACCESS not-accessible
        STATUS  current
        DESCRIPTION
        "This is an arbitrary integer index which is assigned to each
         trace module."
        ::= { extremeWirelessTraceModuleEntry 1 }

extremeWirelessTraceModuleDesc       OBJECT-TYPE
        SYNTAX  DisplayString
        MAX-ACCESS read-only
        STATUS  current
        DESCRIPTION
        "This is a string which briefly describes the purpose of this
         debug trace.  It may include whitespace.  An example is:
                802.1x State Machine"
        ::= { extremeWirelessTraceModuleEntry 2 }

extremeWirelessTraceModuleHeader     OBJECT-TYPE
        SYNTAX  DisplayString
        MAX-ACCESS read-only
        STATUS  current
        DESCRIPTION
        "This is a string which is prepended to the syslog messages
         sent out by this debug level.  It is short (5-6 characters) 
         and does not contain white space. (i.e. DOT1X)"
        ::= { extremeWirelessTraceModuleEntry 3 }

extremeWirelessTraceModuleLevel     OBJECT-TYPE
        SYNTAX  INTEGER(0..5)
        MAX-ACCESS read-write
        STATUS  current
        DESCRIPTION
        "This value is the current debug level for this module.  A
         lower value indicates that fewer messages will be generated
         by the component.  A write on this value will update the
         current debug level."
        ::= { extremeWirelessTraceModuleEntry 4 }

extremeWirelessTraceModuleSuppressed     OBJECT-TYPE
        SYNTAX  INTEGER
        MAX-ACCESS read-only
        STATUS  current
        DESCRIPTION
        "This value indicates the number of messages logged by
         this module which have not been sent out because the
         current log level is less than the level at which the
         message should be logged."
        ::= { extremeWirelessTraceModuleEntry 5 }

extremeWirelessTraceModuleMsgsOut     OBJECT-TYPE
        SYNTAX  INTEGER
        MAX-ACCESS read-only
        STATUS  current
        DESCRIPTION
        "This value indicates the number messages which have
         been logged by this component."
        ::= { extremeWirelessTraceModuleEntry 6 }

extremeWirelessTraceModuleBytesOut     OBJECT-TYPE
        SYNTAX  INTEGER
        MAX-ACCESS read-only
        STATUS  current
        DESCRIPTION
        "This value indicates the number of bytes which have
         been logged by this component.  This count includes 
         the header specified in extremeWirelessTraceModuleHeader."
        ::= { extremeWirelessTraceModuleEntry 7 }

-- *************************************************************** --
--                    Log Diagnostic Counters                      --
--                                                                 --
-- The logging subsystem uses the following division : the event   --
-- logging system recieves all messages.  These message are then   --
-- passed to the syslog facility for remote logging, and then msgs --
-- may be stored in the NVRAM in the case where the log level is   --
-- greater than the log threshold.                                 --
-- *************************************************************** --
extremeWirelessLogDiagTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessLogDiagEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "This table contains counters per-log level for the event log,
         syslog and NVRAM subsystems for logging."
        ::= { extremeAP 102 }

extremeWirelessLogDiagEntry OBJECT-TYPE
        SYNTAX  ExtremeWirelessLogDiagEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "There is one entry in this table per physical port."
        INDEX { ifIndex }
        ::= { extremeWirelessLogDiagTable 1 }

ExtremeWirelessLogDiagEntry ::= SEQUENCE {
        extremeWirelessLogDiagEventLogTotalCount Unsigned32,
        extremeWirelessLogDiagEventLogTotalEmergCount Unsigned32,
        extremeWirelessLogDiagEventLogTotalAlertCount Unsigned32,
        extremeWirelessLogDiagEventLogTotalCritCount Unsigned32,
        extremeWirelessLogDiagEventLogTotalErrorCount Unsigned32,
        extremeWirelessLogDiagEventLogTotalWarnCount Unsigned32,
        extremeWirelessLogDiagEventLogTotalNoticeCount Unsigned32,
        extremeWirelessLogDiagEventLogTotalInfoCount Unsigned32,
        extremeWirelessLogDiagEventLogTotalDebugCount Unsigned32,
        extremeWirelessLogDiagEventLogTotalSuppressedCount Unsigned32,
        extremeWirelessLogDiagEventLogTotalByteCount Unsigned32,
        extremeWirelessLogDiagSyslogTotalEventCount Unsigned32,
        extremeWirelessLogDiagSyslogTotalSuppressedCount Unsigned32,
        extremeWirelessLogDiagSyslogTotalByteCount Unsigned32,
        extremeWirelessLogDiagNVRAMTotalEventCount Unsigned32,
        extremeWirelessLogDiagNVRAMTotalSuppressedCount Unsigned32,
        extremeWirelessLogDiagNVRAMTotalDroppedCount Unsigned32,
        extremeWirelessLogDiagNVRAMTotalByteCount Unsigned32,
        extremeWirelessLogDiagClearStats TruthValue }

extremeWirelessLogDiagEventLogTotalCount OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of messages logged since the
         last time the statistics were cleared."
        ::= { extremeWirelessLogDiagEntry 1 }

extremeWirelessLogDiagEventLogTotalEmergCount OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of messages logged at the EMERG
         level."
        ::= { extremeWirelessLogDiagEntry 2 }

extremeWirelessLogDiagEventLogTotalAlertCount OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of messages logged at the ALERT
         level."
        ::= { extremeWirelessLogDiagEntry 3 }

extremeWirelessLogDiagEventLogTotalCritCount OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of messages logged at the CRIT
         level."
        ::= { extremeWirelessLogDiagEntry 4 }

extremeWirelessLogDiagEventLogTotalErrorCount OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of messages logged at the ERROR
         level."
        ::= { extremeWirelessLogDiagEntry 5 }

extremeWirelessLogDiagEventLogTotalWarnCount OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of messages logged at the WARN
         level."
        ::= { extremeWirelessLogDiagEntry 6 }

extremeWirelessLogDiagEventLogTotalNoticeCount OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of messages logged at the NOTICE
         level."
        ::= { extremeWirelessLogDiagEntry 7 }

extremeWirelessLogDiagEventLogTotalInfoCount OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of messages logged at the INFO
         level."
        ::= { extremeWirelessLogDiagEntry 8 }

extremeWirelessLogDiagEventLogTotalDebugCount OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of messages logged at the DEBUG
         level."
        ::= { extremeWirelessLogDiagEntry 9 }

extremeWirelessLogDiagEventLogTotalSuppressedCount OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of messages which were suppressed
         due to log level."
        ::= { extremeWirelessLogDiagEntry 10 }

extremeWirelessLogDiagEventLogTotalByteCount OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of bytes logged by the logging
         subsystem."
        ::= { extremeWirelessLogDiagEntry 11 }

extremeWirelessLogDiagSyslogTotalEventCount OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of messages which have been sent
         out to remote syslog servers."
        ::= { extremeWirelessLogDiagEntry 12 }

extremeWirelessLogDiagSyslogTotalSuppressedCount OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of syslog messages which have been 
         suppressed due to log level."
        ::= { extremeWirelessLogDiagEntry 13 }

extremeWirelessLogDiagSyslogTotalByteCount OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "This gives the total number of bytes of syslog messages which have
         been logged."
        ::= { extremeWirelessLogDiagEntry 14 }

extremeWirelessLogDiagNVRAMTotalEventCount OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Total number of messages which have been logged to NVRAM."
        ::= { extremeWirelessLogDiagEntry 15 }

extremeWirelessLogDiagNVRAMTotalSuppressedCount OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Total number of messages which have been suppressed by NVRAM
         due to NVRAM threashold."
        ::= { extremeWirelessLogDiagEntry 16 }

extremeWirelessLogDiagNVRAMTotalDroppedCount OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Total number of messages which have been dropped by the 
         NVRAM."
        ::= { extremeWirelessLogDiagEntry 17 }

extremeWirelessLogDiagNVRAMTotalByteCount OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        "Total number of bytes which have been written to the NVRAM."
        ::= { extremeWirelessLogDiagEntry 18 }

extremeWirelessLogDiagClearStats OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "Setting this value to TRUE causes the statistics to be reset to
         0.  Reading this value has no meaning."
        ::= { extremeWirelessLogDiagEntry 19 }

-- *************************************************************** --
--                           TRAPS                                 --
--                                                                 --
-- NOTE: We define client Authentication and association traps but --
--       performance may dictate that this not be done.  In that   --
--       case we have already provided the Authentication and      --
--       association totals which can be watched from RMON.        --
--                                                                 --
-- NOTE: The MAP State Change trap is not sent when the MAP is     --
--       first discovered.  The first trap is sent by EDP.         --
-- *************************************************************** --
extremeWirelessPortStateChange NOTIFICATION-TYPE
        OBJECTS { ifIndex,
                  extremeWirelessPortState }
        STATUS current
        DESCRIPTION
                "This trap is generated when a wireless port moves 
                 into enabled, disabled or online."
        ::= { extremeAPTrapsPrefix 1 }

extremeWirelessPortBootFailure NOTIFICATION-TYPE
       OBJECTS { extremeWirelessPortIfIndex }
       STATUS current
       DESCRIPTION
               "This trap is sent by the platform if a wireless 
                port fails to boot too many times."
       ::= { extremeAPTrapsPrefix 2 }

extremeWirelessClientStationAgedOut NOTIFICATION-TYPE
       OBJECTS { ifIndex, extremeWirelessClientID }
       STATUS current
       DESCRIPTION
               "This trap is generated when a client is aged out 
                of the table."
       ::= { extremeAPTrapsPrefix 3 }

extremeWirelessNetloginClientAssociated NOTIFICATION-TYPE
       OBJECTS { ifIndex, extremeWirelessClientID }
       STATUS current
       DESCRIPTION
               "This trap is generated when a client has associated 
                to an interface that is web based network login 
                enabled."
       ::= { extremeAPTrapsPrefix 4 }

extremeWirelessAPAdded NOTIFICATION-TYPE
       OBJECTS { ifIndex, 
                 extremeWirelessScanResultsStationId,
                 extremeWirelessScanResultsFirstSeen,
                 extremeWirelessScanResultsLastChange,
                 extremeWirelessScanResultsPacketRate,
                 extremeWirelessScanResultsChannel,
                 extremeWirelessScanResultsAvgRSS,
                 extremeWirelessScanResultsSSID,
                 extremeWirelessScanResultsRSNEnabled,
                 extremeWirelessScanResultsPrivacy,
                 extremeWirelessScanResultsNetworkType,
                 extremeWirelessScanWPAIEMcastCipher,
                 extremeWirelessScanWPAUcastCipherCount,
                 extremeWirelessScanWPAUcastCipher,
                 extremeWirelessScanWPAKeyMgmtCount,
                 extremeWirelessScanWPAKeyMgmtSuite,
         extremeWirelessScanResultsRateSet,      
         extremeWirelessScanResultsExtRateSet }
       STATUS current
       DESCRIPTION
               "This is generated when a new AP is added to the
                scan results table.  It will ony be generated if
                the value of extremeWirelessScanSendAPAddedTrap
                is true."
       ::= { extremeAPTrapsPrefix 5 }

extremeWirelessAPRemoved NOTIFICATION-TYPE
       OBJECTS { ifIndex, extremeWirelessScanResultsStationId }
       STATUS current
       DESCRIPTION
               "This is generated when an AP is removed from the
                scan results table.  It will ony be generated if
                the value of extremeWirelessScanSendAPRemovedTrap
                is true."
       ::= { extremeAPTrapsPrefix 6 }

extremeWirelessAPUpdated NOTIFICATION-TYPE
       OBJECTS { ifIndex, 
                 extremeWirelessScanResultsStationId,
                 extremeWirelessScanResultsFirstSeen,
                 extremeWirelessScanResultsLastChange,
                 extremeWirelessScanResultsPacketRate,
                 extremeWirelessScanResultsChannel,
                 extremeWirelessScanResultsAvgRSS,
                 extremeWirelessScanResultsSSID,
                 extremeWirelessScanResultsRSNEnabled,
                 extremeWirelessScanResultsPrivacy,
                 extremeWirelessScanResultsNetworkType,
                 extremeWirelessScanWPAIEMcastCipher,
                 extremeWirelessScanWPAUcastCipherCount,
                 extremeWirelessScanWPAUcastCipher,
                 extremeWirelessScanWPAKeyMgmtCount,
                 extremeWirelessScanWPAKeyMgmtSuite,
         extremeWirelessScanResultsRateSet,
         extremeWirelessScanResultsExtRateSet }
       STATUS current
       DESCRIPTION
               "This is generated when the IEs recorded for an AP
                in the scan results table change.  It will only be
                generated if the value of SendAPUpdatedTrap is true."
       ::= { extremeAPTrapsPrefix 7 }

extremeWirelessProbeInfoAdded NOTIFICATION-TYPE
       OBJECTS { ifIndex, extremeWirelessProbeInfoSource }
       STATUS current
       DESCRIPTION
               "This is generated when a new station is added to the
                probe info table.  It will only be generated if the 
                value of extremeWirelessProbeInfoSendAddedTrap is true."
       ::= { extremeAPTrapsPrefix 8 }

extremeWirelessProbeInfoRemoved NOTIFICATION-TYPE
       OBJECTS { ifIndex, extremeWirelessProbeInfoSource }
       STATUS current
       DESCRIPTION
               "This is generated when a station is removed from the
                probe info table.  It will only be generated if the 
                value of extremeWirelessProbeInfoSendRemovedTrap is 
                true."
       ::= { extremeAPTrapsPrefix 9 }

extremeWirelessOffChannelScanStarted NOTIFICATION-TYPE
        OBJECTS { ifIndex, extremeWirelessOffChannelScanList }
        STATUS current
        DESCRIPTION
                "This is generated when an off-channel scan starts
                 running."
        ::= { extremeAPTrapsPrefix 10 }

extremeWirelessOffChannelScanFinished NOTIFICATION-TYPE
        OBJECTS { ifIndex, extremeWirelessOffChannelScanList }
        STATUS current
        DESCRIPTION
                "This is generated when an off-channel scan finishes
                 running."
        ::= { extremeAPTrapsPrefix 11 }

extremeWirelessCounterMeasureStarted NOTIFICATION-TYPE
        OBJECTS { ifIndex, extremeWirelessCounterMeasureSource }
        STATUS current
        DESCRIPTION
        "This trap is generated when counter measures are started
        on a wireless interface."
        ::= { extremeAPTrapsPrefix 12 }

extremeWirelessCounterMeasureStopped NOTIFICATION-TYPE
        OBJECTS { ifIndex }
        STATUS current
        DESCRIPTION
        "This trap is generated when counter measures are stopped
        on a wireless interface."
        ::= { extremeAPTrapsPrefix 13 }

--DFS related
extremeWirelessInterfaceChannelRescan NOTIFICATION-TYPE
        OBJECTS { ifIndex,
                  extremeWirelessPhysInterfacePHYChannel,
                  extremeWirelessPhysInterfaceChannelAutoSelectStatus
            }
        STATUS current
        DESCRIPTION
                "This trap is generated when a wireless interface tries to
autoselect a channel. It indicates whether a particular channel scan was
successful, or if it failed then the reason for the failure."
        ::= { extremeAPTrapsPrefix 14 }

        --
        -- TODO: Should we move this somewhere else?
        --
extremeWirelessCounterMeasureSource OBJECT-TYPE
        SYNTAX INTEGER { clientReport(1),
            micFailure(2) }
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
            "This value is used in the counter measure traps to indicate the
            reason that counter measures have been invoked."
            ::= { extremeAP 44 }

extremeWirelessClientWPAStatsTable OBJECT-TYPE
        SYNTAX SEQUENCE OF ExtremeWirelessClientWPAStatsEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "This table contains information of the WPA state transitions
        on a per-client basis.  Rows are indexed first by virtual
        interface, then by client MAC."
         ::= { extremeAP 47 }

extremeWirelessClientWPAStatsEntry OBJECT-TYPE
        SYNTAX ExtremeWirelessClientWPAStatsEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "Note that ifIndex here is virtual ifIndex (SSID)."
        INDEX { ifIndex, extremeWirelessClientDiagMac }
         ::= { extremeWirelessClientWPAStatsTable 1 }

ExtremeWirelessClientWPAStatsEntry ::= SEQUENCE {
        extremeWirelessClientWPAStatsStarts     Counter32,
        extremeWirelessClientWPAStatsPairwiseKeySuccesses       Counter32,
        extremeWirelessClientWPAStatsPairwiseKeyFailures        Counter32,
        extremeWirelessClientWPAStatsGroupKeySuccesses          Counter32,
        extremeWirelessClientWPAStatsGroupKeyFailures           Counter32,
        extremeWirelessClientWPAStatsPairwiseKey1Sends          Counter32,
        extremeWirelessClientWPAStatsPairwiseKey3Sends          Counter32,
        extremeWirelessClientWPAStatsGroupKeySends                      Counter32,
        extremeWirelessClientWPAStatsEAPOLKeyReceivedInPairwise1Key     Counter32,
        extremeWirelessClientWPAStatsEAPOLKeyReceivedInPairwise3Key     Counter32,
        extremeWirelessClientWPAStatsEAPOLKeyReceivedInGroupKey         Counter32,
        extremeWirelessClientWPAStatsDoubleEAPOLKeyReceived             Counter32,
        extremeWirelessClientWPAStatsEAPOLKeyIgnores                    Counter32,
        extremeWirelessClientWPAStatsEAPOLKeyErrors                     Counter32,
        extremeWirelessClientWPAStatsEAPOLKeyAborts                     Counter32,
        extremeWirelessClientWPAStatsEAPOLKeyVerificationSuccesses      Counter32
}
extremeWirelessClientWPAStatsStarts OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "Number of starts of the WPA key exchange process"
         ::= { extremeWirelessClientWPAStatsEntry 1 }

extremeWirelessClientWPAStatsPairwiseKeySuccesses OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "Number of successes in the pairwise key handshake"
         ::= { extremeWirelessClientWPAStatsEntry 2 }

extremeWirelessClientWPAStatsPairwiseKeyFailures OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "Number of failures the pairwise key handshake"
         ::= { extremeWirelessClientWPAStatsEntry 3 }

extremeWirelessClientWPAStatsGroupKeySuccesses OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "Number of successes of the group key exchange"
         ::= { extremeWirelessClientWPAStatsEntry 4 }

extremeWirelessClientWPAStatsGroupKeyFailures OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "Number of failures of the group key handshake"
         ::= { extremeWirelessClientWPAStatsEntry 5 }

extremeWirelessClientWPAStatsPairwiseKey1Sends OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "Number of times the first packet of the pairwise key exchange was sent."
         ::= { extremeWirelessClientWPAStatsEntry 6 }

extremeWirelessClientWPAStatsPairwiseKey3Sends OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "Number of times the third packet of the pairwise key exchange was sent."
         ::= { extremeWirelessClientWPAStatsEntry 7 }

extremeWirelessClientWPAStatsGroupKeySends OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "Number of times the group key packet was sent."
         ::= { extremeWirelessClientWPAStatsEntry 8 }

extremeWirelessClientWPAStatsEAPOLKeyReceivedInPairwise1Key OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "Number of times an EAPOL Key packet was recieved after
        sending the 1st pairwise key exchange packet"
         ::= { extremeWirelessClientWPAStatsEntry 9 }

extremeWirelessClientWPAStatsEAPOLKeyReceivedInPairwise3Key OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "Number of times an EAPOL Key packet was recieved after
        sending the 3rd pairwise key exchange packet"
         ::= { extremeWirelessClientWPAStatsEntry 10 }

extremeWirelessClientWPAStatsEAPOLKeyReceivedInGroupKey OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "Number of times an EAPOL Key packet was recieved after
        sending the group key packet"
         ::= { extremeWirelessClientWPAStatsEntry 11 }

extremeWirelessClientWPAStatsDoubleEAPOLKeyReceived OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "Number of times an EAPOL Key packet was recieved when already
        processing a previous key packet."
         ::= { extremeWirelessClientWPAStatsEntry 12 }

extremeWirelessClientWPAStatsEAPOLKeyIgnores OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "Number of times an EAPOL Key packet was ignored."
         ::= { extremeWirelessClientWPAStatsEntry 13 }

extremeWirelessClientWPAStatsEAPOLKeyErrors OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "Number of times an EAPOL Key packet was errored."
         ::= { extremeWirelessClientWPAStatsEntry 14 }

extremeWirelessClientWPAStatsEAPOLKeyAborts OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "Number of times an EAPOL Key packet caused the WPA state machine to abort."
         ::= { extremeWirelessClientWPAStatsEntry 15 }

extremeWirelessClientWPAStatsEAPOLKeyVerificationSuccesses OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
        "Number of times an EAPOL Key packet was verified correctly."
         ::= { extremeWirelessClientWPAStatsEntry 16 }

END

-- ################################################################################

-- ======================================================================
--      CHANGE LOG
--      6/5/97 - jscano
--      1. Added Revision 1-0-1 to MIB for tracking purposes
--      2. Combined the encaps.mib into the original vlan.mib
--      3. Updated preamble comments to accomodate both vlan and encaps xfaces
--         and added general clarifying comments to MIB.
--
--      10/20/96 - jscano
--      1.      Added vlanSesionLayer type to vlan interface.
--      2.      Added vlanNetBeui type to vlan interface.

--      6/5/97 - Paola Biti
--              1.      No change Official MIB implemented on Switch 9000
--      6/9/97 - Paola Biti
--              1. Received new MIB from John Scano.  New Official MIB for Switch 9000

-- ======================================================================
--
--      Interpretation of the Interface Table for VLAN and encapsulation
--      interfaces:
-- 
--      OBJECT  VALUE/USE
--
--      ifIndex Same interpretation as RFC1573.  A unique value,
--                      greater than zero for each VLAN/Encapsulation interface.
--
--      ifDescr Same interpretation as RFC1573.  A textual string
--                      containing information about the interface.  This
--                      string should include the name of the manufacturer,
--                      the product name, the version of the software, and that
--                      the entry is a vlan or encapsulation interface.
--
--                      Example: "3COM LANPlex 2500, version 8.1, VLAN"
--                      Example: "3COM LANPlex 2500, version 8.1, ENCAPS"
--
--      ifType  propVirtual(53)
--
--      ifMtu           Equivalent to the least common denominator MTU of the
--                      set of ports associated with the VLAN or ENCAPS interface.
--                      For example, if the VLAN contains one ethernet port, then
--                      the value of this object is 1518.  If the VLAN contains
--                      all FDDI ports, the value of this object is 4500.  If
--                      a vlan contains a mix of ethernet and FDDI ports, the
--                      value of this object is 1518.  If there are no ports associated
--                      with the interface, then the ifMtu is zero.
--
--      ifSpeed         The value of this object is zero, as defined by RFC1573
--                      for sub-layers that have no concept of bandwidth.             
--
--      ifPhysAddress   The value of this object is always equal to a null octet
--                      string.
--
--      ifAdminStatus   Always equal to up(1).  SetRequest-PDUs fail.
--
--      ifOperStatus    The value of this object is equal to up(1) if the
--                      ifOperStatus of at least one port in in the set of ports
--                      stacked below the VLAN layer is up(1).  The value of this 
--                      object is down(2) if the ifOperStatus of all ports stacked
--                      below the vlan layer is down(2).  The value of this
--                      object is down(2) if there are no ports stacked below the
--                      the vlan sublayer.
--
--      ifLastChange    Same interpretation as RFC1573.  The value of sysUpTime
--                      at the time the interface entered its current operational
--                      state.  If the current state was entered prior to the 
--                      last re-initialization of the local network management
--                      subsystem, then this object contains a zero value.
--       
--      ifInOctets      These objects  return NO_SUCH_NAME on reads and writes. 
--      ifInUcastPkts   This approach is more desireable than returning zero
--      ifInNUcastPkt   on reads because NMS's cannot differentiate between
--      ifInDiscards    returning a zero for non-support vs returning a real
--      ifInErrors      zero value for the counter.  Inability to distinguish
--      ifInUnknownProtos between these two cases would essentially prevent
--      ifOutOctets     future implementation of these objects, therefore
--      ifOutUcastPkts  NO_SUCH_NAME is returned to indicate no-support.
--      ifOutNUcastPkts Future implementations may choose to return real values
--      ifOutDiscards   for these counters.
--      ifOutDiscards                           "
--      ifOutErrors                             "
--      ifLinkUpDownTrapEnable                  "
--      ifConnectorPresent                      "
--      ifHighSpeed                             "
--      ifName                                  "
--
--      ifOutQLen       Deprecated in RFC1573.  Set to zero if present.
--      ifSpecific      Deprecated in RFC1573.  Set to {0.0} if present. 
--
--      linkUp TRAP     Not supported for the vlan/encaps sublayers
--      linkDown TRAP   Not supported for the vlan/encaps sublayer
--
-- ======================================================================


