   RFC1389-MIB DEFINITIONS ::= BEGIN

   IMPORTS
           Counter, TimeTicks, IpAddress
                   FROM RFC1155-SMI
           mib-2
                   FROM RFC1213-MIB
           OBJECT-TYPE
                   FROM RFC-1212;

   --  RIP-2 Management Information Base

     rip2 OBJECT IDENTIFIER ::= { mib-2 23 }
   -- the RouteTag type represents the contents of the
   -- Route Tag field in the packet header or route entry.

   RouteTag ::= OCTET STRING (SIZE (2))

   -- the Validation type is used for the variable that deletes
   -- an entry from a table, and ALWAYS takes at least these values:

   Validation ::= INTEGER { valid (1), invalid (2) }


   --      The RIP-2 Globals Group.
   --      Implementation of this group is mandatory for systems that
   --           implement RIP-2.

   -- These counters are intended to facilitate debugging quickly
   -- changing routes or failing neighbors

   rip2GlobalGroup OBJECT IDENTIFIER ::= { rip2 1 }


       rip2GlobalRouteChanges OBJECT-TYPE
           SYNTAX   Counter
           ACCESS   read-only
           STATUS   mandatory
           DESCRIPTION
              "The number of changes made to the IP Route Da-
              tabase by RIP."
          ::= { rip2GlobalGroup 1 }


       rip2GlobalQueries OBJECT-TYPE
           SYNTAX   Counter
           ACCESS   read-only
           STATUS   mandatory
           DESCRIPTION
              "The number of responses sent  to  RIP  queries
              from other systems."
          ::= { rip2GlobalGroup 2 }


   --  RIP Interfaces Groups
   --  Implementation of these Groups is mandatory for systems that
   --       implement RIP-2.

   -- Since RIP versions 1 and 2 do not deal with addressless links,
   -- it is assumed that RIP "interfaces" are subnets within a
   -- routing domain.
   -- The RIP Interface Status Table.

       rip2IfStatTable OBJECT-TYPE
           SYNTAX   SEQUENCE OF Rip2IfStatEntry
           ACCESS   not-accessible
           STATUS   mandatory
           DESCRIPTION
              "A  list  of  subnets  which  require  separate
              status monitoring in RIP."
          ::= { rip2 2 }

      rip2IfStatEntry OBJECT-TYPE
          SYNTAX   Rip2IfStatEntry
          ACCESS   not-accessible
          STATUS   mandatory
          DESCRIPTION
             "A Single Routing Domain in a single Subnet."
         INDEX { rip2IfStatAddress }
         ::= { rip2IfStatTable 1 }


       Rip2IfStatEntry ::=
           SEQUENCE {
               rip2IfStatAddress
                   IpAddress,
               rip2IfStatRcvBadPackets
                   Counter,
               rip2IfStatRcvBadRoutes
                   Counter,
               rip2IfStatSentUpdates
                   Counter,
               rip2IfStatStatus
                   Validation
       }

       rip2IfStatAddress OBJECT-TYPE
           SYNTAX   IpAddress
           ACCESS   read-only
           STATUS   mandatory
           DESCRIPTION
              "The IP Address of this system on the indicated
              subnet."
          ::= { rip2IfStatEntry 1 }


       rip2IfStatRcvBadPackets OBJECT-TYPE
           SYNTAX   Counter
           ACCESS   read-only
           STATUS   mandatory
           DESCRIPTION
              "The number of RIP response packets received by
              the  RIP  process  which were subsequently dis-
              carded for any reason (e.g. a version 0 packet,
              or an unknown command type)."
          ::= { rip2IfStatEntry 2 }


       rip2IfStatRcvBadRoutes OBJECT-TYPE
           SYNTAX   Counter
           ACCESS   read-only
           STATUS   mandatory
           DESCRIPTION
              "The number of routes, in  valid  RIP  packets,
              which were ignored for any reason (e.g. unknown
              address family, or invalid metric)."
          ::= { rip2IfStatEntry 3 }


       rip2IfStatSentUpdates OBJECT-TYPE
           SYNTAX   Counter
           ACCESS   read-only
           STATUS   mandatory
           DESCRIPTION
              "The number of triggered RIP  updates  actually
              sent  on  this interface.  This explicitly does
              NOT include full updates  sent  containing  new
              information."
          ::= { rip2IfStatEntry 4 }

       rip2IfStatStatus OBJECT-TYPE
           SYNTAX   Validation
           ACCESS   read-write
           STATUS   mandatory
           DESCRIPTION
              "Writing invalid has  the  effect  of  deleting
              this interface."
          DEFVAL { valid }
          ::= { rip2IfStatEntry 5 }


   -- The RIP Interface Configuration Table.


       rip2IfConfTable OBJECT-TYPE
           SYNTAX   SEQUENCE OF Rip2IfConfEntry
           ACCESS   not-accessible
           STATUS   mandatory
           DESCRIPTION
              "A list of subnets which require separate  con-
              figuration in RIP."
          ::= { rip2 3 }

      rip2IfConfEntry OBJECT-TYPE
          SYNTAX   Rip2IfConfEntry
          ACCESS   not-accessible
          STATUS   mandatory
          DESCRIPTION
             "A Single Routing Domain in a single Subnet."
         INDEX { rip2IfConfAddress }
         ::= { rip2IfConfTable 1 }


       Rip2IfConfEntry ::=
           SEQUENCE {
               rip2IfConfAddress
                   IpAddress,
               rip2IfConfDomain
                   RouteTag,
               rip2IfConfAuthType
                   INTEGER,
               rip2IfConfAuthKey
                   OCTET STRING (SIZE(0..16)),
               rip2IfConfSend
                   INTEGER,
               rip2IfConfReceive
                   INTEGER,
               rip2IfConfDefaultMetric
                   INTEGER,
               rip2IfConfStatus
                   Validation
       }

       rip2IfConfAddress OBJECT-TYPE
           SYNTAX   IpAddress
           ACCESS   read-only
           STATUS   mandatory
           DESCRIPTION
              "The IP Address of this system on the indicated
              subnet."
          ::= { rip2IfConfEntry 1 }


       rip2IfConfDomain OBJECT-TYPE
           SYNTAX   RouteTag
           ACCESS   read-write
           STATUS   mandatory
           DESCRIPTION
              "Value inserted into the Routing  Domain  field
              of all RIP packets sent on this interface."
          DEFVAL { '0000'h }
          ::= { rip2IfConfEntry 2 }


       rip2IfConfAuthType OBJECT-TYPE
           SYNTAX   INTEGER {
                       noAuthentication (1),
                       simplePassword (2)
                    }
           ACCESS   read-write
           STATUS   mandatory
           DESCRIPTION
              "The type of Authentication used on this inter-
              face."
          DEFVAL { noAuthentication }
          ::= { rip2IfConfEntry 3 }


       rip2IfConfAuthKey OBJECT-TYPE
           SYNTAX   OCTET STRING (SIZE(0..16))
           ACCESS   read-write
           STATUS   mandatory
           DESCRIPTION
              "The value to be used as the Authentication Key
              whenever    the   corresponding   instance   of
              rip2IfConfAuthType has  the  value  simplePass-
              word.   A modification of the corresponding in-
              stance of rip2IfConfAuthType  does  not  modify
              the rip2IfConfAuthKey value.

              If a string shorter than 16 octets is supplied,
              it  will be left-justified and padded to 16 oc-
              tets, on the right, with nulls (0x00).

              Reading this object always results in an  OCTET
              STRING  of  length zero; authentication may not
              be bypassed by reading the MIB object."
          DEFVAL { ''h }
          ::= { rip2IfConfEntry 4 }


       rip2IfConfSend OBJECT-TYPE
           SYNTAX   INTEGER {
                       doNotSend (1),
                       ripVersion1 (2),
                       rip1Compatible (3),
                       ripVersion2 (4)
                    }
           ACCESS   read-write
           STATUS   mandatory
           DESCRIPTION
              "What  the  router  sends  on  this  interface.
              ripVersion1 implies sending RIP updates compli-
              ant  with  RFC  1058.   rip1Compatible  implies
              broadcasting RIP-2 updates using RFC 1058 route
              subsumption rules.  ripVersion2 implies  multi-
              casting RIP-2 updates."
          DEFVAL { rip1Compatible }
          ::= { rip2IfConfEntry 5 }


       rip2IfConfReceive OBJECT-TYPE
           SYNTAX   INTEGER {
                       rip1 (1),
                       rip2 (2),
                       rip1OrRip2 (3)
                    }
           ACCESS   read-write
           STATUS   mandatory
           DESCRIPTION
              "This indicates which version  of  RIP  updates
              are   to  be  accepted.   Note  that  rip2  and
              rip1OrRip2 implies reception of multicast pack-
              ets."
          DEFVAL { rip1OrRip2 }
          ::= { rip2IfConfEntry 6 }


       rip2IfConfDefaultMetric OBJECT-TYPE
           SYNTAX   INTEGER ( 0..15 )
           ACCESS   read-write
           STATUS   mandatory
           DESCRIPTION
              "This variable indicates what metric is  to  be
              used  as  a  default  route in RIP updates ori-
              ginated on this interface.  A value of zero in-
              dicates  that  no  default route should be ori-
              ginated; in this  case,  a  default  route  via
              another router may be propagated."
          ::= { rip2IfConfEntry 7 }

       rip2IfConfStatus OBJECT-TYPE
           SYNTAX   Validation
           ACCESS   read-write
           STATUS   mandatory
           DESCRIPTION
              "Writing invalid has  the  effect  of  deleting
              this interface."
          DEFVAL { valid }
          ::= { rip2IfConfEntry 8 }


   --  Peer Table

   --      The RIP Peer Group
   --      Implementation of this Group is Optional

   --      This group provides information about active peer
   --      relationships intended to assist in debugging.

       rip2PeerTable OBJECT-TYPE
           SYNTAX   SEQUENCE OF Rip2PeerEntry
           ACCESS   not-accessible
           STATUS   mandatory
           DESCRIPTION
              "A list of RIP Peers."
          ::= { rip2 4 }

      rip2PeerEntry OBJECT-TYPE
          SYNTAX   Rip2PeerEntry
          ACCESS   not-accessible
          STATUS   mandatory
          DESCRIPTION
             "Information regarding a single routing peer."
         INDEX { rip2PeerAddress, rip2PeerDomain }
         ::= { rip2PeerTable 1 }


       Rip2PeerEntry ::=
           SEQUENCE {
               rip2PeerAddress
                   IpAddress,
               rip2PeerDomain
                   RouteTag,
               rip2PeerLastUpdate
                   TimeTicks,
               rip2PeerVersion
                   INTEGER,
               rip2PeerRcvBadPackets
                   Counter,
               rip2PeerRcvBadRoutes
                   Counter
               }


       rip2PeerAddress OBJECT-TYPE
           SYNTAX   IpAddress
           ACCESS   read-only
           STATUS   mandatory
           DESCRIPTION
              "The IP Address of the Peer System."
          ::= { rip2PeerEntry 1 }


       rip2PeerDomain OBJECT-TYPE
           SYNTAX   RouteTag
           ACCESS   read-only
           STATUS   mandatory
           DESCRIPTION
              "The value in the Routing Domain field  in  RIP
              packets received from the peer."
          ::= { rip2PeerEntry 2 }


       rip2PeerLastUpdate OBJECT-TYPE
           SYNTAX   TimeTicks
           ACCESS   read-only
           STATUS   mandatory
           DESCRIPTION
              "The value of sysUpTime when  the  most  recent
              RIP update was received from this system."
          ::= { rip2PeerEntry 3 }


       rip2PeerVersion OBJECT-TYPE
           SYNTAX   INTEGER ( 0..255 )
           ACCESS   read-only
           STATUS   mandatory
           DESCRIPTION
              "The RIP version number in the  header  of  the
              last RIP packet received."
          ::= { rip2PeerEntry 4 }


       rip2PeerRcvBadPackets OBJECT-TYPE
           SYNTAX   Counter
           ACCESS   read-only
           STATUS   mandatory
           DESCRIPTION
              "The number of RIP response packets  from  this
              peer discarded as invalid."
          ::= { rip2PeerEntry 5 }


       rip2PeerRcvBadRoutes OBJECT-TYPE
           SYNTAX   Counter
           ACCESS   read-only
           STATUS   mandatory
           DESCRIPTION
              "The number of routes from this peer that  were
              ignored because the entry format was invalid."
          ::= { rip2PeerEntry 6 }


   END
