-- ****************************************************************
--   
-- AGENT-CAPABILITIES mib for CISCO-ENTITY-FRU-CONTROL-MIB
--   
-- March 2002, Subra Hegde, Sirisha Paturi
-- August 2003, Wen Xu
-- September 2003, Wen Xu
-- Janurary 2004, Wen Xu
-- September 2004, Jaikumar Chidambaram
-- May 2006, Bala Kanchana
-- March 2008, Purna Ghanta
--   
-- Copyright (c) 2002-2009 by Cisco Systems, Inc.
--   
-- ****************************************************************

CISCO-ENTITY-FRU-CONTROL-CAPABILITY DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY
        FROM SNMPv2-SMI
    AGENT-CAPABILITIES
        FROM SNMPv2-CONF
    ciscoAgentCapability
        FROM CISCO-SMI;


ciscoEntityFruControlCapability MODULE-IDENTITY
    LAST-UPDATED    "200912140000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 W Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-snmp@cisco.com
            cs-lan-switch-snmp@cisco.com"
    DESCRIPTION
        "The Agent Capabilities for CISCO-ENTITY-FRU-CONTROL-MIB."
    REVISION        "200912140000Z"
    DESCRIPTION
        "Added capability ciscoEfcCapV15R01TP39XXE"
    REVISION        "200907300000Z"
    DESCRIPTION
        "Added capabilities for ciscoEfcCapV12R04TP3925E,
        and ciscoEfcCapV12R04TP3945E"
    REVISION        "200903250000Z"
    DESCRIPTION
        "Added capabilities for ciscoEfcCapV12R04TP3845nv,
        ciscoEfcCapV12R04TP3825nv, ciscoEfcCapV12R04TP1941,
        ciscoEfcCapV12R04TP29XX, ciscoEfcCapV12R04TP3925 
        and ciscoEfcCapV12R04TP3945"
    REVISION        "200903110000Z"
    DESCRIPTION
        "The capability statement ciscoEfcCapIOSXRV3R08CRS1
        has been added."
    REVISION        "200810280000Z"
    DESCRIPTION
        "Added capabilities ciscoEfcCapV12R0233SXIPCat6K."
    REVISION        "200803240000Z"
    DESCRIPTION
        "The capability statement ciscoEfcCapIOSXRV3R06CRS1
        has been added."
    REVISION        "200709060000Z"
    DESCRIPTION
        "Added capabilities ciscoEfcCapabilityV12R05TP32xx
        for 3200 platform."
    REVISION        "200708310000Z"
    DESCRIPTION
        "Added capabilities ciscoEfcCapV12R0233SXHPCat6K."
    REVISION        "200707190000Z"
    DESCRIPTION
        "Added capabilities ciscoEfcCapabilityV05R05PMGX8850
        for MGX8850 platform."
    REVISION        "200606210000Z"
    DESCRIPTION
        "- Added capabilities ciscoEfcCapV12R05TP18xx
        and ciscoEfcCapV12R05TP2801 for IOS 12.4T
        on platforms 18xx and 2801."
    REVISION        "200604190000Z"
    DESCRIPTION
        "- Added Agent capabilities
        ciscoEfcCapACSWV03R000 for Cisco
        Application Control Engine (ACE)."
    REVISION        "200603160000Z"
    DESCRIPTION
        "- Add VARIATIONs for notifications
        cefcModuleStatusChange,
        cefcPowerStatusChange,
        cefcFRUInserted and cefcFRURemoved
        in ciscoEfcCapabilityCatOSV08R0101,
        ciscoEfcCapabilityCatOSV08R0301
        and ciscoEfcCapCatOSV08R0501."
    REVISION        "200601310000Z"
    DESCRIPTION
        "- Added ciscoEfcCapSanOSV21R1MDS9000 for
        SAN OS 2.1(1) on MDS 9000 series devices.
        - Added ciscoEfcCapSanOSV30R1MDS9000 for
        SAN OS 3.0(1) on MDS 9000 series devices."
    REVISION        "200507120000Z"
    DESCRIPTION
        "- Added ciscoEfcCapCatOSV08R0501."
    REVISION        "200503090000Z"
    DESCRIPTION
        "- Added capabilities ciscoEfcCapV12R04TP26XX
        ciscoEfcCapV12R04TP28XX, ciscoEfcCapV12R04TP3725,
        ciscoEfcCapV12R04TP3745, ciscoEfcCapV12R04TP3825,
        ciscoEfcCapV12R04TP3845, ciscoEfcCapV12R04TPIAD243X,
        ciscoEfcCapV12R04TPVG224 for IOS 12.4T on platforms
        26xx, 28xx, 37xx, 38xx, IAD243x, VG224"
    REVISION        "200409150000Z"
    DESCRIPTION
        "- Added ciscoEfcCapabilityV12R03P5XXX for IOS 12.3
        on Access Server Platforms (AS5350, AS5400 and
        AS5850)."
    REVISION        "200401150000Z"
    DESCRIPTION
        "- Added ciscoEfcCapV12RO217bSXACat6K.
        - Added ciscoEfcCapabilityCatOSV08R0301."
    REVISION        "200309150000Z"
    DESCRIPTION
        "- Added ciscoEfcCapabilityV12R0119ECat6K for IOS
        12.1(19E) on Catalyst 6000/6500 and Cisco
        7600 series devices.
        - Added ciscoEfcCapabilityV12RO217SXCat6K for IOS
        12.2(17SX) on Catalyst 6000/6500 and Cisco
        7600 series devices.
        - Added ciscoEfcCapabilityCatOSV08R0101 for
        Cisco CatOS 8.1(1)."
    REVISION        "200203200000Z"
    DESCRIPTION
        "Initial version of the MIB Module.
        - The ciscoEntityFruControlCapabilityV2R00 is
          for MGX8850 and BPX SES platform.
        - The ciscoEntityFRUControlCapabilityV12R00SGSR
          is for GSR platform."
    ::= { ciscoAgentCapability 264 }



ciscoEntityFruControlCapabilityV2R00 AGENT-CAPABILITIES
    PRODUCT-RELEASE "MGX8850 Release 2.00,
                          BPX SES Release 1.00"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB Capabilities"

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        { cefcMIBModuleGroup }
    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    ::= { ciscoEntityFruControlCapability 1 }

ciscoEntityFRUControlCapabilityV12R00SGSR AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.0S for GSR"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities
        for GSR platform."

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBModuleGroup,
                        cefcMIBNotificationEnablesGroup,
                        cefcMgmtNotificationsGroup
                    }
    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write not implemented"

    VARIATION       cefcModuleStatusChange
    DESCRIPTION
        "This notification is generated when the value of
        cefcModuleOperStatus changes. It can be utilized by
        an NMS to update the status of the module it is
        managing. The varbind for this notification indicates
        the entPhysicalDescr and entPhysicalName of the
        module, the operational-status of the module and the
        value of sysUpTime at the time the
        cefcModuleOperStatus is changed."

    VARIATION       cefcPowerStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported"

    VARIATION       cefcFRUInserted
    DESCRIPTION
        "The cefcFRUInserted notification indicates that a FRU
        was inserted. The varbind for this notification
        indicates the entPhysicalDescr and entPhysicalName of
        the inserted FRU, and the entPhysicalIndex of the
        FRU's container."

    VARIATION       cefcFRURemoved
    DESCRIPTION
        "The cefcFRURemoved notification indicates that a FRU
        was removed. The varbind for this notification
        indicates the entPhysicalDescr and entPhysicalName of
        the removed FRU, and the entPhysicalIndex of the FRU's
        container."

    ::= { ciscoEntityFruControlCapability 2 }

ciscoEfcCapabilityV12R0119ECat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.1(19E) on Catalyst 6000/6500
                      and Cisco 7600 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities."

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBModuleGroup,
                        cefcMIBNotificationEnablesGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBInLinePowerControlGroup
                    }
    VARIATION       cefcMaxDefaultInLinePower
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    ::= { ciscoEntityFruControlCapability 3 }

ciscoEfcCapabilityV12RO217SXCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(17SX) on Catalyst 6000/6500
                      and Cisco 7600 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities."

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBModuleGroup,
                        cefcMIBNotificationEnablesGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBPowerOperModeGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBInLinePowerControlGroupRev1
                    }
    VARIATION       cefcPowerRedundancyOperMode
    SYNTAX          INTEGER  {
                        redundant(2),
                        combined(3)
                    }
    DESCRIPTION
        "notsupported(1) is not supported."

    VARIATION       cefcMaxDefaultInLinePower
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       cefcMaxDefaultHighInLinePower
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    ::= { ciscoEntityFruControlCapability 4 }

ciscoEfcCapabilityCatOSV08R0101 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco CatOS 8.1(1)."
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities."

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBModuleGroup,
                        cefcMIBNotificationEnablesGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBInLinePowerControlGroup
                    }
    VARIATION       cefcModuleStatusChange
    DESCRIPTION
        "In addition to the regular varbinds, the instance
        values of entPhysicalDescr and entPhysicalName are
        appended to the notification."

    VARIATION       cefcPowerStatusChange
    DESCRIPTION
        "In addition to the regular varbinds, the instance
        values of entPhysicalDescr and entPhysicalName are
        appended to the notification."

    VARIATION       cefcFRUInserted
    DESCRIPTION
        "In addition to the regular varbinds, the instance
        values of entPhysicalDescr and entPhysicalName are
        appended to the notification."

    VARIATION       cefcFRURemoved
    DESCRIPTION
        "In addition to the regular varbinds, the instance
        values of entPhysicalDescr and entPhysicalName are
        appended to the notification."

    ::= { ciscoEntityFruControlCapability 5 }

ciscoEfcCapV12RO217bSXACat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(17b)SXA on Catalyst 6000/6500
                      and Cisco 7600 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities."

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBModuleGroup,
                        cefcMIBNotificationEnablesGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBPowerOperModeGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBInLinePowerControlGroupRev1,
                        cefcIntelliModuleGroup
                    }
    VARIATION       cefcPowerRedundancyOperMode
    SYNTAX          INTEGER  {
                        redundant(2),
                        combined(3)
                    }
    DESCRIPTION
        "notsupported(1) is not supported."

    VARIATION       cefcMaxDefaultInLinePower
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       cefcMaxDefaultHighInLinePower
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    ::= { ciscoEntityFruControlCapability 6 }

ciscoEfcCapabilityCatOSV08R0301 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco CatOS 8.3(1) on Catalyst 6000/6500
                      and Cisco 7600 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities."

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBModuleGroup,
                        cefcMIBNotificationEnablesGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcIntelliModuleGroup
                    }
    VARIATION       cefcModuleStatusChange
    DESCRIPTION
        "In addition to the regular varbinds, the instance
        values of entPhysicalDescr and entPhysicalName are
        appended to the notification."

    VARIATION       cefcPowerStatusChange
    DESCRIPTION
        "In addition to the regular varbinds, the instance
        values of entPhysicalDescr and entPhysicalName are
        appended to the notification."

    VARIATION       cefcFRUInserted
    DESCRIPTION
        "In addition to the regular varbinds, the instance
        values of entPhysicalDescr and entPhysicalName are
        appended to the notification."

    VARIATION       cefcFRURemoved
    DESCRIPTION
        "In addition to the regular varbinds, the instance
        values of entPhysicalDescr and entPhysicalName are
        appended to the notification."

    ::= { ciscoEntityFruControlCapability 7 }

ciscoEfcCapabilityV12R03P5XXX AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.3 for Access Server Platforms
                      AS5350, AS5400 and AS5850."
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities."

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBModuleGroup,
                        cefcMIBNotificationEnablesGroup,
                        cefcMgmtNotificationsGroup
                    }
    VARIATION       cefcFRUPowerAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not suppported."

    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "write access is not suppported."

    ::= { ciscoEntityFruControlCapability 8 }

ciscoEfcCapV12R04TP3725 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.4T for c3725 Platform"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities."

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBModuleGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBInLinePowerControlGroupRev1
                    }
    VARIATION       cefcPowerRedundancyMode
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcPowerUnits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalAvailableCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalDrawnCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerRedundancyOperMode
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1)
                    }
    ACCESS          read-only
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUPowerOperStatus
    SYNTAX          INTEGER  {
                        on(2)
                    }
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcMaxDefaultInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcModuleLastClearConfigTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleResetReasonDescription
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleStateChangeReasonDescr
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleUpTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUInserted
    ACCESS          not-implemented
    DESCRIPTION
        "Online Insertion not supported"

    VARIATION       cefcFRURemoved
    ACCESS          not-implemented
    DESCRIPTION
        "Online Removal not supported"

    VARIATION       cefcMaxDefaultHighInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    ::= { ciscoEntityFruControlCapability 9 }

ciscoEfcCapV12R04TP3745 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.4T for c3745 Platforms"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities"

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBModuleGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBInLinePowerControlGroupRev1
                    }
    VARIATION       cefcPowerRedundancyMode
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcPowerUnits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalAvailableCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalDrawnCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerRedundancyOperMode
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1)
                    }
    ACCESS          read-only
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUPowerOperStatus
    SYNTAX          INTEGER  {
                        on(2)
                    }
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcMaxDefaultInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcModuleLastClearConfigTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleResetReasonDescription
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleStateChangeReasonDescr
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleUpTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcMaxDefaultHighInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    ::= { ciscoEntityFruControlCapability 10 }

ciscoEfcCapV12R04TP26XX AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.4T for c26xx XM Platforms"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities"

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBModuleGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBInLinePowerControlGroupRev1
                    }
    VARIATION       cefcPowerRedundancyMode
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcPowerUnits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalAvailableCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalDrawnCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerRedundancyOperMode
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1)
                    }
    ACCESS          read-only
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUPowerOperStatus
    SYNTAX          INTEGER  {
                        on(2)
                    }
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcMaxDefaultInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcModuleLastClearConfigTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleResetReasonDescription
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleStateChangeReasonDescr
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleUpTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUInserted
    ACCESS          not-implemented
    DESCRIPTION
        "Online Insertion not supported"

    VARIATION       cefcFRURemoved
    ACCESS          not-implemented
    DESCRIPTION
        "Online Removal not supported"

    VARIATION       cefcMaxDefaultHighInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    ::= { ciscoEntityFruControlCapability 11 }

ciscoEfcCapV12R04TPIAD243X AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.4T for IAD 243x Platforms"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities"

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBModuleGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBInLinePowerControlGroupRev1
                    }
    VARIATION       cefcPowerRedundancyMode
    ACCESS          read-only
    DESCRIPTION
        "write access not supported"

    VARIATION       cefcPowerUnits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalAvailableCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalDrawnCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerRedundancyOperMode
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1)
                    }
    ACCESS          read-only
    DESCRIPTION
        "Supports enumeration 'on'"

    VARIATION       cefcFRUPowerOperStatus
    SYNTAX          INTEGER  {
                        on(2)
                    }
    DESCRIPTION
        "Supports enumeration 'on'"

    VARIATION       cefcFRUCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcMaxDefaultInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access not supported"

    VARIATION       cefcModuleStatusLastChangeTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleLastClearConfigTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleResetReasonDescription
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleStateChangeReasonDescr
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleUpTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUInserted
    ACCESS          not-implemented
    DESCRIPTION
        "Online Insertion not supported in
        platform IAD243x"

    VARIATION       cefcFRURemoved
    ACCESS          not-implemented
    DESCRIPTION
        "Online Removal not supported in
        platform IAD243x"

    VARIATION       cefcMaxDefaultHighInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    ::= { ciscoEntityFruControlCapability 12 }

ciscoEfcCapV12R04TPVG224 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.4T for VG224 Platform"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities"

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBModuleGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBInLinePowerControlGroupRev1
                    }
    VARIATION       cefcPowerRedundancyMode
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcPowerUnits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalAvailableCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalDrawnCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerRedundancyOperMode
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1)
                    }
    ACCESS          read-only
    DESCRIPTION
        "Supports enumeration 'on'"

    VARIATION       cefcFRUPowerOperStatus
    SYNTAX          INTEGER  {
                        on(2)
                    }
    DESCRIPTION
        "Supports enumeration 'on'"

    VARIATION       cefcFRUCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcMaxDefaultInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcModuleStatusLastChangeTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleLastClearConfigTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleResetReasonDescription
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleStateChangeReasonDescr
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleUpTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUInserted
    ACCESS          not-implemented
    DESCRIPTION
        "Online Insertion not supported"

    VARIATION       cefcFRURemoved
    ACCESS          not-implemented
    DESCRIPTION
        "Online Removal not supported"

    VARIATION       cefcMaxDefaultHighInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    ::= { ciscoEntityFruControlCapability 13 }

ciscoEfcCapV12R04TP2691 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.4T for c2691 Platform"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities"

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBModuleGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBInLinePowerControlGroupRev1
                    }
    VARIATION       cefcPowerRedundancyMode
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcPowerUnits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalAvailableCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalDrawnCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerRedundancyOperMode
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1)
                    }
    ACCESS          read-only
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUPowerOperStatus
    SYNTAX          INTEGER  {
                        on(2)
                    }
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcMaxDefaultInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcModuleLastClearConfigTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleResetReasonDescription
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleStateChangeReasonDescr
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleUpTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUInserted
    ACCESS          not-implemented
    DESCRIPTION
        "Online Insertion not supported"

    VARIATION       cefcFRURemoved
    ACCESS          not-implemented
    DESCRIPTION
        "Online Removal not supported"

    VARIATION       cefcMaxDefaultHighInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    ::= { ciscoEntityFruControlCapability 14 }

ciscoEfcCapV12R04TP28XX AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.4T for c28xx Platforms"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities"

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBModuleGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBInLinePowerControlGroupRev1
                    }
    VARIATION       cefcPowerRedundancyMode
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcPowerUnits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalAvailableCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalDrawnCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerRedundancyOperMode
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1)
                    }
    ACCESS          read-only
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUPowerOperStatus
    SYNTAX          INTEGER  {
                        on(2)
                    }
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcMaxDefaultInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcModuleLastClearConfigTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleResetReasonDescription
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleStateChangeReasonDescr
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleUpTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUInserted
    ACCESS          not-implemented
    DESCRIPTION
        "Online Insertion not supported"

    VARIATION       cefcFRURemoved
    ACCESS          not-implemented
    DESCRIPTION
        "Online Removal not supported"

    VARIATION       cefcMaxDefaultHighInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    ::= { ciscoEntityFruControlCapability 15 }

ciscoEfcCapV12R04TP3825 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.4T for c3825 Platforms"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities"

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBModuleGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBInLinePowerControlGroupRev1
                    }
    VARIATION       cefcPowerRedundancyMode
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcPowerUnits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalAvailableCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalDrawnCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerRedundancyOperMode
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1)
                    }
    ACCESS          read-only
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUPowerOperStatus
    SYNTAX          INTEGER  {
                        on(2)
                    }
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcMaxDefaultInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcModuleLastClearConfigTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleResetReasonDescription
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleStateChangeReasonDescr
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleUpTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUInserted
    ACCESS          not-implemented
    DESCRIPTION
        "Online Insertion not supported"

    VARIATION       cefcFRURemoved
    ACCESS          not-implemented
    DESCRIPTION
        "Online Removal not supported"

    VARIATION       cefcMaxDefaultHighInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    ::= { ciscoEntityFruControlCapability 16 }

ciscoEfcCapV12R04TP3845 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.4T for c3845 Platform"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities"

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBModuleGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBInLinePowerControlGroupRev1
                    }
    VARIATION       cefcPowerRedundancyMode
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcPowerUnits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalDrawnCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalAvailableCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerRedundancyOperMode
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1)
                    }
    ACCESS          read-only
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUPowerOperStatus
    SYNTAX          INTEGER  {
                        on(2)
                    }
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcMaxDefaultInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcModuleLastClearConfigTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleResetReasonDescription
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleStateChangeReasonDescr
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleUpTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcMaxDefaultHighInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    ::= { ciscoEntityFruControlCapability 17 }

ciscoEfcCapCatOSV08R0501 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco CatOS 8.5(1) on Catalyst 6000/6500
                         and Cisco 7600 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities."

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBModuleGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBNotificationEnablesGroup,
                        cefcMIBNotificationEnablesGroup2,
                        cefcMgmtNotificationsGroup,
                        cefcMgmtNotificationsGroup3,
                        cefcIntelliModuleGroup,
                        cefcPowerCapacityGroup,
                        cefcCoolingGroup,
                        cefcConnectorRatingGroup,
                        cefcMIBInLinePowerControlGroupRev1
                    }
    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1),
                        off(2),
                        inlineAuto(3),
                        reset(5)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        are supported."

    VARIATION       cefcModuleAdminStatus
    SYNTAX          INTEGER  {
                        enabled(1),
                        disabled(2),
                        reset(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        are supported."

    VARIATION       cefcModuleStatusChange
    DESCRIPTION
        "In addition to the regular varbinds, the instance
        values of entPhysicalDescr and entPhysicalName are
        appended to the notification."

    VARIATION       cefcPowerStatusChange
    DESCRIPTION
        "In addition to the regular varbinds, the instance
        values of entPhysicalDescr and entPhysicalName are
        appended to the notification."

    VARIATION       cefcFRUInserted
    DESCRIPTION
        "In addition to the regular varbinds, the instance
        values of entPhysicalDescr and entPhysicalName are
        appended to the notification."

    VARIATION       cefcFRURemoved
    DESCRIPTION
        "In addition to the regular varbinds, the instance
        values of entPhysicalDescr and entPhysicalName are
        appended to the notification."

    ::= { ciscoEntityFruControlCapability 18 }

ciscoEfcCapSanOSV21R1MDS9000 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco SanOS 2.1(1) on Cisco MDS 9000 series
                         devices."
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities."

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBPowerFRUValueGroup,
                        cefcMIBModuleGroup,
                        cefcModuleGroupRev1,
                        cefcMIBNotificationEnablesGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBFanTrayStatusGroup,
                        cefcMIBPhysicalGroup
                    }
    VARIATION       cefcFRUInserted
    DESCRIPTION
        "The cefcFRUInserted notification indicates
        that a FRU was inserted. The varbinds for
        this notification indicate the
        entPhysicalDescr of the inserted FRU and the
        entPhysicalIndex of the FRU's container."

    VARIATION       cefcFRURemoved
    DESCRIPTION
        "The cefcFRURemoved notification indicates
        that a FRU was removed. The varbinds for this
        notification indicate the entPhysicalDescr of
        the removed FRU and the entPhysicalIndex of
        the FRU's container."

    ::= { ciscoEntityFruControlCapability 19 }

ciscoEfcCapSanOSV30R1MDS9000 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco SanOS 3.0(1) on Cisco MDS 9000 series
                         devices."
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities."

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBPowerFRUValueGroup,
                        cefcMIBModuleGroup,
                        cefcModuleGroupRev1,
                        cefcMIBNotificationEnablesGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBFanTrayStatusGroup,
                        cefcMIBPhysicalGroup,
                        cefcMgmtNotificationsGroup2
                    }
    VARIATION       cefcFRUInserted
    DESCRIPTION
        "The cefcFRUInserted notification indicates
        that a FRU was inserted. The varbind for
        this notification indicates the
        entPhysicalIndex of the FRU's container,
        entPhysicalDescr of the inserted FRU and
        the entPhysicalName of the inserted FRU's
        container."

    VARIATION       cefcFRURemoved
    DESCRIPTION
        "The cefcFRURemoved notification indicates
        that a FRU was removed. The varbind for this
        notification indicates the entPhysicalIndex
        of the removed FRU's container, the
        entPhysicalDescr of the removed FRU and
        the entPhysicalName of the removed FRU's
        container."

    ::= { ciscoEntityFruControlCapability 20 }

ciscoEfcCapACSWV03R000 AGENT-CAPABILITIES
    PRODUCT-RELEASE "ACSW (Application Control Software) 3.0"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities."

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBModuleGroup,
                        cefcModuleGroupRev1,
                        cefcModuleExtGroup
                    }
    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Create operation not supported."

    ::= { ciscoEntityFruControlCapability 21 }

ciscoEfcCapV12R05TP18xx AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.5T for c18xx Platform"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities"

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBModuleGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBInLinePowerControlGroupRev1
                    }
    VARIATION       cefcPowerRedundancyMode
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcPowerUnits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalDrawnCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalAvailableCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerRedundancyOperMode
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1)
                    }
    ACCESS          read-only
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUPowerOperStatus
    SYNTAX          INTEGER  {
                        on(2)
                    }
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcMaxDefaultInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcModuleLastClearConfigTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleResetReasonDescription
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleStateChangeReasonDescr
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleUpTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUInserted
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRURemoved
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcMaxDefaultHighInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    ::= { ciscoEntityFruControlCapability 22 }

ciscoEfcCapV12R05TP2801 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.5T for c2801 Platform"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities"

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBModuleGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBInLinePowerControlGroupRev1
                    }
    VARIATION       cefcPowerRedundancyMode
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcPowerUnits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalDrawnCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalAvailableCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerRedundancyOperMode
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1)
                    }
    ACCESS          read-only
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUPowerOperStatus
    SYNTAX          INTEGER  {
                        on(2)
                    }
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcMaxDefaultInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcModuleLastClearConfigTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleResetReasonDescription
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleStateChangeReasonDescr
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleUpTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUInserted
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRURemoved
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcMaxDefaultHighInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    ::= { ciscoEntityFruControlCapability 23 }

ciscoEfcCapabilityV05R05PMGX8850 AGENT-CAPABILITIES
    PRODUCT-RELEASE "MGX8850 Release 5.5"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB Capabilities for the following modules of MGX8850:
        AXSM-XG, MPSM-T3E3-155, MPSM-16-T1E1, PXM1E, PXM45, VXSM and VISM."

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBModuleGroup,
                        cefcModuleExtGroup
                    }
    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported.
        Not supported for the following modules: AXSM-XG,
        MPSM-T3E3-155, MPSM-16-T1E1, VXSM and VISM."

    VARIATION       cefcModuleOperStatus
    DESCRIPTION
        "Not supported for the following modules: AXSM-XG,
        MPSM-T3E3-155, MPSM-16-T1E1, VXSM and VISM."

    VARIATION       cefcModuleResetReason
    DESCRIPTION
        "Not supported for the following modules: AXSM-XG,
        MPSM-T3E3-155, MPSM-16-T1E1, VXSM and VISM."

    VARIATION       cefcModuleStatusLastChangeTime
    DESCRIPTION
        "Not supported for the following modules: AXSM-XG,
        MPSM-T3E3-155, MPSM-16-T1E1, VXSM and VISM."

    VARIATION       cefcModuleStateChangeReasonDescr
    ACCESS          not-implemented
    DESCRIPTION
        "Not Supported"

    ::= { ciscoEntityFruControlCapability 24 }

ciscoEfcCapV12R0233SXHPCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(33)SXH on Catalyst 6000/6500
                    series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities."

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBModuleGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBNotificationEnablesGroup,
                        cefcMIBNotificationEnablesGroup2,
                        cefcMgmtNotificationsGroup,
                        cefcMgmtNotificationsGroup3,
                        cefcMIBPowerOperModeGroup,
                        cefcIntelliModuleGroup,
                        cefcPowerCapacityGroup,
                        cefcCoolingGroup,
                        cefcConnectorRatingGroup,
                        cefcMIBInLinePowerControlGroupRev1
                    }
    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1),
                        off(2),
                        inlineAuto(3),
                        powerCycle(5)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        are supported.
        The 'on' value can only be supported for
        ENTITY-MIB entPhysicalTable entries which
        have an entPhysicalClass of 'module',
        'powerSupply' or 'fan'.
        The 'off' value can only be supported for
        ENTITY-MIB entPhysicalTable entries which
        have an entPhysicalClass of 'module' or
        'port'.
        The 'powerCycle' value can only be supported
        for certain ENTITY-MIB entPhysicalTable
        entries which have an entPhysicalClass of
        'powerSupply' and support the power cycle
        feature.
        The 'inlineAuto' value can only be supported
        for ENTITY-MIB entPhysicalTable entries which
        have an entPhysicalClass of 'port'."

    VARIATION       cefcModuleAdminStatus
    SYNTAX          INTEGER  {
                        enabled(1),
                        reset(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        are supported."

    VARIATION       cefcPowerRedundancyMode
    SYNTAX          INTEGER  {
                        redundant(2),
                        combined(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        are supported."

    VARIATION       cefcMaxDefaultHighInLinePower
    DESCRIPTION
        "Modification to the value is not
        supported."

    VARIATION       cefcMaxDefaultInLinePower
    DESCRIPTION
        "Modification to the value is not
        supported."

    VARIATION       cefcModuleStatusChange
    DESCRIPTION
        "In addition to the regular varbinds,
        the instance values of entPhysicalDescr
        and entPhysicalName are appended to the
        notification."

    VARIATION       cefcPowerStatusChange
    DESCRIPTION
        "In addition to the regular varbinds,
        the instance values of entPhysicalDescr
        and entPhysicalName are appended to the
        notification."

    VARIATION       cefcFRUInserted
    DESCRIPTION
        "In addition to the regular varbinds,
        the instance values of entPhysicalDescr
        and entPhysicalName are appended to the
        notification."

    VARIATION       cefcFRURemoved
    DESCRIPTION
        "In addition to the regular varbinds,
        the instance values of entPhysicalDescr
        and entPhysicalName are appended to the
        notification."

    ::= { ciscoEntityFruControlCapability 25 }

ciscoEfcCapabilityV12R05TP32xx AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.5T for Cisco 3200 series routers"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities  for 3220, 3250
        and 3270 routers."

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBModuleGroup,
                        cefcMIBNotificationEnablesGroup
                    }
    VARIATION       cefcFRUPowerAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       cefcFRUCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    ::= { ciscoEntityFruControlCapability 26 }

ciscoEfcCapIOSXRV3R06CRS1 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS-XR Release 3.6 for CRS-1."
    STATUS          current
    DESCRIPTION
        "Agent capabilities for IOS-XR
        Release 3.6 for CRS-1."

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMgmtNotificationsGroup2,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBModuleGroup,
                        cefcModuleExtGroup,
                        cefcMIBFanTrayStatusGroup
                    }
    VARIATION       cefcPowerRedundancyMode
    SYNTAX          INTEGER  {
                        notsupported(1)
                    }
    ACCESS          read-only
    DESCRIPTION
        "This implementation doesn't support write operations
        on this object. The following values are not supported.
        redundant(2),
        combined(3),
        nonRedundant(4),
        psRedundant(5),
        inPwrSrcRedundant(6)"

    VARIATION       cefcTotalDrawnCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported."

    VARIATION       cefcModuleStatusChange
    DESCRIPTION
        "In addition to the regular varbinds, the instance
        values of entPhysicalDescr and entPhysicalName are
        appended to the notification."

    VARIATION       cefcPowerStatusChange
    DESCRIPTION
        "In addition to the regular varbinds, the instance
        values of entPhysicalDescr and entPhysicalName are
        appended to the notification."

    VARIATION       cefcFRUInserted
    DESCRIPTION
        "In addition to the regular varbinds, the instance
        values of entPhysicalDescr and entPhysicalName are
        appended to the notification."

    VARIATION       cefcFRURemoved
    DESCRIPTION
        "In addition to the regular varbinds, the instance
        values of entPhysicalDescr and entPhysicalName are
        appended to the notification."

    VARIATION       cefcUnrecognizedFRU
    ACCESS          not-implemented
    DESCRIPTION
        "This notification is not supported."

    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1),
                        off(2)
                    }
    ACCESS          read-only
    DESCRIPTION
        "This implementation doesn't support write operations
        on this object. The following values are not supported.
        inlineAuto(3),
        inlineOn(4),
        powerCycle(5)"

    VARIATION       cefcFRUPowerOperStatus
    SYNTAX          INTEGER  {
                        offEnvOther(1),
                        on(2),
                        offAdmin(3)
                    }
    DESCRIPTION
        "The following values are not supported.
        offDenied(4),
        offEnvPower(5),
        offEnvTemp(6),
        offEnvFan(7),
        failed(8),
        onButFanFail(9),
        offCooling(10),
        offConnectorRating(11),
        onButInlinePowerFail(12)"

    VARIATION       cefcModuleAdminStatus
    SYNTAX          INTEGER  {
                        enabled(1),
                        disabled(2)
                    }
    ACCESS          read-only
    DESCRIPTION
        "This implementation doesn't support write operations
        on this object. The following values are not supported.
        reset(3),
        outOfServiceAdmin(4)"

    VARIATION       cefcModuleOperStatus
    SYNTAX          INTEGER  {
                        unknown(1),
                        ok(2),
                        disabled(3),
                        boot(5),
                        failed(7),
                        missing(8),
                        mismatchConfig(10),
                        diagFailed(11),
                        outOfServiceAdmin(13)
                    }
    DESCRIPTION
        "The following values are not supported.
        okButDiagFailed(4),
        selfTest(6),
        mismatchWithParent(9),
        dormant(12),
        outOfServiceEnvTemp(14),
        poweredDown(15),
        poweredUp(16),
        powerDenied(17),
        powerCycled(18),
        okButPowerOverWarning(19),
        okButPowerOverCritical(20),
        syncInProgress(21)"

    VARIATION       cefcModuleResetReason
    SYNTAX          INTEGER  {
                        unknown(1),
                        powerUp(2),
                        manualReset(5)
                    }
    DESCRIPTION
        "The following values are not supported.
        parityError(3),
        clearConfigReset(4),
        watchDogTimeoutReset(6),
        resourceOverflowReset(7),
        missingTaskReset(8),
        lowVoltageReset(9),
        controllerReset(10),
        systemReset(11),
        switchoverReset(12),
        upgradeReset(13),
        downgradeReset(14),
        cacheErrorReset(15),
        deviceDriverReset(16),
        softwareExceptionReset(17),
        restoreConfigReset(18),
        abortRevReset(19),
        burnBootReset(20),
        standbyCdHealthierReset(21),
        nonNativeConfigClearReset(22),
        memoryProtectionErrorReset(23)"

    VARIATION       cefcModuleStateChangeReasonDescr
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported."

    VARIATION       cefcFanTrayOperStatus
    SYNTAX          INTEGER  {
                        up(2)
                    }
    DESCRIPTION
        "The following values are not supported.
        unknown(1),
        down(3),
        warning(4)"

    ::= { ciscoEntityFruControlCapability 27 }

ciscoEfcCapV12R0233SXIPCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(33)SXI on Catalyst 6000/6500
                    series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities."

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBModuleGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBNotificationEnablesGroup,
                        cefcMIBNotificationEnablesGroup2,
                        cefcMgmtNotificationsGroup,
                        cefcMgmtNotificationsGroup3,
                        cefcMIBPowerOperModeGroup,
                        cefcIntelliModuleGroup,
                        cefcPowerCapacityGroup,
                        cefcCoolingGroup,
                        cefcConnectorRatingGroup,
                        cefcMIBInLinePowerControlGroupRev1,
                        cefcMIBInLinePowerCurrentGroup,
                        cefcMIBPowerRedundancyInfoGroup,
                        cefcFanCoolingCapGroup
                    }
    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1),
                        off(2),
                        inlineAuto(3),
                        powerCycle(5)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        are supported.
        The 'on' value can only be supported for
        ENTITY-MIB entPhysicalTable entries which
        have an entPhysicalClass of 'module',
        'powerSupply' or 'fan'.
        The 'off' value can only be supported for
        ENTITY-MIB entPhysicalTable entries which
        have an entPhysicalClass of 'module' or
        'port'.
        The 'powerCycle' value can only be supported
        for certain ENTITY-MIB entPhysicalTable
        entries which have an entPhysicalClass of
        'powerSupply' and support the power cycle
        feature.
        The 'inlineAuto' value can only be supported
        for ENTITY-MIB entPhysicalTable entries which
        have an entPhysicalClass of 'port'."

    VARIATION       cefcModuleAdminStatus
    SYNTAX          INTEGER  {
                        enabled(1),
                        disabled(2),
                        reset(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        are supported."

    VARIATION       cefcPowerRedundancyMode
    SYNTAX          INTEGER  {
                        redundant(2),
                        combined(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        are supported."

    VARIATION       cefcMaxDefaultHighInLinePower
    DESCRIPTION
        "Modification to the value is not
        supported."

    VARIATION       cefcMaxDefaultInLinePower
    DESCRIPTION
        "Modification to the value is not
        supported."

    VARIATION       cefcModuleStatusChange
    DESCRIPTION
        "In addition to the regular varbinds,
        the instance values of entPhysicalDescr
        and entPhysicalName are appended to the
        notification."

    VARIATION       cefcPowerStatusChange
    DESCRIPTION
        "In addition to the regular varbinds,
        the instance values of entPhysicalDescr
        and entPhysicalName are appended to the
        notification."

    VARIATION       cefcFRUInserted
    DESCRIPTION
        "In addition to the regular varbinds,
        the instance values of entPhysicalDescr
        and entPhysicalName are appended to the
        notification."

    VARIATION       cefcFRURemoved
    DESCRIPTION
        "In addition to the regular varbinds,
        the instance values of entPhysicalDescr
        and entPhysicalName are appended to the
        notification."

    ::= { ciscoEntityFruControlCapability 28 }

ciscoEfcCapIOSXRV3R08CRS1 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS-XR Release 3.8 for CRS-1."
    STATUS          current
    DESCRIPTION
        "Agent capabilities for IOS-XR
        Release 3.8 for CRS-1."

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMgmtNotificationsGroup2,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBModuleGroup,
                        cefcModuleExtGroup,
                        cefcMIBFanTrayStatusGroup,
                        cefcMIBPhysicalGroup
                    }
    VARIATION       cefcPowerRedundancyMode
    SYNTAX          INTEGER  {
                        notsupported(1)
                    }
    ACCESS          read-only
    DESCRIPTION
        "This implementation doesn't support write operations
        on this object. The following values are not supported.
        redundant(2),
        combined(3),
        nonRedundant(4),
        psRedundant(5),
        inPwrSrcRedundant(6)"

    VARIATION       cefcTotalDrawnCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported."

    VARIATION       cefcModuleStatusChange
    DESCRIPTION
        "In addition to the regular varbinds, the instance
        values of entPhysicalDescr and entPhysicalName are
        appended to the notification."

    VARIATION       cefcPowerStatusChange
    DESCRIPTION
        "In addition to the regular varbinds, the instance
        values of entPhysicalDescr and entPhysicalName are
        appended to the notification."

    VARIATION       cefcFRUInserted
    DESCRIPTION
        "In addition to the regular varbinds, the instance
        values of entPhysicalDescr and entPhysicalName are
        appended to the notification."

    VARIATION       cefcFRURemoved
    DESCRIPTION
        "In addition to the regular varbinds, the instance
        values of entPhysicalDescr and entPhysicalName are
        appended to the notification."

    VARIATION       cefcUnrecognizedFRU
    DESCRIPTION
        "This implementation does not support the following varbinds.
        entPhysicalVendorType
        entPhysicalModelName"

    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1),
                        off(2)
                    }
    ACCESS          read-only
    DESCRIPTION
        "This implementation doesn't support write operations
        on this object. The following values are not supported.
        inlineAuto(3),
        inlineOn(4),
        powerCycle(5)"

    VARIATION       cefcFRUPowerOperStatus
    SYNTAX          INTEGER  {
                        offEnvOther(1),
                        on(2),
                        offAdmin(3)
                    }
    DESCRIPTION
        "The following values are not supported.
        offDenied(4),
        offEnvPower(5),
        offEnvTemp(6),
        offEnvFan(7),
        failed(8),
        onButFanFail(9),
        offCooling(10),
        offConnectorRating(11),
        onButInlinePowerFail(12)"

    VARIATION       cefcModuleAdminStatus
    SYNTAX          INTEGER  {
                        enabled(1),
                        disabled(2)
                    }
    ACCESS          read-only
    DESCRIPTION
        "This implementation doesn't support write operations
        on this object. The following values are not supported.
        reset(3),
        outOfServiceAdmin(4)"

    VARIATION       cefcModuleOperStatus
    SYNTAX          INTEGER  {
                        unknown(1),
                        ok(2),
                        disabled(3),
                        boot(5),
                        failed(7),
                        missing(8),
                        mismatchConfig(10),
                        diagFailed(11),
                        outOfServiceAdmin(13)
                    }
    DESCRIPTION
        "The following values are not supported.
        okButDiagFailed(4),
        selfTest(6),
        mismatchWithParent(9),
        dormant(12),
        outOfServiceEnvTemp(14),
        poweredDown(15),
        poweredUp(16),
        powerDenied(17),
        powerCycled(18),
        okButPowerOverWarning(19),
        okButPowerOverCritical(20),
        syncInProgress(21)"

    VARIATION       cefcModuleResetReason
    SYNTAX          INTEGER  {
                        unknown(1),
                        powerUp(2),
                        manualReset(5)
                    }
    DESCRIPTION
        "The following values are not supported.
        parityError(3),
        clearConfigReset(4),
        watchDogTimeoutReset(6),
        resourceOverflowReset(7),
        missingTaskReset(8),
        lowVoltageReset(9),
        controllerReset(10),
        systemReset(11),
        switchoverReset(12),
        upgradeReset(13),
        downgradeReset(14),
        cacheErrorReset(15),
        deviceDriverReset(16),
        softwareExceptionReset(17),
        restoreConfigReset(18),
        abortRevReset(19),
        burnBootReset(20),
        standbyCdHealthierReset(21),
        nonNativeConfigClearReset(22),
        memoryProtectionErrorReset(23)"

    VARIATION       cefcModuleStateChangeReasonDescr
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported."

    VARIATION       cefcFanTrayOperStatus
    SYNTAX          INTEGER  {
                        up(2)
                    }
    DESCRIPTION
        "The following values are not supported.
        unknown(1),
        down(3),
        warning(4)"

    VARIATION       cefcPhysicalStatus
    SYNTAX          INTEGER  {
                        supported(2),
                        unsupported(3)
                    }
    DESCRIPTION
        "The following values are not supported.
        other(1),
        incompatible(4)"

    ::= { ciscoEntityFruControlCapability 29 }

ciscoEfcCapV12R04TP3845nv AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.4(22)YB1 for c3845nv Platform"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities"

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBModuleGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBInLinePowerControlGroupRev1
                    }
    VARIATION       cefcPowerRedundancyMode
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcPowerUnits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalDrawnCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalAvailableCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerRedundancyOperMode
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1)
                    }
    ACCESS          read-only
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUPowerOperStatus
    SYNTAX          INTEGER  {
                        on(2)
                    }
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcMaxDefaultInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcModuleLastClearConfigTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleResetReasonDescription
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleStateChangeReasonDescr
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleUpTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcMaxDefaultHighInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    ::= { ciscoEntityFruControlCapability 30 }

ciscoEfcCapV12R04TP3825nv AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.4(22)YB1 for c3825nv Platforms"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities"

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBModuleGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBInLinePowerControlGroupRev1
                    }
    VARIATION       cefcPowerRedundancyMode
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcPowerUnits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalAvailableCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalDrawnCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerRedundancyOperMode
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1)
                    }
    ACCESS          read-only
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUPowerOperStatus
    SYNTAX          INTEGER  {
                        on(2)
                    }
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcMaxDefaultInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcModuleLastClearConfigTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleResetReasonDescription
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleStateChangeReasonDescr
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleUpTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUInserted
    ACCESS          not-implemented
    DESCRIPTION
        "Online Insertion not supported"

    VARIATION       cefcFRURemoved
    ACCESS          not-implemented
    DESCRIPTION
        "Online Removal not supported"

    VARIATION       cefcMaxDefaultHighInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    ::= { ciscoEntityFruControlCapability 31 }

ciscoEfcCapV12R04TP1941 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.4T for c1941 Platform"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities"

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBModuleGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBInLinePowerControlGroupRev1
                    }
    VARIATION       cefcPowerRedundancyMode
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcPowerUnits
    ACCESS          read-only
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalAvailableCurrent
    ACCESS          read-only
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalDrawnCurrent
    ACCESS          read-only
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerRedundancyOperMode
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1)
                    }
    ACCESS          read-only
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUPowerOperStatus
    SYNTAX          INTEGER  {
                        on(2)
                    }
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUCurrent
    ACCESS          read-only
    DESCRIPTION
        "Not available for the ehwic slots"

    VARIATION       cefcMaxDefaultInLinePower
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcFRUTotalSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcModuleLastClearConfigTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleResetReasonDescription
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleStateChangeReasonDescr
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleUpTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUInserted
    ACCESS          not-implemented
    DESCRIPTION
        "Online Insertion not supported"

    VARIATION       cefcFRURemoved
    ACCESS          not-implemented
    DESCRIPTION
        "Online Removal not supported"

    VARIATION       cefcMaxDefaultHighInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    ::= { ciscoEntityFruControlCapability 32 }

ciscoEfcCapV12R04TP29XX AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.4T for c29xx Platforms"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities"

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBModuleGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBInLinePowerControlGroupRev1
                    }
    VARIATION       cefcPowerRedundancyMode
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcPowerUnits
    ACCESS          read-only
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalAvailableCurrent
    ACCESS          read-only
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalDrawnCurrent
    ACCESS          read-only
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerRedundancyOperMode
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1)
                    }
    ACCESS          read-only
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUPowerOperStatus
    SYNTAX          INTEGER  {
                        on(2)
                    }
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUCurrent
    ACCESS          read-only
    DESCRIPTION
        "Not available for the ehwic slots"

    VARIATION       cefcMaxDefaultInLinePower
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcFRUTotalSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcModuleLastClearConfigTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleResetReasonDescription
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleStateChangeReasonDescr
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleUpTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUInserted
    ACCESS          not-implemented
    DESCRIPTION
        "Online Insertion not supported"

    VARIATION       cefcFRURemoved
    ACCESS          not-implemented
    DESCRIPTION
        "Online Removal not supported"

    VARIATION       cefcMaxDefaultHighInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    ::= { ciscoEntityFruControlCapability 33 }

ciscoEfcCapV12R04TP3925 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.4T for c3925 Platforms"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities"

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBModuleGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBInLinePowerControlGroupRev1
                    }
    VARIATION       cefcPowerRedundancyMode
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcPowerUnits
    ACCESS          read-only
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalAvailableCurrent
    ACCESS          read-only
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalDrawnCurrent
    ACCESS          read-only
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerRedundancyOperMode
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1)
                    }
    ACCESS          read-only
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUPowerOperStatus
    SYNTAX          INTEGER  {
                        on(2)
                    }
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUCurrent
    ACCESS          read-only
    DESCRIPTION
        "Not available for the ehwic slots"

    VARIATION       cefcMaxDefaultInLinePower
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcFRUTotalSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcModuleLastClearConfigTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleResetReasonDescription
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleStateChangeReasonDescr
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleUpTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUInserted
    ACCESS          not-implemented
    DESCRIPTION
        "Online Insertion not supported"

    VARIATION       cefcFRURemoved
    ACCESS          not-implemented
    DESCRIPTION
        "Online Removal not supported"

    VARIATION       cefcMaxDefaultHighInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    ::= { ciscoEntityFruControlCapability 34 }

ciscoEfcCapV12R04TP3945 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.4T for c3945 Platform"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities"

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBModuleGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBInLinePowerControlGroupRev1
                    }
    VARIATION       cefcPowerRedundancyMode
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcPowerUnits
    ACCESS          read-only
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalDrawnCurrent
    ACCESS          read-only
    DESCRIPTION
        "Information not available"

    VARIATION       cefcTotalAvailableCurrent
    ACCESS          read-only
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerRedundancyOperMode
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1)
                    }
    ACCESS          read-only
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUPowerOperStatus
    SYNTAX          INTEGER  {
                        on(2)
                    }
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUCurrent
    ACCESS          read-only
    DESCRIPTION
        "Not available for the ehwic slots"

    VARIATION       cefcMaxDefaultInLinePower
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcFRUTotalSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcModuleLastClearConfigTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleResetReasonDescription
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleStateChangeReasonDescr
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleUpTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcMaxDefaultHighInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    ::= { ciscoEntityFruControlCapability 35 }

ciscoEfcCapV15R01TP39XXE AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 15.1T for c3925SPE200/c3925SPE250
                      c3945SPE200/c3945SPE250 Platforms"
    STATUS          current
    DESCRIPTION
        "CISCO-ENTITY-FRU-CONTROL-MIB capabilities"

    SUPPORTS        CISCO-ENTITY-FRU-CONTROL-MIB
    INCLUDES        {
                        cefcMIBPowerModeGroup,
                        cefcMIBPowerFRUControlGroup,
                        cefcMIBInLinePowerControlGroup,
                        cefcMIBModuleGroup,
                        cefcMgmtNotificationsGroup,
                        cefcMIBInLinePowerControlGroupRev1
                    }
    VARIATION       cefcPowerRedundancyMode
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcPowerRedundancyOperMode
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUPowerAdminStatus
    SYNTAX          INTEGER  {
                        on(1)
                    }
    ACCESS          read-only
    DESCRIPTION
        "Supports only enumeration 'on' and write access is not supported"

    VARIATION       cefcFRUPowerOperStatus
    SYNTAX          INTEGER  {
                        on(2)
                    }
    DESCRIPTION
        "Supports only enumeration 'on'"

    VARIATION       cefcFRUCurrent
    ACCESS          read-only
    DESCRIPTION
        "Not available for the ehwic slots"

    VARIATION       cefcMaxDefaultInLinePower
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcFRUTotalSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnSystemCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUTotalInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcFRUDrawnInlineCurrent
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleAdminStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    VARIATION       cefcModuleLastClearConfigTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleResetReasonDescription
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleStateChangeReasonDescr
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcModuleUpTime
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcPowerStatusChange
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    VARIATION       cefcMaxDefaultHighInLinePower
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available"

    ::= { ciscoEntityFruControlCapability 36 }

END



