LanMgr-Alerts-II-MIB DEFINITIONS ::= BEGIN

          --
          -- Notes:
          --
          --   This MIB is documented in "LAN Manager 2.0 Management 
          --   Information Base - Alerts, LAN Manager MIB Working Group, 
          --   Internet Draft: LanMgr-Alerts-II" by Microsoft.
          --
          --   This MIB module description file was derived from the OS/2 
          --   LAN Manager SNMP MIB.  It has been seperated into its two 
          --   distinct parts and some general corrections have been made.
          --

          IMPORTS
                  enterprises, OBJECT-TYPE, Counter, Gauge
                          FROM RFC1155-SMI
                  lanmanager
                          FROM LanMgr-Mib-II-MIB ;

    alerts-2    OBJECT IDENTIFIER ::= { lanmanager 2 }

-- Alert Tree

    alerts           OBJECT IDENTIFIER ::= { alerts-2 1 }
    alert-conditions OBJECT IDENTIFIER ::= { alerts-2 2 }
    alert-mgmt       OBJECT IDENTIFIER ::= { alerts-2 3 }

    bytesAvailData   OBJECT IDENTIFIER ::= { alert-conditions 1 }
    netIOErrorsData  OBJECT IDENTIFIER ::= { alert-conditions 2 }
    serverErrorsData OBJECT IDENTIFIER ::= { alert-conditions 3 }
    pwViolationsData OBJECT IDENTIFIER ::= { alert-conditions 4 }
    accessViolatData OBJECT IDENTIFIER ::= { alert-conditions 5 }
    pdcFailData      OBJECT IDENTIFIER ::= { alert-conditions 6 }
    rplFailData      OBJECT IDENTIFIER ::= { alert-conditions 7 }
    diskData         OBJECT IDENTIFIER ::= { alert-conditions 8 }
    auditLogData     OBJECT IDENTIFIER ::= { alert-conditions 9 }
    powerData        OBJECT IDENTIFIER ::= { alert-conditions 10 }


    -- Alert Data Group

    primaryDCName OBJECT-TYPE 
    SYNTAX  DisplayString (size (1..15))
    ACCESS read-only
    STATUS mandatory
    ::= { pdcFailData 1 }

    primaryDCFailed OBJECT-TYPE 
    SYNTAX 
            INTEGER {
                pdc-Status-OK(1),
                pdc-Status-Failed(2)
            }
    ACCESS read-only
    STATUS mandatory
    ::= { pdcFailData 2 }

    replMasterName OBJECT-TYPE 
    SYNTAX  DisplayString (size (1..15))
    ACCESS read-only
    STATUS mandatory
    ::= { rplFailData 1 }

    replMasterFailed OBJECT-TYPE 
    SYNTAX 
            INTEGER {
                rpl-Status-OK(1),
                rpl-Status-Failed(2),
                rpl-Status-Unknown(3)
            }
    ACCESS read-only
    STATUS mandatory
    ::= { rplFailData 2 }

    netIOAlertLevel OBJECT-TYPE 
    SYNTAX INTEGER
    ACCESS read-write
    STATUS mandatory
    ::= { netIOErrorsData 1 }

    numNetIOErrors OBJECT-TYPE 
    SYNTAX INTEGER
    ACCESS not-accessible
    STATUS mandatory
    ::= { netIOErrorsData 2 }

    networkId OBJECT-TYPE 
    SYNTAX INTEGER
    ACCESS not-accessible
    STATUS mandatory
    ::= { netIOErrorsData 3 }

    netIOErrorStatus OBJECT-TYPE 
    SYNTAX 
            INTEGER {
                ioError-Status-OK(1),
                ioError-Status-Alert(2)
            }
    ACCESS read-only
    STATUS mandatory
    ::= {  netIOErrorsData 4 }

    serverErrorAlertLevel OBJECT-TYPE 
    SYNTAX INTEGER
    ACCESS read-write
    STATUS mandatory
    ::= { serverErrorsData 1 }

    numServerErrors OBJECT-TYPE 
    SYNTAX INTEGER
    ACCESS not-accessible
    STATUS mandatory
    ::= { serverErrorsData 2 }

    serverErrorStatus OBJECT-TYPE 
    SYNTAX 
            INTEGER {
                svError-Status-OK(1),
                svError-Status-Alert(2)
            }
    ACCESS read-only
    STATUS mandatory
    ::= {  serverErrorsData 3  }

    pwLogonAlertLevel  OBJECT-TYPE 
    SYNTAX INTEGER
    ACCESS read-write
    STATUS mandatory
    ::= { pwViolationsData 1 }

    numPWViolations OBJECT-TYPE 
    SYNTAX INTEGER
    ACCESS not-accessible
    STATUS mandatory
    ::= { pwViolationsData 2 }

    passwordErrorStatus OBJECT-TYPE 
    SYNTAX 
            INTEGER {
                pwError-Status-OK(1),
                pwError-Status-Alert(2)
            }
    ACCESS read-only
    STATUS mandatory
    ::= { pwViolationsData 3  }

    accessAlertLevel  OBJECT-TYPE 
    SYNTAX INTEGER
    ACCESS read-write
    STATUS mandatory
    ::= { accessViolatData 1 }

    numAccessViolations OBJECT-TYPE    
    SYNTAX INTEGER
    ACCESS not-accessible
    STATUS mandatory
    ::= { accessViolatData 2 }

    accessErrorStatus OBJECT-TYPE 
    SYNTAX 
            INTEGER {
                pwError-Status-OK(1),
                pwError-Status-Alert(2)
            }
    ACCESS read-only
    STATUS mandatory
    ::= { accessViolatData 3 }

    numDiskDrives  OBJECT-TYPE 
    SYNTAX INTEGER
    ACCESS read-only
    STATUS mandatory
    ::= { bytesAvailData 1 }

    bytesAvailTable  OBJECT-TYPE 
    SYNTAX SEQUENCE OF BytesAvailEntry
    ACCESS read-only
    STATUS mandatory
    ::= { bytesAvailData 2 }

    bytesAvailEntry  OBJECT-TYPE 
    SYNTAX BytesAvailEntry
    ACCESS read-only
    STATUS mandatory
    INDEX  { diskDrive }
    ::= { bytesAvailTable 1 }

    BytesAvailEntry  ::= SEQUENCE {
                         diskDrive        
                             DisplayString,
                         bytesAvail       
                             Gauge
                         }

    diskDrive  OBJECT-TYPE
--ERROR    SYNTAX  DisplayString (size (1..20)
    SYNTAX  DisplayString (size (1..20))
    ACCESS read-only
    STATUS mandatory
    ::= { bytesAvailEntry 1 }

    bytesAvail  OBJECT-TYPE 
    SYNTAX Gauge
    ACCESS read-only
    STATUS mandatory
    ::= { bytesAvailEntry 2 }

    diskAlertLevel  OBJECT-TYPE 
    SYNTAX INTEGER
    ACCESS read-write
    STATUS mandatory
    ::= { bytesAvailData 3 }

    diskHotFixes  OBJECT-TYPE 
    SYNTAX Counter
    ACCESS read-write
    STATUS mandatory
    ::= { diskData 1 }

    diskHardErrors  OBJECT-TYPE 
    SYNTAX Counter
    ACCESS read-write
    STATUS mandatory
    ::= { diskData 2 }

    auditLogStatus  OBJECT-TYPE 
    SYNTAX 
            INTEGER {
                audit-log-OK(1),
                audit-log-80(2),
                audit-log-Full(3)
            }
    ACCESS read-write
    STATUS mandatory
    ::= { auditLogData 1 }

    powerStatus  OBJECT-TYPE 
    SYNTAX 
            INTEGER {
                power-OK(1),
                power-Battery(2),
                power-Shutdown(3)
            }
    ACCESS read-only
    STATUS mandatory
    ::= { powerData 1 }


    -- The Alert Management Group

    alertNameNumber  OBJECT-TYPE 
    SYNTAX INTEGER
    ACCESS read-only
    STATUS mandatory
    ::= { alert-mgmt 1 }

    alertNameTable  OBJECT-TYPE 
    SYNTAX SEQUENCE OF SvAlertNameEntry
    ACCESS not-accessible
    STATUS mandatory
    ::= { alert-mgmt 2 }

    svAlertNameEntry OBJECT-TYPE 
    SYNTAX SvAlertNameEntry
    ACCESS not-accessible
    STATUS mandatory
    INDEX  { svAlertName }
    ::= { alertNameTable 1 }

    SvAlertNameEntry ::= SEQUENCE {
                         svAlertName
                           DisplayString

                         }

    svAlertName  OBJECT-TYPE 
    SYNTAX  DisplayString (size (1..20))
    ACCESS read-write 
    STATUS mandatory
    ::= { svAlertNameEntry 1 }

    alertSchedule  OBJECT-TYPE 
    SYNTAX INTEGER
    ACCESS read-write
    STATUS mandatory
    ::= { alert-mgmt 3  }


-- Trap Definitions 

bytesAvailAlert             TRAP-TYPE
    ENTERPRISE	    lanmanager.Alert-2.alerts
--ERROR    VARIABLES       { }
    ::= 1

netIOErrorsAlert            TRAP-TYPE
    ENTERPRISE	    lanmanager.Alert-2.alerts
    VARIABLES       {   alert-conditions.NetIOErrorsData.networkID, 
--ERROR                        alert-conditions.NetIOErrorsData.numNetIOErrors
                        alert-conditions.NetIOErrorsData.numNetIOErrors }
    ::= 2

serverErrorsAlert           TRAP-TYPE
    ENTERPRISE	    lanmanager.Alert-2.alerts
    VARIABLES       { alert-conditions.serverErrorsData }
    ::= 3

pwViolationsAlert           TRAP-TYPE
    ENTERPRISE	    lanmanager.Alert-2.alerts
    VARIABLES       {   alert-conditions.pwViolationsData.numPWViolations }
    ::= 4

accessViolationsAlert       TRAP-TYPE
    ENTERPRISE	    lanmanager.Alert-2.alerts
    VARIABLES       {   
    alert-conditions.accessViolationsData.numAccessViolations 
    }
    ::= 5

auditLogFullAlert           TRAP-TYPE
    ENTERPRISE	    lanmanager.Alert-2.alerts
--ERROR    VARIABLES       { }
    ::= 6

auditLog80Alert             TRAP-TYPE
    ENTERPRISE	    lanmanager.Alert-2.alerts
--ERROR    VARIABLES       { }
    ::= 7

upsPowerOutWarnAlert        TRAP-TYPE
    ENTERPRISE	    lanmanager.Alert-2.alerts
--ERROR    VARIABLES       { }
    ::= 8

upsPowerOutShutdownAlert    TRAP-TYPE
    ENTERPRISE	    lanmanager.Alert-2.alerts
--ERROR    VARIABLES       { }
    ::= 9

upsPowerRestoredAlert       TRAP-TYPE
    ENTERPRISE	    lanmanager.Alert-2.alerts
--ERROR    VARIABLES       { }
    ::= 10


logonPrimaryDCFailureAlert  TRAP-TYPE
    ENTERPRISE	    lanmanager.Alert-2.alerts
    VARIABLES       { alert-conditions.pdcFailData.primaryDCName }
    ::= 11

--ERRORreplMasterFailure alert     TRAP-TYPE
replMasterFailurealert     TRAP-TYPE
    ENTERPRISE	    lanmanager.Alert-2.alerts
    VARIABLES       { alert-conditions.rplFailData.replMasterName }
    ::= 12

--ERRORdiskHotFix alert            TRAP-TYPE
diskHotFixAlert            TRAP-TYPE
    ENTERPRISE	    lanmanager.Alert-2.alerts
    VARIABLES       {
    alert-conditions.bytesAvailData.bytesAvailTable.bytesAvailEntry.diskDrive
    }
    ::= 13

diskHardErrorAlert          TRAP-TYPE
    ENTERPRISE	    lanmanager.Alert-2.alerts
    VARIABLES       {
    alert-conditions.bytesAvailData.bytesAvailTable.bytesAvailEntry.diskDrive
    }
    ::= 14

END