          RFC1398-MIB DEFINITIONS ::= BEGIN


               IMPORTS
                    Counter, Gauge
                         FROM RFC1155-SMI
                    mib-2
                         FROM RFC1213-MIB
                    OBJECT-TYPE
                         FROM RFC-1212;

          --  This MIB module uses the extended OBJECT-TYPE macro as
          --  defined in RFC-1212.

          --  this is the MIB module for ethernet-like objects

          transmission  OBJECT IDENTIFIER ::= { mib-2 10 }
          dot3          OBJECT IDENTIFIER ::= { transmission 7 }

          -- { dot3 1 } is obsolete and has been deleted.

-- The Ethernet-like Statistics Group


          -- the Ethernet-like Statistics group

          -- Implementation of this group is mandatory

          dot3StatsTable   OBJECT-TYPE
               SYNTAX    SEQUENCE OF Dot3StatsEntry
               ACCESS    not-accessible
               STATUS    mandatory
               DESCRIPTION
                         "Statistics for a collection of ethernet-like
                         interfaces attached to a particular system."
               ::= { dot3 2 }


          dot3StatsEntry   OBJECT-TYPE
               SYNTAX    Dot3StatsEntry
               ACCESS    not-accessible
               STATUS    mandatory
               DESCRIPTION
                         "Statistics for a particular interface to an
                         ethernet-like medium."
               INDEX     { dot3StatsIndex }
               ::= { dot3StatsTable 1 }


          Dot3StatsEntry ::= SEQUENCE {
               dot3StatsIndex
                    INTEGER,
               dot3StatsAlignmentErrors
                    Counter,
               dot3StatsFCSErrors
                    Counter,
               dot3StatsSingleCollisionFrames
                    Counter,
               dot3StatsMultipleCollisionFrames
                    Counter,
               dot3StatsSQETestErrors
                    Counter,
               dot3StatsDeferredTransmissions
                    Counter,
               dot3StatsLateCollisions
                    Counter,
               dot3StatsExcessiveCollisions
                    Counter,
               dot3StatsInternalMacTransmitErrors
                    Counter,
               dot3StatsCarrierSenseErrors
                    Counter,
               dot3StatsFrameTooLongs
                    Counter,
               dot3StatsInternalMacReceiveErrors
                    Counter
          }

          dot3StatsIndex   OBJECT-TYPE
               SYNTAX    INTEGER
               ACCESS    read-only
               STATUS    mandatory
               DESCRIPTION
                         "An index value that uniquely identifies an
                         interface to an ethernet-like medium.  The
                         interface identified by a particular value of
                         this index is the same interface as identified
                         by the same value of ifIndex."
               ::= { dot3StatsEntry 1 }


          dot3StatsAlignmentErrors   OBJECT-TYPE
               SYNTAX    Counter
               ACCESS    read-only
               STATUS    mandatory
               DESCRIPTION
                         "A count of frames received on a particular
                         interface that are not an integral number of
                         octets in length and do not pass the FCS check.

                         The count represented by an instance of this
                         object is incremented when the alignmentError
                         status is returned by the MAC service to the
                         LLC (or other MAC user). Received frames for
                         which multiple error conditions obtain are,
                         according to the conventions of IEEE 802.3
                         Layer Management, counted exclusively according
                         to the error status presented to the LLC."
               REFERENCE
                         "IEEE 802.3 Layer Management"
               ::= { dot3StatsEntry 2 }


          dot3StatsFCSErrors   OBJECT-TYPE
               SYNTAX    Counter
               ACCESS    read-only
               STATUS    mandatory
               DESCRIPTION
                         "A count of frames received on a particular
                         interface that are an integral number of octets
                         in length but do not pass the FCS check.

                         The count represented by an instance of this
                         object is incremented when the frameCheckError
                         status is returned by the MAC service to the
                         LLC (or other MAC user). Received frames for
                         which multiple error conditions obtain are,
                         according to the conventions of IEEE 802.3
                         Layer Management, counted exclusively according
                         to the error status presented to the LLC."
               REFERENCE
                         "IEEE 802.3 Layer Management"
               ::= { dot3StatsEntry 3 }


          dot3StatsSingleCollisionFrames   OBJECT-TYPE
               SYNTAX    Counter
               ACCESS    read-only
               STATUS    mandatory
               DESCRIPTION
                         "A count of successfully transmitted frames on
                         a particular interface for which transmission
                         is inhibited by exactly one collision.

                         A frame that is counted by an instance of this
                         object is also counted by the corresponding
                         instance of either the ifOutUcastPkts or
                         ifOutNUcastPkts object and is not counted by
                         the corresponding instance of the
                         dot3StatsMultipleCollisionFrames object."
               REFERENCE
                         "IEEE 802.3 Layer Management"
               ::= { dot3StatsEntry 4 }


          dot3StatsMultipleCollisionFrames   OBJECT-TYPE
               SYNTAX    Counter
               ACCESS    read-only
               STATUS    mandatory
               DESCRIPTION
                         "A count of successfully transmitted frames on
                         a particular interface for which transmission
                         is inhibited by more than one collision.

                         A frame that is counted by an instance of this
                         object is also counted by the corresponding
                         instance of either the ifOutUcastPkts or
                         ifOutNUcastPkts object and is not counted by
                         the corresponding instance of the
                         dot3StatsSingleCollisionFrames object."
               REFERENCE
                         "IEEE 802.3 Layer Management"
               ::= { dot3StatsEntry 5 }


          dot3StatsSQETestErrors   OBJECT-TYPE
               SYNTAX    Counter
               ACCESS    read-only
               STATUS    mandatory
               DESCRIPTION
                         "A count of times that the SQE TEST ERROR
                         message is generated by the PLS sublayer for a
                         particular interface. The SQE TEST ERROR
                         message is defined in section 7.2.2.2.4 of
                         ANSI/IEEE 802.3-1985 and its generation is
                         described in section 7.2.4.6 of the same
                         document."
               REFERENCE
                         "ANSI/IEEE Std 802.3-1985 Carrier Sense
                         Multiple Access with Collision Detection Access
                         Method and Physical Layer Specifications"
               ::= { dot3StatsEntry 6 }

          dot3StatsDeferredTransmissions   OBJECT-TYPE
               SYNTAX    Counter
               ACCESS    read-only
               STATUS    mandatory
               DESCRIPTION
                         "A count of frames for which the first
                         transmission attempt on a particular interface
                         is delayed because the medium is busy.

                         The count represented by an instance of this
                         object does not include frames involved in
                         collisions."
               REFERENCE
                         "IEEE 802.3 Layer Management"
               ::= { dot3StatsEntry 7 }


          dot3StatsLateCollisions   OBJECT-TYPE
               SYNTAX    Counter
               ACCESS    read-only
               STATUS    mandatory
               DESCRIPTION
                         "The number of times that a collision is
                         detected on a particular interface later than
                         512 bit-times into the transmission of a
                         packet.

                         Five hundred and twelve bit-times corresponds
                         to 51.2 microseconds on a 10 Mbit/s system. A
                         (late) collision included in a count
                         represented by an instance of this object is
                         also considered as a (generic) collision for
                         purposes of other collision-related
                         statistics."
               REFERENCE
                         "IEEE 802.3 Layer Management"
               ::= { dot3StatsEntry 8 }


          dot3StatsExcessiveCollisions   OBJECT-TYPE
               SYNTAX    Counter
               ACCESS    read-only
               STATUS    mandatory
               DESCRIPTION
                         "A count of frames for which transmission on a
                         particular interface fails due to excessive
                         collisions."
               REFERENCE
                         "IEEE 802.3 Layer Management"
               ::= { dot3StatsEntry 9 }


          dot3StatsInternalMacTransmitErrors   OBJECT-TYPE
               SYNTAX    Counter
               ACCESS    read-only
               STATUS    mandatory
               DESCRIPTION
                         "A count of frames for which transmission on a
                         particular interface fails due to an internal
                         MAC sublayer transmit error. A frame is only
                         counted by an instance of this object if it is
                         not counted by the corresponding instance of
                         either the dot3StatsLateCollisions object, the
                         dot3StatsExcessiveCollisions object, or the
                         dot3StatsCarrierSenseErrors object.

                         The precise meaning of the count represented by
                         an instance of this object is implementation-
                         specific.  In particular, an instance of this
                         object may represent a count of transmission
                         errors on a particular interface that are not
                         otherwise counted."
               REFERENCE
                         "IEEE 802.3 Layer Management"
               ::= { dot3StatsEntry 10 }


          dot3StatsCarrierSenseErrors   OBJECT-TYPE
               SYNTAX    Counter
               ACCESS    read-only
               STATUS    mandatory
               DESCRIPTION
                         "The number of times that the carrier sense
                         condition was lost or never asserted when
                         attempting to transmit a frame on a particular
                         interface.

                         The count represented by an instance of this
                         object is incremented at most once per
                         transmission attempt, even if the carrier sense
                         condition fluctuates during a transmission
                         attempt."
               REFERENCE
                         "IEEE 802.3 Layer Management"
               ::= { dot3StatsEntry 11 }

          -- { dot3StatsEntry 12 } is not assigned

          dot3StatsFrameTooLongs   OBJECT-TYPE
               SYNTAX    Counter
               ACCESS    read-only
               STATUS    mandatory
               DESCRIPTION
                         "A count of frames received on a particular
                         interface that exceed the maximum permitted
                         frame size.

                         The count represented by an instance of this
                         object is incremented when the frameTooLong
                         status is returned by the MAC service to the
                         LLC (or other MAC user). Received frames for
                         which multiple error conditions obtain are,
                         according to the conventions of IEEE 802.3
                         Layer Management, counted exclusively according
                         to the error status presented to the LLC."
               REFERENCE
                         "IEEE 802.3 Layer Management"
               ::= { dot3StatsEntry 13 }



          -- { dot3StatsEntry 14 } is not assigned


          -- { dot3StatsEntry 15 } is not assigned

          dot3StatsInternalMacReceiveErrors   OBJECT-TYPE
               SYNTAX    Counter
               ACCESS    read-only
               STATUS    mandatory
               DESCRIPTION
                         "A count of frames for which reception on a
                         particular interface fails due to an internal
                         MAC sublayer receive error. A frame is only
                         counted by an instance of this object if it is
                         not counted by the corresponding instance of
                         either the dot3StatsFrameTooLongs object, the
                         dot3StatsAlignmentErrors object, or the
                         dot3StatsFCSErrors object.

                         The precise meaning of the count represented by
                         an instance of this object is implementation-
                         specific.  In particular, an instance of this
                         object may represent a count of receive errors
                         on a particular interface that are not
                         otherwise counted."
               REFERENCE
                         "IEEE 802.3 Layer Management"
               ::= { dot3StatsEntry 16 }

--  802.3 Tests


      --  802.3 Tests

      -- The ifExtnsTestTable defined in RFC 1229 provides a common
      -- means for a manager to test any interface corresponding to
      -- a value of ifIndex.

      -- At this time, one well known test (testFullDuplexLoopBack) is
      -- defined in RFC 1229.  For ethernet-like interfaces, this test
      -- configures the MAC chip and executes an internal loopback
      -- test of memory and the MAC chip logic.  This loopback test can
      -- only be executed if the interface is offline.  Once the test
      -- has completed, the MAC chip should be reinitialized for network
      -- operation, but it should remain offline.

      -- If an error occurs during a test, the object ifExtnsTestResult
      -- (defined in RFC 1229) will be set to failed(7).  The following
      -- two OBJECT IDENTIFIERs may be used to provided more
      -- information as values for the object ifExtnsTestCode in
      -- RFC 1229:

          dot3Errors             OBJECT IDENTIFIER ::= { dot3 7 }

                               -- couldn't initialize MAC chip for test
          dot3ErrorInitError     OBJECT IDENTIFIER ::= { dot3Errors 1 }

                                -- expected data not received (or not
                                -- received correctly) in loopback test
          dot3ErrorLoopbackError OBJECT IDENTIFIER ::= { dot3Errors 2 }

       -- Tests
        --  TDR Test

       -- Another test, specific to ethernet-like interfaces with the
       -- exception of 10BaseT and 10BaseF, is Time-domain Reflectometry
       --    (TDR).
       -- The TDR value may be useful in determining the approximate
       --    distance
       -- to a cable fault.  It is advisable to repeat this test to
       --    check for
       -- a consistent resulting TDR value, to verify that there is a
       --   fault.

          dot3Tests   OBJECT IDENTIFIER ::= { dot3 6 }
          dot3TestTdr OBJECT IDENTIFIER ::= { dot3Tests 1 }

       -- A TDR test returns as its result the time interval, measured
       -- in 10 MHz ticks or 100 nsec units, between the start of
       -- TDR test transmission and the subsequent detection of a
       -- collision or deassertion of carrier.  On successful completion
       -- of a TDR test, the appropriate instance of ifExtnsTestResult
       -- contains the OBJECT IDENTIFIER of the MIB object which
       -- contains the value of this time interval.

--   802.3 Hardware Chipsets


       --  802.3 Hardware Chipsets

       -- The object ifExtnsChipSet is provided in RFC 1229 to identify
       -- the MAC hardware used to communcate on an interface.  The
       -- following hardware chipsets are provided for 802.3:

  dot3ChipSets          OBJECT IDENTIFIER ::= { dot3 8 }
  dot3ChipSetAMD        OBJECT IDENTIFIER ::= { dot3ChipSets 1 }
  dot3ChipSetAMD7990    OBJECT IDENTIFIER ::= { dot3ChipSetAMD 1 }
  dot3ChipSetAMD79900   OBJECT IDENTIFIER ::= { dot3ChipSetAMD 2 }

  dot3ChipSetIntel      OBJECT IDENTIFIER ::= { dot3ChipSets 2 }
  dot3ChipSetIntel82586 OBJECT IDENTIFIER ::= { dot3ChipSetIntel 1 }
  dot3ChipSetIntel82596 OBJECT IDENTIFIER ::= { dot3ChipSetIntel 2 }
  dot3ChipSetSeeq       OBJECT IDENTIFIER ::= { dot3ChipSets 3 }
  dot3ChipSetSeeq8003   OBJECT IDENTIFIER ::= { dot3ChipSetSeeq 1 }

  dot3ChipSetNational      OBJECT IDENTIFIER ::= { dot3ChipSets 4 }
  dot3ChipSetNational8390  OBJECT IDENTIFIER ::=
                                           { dot3ChipSetNational 1 }
  dot3ChipSetNationalSonic OBJECT IDENTIFIER ::=
                                           { dot3ChipSetNational 2 }

  dot3ChipSetFujitsu       OBJECT IDENTIFIER ::= { dot3ChipSets 5 }
  dot3ChipSetFujitsu86950  OBJECT IDENTIFIER ::=
                                           { dot3ChipSetFujitsu 1 }
  dot3ChipSetFujitsu86960  OBJECT IDENTIFIER ::=
                                           { dot3ChipSetFujitsu 2 }

       -- For those chipsets not represented above, OBJECT IDENTIFIER
       -- assignment is required in other documentation, e.g., assignment
       -- within that part of the registration tree delegated to
       -- individual enterprises (see RFC 1155).

          END
