
S5-ETHERNET-COMMON-MIB DEFINITIONS ::= BEGIN

IMPORTS
        MODULE-IDENTITY, OBJECT-TYPE, Counter32
            FROM SNMPv2-SMI
	s5EnCfg, s5EnStat
		FROM S5-ETHERNET-MIB
	TimeIntervalSec, SrcIndx, AttId
		FROM S5-TCS-MIB;
 
s5EthernetCommonMib MODULE-IDENTITY
       LAST-UPDATED    "200407200000Z"
       ORGANIZATION    "Nortel Networks"
       CONTACT-INFO    "Nortel Networks"
       DESCRIPTION
           "5000 Ethernet Common MIB

            Copyright 1993-2004 Nortel Networks, Inc.
            All rights reserved.
            This Nortel Networks SNMP Management Information Base Specification
            (Specification) embodies Nortel Networks' confidential and
            proprietary intellectual property. Nortel Networks retains all
            title and ownership in the Specification, including any
            revisions.

            This Specification is supplied 'AS IS,' and Nortel Networks makes
            no warranty, either express or implied, as to the use,
            operation, condition, or performance of the Specification."

       REVISION "200407200000Z" -- 20 July 2004
       DESCRIPTION "Version 118:  Conversion to SMIv2"

       ::= { s5EnCfg 0 }


-- SECTION 2: Configuration information

-- Port Table

s5EnPortTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S5EnPortEntry
	MAX-ACCESS	not-accessible
	STATUS	current
	DESCRIPTION
		"A table containing information about each
		managed ethernet connectivity port on a board.
		The number of entries is determined by the
		number of managed ports. Those boards
		that do not have any ports do not have
		any entries in this table."
	::= { s5EnCfg 1 }

s5EnPortEntry OBJECT-TYPE
	SYNTAX	S5EnPortEntry
	MAX-ACCESS	not-accessible
	STATUS	current
	DESCRIPTION
		"A row in Ethernet port table. Entries
		can not be created or deleted via SNMP."
	INDEX	{ s5EnPortBrdIndx,
		  s5EnPortIndx }
	::= { s5EnPortTable 1 }

S5EnPortEntry ::= SEQUENCE {
	s5EnPortBrdIndx INTEGER,
	s5EnPortIndx INTEGER,
	s5EnPortPartStatus INTEGER,
	s5EnPortPartTime TimeIntervalSec,
	s5EnPortLinkStatus INTEGER,
	s5EnPortJabberStatus INTEGER
	}

s5EnPortBrdIndx OBJECT-TYPE
	SYNTAX	INTEGER (1..255)
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"The index of the board. This corresponds to
		the index of the slot containing the board."
	::= { s5EnPortEntry 1 }

s5EnPortIndx OBJECT-TYPE
	SYNTAX	INTEGER (1..255)
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"The index of the port on the board. Its
		value ranges between 1 and index of the last
		manageable port on the board."
	::= { s5EnPortEntry 2 }

s5EnPortPartStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		enabled(2),
		partition(3),
		autoPartition(4),
		timedPartition(5)
		}
	MAX-ACCESS	read-write
	STATUS	current
	DESCRIPTION
		"The partition status of the port.
		The following values can be written:
		  enabled(2)..........enabled port
		  partition(3)........partition port
		  timedPartition(5)...time partition port (uses value
		                        from s5EnPortPartTime)

		The following values reflect the partition
		status of the port:
		  other(1).............partition status unknown
		  enabled(2)...........port enabled
		  partition(3).........port partitioned
		  autoPartition(4).....port auto-partitioned by
		                         hardware
		  timedPartition(5)....port is timed partitioned
		                         (see value of
		                         s5EnPortPartTime).
		On GETs with port status of timedPartition(5), if
		the time remaining before the partition is undone
		is available, it will be reported in object
		s5EnPortPartTime as a positive value. If not
		available, the value of s5EnPortPartTime will
		be zero. When changing a port to timedPartition(5),
		the SET request must also contain the value
		for object s5EnPortPartTime. Only value
		partition(3) will survive resets of the host card."
	::= { s5EnPortEntry 3 }

s5EnPortPartTime OBJECT-TYPE
	SYNTAX	TimeIntervalSec
	MAX-ACCESS	read-write
	STATUS	current
	DESCRIPTION
		"The length of time to keep the port
		partitioned when a timed partition is
		done to the port. This object can only
		be written in the same request that sets
		s5EnPortPartStatus to timedPartition(5).
		Afterwards, it indicates the amount of
		time left before the timed partition
		is completed, at which time
		s5EnPortPartStatus is changed to
		enabled(2). This object has the value of
		zero if the port is not time partitioned,
		or if the amount of time is not available."
	::= { s5EnPortEntry 4 }

s5EnPortLinkStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		off(2),
		on(3)
		}
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"Tells whether the port is receiving
		link status. The values are:
		  other(1)...returned for AUI
		  off(2).....link is not connected
		  on(3)......link is connected
		on/off applies to 10BASE-T and Fiber ports only."
	::= { s5EnPortEntry 5 }

s5EnPortJabberStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		jabbering(2),
		ok(3)
		}
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"The jabber status of the DTE(s) connected
		to the port. The values are:
		  other(1).......unknown or other condition
		  jabbering(2)...port receiving jabber
		  ok(3)..........no jabber detected."
	::= { s5EnPortEntry 6 }


-- The System 5000 Port Extension Table
 
-- Implementation of the Port Extension Table is optional
 
s5EnPortExtTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF S5EnPortExtEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
                "An extension table to s5EnPortTable containing 
                additional information about per port
                switchable, autonegotiating 10/100 Mbit
                ethernet connectivity ports on a board.
                The number of entries is determined by the
                number of managed ports. Those boards
                that do not have any ports do not have
                any entries in this table."
        ::= { s5EnCfg 3 }
 
s5EnPortExtEntry OBJECT-TYPE
        SYNTAX  S5EnPortExtEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
                "A row in Ethernet port extension table. 
                Entries can not be created or deleted 
                via SNMP."
        INDEX   { s5EnPortExtBrdIndx,
                  s5EnPortExtIndx }
        ::= { s5EnPortExtTable 1 }
 
S5EnPortExtEntry ::= SEQUENCE {
        s5EnPortExtBrdIndx INTEGER,
        s5EnPortExtIndx INTEGER,
        s5EnPortExtHwCapability OCTET STRING,
        s5EnPortExtAutoNegAdv OCTET STRING,
        s5EnPortExtAutoNegRcvd OCTET STRING,
        s5EnPortExt10MbSegAttCfg AttId,
        s5EnPortExt100MbSegAttCfg AttId,
        s5EnPortExt10MbSegConnCapability OCTET STRING,
        s5EnPortExt100MbSegConnCapability OCTET STRING,
        s5EnPortExtActiveSpeed INTEGER,
        s5EnPortExtCurDuplexMode INTEGER
        }
 
s5EnPortExtBrdIndx OBJECT-TYPE
        SYNTAX  INTEGER (1..255)
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "The index of the board. This corresponds to
                the index of the slot containing the board."
        ::= { s5EnPortExtEntry 1 }
 
s5EnPortExtIndx OBJECT-TYPE
        SYNTAX  INTEGER (1..255)
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "The index of the port on the board. Its
                value ranges between 1 and index of the last
                manageable port on the board."
        ::= { s5EnPortExtEntry 2 }
 
s5EnPortExtHwCapability OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE(1))
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "A bit array that contains the bit map
                representing the hardware capabilites
                of the port.   The bit 7 tells if the port
                supports auto-negotiation.  If the auto negotiation
                is on,  the port will have multiple speed capabilities
                while if the auto negotiation is not supported, the
                hardware will only be capable for one speed:
 
                 bit 0 - 10 BASE-T half duplex capable
                 bit 1 - 10 BASE-T full duplex capable
                 bit 2 - 100 BASE-TX half duplex capable
                 bit 3 - 100 BASE-TX full duplex capable

                 bit 5 - 100 BASE-FX full duplex capable
                 bit 6 - 100 BASE-FX half duplex capable
                 bit 7 - auto negotiation support capability

                When auto negotiation is supported only bits 0-3
                are used to indicate the capabilities available
                for negotiation, and any or all of these bits may
                be set as long as at least one bit is set.

                When auto negotiation is NOT supported (bit 7 = 0)
                all other bits are used to indicate the capabilities
                supported by the port, but which must be manually
                configured."
        ::= { s5EnPortExtEntry 3 }
 
s5EnPortExtAutoNegAdv OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE(1))
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
                "A bit array that contains the bit map
                representing the abilities advertised
                during link negociation.  The bit 7 tells
                if auto negotiation is enabled or disabled:
                 bit 0 - 10 BASE-T half duplex capable
                 bit 1 - 10 BASE-T full duplex capable
                 bit 2 - 100 BASE-TX half duplex capable
                 bit 3 - 100 BASE-TX full duplex capable

                 bit 5 - 100 BASE-FX full duplex capable
                 bit 6 - 100 BASE-FX half duplex capable
                 bit 7 - auto negotiation is enabled or disabled
                Only capabilites present in the hardware as
                indicated by s5EnPortExtHwCapability can be
                advertised.

                If auto negotiation is enabled only bits 0-3
                are used to indicate the capabilities available
                for negotiation. Any or all of these bits may be
                set as long as at least one bit is set, AND the
                settings are in accordance with s5EnPortExtHwCapability.

                If auto negotiation is disabled one and only
                one of the speed setting bits MUST be set in
                accordance with s5EnPortExtHwCapability."
        ::= { s5EnPortExtEntry 4 }
 
s5EnPortExtAutoNegRcvd OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE(1))
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "A bit array that contains the bit map
                representing the auto-negotiation
                abilities of the remote end of the link:
                 bit 0 - 10 BASE-T half duplex capable
                 bit 1 - 10 BASE-T full duplex capable
                 bit 2 - 100 BASE-TX half duplex capable
                 bit 3 - 100 BASE-TX full duplex capable
                "
        ::= { s5EnPortExtEntry 5 }
 
s5EnPortExt10MbSegAttCfg OBJECT-TYPE
        SYNTAX  AttId
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
                "The index for the segment used in case 
                a 10 Mbit link is established."
        ::= { s5EnPortExtEntry 6 }
 
s5EnPortExt100MbSegAttCfg OBJECT-TYPE
        SYNTAX  AttId
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
                "The index for the segment used in case 
                a 100 Mbit link is established."
        ::= { s5EnPortExtEntry 7 }
 
s5EnPortExt10MbSegConnCapability OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE(8))
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "A bit array that contains the bit map
                representing all available 10Mbit backplane
                segment and local segment connections for
                the port.  One bit is also reserved to
                indicate if the cluster has an isolate
                capability.
 
                The first 31 bits of the array represent
                the backplane numbers, starting from the
                lower order bit. Bit 32 indicates whether
                the port has a null connection capability.
                The bits in the fifth and sixth octets,
                starting with bits in the lower order octet,
                represent local segments that the port
                can connect to.
 
                A bit with a value of 1 means that the
                port is capable of  connecting to the
                corresponding backplane segment, local segment
                or null segment."
        ::= { s5EnPortExtEntry 8 }
 
 s5EnPortExt100MbSegConnCapability OBJECT-TYPE
        SYNTAX  OCTET STRING (SIZE(8))
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "A bit array that contains the bit map
                representing all available 100Mbit backplane
                segment and local segment connections for
                the port.  One bit is also reserved to
                indicate if the cluster has an isolate
                capability.
 
                The first 31 bits of the array represent
                the backplane numbers, starting from the
                lower order bit. Bit 32 indicates whether
                the port has a null connection capability.
                The bits in the fifth and sixth octets,
                starting with bits in the lower order octet,
                represent local segments that the port
                can connect to.
 
                A bit with a value of 1 means that the
                port is capable of  connecting to the
                corresponding backplane segment, local segment
                or null segment."
        ::= { s5EnPortExtEntry 9 }
 
s5EnPortExtActiveSpeed OBJECT-TYPE
        SYNTAX  INTEGER {
                unknown(1),
                bps10M(2),
                bps100M(3)
                }
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "The speed of the link. The possible
                values are:
                  unknown(1)........unknown, no link
                  bps10M(2).........10 Mbit link
                  bps100M(3)........100 Mbit link"
        ::= { s5EnPortExtEntry 10 }
 
s5EnPortExtCurDuplexMode OBJECT-TYPE
        SYNTAX  INTEGER {
                unknown(1),
                halfDuplex(2),
                fullDuplex(3)
                }
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
                "The status of duplex mode. The possible
                values are:
                  unknown(1)........unknown, no link
                  halfDuplex(2).........half duplex mode
                  fullDuplex(3)........full duplex mode"
        ::= { s5EnPortExtEntry 11 }
 


-- SECTION 3: Statistics

-- Basic Statistics Table

s5EnBStatTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S5EnBStatEntry
	MAX-ACCESS	not-accessible
	STATUS	current
	DESCRIPTION
		"A table containing Ethernet basic
		statistics. The entries in the table
		may come from several different data
		sources. The number of entries is
		determined by the number of sources
		that can provide the information."
	::= { s5EnStat 1 }

s5EnBStatEntry OBJECT-TYPE
	SYNTAX	S5EnBStatEntry
	MAX-ACCESS	not-accessible
	STATUS	current
	DESCRIPTION
		"A row in Ethernet basic statistics table.
		Entries can not be created or deleted via
		SNMP."
	INDEX	{ s5EnBStatSrcIndx }
	::= { s5EnBStatTable 1 }

S5EnBStatEntry ::= SEQUENCE {
	s5EnBStatSrcIndx SrcIndx,

	s5EnBStatGoodOctets Counter32,
	s5EnBStatGoodFrms Counter32,
	s5EnBStatBcastFrms Counter32,
	s5EnBStatMcastFrms Counter32,

	s5EnBStatAlignErrors Counter32,
	s5EnBStatFcsErrors Counter32,
	s5EnBStatRunts Counter32,
	s5EnBStatTooLongFrms Counter32,
	s5EnBStatFragments Counter32,
	s5EnBStatVeryLongEvents Counter32,
	s5EnBStatColls Counter32,

	s5EnBStatLateColls Counter32,
	s5EnBStatShortEvents Counter32,
	s5EnBStatRateMismatches Counter32,
	s5EnBStatBackOffFailures Counter32,
	s5EnBStatAutoPartitions Counter32,
	s5EnBStatShortIPGs Counter32,
	s5EnBStatNullFrames Counter32
	}

s5EnBStatSrcIndx OBJECT-TYPE
	SYNTAX	SrcIndx
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"The index of the entry in the table.
		This index identifies the source of the
		information. Only those sources that provide
		these statistics are in this table."
	::= { s5EnBStatEntry 1 }

s5EnBStatGoodOctets OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"A count of octets contained in frames received
		which had no errors.

		This counter includes octets in unicast, broadcast,
		and multicast frames. This counter includes octets
		after the start frame delimiter up to FCS but not
		including FCS octets."
	::= { s5EnBStatEntry 2 }

s5EnBStatGoodFrms OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"A count of frames that are detected without
		errors. This does not include frames received
		with a frame-too-long, runt, FCS, or alignment errors.
		This counter includes unicast, broadcast, and multicast
		frames."
	::= { s5EnBStatEntry 3 }

s5EnBStatBcastFrms OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"A count of frames that are detected without
		errors and are directed to the broadcast group
		address. This does not include frames received
		with a frame-too-long, runt, FCS, or alignment
		errors. Multicast frames are not included."
	::= { s5EnBStatEntry 4 }

s5EnBStatMcastFrms OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"A count of frames that are detected
		without errors and are directed to a
		non-broadcast group address. This does not
		include frames received with a frame-too-long,
		runt, FCS, or alignment errors."
	::= { s5EnBStatEntry 5 }

s5EnBStatAlignErrors OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"A count of frames detected
		that are not an integral number of octets
		in length and do not pass the FCS check.
		This counter is incremented when the
		frame is received with FramingError and
		FcsError and whose OctetCount is greater
		than of equal to minFramSize and less than
		or equal to maxFramSize."
	::= { s5EnBStatEntry 6 }

s5EnBStatFcsErrors OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"A count of frames detected that are an
		integral number of octets in length that
		do not pass the FCS check. This counter is
		incremented when the frame is received with
		FcsError and NoFramingError and NoCollisions
		and whose OctetCount is greater than or equal
		to minFramsize and less than or equal to
		maxFrameSize."
	::= { s5EnBStatEntry 7 }

s5EnBStatRunts OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"A count of frames detected that are less than
		the minimum permitted frame size and have a
		good FCS."
	::= { s5EnBStatEntry 8 }

s5EnBStatTooLongFrms OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"A count of frames detected that exceed the
		maximum permitted frame size. This counter is
		incremented when a frame received on this port whose
		OctetCount is greater than maxFramSize."
	::= { s5EnBStatEntry 9 }

s5EnBStatFragments OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"A count of fragments detected between 80-512 bits
		(64 bytes), inclusively, with invalid FCS. (These
		commonly represent collision fragments, and are
		not errors)."
	::= { s5EnBStatEntry 10 }

s5EnBStatVeryLongEvents OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"A count of the times that MAU
		jabber lockup protection (MJLP) was detected
		due to transmission of data that exceeded
		5 msec in duration(OctetCount greater than
		maxFramSize). This information can be useful
		in identifying faulty stations."
	::= { s5EnBStatEntry 11 }

s5EnBStatColls OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"A count of receive collisions detected."
	::= { s5EnBStatEntry 12 }

s5EnBStatLateColls OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"A count of late receive collisions detected.
		This counter is incremented for each event
		in which there is a receive Collision and
		ActivityDuration is greater than the
		LateEventThreshold."
	::= { s5EnBStatEntry 13 }

s5EnBStatShortEvents OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"A count of fragments detected with
		ActivityDuration less than ShortEventMaxTime.
		ShortEventMaxTime is greater than 74 bit times and
		less than 82 bit times."
	::= { s5EnBStatEntry 14 }

s5EnBStatRateMismatches OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"A count of the occurrences of
		out of spec bit rates. This indicates the
		number of times the FIFO buffer over-runs or
		under-runs due to transmission rate errors."
	::= { s5EnBStatEntry 15 }

s5EnBStatBackOffFailures OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"This counter is incremented by one for each
		frame received on this port with collision and
		port activity time greater than 552 to 560 bit time."
	::= { s5EnBStatEntry 16 }

s5EnBStatAutoPartitions OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"A count of the number of times that this port
		was automatically partitioned. The condition
		occurs when 32 consecutive collisions are
		detected on the port."
	::= { s5EnBStatEntry 17 }

s5EnBStatShortIPGs OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"A count of occurrences of a too short IPG
		(inter packet gap before a good packet) that were
		detected."
	::= { s5EnBStatEntry 18 }

s5EnBStatNullFrames OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"A count of the occurrences of
		frames received with no collision and whose
		octetCount is equal to 0 and activity time is
		greater than ValidPacketMinTime."
	::= { s5EnBStatEntry 19 }



-- Port Extension Statistics Table

s5EnPStatTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S5EnPStatEntry
	MAX-ACCESS	not-accessible
	STATUS	current
	DESCRIPTION
		"A table containing Ethernet port
		extension statistics. This table extends
		table s5EnBStatTable for ports. The entries
		in the table may come only from port
		sources. The number of entries is determined
		by the number of sources that can provide the
		information."
	::= { s5EnStat 2 }

s5EnPStatEntry OBJECT-TYPE
	SYNTAX	S5EnPStatEntry
	MAX-ACCESS	not-accessible
	STATUS	current
	DESCRIPTION
		"A row in Ethernet port extension statistic table.
		Entries can not be created or deleted via
		SNMP."
	INDEX	{ s5EnPStatSrcIndx }
	::= { s5EnPStatTable 1 }

S5EnPStatEntry ::= SEQUENCE {
	s5EnPStatSrcIndx SrcIndx,

	s5EnPStatSourceAddrChngs Counter32,
	s5EnPStatLinkStatusChngs Counter32,
	s5EnPStatLastSourceAddr OCTET STRING
	}

s5EnPStatSrcIndx OBJECT-TYPE
	SYNTAX	SrcIndx
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"The index of the entry in the table.
		This index identifies the source of the
		information. Only those sources that provide
		these statistics are in this table."
	::= { s5EnPStatEntry 1 }

s5EnPStatSourceAddrChngs OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"A count of changes in Last Source Address."
	::= { s5EnPStatEntry 2 }

s5EnPStatLinkStatusChngs OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"Contains a count of number of changes in
		link status from on(3) to off(2)."
	::= { s5EnPStatEntry 3 }

s5EnPStatLastSourceAddr	OBJECT-TYPE
	SYNTAX	OCTET STRING (SIZE (0..6))
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"The Source Address of the last readable frame
		received by this port.  If no frames have been
		received by this port since the agent began
		monitoring this port, the agent shall return
		a string of length zero."
	::= { s5EnPStatEntry 4 }

-- Segment Extension Statistics Table

s5EnSStatTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S5EnSStatEntry
	MAX-ACCESS	not-accessible
	STATUS	current
	DESCRIPTION
		"A table containing Ethernet Segment
		extension statistics. This table extends
		table s5EnBStatTable for segments. The
		entries in the table may come from several
		different data sources. The number
		of entries is determined by the number
		of sources that can provide the information."
	::= { s5EnStat 3 }

s5EnSStatEntry OBJECT-TYPE
	SYNTAX	S5EnSStatEntry
	MAX-ACCESS	not-accessible
	STATUS	current
	DESCRIPTION
		"A row in Ethernet segment statistics table.
		Entries can not be created or deleted via
		SNMP."
	INDEX	{ s5EnSStatSrcIndx }
	::= { s5EnSStatTable 1 }

S5EnSStatEntry ::= SEQUENCE {
	s5EnSStatSrcIndx SrcIndx,
	s5EnSStatSegColls Counter32,
	s5EnSStatSegRate INTEGER
	}

s5EnSStatSrcIndx OBJECT-TYPE
	SYNTAX	SrcIndx
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"The index of the entry in the table.
		This index identifies the source of the
		information. Only those sources that provide
		these statistics are in this table."
	::= { s5EnSStatEntry 1 }

s5EnSStatSegColls OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"A count of number of transmit collision 
		events(one per packet activity) for a
		segment (i.e., local channel or backplane
		network)."
	::= { s5EnSStatEntry 2 }

s5EnSStatSegRate OBJECT-TYPE
   SYNTAX   INTEGER {
      unknown (1),
      bps10m (2),
      bps100m (3)
      }
   MAX-ACCESS   read-only
   STATUS   current
   DESCRIPTION
      "The segment speed type of this ethernet segment.
      The following values are currently defined:
      unknown (1) ------- unknown type
      bps10m (2) ------- 10Mbps ethernet
      bps100m (3) ------ 100Mbps ethernet"
   ::= { s5EnSStatEntry 3 }

END
