IEEE8021-PAE-MIB DEFINITIONS ::= BEGIN
-- ---------------------------------------------------------- --
-- IEEE 802.1X MIB
-- ---------------------------------------------------------- --
IMPORTS
MODULE-IDENTITY, OBJECT-TYPE, Counter32, Counter64,
Unsigned32, TimeTicks
FROM SNMPv2-SMI
MacAddress, TEXTUAL-CONVENTION, TruthValue
FROM SNMPv2-TC
MODULE-COMPLIANCE, OBJECT-GROUP
FROM SNMPv2-CONF
SnmpAdminString
FROM SNMP-FRAMEWORK-MIB
InterfaceIndex
FROM IF-MIB
;
ieee8021paeMIB MODULE-IDENTITY
LAST-UPDATED "200101160000Z"
ORGANIZATION "IEEE 802.1 Working Group"
CONTACT-INFO
"http://grouper.ieee.org/groups/802/1/index.html"
DESCRIPTION
"The Port Access Entity module for managing IEEE
802.1X."
::= { iso std(0) iso8802(8802) ieee802dot1(1) ieee802dot1mibs(1) 1 }
paeMIBObjects OBJECT IDENTIFIER ::= { ieee8021paeMIB 1 }
-- ---------------------------------------------------------- --
-- Textual Conventions
-- ---------------------------------------------------------- --
PaeControlledDirections ::= TEXTUAL-CONVENTION
STATUS current
DESCRIPTION
"The control mode values for the Authenticator PAE."
SYNTAX INTEGER {
both(0),
in(1)
}
PaeControlledPortStatus ::= TEXTUAL-CONVENTION
STATUS current
DESCRIPTION
"The status values of the Authenticator PAE controlled
Port."
SYNTAX INTEGER {
authorized(1),
unauthorized(2)
}
PaeControlledPortControl ::= TEXTUAL-CONVENTION
STATUS current
DESCRIPTION
"The control values of the Authenticator PAE controlled
Port."
SYNTAX INTEGER {
forceUnauthorized(1),
auto(2),
forceAuthorized(3)
}
-- ---------------------------------------------------------- --
-- ---------------------------------------------------------- --
-- groups in the PAE MIB
-- ---------------------------------------------------------- --
dot1xPaeSystem OBJECT IDENTIFIER ::= { paeMIBObjects 1 }
dot1xPaeAuthenticator OBJECT IDENTIFIER ::= { paeMIBObjects 2 }
dot1xPaeSupplicant OBJECT IDENTIFIER ::= { paeMIBObjects 3 }
-- ---------------------------------------------------------- --
-- ---------------------------------------------------------- --
-- The PAE System Group
-- ---------------------------------------------------------- --
dot1xPaeSystemAuthControl OBJECT-TYPE
SYNTAX INTEGER { enabled(1), disabled(2) }
MAX-ACCESS read-write
STATUS current
DESCRIPTION
"The administrative enable/disable state for
Port Access Control in a System."
REFERENCE
"9.6.1, SystemAuthControl"
::= { dot1xPaeSystem 1 }
-- ---------------------------------------------------------- --
-- The PAE Port Table
-- ---------------------------------------------------------- --
dot1xPaePortTable OBJECT-TYPE
SYNTAX SEQUENCE OF Dot1xPaePortEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"A table of system level information for each port
supported by the Port Access Entity. An entry appears
in this table for each port of this system."
REFERENCE
"9.6.1"
::= { dot1xPaeSystem 2 }
dot1xPaePortEntry OBJECT-TYPE
SYNTAX Dot1xPaePortEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"The Port number, protocol version, and
initialization control for a Port."
INDEX { dot1xPaePortNumber }
::= { dot1xPaePortTable 1 }
Dot1xPaePortEntry ::=
SEQUENCE {
dot1xPaePortNumber
InterfaceIndex,
dot1xPaePortProtocolVersion
Unsigned32,
dot1xPaePortCapabilities
BITS,
dot1xPaePortInitialize
TruthValue,
dot1xPaePortReauthenticate
TruthValue
}
dot1xPaePortNumber OBJECT-TYPE
SYNTAX InterfaceIndex
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"The Port number associated with this Port."
REFERENCE
"9.6.1, Port number"
::= { dot1xPaePortEntry 1 }
dot1xPaePortProtocolVersion OBJECT-TYPE
SYNTAX Unsigned32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The protocol version associated with this Port."
REFERENCE
"9.6.1, Protocol version"
::= { dot1xPaePortEntry 2 }
dot1xPaePortCapabilities OBJECT-TYPE
SYNTAX BITS {
dot1xPaePortAuthCapable(0),
-- Authenticator functions are supported
dot1xPaePortSuppCapable(1)
-- Supplicant functions are supported
}
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Indicates the PAE functionality that this Port
supports and that may be managed through this MIB."
REFERENCE
"9.6.1, PAE Capabilities"
::= { dot1xPaePortEntry 3 }
dot1xPaePortInitialize OBJECT-TYPE
SYNTAX TruthValue
MAX-ACCESS read-write
STATUS current
DESCRIPTION
"The initialization control for this Port. Setting this
attribute TRUE causes the Port to be initialized.
The attribute value reverts to FALSE once initialization
has completed."
REFERENCE
"9.6.1.2, Initialize Port"
::= { dot1xPaePortEntry 4 }
dot1xPaePortReauthenticate OBJECT-TYPE
SYNTAX TruthValue
MAX-ACCESS read-write
STATUS current
DESCRIPTION
"The reauthentication control for this port. Setting
this attribute TRUE causes the Authenticator PAE state
machine for the Port to reauthenticate the Supplicant.
Setting this attribute FALSE has no effect.
This attribute always returns FALSE when it is read."
REFERENCE
"9.4.1.3 Reauthenticate"
::= { dot1xPaePortEntry 5 }
-- ---------------------------------------------------------- --
-- The PAE Authenticator Group
-- ---------------------------------------------------------- --
-- ---------------------------------------------------------- --
-- The Authenticator Configuration Table
-- ---------------------------------------------------------- --
dot1xAuthConfigTable OBJECT-TYPE
SYNTAX SEQUENCE OF Dot1xAuthConfigEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"A table that contains the configuration objects for the
Authenticator PAE associated with each port.
An entry appears in this table for each port that may
authenticate access to itself."
REFERENCE
"9.4.1 Authenticator Configuration"
::= { dot1xPaeAuthenticator 1 }
dot1xAuthConfigEntry OBJECT-TYPE
SYNTAX Dot1xAuthConfigEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"The configuration information for an Authenticator
PAE."
INDEX { dot1xPaePortNumber }
::= { dot1xAuthConfigTable 1 }
Dot1xAuthConfigEntry ::=
SEQUENCE {
dot1xAuthPaeState
INTEGER,
dot1xAuthBackendAuthState
INTEGER,
dot1xAuthAdminControlledDirections
PaeControlledDirections,
dot1xAuthOperControlledDirections
PaeControlledDirections,
dot1xAuthAuthControlledPortStatus
PaeControlledPortStatus,
dot1xAuthAuthControlledPortControl
PaeControlledPortControl,
dot1xAuthQuietPeriod
Unsigned32,
dot1xAuthTxPeriod
Unsigned32,
dot1xAuthSuppTimeout
Unsigned32,
dot1xAuthServerTimeout
Unsigned32,
dot1xAuthMaxReq
Unsigned32,
dot1xAuthReAuthPeriod
Unsigned32,
dot1xAuthReAuthEnabled
TruthValue,
dot1xAuthKeyTxEnabled
TruthValue
}
dot1xAuthPaeState OBJECT-TYPE
SYNTAX INTEGER {
initialize(1),
disconnected(2),
connecting(3),
authenticating(4),
authenticated(5),
aborting(6),
held(7),
forceAuth(8),
forceUnauth(9)
}
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The current value of the Authenticator PAE state
machine."
REFERENCE
"9.4.1, Authenticator PAE state"
::= { dot1xAuthConfigEntry 1 }
dot1xAuthBackendAuthState OBJECT-TYPE
SYNTAX INTEGER {
request(1),
response(2),
success(3),
fail(4),
timeout(5),
idle(6),
initialize(7)
}
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The current state of the Backend Authentication
state machine."
REFERENCE
"9.4.1, Backend Authentication state"
::= { dot1xAuthConfigEntry 2 }
dot1xAuthAdminControlledDirections OBJECT-TYPE
SYNTAX PaeControlledDirections
MAX-ACCESS read-write
STATUS current
DESCRIPTION
"The current value of the administrative controlled
directions parameter for the Port."
REFERENCE
"9.4.1, Admin Control Mode"
::= { dot1xAuthConfigEntry 3 }
dot1xAuthOperControlledDirections OBJECT-TYPE
SYNTAX PaeControlledDirections
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The current value of the operational controlled
directions parameter for the Port."
REFERENCE
"9.4.1, Oper Control Mode"
::= { dot1xAuthConfigEntry 4 }
dot1xAuthAuthControlledPortStatus OBJECT-TYPE
SYNTAX PaeControlledPortStatus
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The current value of the controlled Port
status parameter for the Port."
REFERENCE
"9.4.1, AuthControlledPortStatus"
::= { dot1xAuthConfigEntry 5 }
dot1xAuthAuthControlledPortControl OBJECT-TYPE
SYNTAX PaeControlledPortControl
MAX-ACCESS read-write
STATUS current
DESCRIPTION
"The current value of the controlled Port
control parameter for the Port."
REFERENCE
"9.4.1, AuthControlledPortControl"
::= { dot1xAuthConfigEntry 6 }
dot1xAuthQuietPeriod OBJECT-TYPE
SYNTAX Unsigned32
MAX-ACCESS read-write
STATUS current
DESCRIPTION
"The value, in seconds, of the quietPeriod constant
currently in use by the Authenticator PAE state
machine."
REFERENCE
"9.4.1, quietPeriod"
DEFVAL { 60 }
::= { dot1xAuthConfigEntry 7 }
dot1xAuthTxPeriod OBJECT-TYPE
SYNTAX Unsigned32
MAX-ACCESS read-write
STATUS current
DESCRIPTION
"The value, in seconds, of the txPeriod constant
currently in use by the Authenticator PAE state
machine."
REFERENCE
"9.4.1, txPeriod"
DEFVAL { 30 }
::= { dot1xAuthConfigEntry 8 }
dot1xAuthSuppTimeout OBJECT-TYPE
SYNTAX Unsigned32
MAX-ACCESS read-write
STATUS current
DESCRIPTION
"The value, in seconds, of the suppTimeout constant
currently in use by the Backend Authentication state
machine."
REFERENCE
"9.4.1, suppTimeout"
DEFVAL { 30 }
::= { dot1xAuthConfigEntry 9 }
dot1xAuthServerTimeout OBJECT-TYPE
SYNTAX Unsigned32
MAX-ACCESS read-write
STATUS current
DESCRIPTION
"The value, in seconds, of the serverTimeout constant
currently in use by the Backend Authentication state
machine."
REFERENCE
"9.4.1, serverTimeout"
DEFVAL { 30 }
::= { dot1xAuthConfigEntry 10 }
dot1xAuthMaxReq OBJECT-TYPE
SYNTAX Unsigned32
MAX-ACCESS read-write
STATUS current
DESCRIPTION
"The value of the maxReq constant currently in use by
the Backend Authentication state machine."
REFERENCE
"9.4.1, maxReq"
DEFVAL { 2 }
::= { dot1xAuthConfigEntry 11 }
dot1xAuthReAuthPeriod OBJECT-TYPE
SYNTAX Unsigned32
MAX-ACCESS read-write
STATUS current
DESCRIPTION
"The value, in seconds, of the reAuthPeriod constant
currently in use by the Reauthentication Timer state
machine."
REFERENCE
"9.4.1, reAuthPeriod"
DEFVAL { 3600 }
::= { dot1xAuthConfigEntry 12 }
dot1xAuthReAuthEnabled OBJECT-TYPE
SYNTAX TruthValue
MAX-ACCESS read-write
STATUS current
DESCRIPTION
"The enable/disable control used by the Reauthentication
Timer state machine (8.5.5.1)."
REFERENCE
"9.4.1, reAuthEnabled"
DEFVAL { false }
::= { dot1xAuthConfigEntry 13 }
dot1xAuthKeyTxEnabled OBJECT-TYPE
SYNTAX TruthValue
MAX-ACCESS read-write
STATUS current
DESCRIPTION
"The value of the keyTransmissionEnabled constant
currently in use by the Authenticator PAE state
machine."
REFERENCE
"9.4.1, keyTransmissionEnabled"
::= { dot1xAuthConfigEntry 14 }
-- ---------------------------------------------------------- --
-- The Authenticator Statistics Table
-- ---------------------------------------------------------- --
dot1xAuthStatsTable OBJECT-TYPE
SYNTAX SEQUENCE OF Dot1xAuthStatsEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"A table that contains the statistics objects for the
Authenticator PAE associated with each Port.
An entry appears in this table for each port that may
authenticate access to itself."
REFERENCE
"9.4.2 Authenticator Statistics"
::= { dot1xPaeAuthenticator 2 }
dot1xAuthStatsEntry OBJECT-TYPE
SYNTAX Dot1xAuthStatsEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"The statistics information for an Authenticator PAE."
INDEX { dot1xPaePortNumber }
::= { dot1xAuthStatsTable 1 }
Dot1xAuthStatsEntry ::=
SEQUENCE {
dot1xAuthEapolFramesRx
Counter32,
dot1xAuthEapolFramesTx
Counter32,
dot1xAuthEapolStartFramesRx
Counter32,
dot1xAuthEapolLogoffFramesRx
Counter32,
dot1xAuthEapolRespIdFramesRx
Counter32,
dot1xAuthEapolRespFramesRx
Counter32,
dot1xAuthEapolReqIdFramesTx
Counter32,
dot1xAuthEapolReqFramesTx
Counter32,
dot1xAuthInvalidEapolFramesRx
Counter32,
dot1xAuthEapLengthErrorFramesRx
Counter32,
dot1xAuthLastEapolFrameVersion
Unsigned32,
dot1xAuthLastEapolFrameSource
MacAddress
}
dot1xAuthEapolFramesRx OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of valid EAPOL frames of any type
that have been received by this Authenticator."
REFERENCE
"9.4.2, EAPOL frames received"
::= { dot1xAuthStatsEntry 1 }
dot1xAuthEapolFramesTx OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of EAPOL frames of any type
that have been transmitted by this Authenticator."
REFERENCE
"9.4.2, EAPOL frames transmitted"
::= { dot1xAuthStatsEntry 2 }
dot1xAuthEapolStartFramesRx OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of EAPOL Start frames that have
been received by this Authenticator."
REFERENCE
"9.4.2, EAPOL Start frames received"
::= { dot1xAuthStatsEntry 3 }
dot1xAuthEapolLogoffFramesRx OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of EAPOL Logoff frames that have
been received by this Authenticator."
REFERENCE
"9.4.2, EAPOL Logoff frames received"
::= { dot1xAuthStatsEntry 4 }
dot1xAuthEapolRespIdFramesRx OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of EAP Resp/Id frames that have
been received by this Authenticator."
REFERENCE
"9.4.2, EAPOL Resp/Id frames received"
::= { dot1xAuthStatsEntry 5 }
dot1xAuthEapolRespFramesRx OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of valid EAP Response frames
(other than Resp/Id frames) that have been
received by this Authenticator."
REFERENCE
"9.4.2, EAPOL Response frames received"
::= { dot1xAuthStatsEntry 6 }
dot1xAuthEapolReqIdFramesTx OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of EAP Req/Id frames that have been
transmitted by this Authenticator."
REFERENCE
"9.4.2, EAPOL Req/Id frames transmitted"
::= { dot1xAuthStatsEntry 7 }
dot1xAuthEapolReqFramesTx OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of EAP Request frames
(other than Rq/Id frames) that have been
transmitted by this Authenticator."
REFERENCE
"9.4.2, EAPOL Request frames transmitted"
::= { dot1xAuthStatsEntry 8 }
dot1xAuthInvalidEapolFramesRx OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of EAPOL frames that have been
received by this Authenticator in which the
frame type is not recognized."
REFERENCE
"9.4.2, Invalid EAPOL frames received"
::= { dot1xAuthStatsEntry 9 }
dot1xAuthEapLengthErrorFramesRx OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of EAPOL frames that have been received
by this Authenticator in which the Packet Body
Length field is invalid."
REFERENCE
"9.4.2, EAP length error frames received"
::= { dot1xAuthStatsEntry 10 }
dot1xAuthLastEapolFrameVersion OBJECT-TYPE
SYNTAX Unsigned32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The protocol version number carried in the
most recently received EAPOL frame."
REFERENCE
"9.4.2, Last EAPOL frame version"
::= { dot1xAuthStatsEntry 11 }
dot1xAuthLastEapolFrameSource OBJECT-TYPE
SYNTAX MacAddress
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The source MAC address carried in the
most recently received EAPOL frame."
REFERENCE
"9.4.2, Last EAPOL frame source"
::= { dot1xAuthStatsEntry 12 }
-- ---------------------------------------------------------- --
-- The Authenticator Diagnostics Table
-- ---------------------------------------------------------- --
dot1xAuthDiagTable OBJECT-TYPE
SYNTAX SEQUENCE OF Dot1xAuthDiagEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"A table that contains the diagnostics objects for the
Authenticator PAE associated with each Port.
An entry appears in this table for each port that may
authenticate access to itself."
REFERENCE
"9.4.3 Authenticator Diagnostics"
::= { dot1xPaeAuthenticator 3 }
dot1xAuthDiagEntry OBJECT-TYPE
SYNTAX Dot1xAuthDiagEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"The diagnostics information for an Authenticator PAE."
INDEX { dot1xPaePortNumber }
::= { dot1xAuthDiagTable 1 }
Dot1xAuthDiagEntry ::=
SEQUENCE {
dot1xAuthEntersConnecting
Counter32,
dot1xAuthEapLogoffsWhileConnecting
Counter32,
dot1xAuthEntersAuthenticating
Counter32,
dot1xAuthAuthSuccessWhileAuthenticating
Counter32,
dot1xAuthAuthTimeoutsWhileAuthenticating
Counter32,
dot1xAuthAuthFailWhileAuthenticating
Counter32,
dot1xAuthAuthReauthsWhileAuthenticating
Counter32,
dot1xAuthAuthEapStartsWhileAuthenticating
Counter32,
dot1xAuthAuthEapLogoffWhileAuthenticating
Counter32,
dot1xAuthAuthReauthsWhileAuthenticated
Counter32,
dot1xAuthAuthEapStartsWhileAuthenticated
Counter32,
dot1xAuthAuthEapLogoffWhileAuthenticated
Counter32,
dot1xAuthBackendResponses
Counter32,
dot1xAuthBackendAccessChallenges
Counter32,
dot1xAuthBackendOtherRequestsToSupplicant
Counter32,
dot1xAuthBackendNonNakResponsesFromSupplicant
Counter32,
dot1xAuthBackendAuthSuccesses
Counter32,
dot1xAuthBackendAuthFails
Counter32
}
dot1xAuthEntersConnecting OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Counts the number of times that the state machine
transitions to the CONNECTING state from any other
state."
REFERENCE
"9.4.2, 8.5.4.2.1"
::= { dot1xAuthDiagEntry 1 }
dot1xAuthEapLogoffsWhileConnecting OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Counts the number of times that the state machine
transitions from CONNECTING to DISCONNECTED as a result
of receiving an EAPOL-Logoff message."
REFERENCE
"9.4.2, 8.5.4.2.2"
::= { dot1xAuthDiagEntry 2 }
dot1xAuthEntersAuthenticating OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Counts the number of times that the state machine
transitions from CONNECTING to AUTHENTICATING, as a
result of an EAP-Response/Identity message being
received from the Supplicant."
REFERENCE
"9.4.2, 8.5.4.2.3"
::= { dot1xAuthDiagEntry 3 }
dot1xAuthAuthSuccessWhileAuthenticating OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Counts the number of times that the state machine
transitions from AUTHENTICATING to AUTHENTICATED, as a
result of the Backend Authentication state machine
indicating successful authentication of the Supplicant
(authSuccess = TRUE)."
REFERENCE
"9.4.2, 8.5.4.2.4"
::= { dot1xAuthDiagEntry 4 }
dot1xAuthAuthTimeoutsWhileAuthenticating OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Counts the number of times that the state machine
transitions from AUTHENTICATING to ABORTING, as a result
of the Backend Authentication state machine indicating
authentication timeout (authTimeout = TRUE)."
REFERENCE
"9.4.2, 8.5.4.2.5"
::= { dot1xAuthDiagEntry 5 }
dot1xAuthAuthFailWhileAuthenticating OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Counts the number of times that the state machine
transitions from AUTHENTICATING to HELD, as a result
of the Backend Authentication state machine indicating
authentication failure (authFail = TRUE)."
REFERENCE
"9.4.2, 8.5.4.2.6"
::= { dot1xAuthDiagEntry 6 }
dot1xAuthAuthReauthsWhileAuthenticating OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Counts the number of times that the state machine
transitions from AUTHENTICATING to ABORTING, as a result
of a reauthentication request (reAuthenticate = TRUE)."
REFERENCE
"9.4.2, 8.5.4.2.7"
::= { dot1xAuthDiagEntry 7 }
dot1xAuthAuthEapStartsWhileAuthenticating OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Counts the number of times that the state machine
transitions from AUTHENTICATING to ABORTING, as a result
of an EAPOL-Start message being received
from the Supplicant."
REFERENCE
"9.4.2, 8.5.4.2.8"
::= { dot1xAuthDiagEntry 8 }
dot1xAuthAuthEapLogoffWhileAuthenticating OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Counts the number of times that the state machine
transitions from AUTHENTICATING to ABORTING, as a result
of an EAPOL-Logoff message being received
from the Supplicant."
REFERENCE
"9.4.2, 8.5.4.2.9"
::= { dot1xAuthDiagEntry 9 }
dot1xAuthAuthReauthsWhileAuthenticated OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Counts the number of times that the state machine
transitions from AUTHENTICATED to CONNECTING, as a
result of a reauthentication request
(reAuthenticate = TRUE)."
REFERENCE
"9.4.2, 8.5.4.2.10"
::= { dot1xAuthDiagEntry 10 }
dot1xAuthAuthEapStartsWhileAuthenticated OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Counts the number of times that the state machine
transitions from AUTHENTICATED to CONNECTING, as a
result of an EAPOL-Start message being received from the
Supplicant."
REFERENCE
"9.4.2, 8.5.4.2.11"
::= { dot1xAuthDiagEntry 11 }
dot1xAuthAuthEapLogoffWhileAuthenticated OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Counts the number of times that the state machine
transitions from AUTHENTICATED to DISCONNECTED, as a
result of an EAPOL-Logoff message being received from
the Supplicant."
REFERENCE
"9.4.2, 8.5.4.2.12"
::= { dot1xAuthDiagEntry 12 }
dot1xAuthBackendResponses OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Counts the number of times that the state machine sends
an initial Access-Request packet to the Authentication
server (i.e., executes sendRespToServer on entry to the
RESPONSE state). Indicates that the Authenticator
attempted communication with the Authentication Server."
REFERENCE
"9.4.2, 8.5.6.2.1"
::= { dot1xAuthDiagEntry 13 }
dot1xAuthBackendAccessChallenges OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Counts the number of times that the state machine
receives an initial Access-Challenge packet from the
Authentication server (i.e., aReq becomes TRUE,
causing exit from the RESPONSE state). Indicates that
the Authentication Server has communication with
the Authenticator."
REFERENCE
"9.4.2, 8.5.6.2.2"
::= { dot1xAuthDiagEntry 14 }
dot1xAuthBackendOtherRequestsToSupplicant OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Counts the number of times that the state machine
sends an EAP-Request packet (other than an Identity,
Notification, Failure or Success message) to the
Supplicant (i.e., executes txReq on entry to the
REQUEST state). Indicates that the Authenticator chose
an EAP-method."
REFERENCE
"9.4.2, 8.5.6.2.3"
::= { dot1xAuthDiagEntry 15 }
dot1xAuthBackendNonNakResponsesFromSupplicant OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Counts the number of times that the state machine
receives a response from the Supplicant to an initial
EAP-Request, and the response is something other than
EAP-NAK (i.e., rxResp becomes TRUE, causing the state
machine to transition from REQUEST to RESPONSE,
and the response is not an EAP-NAK). Indicates that
the Supplicant can respond to the Authenticator's
chosen EAP-method."
REFERENCE
"9.4.2, 8.5.6.2.4"
::= { dot1xAuthDiagEntry 16 }
dot1xAuthBackendAuthSuccesses OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Counts the number of times that the state machine
receives an EAP-Success message from the Authentication
Server (i.e., aSuccess becomes TRUE, causing a
transition from RESPONSE to SUCCESS). Indicates that
the Supplicant has successfully authenticated to
the Authentication Server."
REFERENCE
"9.4.2, 8.5.6.2.5"
::= { dot1xAuthDiagEntry 17 }
dot1xAuthBackendAuthFails OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Counts the number of times that the state machine
receives an EAP-Failure message from the Authentication
Server (i.e., aFail becomes TRUE, causing a transition
from RESPONSE to FAIL). Indicates that the Supplicant
has not authenticated to the Authentication Server."
REFERENCE
"9.4.2, 8.5.6.2.6"
::= { dot1xAuthDiagEntry 18 }
-- ---------------------------------------------------------- --
-- The Authenticator Session Statistics Table
-- ---------------------------------------------------------- --
dot1xAuthSessionStatsTable OBJECT-TYPE
SYNTAX SEQUENCE OF Dot1xAuthSessionStatsEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"A table that contains the session statistics objects
for the Authenticator PAE associated with each Port.
An entry appears in this table for each port that may
authenticate access to itself."
REFERENCE
"9.4.4"
::= { dot1xPaeAuthenticator 4 }
dot1xAuthSessionStatsEntry OBJECT-TYPE
SYNTAX Dot1xAuthSessionStatsEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"The session statistics information for an Authenticator
PAE. This shows the current values being collected for
each session that is still in progress, or the final
values for the last valid session on each port where
there is no session currently active."
INDEX { dot1xPaePortNumber }
::= { dot1xAuthSessionStatsTable 1 }
Dot1xAuthSessionStatsEntry ::=
SEQUENCE {
dot1xAuthSessionOctetsRx
Counter64,
dot1xAuthSessionOctetsTx
Counter64,
dot1xAuthSessionFramesRx
Counter32,
dot1xAuthSessionFramesTx
Counter32,
dot1xAuthSessionId
SnmpAdminString,
dot1xAuthSessionAuthenticMethod
INTEGER,
dot1xAuthSessionTime
TimeTicks,
dot1xAuthSessionTerminateCause
INTEGER,
dot1xAuthSessionUserName
SnmpAdminString
}
dot1xAuthSessionOctetsRx OBJECT-TYPE
SYNTAX Counter64
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of octets received in user data
frames on this Port during the session."
REFERENCE
"9.4.4, Session Octets Received"
::= { dot1xAuthSessionStatsEntry 1 }
dot1xAuthSessionOctetsTx OBJECT-TYPE
SYNTAX Counter64
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of octets transmitted in user data
frames on this Port during the session."
REFERENCE
"9.4.4, Session Octets Transmitted"
::= { dot1xAuthSessionStatsEntry 2 }
dot1xAuthSessionFramesRx OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of user data frames received
on this Port during the session."
REFERENCE
"9.4.4, Session Frames Received"
::= { dot1xAuthSessionStatsEntry 3 }
dot1xAuthSessionFramesTx OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of user data frames transmitted
on this Port during the session."
REFERENCE
"9.4.4, Session Frames Transmitted"
::= { dot1xAuthSessionStatsEntry 4 }
dot1xAuthSessionId OBJECT-TYPE
SYNTAX SnmpAdminString
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"A unique identifier for the session, in the
form of a printable ASCII string of at least
three characters."
REFERENCE
"9.4.4, Session Identifier"
::= { dot1xAuthSessionStatsEntry 5 }
dot1xAuthSessionAuthenticMethod OBJECT-TYPE
SYNTAX INTEGER {
remoteAuthServer(1),
localAuthServer(2)
}
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The authentication method used to establish the
session."
REFERENCE
"9.4.4, Session Authentication Method"
::= { dot1xAuthSessionStatsEntry 6 }
dot1xAuthSessionTime OBJECT-TYPE
SYNTAX TimeTicks
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The duration of the session in seconds."
REFERENCE
"9.4.4, Session Time"
::= { dot1xAuthSessionStatsEntry 7 }
dot1xAuthSessionTerminateCause OBJECT-TYPE
SYNTAX INTEGER {
supplicantLogoff(1),
portFailure(2),
supplicantRestart(3),
reauthFailed(4),
authControlForceUnauth(5),
portReInit(6),
portAdminDisabled(7),
notTerminatedYet(999)
}
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The reason for the session termination."
REFERENCE
"9.4.4, Session Terminate Cause"
::= { dot1xAuthSessionStatsEntry 8 }
dot1xAuthSessionUserName OBJECT-TYPE
SYNTAX SnmpAdminString
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The User-Name representing the identity of the
Supplicant PAE."
REFERENCE
"9.4.4, Session User Name"
::= { dot1xAuthSessionStatsEntry 9 }
-- ---------------------------------------------------------- --
-- The PAE Supplicant Group
-- ---------------------------------------------------------- --
-- ---------------------------------------------------------- --
-- The Supplicant Configuration Table
-- ---------------------------------------------------------- --
dot1xSuppConfigTable OBJECT-TYPE
SYNTAX SEQUENCE OF Dot1xSuppConfigEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"A table that contains the configuration objects for the
Supplicant PAE associated with each port.
An entry appears in this table for each port that may
authenticate itself when challenged by a remote system."
REFERENCE
"9.5.1"
::= { dot1xPaeSupplicant 1 }
dot1xSuppConfigEntry OBJECT-TYPE
SYNTAX Dot1xSuppConfigEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"The configuration information for a Supplicant PAE."
INDEX { dot1xPaePortNumber }
::= { dot1xSuppConfigTable 1 }
Dot1xSuppConfigEntry ::=
SEQUENCE {
dot1xSuppPaeState
INTEGER,
dot1xSuppHeldPeriod
Unsigned32,
dot1xSuppAuthPeriod
Unsigned32,
dot1xSuppStartPeriod
Unsigned32,
dot1xSuppMaxStart
Unsigned32
}
dot1xSuppPaeState OBJECT-TYPE
SYNTAX INTEGER {
disconnected(1),
logoff(2),
connecting(3),
authenticating(4),
authenticated(5),
acquired(6),
held(7)
}
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The current state of the Supplicant PAE state
machine (8.5.8)."
REFERENCE
"9.5.1, Supplicant PAE State"
::= { dot1xSuppConfigEntry 1 }
dot1xSuppHeldPeriod OBJECT-TYPE
SYNTAX Unsigned32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The value, in seconds, of the heldPeriod
constant currently in use by the Supplicant
PAE state machine (8.5.8.1.2)."
REFERENCE
"9.5.1, heldPeriod"
DEFVAL { 60 }
::= { dot1xSuppConfigEntry 2 }
dot1xSuppAuthPeriod OBJECT-TYPE
SYNTAX Unsigned32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The value, in seconds, of the authPeriod
constant currently in use by the Supplicant
PAE state machine (8.5.8.1.2)."
REFERENCE
"9.5.1, authPeriod"
DEFVAL { 30 }
::= { dot1xSuppConfigEntry 3 }
dot1xSuppStartPeriod OBJECT-TYPE
SYNTAX Unsigned32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The value, in seconds, of the startPeriod
constant currently in use by the Supplicant
PAE state machine (8.5.8.1.2)."
REFERENCE
"9.5.1, startPeriod"
DEFVAL { 30 }
::= { dot1xSuppConfigEntry 4 }
dot1xSuppMaxStart OBJECT-TYPE
SYNTAX Unsigned32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The value of the maxStart constant currently in use by
the Supplicant PAE state machine (8.5.8.1.2)."
REFERENCE
"9.5.1, maxStart"
DEFVAL { 3}
::= { dot1xSuppConfigEntry 5 }
-- ---------------------------------------------------------- --
-- The Supplicant Statistics Table
-- ---------------------------------------------------------- --
dot1xSuppStatsTable OBJECT-TYPE
SYNTAX SEQUENCE OF Dot1xSuppStatsEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"A table that contains the statistics objects for the
Supplicant PAE associated with each port.
An entry appears in this table for each port that may
authenticate itself when challenged by a remote system."
REFERENCE
"9.5.2"
::= { dot1xPaeSupplicant 2 }
dot1xSuppStatsEntry OBJECT-TYPE
SYNTAX Dot1xSuppStatsEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"The statistics information for a Supplicant PAE."
INDEX { dot1xPaePortNumber }
::= { dot1xSuppStatsTable 1 }
Dot1xSuppStatsEntry ::=
SEQUENCE {
dot1xSuppEapolFramesRx
Counter32,
dot1xSuppEapolFramesTx
Counter32,
dot1xSuppEapolStartFramesTx
Counter32,
dot1xSuppEapolLogoffFramesTx
Counter32,
dot1xSuppEapolRespIdFramesTx
Counter32,
dot1xSuppEapolRespFramesTx
Counter32,
dot1xSuppEapolReqIdFramesRx
Counter32,
dot1xSuppEapolReqFramesRx
Counter32,
dot1xSuppInvalidEapolFramesRx
Counter32,
dot1xSuppEapLengthErrorFramesRx
Counter32,
dot1xSuppLastEapolFrameVersion
Unsigned32,
dot1xSuppLastEapolFrameSource
MacAddress
}
dot1xSuppEapolFramesRx OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of EAPOL frames of any type
that have been received by this Supplicant."
REFERENCE
"9.5.2, EAPOL frames received"
::= { dot1xSuppStatsEntry 1 }
dot1xSuppEapolFramesTx OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of EAPOL frames of any type
that have been transmitted by this Supplicant."
REFERENCE
"9.5.2, EAPOL frames transmitted"
::= { dot1xSuppStatsEntry 2 }
dot1xSuppEapolStartFramesTx OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of EAPOL Start frames
that have been transmitted by this Supplicant."
REFERENCE
"9.5.2, EAPOL Start frames transmitted"
::= { dot1xSuppStatsEntry 3 }
dot1xSuppEapolLogoffFramesTx OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of EAPOL Logoff frames
that have been transmitted by this Supplicant."
REFERENCE
"9.5.2, EAPOL Logoff frames transmitted"
::= { dot1xSuppStatsEntry 4 }
dot1xSuppEapolRespIdFramesTx OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of EAP Resp/Id frames
that have been transmitted by this Supplicant."
REFERENCE
"9.5.2, EAP Resp/Id frames transmitted"
::= { dot1xSuppStatsEntry 5 }
dot1xSuppEapolRespFramesTx OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of valid EAP Response frames
(other than Resp/Id frames)
that have been transmitted by this Supplicant."
REFERENCE
"9.5.2, EAP Resp frames transmitted"
::= { dot1xSuppStatsEntry 6 }
dot1xSuppEapolReqIdFramesRx OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of EAP Req/Id frames
that have been received by this Supplicant."
REFERENCE
"9.5.2, EAP Req/Id frames received"
::= { dot1xSuppStatsEntry 7 }
dot1xSuppEapolReqFramesRx OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of EAP Request frames (other than Rq/Id
frames) that have been received by this Supplicant."
REFERENCE
"9.5.2, EAP Req frames received"
::= { dot1xSuppStatsEntry 8 }
dot1xSuppInvalidEapolFramesRx OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of EAPOL frames that have been
received by this Supplicant in which the
frame type is not recognized."
REFERENCE
"9.5.2, Invalid EAPOL frames received"
::= { dot1xSuppStatsEntry 9 }
dot1xSuppEapLengthErrorFramesRx OBJECT-TYPE
SYNTAX Counter32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The number of EAPOL frames that have been
received by this Supplicant in which the Packet
Body Length field (7.5.5) is invalid."
REFERENCE
"9.5.2, EAP length error frames received"
::= { dot1xSuppStatsEntry 10 }
dot1xSuppLastEapolFrameVersion OBJECT-TYPE
SYNTAX Unsigned32
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The protocol version number carried in the
most recently received EAPOL frame."
REFERENCE
"9.5.2, Last EAPOL frame version"
::= { dot1xSuppStatsEntry 11 }
dot1xSuppLastEapolFrameSource OBJECT-TYPE
SYNTAX MacAddress
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The source MAC address carried in the
most recently received EAPOL frame."
REFERENCE
"9.5.2, Last EAPOL frame source"
::= { dot1xSuppStatsEntry 12 }
-- ---------------------------------------------------------- --
-- IEEE 802.1X MIB - Conformance Information
-- ---------------------------------------------------------- --
dot1xPaeConformance OBJECT IDENTIFIER ::= { ieee8021paeMIB 2 }
dot1xPaeGroups OBJECT IDENTIFIER ::= { dot1xPaeConformance 1 }
dot1xPaeCompliances OBJECT IDENTIFIER
::= { dot1xPaeConformance 2 }
-- ---------------------------------------------------------- --
-- units of conformance
-- ---------------------------------------------------------- --
dot1xPaeSystemGroup OBJECT-GROUP
OBJECTS {
dot1xPaeSystemAuthControl,
dot1xPaePortProtocolVersion,
dot1xPaePortCapabilities,
dot1xPaePortInitialize
}
STATUS current
DESCRIPTION
"A collection of objects providing system information
about, and control over, a PAE."
::= { dot1xPaeGroups 1 }
dot1xPaeAuthConfigGroup OBJECT-GROUP
OBJECTS {
dot1xAuthPaeState,
dot1xAuthBackendAuthState,
dot1xAuthAdminControlledDirections,
dot1xAuthOperControlledDirections,
dot1xAuthAuthControlledPortStatus,
dot1xAuthAuthControlledPortControl,
dot1xAuthQuietPeriod,
dot1xAuthTxPeriod,
dot1xAuthSuppTimeout,
dot1xAuthServerTimeout,
dot1xAuthMaxReq,
dot1xAuthReAuthPeriod,
dot1xAuthReAuthEnabled,
dot1xAuthKeyTxEnabled
}
STATUS current
DESCRIPTION
"A collection of objects providing configuration
information about an Authenticator PAE."
::= { dot1xPaeGroups 2 }
dot1xPaeAuthStatsGroup OBJECT-GROUP
OBJECTS {
dot1xAuthEapolFramesRx,
dot1xAuthEapolFramesTx,
dot1xAuthEapolStartFramesRx,
dot1xAuthEapolLogoffFramesRx,
dot1xAuthEapolRespIdFramesRx,
dot1xAuthEapolRespFramesRx,
dot1xAuthEapolReqIdFramesTx,
dot1xAuthEapolReqFramesTx,
dot1xAuthInvalidEapolFramesRx,
dot1xAuthEapLengthErrorFramesRx,
dot1xAuthLastEapolFrameVersion,
dot1xAuthLastEapolFrameSource
}
STATUS current
DESCRIPTION
"A collection of objects providing statistics about an
Authenticator PAE."
::= { dot1xPaeGroups 3 }
dot1xPaeAuthDiagGroup OBJECT-GROUP
OBJECTS {
dot1xAuthEntersConnecting,
dot1xAuthEapLogoffsWhileConnecting,
dot1xAuthEntersAuthenticating,
dot1xAuthAuthSuccessWhileAuthenticating,
dot1xAuthAuthTimeoutsWhileAuthenticating,
dot1xAuthAuthFailWhileAuthenticating,
dot1xAuthAuthReauthsWhileAuthenticating,
dot1xAuthAuthEapStartsWhileAuthenticating,
dot1xAuthAuthEapLogoffWhileAuthenticating,
dot1xAuthAuthReauthsWhileAuthenticated,
dot1xAuthAuthEapStartsWhileAuthenticated,
dot1xAuthAuthEapLogoffWhileAuthenticated,
dot1xAuthBackendResponses,
dot1xAuthBackendAccessChallenges,
dot1xAuthBackendOtherRequestsToSupplicant,
dot1xAuthBackendNonNakResponsesFromSupplicant,
dot1xAuthBackendAuthSuccesses,
dot1xAuthBackendAuthFails
}
STATUS current
DESCRIPTION
"A collection of objects providing diagnostic statistics
about an Authenticator PAE."
::= { dot1xPaeGroups 4 }
dot1xPaeAuthSessionStatsGroup OBJECT-GROUP
OBJECTS {
dot1xAuthSessionOctetsRx,
dot1xAuthSessionOctetsTx,
dot1xAuthSessionFramesRx,
dot1xAuthSessionFramesTx,
dot1xAuthSessionId,
dot1xAuthSessionAuthenticMethod,
dot1xAuthSessionTime,
dot1xAuthSessionTerminateCause
}
STATUS current
DESCRIPTION
"A collection of objects providing statistics about the
current, or last session for an Authenticator PAE."
::= { dot1xPaeGroups 5 }
dot1xPaeSuppConfigGroup OBJECT-GROUP
OBJECTS {
dot1xSuppPaeState,
dot1xSuppHeldPeriod,
dot1xSuppAuthPeriod,
dot1xSuppStartPeriod,
dot1xSuppMaxStart
}
STATUS current
DESCRIPTION
"A collection of objects providing configuration
information about a Supplicant PAE."
::= { dot1xPaeGroups 6 }
dot1xPaeSuppStatsGroup OBJECT-GROUP
OBJECTS {
dot1xSuppEapolFramesRx,
dot1xSuppEapolFramesTx,
dot1xSuppEapolStartFramesTx,
dot1xSuppEapolLogoffFramesTx,
dot1xSuppEapolRespIdFramesTx,
dot1xSuppEapolRespFramesTx,
dot1xSuppEapolReqIdFramesRx,
dot1xSuppEapolReqFramesRx,
dot1xSuppInvalidEapolFramesRx,
dot1xSuppEapLengthErrorFramesRx,
dot1xSuppLastEapolFrameVersion,
dot1xSuppLastEapolFrameSource
}
STATUS current
DESCRIPTION
"A collection of objects providing statistics about a
Supplicant PAE."
::= { dot1xPaeGroups 7 }
-- ---------------------------------------------------------- --
-- compliance statements
-- ---------------------------------------------------------- --
dot1xPaeCompliance MODULE-COMPLIANCE
STATUS current
DESCRIPTION
"The compliance statement for device support of
Port Access Control."
MODULE
MANDATORY-GROUPS {
dot1xPaeSystemGroup
}
GROUP dot1xPaeAuthConfigGroup
DESCRIPTION
"This group is mandatory for systems that support
the Authenticator functions of the PAE."
OBJECT dot1xAuthAdminControlledDirections
SYNTAX INTEGER {
both(0)
}
MIN-ACCESS read-only
DESCRIPTION
"Support for in(1) is optional."
OBJECT dot1xAuthOperControlledDirections
SYNTAX INTEGER {
both(0)
}
DESCRIPTION
"Support for in(1) is optional."
OBJECT dot1xAuthKeyTxEnabled
MIN-ACCESS read-only
DESCRIPTION
"An Authenticator PAE that does not support
EAPOL-Key frames may implement this object as
read-only, returning a value of FALSE."
GROUP dot1xPaeAuthStatsGroup
DESCRIPTION
"This group is mandatory for systems that support
the Authenticator functions of the PAE."
GROUP dot1xPaeAuthDiagGroup
DESCRIPTION
"This group is optional for systems that support
the Authenticator functions of the PAE."
GROUP dot1xPaeAuthSessionStatsGroup
DESCRIPTION
"This group is optional for systems that support
the Authenticator functions of the PAE."
GROUP dot1xPaeSuppConfigGroup
DESCRIPTION
"This group is mandatory for systems that support
the Supplicant functions of the PAE."
GROUP dot1xPaeSuppStatsGroup
DESCRIPTION
"This group is mandatory for systems that support
the Supplicant functions of the PAE."
::= { dot1xPaeCompliances 1 }
END

