-- MIB created 3/21/96 14:37:01, by
--   SMIC (the next generation) version 1.6.31, December 11, 1994.

SNMPv2-TC-v1 DEFINITIONS ::= BEGIN

-- From file: "rfc1443.sm2"
-- Compile options "G A"

IMPORTS
    TimeTicks
            FROM RFC1155-SMI;

-- No macro TEXTUAL-CONVENTION in SNMPv1

DisplayString ::= OCTET STRING
-- TEXTUAL-CONVENTION
--  DspHint
--    255a
--  Status
--    mandatory
--  Descr
--    Represents textual information taken from the NVT
--    ASCII character set, as defined in pages 4, 10-11
--    of RFC 854.  Any object defined using this syntax
--    may not exceed 255 characters in length.

PhysAddress ::= OCTET STRING
-- TEXTUAL-CONVENTION
--  DspHint
--    1x:
--  Status
--    mandatory
--  Descr
--    Represents media- or physical-level addresses.

MacAddress ::= OCTET STRING (SIZE (6))
-- TEXTUAL-CONVENTION
--  DspHint
--    1x:
--  Status
--    mandatory
--  Descr
--    Represents an 802 MAC address represented in the
--    'canonical' order defined by IEEE 802.1a, i.e., as
--    if it were transmitted least significant bit
--    first, even though 802.5 (in contrast to other
--    802.x protocols) requires MAC addresses to be
--    transmitted most significant bit first.

TruthValue ::= INTEGER {
        true(1),
        false(2)
        }
-- TEXTUAL-CONVENTION
--  Status
--    mandatory
--  Descr
--    Represents a boolean value.

TestAndIncr ::= INTEGER(0..2147483647)
-- TEXTUAL-CONVENTION
--  Status
--    mandatory
--  Descr
--    Represents integer-valued information used for
--    atomic operations.  When the management protocol
--    is used to specify that an object instance having
--    this syntax is to be modified, the new value
--    supplied via the management protocol must
--    precisely match the value presently held by the
--    instance.  If not, the management protocol set
--    operation fails with an error of
--    'inconsistentValue'.  Otherwise, if the current
--    value is the maximum value of 2^31-1 (2147483647
--    decimal), then the value held by the instance is
--    wrapped to zero; otherwise, the value held by the
--    instance is incremented by one.  (Note that
--    regardless of whether the management protocol set
--    operation succeeds, the variable-binding in the
--    request and response PDUs are identical.)
--    
--    The value of the ACCESS clause for objects having
--    this syntax is either 'read-write' or 'read-
--    create'.  When an instance of a columnar object
--    having this syntax is created, any value may be
--    supplied via the management protocol.

AutonomousType ::= OBJECT IDENTIFIER
-- TEXTUAL-CONVENTION
--  Status
--    mandatory
--  Descr
--    Represents an independently extensible type
--    identification value.  It may, for example,
--    indicate a particular sub-tree with further MIB
--    definitions, or define a particular type of
--    protocol or hardware.

InstancePointer ::= OBJECT IDENTIFIER
-- TEXTUAL-CONVENTION
--  Status
--    mandatory
--  Descr
--    A pointer to a specific instance of a conceptual
--    row of a MIB table in the managed device.  By
--    convention, it is the name of the particular
--    instance of the first columnar object in the
--    conceptual row.

RowStatus ::= INTEGER {
        active(1),
        notInService(2),
        notReady(3),
        createAndGo(4),
        createAndWait(5),
        destroy(6)
        }
-- TEXTUAL-CONVENTION
--  Status
--    mandatory
--  Descr
--    The RowStatus textual convention is used to
--    manage the creation and deletion of conceptual
--    rows, and is used as the value of the SYNTAX
--    clause for the status column of a conceptual row
--    (as described in Section 7.7.1 of [2].)
--    
--    The status column has six defined values:
--    
--         - 'active', which indicates that the
--         conceptual row is available for use by the
--         managed device;
--    
--         - 'notInService', which indicates that the
--         conceptual row exists in the agent, but is
--         unavailable for use by the managed device
--         (see NOTE below);
--    
--         - 'notReady', which indicates that the
--         conceptual row exists in the agent, but is
--         missing information necessary in order to be
--         available for use by the managed device;
--    
--         - 'createAndGo', which is supplied by a
--         management station wishing to create a new
--         instance of a conceptual row and to have it
--         available for use by the managed device;
--    
--         - 'createAndWait', which is supplied by a
--         management station wishing to create a new
--         instance of a conceptual row but not to have
--         it available for use by the managed device;
--         and,
--    
--         - 'destroy', which is supplied by a
--         management station wishing to delete all of
--         the instances associated with an existing
--         conceptual row.
--    
--    Whereas five of the six values (all except
--    'notReady') may be specified in a management
--    protocol set operation, only three values will be
--    returned in response to a management protocol
--    retrieval operation: 'notReady', 'notInService' or
--    'active'.  That is, when queried, an existing
--    conceptual row has only three states: it is either
--    available for use by the managed device (the
--    status column has value 'active'); it is not
--    available for use by the managed device, though
--    the agent has sufficient information to make it so
--    (the status column has value 'notInService'); or,
--    it is not available for use by the managed device,
--    because the agent lacks sufficient information
--    (the status column has value 'notReady').
--    
--                        NOTE WELL
--    
--         This textual convention may be used for a MIB
--         table, irrespective of whether the values of
--         that table's conceptual rows are able to be
--         modified while it is active, or whether its
--         conceptual rows must be taken out of service
--         in order to be modified.  That is, it is the
--         responsibility of the DESCRIPTION clause of
--         the status column to specify whether the
--         status column must be 'notInService' in order
--         for the value of some other column of the
--         same conceptual row to be modified.
--    
--    
--    To summarize the effect of having a conceptual row
--    with a status column having a SYNTAX clause value
--    of RowStatus, consider the following state
--    diagram:
--    
--    
--                          STATE
--    +==============+===========+=============+=============
--    |      A       |     B     |      C      |      D
--    |              |status col.|status column|
--    |status column |    is     |      is     |status column
--    ACTION    |does not exist|  notReady | notInService|  is active
--    ==============+==============+===========+=============+=============
--    set status    |noError    ->D|inconsist- |inconsistent-|inconsistent-
--    column to     |       or     |   entValue|        Value|        Value
--    createAndGo   |inconsistent- |           |             |
--    |         Value|           |             |
--    ==============+==============+===========+=============+=============
--    set status    |noError  see 1|inconsist- |inconsistent-|inconsistent-
--    column to     |       or     |   entValue|        Value|        Value
--    createAndWait |wrongValue    |           |             |
--    ==============+==============+===========+=============+=============
--    set status    |inconsistent- |inconsist- |noError      |noError
--    column to     |         Value|   entValue|             |
--    active        |              |           |             |
--    |              |     or    |             |
--    |              |           |             |
--    |              |see 2   ->D|          ->D|          ->D
--    ==============+==============+===========+=============+=============
--    set status    |inconsistent- |inconsist- |noError      |noError   ->C
--    column to     |         Value|   entValue|             |
--    notInService  |              |           |             |
--    |              |     or    |             |      or
--    |              |           |             |
--    |              |see 3   ->C|          ->C|wrongValue
--    ==============+==============+===========+=============+=============
--    set status    |noError       |noError    |noError      |noError
--    column to     |              |           |             |
--    destroy       |           ->A|        ->A|          ->A|          ->A
--    ==============+==============+===========+=============+=============
--    set any other |see 4         |noError    |noError      |noError
--    column to some|              |           |             |
--    value         |           ->A|      see 1|          ->C|          ->D
--    ==============+==============+===========+=============+=============
--    
--    
--    (1) goto B or C, depending on information
--    available to the agent.
--    
--    (2) if other variable bindings included in the
--    same PDU, provide values for all columns which are
--    missing but required, then return noError and goto
--    D.
--    
--    (3) if other variable bindings included in the
--    same PDU, provide values for all columns which are
--    missing but required, then return noError and goto
--    C.
--    
--    (4) at the discretion of the agent, either noError
--    or inconsistentValue may be returned.
--    
--    NOTE: Other processing of the set request may
--    result in a response other than noError being
--    returned, e.g., wrongValue, noCreation, etc.
--    
--    
--                 Conceptual Row Creation
--    
--    There are four potential interactions when
--    creating a conceptual row: selecting an instance-
--    identifier which is not in use; creating the
--    conceptual row; initializing any objects for which
--    the agent does not supply a default; and, making
--    the conceptual row available for use by the
--    managed device.
--    
--    Interaction 1: Selecting an Instance-Identifier
--    
--    The algorithm used to select an instance-
--    identifier varies for each conceptual row.  In
--    some cases, the instance-identifier is
--    semantically significant, e.g., the destination
--    address of a route, and a management station
--    selects the instance-identifier according to the
--    semantics.
--    
--    In other cases, the instance-identifier is used
--    solely to distinguish conceptual rows, and a
--    management station without specific knowledge of
--    the conceptual row might examine the instances
--    present in order to determine an unused instance-
--    identifier.  (This approach may be used, but it is
--    often highly sub-optimal; however, it is also a
--    questionable practice for a naive management
--    station to attempt conceptual row creation.)
--    
--    Alternately, the MIB module which defines the
--    conceptual row might provide one or more objects
--    which provide assistance in determining an unused
--    instance-identifier.  For example, if the
--    conceptual row is indexed by an integer-value,
--    then an object having an integer-valued SYNTAX
--    clause might be defined for such a purpose,
--    allowing a management station to issue a
--    management protocol retrieval operation.  In order
--    to avoid unnecessary collisions between competing
--    management stations, 'adjacent' retrievals of this
--    object should be different.
--    
--    Finally, the management station could select a
--    pseudo-random number to use as the index.  In the
--    event that this index was already in use and an
--    inconsistentValue was returned in response to the
--    management protocol set operation, the management
--    station should simply select a new pseudo-random
--    number and retry the operation.
--    
--    A MIB designer should choose between the two
--    latter algorithms based on the size of the table
--    (and therefore the efficiency of each algorithm).
--    For tables in which a large number of entries are
--    expected, it is recommended that a MIB object be
--    defined that returns an acceptable index for
--    creation.  For tables with small numbers of
--    entries, it is recommended that the latter
--    pseudo-random index mechanism be used.
--    
--    Interaction 2: Creating the Conceptual Row
--    
--    Once an unused instance-identifier has been
--    selected, the management station determines if it
--    wishes to create and activate the conceptual row
--    in one transaction or in a negotiated set of
--    interactions.
--    
--    Interaction 2a: Creating and Activating the
--    Conceptual Row
--    
--    The management station must first determine the
--    column requirements, i.e., it must determine those
--    columns for which it must or must not provide
--    values.  Depending on the complexity of the table
--    and the management station's knowledge of the
--    agent's capabilities, this determination can be
--    made locally by the management station.
--    Alternately, the management station issues a
--    management protocol get operation to examine all
--    columns in the conceptual row that it wishes to
--    create.  In response, for each column, there are
--    three possible outcomes:
--    
--         - a value is returned, indicating that some
--         other management station has already created
--         this conceptual row.  We return to
--         interaction 1.
--    
--         - the exception 'noSuchInstance' is returned,
--         indicating that the agent implements the
--         object-type associated with this column, and
--         that this column in at least one conceptual
--         row would be accessible in the MIB view used
--         by the retrieval were it to exist. For those
--         columns to which the agent provides read-
--         create access, the 'noSuchInstance' exception
--         tells the management station that it should
--         supply a value for this column when the
--         conceptual row is to be created.
--    
--         - the exception 'noSuchObject' is returned,
--         indicating that the agent does not implement
--         the object-type associated with this column
--         or that there is no conceptual row for which
--         this column would be accessible in the MIB
--         view used by the retrieval.  As such, the
--         management station can not issue any
--         management protocol set operations to create
--         an instance of this column.
--    
--    Once the column requirements have been determined,
--    a management protocol set operation is accordingly
--    issued.  This operation also sets the new instance
--    of the status column to 'createAndGo'.
--    
--    When the agent processes the set operation, it
--    verifies that it has sufficient information to
--    make the conceptual row available for use by the
--    managed device.  The information available to the
--    agent is provided by two sources: the management
--    protocol set operation which creates the
--    conceptual row, and, implementation-specific
--    defaults supplied by the agent (note that an agent
--    must provide implementation-specific defaults for
--    at least those objects which it implements as
--    read-only).  If there is sufficient information
--    available, then the conceptual row is created, a
--    'noError' response is returned, the status column
--    is set to 'active', and no further interactions
--    are necessary (i.e., interactions 3 and 4 are
--    skipped).  If there is insufficient information,
--    then the conceptual row is not created, and the
--    set operation fails with an error of
--    'inconsistentValue'.  On this error, the
--    management station can issue a management protocol
--    retrieval operation to determine if this was
--    because it failed to specify a value for a
--    required column, or, because the selected instance
--    of the status column already existed.  In the
--    latter case, we return to interaction 1.  In the
--    former case, the management station can re-issue
--    the set operation with the additional information,
--    or begin interaction 2 again using 'createAndWait'
--    in order to negotiate creation of the conceptual
--    row.
--    
--                        NOTE WELL
--    
--         Regardless of the method used to determine
--         the column requirements, it is possible that
--         the management station might deem a column
--         necessary when, in fact, the agent will not
--         allow that particular columnar instance to be
--         created or written.  In this case, the
--         management protocol set operation will fail
--         with an error such as 'noCreation' or
--         'notWritable'.  In this case, the management
--         station decides whether it needs to be able
--         to set a value for that particular columnar
--         instance.  If not, the management station
--         re-issues the management protocol set
--         operation, but without setting a value for
--         that particular columnar instance; otherwise,
--         the management station aborts the row
--         creation algorithm.
--    
--    Interaction 2b: Negotiating the Creation of the
--    Conceptual Row
--    
--    The management station issues a management
--    protocol set operation which sets the desired
--    instance of the status column to 'createAndWait'.
--    If the agent is unwilling to process a request of
--    this sort, the set operation fails with an error
--    of 'wrongValue'.  (As a consequence, such an agent
--    must be prepared to accept a single management
--    protocol set operation, i.e., interaction 2a
--    above, containing all of the columns indicated by
--    its column requirements.) Otherwise, the
--    conceptual row is created, a 'noError' response is
--    returned, and the status column is immediately set
--    to either 'notInService' or 'notReady', depending
--    on whether it has sufficient information to make
--    the conceptual row available for use by the
--    managed device.  If there is sufficient
--    information available, then the status column is
--    set to 'notInService'; otherwise, if there is
--    insufficient information, then the status column
--    is set to 'notReady'.  Regardless, we proceed to
--    interaction 3.
--    
--    Interaction 3: Initializing non-defaulted Objects
--    
--    The management station must now determine the
--    column requirements.  It issues a management
--    protocol get operation to examine all columns in
--    the created conceptual row.  In the response, for
--    each column, there are three possible outcomes:
--    
--         - a value is returned, indicating that the
--         agent implements the object-type associated
--         with this column and had sufficient
--         information to provide a value.  For those
--         columns to which the agent provides read-
--         create access, a value return tells the
--         management station that it may issue
--         additional management protocol set
--         operations, if it desires, in order to change
--         the value associated with this column.
--    
--         - the exception 'noSuchInstance' is returned,
--         indicating that the agent implements the
--         object-type associated with this column, and
--         that this column in at least one conceptual
--         row would be accessible in the MIB view used
--         by the retrieval were it to exist. However,
--         the agent does not have sufficient
--         information to provide a value, and until a
--         value is provided, the conceptual row may not
--         be made available for use by the managed
--         device.  For those columns to which the agent
--         provides read-create access, the
--         'noSuchInstance' exception tells the
--         management station that it must issue
--         additional management protocol set
--         operations, in order to provide a value
--         associated with this column.
--    
--         - the exception 'noSuchObject' is returned,
--         indicating that the agent does not implement
--         the object-type associated with this column
--         or that there is no conceptual row for which
--         this column would be accessible in the MIB
--         view used by the retrieval.  As such, the
--         management station can not issue any
--         management protocol set operations to create
--         an instance of this column.
--    
--    If the value associated with the status column is
--    'notReady', then the management station must first
--    deal with all 'noSuchInstance' columns, if any.
--    Having done so, the value of the status column
--    becomes 'notInService', and we proceed to
--    interaction 4.
--    
--    Interaction 4: Making the Conceptual Row Available
--    
--    Once the management station is satisfied with the
--    values associated with the columns of the
--    conceptual row, it issues a management protocol
--    set operation to set the status column to
--    'active'.  If the agent has sufficient information
--    to make the conceptual row available for use by
--    the managed device, the management protocol set
--    operation succeeds (a 'noError' response is
--    returned).  Otherwise, the management protocol set
--    operation fails with an error of
--    'inconsistentValue'.
--    
--                        NOTE WELL
--    
--         A conceptual row having a status column with
--         value 'notInService' or 'notReady' is
--         unavailable to the managed device.  As such,
--         it is possible for the managed device to
--         create its own instances during the time
--         between the management protocol set operation
--         which sets the status column to
--         'createAndWait' and the management protocol
--         set operation which sets the status column to
--         'active'.  In this case, when the management
--         protocol set operation is issued to set the
--         status column to 'active', the values held in
--         the agent supersede those used by the managed
--         device.
--    
--    If the management station is prevented from
--    setting the status column to 'active' (e.g., due
--    to management station or network failure) the
--    conceptual row will be left in the 'notInService'
--    or 'notReady' state, consuming resources
--    indefinitely.  The agent must detect conceptual
--    rows that have been in either state for an
--    abnormally long period of time and remove them.
--    This period of time should be long enough to allow
--    for human response time (including 'think time')
--    between the creation of the conceptual row and the
--    setting of the status to 'active'.  It is
--    suggested that this period be approximately 5
--    minutes in length.
--    
--    
--                Conceptual Row Suspension
--    
--    When a conceptual row is 'active', the management
--    station may issue a management protocol set
--    operation which sets the instance of the status
--    column to 'notInService'.  If the agent is
--    unwilling to do so, the set operation fails with
--    an error of 'wrongValue'.  Otherwise, the
--    conceptual row is taken out of service, and a
--    'noError' response is returned.  It is the
--    responsibility of the the DESCRIPTION clause of
--    the status column to indicate under what
--    circumstances the status column should be taken
--    out of service (e.g., in order for the value of
--    some other column of the same conceptual row to be
--    modified).
--    
--    
--                 Conceptual Row Deletion
--    
--    For deletion of conceptual rows, a management
--    protocol set operation is issued which sets the
--    instance of the status column to 'destroy'.  This
--    request may be made regardless of the current
--    value of the status column (e.g., it is possible
--    to delete conceptual rows which are either
--    'notReady', 'notInService' or 'active'.) If the
--    operation succeeds, then all instances associated
--    with the conceptual row are immediately removed.

TimeStamp ::= TimeTicks
-- TEXTUAL-CONVENTION
--  Status
--    mandatory
--  Descr
--    The value of MIB-II's sysUpTime object at which a
--    specific occurrence happened.  The specific
--    occurrence must be defined in the description of
--    any object defined using this type.

TimeInterval ::= INTEGER(0..2147483647)
-- TEXTUAL-CONVENTION
--  Status
--    mandatory
--  Descr
--    A period of time, measured in units of 0.01
--    seconds.

DateAndTime ::= OCTET STRING(SIZE(8..11))
-- TEXTUAL-CONVENTION
--  DspHint
--    2d-1d-1d,1d:1d:1d.1d,1a1d:1d
--  Status
--    mandatory
--  Descr
--    A date-time specification.
--    
--    field  octets  contents                  range
--    =====  ======  ========                  =====
--      1      1-2   year                      0..65536
--      2       3    month                     1..12
--      3       4    day                       1..31
--      4       5    hour                      0..23
--      5       6    minutes                   0..59
--      6       7    seconds                   0..60
--                   (use 60 for leap-second)
--      7       8    deci-seconds              0..9
--      8       9    direction from UTC        '+' / '-'
--      9      10    hours from UTC            0..11
--     10      11    minutes from UTC          0..59
--    
--    For example, Tuesday May 26, 1992 at 1:30:15 PM
--    EDT would be displayed as:
--    
--                1992-5-26,13:30:15.0,-4:0
--    
--    Note that if only local time is known, then
--    timezone information (fields 8-10) is not
--    present.


END
