-- *****************************************************************
-- CISCO-WLAN-MAN-MIB.my: CISCO Wireless LAN Management MIB file
--
-- February 2004, Francis Pang
--
-- Copyright (c) 2004 by Cisco Systems, Inc.
-- All rights reserved.
-- *****************************************************************
--
CISCO-WLAN-MAN-MIB DEFINITIONS ::= BEGIN

IMPORTS
        MODULE-IDENTITY,
        OBJECT-TYPE
                FROM SNMPv2-SMI
        MODULE-COMPLIANCE,
        OBJECT-GROUP
                FROM SNMPv2-CONF
        TruthValue
                FROM SNMPv2-TC
        ciscoMgmt
                FROM CISCO-SMI;


ciscoWlanManMIB MODULE-IDENTITY
        LAST-UPDATED    "200403220000Z"
        ORGANIZATION    "Cisco System Inc."
        CONTACT-INFO
                "       Cisco Systems
                        Customer Service

                Postal: 170 West Tasman Drive,
                        San Jose CA 95134-1706.
                        USA

                   Tel: +1 800 553-NETS

                 Email: cs-dot11@cisco.com"
        DESCRIPTION
                "This MIB module provides network management
                and configuration support for IEEE 802.11
                Wireless LAN devices.

                          ACRONYMS

                HTTP
                    Hypertext Transfer Protocol."

        REVISION        "200403220000Z"
        DESCRIPTION
                "Initial version of this MIB module."
        ::= { ciscoMgmt 415 }



ciscoWlanManMIBNotifs   OBJECT IDENTIFIER
        ::= { ciscoWlanManMIB 0 }

ciscoWlanManMIBObjects  OBJECT IDENTIFIER
        ::= { ciscoWlanManMIB 1 }

ciscoWlanManMIBConform  OBJECT IDENTIFIER
        ::= { ciscoWlanManMIB 2 }

cwmDeviceConfig         OBJECT IDENTIFIER
        ::= { ciscoWlanManMIBObjects 1 }

cwmNetworkConfig        OBJECT IDENTIFIER
        ::= { ciscoWlanManMIBObjects 2 }


-- Per device configurations

cwmHttpServerEnabled OBJECT-TYPE
        SYNTAX     TruthValue
        MAX-ACCESS read-write
        STATUS     current
        DESCRIPTION
                "This object enables the HTTP Web server as follows:
                    'true'  - HTTP Web server function is enabled,
                    'false' - HTTP Web server function is disabled."
        ::= { cwmDeviceConfig 1 }

cwmTelnetLoginEnabled OBJECT-TYPE
        SYNTAX     TruthValue
        MAX-ACCESS read-write
        STATUS     current
        DESCRIPTION
                "This object enables the telnet console login as 
                follows:                         
                    'true'  - telnet console login is enabled,
                    'false' - telnet console login is disabled."
        ::= { cwmDeviceConfig 2 }


-- *****************************************************************
--   Conformance information
-- *****************************************************************

ciscoWlanManMIBCompliances OBJECT IDENTIFIER
        ::= { ciscoWlanManMIBConform 1 }

ciscoWlanManMIBGroups OBJECT IDENTIFIER
        ::= { ciscoWlanManMIBConform 2 }



-- *****************************************************************
--   Compliance statements
-- *****************************************************************

ciscoWlanManMIBCompliance MODULE-COMPLIANCE
        STATUS     current
        DESCRIPTION
                "The compliance statement for the
                ciscoWlanManMIB module."
        MODULE
                MANDATORY-GROUPS {
                    cwmWirelessDeviceGroup
                }  
        ::= { ciscoWlanManMIBCompliances 1 }



-- *****************************************************************
--   Units of conformance
-- *****************************************************************

cwmWirelessDeviceGroup OBJECT-GROUP
        OBJECTS {
                cwmHttpServerEnabled,
                cwmTelnetLoginEnabled
                }
        STATUS     current
        DESCRIPTION
                "Configuration for Wireless LAN Access Points
                and bridges."
        ::= { ciscoWlanManMIBGroups 1 }

END

