-- ********************************************************************
-- CISCO-DS0-CROSS-CONNECT-MIB.my
--
-- March 2003, Kiet Tran
--
-- Copyright (c) 2003 by cisco Systems, Inc.
-- All rights reserved.
--
-- *********************************************************************
CISCO-DS0-CROSS-CONNECT-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Unsigned32
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    InterfaceIndex         
        FROM IF-MIB
    RowStatus
        FROM SNMPv2-TC
    ciscoMgmt
        FROM CISCO-SMI;

ciscoDs0CrossConnectMIB    MODULE-IDENTITY
    LAST-UPDATED  "200303050000Z"
    ORGANIZATION  "Cisco Systems, Inc."
    CONTACT-INFO
		  "Cisco Systems
                   Customer Service

                   Postal: 170 W. Tasman Drive
                           San Jose, CA  95134
                           USA

		   Tel: +1 800 553-NETS

		   E-mail: cs-voice@cisco.com"
    DESCRIPTION
        "The MIB for Ds0 cross connection.
	"
    REVISION "200303050000Z"
    DESCRIPTION
        "Initial version of the MIB module."
    ::= { ciscoMgmt 9999 }


ciscoDs0CrossConnectMIBNotifs      OBJECT IDENTIFIER 
    ::= { ciscoDs0CrossConnectMIB 0 }

ciscoDs0CrossConnectMIBObjects     OBJECT IDENTIFIER 
    ::= { ciscoDs0CrossConnectMIB 1 }

ciscoDs0CrossConnectMIBConformance OBJECT IDENTIFIER 
    ::= { ciscoDs0CrossConnectMIB 2 }

cDs0CrossConnectConfig             OBJECT IDENTIFIER 
    ::= { ciscoDs0CrossConnectMIBObjects 1 }


-- ---------------------------------------------------------------------
--  cds0CrossConnectConfigTable
-- ---------------------------------------------------------------------

cds0CrossConnectConfigTable  OBJECT-TYPE
    SYNTAX           SEQUENCE OF Cds0CrossConnectConfigEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "This table is used to establish a DS0 cross connection.
         A DS0 cross connect is established by binding a unique
         DS0 group containing one or more DS0s of a single Ds1 
         interface to another unique DS0 group containing one or 
         more DS0s of a single DS1 interface.  
        "
	::= { cDs0CrossConnectConfig 1 }

cds0CrossConnectConfigEntry  OBJECT-TYPE
    SYNTAX           Cds0CrossConnectConfigEntry
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
	"An entry in cds0CrossConnectConfigTable table represents a DS0 
         cross connection. The two end point of the connection are:
            end point 1: cds0Endpt1Ds1 cds0Endpt1Ds0Group
            end point 2: cds0Endpt2Ds1 cds0Endpt2Ds0Group

         The end points of this connection should be entries
         of ccasGrpCfgTable and 'ccasGrpCfgServiceType' of 
         of the entries should be 'tdmxconn'. The ccasGrpCfgTable is 
         defined in CISCO-CAS-IF-MIB.
        "
    INDEX {cds0Endpt1Ds1, cds0Endpt1Ds0Group }
    ::= { cds0CrossConnectConfigTable 1 }

Cds0CrossConnectConfigEntry ::=
    SEQUENCE {
              cds0Endpt1Ds1           InterfaceIndex,
              cds0Endpt1Ds0Group      Unsigned32,
              cds0Endpt2Ds1           InterfaceIndex,
              cds0Endpt2Ds0Group      Unsigned32,
              cds0ConnRowStatus       RowStatus
             }

cds0Endpt1Ds1        OBJECT-TYPE
    SYNTAX           InterfaceIndex
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "The value of this object equals to the 'ifIndex' of a
         Ds1 interface.
         This Ds1 interface is used as the first end point of the 
         Ds0 connection.
        "
    ::= { cds0CrossConnectConfigEntry 1}

cds0Endpt1Ds0Group   OBJECT-TYPE
    SYNTAX           Unsigned32 (0..31)
    MAX-ACCESS       not-accessible
    STATUS           current
    DESCRIPTION
        "The value of this object identifies a Ds0 group which contains 
         one of more Ds0(s) within the Ds1 interface represented by
         'cDs0Endpt1Ds1'.
         This Ds0 group is used as the first end point of the 
         Ds0 connection.
        "
    ::= { cds0CrossConnectConfigEntry 2 }

cds0Endpt2Ds1        OBJECT-TYPE
    SYNTAX           InterfaceIndex
    MAX-ACCESS       read-create 
    STATUS           current
    DESCRIPTION
        "The value of this object equals to the 'ifIndex' of a
         Ds1 interface.
         This Ds1 interface is used as the second end point of the 
         Ds0 connection.
        "
    ::= { cds0CrossConnectConfigEntry 3}

cds0Endpt2Ds0Group   OBJECT-TYPE
    SYNTAX           Unsigned32 (0..31)
    MAX-ACCESS       read-create 
    STATUS           current
    DESCRIPTION
        "The value of this object identifies a Ds0 group which contains 
         one of more Ds0(s) within the Ds1 interface represented by
         'cDs0Endpt2Ds1'.
         This Ds0 group is used as the second end point of the 
         Ds0 connection. 
        "
    ::= { cds0CrossConnectConfigEntry 4 }

cds0ConnRowStatus    OBJECT-TYPE
    SYNTAX	     RowStatus
    MAX-ACCESS       read-create
    STATUS           current
    DESCRIPTION		
        "This object is used to create or delete an entry.

         The mandatory objects for creating an entry in this table:
           'cds0Endpt2Ds1'
           'cds0Endpt2Ds0Group'

         The following objects are not allowed to be modified after 
         the entry to be added:
           'cds0Endpt2Ds1'
           'cds0Endpt2Ds0Group'
        "
    ::= { cds0CrossConnectConfigEntry 5 }

-- *********************************************************************
-- Conformance and compliance statements
-- *********************************************************************

ciscoDs0CrossConnectMIBCompliances   OBJECT IDENTIFIER ::= 
				{ ciscoDs0CrossConnectMIBConformance 1 }

ciscoDs0CrossConnectMIBGroups        OBJECT IDENTIFIER  ::= 
                                { ciscoDs0CrossConnectMIBConformance 2}

ciscoDs0CrossConnectMIBCompliance MODULE-COMPLIANCE

    STATUS	     current
    DESCRIPTION
        "The compliance statement for Cisco agents which implement
         the CISCO-DSO-CROSS-CONNECT-MIB." 
    MODULE
    MANDATORY-GROUPS { cDs0CrossConnectConfigGroup
	 	     }
    ::= {ciscoDs0CrossConnectMIBCompliances 1 }


-- *********************************************************************
-- units of conformance
-- *********************************************************************

cDs0CrossConnectConfigGroup  OBJECT-GROUP
    OBJECTS {   
             cds0Endpt2Ds1,           
             cds0Endpt2Ds0Group,        
             cds0ConnRowStatus    
	    }

    STATUS	     current
    DESCRIPTION
        "A collection of objects for general configuration of  
         Ds0 cross connection."
    ::= { ciscoDs0CrossConnectMIBGroups 1 }

END

