-- *****************************************************************
-- CISCO-ERR-DISABLE-CAPABILITY.my:
-- Cisco CISCO-ERR-DISABLE-MIB AGENT-CAPABILITIES
--   
-- March 2010, Lilian Jiang
--   
-- Copyright (c) 2010 by Cisco Systems, Inc.
-- All rights reserved.
-- *****************************************************************

CISCO-ERR-DISABLE-CAPABILITY DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    Unsigned32
        FROM SNMPv2-SMI
    AGENT-CAPABILITIES
        FROM SNMPv2-CONF
    TimeIntervalSec
        FROM CISCO-TC
    ciscoAgentCapability
        FROM CISCO-SMI;


ciscoErrDisableCapability MODULE-IDENTITY
    LAST-UPDATED    "201005050000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 West Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-lan-switch-snmp@cisco.com"
    DESCRIPTION
        "The capabilities description of
        CISCO-ERR-DISABLE-MIB."
    REVISION        "201005050000Z"
    DESCRIPTION
        "Added agent capabilities statement
        cErrDisableCapV12R0254SGPCat4K."
    REVISION        "201003110000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoAgentCapability 589 }



cErrDisableCapV12R0233SXI4PCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(33)SXI4 on Catalyst 6000/6500
                     series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-ERR-DISABLE-MIB capabilities."

    SUPPORTS        CISCO-ERR-DISABLE-MIB
    INCLUDES        {
                        ciscoErrDisableGlobalCfgGroup,
                        ciscoErrDisableFeatureCfgGroup,
                        ciscoErrDisableIfStatusGroup,
                        ciscoErrDisableNotifCfgGroup,
                        ciscoErrDisableNotifGroupRev1,
                        ciscoErrDisableShutdownVlanGroup
                    }
    VARIATION       cErrDisableRecoveryInterval
    SYNTAX          TimeIntervalSec (30..86400)
    DESCRIPTION
        "Only limited set of values is supported."

    VARIATION       cErrDisableNotifRate
    SYNTAX          Unsigned32 (0..10000)
    DESCRIPTION
        "Only limited set of values is supported."

    ::= { ciscoErrDisableCapability 1 }

cErrDisableCapV12R0254SGPCat4K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(54)SG on CAT4K family switches."
    STATUS          current
    DESCRIPTION
        "CISCO-ERR-DISABLE-MIB capabilities."

    SUPPORTS        CISCO-ERR-DISABLE-MIB
    INCLUDES        {
                        ciscoErrDisableGlobalCfgGroup,
                        ciscoErrDisableFeatureCfgGroup,
                        ciscoErrDisableIfStatusGroup,
                        ciscoErrDisableNotifCfgGroup,
                        ciscoErrDisableNotifGroupRev1,
                        ciscoErrDisableShutdownVlanGroup
                    }

    VARIATION       cErrDisableRecoveryInterval
    SYNTAX          TimeIntervalSec (30..86400)
    DESCRIPTION
        "Only limited set of values is supported."

    VARIATION       cErrDisableNotifRate
    SYNTAX          Unsigned32 (0..10000)
    DESCRIPTION
        "Only limited set of values is supported."

    ::= { ciscoErrDisableCapability 2 }

END



