
-- *****************************************************************
-- CISCO-SNMP-USM-OIDS-MIB.my 
--
-- Cisco Extension to define OIDS for SNMP-USM-MIB & SNMP-USM-AES-MIB
--           
--  April 2004, Vanaja Palanisamy
--           
-- Copyright (c) 2004 by cisco Systems, Inc.
-- All rights reserved.
--           
-- *****************************************************************
--           

CISCO-SNMP-USM-OIDS-MIB DEFINITIONS ::= BEGIN

IMPORTS
        MODULE-IDENTITY 
                FROM SNMPv2-SMI
        ciscoModules
                FROM CISCO-SMI;

ciscoSnmpUsmOidsMIB MODULE-IDENTITY
        LAST-UPDATED    "200602280000Z"
        ORGANIZATION    "Cisco Systems, Inc."
        CONTACT-INFO
                "       Cisco Systems
                        Customer Service

                Postal: 170 W. Tasman Drive
                        San Jose, CA 95134
                        USA

                   Tel: +1 800 553-NETS

                E-mail: cs-snmp@cisco.com"
        DESCRIPTION
                "This MIB extends the OID's for SNMP-USM-MIB
                 specified in RFC 3414.

                The privacy protocol OID's specified herein 
                are intended to be used as values  for 
                usmUserPrivProtocol when managing SNMPv3  
                users via the snmpUsmMIB.

                This MIB defines the OID's for the following
                encryption options:

                        * 192 bit key size AES
                        * 256 bit key size AES
                        * 168 bit key size 3DES.

                OID for 128 bit key size AES encryption is 
                defined in SNMP-USM-AES-MIB as per the 
                RFC 3826." 

        REVISION    "200602280000Z"
        DESCRIPTION
                "Initial version of this MIB module."
        ::= { ciscoModules 6 }

ciscoSnmpPrivProtocols  
        OBJECT IDENTIFIER ::= { ciscoSnmpUsmOidsMIB 1 }
                 
-- The CFB128-AES-192/256 & 3DES 168 bit Privacy Protocols

cusmAESCfb192PrivProtocol 
        OBJECT IDENTIFIER ::= { ciscoSnmpPrivProtocols 1 } 

cusmAESCfb256PrivProtocol 
        OBJECT IDENTIFIER ::= { ciscoSnmpPrivProtocols 2 } 

cusm3DES168PrivProtocol 
        OBJECT IDENTIFIER ::= { ciscoSnmpPrivProtocols 3 } 

END

 

