-- *****************************************************************
-- CISCO-SWITCH-ENGINE-CAPABILITY.my:
-- Cisco CISCO-SWITCH-ENGINE-MIB AGENT-CAPABILITIES
--   
-- July 2003, Edward Pham, Jayakumar Kadirvelu
--   
-- Copyright (c) 2003-2008, 2010 by Cisco Systems, Inc.
-- All rights reserved.
-- *****************************************************************

CISCO-SWITCH-ENGINE-CAPABILITY DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    Counter32,
    Counter64
        FROM SNMPv2-SMI
    AGENT-CAPABILITIES
        FROM SNMPv2-CONF
    InetAddressType
        FROM INET-ADDRESS-MIB
    ciscoAgentCapability
        FROM CISCO-SMI;


ciscoSwitchEngineCapability MODULE-IDENTITY
    LAST-UPDATED    "201003220000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 West Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-lan-switch-snmp@cisco.com"
    DESCRIPTION
        "The agent capabilities description of
        CISCO-SWITCH-ENGINE-MIB."
    REVISION        "201003220000Z"
    DESCRIPTION
        "Added capability statement cseCapV12R0233SXI4PCat6K."
    REVISION        "200810300000Z"
    DESCRIPTION
        "Added capability statement
        cseCapV12R0233SXIPCat6K.

        Added the following missing groups to 
        previous releases:
            cse4kVlanGroup
            cseNDEReportGroup
            cseCefAdjacencyEncapGroup
            cseCefAdjacencyMTUGroup"
    REVISION        "200707160000Z"
    DESCRIPTION
        "Added capability statement
        cseCapV12R0233SXHPCat6K."
    REVISION        "200509160000Z"
    DESCRIPTION
        "Added capability statement
        cseCapV12R0218SXGPCat6K.

        Added variation for cseFlowIPFlowMask to
        cseCapV12R0119ECat6KPfc,
        cseCapV12R0119ECat6KPfc2,
        cseCapV12R0217SXCat6KPfc3 and
        cseCapV12R0218SXEPCat6K."
    REVISION        "200508240000Z"
    DESCRIPTION
        "Added capability statement
        cseCapCatOSV08R0501PCat6KPfc3

        Added variation for cseFlowIPFlowMask to 
        cseCapCatOSV08R0101Cat6KPfc,
        cseCapCatOSV08R0101Cat6KPfc2,
        cseCapCatOSV08R0101Cat6KPfc3,
        cseCapCatOSV08R0301Cat6KPfc2,
        cseCapCatOSV08R0301Cat6KPfc3 and
        cseCapCatOSV08R0401Cat6KPfc3."
    REVISION        "200412220000Z"
    DESCRIPTION
        "Added capability statement
        cseCapV12R0218SXEPCat6K."
    REVISION        "200406140000Z"
    DESCRIPTION
        "Added capability statement
        cseCapCatOSV08R0401Cat6KPfc3."
    REVISION        "200401150000Z"
    DESCRIPTION
        "Added capability statement cseCapCatOSV08R0301Cat6KPfc2
        and cseCapCatOSV08R0301Cat6KPfc3."
    REVISION        "200312040000Z"
    DESCRIPTION
        "Fixed description for cseCapV12R0217SXCat6KPfc3
        to match actual product release and added
        cseTcamUsageGroup to the INCLUDES section."
    REVISION        "200308120000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoAgentCapability 343 }



cseCapCatOSV08R0101Cat6KPfc AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco CatOS 8.1(1) on Catalyst 6000/6500
                         series devices with PFC card."
    STATUS          current
    DESCRIPTION
        "CISCO-SWITCH-ENGINE-MIB agent capabilities."

    SUPPORTS        CISCO-SWITCH-ENGINE-MIB
    INCLUDES        {
                        cseStatisticsGroup,
                        cseStatisticsGroup2,
                        cseRouterGroup,
                        cseFlowMgmtGroup,
                        cseNetflowLSGroup,
                        cseProtocolFilterGroup,
                        cseFlowMcastMgmtGroup,
                        cseFlowMgmtOperStatusGroup,
                        cse4kVlanGroup,
                        cseNDEMandatoryGroup,
                        cseNDESingleFilterGroup,
                        cseFlowMgmtGroupRev1,
                        cseL3ErrorsGroup,
                        cseBridgedFlowGroup,
                        cseProtocolFilterExtGroup,
                        cseFlowMgmtExtGroup,
                        cseFlowMgmtExtGroup1,
                        cseNDESingleFilterGroupRev1
                    }
    VARIATION       cseCacheUtilization
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowMcastResultDstVlans
    SYNTAX          OCTET STRING
    DESCRIPTION
        "A NULL octet string is returned."

    VARIATION       cseFlowMcastResultDstVlans2k
    SYNTAX          OCTET STRING
    DESCRIPTION
        "A NULL octet string is returned."

    VARIATION       cseFlowMcastResultDstVlans3k
    SYNTAX          OCTET STRING
    DESCRIPTION
        "A NULL octet string is returned."

    VARIATION       cseFlowMcastResultDstVlans4k
    SYNTAX          OCTET STRING
    DESCRIPTION
        "A NULL octet string is returned."

    VARIATION       cseNetflowLSFilterSupport
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowIPFlowMask
    SYNTAX          INTEGER  {
                        dstOnly(1),
                        srcDst(2),
                        fullFlow(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    ::= { ciscoSwitchEngineCapability 1 }

cseCapCatOSV08R0101Cat6KPfc2 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco CatOS 8.1(1) on Catalyst 6000/6500
                         and Cisco 7600 series devices with PFC2 card."
    STATUS          current
    DESCRIPTION
        "CISCO-SWITCH-ENGINE-MIB agent capabilities."

    SUPPORTS        CISCO-SWITCH-ENGINE-MIB
    INCLUDES        {
                        cseStatisticsGroup,
                        cseStatisticsGroup2,
                        cseVlanStatisticsGroup,
                        cseRouterGroup,
                        cseFlowMgmtGroup,
                        cseNetflowLSGroup,
                        cseProtocolFilterGroup,
                        cseFlowMcastMgmtGroup,
                        cseFlowMgmtOperStatusGroup,
                        cse4kVlanGroup,
                        cseNDEMandatoryGroup,
                        cseNDESingleFilterGroup,
                        cseFlowMgmtGroupRev1,
                        cseL3ErrorsGroup,
                        cseBridgedFlowGroup,
                        cseVlanStatisticsExtGroup,
                        cseProtocolFilterExtGroup,
                        cseFlowMgmtExtGroup,
                        cseFlowMgmtExtGroup1,
                        cseNDEReportGroup,
                        cseStatisticsFlowGroup,
                        cseNDESingleFilterGroupRev1
                    }
    VARIATION       cseL3VlanInPkts
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseL3VlanInOctets
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseCacheUtilization
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowMcastResultDstVlans
    SYNTAX          OCTET STRING
    DESCRIPTION
        "A NULL octet string is returned."

    VARIATION       cseFlowMcastResultDstVlans2k
    SYNTAX          OCTET STRING
    DESCRIPTION
        "A NULL octet string is returned."

    VARIATION       cseFlowMcastResultDstVlans3k
    SYNTAX          OCTET STRING
    DESCRIPTION
        "A NULL octet string is returned."

    VARIATION       cseFlowMcastResultDstVlans4k
    SYNTAX          OCTET STRING
    DESCRIPTION
        "A NULL octet string is returned."

    VARIATION       cseNetflowLSFilterSupport
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowIPFlowMask
    SYNTAX          INTEGER  {
                        dstOnly(1),
                        srcDst(2),
                        fullFlow(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    ::= { ciscoSwitchEngineCapability 2 }

cseCapCatOSV08R0101Cat6KPfc3 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco CatOS 8.1(1) on Catalyst 6000/6500
                         and Cisco 7600 series devices with 
                         PFC3 card."
    STATUS          current
    DESCRIPTION
        "CISCO-SWITCH-ENGINE-MIB agent capabilities."

    SUPPORTS        CISCO-SWITCH-ENGINE-MIB
    INCLUDES        {
                        cseStatisticsGroup,
                        cseStatisticsGroup2,
                        cseVlanStatisticsGroup,
                        cseRouterGroup,
                        cseFlowMgmtGroup,
                        cseNetflowLSGroup,
                        cseProtocolFilterGroup,
                        cseFlowMcastMgmtGroup,
                        cseFlowMgmtOperStatusGroup,
                        cse4kVlanGroup,
                        cseNDEMandatoryGroup,
                        cseNDESingleFilterGroup,
                        cseFlowMgmtGroupRev1,
                        cseL3ErrorsGroup,
                        cseVlanStatisticsExtGroup,
                        cseFlowMgmtExtGroup,
                        cseFlowMgmtExtGroup1,
                        cseNDEReportGroup,
                        cseStatisticsFlowGroup,
                        cseNDESingleFilterGroupRev1
                    }
    VARIATION       cseCacheUtilization
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseProtocolFilterPortAdminStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseProtocolFilterPortOperStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowMcastResultDstVlans
    SYNTAX          OCTET STRING
    DESCRIPTION
        "A NULL octet string is returned."

    VARIATION       cseFlowMcastResultDstVlans2k
    SYNTAX          OCTET STRING
    DESCRIPTION
        "A NULL octet string is returned."

    VARIATION       cseFlowMcastResultDstVlans3k
    SYNTAX          OCTET STRING
    DESCRIPTION
        "A NULL octet string is returned."

    VARIATION       cseFlowMcastResultDstVlans4k
    SYNTAX          OCTET STRING
    DESCRIPTION
        "A NULL octet string is returned."

    VARIATION       cseNetflowLSFilterSupport
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowIPFlowMask
    SYNTAX          INTEGER  {
                        dstOnly(1),
                        srcDst(2),
                        fullFlow(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    ::= { ciscoSwitchEngineCapability 3 }

cseCapV12R0119ECat6KPfc AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.1(19E) on Catalyst 6000/6500
                         series devices with PFC card."
    STATUS          current
    DESCRIPTION
        "CISCO-SWITCH-ENGINE-MIB agent capabilities."

    SUPPORTS        CISCO-SWITCH-ENGINE-MIB
    INCLUDES        {
                        cseStatisticsGroup,
                        cseStatisticsGroup2,
                        cseVlanStatisticsGroup,
                        cseNetflowLSGroup,
                        cseNDEMandatoryGroup,
                        cseNDEMultipleFiltersGroup,
                        cseL3ErrorsGroup,
                        cseVlanStatisticsExtGroup
                    }
    VARIATION       cseNetflowLSExportHost
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportTransportNumber
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataSource
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataSourceMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataDest
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataDestMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataProtocol
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataFilterSelection
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseL3VlanInPkts
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseL3VlanInOctets
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowIPFlowMask
    SYNTAX          INTEGER  {
                        dstOnly(1),
                        srcDst(2),
                        fullFlow(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    ::= { ciscoSwitchEngineCapability 4 }

cseCapV12R0119ECat6KPfc2 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.1(19E) on Catalyst 6000/6500
                         and Cisco 7600 series devices with 
                         PFC2 card."
    STATUS          current
    DESCRIPTION
        "CISCO-SWITCH-ENGINE-MIB agent capabilities."

    SUPPORTS        CISCO-SWITCH-ENGINE-MIB
    INCLUDES        {
                        cseStatisticsGroup,
                        cseStatisticsGroup2,
                        cseVlanStatisticsGroup,
                        cseNetflowLSGroup,
                        cseNDEMandatoryGroup,
                        cseNDEMultipleFiltersGroup,
                        cseL3ErrorsGroup,
                        cseVlanStatisticsExtGroup
                    }
    VARIATION       cseL2ForwardedLocalPkts
    SYNTAX          Counter32
    DESCRIPTION
        "Always return 0."

    VARIATION       cseL2ForwardedLocalOctets
    SYNTAX          Counter64
    DESCRIPTION
        "Always return 0."

    VARIATION       cseL2HCOverflowForwardedLocalPkts
    SYNTAX          Counter64
    DESCRIPTION
        "Always return 0."

    VARIATION       cseNetflowLSExportHost
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportTransportNumber
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataSource
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataSourceMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataDest
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataDestMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataProtocol
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataFilterSelection
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseL3VlanInPkts
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseL3VlanInOctets
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowIPFlowMask
    SYNTAX          INTEGER  {
                        dstOnly(1),
                        srcDst(2),
                        fullFlow(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    ::= { ciscoSwitchEngineCapability 5 }

cseCapV12R0217SXCat6KPfc3 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(17SX) on Catalyst 6000/6500
                         and Cisco 7600 series devices with 
                         PFC3 card."
    STATUS          current
    DESCRIPTION
        "CISCO-SWITCH-ENGINE-MIB agent capabilities."

    SUPPORTS        CISCO-SWITCH-ENGINE-MIB
    INCLUDES        {
                        cseStatisticsGroup,
                        cseStatisticsGroup2,
                        cseVlanStatisticsGroup,
                        cseFlowMcastMgmtGroup,
                        cseNetflowLSGroup,
                        cseFlowMgmtOperStatusGroup,
                        cse4kVlanGroup,
                        cseNDEMandatoryGroup,
                        cseNDEMultipleFiltersGroup,
                        cseFlowMgmtGroupRev1,
                        cseL3ErrorsGroup,
                        cseVlanStatisticsExtGroup,
                        cseFlowMgmtExtGroup,
                        cseFlowMgmtExtGroup1,
                        cseNDEReportGroup,
                        cseTcamUsageGroup
                    }
    VARIATION       cseL2ForwardedLocalPkts
    SYNTAX          Counter32
    DESCRIPTION
        "Always return 0."

    VARIATION       cseL2ForwardedLocalOctets
    SYNTAX          Counter64
    DESCRIPTION
        "Always return 0."

    VARIATION       cseL2HCOverflowForwardedLocalPkts
    SYNTAX          Counter64
    DESCRIPTION
        "Always return 0."

    VARIATION       cseNetflowLSExportHost
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportTransportNumber
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataSource
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataSourceMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataDest
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataDestMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataProtocol
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataFilterSelection
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowMaxQueries
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryTransport
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQuerySource
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQuerySourceMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryDestination
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryDestinationMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryRouterIndex
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryOwner
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultingRows
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultTotalPkts
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultTotalOctets
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultAvgDuration
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultAvgIdle
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryCreateTime
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryTotalFlows
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataSrcMac
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataDstMac
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataEncapType
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataSource
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataStaticFlow
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataDestination
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataIpQOS
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataIpQOSPolicy
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataWhenCreated
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataLastUsed
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataPkts
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataOctets
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowSwitchStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseStatsFlowAged
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseStatsFlowPurged
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseStatsFlowParityFail
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowIPXEstablishedAgingTime
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowOperIPXAgingTime
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowIPXFlowMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseTcamResourceType
    SYNTAX          INTEGER  {
                        aclStorageMask(1),
                        aclStorageValue(2),
                        qosStorageMask(5),
                        qosStorageValue(6),
                        l4PortOperator(9),
                        interfaceMapping(10)
                    }
    DESCRIPTION
        "No support for aclDynamicStorageMask(3),
        aclDynamicStorageValue(4),
        qosDynamicStorageMask(7) and
        qosDynamicStorageValue(8)."

    VARIATION       cseFlowIPFlowMask
    SYNTAX          INTEGER  {
                        dstOnly(1),
                        srcDst(2),
                        fullFlow(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    ::= { ciscoSwitchEngineCapability 6 }

cseCapCatOSV08R0301Cat6KPfc2 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco CatOS 8.3(1) on Catalyst 6000/6500
                         and Cisco 7600 series devices with PFC2 card."
    STATUS          current
    DESCRIPTION
        "CISCO-SWITCH-ENGINE-MIB agent capabilities."

    SUPPORTS        CISCO-SWITCH-ENGINE-MIB
    INCLUDES        {
                        cseStatisticsGroup,
                        cseStatisticsGroup2,
                        cseVlanStatisticsGroup,
                        cseRouterGroup,
                        cseFlowMgmtGroup,
                        cseNetflowLSGroup,
                        cseProtocolFilterGroup,
                        cseFlowMcastMgmtGroup,
                        cseFlowMgmtOperStatusGroup,
                        cse4kVlanGroup,
                        cseNDEMandatoryGroup,
                        cseNDESingleFilterGroup,
                        cseFlowMgmtGroupRev1,
                        cseL3ErrorsGroup,
                        cseBridgedFlowGroup,
                        cseVlanStatisticsExtGroup,
                        cseProtocolFilterExtGroup,
                        cseFlowMgmtExtGroup,
                        cseFlowMgmtExtGroup1,
                        cseNDEReportGroup,
                        cseStatisticsFlowGroup,
                        cseNDESingleFilterGroupRev1,
                        cseCefFibAdjacencyGroup,
                        cseCefAdjacencyEncapGroup,
                        cseTcamUsageGroup
                    }
    VARIATION       cseL3VlanInPkts
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseL3VlanInOctets
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseCacheUtilization
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowMcastResultDstVlans
    SYNTAX          OCTET STRING
    DESCRIPTION
        "A NULL octet string is returned."

    VARIATION       cseFlowMcastResultDstVlans2k
    SYNTAX          OCTET STRING
    DESCRIPTION
        "A NULL octet string is returned."

    VARIATION       cseFlowMcastResultDstVlans3k
    SYNTAX          OCTET STRING
    DESCRIPTION
        "A NULL octet string is returned."

    VARIATION       cseFlowMcastResultDstVlans4k
    SYNTAX          OCTET STRING
    DESCRIPTION
        "A NULL octet string is returned."

    VARIATION       cseNetflowLSFilterSupport
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowIPFlowMask
    SYNTAX          INTEGER  {
                        dstOnly(1),
                        srcDst(2),
                        fullFlow(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    ::= { ciscoSwitchEngineCapability 7 }

cseCapCatOSV08R0301Cat6KPfc3 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco CatOS 8.3(1) on Catalyst 6000/6500
                         and Cisco 7600 series devices with 
                         PFC3 card."
    STATUS          current
    DESCRIPTION
        "CISCO-SWITCH-ENGINE-MIB agent capabilities."

    SUPPORTS        CISCO-SWITCH-ENGINE-MIB
    INCLUDES        {
                        cseStatisticsGroup,
                        cseStatisticsGroup2,
                        cseVlanStatisticsGroup,
                        cseRouterGroup,
                        cseFlowMgmtGroup,
                        cseNetflowLSGroup,
                        cseProtocolFilterGroup,
                        cseFlowMcastMgmtGroup,
                        cseFlowMgmtOperStatusGroup,
                        cse4kVlanGroup,
                        cseNDEMandatoryGroup,
                        cseNDESingleFilterGroup,
                        cseFlowMgmtGroupRev1,
                        cseL3ErrorsGroup,
                        cseVlanStatisticsExtGroup,
                        cseFlowMgmtExtGroup,
                        cseFlowMgmtExtGroup1,
                        cseNDEReportGroup,
                        cseStatisticsFlowGroup,
                        cseNDESingleFilterGroupRev1,
                        cseCefFibAdjacencyGroup,
                        cseCefAdjacencyEncapGroup,
                        cseTcamUsageGroup
                    }
    VARIATION       cseCacheUtilization
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseProtocolFilterPortAdminStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseProtocolFilterPortOperStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowMcastResultDstVlans
    SYNTAX          OCTET STRING
    DESCRIPTION
        "A NULL octet string is returned."

    VARIATION       cseFlowMcastResultDstVlans2k
    SYNTAX          OCTET STRING
    DESCRIPTION
        "A NULL octet string is returned."

    VARIATION       cseFlowMcastResultDstVlans3k
    SYNTAX          OCTET STRING
    DESCRIPTION
        "A NULL octet string is returned."

    VARIATION       cseFlowMcastResultDstVlans4k
    SYNTAX          OCTET STRING
    DESCRIPTION
        "A NULL octet string is returned."

    VARIATION       cseNetflowLSFilterSupport
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowIPFlowMask
    SYNTAX          INTEGER  {
                        dstOnly(1),
                        srcDst(2),
                        fullFlow(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    ::= { ciscoSwitchEngineCapability 8 }

cseCapCatOSV08R0401Cat6KPfc3 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco CatOS 8.4(1) on Catalyst 6000/6500
                         and Cisco 7600 series devices with 
                         PFC3 card."
    STATUS          current
    DESCRIPTION
        "CISCO-SWITCH-ENGINE-MIB agent capabilities."

    SUPPORTS        CISCO-SWITCH-ENGINE-MIB
    INCLUDES        {
                        cseStatisticsGroup,
                        cseStatisticsGroup2,
                        cseVlanStatisticsGroup,
                        cseRouterGroup,
                        cseFlowMgmtGroup,
                        cseNetflowLSGroup,
                        cseProtocolFilterGroup,
                        cseFlowMcastMgmtGroup,
                        cseFlowMgmtOperStatusGroup,
                        cse4kVlanGroup,
                        cseNDEMandatoryGroup,
                        cseNDESingleFilterGroup,
                        cseFlowMgmtGroupRev1,
                        cseL3ErrorsGroup,
                        cseVlanStatisticsExtGroup,
                        cseFlowMgmtExtGroup,
                        cseFlowMgmtExtGroup1,
                        cseNDEReportGroup,
                        cseStatisticsFlowGroup,
                        cseNDESingleFilterGroupRev1,
                        cseCefFibAdjacencyGroup,
                        cseCefAdjacencyEncapGroup,
                        cseTcamUsageGroup,
                        cseNetflowASInfoExportGroup,
                        cseNetflowPerVlanIfGroup
                    }
    VARIATION       cseCacheUtilization
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseProtocolFilterPortAdminStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseProtocolFilterPortOperStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowMcastResultDstVlans
    DESCRIPTION
        "A zero-length octet string is returned."

    VARIATION       cseFlowMcastResultDstVlans2k
    DESCRIPTION
        "A zero-length octet string is returned."

    VARIATION       cseFlowMcastResultDstVlans3k
    DESCRIPTION
        "A zero-length octet string is returned."

    VARIATION       cseFlowMcastResultDstVlans4k
    DESCRIPTION
        "A zero-length octet string is returned."

    VARIATION       cseNetflowLSFilterSupport
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowIPFlowMask
    SYNTAX          INTEGER  {
                        dstOnly(1),
                        srcDst(2),
                        fullFlow(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    ::= { ciscoSwitchEngineCapability 9 }

cseCapV12R0218SXEPCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(18)SXE on Catalyst 6000/6500
                         and Cisco 7600 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-SWITCH-ENGINE-MIB agent capabilities."

    SUPPORTS        CISCO-SWITCH-ENGINE-MIB
    INCLUDES        {
                        cseStatisticsGroup,
                        cseStatisticsGroup2,
                        cseVlanStatisticsGroup,
                        cseFlowMcastMgmtGroup,
                        cseNetflowLSGroup,
                        cseFlowMgmtOperStatusGroup,
                        cse4kVlanGroup,
                        cseNDEMandatoryGroup,
                        cseNDEMultipleFiltersGroup,
                        cseFlowMgmtGroupRev1,
                        cseL3ErrorsGroup,
                        cseVlanStatisticsExtGroup,
                        cseFlowMgmtExtGroup,
                        cseFlowMgmtExtGroup1,
                        cse4kVlanGroup,
                        cseTcamUsageGroup,
                        cseCefFibAdjacencyGroup
                    }
    VARIATION       cseL2ForwardedLocalPkts
    SYNTAX          Counter32
    DESCRIPTION
        "Always return 0."

    VARIATION       cseL2ForwardedLocalOctets
    SYNTAX          Counter64
    DESCRIPTION
        "Always return 0."

    VARIATION       cseL2HCOverflowForwardedLocalPkts
    SYNTAX          Counter64
    DESCRIPTION
        "Always return 0."

    VARIATION       cseNetflowLSExportHost
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportTransportNumber
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataSource
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataSourceMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataDest
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataDestMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataProtocol
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataFilterSelection
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowMaxQueries
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryTransport
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQuerySource
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQuerySourceMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryDestination
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryDestinationMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryRouterIndex
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryOwner
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultingRows
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultTotalPkts
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultTotalOctets
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultAvgDuration
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultAvgIdle
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryCreateTime
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryTotalFlows
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataSrcMac
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataDstMac
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataEncapType
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataSource
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataStaticFlow
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataDestination
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataIpQOS
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataIpQOSPolicy
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataWhenCreated
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataLastUsed
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataPkts
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataOctets
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowSwitchStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseStatsFlowAged
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseStatsFlowPurged
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseStatsFlowParityFail
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowIPXEstablishedAgingTime
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowOperIPXAgingTime
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowIPXFlowMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseTcamResourceType
    SYNTAX          INTEGER  {
                        aclStorageMask(1),
                        aclStorageValue(2),
                        qosStorageMask(5),
                        qosStorageValue(6),
                        l4PortOperator(9),
                        interfaceMapping(10)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       cseCefFibAddrType
    SYNTAX          InetAddressType {
                        ipv4(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       cseCefAdjacencyAddrType
    SYNTAX          InetAddressType {
                        ipv4(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       cseFlowIPFlowMask
    SYNTAX          INTEGER  {
                        dstOnly(1),
                        srcDst(2),
                        fullFlow(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    ::= { ciscoSwitchEngineCapability 10 }

cseCapCatOSV08R0501PCat6KPfc3 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco CatOS 8.5(1) on Catalyst 6000/6500
                         and Cisco 7600 series devices with 
                         PFC3 card."
    STATUS          current
    DESCRIPTION
        "CISCO-SWITCH-ENGINE-MIB agent capabilities."

    SUPPORTS        CISCO-SWITCH-ENGINE-MIB
    INCLUDES        {
                        cseStatisticsGroup,
                        cseStatisticsGroup2,
                        cseVlanStatisticsGroup,
                        cseRouterGroup,
                        cseFlowMgmtGroup,
                        cseNetflowLSGroup,
                        cseProtocolFilterGroup,
                        cseFlowMcastMgmtGroup,
                        cseFlowMgmtOperStatusGroup,
                        cse4kVlanGroup,
                        cseNDEMandatoryGroup,
                        cseNDESingleFilterGroup,
                        cseFlowMgmtGroupRev1,
                        cseL3ErrorsGroup,
                        cseVlanStatisticsExtGroup,
                        cseFlowMgmtExtGroup,
                        cseFlowMgmtExtGroup1,
                        cseNDEReportGroup,
                        cseStatisticsFlowGroup,
                        cseNDESingleFilterGroupRev1,
                        cseCefFibAdjacencyGroup,
                        cseCefAdjacencyEncapGroup,
                        cseTcamUsageGroup,
                        cseNetflowASInfoExportGroup,
                        cseNetflowPerVlanIfGroup
                    }
    VARIATION       cseCacheUtilization
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseProtocolFilterPortAdminStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseProtocolFilterPortOperStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowMcastResultDstVlans
    DESCRIPTION
        "A zero-length octet string is returned."

    VARIATION       cseFlowMcastResultDstVlans2k
    DESCRIPTION
        "A zero-length octet string is returned."

    VARIATION       cseFlowMcastResultDstVlans3k
    DESCRIPTION
        "A zero-length octet string is returned."

    VARIATION       cseFlowMcastResultDstVlans4k
    DESCRIPTION
        "A zero-length octet string is returned."

    VARIATION       cseNetflowLSFilterSupport
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowIPFlowMask
    SYNTAX          INTEGER  {
                        dstOnly(1),
                        srcDst(2),
                        fullFlow(3),
                        null(7)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    ::= { ciscoSwitchEngineCapability 11 }

cseCapV12R0233SXHPCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(33)SXH on Catalyst 6000/6500
                         series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-SWITCH-ENGINE-MIB agent capabilities."

    SUPPORTS        CISCO-SWITCH-ENGINE-MIB
    INCLUDES        {
                        cseStatisticsGroup,
                        cseStatisticsGroup2,
                        cseVlanStatisticsGroup,
                        cseNetflowLSGroup,
                        cseFlowMgmtOperStatusGroup,
                        cse4kVlanGroup,
                        cseNDEMandatoryGroup,
                        cseNDEMultipleFiltersGroup,
                        cseFlowMgmtGroupRev1,
                        cseL3ErrorsGroup,
                        cseVlanStatisticsExtGroup,
                        cseFlowMgmtExtGroup,
                        cseFlowMgmtExtGroup1,
                        cseStatisticsFlowGroup,
                        cseFlowMgmtExtGroup2,
                        cseNDEReportGroup,
                        cseTcamUsageGroup,
                        cseL3ErrorsLCGroup,
                        cseCefFibAdjacencyGroup,
                        cseCefAdjacencyEncapGroup,
                        cseCefAdjacencyMTUGroup,
                        cseFlowMcastMgmtGroup1,
                        cseFlowMcastMgmtGroup2,
                        cseMetUsageGroup
                    }
    VARIATION       cseL2ForwardedLocalPkts
    SYNTAX          Counter32
    DESCRIPTION
        "Always return 0."

    VARIATION       cseL2ForwardedLocalOctets
    SYNTAX          Counter64
    DESCRIPTION
        "Always return 0."

    VARIATION       cseL2HCOverflowForwardedLocalPkts
    SYNTAX          Counter64
    DESCRIPTION
        "Always return 0."

    VARIATION       cseNetflowLSExportHost
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportTransportNumber
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataSource
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataSourceMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataDest
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataDestMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataProtocol
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataFilterSelection
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowMaxQueries
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryTransport
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQuerySource
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQuerySourceMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryDestination
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryDestinationMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryRouterIndex
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryOwner
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultingRows
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultTotalPkts
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultTotalOctets
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultAvgDuration
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultAvgIdle
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryCreateTime
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryTotalFlows
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataSrcMac
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataDstMac
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataEncapType
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataSource
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataStaticFlow
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataDestination
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataIpQOS
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataIpQOSPolicy
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataWhenCreated
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataLastUsed
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataPkts
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataOctets
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowSwitchStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseStatsFlowAged
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseStatsFlowPurged
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseStatsFlowParityFail
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowIPXEstablishedAgingTime
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowOperIPXAgingTime
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowIPXFlowMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseTcamResourceType
    SYNTAX          INTEGER  {
                        aclStorageMask(1),
                        aclStorageValue(2),
                        qosStorageMask(5),
                        qosStorageValue(6),
                        l4PortOperator(9),
                        interfaceMapping(10),
                        ingressInterfaceMapping(11),
                        egressInterfaceMapping(12)
                    }
    DESCRIPTION
        "Only limited set of values is supported."

    VARIATION       cseCefFibAddrType
    SYNTAX          InetAddressType {
                        ipv4(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       cseCefAdjacencyAddrType
    SYNTAX          InetAddressType {
                        ipv4(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    ::= { ciscoSwitchEngineCapability 12 }

cseCapV12R0233SXIPCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(33)SXI on Catalyst 6000/6500
                         series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-SWITCH-ENGINE-MIB agent capabilities."

    SUPPORTS        CISCO-SWITCH-ENGINE-MIB
    INCLUDES        {
                        cseStatisticsGroup,
                        cseStatisticsGroup2,
                        cseVlanStatisticsGroup,
                        cseNetflowLSGroup,
                        cseFlowMgmtOperStatusGroup,
                        cse4kVlanGroup,
                        cseNDEMandatoryGroup,
                        cseNDEMultipleFiltersGroup,
                        cseFlowMgmtGroupRev1,
                        cseL3ErrorsGroup,
                        cseVlanStatisticsExtGroup,
                        cseFlowMgmtExtGroup,
                        cseFlowMgmtExtGroup1,
                        cseNDEReportGroup,
                        cseStatisticsFlowGroup,
                        cseFlowMgmtExtGroup2,
                        cseTcamUsageGroup,
                        cseL3ErrorsLCGroup,
                        cseCefFibAdjacencyGroup,
                        cseCefAdjacencyEncapGroup,
                        cseCefAdjacencyMTUGroup,
                        cseFlowMcastMgmtGroup1,
                        cseFlowMcastMgmtGroup2,
                        cseMetUsageGroup,
                        cseFlowMcastRtrMgmtGroup,
                        cseCacheStatisticsGroup,
                        cseL3SwitchedPktsPerSecGroup
                    }
    VARIATION       cseL2ForwardedLocalPkts
    SYNTAX          Counter32
    DESCRIPTION
        "Always return 0."

    VARIATION       cseL2ForwardedLocalOctets
    SYNTAX          Counter64
    DESCRIPTION
        "Always return 0."

    VARIATION       cseL2HCOverflowForwardedLocalPkts
    SYNTAX          Counter64
    DESCRIPTION
        "Always return 0."

    VARIATION       cseNetflowLSExportHost
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportTransportNumber
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataSource
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataSourceMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataDest
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataDestMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataProtocol
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataFilterSelection
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowMaxQueries
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryTransport
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQuerySource
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQuerySourceMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryDestination
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryDestinationMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryRouterIndex
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryOwner
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultingRows
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultTotalPkts
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultTotalOctets
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultAvgDuration
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultAvgIdle
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryCreateTime
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryTotalFlows
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataSrcMac
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataDstMac
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataEncapType
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataSource
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataStaticFlow
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataDestination
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataIpQOS
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataIpQOSPolicy
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataWhenCreated
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataLastUsed
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataPkts
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataOctets
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowSwitchStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseStatsFlowAged
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseStatsFlowPurged
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseStatsFlowParityFail
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowIPXEstablishedAgingTime
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowOperIPXAgingTime
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowIPXFlowMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseTcamResourceType
    SYNTAX          INTEGER  {
                        aclStorageMask(1),
                        aclStorageValue(2),
                        qosStorageMask(5),
                        qosStorageValue(6),
                        l4PortOperator(9),
                        interfaceMapping(10),
                        ingressInterfaceMapping(11),
                        egressInterfaceMapping(12),
                        louSource(13),
                        louDestination(14),
                        andOr(15),
                        orAnd(16),
                        aclAdjacency(17)
                    }
    DESCRIPTION
        "Only limited set of values is supported."

    VARIATION       cseCefFibAddrType
    SYNTAX          InetAddressType {
                        ipv4(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       cseCefAdjacencyAddrType
    SYNTAX          InetAddressType {
                        ipv4(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    ::= { ciscoSwitchEngineCapability 13 }

cseCapV12R0233SXI4PCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(33)SXI4 on Catalyst 6000/6500
                         series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-SWITCH-ENGINE-MIB agent capabilities."

    SUPPORTS        CISCO-SWITCH-ENGINE-MIB
    INCLUDES        {
                        cseStatisticsGroup,
                        cseStatisticsGroup2,
                        cseVlanStatisticsGroup,
                        cseNetflowLSGroup,
                        cseFlowMgmtOperStatusGroup,
                        cse4kVlanGroup,
                        cseNDEMandatoryGroup,
                        cseNDEMultipleFiltersGroup,
                        cseFlowMgmtGroupRev1,
                        cseL3ErrorsGroup,
                        cseVlanStatisticsExtGroup,
                        cseFlowMgmtExtGroup,
                        cseFlowMgmtExtGroup1,
                        cseNDEReportGroup,
                        cseStatisticsFlowGroup,
                        cseFlowMgmtExtGroup2,
                        cseTcamUsageGroup,
                        cseL3ErrorsLCGroup,
                        cseCefFibAdjacencyGroup,
                        cseCefAdjacencyEncapGroup,
                        cseCefAdjacencyMTUGroup,
                        cseFlowMcastMgmtGroup1,
                        cseFlowMcastMgmtGroup2,
                        cseMetUsageGroup,
                        cseFlowMcastRtrMgmtGroup,
                        cseCacheStatisticsGroup,
                        cseL3SwitchedPktsPerSecGroup
                    }
    VARIATION       cseL2ForwardedLocalPkts
    SYNTAX          Counter32
    DESCRIPTION
        "Always return 0."

    VARIATION       cseL2ForwardedLocalOctets
    SYNTAX          Counter64
    DESCRIPTION
        "Always return 0."

    VARIATION       cseL2HCOverflowForwardedLocalPkts
    SYNTAX          Counter64
    DESCRIPTION
        "Always return 0."

    VARIATION       cseNetflowLSExportHost
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportTransportNumber
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataSource
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataSourceMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataDest
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataDestMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataProtocol
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseNetflowLSExportDataFilterSelection
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowMaxQueries
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryTransport
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQuerySource
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQuerySourceMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryDestination
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryDestinationMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryRouterIndex
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryOwner
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultingRows
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultTotalPkts
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultTotalOctets
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultAvgDuration
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryResultAvgIdle
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryCreateTime
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowQueryTotalFlows
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataSrcMac
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataDstMac
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataEncapType
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataSource
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataStaticFlow
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataDestination
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataIpQOS
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataIpQOSPolicy
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataWhenCreated
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataLastUsed
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataPkts
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowDataOctets
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowSwitchStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseStatsFlowAged
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseStatsFlowPurged
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseStatsFlowParityFail
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowIPXEstablishedAgingTime
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowOperIPXAgingTime
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseFlowIPXFlowMask
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       cseTcamResourceType
    SYNTAX          INTEGER  {
                        aclStorageMask(1),
                        aclStorageValue(2),
                        qosStorageMask(5),
                        qosStorageValue(6),
                        l4PortOperator(9),
                        interfaceMapping(10),
                        ingressInterfaceMapping(11),
                        egressInterfaceMapping(12),
                        louSource(13),
                        louDestination(14),
                        andOr(15),
                        orAnd(16),
                        aclAdjacency(17),
                        aclHighStorageMask(18),
                        aclHighStorageValue(19),
                        aclLowStorageMask(20),
                        aclLowStorageValue(21),
                        qosHighStorageMask(22),
                        qosHighStorageValue(23),
                        qosLowStorageMask(24),
                        qosLowStorageValue(25)
                    }
    DESCRIPTION
        "Only limited set of values is supported."

    VARIATION       cseCefFibAddrType
    SYNTAX          InetAddressType {
                        ipv4(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       cseCefAdjacencyAddrType
    SYNTAX          InetAddressType {
                        ipv4(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    ::= { ciscoSwitchEngineCapability 14 }

END



