-- *****************************************************************
-- CISCO-VTP-CAPABILITY.my:
-- Cisco CISCO-VTP-MIB AGENT-CAPABILITIES
--   
-- August 2003, Wen Xu
--   
-- Copyright (c) 2003-2008, 2010 by Cisco Systems, Inc.
-- All rights reserved.
--   
-- ***************************************************************

CISCO-VTP-CAPABILITY DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY
        FROM SNMPv2-SMI
    RowStatus
        FROM SNMPv2-TC
    AGENT-CAPABILITIES
        FROM SNMPv2-CONF
    ciscoAgentCapability
        FROM CISCO-SMI;


ciscoVtpCapability MODULE-IDENTITY
    LAST-UPDATED    "201011100000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 W Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS
            E-mail: cs-lan-switch-snmp@cisco.com"
    DESCRIPTION
        "The capabilities description of CISCO-VTP-MIB."
    REVISION        "201011100000Z"
    DESCRIPTION
        "Added capability statement ciscoVtpCapNxOSV05R0101PN7K."
    REVISION        "201003220000Z"
    DESCRIPTION
        "Added capability statement
        ciscoVtpCapV12R0254SGPCat4K."
    REVISION        "201003100000Z"
    DESCRIPTION
        "Added capability statement
        ciscoVtpCapV12R0233SXI4PCat6K.

        Removed vtpVlanInfoEditGroup2 and 
        added VARIATION on vtpVlanEditRowStatus
        to the following capability statements:
        ciscoVtpCapCatOSV08R0101,
        ciscoVtpCapCatOSV08R0301,
        ciscoVtpCapCatOSV08R0701

        Removed vtpVlanInfoEditGroup2 and  
        vtpDot1qTunnelGroup, added vtpDot1qTunnelGroup2,
        and added VARIATION on vtpVlanEditRowStatus to 
        the following capability statements:
        ciscoVtpCapV12R0119ECat6K,
        ciscoVtpCapV12R0217SXCat6K,
        ciscoVtpCapV12R0217SXACat6K,
        ciscoVtpCapV12R0218SXECat6K,
        ciscoVtpCapV12R0233SXHPCat6K,
        ciscoVtpCapV12R0233SXIPCat6K."
    REVISION        "200810280000Z"
    DESCRIPTION
        "Added capability statement
        ciscoVtpCapV12R0233SXIPCat6K."
    REVISION        "200805280000Z"
    DESCRIPTION
        "Added capability statement ciscoVtpCapCatOSV08R0701."
    REVISION        "200707180000Z"
    DESCRIPTION
        "Added capability statement
        ciscoVtpCapV12R0233SXHPCat6K."
    REVISION        "200603150000Z"
    DESCRIPTION
        "Added VARIATION clause for managementDomainLocalMode
        in capability statement ciscoVtpCapV12R0119ECat6K,
        ciscoVtpCapV12R0217SXCat6K,ciscoVtpCapV12R0217SXACat6K
        and ciscoVtpCapV12R0218SXECat6K."
    REVISION        "200503090000Z"
    DESCRIPTION
        "Added capability statement ciscoVtpCapV12R0218SXECat6K.

        Added VARIATION clause for vtpVlanTypeExt 
        and vtpVlanEditTypeExt2 in capability
        statement ciscoVtpCapV12R0119ECat6K, 
        ciscoVtpCapV12R0217SXCat6K and 
        ciscoVtpCapV12R0217SXACat6K."
    REVISION        "200404150000Z"
    DESCRIPTION
        "Added capability statement ciscoVtpCapV12R0217SXACat6K.

        Added a VARIATION statement for the object
        vlanTrunkPortDynamicStatus in capability
        statement ciscoVtpCapV12R0119ECat6K and
        ciscoVtpCapV12R0217SXCat6K."
    REVISION        "200312010000Z"
    DESCRIPTION
        "Added capability statement ciscoVtpCapCatOSV08R0301."
    REVISION        "200309150000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoAgentCapability 329 }



ciscoVtpCapV12R0119ECat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.1(19E) on Catalyst 6000/6500
                         and Cisco 7600 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-VTP-MIB capabilities."

    SUPPORTS        CISCO-VTP-MIB
    INCLUDES        {
                        vtpBasicGroup,
                        vtpVlanInfoGroup,
                        vtpConfigNotificationsGroupRev1,
                        vtpStatsGroup,
                        vtpTrunkPortGroup,
                        vtpVersion2BasicGroup,
                        vtpVlanInfoEditGroup,
                        vtpTrunkPortGroup2,
                        vtpTrunkPortGroup3,
                        vtpTrunkPruningGroup,
                        vtpTrunkPruningGroup2,
                        vtpVlanIfIndexGroup,
                        vtp4kVlanGroupRev1,
                        vtpDot1qTunnelGroup2,
                        vtpConfigNotificationsGroup2,
                        vtpVlanNotifEnabledGroup,
                        vtpConfigNotificationsGroup3
                    }
    VARIATION       vtpVersion
    SYNTAX          INTEGER  {
                        one(1),
                        two(2)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       managementDomainRowStatus
    SYNTAX          RowStatus {
                        active(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vlanTrunkPortRowStatus
    SYNTAX          RowStatus {
                        active(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       managementDomainVersionInUse
    SYNTAX          INTEGER  {
                        version1(1),
                        version2(2)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vlanTrunkPortDynamicStatus
    SYNTAX          INTEGER  {
                        trunking(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported.
        vlanTrunkPortTable only includes the
        trunking ports."

    VARIATION       vtpVlanTypeExt
    SYNTAX          BITS {
                        vtpmanageable(0),
                        rspan(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    VARIATION       vtpVlanEditTypeExt2
    SYNTAX          BITS {
                        vtpmanageable(0),
                        rspan(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    VARIATION       managementDomainLocalMode
    SYNTAX          INTEGER  {
                        client(1),
                        server(2),
                        transparent(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    VARIATION       vtpVlanEditRowStatus
    SYNTAX          RowStatus {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    ::= { ciscoVtpCapability 1 }

ciscoVtpCapV12R0217SXCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(17)SX on Catalyst 6000/6500
                         and Cisco 7600 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-VTP-MIB capabilities."

    SUPPORTS        CISCO-VTP-MIB
    INCLUDES        {
                        vtpBasicGroup,
                        vtpVlanInfoGroup,
                        vtpConfigNotificationsGroupRev1,
                        vtpStatsGroup,
                        vtpTrunkPortGroup,
                        vtpVersion2BasicGroup,
                        vtpVlanInfoEditGroup,
                        vtpTrunkPortGroup2,
                        vtpTrunkPortGroup3,
                        vtpTrunkPruningGroup,
                        vtpTrunkPruningGroup2,
                        vtpVlanIfIndexGroup,
                        vtp4kVlanGroupRev1,
                        vtpDot1qTunnelGroup2,
                        vtpConfigNotificationsGroup2,
                        vtpVlanNotifEnabledGroup,
                        vtpConfigNotificationsGroup3
                    }
    VARIATION       vtpVersion
    SYNTAX          INTEGER  {
                        one(1),
                        two(2)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       managementDomainRowStatus
    SYNTAX          RowStatus {
                        active(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vlanTrunkPortRowStatus
    SYNTAX          RowStatus {
                        active(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       managementDomainVersionInUse
    SYNTAX          INTEGER  {
                        version1(1),
                        version2(2)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vlanTrunkPortDynamicStatus
    SYNTAX          INTEGER  {
                        trunking(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported.
        vlanTrunkPortTable only includes the
        trunking ports."

    VARIATION       vtpVlanTypeExt
    SYNTAX          BITS {
                        vtpmanageable(0),
                        rspan(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    VARIATION       vtpVlanEditTypeExt2
    SYNTAX          BITS {
                        vtpmanageable(0),
                        rspan(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    VARIATION       managementDomainLocalMode
    SYNTAX          INTEGER  {
                        client(1),
                        server(2),
                        transparent(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    VARIATION       vtpVlanEditRowStatus
    SYNTAX          RowStatus {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    ::= { ciscoVtpCapability 2 }

ciscoVtpCapCatOSV08R0101 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco CatOS 8.1(1)."
    STATUS          current
    DESCRIPTION
        "CISCO-VTP-MIB capabilities."

    SUPPORTS        CISCO-VTP-MIB
    INCLUDES        {
                        vtpBasicGroup,
                        vtpVlanInfoGroup,
                        vtpConfigNotificationsGroupRev1,
                        vtpStatsGroup,
                        vtpTrunkPortGroup,
                        vtpVersion2BasicGroup,
                        vtpVlanInfoEditGroup,
                        vtpDot1qTunnelGroup,
                        vtpTrunkPortGroup2,
                        vtpTrunkPortGroup3,
                        vtpTrunkPruningGroup,
                        vtpTrunkPruningGroup2,
                        vtpVlanIfIndexGroup,
                        vtp4kVlanGroup,
                        vtp4kVlanGroupRev1,
                        vtpConfigNotificationsGroup2,
                        vtpVlanNotifEnabledGroup,
                        vtpConfigNotificationsGroup3,
                        vtpDiscoverGroup,
                        vtpDatabaseGroup,
                        vtpAuthGroup
                    }
    VARIATION       vtpVersion
    SYNTAX          INTEGER  {
                        one(1),
                        two(2),
                        three(4)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       managementDomainRowStatus
    SYNTAX          RowStatus {
                        active(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vlanTrunkPortRowStatus
    SYNTAX          RowStatus {
                        active(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       managementDomainVersionInUse
    SYNTAX          INTEGER  {
                        version1(1),
                        version2(2),
                        version3(4)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vtpVlanEditRowStatus
    SYNTAX          RowStatus {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    ::= { ciscoVtpCapability 3 }

ciscoVtpCapCatOSV08R0301 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco CatOS 8.3(1)."
    STATUS          current
    DESCRIPTION
        "CISCO-VTP-MIB capabilities."

    SUPPORTS        CISCO-VTP-MIB
    INCLUDES        {
                        vtpBasicGroup,
                        vtpVlanInfoGroup,
                        vtpConfigNotificationsGroupRev1,
                        vtpStatsGroup,
                        vtpTrunkPortGroup,
                        vtpVersion2BasicGroup,
                        vtpVlanInfoEditGroup,
                        vtpDot1qTunnelGroup,
                        vtpTrunkPortGroup2,
                        vtpTrunkPortGroup3,
                        vtpTrunkPruningGroup,
                        vtpTrunkPruningGroup2,
                        vtpVlanIfIndexGroup,
                        vtp4kVlanGroup,
                        vtp4kVlanGroupRev1,
                        vtpConfigNotificationsGroup2,
                        vtpVlanNotifEnabledGroup,
                        vtpConfigNotificationsGroup3,
                        vtpDiscoverGroup,
                        vtpDatabaseGroup,
                        vtpAuthGroup,
                        vtpInternalVlanGrp
                    }
    VARIATION       vtpVersion
    SYNTAX          INTEGER  {
                        one(1),
                        two(2),
                        three(4)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       managementDomainRowStatus
    SYNTAX          RowStatus {
                        active(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vlanTrunkPortRowStatus
    SYNTAX          RowStatus {
                        active(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       managementDomainVersionInUse
    SYNTAX          INTEGER  {
                        version1(1),
                        version2(2),
                        version3(4)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vtpVlanEditRowStatus
    SYNTAX          RowStatus {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    ::= { ciscoVtpCapability 4 }

ciscoVtpCapV12R0217SXACat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(17)SXA on Catalyst 6000/6500
                         and Cisco 7600 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-VTP-MIB capabilities."

    SUPPORTS        CISCO-VTP-MIB
    INCLUDES        {
                        vtpBasicGroup,
                        vtpVlanInfoGroup,
                        vtpConfigNotificationsGroupRev1,
                        vtpStatsGroup,
                        vtpTrunkPortGroup,
                        vtpVersion2BasicGroup,
                        vtpVlanInfoEditGroup,
                        vtpTrunkPortGroup2,
                        vtpTrunkPortGroup3,
                        vtpTrunkPruningGroup,
                        vtpTrunkPruningGroup2,
                        vtpVlanIfIndexGroup,
                        vtp4kVlanGroupRev1,
                        vtpDot1qTunnelGroup2,
                        vtpConfigNotificationsGroup2,
                        vtpVlanNotifEnabledGroup,
                        vtpConfigNotificationsGroup3
                    }
    VARIATION       vtpVersion
    SYNTAX          INTEGER  {
                        one(1),
                        two(2)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       managementDomainRowStatus
    SYNTAX          RowStatus {
                        active(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vlanTrunkPortRowStatus
    SYNTAX          RowStatus {
                        active(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       managementDomainVersionInUse
    SYNTAX          INTEGER  {
                        version1(1),
                        version2(2)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vtpVlanTypeExt
    SYNTAX          BITS {
                        vtpmanageable(0),
                        rspan(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    VARIATION       vtpVlanEditTypeExt2
    SYNTAX          BITS {
                        vtpmanageable(0),
                        rspan(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    VARIATION       managementDomainLocalMode
    SYNTAX          INTEGER  {
                        client(1),
                        server(2),
                        transparent(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    VARIATION       vtpVlanEditRowStatus
    SYNTAX          RowStatus {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    ::= { ciscoVtpCapability 5 }

ciscoVtpCapV12R0218SXECat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(18)SXE on Catalyst 6000/6500
                         and Cisco 7600 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-VTP-MIB capabilities."

    SUPPORTS        CISCO-VTP-MIB
    INCLUDES        {
                        vtpBasicGroup,
                        vtpVlanInfoGroup,
                        vtpConfigNotificationsGroupRev1,
                        vtpStatsGroup,
                        vtpTrunkPortGroup,
                        vtpVersion2BasicGroup,
                        vtpVlanInfoEditGroup,
                        vtpTrunkPortGroup2,
                        vtpTrunkPortGroup3,
                        vtpTrunkPruningGroup,
                        vtpTrunkPruningGroup2,
                        vtpVlanIfIndexGroup,
                        vtp4kVlanGroupRev1,
                        vtpDot1qTunnelGroup2,
                        vtpConfigNotificationsGroup2,
                        vtpVlanNotifEnabledGroup,
                        vtpConfigNotificationsGroup3,
                        vtpInternalVlanGrp
                    }
    VARIATION       vtpVersion
    SYNTAX          INTEGER  {
                        one(1),
                        two(2)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       managementDomainRowStatus
    SYNTAX          RowStatus {
                        active(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vlanTrunkPortRowStatus
    SYNTAX          RowStatus {
                        active(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       managementDomainVersionInUse
    SYNTAX          INTEGER  {
                        version1(1),
                        version2(2)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vtpVlanTypeExt
    SYNTAX          BITS {
                        vtpmanageable(0),
                        rspan(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    VARIATION       vtpVlanEditTypeExt2
    SYNTAX          BITS {
                        vtpmanageable(0),
                        rspan(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    VARIATION       managementDomainLocalMode
    SYNTAX          INTEGER  {
                        client(1),
                        server(2),
                        transparent(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    VARIATION       vtpVlanEditRowStatus
    SYNTAX          RowStatus {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    ::= { ciscoVtpCapability 6 }

ciscoVtpCapV12R0233SXHPCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(33)SXH on Catalyst 6000/6500
                         and Cisco 7600 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-VTP-MIB capabilities."

    SUPPORTS        CISCO-VTP-MIB
    INCLUDES        {
                        vtpBasicGroup,
                        vtpVlanInfoGroup,
                        vtpConfigNotificationsGroupRev1,
                        vtpStatsGroup,
                        vtpTrunkPortGroup,
                        vtpVersion2BasicGroup,
                        vtpVlanInfoEditGroup,
                        vtpTrunkPortGroup2,
                        vtpTrunkPortGroup3,
                        vtpTrunkPruningGroup,
                        vtpTrunkPruningGroup2,
                        vtpVlanIfIndexGroup,
                        vtp4kVlanGroupRev1,
                        vtpDot1qTunnelGroup2,
                        vtpConfigNotificationsGroup2,
                        vtpVlanNotifEnabledGroup,
                        vtpConfigNotificationsGroup3,
                        vtpInternalVlanGrp
                    }
    VARIATION       vtpVersion
    SYNTAX          INTEGER  {
                        one(1),
                        two(2)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       managementDomainRowStatus
    SYNTAX          RowStatus {
                        active(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vlanTrunkPortRowStatus
    SYNTAX          RowStatus {
                        active(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       managementDomainVersionInUse
    SYNTAX          INTEGER  {
                        version1(1),
                        version2(2)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vtpVlanTypeExt
    SYNTAX          BITS {
                        vtpmanageable(0),
                        rspan(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    VARIATION       vtpVlanEditTypeExt2
    SYNTAX          BITS {
                        vtpmanageable(0),
                        rspan(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    VARIATION       managementDomainLocalMode
    SYNTAX          INTEGER  {
                        client(1),
                        server(2),
                        transparent(3),
                        off(4)
                    }
    DESCRIPTION
        "The enumerated values supported are all
        those defined at the time this clause
        was written."

    VARIATION       vtpVlanEditRowStatus
    SYNTAX          RowStatus {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    ::= { ciscoVtpCapability 7 }

ciscoVtpCapCatOSV08R0701 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco CatOS 8.7(1)."
    STATUS          current
    DESCRIPTION
        "CISCO-VTP-MIB capabilities."

    SUPPORTS        CISCO-VTP-MIB
    INCLUDES        {
                        vtpBasicGroup,
                        vtpVlanInfoGroup,
                        vtpConfigNotificationsGroupRev1,
                        vtpStatsGroup,
                        vtpTrunkPortGroup,
                        vtpVersion2BasicGroup,
                        vtpVlanInfoEditGroup,
                        vtpDot1qTunnelGroup,
                        vtpTrunkPortGroup2,
                        vtpTrunkPortGroup3,
                        vtpTrunkPruningGroup,
                        vtpTrunkPruningGroup2,
                        vtpVlanIfIndexGroup,
                        vtp4kVlanGroup,
                        vtp4kVlanGroupRev1,
                        vtpConfigNotificationsGroup2,
                        vtpVlanNotifEnabledGroup,
                        vtpConfigNotificationsGroup3,
                        vtpDiscoverGroup,
                        vtpDatabaseGroup,
                        vtpAuthGroup,
                        vtpInternalVlanGrp,
                        vtpConfigNotificationsGroup6
                    }
    VARIATION       vtpVersion
    SYNTAX          INTEGER  {
                        one(1),
                        two(2),
                        three(4)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       managementDomainRowStatus
    SYNTAX          RowStatus {
                        active(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vlanTrunkPortRowStatus
    SYNTAX          RowStatus {
                        active(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       managementDomainVersionInUse
    SYNTAX          INTEGER  {
                        version1(1),
                        version2(2),
                        version3(4)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vtpVlanEditRowStatus
    SYNTAX          RowStatus {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    ::= { ciscoVtpCapability 8 }

ciscoVtpCapV12R0233SXIPCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(33)SXI on Catalyst 6000/6500
                    series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-VTP-MIB capabilities."

    SUPPORTS        CISCO-VTP-MIB
    INCLUDES        {
                        vtpBasicGroup,
                        vtpVlanInfoGroup,
                        vtpConfigNotificationsGroupRev1,
                        vtpStatsGroup,
                        vtpTrunkPortGroup,
                        vtpVersion2BasicGroup,
                        vtpVlanInfoEditGroup,
                        vtpTrunkPortGroup2,
                        vtpTrunkPortGroup3,
                        vtpTrunkPruningGroup,
                        vtpTrunkPruningGroup2,
                        vtpVlanIfIndexGroup,
                        vtp4kVlanGroupRev1,
                        vtpDot1qTunnelGroup2,
                        vtpConfigNotificationsGroup2,
                        vtpVlanNotifEnabledGroup,
                        vtpConfigNotificationsGroup3,
                        vtpInternalVlanGrp,
                        vtpDiscoverGroup,
                        vtpDatabaseGroup,
                        vtpAuthGroup,
                        vlanStatsGroup,
                        vtpConfigNotificationsGroup6
                    }
    VARIATION       vtpVersion
    SYNTAX          INTEGER  {
                        one(1),
                        two(2),
                        three(4)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       managementDomainRowStatus
    SYNTAX          RowStatus {
                        active(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vlanTrunkPortRowStatus
    SYNTAX          RowStatus {
                        active(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       managementDomainVersionInUse
    SYNTAX          INTEGER  {
                        version1(1),
                        version2(2),
                        version3(4)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vtpVlanTypeExt
    SYNTAX          BITS {
                        vtpmanageable(0),
                        rspan(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    VARIATION       vtpVlanEditTypeExt2
    SYNTAX          BITS {
                        vtpmanageable(0),
                        rspan(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    VARIATION       managementDomainLocalMode
    SYNTAX          INTEGER  {
                        client(1),
                        server(2),
                        transparent(3),
                        off(4)
                    }
    DESCRIPTION
        "The enumerated values supported are all
        those defined at the time this clause
        was written."

    VARIATION       vtpVlanEditRowStatus
    SYNTAX          RowStatus {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    ::= { ciscoVtpCapability 9 }

ciscoVtpCapV12R0233SXI4PCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(33)SXI4 on Catalyst 6000/6500
                    series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-VTP-MIB capabilities."

    SUPPORTS        CISCO-VTP-MIB
    INCLUDES        {
                        vtpBasicGroup,
                        vtpVlanInfoGroup,
                        vtpConfigNotificationsGroupRev1,
                        vtpStatsGroup,
                        vtpTrunkPortGroup,
                        vtpVersion2BasicGroup,
                        vtpVlanInfoEditGroup,
                        vtpTrunkPortGroup2,
                        vtpTrunkPortGroup3,
                        vtpTrunkPruningGroup,
                        vtpTrunkPruningGroup2,
                        vtpVlanIfIndexGroup,
                        vtp4kVlanGroupRev1,
                        vtpDot1qTunnelGroup2,
                        vtpConfigNotificationsGroup2,
                        vtpVlanNotifEnabledGroup,
                        vtpConfigNotificationsGroup3,
                        vtpInternalVlanGrp,
                        vtpDiscoverGroup,
                        vtpDatabaseGroup,
                        vtpAuthGroup,
                        vlanStatsGroup,
                        vtpConfigNotificationsGroup6,
                        vtpTrunkPruningGroup3,
                        vtpConfigNotificationsGroup8
                    }
    VARIATION       vtpVersion
    SYNTAX          INTEGER  {
                        one(1),
                        two(2),
                        three(4)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       managementDomainRowStatus
    SYNTAX          RowStatus {
                        active(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vlanTrunkPortRowStatus
    SYNTAX          RowStatus {
                        active(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       managementDomainVersionInUse
    SYNTAX          INTEGER  {
                        version1(1),
                        version2(2),
                        version3(4)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vtpVlanTypeExt
    SYNTAX          BITS {
                        vtpmanageable(0),
                        rspan(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    VARIATION       vtpVlanEditTypeExt2
    SYNTAX          BITS {
                        vtpmanageable(0),
                        rspan(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    VARIATION       managementDomainLocalMode
    SYNTAX          INTEGER  {
                        client(1),
                        server(2),
                        transparent(3),
                        off(4)
                    }
    DESCRIPTION
        "The enumerated values supported are all
        those defined at the time this clause
        was written."

    VARIATION       vtpVlanEditRowStatus
    SYNTAX          RowStatus {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    ::= { ciscoVtpCapability 10 }

ciscoVtpCapV12R0254SGPCat4K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(54)SG on CAT4K family switches."
    STATUS          current
    DESCRIPTION
        "CISCO-VTP-MIB capabilities."

    SUPPORTS        CISCO-VTP-MIB
    INCLUDES        {
                        vtpBasicGroup,
                        vtpVlanInfoGroup,
                        vtpConfigNotificationsGroupRev1,
                        vtpStatsGroup,
                        vtpTrunkPortGroup,
                        vtpVersion2BasicGroup,
                        vtpVlanInfoEditGroup,
                        vtpTrunkPortGroup2,
                        vtpTrunkPortGroup3,
                        vtpTrunkPruningGroup,
                        vtpTrunkPruningGroup2,
                        vtpVlanIfIndexGroup,
                        vtp4kVlanGroupRev1,
                        vtpDot1qTunnelGroup2,
                        vtpConfigNotificationsGroup2,
                        vtpVlanNotifEnabledGroup,
                        vtpConfigNotificationsGroup3,
                        vtpInternalVlanGrp,
                        vtpDiscoverGroup,
                        vtpDatabaseGroup,
                        vtpAuthGroup,
                        vtpConfigNotificationsGroup6
                    }
    VARIATION       vtpVersion
    SYNTAX          INTEGER  {
                        one(1),
                        two(2),
                        three(4)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       managementDomainRowStatus
    SYNTAX          RowStatus {
                        active(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vlanTrunkPortRowStatus
    SYNTAX          RowStatus {
                        active(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       managementDomainVersionInUse
    SYNTAX          INTEGER  {
                        version1(1),
                        version2(2),
                        version3(4)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vtpVlanTypeExt
    SYNTAX          BITS {
                        vtpmanageable(0),
                        rspan(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    VARIATION       vtpVlanEditTypeExt2
    SYNTAX          BITS {
                        vtpmanageable(0),
                        rspan(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    VARIATION       managementDomainLocalMode
    SYNTAX          INTEGER  {
                        client(1),
                        server(2),
                        transparent(3),
                        off(4)
                    }
    DESCRIPTION
        "The enumerated values supported are all
        those defined at the time this clause
        was written."

    VARIATION       vtpVlanEditRowStatus
    SYNTAX          RowStatus {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is
        supported."

    ::= { ciscoVtpCapability 11 }

ciscoVtpCapNxOSV05R0101PN7K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco NX-OS 5.1(1) on Nexus 7000 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-VTP-MIB capabilities."

    SUPPORTS        CISCO-VTP-MIB
    INCLUDES        {
                        vtpBasicGroup,
                        vtpVlanInfoGroup,
                        vtpConfigNotificationsGroupRev1,
                        vtpStatsGroup,
                        vtpTrunkPortGroup,
                        vtpVersion2BasicGroup,
                        vtpTrunkPortGroup2,
                        vtpTrunkPortGroup3,
                        vtpTrunkPruningGroup,
                        vtpTrunkPruningGroup2,
                        vtpVlanIfIndexGroup,
                        vtp4kVlanGroupRev1,
                        vtpConfigNotificationsGroup2,
                        vtpVlanNotifEnabledGroup,
                        vtpConfigNotificationsGroup3,
                        vtpInternalVlanGrp,
                        vtpAuthGroup,
                        vlanStatsGroup,
                        vtpConfigNotificationsGroup6,
                        vtpTrunkPruningGroup3,
                        vlanTrunkPortActiveVlansGroup
                    }
    VARIATION       vtpVersion
    SYNTAX          INTEGER  {
                        two(2),
                        none(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       vtpNotificationsEnabled
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       managementDomainName
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       managementDomainLocalMode
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       managementDomainTftpServer
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       managementDomainTftpPathname
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       managementDomainRowStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       vlanTrunkPortManagementDomain
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       vlanTrunkPortEncapsulationType
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       vlanTrunkPortNativeVlan
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       vlanTrunkPortRowStatus
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       vlanTrunkPortSetSerialNo
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       vlanTrunkPortVlansPruningEligible
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       managementDomainPruningState
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       vlanTrunkPortDynamicState
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       vlanTrunkPortVtpEnabled
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       managementDomainVersionInUse
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       vtpVlanCreatedNotifEnabled
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       vtpVlanDeletedNotifEnabled
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       vtpVlanEditTypeExt2
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       vtpVlansPruningEligible2k
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       vtpVlansPruningEligible3k
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       vtpVlansPruningEligible4k
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       vtpAuthPassword
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       vtpAuthPasswordType
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       vtpAuthSecretKey
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       vtpInternalVlanAllocPolicy
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    ::= { ciscoVtpCapability 12 }

END



