-- *********************************************************************
-- CISCO-L2-CONTROL-CAPABILITY.my:
-- Cisco CISCO-L2-CONTROL-MIB AGENT-CAPABILITIES
--
-- Oct. 2003, Frank Chao
--
-- Copyright(c) 2003, 2004, 2005, 2006, 2007 by Cisco Systems, Inc.
--
-- *********************************************************************

CISCO-L2-CONTROL-CAPABILITY DEFINITIONS ::= BEGIN
IMPORTS
        Unsigned32
            FROM SNMPv2-SMI
        MODULE-IDENTITY
                FROM SNMPv2-SMI
        AGENT-CAPABILITIES
                FROM SNMPv2-CONF
        ciscoAgentCapability
                FROM CISCO-SMI;   

ciscoL2ControlCapability MODULE-IDENTITY
        LAST-UPDATED    "200706300000Z"
        ORGANIZATION    "Cisco Systems, Inc."
        CONTACT-INFO
                "       Cisco Systems
                        Customer Service

                Postal: 170 W Tasman Drive
                        San Jose, CA  95134
                        USA

                        Tel: +1 800 553-NETS

                E-mail: cs-lan-switch-snmp@cisco.com"
        DESCRIPTION
                "The Agent capabilities for CISCO-L2-CONTROL-MIB."
        REVISION        "200706300000Z"
        DESCRIPTION
                "Added clcCapabilityV12R0233SXHPCat6K agent
                 capability statement."
        REVISION        "200702280000Z"
        DESCRIPTION
                "Added clcCapabilityCatOSV08R0601 agent
                 capability statement and added VARIATIONS 
                 of clcMacLimitExceededActionDefault to
                 clcCapabilityV12R0217aSXCat6K."
        REVISION        "200411010000Z"
        DESCRIPTION
                "clcVlanMacAddressLimitGroup is supported in
                 clcCapabilityV12R0217aSXCat6K capability
                 statement."
        REVISION        "200403290000Z"
        DESCRIPTION
                "Added clcCapabilityCatOSV08R0301 agent
                 capability statement."
        REVISION        "200310310000Z"
        DESCRIPTION
                "Initial version of this MIB module."
        ::= { ciscoAgentCapability 397 }


clcCapabilityV12R0217aSXCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE  "Cisco IOS 12.2(17a)SX on Catalyst 6000/6500
                      and Cisco 7600 series devices."
    STATUS            current
    DESCRIPTION       "CISCO-L2-CONTROL-MIB capabilities."

    SUPPORTS          CISCO-L2-CONTROL-MIB
        INCLUDES      {
                          clcMacAddressLimitGroup,
                          clcVlanMacAddressLimitGroup,
                          clcVlanMacLimitNotifsGroup
                      }
        VARIATION       clcMacLimitExceededActionDefault
            SYNTAX      INTEGER { warning(1), limit(2),
                                  shutdown(4) }
            DESCRIPTION "Only limited set of enumerated values
                         are supported."

    ::= { ciscoL2ControlCapability 1 }

clcCapabilityCatOSV08R0301 AGENT-CAPABILITIES
    PRODUCT-RELEASE  "Cisco CatOS 8.3(1)."
    STATUS            current
    DESCRIPTION      "CISCO-L2-CONTROL-MIB capabilities."

    SUPPORTS         CISCO-L2-CONTROL-MIB
        INCLUDES     {
                         clcUnicastFloodGroup
                     }

    ::= { ciscoL2ControlCapability 2 }

clcCapabilityCatOSV08R0601 AGENT-CAPABILITIES
    PRODUCT-RELEASE  "Cisco CatOS 8.6(1) on Catalyst 6000/6500
                      and Cisco 7600 series devices."
    STATUS            current
    DESCRIPTION      "CISCO-L2-CONTROL-MIB capabilities."

    SUPPORTS         CISCO-L2-CONTROL-MIB
        INCLUDES     {
                         clcMacAddressLimitGroup,
                         clcVlanMacAddressLimitGroup,
                         clcVlanMacLimitNotifsGroup,
                         clcUnicastFloodGroup,
                         clcMacAddressLimitIntervalGroup,
                         clcMacAddressLimitGroup1,
                         clcVlanMacAddressLimitGroup1,
                         clcVlanMacLimitEnableGroup,
                         clcVlanMacLimitNotifControlGroup,
                         clcVlanMacLimitNotifControlGroup1,
                         clcVlanMacLimitNotifsGroup1,
                         clcIfMacAddressLimitGroup,
                         clcIfMacLimitEnableGroup,
                         clcIfMacLimitNotifControlGroup,
                         clcIfMacLimitNotifsGroup,
                         clcIfVlanMacAddressLimitGroup,
                         clcIfVlanMacLimitEnableGroup,
                         clcIfVlanMacLimitNotifControlGroup,
                         clcIfVlanMacLimitNotifsGroup
                     }
        VARIATION       clcMaxMacLimitDefault
            ACCESS      read-only
            DESCRIPTION "Implementation supports read-only access
                          for this object." 

        VARIATION       clcMacLimitExceededActionDefault
            ACCESS      read-only
            DESCRIPTION "Implementation supports read-only access
                         for this object."

        VARIATION       clcMacLimitExceedNotifOption
            ACCESS      read-only
            DESCRIPTION "Implementation supports read-only access
                         for this object."

        VARIATION       clcMacLimitHighDefault
            ACCESS      read-only
            DESCRIPTION "Implementation supports read-only access
                         for this object." 

        VARIATION       clcMacLimitHighExceedActionDef
            ACCESS      read-only
            DESCRIPTION "Implementation supports read-only access
                         for this object."

        VARIATION       clcMacLimitInterval
            SYNTAX      Unsigned32(5..3600)
            DESCRIPTION "Only limited set of values are supported."

        VARIATION       clcVlanMaxMacLimit
            SYNTAX      Unsigned32(0 | 5..32000)
            DESCRIPTION "Only limited set of values are supported."

        VARIATION       clcVlanMacLimitExceededAction
            SYNTAX      INTEGER {
                            warning(1),
                            limit(2)
                        }
            DESCRIPTION "Only limited set of enumerated values 
                         are supported."

        VARIATION       clcVlanMacLimitHigh
            SYNTAX      Unsigned32(0 | 5..32000)
            DESCRIPTION "Only limited set of values are supported."

        VARIATION       clcVlanMacLimitHighExceedAction
            SYNTAX      INTEGER {
                            warning(1),
                            limit(2),
                            shutdown(4)
                        }
            DESCRIPTION "Only limited set of enumerated values 
                         are supported."

        VARIATION       clcIfMacLimitLow
            SYNTAX      Unsigned32(0 | 5..32000)
            DESCRIPTION "Only limited set of values are supported."

        VARIATION       clcIfMacLimitLowExceedAction
            SYNTAX      INTEGER {
                            warning(1),
                            limit(2)
                        }
            DESCRIPTION "Only limited set of enumerated values 
                         are supported."

        VARIATION       clcIfMacLimitHigh
            SYNTAX      Unsigned32(0 | 5..32000)
            DESCRIPTION "Only limited set of values are supported."

        VARIATION       clcIfMacLimitHighExceedAction
            SYNTAX      INTEGER {
                            warning(1),
                            limit(2),
                            shutdown(4)
                        }
            DESCRIPTION "Only limited set of enumerated values 
                         are supported."

        VARIATION       clcIfVlanMacLimitLow
            SYNTAX      Unsigned32(0 | 5..32000)
            DESCRIPTION "Only limited set of values are supported."

        VARIATION       clcIfVlanMacLimitLowExceedAction
            SYNTAX      INTEGER {
                            warning(1),
                            limit(2)
                        }
            DESCRIPTION "Only limited set of enumerated values 
                         are supported."

        VARIATION       clcIfVlanMacLimitHigh
            SYNTAX      Unsigned32(0 | 5..32000)
            DESCRIPTION "Only limited set of values are supported."

        VARIATION       clcIfVlanMacLimitHiExceedAction
            SYNTAX      INTEGER {
                            warning(1),
                            limit(2),
                            shutdown(4)
                        }
            DESCRIPTION "Only limited set of enumerated values 
                         are supported."

    ::= { ciscoL2ControlCapability 3 }

clcCapabilityV12R0233SXHPCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE   "Cisco IOS 12.2(33)SXH on Catalyst 6000/6500
                       series devices."
    STATUS            current
    DESCRIPTION       "CISCO-L2-CONTROL-MIB capabilities."

    SUPPORTS          CISCO-L2-CONTROL-MIB
        INCLUDES      {
                          clcMacAddressLimitGroup,
                          clcVlanMacAddressLimitGroup,
                          clcVlanMacLimitNotifsGroup,
                          clcUnicastFloodGroup
                      }
        VARIATION       clcMacLimitExceededActionDefault
            SYNTAX      INTEGER { warning(1), limit(2),
                                  shutdown(4) }
            DESCRIPTION "Only limited set of enumerated values
                         are supported."

    ::= { ciscoL2ControlCapability 4 }
END
