EXTREME-FILETRANSFER-MIB DEFINITIONS ::= BEGIN

IMPORTS
      MODULE-IDENTITY, IpAddress, OBJECT-TYPE        
                        FROM SNMPv2-SMI
      DisplayString, TestAndIncr, RowStatus
            FROM SNMPv2-TC
      OwnerString       FROM RMON-MIB
      extremeAgent    FROM EXTREME-BASE-MIB;

extremeFileTransfer    MODULE-IDENTITY
    LAST-UPDATED    "9810211630Z"
    ORGANIZATION    "Extreme Networks, Inc."
    CONTACT-INFO    "www.extremenetworks.com"
    DESCRIPTION    "Extreme File transfer objects"
    ::= {extremeAgent 10}

-- The file transfer group

extremeFileTransferGroup OBJECT IDENTIFIER ::= { extremeFileTransfer 1 }

extremeFileTransferNextAvailableIndex OBJECT-TYPE
    SYNTAX  TestAndIncr
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
          "The index of the next free row in the extremeFileTransferTable."
    ::= { extremeFileTransferGroup 1}

extremeFileTransferTable OBJECT-TYPE
    SYNTAX    SEQUENCE OF FileTransferEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A table of pending and completed file transfers."
    ::= { extremeFileTransferGroup 2 }

extremeFileTransferEntry OBJECT-TYPE
    SYNTAX    FileTransferEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
                "A table entry containing information on a pending
                or completed file transfer."
    INDEX    { extremeFileTransferIndex }
    ::= { extremeFileTransferTable 1 }

FileTransferEntry ::=
    SEQUENCE {
        extremeFileTransferIndex            INTEGER,
        extremeFileTransferServerAddress        IpAddress,
        extremeFileTransferFileName                    DisplayString,
        extremeFileTransferOperation            INTEGER,
        extremeFileTransferScheduledTime        OCTET STRING,
        extremeFileTransferStartAdminStatus        INTEGER,
        extremeFileTransferStartOperStatus        INTEGER,
        extremeFileTransferLastExecutionStatus        INTEGER,
        extremeFileTransferOwner                       OwnerString,
        extremeFileTransferRowStatus            RowStatus
    }
        
extremeFileTransferIndex OBJECT-TYPE
        SYNTAX  INTEGER
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
        "An index into the file transfer table."
        ::= { extremeFileTransferEntry 1 }

extremeFileTransferServerAddress OBJECT-TYPE
        SYNTAX  IpAddress
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
        "This is the address of the TFTP server from which to
        download the image or configuration or upload the 
        configuration."
        ::= { extremeFileTransferEntry 2 }

extremeFileTransferFileName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(0..64))
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
        "This is the name of the file to be downloaded or uploaded."
        ::= { extremeFileTransferEntry 3 }

extremeFileTransferOperation OBJECT-TYPE
         SYNTAX  INTEGER {
                    downloadImageToPrimaryImmediate(1),
                    downloadImageToSecondaryImmediate(2),
                    downloadConfigImmediate(3),
                    uploadConfigImmediate(4),
                    scheduleConfigUploadPeriodic(5),
                    scheduleConfigUploadOnce(6),
                    scheduleImageDownloadToPrimaryOnce(7),
                    scheduleImageDownloadToSecondaryOnce(8),
            scheduleConfigDownloadOnce(9)
                 }
         MAX-ACCESS  read-create
         STATUS  current
         DESCRIPTION 
                 "Indication of the file transfer operation.
                  This object allows configuration of uploads and/or
                  downloads either immediately or at a scheduled time.

          A value of downloadImageToPrimaryImmediate(1) or 
          downloadImageToSecondaryImmediate(2) describes immediate 
          download of a software image to either the primary or 
          secondary permanent store. A value of 
          downloadConfigImmediate(3) describes immediate download
          of a configuration file to non-volatile store. A value
          of uploadConfigImmediate(4) describes the immediate upload
          of the currently running configuration to the server.

          A value of scheduleConfigUploadOnce(6) describes a single 
          upload of the current configuration to the server at the 
          time extremeFileTransferScheduledTime. A value of 
          scheduleConfigUploadPeriodic(5) describes daily uploads 
          of the current configuration to the server at the time 
          extremeFileTransferScheduledTime every day.

          A value of scheduleImageDownloadToPrimaryOnce(7) or 
          scheduleImageDownloadToSecondaryOnce(8) describes a single 
          download of a software image to either the primary or 
          secondary permanent store at the time
          extremeFileTransferScheduledTime.

          This object can be modified only if
          extremeFileTransferStartOperStatus for this entry is idle(1).

                  Note that any attempts to modify this object including
                  row creation which would result in multiple downloads
                  would cause the operation to fail. Managers are
                  strongly recommened to examine the 
                  extremeFileTransferStartOperStatus object for the entries
                  in the table to determine the status of downloads
                  before attempting to modify this object."
         ::= { extremeFileTransferEntry 4 }

extremeFileTransferScheduledTime OBJECT-TYPE -- This convention is from RMON2
        SYNTAX  OCTET STRING (SIZE (0 | 8 | 11))
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
                "The time of the day at which the file transfer operation 
                should be initiated. This object is meaningful only for
                scheduled file transfers.

                field  octets  contents                  range
                -----  ------  --------                  -----
                1      1-2   year                      0..65536
                2       3    month                     1..12
                3       4    day                       1..31
                4       5    hour                      0..23
                5       6    minutes                   0..59
                6       7    seconds                   0..60
                                         (use 60 for leap-second)
                7       8    deci-seconds              0..9
                8       9    direction from UTC        '+' / '-'
                9      10    hours from UTC            0..11
                10      11    minutes from UTC         0..59

                For example, Tuesday May 26, 1992 at 1:30:15 PM
                EDT would be displayed as:

                     1992-5-26,13:30:15.0,-4:0

                Note that if only local time is known, then
                timezone information (fields 8-10) is not
                present, and if no time information is known, the null
                string is returned."
        ::= { extremeFileTransferEntry 5 }
    
extremeFileTransferStartAdminStatus OBJECT-TYPE
         SYNTAX  INTEGER {
                    start(1),
                    cancel(2)       
                 }
         MAX-ACCESS  read-create
         STATUS  current
         DESCRIPTION 
                 "Writing to this object initiates the upload/download or
                 schedules one. The extremeFileTransferStartOperStatus object
                 should be checked before attempting to set this object.
                 This object cannot be modified while the 
                 extremeFileTransferStartOperStatus is inProgress(3). This
         object can be set start(1) only if the
         extremeFileTransferStartOperStatus is idle(1). A scheduled
         upload/download will be cancelled by setting the value of
         this object to cancel(2)."
         DEFVAL { cancel }
        ::= { extremeFileTransferEntry 6}
    
extremeFileTransferStartOperStatus OBJECT-TYPE
        SYNTAX  INTEGER {
                  idle(1),
                  scheduled(2),
                  inProgress(3)
                }
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION 
        "The agent sets this value to reflect the current status of 
                the file transfer operation. Reading this object is meaningful 
                only if the extremeFileTransferRowStatus is active(1). The
        current status is determined by the agent by examining the
        values for extremeFileTransferOperation and
        extremeFileTransferStartAdminStatus."
        ::= { extremeFileTransferEntry 7 }

extremeFileTransferLastExecutionStatus OBJECT-TYPE
        SYNTAX  INTEGER { -- These values are from RMON-2
                    success(1),
                    statusUnknown(2),
                    generalError(3),
                    noResponseFromServer(4),
                    checksumError(5),
                    incompatibleImage(6),
                    tftpFileNotFound(7),
                    tftpAccessViolation(8),
            fileTooLarge(9),
            downloadInProgress(10)
                }
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION 
        "The  status of the last file transfer operation. This value 
                is returned as statusUnknown(1) until the
        extremeFileTransferRowStatus is set to active(1) or when the
        extremeFileTransferStartOperStatus is inProgress(3). After an
        upload/download, the agent will update this value with the
        result of the file transfer. Managers should read this object
        before modifying extremeFileTransferOperation because the
        agent would set this value to statusUnknown(2) in such cases."
        ::= { extremeFileTransferEntry 8 }

extremeFileTransferOwner OBJECT-TYPE
        SYNTAX  OwnerString(SIZE (0..32))
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
                "Indicates the identity of the manager that configured this
                 file transfer entry."
        ::= { extremeFileTransferEntry 9 }

extremeFileTransferRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
                "The status of this table entry. This object can not be
        modified while the extremeFileTransferStatus is inProgress(1).
        Setting this object to notInService(2) or destroy(6) will
        cancel any scheduled uploads if this entry was configured for
        one.

                Note that any attempts to create new rows which would result
        in multiple downloads would cause the row creation to fail.
        Similarly, attempting to delete a row while
        extremeFileTransferStartOperStatus is inProgress(3) would fail.
        Managers are strongly recommened to examine the
        extremeFileTransferStartOperStatus object for the entries in 
                the table to determine the status of downloads before
        attempting row creation/deletion."
        ::= { extremeFileTransferEntry 10 }

END

-- ################################################################################

