-- $Id: OLD-CISCO-TS.MIB 1.1 2005/03/14 16:34:08Z aminchew Exp $
-- $Source: v:/mksroot/rcs/OLD-CISCO-TS.MIB $
-- *****************************************************************
-- OLD-CISCO-TS-MIB.my:  Cisco Terminal Service MIB file
--
-- May 1994, Jeffrey T. Johnson
--
-- Copyright (c) 1994-1997, 1998, 1999 by cisco Systems, Inc.
-- All rights reserved.
--
-- NOTE WELL
-- Starting with IOS 12.0, all objects defined in this mib have been
-- deprecated.  Management applications should no longer
-- be examining the objects defined in this document
-- NOTE WELL
-- 
-- *****************************************************************
-- $Log: OLD-CISCO-TS.MIB $
-- Revision 1.1  2005/03/14 16:34:08Z  aminchew
-- Initial revision
-- Revision 1.1.2.1  2005/02/08 01:45:11  bruceg
-- CGESM_12_2_25
--
-- Revision 3.2  1995/11/17  08:36:20  hampton
-- Remove old entries from the RCS header logs.
--
-- Revision 3.1  1995/11/09  10:51:48  shaker
-- Bump version numbers from 2.x to 3.x.
--
-- Revision 2.1  1995/06/07  20:02:32  hampton
-- Bump version numbers from 1.x to 2.x.
--
-- *****************************************************************
-- $Endlog$
--

               OLD-CISCO-TS-MIB DEFINITIONS ::= BEGIN

               IMPORTS
			IpAddress
				FROM RFC1155-SMI
			OBJECT-TYPE
				FROM RFC-1212
			DisplayString
				FROM RFC1213-MIB
			local
				FROM CISCO-SMI;
          
               lts                 OBJECT IDENTIFIER ::= { local 9 }

               -- Local cisco Terminal Service Group

          -- This group is present in all products which contain
          -- asynchronous terminal lines.

               tsLines OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Number of terminal lines on this device.
                           Includes virtual lines."
                   ::= { lts 1 }


               -- Local Terminal Service Line Table

          -- This group contains terminal service specific
          -- information on a per line basis.

               ltsLineTable OBJECT-TYPE
                   SYNTAX  SEQUENCE OF LtsLineEntry
                   ACCESS  not-accessible
                   STATUS  deprecated
                   DESCRIPTION
                            "A list of terminal server line entries."
                   ::= { lts 2 }

               ltsLineEntry OBJECT-TYPE
                   SYNTAX LtsLineEntry
                   ACCESS  not-accessible
                   STATUS  deprecated
                   DESCRIPTION
                            "A collection of per TTY objects in the
                            cisco Terminal Server implementation."
                   INDEX { tsLineNumber }
               ::= { ltsLineTable 1 }

               LtsLineEntry ::=
                   SEQUENCE {
                       tsLineActive
                           INTEGER,
                       tsLineType
                           INTEGER,
                       tsLineAutobaud
                           INTEGER,
                       tsLineSpeedin
                           INTEGER,
                       tsLineSpeedout
                           INTEGER,
                       tsLineFlow
                           INTEGER,
                       tsLineModem
                           INTEGER,
                       tsLineLoc
                           DisplayString,
                       tsLineTerm
                           DisplayString,
                       tsLineScrlen
                           INTEGER,
                       tsLineScrwid
                           INTEGER,
                       tsLineEsc
                           DisplayString,
                       tsLineTmo
                           INTEGER,
                       tsLineSestmo
                           INTEGER,
                       tsLineRotary
                           INTEGER,
                       tsLineUses
                           INTEGER,
                       tsLineNses
                           INTEGER,
                       tsLineUser
                           DisplayString,
                       tsLineNoise
                           INTEGER,
                       tsLineNumber
                           INTEGER,
                       tsLineTimeActive
                           INTEGER
                   }


          -- The following section describes the components of the
          -- table.

               tsLineActive OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Boolean whether this line is active or not."
                   ::= { ltsLineEntry 1 }

               tsLineType OBJECT-TYPE
                   SYNTAX  INTEGER {
                        unknown(1),
                        console(2),
                        terminal(3),
                        line-printer(4),
                        virtual-terminal(5),
                        auxiliary(6)
                   }
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Type of line."
                   ::= { ltsLineEntry 2 }

               tsLineAutobaud OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Boolean whether line will autobaud or not."
                   ::= { ltsLineEntry 3 }

               tsLineSpeedin OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "What input speed the line is running at."
                   ::= { ltsLineEntry 4 }

               tsLineSpeedout OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "What output speed the line is running at."
                   ::= { ltsLineEntry 5 }

               tsLineFlow OBJECT-TYPE
                   SYNTAX  INTEGER {
                        unknown(1),
                        none(2),
                        software-input(3),
                        software-output(4),
                        software-both(5),
                        hardware-input(6),
                        hardware-output(7),
                        hardware-both(8)
                   }
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "What kind of flow control the line is
                           using."
                   ::= { ltsLineEntry 6 }

               tsLineModem OBJECT-TYPE
                   SYNTAX  INTEGER {
                        unknown(1),
                        none(2),
                        call-in(3),
                        call-out(4),
                        cts-required(5),
                        ri-is-cd(6),
                        inout(7)
                   }
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "What kind of modem control the line is
                           using."
                   ::= { ltsLineEntry 7 }

               tsLineLoc OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Describes the line's physical location."
                   ::= { ltsLineEntry 8 }

               tsLineTerm OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Describes the line's terminal type."
                   ::= { ltsLineEntry 9 }

               tsLineScrlen OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Length in lines of the screen of terminal
                           attached to this line."
                   ::= { ltsLineEntry 10 }

               tsLineScrwid OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Width in characters of the screen of
                           terminal attached to this line."
                   ::= { ltsLineEntry 11 }

               tsLineEsc OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Escape character used to break out of active
                           sessions."
                   ::= { ltsLineEntry 12 }

               tsLineTmo OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Line idleness timeout in seconds."
                   ::= { ltsLineEntry 13 }

               tsLineSestmo OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Session idleness timeout in seconds."
                   ::= { ltsLineEntry 14 }

               tsLineRotary OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Rotary group number the line belongs in."
                   ::= { ltsLineEntry 15 }

               tsLineUses OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Number of times a connection has been made
                           to or from this line."
                   ::= { ltsLineEntry 16 }

               tsLineNses OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Current number of sessions in use on this
                           line."
                   ::= { ltsLineEntry 17 }

               tsLineUser OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "TACACS user name, if TACACS enabled, of user
                           on this line."
                   ::= { ltsLineEntry 18 }

               tsLineNoise OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Count of garbage characters received when
                           line inactive."
                   ::= { ltsLineEntry 19 }

               tsLineNumber OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "The line i've been talking about."
                   ::= { ltsLineEntry 20 }

               tsLineTimeActive OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "The time in seconds since line was activated."
                   ::= { ltsLineEntry 21 }
               -- End of table

               -- Local Terminal Service Line Session Table

          -- This group contains terminal server specific
          -- information on a per line and per session basis.

               ltsLineSessionTable OBJECT-TYPE
                   SYNTAX  SEQUENCE OF LtsLineSessionEntry
                   ACCESS  not-accessible
                   STATUS  deprecated
                   DESCRIPTION
                            "A list of terminal server line and session
                            entries."
                   ::= { lts 3 }

               ltsLineSessionEntry OBJECT-TYPE
                   SYNTAX LtsLineSessionEntry
                   ACCESS  not-accessible
                   STATUS  deprecated
                   DESCRIPTION
                            "A collection of per session and per TTY
                            objects in the cisco Terminal Server
                            implementation."
                   INDEX { tslineSesLine, tslineSesSession }
               ::= { ltsLineSessionTable 1 }

               LtsLineSessionEntry ::=
                   SEQUENCE {
                       tslineSesType
                           INTEGER,
                       tslineSesDir
                           INTEGER,
                       tslineSesAddr
                           IpAddress,
                       tslineSesName
                           DisplayString,
                       tslineSesCur
                           INTEGER,
                       tslineSesIdle
                           INTEGER,
                       tslineSesLine
                           INTEGER,
                       tslineSesSession 
                           INTEGER
                   }


          -- The following section describes the components of the
          -- table.

               tslineSesType OBJECT-TYPE
                   SYNTAX  INTEGER {
                        unknown(1),
                        pad(2),
                        stream(3),
                        rlogin(4),
                        telnet(5),
                        tcp(6),
                        lat(7),
                        mop(8),
                        slip(9),
                        xremote(10),
			rshell(11),
			ipc(12),
			udptn(13)
                   }
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Type of session."
                   ::= { ltsLineSessionEntry 1 }

               tslineSesDir OBJECT-TYPE
                   SYNTAX  INTEGER {
                        unknown(1),
                        incoming(2),
                        outgoing(3)
                   }
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Direction of session."
                   ::= { ltsLineSessionEntry 2 }

               tslineSesAddr OBJECT-TYPE
                   SYNTAX  IpAddress
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Remote host address of session. [What about
                           PAD connections?]"
                   ::= { ltsLineSessionEntry 3 }

               tslineSesName OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Remote host name of session."
                   ::= { ltsLineSessionEntry 4 }

               tslineSesCur OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Boolean whether session is the currently
                           active one."
                   ::= { ltsLineSessionEntry 5 }

               tslineSesIdle OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Time in seconds session has been idle."
                   ::= { ltsLineSessionEntry 6 }

               tslineSesLine OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Table index 1."
                   ::= { ltsLineSessionEntry 7 }

               tslineSesSession OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-only
                   STATUS  deprecated
                   DESCRIPTION
                           "Table index 2."
                   ::= { ltsLineSessionEntry 8 }

               -- End of table


               tsMsgTtyLine OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-write
                   STATUS  deprecated
                   DESCRIPTION
                           "tty line to send the message to. -1 will
                           send it to all tty lines"
                   ::= { lts 4 }

               tsMsgIntervaltim OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-write
                   STATUS  deprecated
                   DESCRIPTION
                           "Interval between reissuing message in
                           milliseconds. Minimum non-zero setting is
                           10000. 0 will cause the routine to choose its
                           own intervals becoming more frequent as
                           MessageDuration gets close to expiring. 2hr,
                           1hr, 30min, 5min, 1min"
                   ::= { lts 5 }

               tsMsgDuration OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-write
                   STATUS  deprecated
                   DESCRIPTION
                           "Length of time to reissue message in
                           milliseconds. Minimum non-zero setting is
                           10000. A setting of 0 will not repeat the
                           message."
                   ::= { lts 6 }

               tsMsgText OBJECT-TYPE
                   SYNTAX  DisplayString
                   ACCESS  read-write
                   STATUS  deprecated
                   DESCRIPTION
                           "Up to 256 characters that will make up the
                           message"
                   ::= { lts 7 }

               tsMsgTmpBanner OBJECT-TYPE
                   SYNTAX  INTEGER {
                        no(1),
                        additive(2)
                   }
                   ACCESS  read-write
                   STATUS  deprecated
                   DESCRIPTION
                           "Should the message be used as a temporary
                           banner. 1 - No. 2 - In addition to the normal
                           banner"
                   ::= { lts 8 }

               tsMsgSend OBJECT-TYPE
                   SYNTAX  INTEGER {
                        nothing(1),
                        reload(2),
                        messagedone(3),
                        abort(4)
                   }
                   ACCESS  read-write
                   STATUS  deprecated
                   DESCRIPTION
                           "Sends the message. The value determines what
                           to do after the message has completed."
                   ::= { lts 9 }

               tsClrTtyLine OBJECT-TYPE
                   SYNTAX  INTEGER
                   ACCESS  read-write
                   STATUS  deprecated
                   DESCRIPTION
                           "tty line to clear.  Read returns the last line
                           cleared.  A value of -1 indicates no lines have 
                           been cleared."
                   ::= { lts 10 }

END

