-- **********************************************************
-- Copyright 2007-20009 VMware, Inc.  All rights reserved. 
-- **********************************************************

VMWARE-RESOURCES-MIB DEFINITIONS ::= BEGIN

    IMPORTS
        MODULE-IDENTITY, OBJECT-IDENTITY, OBJECT-TYPE, Gauge32, Integer32
    FROM SNMPv2-SMI
        DisplayString
    FROM SNMPv2-TC
        MODULE-COMPLIANCE, OBJECT-GROUP
    FROM SNMPv2-CONF
        VmwSubsystemStatus
    FROM VMWARE-TC-MIB
        vmwResources
    FROM VMWARE-ROOT-MIB;

    vmwResourcesMIB MODULE-IDENTITY
    LAST-UPDATED "200810150000Z"
    ORGANIZATION "VMware, Inc"
    CONTACT-INFO
    "VMware, Inc
    3401 Hillview Ave
    Palo Alto, CA 94304
    Tel: 1-877-486-9273 or 650-427-5000
    Fax: 650-427-5001
    Web: http://communities.vmware.com/community/developer/forums/managementapi
    "
DESCRIPTION
     "This MIB module provides instrumentation of ESX Hypervisor resources such 
      as cpu, memory, and disk."

REVISION      "200810150000Z"
DESCRIPTION
     "All per-VM managed objects were moved to new managed objects in VMWARE-VMINFO MIB.
      See VMWARE-OBSOLETE-RESOURCE-MIB for oid assignments in prior version of this mib module.
      Add to comments the Managed Object Browser (MOB) URLs which provide 
      data this MIB module exposes."

REVISION      "200712270000Z"
DESCRIPTION
    "This is the first revision in SMIv2 format. Prior version was published as SMIv1."
::= { vmwResources 10 }

vmwCPU OBJECT-IDENTITY
STATUS  current
DESCRIPTION
    "Information about physical CPU(s)"
::= { vmwResources 1 }

vmwNumCPUs OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of physical CPUs on the system."
    ::= { vmwCPU 1 }

-- Memory subtree 

vmwMemory OBJECT IDENTIFIER ::= { vmwResources 2 }

vmwMemSize OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Amount of physical memory present on machine as provided by Hypervisor.
         It is computed from the sum of vmwMemCOS plus unreserved property as
         reported VIM subsystem. Unreserved is computed from hypervisor's total
         number of memory pages.

         VIM Parent Container: https://esx.example.com/mob/?moid=memorySystem
         VIM property: unreserved
         MOB: https://esx.example.com/mob/?moid=memoryManagerSystem&doPath=consoleReservationInfo

         For reference here two other related VIM properties:
         VIM property: memorySize
         MOB: https://esx.example.com/mob/?moid=ha%2dhost&doPath=summary%2ehardware
         
         VIM property: totalMemory
         MOB: https://esx.example.com/mob/?moid=ha%2dcompute%2dres&doPath=summary
         "
    ::= { vmwMemory 1 }

vmwMemCOS OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This managed object reports memory allocated for COS, theConsole OS
         (aka Service Console) which is a memory region carved out of physical
         memory to boot a RedHat Linux distribution/provides device management
         interface.

         Note that in the VMware ESXi product there is no COS so this will report 0.
         
         This managed object reports the amount of physical memory allocated to the COS.
         VIM Parent Container: https://esx.example.com/mob/?moid=memorySystem
         VIM property: serviceConsoleReserved
         MOB: https://esx.example.com/mob/?moid=memoryManagerSystem&doPath=consoleReservationInfo
        "
    ::= { vmwMemory 2 }

vmwMemAvail OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "kilobytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Amount of memory available to run Virutal Machines and to allocate for
         hypervisor needs. It is computed by subtracting vmwMemCOS from
         vmwMemSize. The result is the amount of memory available to VMs and to
         the hypervisor.

         To get a more accurate view of memory available to VMs the following property
         represents the amount of resources available for the root resource pool for running 
         virtual machines.

         VIM property: effectiveMemory
         MOB: https://esx.example.com/mob/?moid=ha%2dcompute%2dres&doPath=summary
        "
    ::= { vmwMemory 3 }


-- Storage subtree

vmwStorage OBJECT IDENTIFIER ::= { vmwResources 5 }
vmwHostBusAdapterNumber OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of entries in vmwHostBusAdapterTable."
    ::= { vmwStorage 1 }

vmwHostBusAdapterTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF VmwHostBusAdapterEntry
    MAX-ACCESS  not-accessible  
    STATUS      current
    DESCRIPTION
        "Inventory of Host Bus Adatpers found in this system. 
         CLI: esxcfg-scsidevs -a
         VIM Parent Container: https://esx.example.com/mob/?moid=storageSystem
         VIM property: hostBusAdapter
         MOB: https://esx.example.com/mob/?moid=storageSystem&doPath=storageDeviceInfo"
    ::= { vmwStorage 2 }

vmwHostBusAdapterEntry OBJECT-TYPE
    SYNTAX      VmwHostBusAdapterEntry
    MAX-ACCESS  not-accessible  
    STATUS      current
    DESCRIPTION
        "Details for this adapter."
    INDEX       { vmwHostBusAdapterIndex }
    ::= { vmwHostBusAdapterTable 1 }

VmwHostBusAdapterEntry ::= SEQUENCE
{
vmwHostBusAdapterIndex   Integer32,
vmwHbaDeviceName         DisplayString,
vmwHbaBusNumber          Integer32,
vmwHbaStatus             VmwSubsystemStatus,
vmwHbaModelName          DisplayString,
vmwHbaDriverName         DisplayString,
vmwHbaPci                DisplayString
}

vmwHostBusAdapterIndex OBJECT-TYPE
    SYNTAX      Integer32 (0..1023)
    MAX-ACCESS  not-accessible  
    STATUS      current
    DESCRIPTION
        "An arbitrary index assigned to this adapter."
    ::= { vmwHostBusAdapterEntry 1 }

vmwHbaDeviceName OBJECT-TYPE
    SYNTAX      DisplayString   
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The system device name for this host bus adapter."
    ::= { vmwHostBusAdapterEntry 2 }

vmwHbaBusNumber   OBJECT-TYPE
    SYNTAX      Integer32 (-1|0..1023)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The host bus number. For unsuported HBA's reports -1."
    ::= { vmwHostBusAdapterEntry 3 }

vmwHbaStatus    OBJECT-TYPE
    SYNTAX      VmwSubsystemStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The operational status of the adapter."
    ::= { vmwHostBusAdapterEntry 4 }

vmwHbaModelName  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The model name of the host bus adapter."
    ::= { vmwHostBusAdapterEntry 5 }

vmwHbaDriverName OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The name of the driver."
    ::= { vmwHostBusAdapterEntry 6 }

vmwHbaPci OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The Peripheral Connect Interface (PCI) ID of the device."
    ::= { vmwHostBusAdapterEntry 7 }

-- Net subtree
-- See IF-MIB for details of network interfaces


-- conformance information
vmwResourceMIBConformance
OBJECT IDENTIFIER ::= { vmwResourcesMIB 2 }
vmwResourceMIBCompliances
OBJECT IDENTIFIER ::= { vmwResourceMIBConformance 1 }
vmwResMIBGroups  OBJECT IDENTIFIER ::= { vmwResourceMIBConformance 2 }

-- compliance statements
vmwResourceMIBCompliance MODULE-COMPLIANCE
STATUS  current
DESCRIPTION
    "The compliance statement for entities which implement the 
    VMWARE-RESOURCE-MIB."
MODULE  -- this module
MANDATORY-GROUPS { vmwResourceGroup }
::= { vmwResourceMIBCompliances 2 }

vmwResourceGroup OBJECT-GROUP
    OBJECTS { 
    vmwNumCPUs,
    vmwMemSize,
    vmwMemCOS,
    vmwMemAvail,
    vmwHostBusAdapterNumber,
    vmwHbaDeviceName,
    vmwHbaBusNumber,
    vmwHbaStatus,
    vmwHbaModelName,
    vmwHbaDriverName,
    vmwHbaPci
    }
    STATUS  current
    DESCRIPTION
        "These objects provide resource details."
    ::= { vmwResMIBGroups 1 }


END
